<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.3">
<drawing>
<library>
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
This library contains footprints for SparkFun breakout boards, microcontrollers (Arduino, Particle, Teensy, etc.),  breadboards, non-RF modules, etc.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ARDUINO_MEGA_NO_SILK">
<description>&lt;h3&gt; Arduino MEGA R3 footprint&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:82&lt;/li&gt;
&lt;li&gt;Area:4x2.15 in&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;

&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Arduino Mega R3&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="BREADBOARD-MINI">
<description>&lt;h3&gt;Breadboard Mini&lt;/h3&gt;
&lt;p&gt; Includes tdocu indicating solderable breadboard mini footprint&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Specifications:&lt;/b&gt;
&lt;li&gt;Area:1.8x 1.4 inch&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;

&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Breadboard Mini&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="MICRO-SDCARD">
<description>&lt;h3&gt;microSD Card Footprint&lt;/h3&gt;
Silk outline with pads for SMD. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Area:0.45x0.6 in&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;MicroSD Card&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SD-MMC-CARD">
<description>&lt;h3&gt; SD MMC Card Footprint&lt;/h3&gt;
Basic reference with pads for SMD mounting of SD card. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:9&lt;/li&gt;
&lt;li&gt;Area:0.95x1.25 inch&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;SD Card&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="WIZ811MJ">
<description>&lt;h3&gt;WIZnet W5100 Network Module with MagJack - WIZ811MJ Footprint&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:40&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;li&gt;Area:2.05x1.0"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;WIZNet&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="AUDIO-AMP-MONO">
<description>&lt;h3&gt;Audio Amp Mono PCB&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 10&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;li&gt;Area:0.8x0.8 in&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;

&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Audio Amp Mono&lt;/li&gt;

&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="ARDUINO_PRO_MINI">
<description>&lt;h3&gt;Arduino Pro Mini Footprint&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 34&lt;/li&gt;
&lt;li&gt;Area: 1.7 x 0.3 in&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Arduino Pro Mini&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SPARKFUN_LOGIC_LEVEL_CONVERTER">
<description>&lt;h3&gt;SparkFun Logic Level Converter&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:12&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;li&gt;Area: 0.6x 0.5 "&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;SparkFun Logic Level Converter&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="UNO_R3_SHIELD">
<description>&lt;h3&gt;Arduino Uno-Compatible Footprint&lt;/h3&gt;
No holes, no ICSP connections.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 32&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;li&gt;Area:2.1x2.35"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Arduino Uno R3 Shield&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SPARKFUN_PRO_MICRO">
<description>&lt;h3&gt;SparkFun Pro Mico Footprint (with USB connector)&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 24&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;li&gt;Area:0.7x1.3"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;SparkFun Pro Micro&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="UNO_R3_SHIELD_NOLABELS">
<description>&lt;h3&gt;Arduino Uno-Compatible Footprint&lt;/h3&gt;
No holes, no ICSP connections, no silk labels. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 32&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;li&gt;Area:2.1x2.35"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Arduino Uno R3 Shield&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="BEAGLE_BONE_BLACK_CAPE">
<description>&lt;h3&gt;BeagleBone Black Cape Footprint&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:92&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;li&gt;Area:3.4x2.15 in&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;BeagleBone Black Cape&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SPARKFUN_BLACKBERRY_TRACKBALLER">
<description>&lt;h3&gt; SparkFun BlackBerry Trackballer&lt;/h3&gt;
Footprint for Blackberry trackball.  
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:11&lt;/li&gt;
&lt;li&gt;Area:1.10x0.95 inch&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;SparkFun Blackberry Trackball&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="UNO_R3_SHIELD_LOCK">
<description>&lt;h3&gt;Arduino Uno-Compatible Footprint&lt;/h3&gt;
No holes, no ICSP connections.
Locking footprint for headers.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 32&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;li&gt;Area:2.1x2.35"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Arduino Uno R3 Shield&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="UNO_R3_SHIELD_NOLABELS_LOCK">
<description>&lt;h3&gt;Arduino Uno-Compatible Footprint&lt;/h3&gt;
No holes, no ICSP connections, no silk labels.
Looking footprint for headers.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 32&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;li&gt;Area:2.1x2.35"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Arduino Uno R3 Shield&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="FLANGED_RED_ENCLOSURE-OUTLINE">
<description>&lt;h3&gt;Big Red Enclosure PCB&lt;/h3&gt;
&lt;p&gt;Dimension Footprint for mounting holes only&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:0&lt;/li&gt;
&lt;li&gt;Area:5.91x3.23 in&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Big Red Box-PCB&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="FLANGED_RED_ENCLOSURE-DIMENSION">
<description>&lt;h3&gt;Big Red Enclosure PCB&lt;/h3&gt;
&lt;p&gt;Basic dimension for board outline and mounting  holes&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:0&lt;/li&gt;
&lt;li&gt;Area:5.91x3.23 in&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Big Red Box-PCB&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="ARDUINO_R3">
<description>&lt;h3&gt;Arduino Uno R3 Footprint&lt;/h3&gt;
Includes mounting holes, and holes for ICSP header
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 38&lt;/li&gt;
&lt;li&gt;Area:2.7x2.1in&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Arduino Uno R3&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="ARDUINO_R3_NO_HOLES">
<description>&lt;h3&gt;Arduino Uno R3 Footprint&lt;/h3&gt;
Includes holes for ICSP header
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 38&lt;/li&gt;
&lt;li&gt;Area:2.7x2.1in&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Arduino Uno R3&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="TEENSY-3.1">
<description>&lt;h3&gt;Teensy 3 Footprint&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:37&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;li&gt;Area:0.7x1.4"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Teensy 3.1&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="TEENSY-3.1_NOSILK">
<description>&lt;h3&gt;Teensy 3 Footprint- No Silk Label on Pins&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:37&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;li&gt;Area:0.7x1.4"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Teensy 3.1&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="MOJO_V3">
<description>&lt;h3&gt;Mojo v3 FPGA Footprint&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:110&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;li&gt;Area:3.1x2.5 inch&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Mojo&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="MOJO_V3_NO_LABEL">
<description>&lt;h3&gt;Mojo v3 FPGA Footprint&lt;/h3&gt;
No silk labels on pins
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:110&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;li&gt;Area:3.1x2.5 inch&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Mojo&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SPARKFUN_EDISON_PCB">
<description>&lt;h3&gt; SparkFun Edison PCB&lt;/h3&gt;
Footprint for Edison PCBs (view that mates with Edison SBC).
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:11&lt;/li&gt;
&lt;li&gt;Area:1.20 x 1.75 inch&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;SparkFun Edison&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="ISL29125">
<description>&lt;h3&gt;SparkFun ISL29125 Breakout&lt;/h3&gt;
Has dimension references for mounting holes and board outline. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 5&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;li&gt;Area: 0.7x0.65 in&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;ISL29125 Breakout&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="UNO_R3_SHIELD_ICSP">
<description>&lt;h3&gt;Arduino Uno-Compatible Footprint with ICSP&lt;/h3&gt;
No mounting holes.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 38&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;li&gt;Area:2.1x2.35"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Arduino Uno R3 Shield ICSP&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="UNO_R3_SHIELD_ICSP_NOLABELS">
<description>&lt;h3&gt;Arduino Uno-Compatible Footprint with ICSP&lt;/h3&gt;
No mounting holes, no silk labels on pins. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 38&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;li&gt;Area:2.1x2.35"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Arduino Uno R3 Shield ICSP&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SPARKFUN_ESP8266_THING">
<description>&lt;h3&gt;SparkFun Thing Board Footprint&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 20&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1 inch&lt;/li&gt;
&lt;li&gt;Area: 2.2 x 1.0 inchees&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;SparkFun Thing&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SPARKFUN_ESP8266_THING_DEV">
<description>&lt;h3&gt;SparkFun Thing Development Board Footprint&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 20&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1 inch&lt;/li&gt;
&lt;li&gt;Area: 2.2 x 1.0 inchees&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;SparkFun Thing Development Board&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SPARKFUN_EDISON_DAUGHTER">
<description>&lt;h3&gt; SparkFun Edison Daughter&lt;/h3&gt;
Footprint for mating with Edison SBC.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:11&lt;/li&gt;
&lt;li&gt;Area: 0.98 x 1.4 inch&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;SparkFun Edison&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="ELECTRIC_IMP_IMP002">
</package>
<package name="DIL40_0.9">
<description>Dual inline 40 pin package for mbed microcontroller development platform.</description>
</package>
<package name="QDUINO_MINI_V15">
<description>&lt;h3&gt;Qduino Mini Board Outline and Pins&lt;/h3&gt;
&lt;p&gt;Board outline for &lt;a href="https://www.sparkfun.com/products/13614"&gt;SparkFun Qduino Mini&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Devices using:&lt;ul&gt;
&lt;li&gt;QDUINOMINI&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="PARTICLE_PHOTON">
<description>&lt;h3&gt;Particle Photon&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 24&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;li&gt;Area: 0.8 x 1.4 inches&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Particle Photon&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="PARTICLE_PHOTON_TEMPLATE">
<description>&lt;h3&gt;Particle Photon Template&lt;/h3&gt;
&lt;p&gt; Used for laying out a shield that breaks out Photon pins.&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:48&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;li&gt;Area: 0.8 x 1.4 inches&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Particle Photon&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="PARTICLE_PHOTON_TEMPLATE_WIDE">
<description>&lt;h3&gt;Particle Photon Template wIDE&lt;/h3&gt;
&lt;p&gt; Used for laying out a shield that breaks out Photon pins with 0.2" spacing.&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:48&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;li&gt;Area: 1.6 x 1.4 inches&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Particle Photon&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SPARKFUN_MS5803-14BA_BREAKOUT">
<description>&lt;h3&gt;SparkFun MS5803-14BA Breakout&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:7&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;li&gt;Area: 0.8x0.7"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;SPARKFUN_MS5803-14BA_BREAKOUT&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SPARKFUN_NRF52832_BREAKOUT">
<description>&lt;h3&gt;SparkFun nRF42832 Breakout&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:42&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;li&gt;Area: 0.7x2.05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;SPARKFUN_NRF42832_BREAKOUT&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="ESP32_THING">
<description>&lt;h3&gt;SparkFun ESP32 Thing Board&lt;/h3&gt;
&lt;p&gt;Pins, silkscreen, and logos matching the layout of the &lt;a href=https://www.sparkfun.com/products/13907&gt;SparkFun ESP32 Thing&lt;/a&gt;&lt;/p&gt;

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 40&lt;/li&gt;
&lt;li&gt;Area: 2.32" x 1.00"&lt;/li&gt;
&lt;/p&gt;</description>
</package>
<package name="PARTICLE_PHOTON_TEMPLATE_NO_STANDOFF">
</package>
<package name="SPARKFUN_LOGIC_LEVEL_CONVERTER_LOCK">
</package>
<package name="ESP32_THING_NO_ANT">
</package>
<package name="TEENSYVIEW">
</package>
<package name="CAN485">
</package>
<package name="CAN485_PRO_MINI">
</package>
<package name="RFM69_BOB">
</package>
<package name="ARDUINO_R3_LOCK_HOLES">
</package>
<package name="MICROSD-BREAKOUT">
</package>
<package name="ATLAS_CONDUCTIVITY">
</package>
<package name="ATLAS_BNC">
</package>
<package name="CAN485_OUTER_ONLY">
</package>
<package name="SPARKFUN_OPTOISOLATOR-BOB">
</package>
</packages>
<symbols>
<symbol name="ARDUINO-MEGA">
<description>&lt;h3&gt;Arduino Mega R3&lt;/h3&gt;
&lt;p&gt;Symbol showing all pin connections for Arduino Mega R3.&lt;/p&gt;</description>
<pin name="5V"/>
<pin name="!RESET"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="A9"/>
<pin name="A10"/>
<pin name="A11"/>
<pin name="A12"/>
<pin name="A13"/>
<pin name="A14"/>
<pin name="A15"/>
<pin name="1(TX0)"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="16(TX2)"/>
<pin name="17(RX2)"/>
<pin name="18(TX1)"/>
<pin name="22"/>
<pin name="23"/>
<pin name="24"/>
<pin name="25"/>
<pin name="26"/>
<pin name="27"/>
<pin name="28"/>
<pin name="29"/>
<pin name="30"/>
<pin name="31"/>
<pin name="32"/>
<pin name="33"/>
<pin name="34"/>
<pin name="35"/>
<pin name="36"/>
<pin name="37"/>
<pin name="38"/>
<pin name="40"/>
<pin name="39"/>
<pin name="41"/>
<pin name="42"/>
<pin name="43"/>
<pin name="44"/>
<pin name="45"/>
<pin name="46"/>
<pin name="47"/>
<pin name="48"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="15(RX3)"/>
<pin name="14(TX3)"/>
<pin name="GND"/>
<pin name="53/!CS"/>
<pin name="52/SCK"/>
<pin name="51/MOSI"/>
<pin name="50/MISO"/>
<pin name="49"/>
<pin name="3.3V"/>
<pin name="AREF"/>
<pin name="21(SCL)"/>
<pin name="20(SDA)"/>
<pin name="19(RX1)"/>
<pin name="VIN"/>
<pin name="0(RX0)"/>
<pin name="GND@3"/>
<pin name="GND@2"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="IOREF"/>
</symbol>
<symbol name="BREADBOARD">
<description>&lt;h3&gt;Breadboard&lt;/h3&gt;
&lt;p&gt;Placeholder symbol for board silk for small breadboard.&lt;/p&gt;</description>
</symbol>
<symbol name="MICRO-SDCARD">
<description>&lt;h3&gt; microSD Card&lt;/h3&gt;

&lt;p&gt;Breaks out all standard pins from microSD spec.&lt;/p&gt;</description>
<pin name="CD/DAT3"/>
<pin name="CMD"/>
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="CLK"/>
<pin name="DAT0"/>
<pin name="DAT1"/>
<pin name="DAT2"/>
</symbol>
<symbol name="SD-MMC-CARD">
<description>&lt;h3&gt;SD/MMC Card &lt;/h3&gt;
&lt;p&gt;Breaks out all 9 pins for SD/MMC cards&lt;/p&gt;</description>
<pin name="DAT2"/>
<pin name="CD/DAT3"/>
<pin name="CMD"/>
<pin name="VSS1"/>
<pin name="VDD"/>
<pin name="DAT1"/>
<pin name="DAT0"/>
<pin name="VSS2"/>
<pin name="CLK"/>
</symbol>
<symbol name="WIZ811MJ">
<description>&lt;h3&gt;WIZNet 811MJ Breakout board&lt;/h3&gt;
&lt;p&gt;WIZnet’s WIZ811MJ works as a breakout board for their W5100 embedded TCP/IP chip. Also included on the board is an RJ-45 MagJack connector (RJ45 with X’FMR). It can be used as a component and little effort is required to interface to the W5100. The WIZ811MJ is an ideal option for users who want a simple solution to adding TCP/IP capability to their project.

There is no on-board regulation. All pins of the W5100 are broken out to two pairs of 10-pin, 0.1" pitch headers.&lt;/p&gt;</description>
<pin name="VCC@1"/>
<pin name="VCC@2"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="GND@4"/>
<pin name="GND@5"/>
<pin name="SCLK"/>
<pin name="/SCS"/>
<pin name="MOSI"/>
<pin name="MISO"/>
<pin name="A14"/>
<pin name="A13"/>
<pin name="A12"/>
<pin name="A11"/>
<pin name="A10"/>
<pin name="A9"/>
<pin name="A8"/>
<pin name="A7"/>
<pin name="D7"/>
<pin name="D6"/>
<pin name="D5"/>
<pin name="D4"/>
<pin name="D3"/>
<pin name="D2"/>
<pin name="D1"/>
<pin name="/RD"/>
<pin name="/CS"/>
<pin name="/WR"/>
<pin name="/INT"/>
<pin name="D0"/>
<pin name="/RESET"/>
<pin name="A6"/>
<pin name="A5"/>
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
</symbol>
<symbol name="AUDIO-AMP-MONO">
<description>&lt;h3&gt;SparkFun Mono Audio Amplifier&lt;/h3&gt;
&lt;p&gt;2.5V to 5.5V input, 1.4W in 8Ohms&lt;/p&gt;</description>
<pin name="OUT+"/>
<pin name="OUT-"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="*SHTDWN"/>
<pin name="VCC@VOL"/>
<pin name="VOL"/>
<pin name="GND@VOL"/>
<pin name="IN-"/>
<pin name="IN+"/>
</symbol>
<symbol name="PRO_MINI">
<description>&lt;h3&gt;Arduino Pro Mini&lt;/h3&gt;
&lt;p&gt;3.3V/5V and 8MHz/16MHz. Includes connections for the updated ADC6/ADC7 pins.&lt;/p&gt;</description>
<pin name="2"/>
<pin name="*3"/>
<pin name="4"/>
<pin name="*5"/>
<pin name="*6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="*9"/>
<pin name="*10"/>
<pin name="*11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="RAW" direction="pwr"/>
<pin name="RST"/>
<pin name="RST@2"/>
<pin name="RXI"/>
<pin name="TXO"/>
<pin name="VCC" direction="pwr"/>
<pin name="A7"/>
<pin name="A6"/>
<pin name="A4"/>
<pin name="A5"/>
</symbol>
<symbol name="LOGIC_LEVEL_CONVERTER">
<description>&lt;h3&gt;SparkFun Logic Level Converter - Bidirectional&lt;/h3&gt;
&lt;p&gt;3.3v-5v&lt;/p&gt;</description>
<pin name="HV_TXO_1"/>
<pin name="HV_RXI_1"/>
<pin name="HV" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="HV_RXI_2"/>
<pin name="HV_TXO_2"/>
<pin name="LV_TXI_1"/>
<pin name="LV" direction="pwr"/>
<pin name="LV_RXO_1"/>
<pin name="GND" direction="pwr"/>
<pin name="LV_RXO_2"/>
<pin name="LV_TXI_2"/>
</symbol>
<symbol name="ARDUINO_R3_SHIELD">
<description>&lt;h3&gt;Arduino Uno R3-No ICSP&lt;/h3&gt;
&lt;p&gt;Symbol showing all standard pins on Arduino Uno R3 footprint (no ICSP pins)&lt;/p&gt;</description>
<pin name="RX"/>
<pin name="TX"/>
<pin name="D2"/>
<pin name="*D3"/>
<pin name="D4"/>
<pin name="*D5"/>
<pin name="*D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="*D9"/>
<pin name="*D10"/>
<pin name="*D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="VIN"/>
<pin name="RES"/>
<pin name="5V"/>
<pin name="AREF"/>
<pin name="GND@2"/>
<pin name="GND@1"/>
<pin name="GND@0"/>
<pin name="3.3V"/>
<pin name="IOREF"/>
<pin name="SDA"/>
<pin name="SCL"/>
</symbol>
<symbol name="SPARKFUN_PRO_MICRO">
<description>&lt;h3&gt;SparkFun Pro Micro&lt;/h3&gt;
&lt;p&gt;3.3V/5V at 8MHz/16MHz. Does not require a USB to serial converter board for programming.  &lt;/p&gt;</description>
<pin name="2"/>
<pin name="*3"/>
<pin name="4"/>
<pin name="*5"/>
<pin name="*6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="*9"/>
<pin name="*10"/>
<pin name="11(MOSI)"/>
<pin name="12(MISO)"/>
<pin name="13(SCK)"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="RAW" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="RESET"/>
<pin name="RXI"/>
<pin name="TXO"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="BEAGLE_BONE_BLACK_P8">
<description>&lt;h3&gt;Beagle Bone Black - Expansion Header P8 Pinout &lt;/h3&gt;
&lt;p&gt; Default configuration of pins on power up on P8 expansion header. &lt;/p&gt;</description>
<pin name="DGND@1"/>
<pin name="GPIO_38"/>
<pin name="GPIO_39"/>
<pin name="GPIO_34"/>
<pin name="GPIO_35"/>
<pin name="GPIO_66"/>
<pin name="GPIO_67"/>
<pin name="GPIO_69"/>
<pin name="GPIO_68"/>
<pin name="GPIO_45"/>
<pin name="GPIO_44"/>
<pin name="GPIO_23"/>
<pin name="GPIO_26"/>
<pin name="GPIO_47"/>
<pin name="GPIO_46"/>
<pin name="GPIO_27"/>
<pin name="GPIO_65"/>
<pin name="GPIO_22"/>
<pin name="GPIO_63"/>
<pin name="GPIO_62"/>
<pin name="GPIO_37"/>
<pin name="GPIO_36"/>
<pin name="GPIO_61"/>
<pin name="GPIO_32"/>
<pin name="GPIO_88"/>
<pin name="GPIO_86"/>
<pin name="GPIO_89"/>
<pin name="GPIO_87"/>
<pin name="GPIO_11"/>
<pin name="GPIO_10"/>
<pin name="GPIO_81"/>
<pin name="GPIO_9"/>
<pin name="GPIO_80"/>
<pin name="GPIO_8"/>
<pin name="GPIO_79"/>
<pin name="GPIO_76"/>
<pin name="GPIO_77"/>
<pin name="GPIO_74"/>
<pin name="GPIO_75"/>
<pin name="DGND@2"/>
<pin name="GPIO_72"/>
<pin name="GPIO_73"/>
<pin name="GPIO_70"/>
<pin name="GPIO_71"/>
<pin name="GPIO_78"/>
<pin name="GPIO_33"/>
</symbol>
<symbol name="BEAGLE_BONE_BLACK_P9">
<description>&lt;h3&gt;Beagle Bone Black - Expansion Header P9 Pinout &lt;/h3&gt;
&lt;p&gt; Default configuration of pins on power up on P9 expansion header. &lt;/p&gt;</description>
<pin name="DGND@1"/>
<pin name="VDD_3V3@1"/>
<pin name="VDD_3V3@2"/>
<pin name="SYS_5V@1"/>
<pin name="SYS_5V@2"/>
<pin name="PWR_BUT"/>
<pin name="SYS_RESET!N"/>
<pin name="GPIO_30"/>
<pin name="GPIO_60"/>
<pin name="GPIO_31"/>
<pin name="GPIO_40"/>
<pin name="GPIO_48"/>
<pin name="GPIO_51"/>
<pin name="GPIO_4"/>
<pin name="GPIO_5"/>
<pin name="I2C2_SCL"/>
<pin name="I2C2_SDA"/>
<pin name="GPIO_3"/>
<pin name="GPIO_2"/>
<pin name="GPIO_49"/>
<pin name="GPIO_15"/>
<pin name="GPIO_117"/>
<pin name="GPIO_14"/>
<pin name="GPIO_125"/>
<pin name="GPIO_123"/>
<pin name="GPIO_121"/>
<pin name="GPIO_122"/>
<pin name="GPIO_120"/>
<pin name="VDD_ADC"/>
<pin name="AIN4"/>
<pin name="GNDA_ADC"/>
<pin name="AIN6"/>
<pin name="AIN5"/>
<pin name="AIN2"/>
<pin name="AIN3"/>
<pin name="AIN0"/>
<pin name="AIN1"/>
<pin name="GPIO_20"/>
<pin name="GPIO_7"/>
<pin name="DGND@2"/>
<pin name="DGND@3"/>
<pin name="DGND@4"/>
<pin name="DGND@5"/>
<pin name="DGND@6"/>
<pin name="VDD_5V@1"/>
<pin name="VDD_5V@2"/>
</symbol>
<symbol name="BLACKBERRY_TRACKBALLER">
<description>&lt;h3&gt;SparkFun BlackBerry Trackballer&lt;/h3&gt;
&lt;p&gt;&lt;li&gt;2.5-5.5V input&lt;/li&gt;
&lt;li&gt;RGBW LED included in trackball&lt;/li&gt;
&lt;li&gt;Reads directions Up, Down, Left, Right, and Button Click&lt;/li&gt;&lt;/p&gt;</description>
<pin name="UP" direction="out"/>
<pin name="DWN" direction="out"/>
<pin name="LFT" direction="out"/>
<pin name="RHT" direction="out"/>
<pin name="WHT" direction="in"/>
<pin name="RED" direction="in"/>
<pin name="BLU" direction="in"/>
<pin name="GRN" direction="in"/>
<pin name="BTN" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="ARDUINO_R3">
<description>&lt;h3&gt;Arduino Uno R3&lt;/h3&gt;
&lt;p&gt;Symbol showing all available pins on Arduino Uno R3 footprint (including ICSP)&lt;/p&gt;</description>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="*D3"/>
<pin name="D4"/>
<pin name="*D5"/>
<pin name="*D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="*D9"/>
<pin name="*D10"/>
<pin name="*D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="VIN"/>
<pin name="!RESET!@1"/>
<pin name="5V"/>
<pin name="AREF"/>
<pin name="GND@2"/>
<pin name="GND@1"/>
<pin name="GND@0"/>
<pin name="3.3V"/>
<pin name="IOREF"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="VCC"/>
<pin name="MISO"/>
<pin name="MOSI"/>
<pin name="SCK"/>
<pin name="!RESET!@2"/>
<pin name="GND"/>
</symbol>
<symbol name="TEENSY-31">
<description>&lt;h3&gt;Teensy 3.1&lt;/h3&gt;
&lt;p&gt;Breaks out all the PTH pins on the Teensy 3.1. Does not break out all of the additional SMD pins on the underside of the Teensy, or the external crystal pins. &lt;/p&gt;</description>
<pin name="GND1" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="VBAT" direction="pwr"/>
<pin name="3.3V" direction="pwr"/>
<pin name="3V" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="A0/14"/>
<pin name="A1/15"/>
<pin name="A2/16"/>
<pin name="A3/17"/>
<pin name="A4/18/SDA0"/>
<pin name="A5/19/SCL0"/>
<pin name="A6/20*"/>
<pin name="A7/21*"/>
<pin name="A8/22*"/>
<pin name="A9/23*"/>
<pin name="10*/TX2/CS"/>
<pin name="11/DOUT"/>
<pin name="12/DIN"/>
<pin name="13/SCK"/>
<pin name="A10"/>
<pin name="A11"/>
<pin name="A14/DAC"/>
<pin name="AREF"/>
<pin name="VUSB" direction="pwr"/>
<pin name="8/TX3"/>
<pin name="7/RX3"/>
<pin name="6*"/>
<pin name="5*"/>
<pin name="4*"/>
<pin name="3*"/>
<pin name="2"/>
<pin name="1/TX1"/>
<pin name="0/RX1"/>
<pin name="9*/RX2"/>
<pin name="PROG"/>
</symbol>
<symbol name="MOJO_ANALOG_HEADER">
<description>&lt;h3&gt;Mojo v3 FPGA Dev Board - Analog Pins &lt;/h3&gt;
&lt;p&gt;Only shows the analog pins available on the board.&lt;/p&gt;</description>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="AREF" direction="in"/>
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="MOJO_HEADER_1">
<description>&lt;h3&gt;Mojo v3 FPGA Dev Board - Header 1 &lt;/h3&gt;
&lt;p&gt;Only shows the header 1 pins available on the board.&lt;/p&gt;</description>
<pin name="+V" direction="sup"/>
<pin name="1"/>
<pin name="2"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="21"/>
<pin name="22"/>
<pin name="23"/>
<pin name="24"/>
<pin name="26"/>
<pin name="27"/>
<pin name="29"/>
<pin name="30"/>
<pin name="32"/>
<pin name="33"/>
<pin name="34"/>
<pin name="35"/>
<pin name="40"/>
<pin name="41"/>
<pin name="50"/>
<pin name="51"/>
<pin name="123"/>
<pin name="124"/>
<pin name="126"/>
<pin name="127"/>
<pin name="131"/>
<pin name="132"/>
<pin name="133"/>
<pin name="134"/>
<pin name="137"/>
<pin name="138"/>
<pin name="139"/>
<pin name="140"/>
<pin name="141"/>
<pin name="142"/>
<pin name="143"/>
<pin name="144"/>
<pin name="GND@1" direction="sup"/>
<pin name="GND@2" direction="sup"/>
<pin name="RAW" direction="sup"/>
</symbol>
<symbol name="MOJO_HEADER_2">
<description>&lt;h3&gt;Mojo v3 FPGA Dev Board - Header 2 Pins &lt;/h3&gt;
&lt;p&gt;Only shows the Header 2 pins available on the board.&lt;/p&gt;</description>
<pin name="+V" direction="sup"/>
<pin name="57"/>
<pin name="58"/>
<pin name="66"/>
<pin name="67"/>
<pin name="74"/>
<pin name="75"/>
<pin name="78"/>
<pin name="79"/>
<pin name="80"/>
<pin name="81"/>
<pin name="82"/>
<pin name="83"/>
<pin name="84"/>
<pin name="85"/>
<pin name="87"/>
<pin name="88"/>
<pin name="92"/>
<pin name="93"/>
<pin name="94"/>
<pin name="95"/>
<pin name="97"/>
<pin name="98"/>
<pin name="99"/>
<pin name="100"/>
<pin name="101"/>
<pin name="102"/>
<pin name="104"/>
<pin name="105"/>
<pin name="111"/>
<pin name="112"/>
<pin name="114"/>
<pin name="115"/>
<pin name="116"/>
<pin name="117"/>
<pin name="118"/>
<pin name="119"/>
<pin name="120"/>
<pin name="121"/>
<pin name="DONE"/>
<pin name="GND@1" direction="sup"/>
<pin name="GND@2" direction="sup"/>
<pin name="GND@3" direction="sup"/>
<pin name="RAW" direction="sup"/>
<pin name="RST" direction="in"/>
<pin name="SUS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="TMS" direction="in"/>
</symbol>
<symbol name="MOJO_OUTLINE">
<description>&lt;h3&gt;Mojo v3 FPGA Dev Board -Outline &lt;/h3&gt;
&lt;p&gt;Silk outline of the Mojo board.&lt;/p&gt;</description>
</symbol>
<symbol name="EDISON_CONNECTOR_BASE">
<description>&lt;h3&gt;Intel Edison - Basic Connections&lt;/h3&gt;
&lt;p&gt;Basic power/IO connections required to get started with the module. 
Only shows part of the Hirose pins available on the Edison. &lt;/p&gt;</description>
<pin name="VSYS@1" direction="pwr"/>
<pin name="3.3V@1" direction="pwr"/>
<pin name="1.8V" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="3.3V@2" direction="pwr"/>
<pin name="VSYS@2" direction="pwr"/>
<pin name="VSYS@3" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="MSIC_SLP_CLK"/>
<pin name="PWRBTN#"/>
<pin name="V_VAT_BKUP" direction="pwr"/>
<pin name="RESET_OUT#"/>
<pin name="OSC_CLK_OUT_0"/>
<pin name="RCVR_MODE"/>
<pin name="FW_RCVR"/>
<pin name="DCIN" direction="pwr"/>
</symbol>
<symbol name="EDISON_CONNECTOR_GPIO">
<description>&lt;h3&gt;Intel Edison - GPIO Connections&lt;/h3&gt;
&lt;p&gt;GPIO connections on the module. 
Only shows part of the Hirose pins available on the Edison. &lt;/p&gt;</description>
<pin name="GP44"/>
<pin name="GP165"/>
<pin name="GP45"/>
<pin name="GP46"/>
<pin name="GP47"/>
<pin name="GP48"/>
<pin name="GP49"/>
<pin name="GP15"/>
<pin name="GP14"/>
<pin name="GP12_PWM0"/>
<pin name="GP13_PWM1"/>
<pin name="GP182_PWM2"/>
<pin name="GP183_PWM3"/>
</symbol>
<symbol name="EDISON_CONNECTOR_I2C_1">
<description>&lt;h3&gt;Intel Edison - I2C 1&lt;/h3&gt;
&lt;p&gt;I2C_1 connections on the module. 
Only shows part of the Hirose pins available on the Edison. &lt;/p&gt;</description>
<pin name="GP19_I2C_1_SCL"/>
<pin name="GP20_I2C_1_SDA"/>
</symbol>
<symbol name="EDISON_CONNECTOR_I2C_6">
<description>&lt;h3&gt;Intel Edison - I2C 6&lt;/h3&gt;
&lt;p&gt;I2C_6 connections on the module. 
Only shows part of the Hirose pins available on the Edison. &lt;/p&gt;</description>
<pin name="GP27_I2C_6_SCL"/>
<pin name="GP28_I2C_6_SDA"/>
</symbol>
<symbol name="EDISON_CONNECTOR_I2S_2">
<description>&lt;h3&gt;Intel Edison - I2S2&lt;/h3&gt;
&lt;p&gt;I2S2 connections on the module. 
Only shows part of the Hirose pins available on the Edison. &lt;/p&gt;</description>
<pin name="GP42_I2S_2_RXD"/>
<pin name="GP40_I2S_2_CLK"/>
<pin name="GP41_I2S_2_FS"/>
<pin name="GP43_I2S_2_TXD"/>
</symbol>
<symbol name="EDISON_CONNECTOR_SD">
<description>&lt;h3&gt;Intel Edison - SD&lt;/h3&gt;
&lt;p&gt;SD connections on the module. 
Only shows part of the Hirose pins available on the Edison. &lt;/p&gt;</description>
<pin name="GP78_SD_0_CLK"/>
<pin name="!GP77_SD_0_CD#"/>
<pin name="GP79_SD_0_CMD"/>
<pin name="GP80_SD_0_DAT0"/>
<pin name="GP81_SD_0_DAT1"/>
<pin name="GP82_SD_0_DAT2"/>
<pin name="GP83_SD_0_DAT3"/>
<pin name="GP84_SD_0_CLK_FB"/>
</symbol>
<symbol name="EDISON_CONNECTOR_SPI_2">
<description>&lt;h3&gt;Intel Edison - SPI 2&lt;/h3&gt;
&lt;p&gt;SPI 2 connections on the module. 
Only shows part of the Hirose pins available on the Edison. &lt;/p&gt;</description>
<pin name="GP111_SPI_2_FS1"/>
<pin name="GP110_SPI_2_FS0"/>
<pin name="GP109_SPI_2_CLK"/>
<pin name="GP115_SPI_2_TXD"/>
<pin name="GP114_SPI_2_RXD"/>
</symbol>
<symbol name="EDISON_CONNECTOR_UART_1">
<description>&lt;h3&gt;Intel Edison - UART 1&lt;/h3&gt;
&lt;p&gt;UART 1 connections on the module. 
Only shows part of the Hirose pins available on the Edison. &lt;/p&gt;</description>
<pin name="GP131_UART_1_TX"/>
<pin name="GP130_UART_1_RX"/>
<pin name="GP129_UART_1_RTS"/>
<pin name="GP128_UART_1_CTS"/>
</symbol>
<symbol name="EDISON_CONNECTOR_UART_2">
<description>&lt;h3&gt;Intel Edison - UART 2&lt;/h3&gt;
&lt;p&gt;UART 2 connections on the module. 
Only shows part of the Hirose pins available on the Edison. &lt;/p&gt;</description>
<pin name="GP134_UART_2_RX"/>
<pin name="GP135_UART_2_TX"/>
</symbol>
<symbol name="EDISON_CONNECTOR_USB">
<description>&lt;h3&gt;Intel Edison - USB&lt;/h3&gt;
&lt;p&gt;USB connections on the module. 
Only shows part of the Hirose pins available on the Edison. &lt;/p&gt;</description>
<pin name="USB_ID"/>
<pin name="USB_DP"/>
<pin name="USB_DN"/>
<pin name="USB_VBUS"/>
<pin name="FAULT"/>
<pin name="PSW"/>
</symbol>
<symbol name="RGB_LIGHT_SENSOR_ISL29125">
<description>&lt;h3&gt;SparkFun RGB Light Sensor - ISL29125&lt;/h3&gt;
&lt;p&gt;3.3V, I2C&lt;/li&gt;
&lt;li&gt;RGB Light sensor&lt;/li&gt;
&lt;/p&gt;</description>
<pin name="GND" direction="pwr"/>
<pin name="3.3V" direction="pwr"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="INT"/>
</symbol>
<symbol name="BIG_RED_PCB">
<description>&lt;h3&gt;Big Red PCB Symbol&lt;/h3&gt;

Symbol for the Big Red Enclosure PCB layout. This part is dimension-reference only, so there are no pins.</description>
</symbol>
<symbol name="ESP8266_THING">
<description>&lt;h3&gt;SparkFun Thing&lt;/h3&gt;
&lt;p&gt;Basic Breakout for ESP8266 WiFi IC. Includes:
&lt;li&gt;JST Battery connector&lt;/li&gt;
&lt;li&gt;On/off switch&lt;/li&gt;
Does not include connections for the onboard sensor footprints. &lt;/p&gt;</description>
<pin name="NC" direction="nc"/>
<pin name="DTR"/>
<pin name="TXO" direction="out"/>
<pin name="RXI" direction="in"/>
<pin name="VIN" direction="pwr"/>
<pin name="3.3V@1" direction="pwr"/>
<pin name="3.3V@2" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="SDA/2"/>
<pin name="SCL/14/SCLK"/>
<pin name="5"/>
<pin name="0"/>
<pin name="4"/>
<pin name="13/MOSI"/>
<pin name="12/MISO"/>
<pin name="XPD/16"/>
<pin name="ADC/A0"/>
<pin name="EN" direction="in"/>
</symbol>
<symbol name="ESP8266_THING_DEV">
<description>&lt;h3&gt;SparkFun Thing Dev Board&lt;/h3&gt;
&lt;p&gt;Basic Breakout for ESP8266 WiFi SoC with built-in FTDI USB-to-Serial.&lt;/p&gt;</description>
<pin name="NC" direction="nc"/>
<pin name="RST" direction="in"/>
<pin name="TXO/7" direction="out"/>
<pin name="RXI/8" direction="in"/>
<pin name="VIN" direction="pwr"/>
<pin name="3.3V" direction="pwr"/>
<pin name="5V" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="SDA/2"/>
<pin name="SCL/14/SCLK"/>
<pin name="5"/>
<pin name="0"/>
<pin name="4"/>
<pin name="13/MOSI"/>
<pin name="12/MISO"/>
<pin name="XPD/16"/>
<pin name="ADC/A0"/>
<pin name="15"/>
</symbol>
<symbol name="ELECTRIC_IMP_IMP002">
<pin name="PIN_1"/>
<pin name="PIN_2"/>
<pin name="PIN_5"/>
<pin name="PIN_6"/>
<pin name="PIN_7"/>
<pin name="PIN_8"/>
<pin name="PIN_9"/>
<pin name="PIN_A"/>
<pin name="PIN_B"/>
<pin name="PIN_C"/>
<pin name="PIN_D"/>
<pin name="PIN_E"/>
<pin name="OPTO_BIAS"/>
<pin name="OPTO_IN"/>
<pin name="LED_RED"/>
<pin name="LED_GREEN"/>
<pin name="POWER_EN"/>
<pin name="VDD@18"/>
<pin name="VDD@33"/>
<pin name="VDDA"/>
<pin name="GND@1"/>
<pin name="GND@7"/>
<pin name="GND@13"/>
<pin name="GND@17"/>
<pin name="GND@23"/>
<pin name="GND@24"/>
<pin name="GND@25"/>
<pin name="GND@26"/>
<pin name="GND@27"/>
<pin name="GND@28"/>
<pin name="GND@29"/>
<pin name="GND@30"/>
<pin name="GND@31"/>
<pin name="GND@32"/>
<pin name="GND@35"/>
</symbol>
<symbol name="MBED_NXP_LPC1768">
<description>&lt;h3&gt;mbed NXP LPC1768&lt;/h3&gt;
&lt;p&gt;Microcontroller development board featuring an ARM cortex M3 and an online IDE with driverless USB programming.&lt;/p&gt;</description>
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
<pin name="P$11"/>
<pin name="P$12"/>
<pin name="P$13"/>
<pin name="P$14"/>
<pin name="P$15"/>
<pin name="P$16"/>
<pin name="P$17"/>
<pin name="P$18"/>
<pin name="P$19"/>
<pin name="P$20"/>
<pin name="P$21"/>
<pin name="P$22"/>
<pin name="P$23"/>
<pin name="P$24"/>
<pin name="P$25"/>
<pin name="P$26"/>
<pin name="P$27"/>
<pin name="P$28"/>
<pin name="P$29"/>
<pin name="P$30"/>
<pin name="P$31"/>
<pin name="P$32"/>
<pin name="P$33"/>
<pin name="P$34"/>
<pin name="P$35"/>
<pin name="P$36"/>
<pin name="P$37"/>
<pin name="P$38"/>
<pin name="P$39"/>
<pin name="P$40"/>
</symbol>
<symbol name="QDUINOMINI">
<description>&lt;h3&gt;Qduino Mini Board Outline and Pins&lt;/h3&gt;
&lt;p&gt;Board outline for &lt;a href="https://www.sparkfun.com/products/13614"&gt;SparkFun Qduino Mini&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Devices using:&lt;ul&gt;
&lt;li&gt;QDUINOMINI&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="GND"/>
<pin name="LIPO"/>
<pin name="MISO"/>
<pin name="MOSI"/>
<pin name="RST"/>
<pin name="D0"/>
<pin name="SCK"/>
<pin name="D1"/>
<pin name="VCC"/>
<pin name="VUSB"/>
</symbol>
<symbol name="PARTICLE_PHOTON">
<description>&lt;h3&gt;Particle Photon &lt;/h3&gt;
&lt;p&gt;24 pin Particle PO Wi-Fi module&lt;/p&gt;</description>
<pin name="!RST!"/>
<pin name="(JTAG_TCK)D6"/>
<pin name="(JTAG_TDI)D5"/>
<pin name="(JTAG_TDO)D4"/>
<pin name="(JTAG_TMS)D7"/>
<pin name="(JTAG_TRST)D3"/>
<pin name="(SCL)D1"/>
<pin name="(SDA)D0"/>
<pin name="+3V3" direction="pwr"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2(SPI1_SS)"/>
<pin name="A3(SPI1_SCK)"/>
<pin name="A4(SPI1_MISO)"/>
<pin name="A5(SPI1_MOSI)"/>
<pin name="D2"/>
<pin name="DAC"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@21" direction="pwr"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="WKP"/>
</symbol>
<symbol name="SPARKFUN_MS5803-14BA_BREAKOUT">
<description>&lt;h3&gt;SparkFun MS5803-14BA_Breakout&lt;/h3&gt;
I2C Pressure Sensor Breakout.</description>
<pin name="GND"/>
<pin name="3.3V"/>
<pin name="PS"/>
<pin name="SDA/SDI"/>
<pin name="SCL/SCLK"/>
<pin name="SDO"/>
<pin name="AD/CS"/>
</symbol>
<symbol name="SPARKFUN_NRF52832_BREAKOUT">
<description>&lt;h3&gt;SparkFun nRF52832 Breakout&lt;/h3&gt;
&lt;p&gt;
SoC with a list of features including:
&lt;li&gt; 32 configurable I/O pins &lt;/li&gt;
&lt;li&gt;SPI&lt;/li&gt;
&lt;li&gt;I&lt;sup&gt;2&lt;/sup&gt;C&lt;/li&gt;
&lt;li&gt;UART&lt;/li&gt;
&lt;li&gt;PWM&lt;/li&gt;
&lt;li&gt;ADC&lt;/li&gt;
&lt;li&gt;512kB Flash&lt;/li&gt;
&lt;li&gt;64kB RAM&lt;/li&gt;
&lt;li&gt;2.4GHz multiprotocol radio&lt;/li&gt;
&lt;li&gt;supporting Bluetooth low energy (BLE)&lt;/li&gt;
&lt;li&gt;ANT&lt;/li&gt;
&lt;li&gt;on-chip NFC tag support&lt;/li&gt;</description>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="19"/>
<pin name="20"/>
<pin name="22"/>
<pin name="23"/>
<pin name="24"/>
<pin name="25"/>
<pin name="28/A4"/>
<pin name="29/A5"/>
<pin name="30/A6"/>
<pin name="31/A7"/>
<pin name="!RST"/>
<pin name="3.3V"/>
<pin name="VIN"/>
<pin name="GND"/>
<pin name="1-NFC"/>
<pin name="2-NFC"/>
<pin name="15"/>
<pin name="14"/>
<pin name="13"/>
<pin name="12"/>
<pin name="11"/>
<pin name="10"/>
<pin name="09"/>
<pin name="08"/>
<pin name="05/A3"/>
<pin name="04/A2"/>
<pin name="03/A1"/>
<pin name="02/A0"/>
<pin name="01/X2"/>
<pin name="VCC"/>
<pin name="00/X1"/>
<pin name="27/TX"/>
<pin name="26/RX"/>
</symbol>
<symbol name="ESP32_THING">
<description>&lt;h3&gt;SparkFun ESP32 Thing Board&lt;/h3&gt;
&lt;p&gt;Pins, silkscreen, and logos matching the layout of the &lt;a href=https://www.sparkfun.com/products/13907&gt;SparkFun ESP32 Thing&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Dimensions: 2.32" x 1.00"&lt;/p&gt;</description>
<pin name="GND@1"/>
<pin name="VUSB@2"/>
<pin name="VBAT@3"/>
<pin name="GND@4"/>
<pin name="3V3@5"/>
<pin name="!RST!"/>
<pin name="13"/>
<pin name="12"/>
<pin name="14"/>
<pin name="27"/>
<pin name="26"/>
<pin name="25"/>
<pin name="35"/>
<pin name="34"/>
<pin name="33"/>
<pin name="32"/>
<pin name="39"/>
<pin name="38"/>
<pin name="37"/>
<pin name="36"/>
<pin name="GND@40"/>
<pin name="VUSB@39"/>
<pin name="VBAT@38"/>
<pin name="GND@37"/>
<pin name="3V3@36"/>
<pin name="16"/>
<pin name="17"/>
<pin name="4"/>
<pin name="0"/>
<pin name="2"/>
<pin name="15"/>
<pin name="5"/>
<pin name="18"/>
<pin name="23"/>
<pin name="19"/>
<pin name="22"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="21"/>
<pin name="GND@21"/>
</symbol>
<symbol name="TEENSYVIEW_1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="TEENSYVIEW_2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="CAN485">
<pin name="485A"/>
<pin name="485B"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="CANHI"/>
<pin name="CANLO"/>
<pin name="CTS"/>
<pin name="D2/INT0/SCL"/>
<pin name="D3/INT1/SDA"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="DTR"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="GND3"/>
<pin name="GND4"/>
<pin name="MISO/D12"/>
<pin name="MOSI/D11"/>
<pin name="RAW"/>
<pin name="RESET1"/>
<pin name="RESET"/>
<pin name="RXI"/>
<pin name="RXI1"/>
<pin name="SCK/D13"/>
<pin name="TXO"/>
<pin name="TXO1"/>
<pin name="VCC"/>
<pin name="VCC1"/>
<pin name="A6"/>
<pin name="A7"/>
</symbol>
<symbol name="CAN485_PRO_MINI">
<pin name="485A"/>
<pin name="485B"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4M"/>
<pin name="A5M"/>
<pin name="CANHI"/>
<pin name="CANLO"/>
<pin name="CTS"/>
<pin name="D2/INT0/SCL"/>
<pin name="D3/INT1/SDA"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="DTR"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="GND3"/>
<pin name="GND4"/>
<pin name="MISO/D12"/>
<pin name="MOSI/D11"/>
<pin name="RAW"/>
<pin name="RESET1"/>
<pin name="RESET"/>
<pin name="RXI"/>
<pin name="RXI1"/>
<pin name="SCK/D13"/>
<pin name="TXO"/>
<pin name="TXO1"/>
<pin name="VCC"/>
<pin name="VCC1"/>
</symbol>
<symbol name="RFM69_BOB">
<pin name="O"/>
<pin name="I"/>
<pin name="C"/>
<pin name="S"/>
<pin name="R"/>
<pin name="0"/>
<pin name="G"/>
<pin name="3.3V"/>
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="G2"/>
<pin name="A"/>
<pin name="GND"/>
</symbol>
<symbol name="MICROSD-BREAKOUT">
<description>&lt;h3&gt; microSD Card&lt;/h3&gt;

&lt;p&gt;Breaks out all standard pins from microSD spec.&lt;/p&gt;</description>
<pin name="DI"/>
<pin name="VCC"/>
<pin name="SCK"/>
<pin name="GND" direction="pwr"/>
<pin name="DO"/>
<pin name="CD"/>
<pin name="CS"/>
</symbol>
<symbol name="ATLAS_CONDUCTIVITY">
<description>&lt;h3&gt; microSD Card&lt;/h3&gt;

&lt;p&gt;Breaks out all standard pins from microSD spec.&lt;/p&gt;</description>
<pin name="VCC" direction="pwr"/>
<pin name="TX/SDA"/>
<pin name="RX/SCL"/>
<pin name="GND" direction="pwr"/>
<pin name="PRB@2"/>
<pin name="PRB@1"/>
</symbol>
<symbol name="ATLAS_BNC">
<description>&lt;h3&gt; microSD Card&lt;/h3&gt;

&lt;p&gt;Breaks out all standard pins from microSD spec.&lt;/p&gt;</description>
<pin name="@NC" direction="nc"/>
<pin name="CENTER"/>
<pin name="GND"/>
</symbol>
<symbol name="CAN485_OUTER_ONLY">
<pin name="485A"/>
<pin name="485B"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="CANHI"/>
<pin name="CANLO"/>
<pin name="CTS"/>
<pin name="D2/INT0/SCL"/>
<pin name="D3/INT1/SDA"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="DTR"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="GND3"/>
<pin name="GND4"/>
<pin name="MISO/D12"/>
<pin name="MOSI/D11"/>
<pin name="RAW"/>
<pin name="RESET1"/>
<pin name="RESET"/>
<pin name="RXI"/>
<pin name="RXI1"/>
<pin name="SCK/D13"/>
<pin name="TXO"/>
<pin name="TXO1"/>
<pin name="VCC"/>
<pin name="VCC1"/>
</symbol>
<symbol name="SPARKFUN_OPTOISOLATOR-BOB">
<pin name="GND"/>
<pin name="HV"/>
<pin name="HVG"/>
<pin name="IN1"/>
<pin name="IN2"/>
<pin name="NC"/>
<pin name="OUT1"/>
<pin name="OUT2"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ARDUINO_MEGA_R3" prefix="B">
<description>&lt;h3&gt;Arduino Mega R3&lt;/h3&gt;
&lt;p&gt;ATmega2560 R3 compatible footprint. &lt;/p&gt;


&lt;b&gt;&lt;p&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/11061”&gt;Arduino Mega 2560 R3&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="B1" symbol="ARDUINO-MEGA"/>
</gates>
<devices>
<device name="FULL" package="ARDUINO_MEGA_NO_SILK">
<connects>
<connect gate="B1" pin="!RESET" pad="RESET"/>
<connect gate="B1" pin="0(RX0)" pad="0"/>
<connect gate="B1" pin="1(TX0)" pad="1"/>
<connect gate="B1" pin="10" pad="10"/>
<connect gate="B1" pin="11" pad="11"/>
<connect gate="B1" pin="12" pad="12"/>
<connect gate="B1" pin="13" pad="13"/>
<connect gate="B1" pin="14(TX3)" pad="14"/>
<connect gate="B1" pin="15(RX3)" pad="15"/>
<connect gate="B1" pin="16(TX2)" pad="16"/>
<connect gate="B1" pin="17(RX2)" pad="17"/>
<connect gate="B1" pin="18(TX1)" pad="18"/>
<connect gate="B1" pin="19(RX1)" pad="19"/>
<connect gate="B1" pin="2" pad="2"/>
<connect gate="B1" pin="20(SDA)" pad="20"/>
<connect gate="B1" pin="21(SCL)" pad="21"/>
<connect gate="B1" pin="22" pad="22"/>
<connect gate="B1" pin="23" pad="23"/>
<connect gate="B1" pin="24" pad="24"/>
<connect gate="B1" pin="25" pad="25"/>
<connect gate="B1" pin="26" pad="26"/>
<connect gate="B1" pin="27" pad="27"/>
<connect gate="B1" pin="28" pad="28"/>
<connect gate="B1" pin="29" pad="29"/>
<connect gate="B1" pin="3" pad="3"/>
<connect gate="B1" pin="3.3V" pad="3.3V"/>
<connect gate="B1" pin="30" pad="30"/>
<connect gate="B1" pin="31" pad="31"/>
<connect gate="B1" pin="32" pad="32"/>
<connect gate="B1" pin="33" pad="33"/>
<connect gate="B1" pin="34" pad="34"/>
<connect gate="B1" pin="35" pad="35"/>
<connect gate="B1" pin="36" pad="36"/>
<connect gate="B1" pin="37" pad="37"/>
<connect gate="B1" pin="38" pad="38"/>
<connect gate="B1" pin="39" pad="39"/>
<connect gate="B1" pin="4" pad="4"/>
<connect gate="B1" pin="40" pad="40"/>
<connect gate="B1" pin="41" pad="41"/>
<connect gate="B1" pin="42" pad="42"/>
<connect gate="B1" pin="43" pad="43"/>
<connect gate="B1" pin="44" pad="44"/>
<connect gate="B1" pin="45" pad="45"/>
<connect gate="B1" pin="46" pad="46"/>
<connect gate="B1" pin="47" pad="47"/>
<connect gate="B1" pin="48" pad="48"/>
<connect gate="B1" pin="49" pad="49"/>
<connect gate="B1" pin="5" pad="5"/>
<connect gate="B1" pin="50/MISO" pad="50"/>
<connect gate="B1" pin="51/MOSI" pad="51"/>
<connect gate="B1" pin="52/SCK" pad="52"/>
<connect gate="B1" pin="53/!CS" pad="53"/>
<connect gate="B1" pin="5V" pad="5V 5V@1 5V@2"/>
<connect gate="B1" pin="6" pad="6"/>
<connect gate="B1" pin="7" pad="7"/>
<connect gate="B1" pin="8" pad="8"/>
<connect gate="B1" pin="9" pad="9"/>
<connect gate="B1" pin="A0" pad="A0"/>
<connect gate="B1" pin="A1" pad="A1"/>
<connect gate="B1" pin="A10" pad="A10"/>
<connect gate="B1" pin="A11" pad="A11"/>
<connect gate="B1" pin="A12" pad="A12"/>
<connect gate="B1" pin="A13" pad="A13"/>
<connect gate="B1" pin="A14" pad="A14"/>
<connect gate="B1" pin="A15" pad="A15"/>
<connect gate="B1" pin="A2" pad="A2"/>
<connect gate="B1" pin="A3" pad="A3"/>
<connect gate="B1" pin="A4" pad="A4"/>
<connect gate="B1" pin="A5" pad="A5"/>
<connect gate="B1" pin="A6" pad="A6"/>
<connect gate="B1" pin="A7" pad="A7"/>
<connect gate="B1" pin="A8" pad="A8"/>
<connect gate="B1" pin="A9" pad="A9"/>
<connect gate="B1" pin="AREF" pad="AREF"/>
<connect gate="B1" pin="GND" pad="GND GND@3 GND@4" route="any"/>
<connect gate="B1" pin="GND@2" pad="GND@1"/>
<connect gate="B1" pin="GND@3" pad="GND@2"/>
<connect gate="B1" pin="IOREF" pad="IOREF"/>
<connect gate="B1" pin="SCL" pad="SCL"/>
<connect gate="B1" pin="SDA" pad="SDA"/>
<connect gate="B1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOJO" prefix="B">
<description>&lt;h3&gt;Mojo v3 FPGA Development Board&lt;/h3&gt;
&lt;p&gt;Mechanical footprint with connectors for Mojo FPGA dev board.&lt;/p&gt;

&lt;b&gt;&lt;p&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/11953"&gt;Mojo v3&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MOJO_ANALOG_HEADER"/>
<gate name="G$2" symbol="MOJO_HEADER_1"/>
<gate name="G$3" symbol="MOJO_HEADER_2"/>
</gates>
<devices>
<device name="V3" package="MOJO_V3">
<connects>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="GND" pad="GND@5"/>
<connect gate="G$2" pin="+V" pad="V@1"/>
<connect gate="G$2" pin="1" pad="1"/>
<connect gate="G$2" pin="10" pad="10"/>
<connect gate="G$2" pin="11" pad="11"/>
<connect gate="G$2" pin="12" pad="12"/>
<connect gate="G$2" pin="123" pad="123"/>
<connect gate="G$2" pin="124" pad="124"/>
<connect gate="G$2" pin="126" pad="126"/>
<connect gate="G$2" pin="127" pad="127"/>
<connect gate="G$2" pin="131" pad="131"/>
<connect gate="G$2" pin="132" pad="132"/>
<connect gate="G$2" pin="133" pad="133"/>
<connect gate="G$2" pin="134" pad="134"/>
<connect gate="G$2" pin="137" pad="137"/>
<connect gate="G$2" pin="138" pad="138"/>
<connect gate="G$2" pin="139" pad="139"/>
<connect gate="G$2" pin="14" pad="14"/>
<connect gate="G$2" pin="140" pad="140"/>
<connect gate="G$2" pin="141" pad="141"/>
<connect gate="G$2" pin="142" pad="142"/>
<connect gate="G$2" pin="143" pad="143"/>
<connect gate="G$2" pin="144" pad="144"/>
<connect gate="G$2" pin="15" pad="15"/>
<connect gate="G$2" pin="16" pad="16"/>
<connect gate="G$2" pin="17" pad="17"/>
<connect gate="G$2" pin="2" pad="2"/>
<connect gate="G$2" pin="21" pad="21"/>
<connect gate="G$2" pin="22" pad="22"/>
<connect gate="G$2" pin="23" pad="23"/>
<connect gate="G$2" pin="24" pad="24"/>
<connect gate="G$2" pin="26" pad="26"/>
<connect gate="G$2" pin="27" pad="27"/>
<connect gate="G$2" pin="29" pad="29"/>
<connect gate="G$2" pin="30" pad="30"/>
<connect gate="G$2" pin="32" pad="32"/>
<connect gate="G$2" pin="33" pad="33"/>
<connect gate="G$2" pin="34" pad="34"/>
<connect gate="G$2" pin="35" pad="35"/>
<connect gate="G$2" pin="40" pad="40"/>
<connect gate="G$2" pin="41" pad="41"/>
<connect gate="G$2" pin="5" pad="5"/>
<connect gate="G$2" pin="50" pad="50"/>
<connect gate="G$2" pin="51" pad="51"/>
<connect gate="G$2" pin="6" pad="6"/>
<connect gate="G$2" pin="7" pad="7"/>
<connect gate="G$2" pin="8" pad="8"/>
<connect gate="G$2" pin="9" pad="9"/>
<connect gate="G$2" pin="GND@1" pad="GND@1"/>
<connect gate="G$2" pin="GND@2" pad="GND@2"/>
<connect gate="G$2" pin="RAW" pad="RAW@1"/>
<connect gate="G$3" pin="+V" pad="V@2"/>
<connect gate="G$3" pin="100" pad="100"/>
<connect gate="G$3" pin="101" pad="101"/>
<connect gate="G$3" pin="102" pad="102"/>
<connect gate="G$3" pin="104" pad="104"/>
<connect gate="G$3" pin="105" pad="105"/>
<connect gate="G$3" pin="111" pad="111"/>
<connect gate="G$3" pin="112" pad="112"/>
<connect gate="G$3" pin="114" pad="114"/>
<connect gate="G$3" pin="115" pad="115"/>
<connect gate="G$3" pin="116" pad="116"/>
<connect gate="G$3" pin="117" pad="117"/>
<connect gate="G$3" pin="118" pad="118"/>
<connect gate="G$3" pin="119" pad="119"/>
<connect gate="G$3" pin="120" pad="120"/>
<connect gate="G$3" pin="121" pad="121"/>
<connect gate="G$3" pin="57" pad="57"/>
<connect gate="G$3" pin="58" pad="58"/>
<connect gate="G$3" pin="66" pad="66"/>
<connect gate="G$3" pin="67" pad="67"/>
<connect gate="G$3" pin="74" pad="74"/>
<connect gate="G$3" pin="75" pad="75"/>
<connect gate="G$3" pin="78" pad="78"/>
<connect gate="G$3" pin="79" pad="79"/>
<connect gate="G$3" pin="80" pad="80"/>
<connect gate="G$3" pin="81" pad="81"/>
<connect gate="G$3" pin="82" pad="82"/>
<connect gate="G$3" pin="83" pad="83"/>
<connect gate="G$3" pin="84" pad="84"/>
<connect gate="G$3" pin="85" pad="85"/>
<connect gate="G$3" pin="87" pad="87"/>
<connect gate="G$3" pin="88" pad="88"/>
<connect gate="G$3" pin="92" pad="92"/>
<connect gate="G$3" pin="93" pad="93"/>
<connect gate="G$3" pin="94" pad="94"/>
<connect gate="G$3" pin="95" pad="95"/>
<connect gate="G$3" pin="97" pad="97"/>
<connect gate="G$3" pin="98" pad="98"/>
<connect gate="G$3" pin="99" pad="99"/>
<connect gate="G$3" pin="DONE" pad="DONE"/>
<connect gate="G$3" pin="GND@1" pad="GND@3"/>
<connect gate="G$3" pin="GND@2" pad="GND@4"/>
<connect gate="G$3" pin="GND@3" pad="GND@6"/>
<connect gate="G$3" pin="RAW" pad="RAW@2"/>
<connect gate="G$3" pin="RST" pad="RST"/>
<connect gate="G$3" pin="SUS" pad="SUS"/>
<connect gate="G$3" pin="TCK" pad="TCK"/>
<connect gate="G$3" pin="TDI" pad="TDI"/>
<connect gate="G$3" pin="TDO" pad="TDO"/>
<connect gate="G$3" pin="TMS" pad="TMS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V3_NO_LABEL" package="MOJO_V3_NO_LABEL">
<connects>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A9" pad="A9"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="GND" pad="GND@5"/>
<connect gate="G$2" pin="+V" pad="V@1"/>
<connect gate="G$2" pin="1" pad="1"/>
<connect gate="G$2" pin="10" pad="10"/>
<connect gate="G$2" pin="11" pad="11"/>
<connect gate="G$2" pin="12" pad="12"/>
<connect gate="G$2" pin="123" pad="123"/>
<connect gate="G$2" pin="124" pad="124"/>
<connect gate="G$2" pin="126" pad="126"/>
<connect gate="G$2" pin="127" pad="127"/>
<connect gate="G$2" pin="131" pad="131"/>
<connect gate="G$2" pin="132" pad="132"/>
<connect gate="G$2" pin="133" pad="133"/>
<connect gate="G$2" pin="134" pad="134"/>
<connect gate="G$2" pin="137" pad="137"/>
<connect gate="G$2" pin="138" pad="138"/>
<connect gate="G$2" pin="139" pad="139"/>
<connect gate="G$2" pin="14" pad="14"/>
<connect gate="G$2" pin="140" pad="140"/>
<connect gate="G$2" pin="141" pad="141"/>
<connect gate="G$2" pin="142" pad="142"/>
<connect gate="G$2" pin="143" pad="143"/>
<connect gate="G$2" pin="144" pad="144"/>
<connect gate="G$2" pin="15" pad="15"/>
<connect gate="G$2" pin="16" pad="16"/>
<connect gate="G$2" pin="17" pad="17"/>
<connect gate="G$2" pin="2" pad="2"/>
<connect gate="G$2" pin="21" pad="21"/>
<connect gate="G$2" pin="22" pad="22"/>
<connect gate="G$2" pin="23" pad="23"/>
<connect gate="G$2" pin="24" pad="24"/>
<connect gate="G$2" pin="26" pad="26"/>
<connect gate="G$2" pin="27" pad="27"/>
<connect gate="G$2" pin="29" pad="29"/>
<connect gate="G$2" pin="30" pad="30"/>
<connect gate="G$2" pin="32" pad="32"/>
<connect gate="G$2" pin="33" pad="33"/>
<connect gate="G$2" pin="34" pad="34"/>
<connect gate="G$2" pin="35" pad="35"/>
<connect gate="G$2" pin="40" pad="40"/>
<connect gate="G$2" pin="41" pad="41"/>
<connect gate="G$2" pin="5" pad="5"/>
<connect gate="G$2" pin="50" pad="50"/>
<connect gate="G$2" pin="51" pad="51"/>
<connect gate="G$2" pin="6" pad="6"/>
<connect gate="G$2" pin="7" pad="7"/>
<connect gate="G$2" pin="8" pad="8"/>
<connect gate="G$2" pin="9" pad="9"/>
<connect gate="G$2" pin="GND@1" pad="GND@1"/>
<connect gate="G$2" pin="GND@2" pad="GND@2"/>
<connect gate="G$2" pin="RAW" pad="RAW@1"/>
<connect gate="G$3" pin="+V" pad="V@2"/>
<connect gate="G$3" pin="100" pad="100"/>
<connect gate="G$3" pin="101" pad="101"/>
<connect gate="G$3" pin="102" pad="102"/>
<connect gate="G$3" pin="104" pad="104"/>
<connect gate="G$3" pin="105" pad="105"/>
<connect gate="G$3" pin="111" pad="111"/>
<connect gate="G$3" pin="112" pad="112"/>
<connect gate="G$3" pin="114" pad="114"/>
<connect gate="G$3" pin="115" pad="115"/>
<connect gate="G$3" pin="116" pad="116"/>
<connect gate="G$3" pin="117" pad="117"/>
<connect gate="G$3" pin="118" pad="118"/>
<connect gate="G$3" pin="119" pad="119"/>
<connect gate="G$3" pin="120" pad="120"/>
<connect gate="G$3" pin="121" pad="121"/>
<connect gate="G$3" pin="57" pad="57"/>
<connect gate="G$3" pin="58" pad="58"/>
<connect gate="G$3" pin="66" pad="66"/>
<connect gate="G$3" pin="67" pad="67"/>
<connect gate="G$3" pin="74" pad="74"/>
<connect gate="G$3" pin="75" pad="75"/>
<connect gate="G$3" pin="78" pad="78"/>
<connect gate="G$3" pin="79" pad="79"/>
<connect gate="G$3" pin="80" pad="80"/>
<connect gate="G$3" pin="81" pad="81"/>
<connect gate="G$3" pin="82" pad="82"/>
<connect gate="G$3" pin="83" pad="83"/>
<connect gate="G$3" pin="84" pad="84"/>
<connect gate="G$3" pin="85" pad="85"/>
<connect gate="G$3" pin="87" pad="87"/>
<connect gate="G$3" pin="88" pad="88"/>
<connect gate="G$3" pin="92" pad="92"/>
<connect gate="G$3" pin="93" pad="93"/>
<connect gate="G$3" pin="94" pad="94"/>
<connect gate="G$3" pin="95" pad="95"/>
<connect gate="G$3" pin="97" pad="97"/>
<connect gate="G$3" pin="98" pad="98"/>
<connect gate="G$3" pin="99" pad="99"/>
<connect gate="G$3" pin="DONE" pad="DONE"/>
<connect gate="G$3" pin="GND@1" pad="GND@3"/>
<connect gate="G$3" pin="GND@2" pad="GND@4"/>
<connect gate="G$3" pin="GND@3" pad="GND@6"/>
<connect gate="G$3" pin="RAW" pad="RAW@2"/>
<connect gate="G$3" pin="RST" pad="RST"/>
<connect gate="G$3" pin="SUS" pad="SUS"/>
<connect gate="G$3" pin="TCK" pad="TCK"/>
<connect gate="G$3" pin="TDI" pad="TDI"/>
<connect gate="G$3" pin="TDO" pad="TDO"/>
<connect gate="G$3" pin="TMS" pad="TMS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BREADBOARD" prefix="B">
<description>&lt;h3&gt;SparkFun Breadboard Mini&lt;/h3&gt;
&lt;p&gt;This is the mechnical outline for the very small self adhesive breadboard from SparkFun Electronics and our prototyping breadboard of the same size. Good for very small proto areas.&lt;/p&gt;


&lt;b&gt;&lt;p&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/7916”&gt;White&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12046”&gt;Green&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12047”&gt;Black&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12044"&gt;Red&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12045"&gt;Blue&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12702"&gt;SparkFun Solder-able Breadboard-Mini&lt;/a&gt;&lt;/li&gt;

&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BREADBOARD"/>
</gates>
<devices>
<device name="MINI" package="BREADBOARD-MINI">
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-12034"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MICRO-SDCARD" prefix="B">
<description>&lt;h3&gt;microSD Card Footprint &lt;/h3&gt;
&lt;p&gt;This is the mechnical footprint with connections for soldering a microSD card - &lt;b&gt;NOT&lt;/b&gt; for a socket for the card.&lt;/p&gt;

&lt;b&gt;&lt;p&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/11609"&gt;MicroSD Card with Adapter - 8 GB&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/9419"&gt;SparkFun microSD Sniffer&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MICRO-SDCARD"/>
</gates>
<devices>
<device name="" package="MICRO-SDCARD">
<connects>
<connect gate="G$1" pin="CD/DAT3" pad="CD/DAT3"/>
<connect gate="G$1" pin="CLK" pad="CLK"/>
<connect gate="G$1" pin="CMD" pad="CMD"/>
<connect gate="G$1" pin="DAT0" pad="DAT0"/>
<connect gate="G$1" pin="DAT1" pad="DAT1"/>
<connect gate="G$1" pin="DAT2" pad="DAT2"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VDD" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SD_MMC_CARD" prefix="B">
<description>&lt;h3&gt;SD MMC Card Footprint&lt;/h3&gt;
&lt;p&gt;Mechanical footprint with connectors of an SD/MMC card- &lt;b&gt;NOT&lt;/b&gt; a socket!&lt;/p&gt;

&lt;b&gt;&lt;p&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/11395"&gt;Electric Imp&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13833"&gt;microSD Card with SD adapter&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SD-MMC-CARD"/>
</gates>
<devices>
<device name="SD_PCB" package="SD-MMC-CARD">
<connects>
<connect gate="G$1" pin="CD/DAT3" pad="1"/>
<connect gate="G$1" pin="CLK" pad="5"/>
<connect gate="G$1" pin="CMD" pad="2"/>
<connect gate="G$1" pin="DAT0" pad="7"/>
<connect gate="G$1" pin="DAT1" pad="8"/>
<connect gate="G$1" pin="DAT2" pad="9"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS1" pad="3"/>
<connect gate="G$1" pin="VSS2" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WIZ811MJ" prefix="B">
<description>&lt;h3&gt;WIZnet W%100 Network Module with Mag Jack - WIZ811MJ&lt;/h3&gt;
&lt;p&gt;Mechanical footprint with connectors for WIZ811MJ Breakout board with RJ45 connector.&lt;/p&gt;

&lt;b&gt;&lt;p&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/9473"&gt;WIZ811MJ Breakout&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="WIZ811MJ"/>
</gates>
<devices>
<device name="" package="WIZ811MJ">
<connects>
<connect gate="G$1" pin="/CS" pad="27"/>
<connect gate="G$1" pin="/INT" pad="28"/>
<connect gate="G$1" pin="/RD" pad="26"/>
<connect gate="G$1" pin="/RESET" pad="22"/>
<connect gate="G$1" pin="/SCS" pad="24"/>
<connect gate="G$1" pin="/WR" pad="25"/>
<connect gate="G$1" pin="A0" pad="31"/>
<connect gate="G$1" pin="A1" pad="32"/>
<connect gate="G$1" pin="A10" pad="15"/>
<connect gate="G$1" pin="A11" pad="16"/>
<connect gate="G$1" pin="A12" pad="17"/>
<connect gate="G$1" pin="A13" pad="18"/>
<connect gate="G$1" pin="A14" pad="19"/>
<connect gate="G$1" pin="A2" pad="33"/>
<connect gate="G$1" pin="A3" pad="34"/>
<connect gate="G$1" pin="A4" pad="35"/>
<connect gate="G$1" pin="A5" pad="36"/>
<connect gate="G$1" pin="A6" pad="37"/>
<connect gate="G$1" pin="A7" pad="38"/>
<connect gate="G$1" pin="A8" pad="13"/>
<connect gate="G$1" pin="A9" pad="14"/>
<connect gate="G$1" pin="D0" pad="4"/>
<connect gate="G$1" pin="D1" pad="3"/>
<connect gate="G$1" pin="D2" pad="6"/>
<connect gate="G$1" pin="D3" pad="5"/>
<connect gate="G$1" pin="D4" pad="8"/>
<connect gate="G$1" pin="D5" pad="7"/>
<connect gate="G$1" pin="D6" pad="10"/>
<connect gate="G$1" pin="D7" pad="9"/>
<connect gate="G$1" pin="GND@1" pad="11"/>
<connect gate="G$1" pin="GND@2" pad="29"/>
<connect gate="G$1" pin="GND@3" pad="39"/>
<connect gate="G$1" pin="GND@4" pad="40"/>
<connect gate="G$1" pin="GND@5" pad="30"/>
<connect gate="G$1" pin="MISO" pad="2"/>
<connect gate="G$1" pin="MOSI" pad="1"/>
<connect gate="G$1" pin="SCLK" pad="23"/>
<connect gate="G$1" pin="VCC@1" pad="12"/>
<connect gate="G$1" pin="VCC@2" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARKFUN_AUDIO-AMP-MONO" prefix="B">
<description>&lt;h3&gt;SparkFun Mono Audio Amp Breakout- TPA2005D1&lt;/h3&gt;
&lt;p&gt;This tiny audio amplifier is based on the Texas Instruments TPA2005D1. 
Its efficient class-D operation means low heat and long battery life.
 It can drive an 8-Ohm speaker at up to 1.4 Watts&lt;/p&gt;


&lt;b&gt;&lt;p&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/11044”&gt;Mono Audio Amp Breakout&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="U1" symbol="AUDIO-AMP-MONO"/>
</gates>
<devices>
<device name="DIP" package="AUDIO-AMP-MONO">
<connects>
<connect gate="U1" pin="*SHTDWN" pad="S"/>
<connect gate="U1" pin="GND" pad="PWR-"/>
<connect gate="U1" pin="GND@VOL" pad="VOL-"/>
<connect gate="U1" pin="IN+" pad="IN+"/>
<connect gate="U1" pin="IN-" pad="IN-"/>
<connect gate="U1" pin="OUT+" pad="OUT+"/>
<connect gate="U1" pin="OUT-" pad="OUT-"/>
<connect gate="U1" pin="VCC" pad="PWR+"/>
<connect gate="U1" pin="VCC@VOL" pad="VOL+"/>
<connect gate="U1" pin="VOL" pad="VOL"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO_PRO_MINI" prefix="B">
<description>&lt;h3&gt;SparkFun Pro Mini &lt;/h3&gt;
&lt;p&gt;Pro Mini compatible footprint.&lt;/p&gt;


&lt;p&gt;
&lt;li&gt;&lt;b&gt;Dimensions:&lt;/b&gt; 0.7 x 1.3"
&lt;li&gt;&lt;b&gt;PCB Thickness:&lt;/b&gt; 0.8mm
&lt;/p&gt;

&lt;b&gt;&lt;p&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/11114”&gt;3.3V/8MHz&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/11113”&gt;5V/16MHz&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="PRO_MINI"/>
</gates>
<devices>
<device name="" package="ARDUINO_PRO_MINI">
<connects>
<connect gate="G$1" pin="*10" pad="13"/>
<connect gate="G$1" pin="*11" pad="14"/>
<connect gate="G$1" pin="*3" pad="6"/>
<connect gate="G$1" pin="*5" pad="8"/>
<connect gate="G$1" pin="*6" pad="9"/>
<connect gate="G$1" pin="*9" pad="12"/>
<connect gate="G$1" pin="12" pad="15"/>
<connect gate="G$1" pin="13" pad="16"/>
<connect gate="G$1" pin="2" pad="5"/>
<connect gate="G$1" pin="4" pad="7"/>
<connect gate="G$1" pin="7" pad="10"/>
<connect gate="G$1" pin="8" pad="11"/>
<connect gate="G$1" pin="A0" pad="17"/>
<connect gate="G$1" pin="A1" pad="18"/>
<connect gate="G$1" pin="A2" pad="19"/>
<connect gate="G$1" pin="A3" pad="20"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="23"/>
<connect gate="G$1" pin="RAW" pad="24"/>
<connect gate="G$1" pin="RST" pad="3"/>
<connect gate="G$1" pin="RST@2" pad="22"/>
<connect gate="G$1" pin="RXI" pad="2"/>
<connect gate="G$1" pin="TXO" pad="1"/>
<connect gate="G$1" pin="VCC" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARKFUN_LOGIC_LEVEL_CONVERTER" prefix="B">
<description>&lt;h3&gt;SparkFun Logic Level Converter -Bi-Directional &lt;/h3&gt;
&lt;p&gt;This is the mechnical outline for the 3.3V - 5V bi directional logic level converter. &lt;/p&gt;

&lt;p&gt;*Note, the "LOCK" Package has the header pins staggered by an offset of 5 mils (off center line), so that when you slide a row of standard 0.1" headers into the PTH pads, it will hold position vertically.&lt;/p&gt;

See the follwing turorial for more information on this type of special footprints:

&lt;a href="https://www.sparkfun.com/tutorials/114"&gt;Sneaky Footprints&lt;/a&gt;


&lt;b&gt;&lt;p&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12009”&gt;SparkFun Logic Level Converter - Bi-Directional&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LOGIC_LEVEL_CONVERTER"/>
</gates>
<devices>
<device name="" package="SPARKFUN_LOGIC_LEVEL_CONVERTER">
<connects>
<connect gate="G$1" pin="GND" pad="GND1"/>
<connect gate="G$1" pin="GND@2" pad="GND2"/>
<connect gate="G$1" pin="HV" pad="HV"/>
<connect gate="G$1" pin="HV_RXI_1" pad="HV2"/>
<connect gate="G$1" pin="HV_RXI_2" pad="HV3"/>
<connect gate="G$1" pin="HV_TXO_1" pad="HV1"/>
<connect gate="G$1" pin="HV_TXO_2" pad="HV4"/>
<connect gate="G$1" pin="LV" pad="LV"/>
<connect gate="G$1" pin="LV_RXO_1" pad="LV2"/>
<connect gate="G$1" pin="LV_RXO_2" pad="LV3"/>
<connect gate="G$1" pin="LV_TXI_1" pad="LV1"/>
<connect gate="G$1" pin="LV_TXI_2" pad="LV4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="SPARKFUN_LOGIC_LEVEL_CONVERTER_LOCK">
<connects>
<connect gate="G$1" pin="GND" pad="GND1"/>
<connect gate="G$1" pin="GND@2" pad="GND2"/>
<connect gate="G$1" pin="HV" pad="HV"/>
<connect gate="G$1" pin="HV_RXI_1" pad="HV2"/>
<connect gate="G$1" pin="HV_RXI_2" pad="HV3"/>
<connect gate="G$1" pin="HV_TXO_1" pad="HV1"/>
<connect gate="G$1" pin="HV_TXO_2" pad="HV4"/>
<connect gate="G$1" pin="LV" pad="LV"/>
<connect gate="G$1" pin="LV_RXO_1" pad="LV2"/>
<connect gate="G$1" pin="LV_RXO_2" pad="LV3"/>
<connect gate="G$1" pin="LV_TXI_1" pad="LV1"/>
<connect gate="G$1" pin="LV_TXI_2" pad="LV4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO_UNO_R3_SHIELD" prefix="B">
<description>&lt;h3&gt;Arduino R3 Shield Footprint&lt;/h3&gt;

Shield form compatible with the Arduino Uno R3.

&lt;p&gt;SparkFun Products:
&lt;ul&gt;&lt;li&gt;&lt;a href=https://www.sparkfun.com/products/13120&gt;MG2639 Cellular Shield&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=https://www.sparkfun.com/products/12898&gt;MIDI Shield&lt;/a&gt;
&lt;li&gt;&lt;a href=https://www.sparkfun.com/products/11417&gt;R3 Stackable Headers Kit&lt;/a&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ARDUINO_R3_SHIELD"/>
</gates>
<devices>
<device name="BASIC" package="UNO_R3_SHIELD">
<connects>
<connect gate="G$1" pin="*D10" pad="D10"/>
<connect gate="G$1" pin="*D11" pad="D11"/>
<connect gate="G$1" pin="*D3" pad="D3"/>
<connect gate="G$1" pin="*D5" pad="D5"/>
<connect gate="G$1" pin="*D6" pad="D6"/>
<connect gate="G$1" pin="*D9" pad="D9"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="GND@0" pad="GND@0"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="IOREF" pad="IOREF"/>
<connect gate="G$1" pin="RES" pad="RES"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NOLABELS" package="UNO_R3_SHIELD_NOLABELS">
<connects>
<connect gate="G$1" pin="*D10" pad="D10"/>
<connect gate="G$1" pin="*D11" pad="D11"/>
<connect gate="G$1" pin="*D3" pad="D3"/>
<connect gate="G$1" pin="*D5" pad="D5"/>
<connect gate="G$1" pin="*D6" pad="D6"/>
<connect gate="G$1" pin="*D9" pad="D9"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="GND@0" pad="GND@0"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="IOREF" pad="IOREF"/>
<connect gate="G$1" pin="RES" pad="RES"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="UNO_R3_SHIELD_LOCK" package="UNO_R3_SHIELD_LOCK">
<connects>
<connect gate="G$1" pin="*D10" pad="D10"/>
<connect gate="G$1" pin="*D11" pad="D11"/>
<connect gate="G$1" pin="*D3" pad="D3"/>
<connect gate="G$1" pin="*D5" pad="D5"/>
<connect gate="G$1" pin="*D6" pad="D6"/>
<connect gate="G$1" pin="*D9" pad="D9"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="GND@0" pad="GND@0"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="IOREF" pad="IOREF"/>
<connect gate="G$1" pin="RES" pad="RES"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="UNO_R3_SHIELD_NOLABELS_LOCK" package="UNO_R3_SHIELD_NOLABELS_LOCK">
<connects>
<connect gate="G$1" pin="*D10" pad="D10"/>
<connect gate="G$1" pin="*D11" pad="D11"/>
<connect gate="G$1" pin="*D3" pad="D3"/>
<connect gate="G$1" pin="*D5" pad="D5"/>
<connect gate="G$1" pin="*D6" pad="D6"/>
<connect gate="G$1" pin="*D9" pad="D9"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="GND@0" pad="GND@0"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="IOREF" pad="IOREF"/>
<connect gate="G$1" pin="RES" pad="RES"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARKFUN_PRO_MICRO" prefix="B">
<description>&lt;h3&gt;SparkFun Pro Micro &lt;/h3&gt;
&lt;p&gt;Atmega32U4 compatible footprint.&lt;/p&gt;

&lt;b&gt;&lt;p&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12587”&gt;3.3V/8MHz&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12640”&gt;5V/16MHz&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SPARKFUN_PRO_MICRO"/>
</gates>
<devices>
<device name="" package="SPARKFUN_PRO_MICRO">
<connects>
<connect gate="G$1" pin="*10" pad="13"/>
<connect gate="G$1" pin="*3" pad="6"/>
<connect gate="G$1" pin="*5" pad="8"/>
<connect gate="G$1" pin="*6" pad="9"/>
<connect gate="G$1" pin="*9" pad="12"/>
<connect gate="G$1" pin="11(MOSI)" pad="14"/>
<connect gate="G$1" pin="12(MISO)" pad="15"/>
<connect gate="G$1" pin="13(SCK)" pad="16"/>
<connect gate="G$1" pin="2" pad="5"/>
<connect gate="G$1" pin="4" pad="7"/>
<connect gate="G$1" pin="7" pad="10"/>
<connect gate="G$1" pin="8" pad="11"/>
<connect gate="G$1" pin="A0" pad="17"/>
<connect gate="G$1" pin="A1" pad="18"/>
<connect gate="G$1" pin="A2" pad="19"/>
<connect gate="G$1" pin="A3" pad="20"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="23"/>
<connect gate="G$1" pin="RAW" pad="24"/>
<connect gate="G$1" pin="RESET" pad="22"/>
<connect gate="G$1" pin="RXI" pad="2"/>
<connect gate="G$1" pin="TXO" pad="1"/>
<connect gate="G$1" pin="VCC" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARKFUN_BEAGLE_BONE_BLACK_CAPE" prefix="B">
<description>&lt;h3&gt;BeagleBone Black Rev C Cape &lt;/h3&gt;
&lt;p&gt; Generic footprint for BeagleBone Black Rev C Capes.&lt;/p&gt;


&lt;b&gt;&lt;p&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12774”&gt;SparkFun BeagleBone Black Proto Cape&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12773”&gt;SparkFun CryptoCape&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="P8" symbol="BEAGLE_BONE_BLACK_P8"/>
<gate name="P9" symbol="BEAGLE_BONE_BLACK_P9"/>
</gates>
<devices>
<device name="" package="BEAGLE_BONE_BLACK_CAPE">
<connects>
<connect gate="P8" pin="DGND@1" pad="P8.1"/>
<connect gate="P8" pin="DGND@2" pad="P8.2"/>
<connect gate="P8" pin="GPIO_10" pad="P8.31"/>
<connect gate="P8" pin="GPIO_11" pad="P8.32"/>
<connect gate="P8" pin="GPIO_22" pad="P8.19"/>
<connect gate="P8" pin="GPIO_23" pad="P8.13"/>
<connect gate="P8" pin="GPIO_26" pad="P8.14"/>
<connect gate="P8" pin="GPIO_27" pad="P8.17"/>
<connect gate="P8" pin="GPIO_32" pad="P8.25"/>
<connect gate="P8" pin="GPIO_33" pad="P8.24"/>
<connect gate="P8" pin="GPIO_34" pad="P8.5"/>
<connect gate="P8" pin="GPIO_35" pad="P8.6"/>
<connect gate="P8" pin="GPIO_36" pad="P8.23"/>
<connect gate="P8" pin="GPIO_37" pad="P8.22"/>
<connect gate="P8" pin="GPIO_38" pad="P8.3"/>
<connect gate="P8" pin="GPIO_39" pad="P8.4"/>
<connect gate="P8" pin="GPIO_44" pad="P8.12"/>
<connect gate="P8" pin="GPIO_45" pad="P8.11"/>
<connect gate="P8" pin="GPIO_46" pad="P8.16"/>
<connect gate="P8" pin="GPIO_47" pad="P8.15"/>
<connect gate="P8" pin="GPIO_61" pad="P8.26"/>
<connect gate="P8" pin="GPIO_62" pad="P8.21"/>
<connect gate="P8" pin="GPIO_63" pad="P8.20"/>
<connect gate="P8" pin="GPIO_65" pad="P8.18"/>
<connect gate="P8" pin="GPIO_66" pad="P8.7"/>
<connect gate="P8" pin="GPIO_67" pad="P8.8"/>
<connect gate="P8" pin="GPIO_68" pad="P8.10"/>
<connect gate="P8" pin="GPIO_69" pad="P8.9"/>
<connect gate="P8" pin="GPIO_70" pad="P8.45"/>
<connect gate="P8" pin="GPIO_71" pad="P8.46"/>
<connect gate="P8" pin="GPIO_72" pad="P8.43"/>
<connect gate="P8" pin="GPIO_73" pad="P8.44"/>
<connect gate="P8" pin="GPIO_74" pad="P8.41"/>
<connect gate="P8" pin="GPIO_75" pad="P8.42"/>
<connect gate="P8" pin="GPIO_76" pad="P8.39"/>
<connect gate="P8" pin="GPIO_77" pad="P8.40"/>
<connect gate="P8" pin="GPIO_78" pad="P8.37"/>
<connect gate="P8" pin="GPIO_79" pad="P8.38"/>
<connect gate="P8" pin="GPIO_8" pad="P8.35"/>
<connect gate="P8" pin="GPIO_80" pad="P8.36"/>
<connect gate="P8" pin="GPIO_81" pad="P8.34"/>
<connect gate="P8" pin="GPIO_86" pad="P8.27"/>
<connect gate="P8" pin="GPIO_87" pad="P8.29"/>
<connect gate="P8" pin="GPIO_88" pad="P8.28"/>
<connect gate="P8" pin="GPIO_89" pad="P8.30"/>
<connect gate="P8" pin="GPIO_9" pad="P8.33"/>
<connect gate="P9" pin="AIN0" pad="P9.39"/>
<connect gate="P9" pin="AIN1" pad="P9.40"/>
<connect gate="P9" pin="AIN2" pad="P9.37"/>
<connect gate="P9" pin="AIN3" pad="P9.38"/>
<connect gate="P9" pin="AIN4" pad="P9.33"/>
<connect gate="P9" pin="AIN5" pad="P9.36"/>
<connect gate="P9" pin="AIN6" pad="P9.35"/>
<connect gate="P9" pin="DGND@1" pad="P9.1"/>
<connect gate="P9" pin="DGND@2" pad="P9.2"/>
<connect gate="P9" pin="DGND@3" pad="P9.43"/>
<connect gate="P9" pin="DGND@4" pad="P9.44"/>
<connect gate="P9" pin="DGND@5" pad="P9.45"/>
<connect gate="P9" pin="DGND@6" pad="P9.46"/>
<connect gate="P9" pin="GNDA_ADC" pad="P9.34"/>
<connect gate="P9" pin="GPIO_117" pad="P9.25"/>
<connect gate="P9" pin="GPIO_120" pad="P9.31"/>
<connect gate="P9" pin="GPIO_121" pad="P9.29"/>
<connect gate="P9" pin="GPIO_122" pad="P9.30"/>
<connect gate="P9" pin="GPIO_123" pad="P9.28"/>
<connect gate="P9" pin="GPIO_125" pad="P9.27"/>
<connect gate="P9" pin="GPIO_14" pad="P9.26"/>
<connect gate="P9" pin="GPIO_15" pad="P9.24"/>
<connect gate="P9" pin="GPIO_2" pad="P9.22"/>
<connect gate="P9" pin="GPIO_20" pad="P9.41"/>
<connect gate="P9" pin="GPIO_3" pad="P9.21"/>
<connect gate="P9" pin="GPIO_30" pad="P9.11"/>
<connect gate="P9" pin="GPIO_31" pad="P9.13"/>
<connect gate="P9" pin="GPIO_4" pad="P9.17"/>
<connect gate="P9" pin="GPIO_40" pad="P9.14"/>
<connect gate="P9" pin="GPIO_48" pad="P9.15"/>
<connect gate="P9" pin="GPIO_49" pad="P9.23"/>
<connect gate="P9" pin="GPIO_5" pad="P9.18"/>
<connect gate="P9" pin="GPIO_51" pad="P9.16"/>
<connect gate="P9" pin="GPIO_60" pad="P9.12"/>
<connect gate="P9" pin="GPIO_7" pad="P9.42"/>
<connect gate="P9" pin="I2C2_SCL" pad="P9.19"/>
<connect gate="P9" pin="I2C2_SDA" pad="P9.20"/>
<connect gate="P9" pin="PWR_BUT" pad="P9.9"/>
<connect gate="P9" pin="SYS_5V@1" pad="P9.7"/>
<connect gate="P9" pin="SYS_5V@2" pad="P9.8"/>
<connect gate="P9" pin="SYS_RESET!N" pad="P9.10"/>
<connect gate="P9" pin="VDD_3V3@1" pad="P9.3"/>
<connect gate="P9" pin="VDD_3V3@2" pad="P9.4"/>
<connect gate="P9" pin="VDD_5V@1" pad="P9.5"/>
<connect gate="P9" pin="VDD_5V@2" pad="P9.6"/>
<connect gate="P9" pin="VDD_ADC" pad="P9.32"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARKFUN_BLACKBERRY_TRACKBALLER" prefix="B">
<description>&lt;h3&gt;SparkFun Blackberry Trackballer Breakout &lt;/h3&gt;
&lt;p&gt;The SparkFun BlackBerry Trackballer Breakout gives you easy access to a trackball which measures up, down, left, and right movements, clicks on the board, as well as adding a bit of flair to your project with four built-in LEDs.&lt;/p&gt;


&lt;b&gt;&lt;p&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13169”&gt;SparkFun Blackberry Trackballer Breakout&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BLACKBERRY_TRACKBALLER"/>
</gates>
<devices>
<device name="" package="SPARKFUN_BLACKBERRY_TRACKBALLER">
<technologies>
<technology name="">
<attribute name="PROD_ID" value="PCB-12486"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO_UNO_R3" prefix="B">
<description>&lt;h3&gt;Arduino R3 Footprint with SPI header&lt;/h3&gt;

Arduino Uno R3 Compatible Footprint. Matches PCB size of the original board. 

&lt;p&gt;SparkFun Products:
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13672”&gt;SAMD21 Dev Breakout&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12757”&gt;RedBoard &lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/11417&gt;R3 Stackable Headers &lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ARDUINO_R3"/>
</gates>
<devices>
<device name="" package="ARDUINO_R3">
<connects>
<connect gate="G$1" pin="!RESET!@1" pad="RESET@1"/>
<connect gate="G$1" pin="!RESET!@2" pad="RESET@2"/>
<connect gate="G$1" pin="*D10" pad="D10"/>
<connect gate="G$1" pin="*D11" pad="D11"/>
<connect gate="G$1" pin="*D3" pad="D3"/>
<connect gate="G$1" pin="*D5" pad="D5"/>
<connect gate="G$1" pin="*D6" pad="D6"/>
<connect gate="G$1" pin="*D9" pad="D9"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D0" pad="D0"/>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="GND" pad="GND@1"/>
<connect gate="G$1" pin="GND@0" pad="GND@2"/>
<connect gate="G$1" pin="GND@1" pad="GND@3"/>
<connect gate="G$1" pin="GND@2" pad="GND@4"/>
<connect gate="G$1" pin="IOREF" pad="IOREF"/>
<connect gate="G$1" pin="MISO" pad="MISO"/>
<connect gate="G$1" pin="MOSI" pad="MOSI"/>
<connect gate="G$1" pin="SCK" pad="SCK"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NO_HOLES" package="ARDUINO_R3_NO_HOLES">
<connects>
<connect gate="G$1" pin="!RESET!@1" pad="RESET@1"/>
<connect gate="G$1" pin="!RESET!@2" pad="RESET@2"/>
<connect gate="G$1" pin="*D10" pad="D10"/>
<connect gate="G$1" pin="*D11" pad="D11"/>
<connect gate="G$1" pin="*D3" pad="D3"/>
<connect gate="G$1" pin="*D5" pad="D5"/>
<connect gate="G$1" pin="*D6" pad="D6"/>
<connect gate="G$1" pin="*D9" pad="D9"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D0" pad="D0"/>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="GND" pad="GND@1"/>
<connect gate="G$1" pin="GND@0" pad="GND@2"/>
<connect gate="G$1" pin="GND@1" pad="GND@3"/>
<connect gate="G$1" pin="GND@2" pad="GND@4"/>
<connect gate="G$1" pin="IOREF" pad="IOREF"/>
<connect gate="G$1" pin="MISO" pad="MISO"/>
<connect gate="G$1" pin="MOSI" pad="MOSI"/>
<connect gate="G$1" pin="SCK" pad="SCK"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_HOLES" package="ARDUINO_R3_LOCK_HOLES">
<connects>
<connect gate="G$1" pin="!RESET!@1" pad="RESET@1"/>
<connect gate="G$1" pin="!RESET!@2" pad="RESET@2"/>
<connect gate="G$1" pin="*D10" pad="D10"/>
<connect gate="G$1" pin="*D11" pad="D11"/>
<connect gate="G$1" pin="*D3" pad="D3"/>
<connect gate="G$1" pin="*D5" pad="D5"/>
<connect gate="G$1" pin="*D6" pad="D6"/>
<connect gate="G$1" pin="*D9" pad="D9"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D0" pad="D0"/>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="GND" pad="GND@1"/>
<connect gate="G$1" pin="GND@0" pad="GND@2"/>
<connect gate="G$1" pin="GND@1" pad="GND@3"/>
<connect gate="G$1" pin="GND@2" pad="GND@4"/>
<connect gate="G$1" pin="IOREF" pad="IOREF"/>
<connect gate="G$1" pin="MISO" pad="MISO"/>
<connect gate="G$1" pin="MOSI" pad="MOSI"/>
<connect gate="G$1" pin="SCK" pad="SCK"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEENSY-3.1" prefix="B">
<description>&lt;h3&gt;Teensy 3+ Footprint&lt;/h3&gt;
&lt;p&gt;Mechanical footprint with connectors for Teensy Development Board with ARM Cortex.&lt;/p&gt;

&lt;b&gt;&lt;p&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13736"&gt;Teensy 3.2&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13305"&gt;Teensy LC&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TEENSY-31"/>
</gates>
<devices>
<device name="SILK" package="TEENSY-3.1">
<connects>
<connect gate="G$1" pin="0/RX1" pad="0"/>
<connect gate="G$1" pin="1/TX1" pad="1"/>
<connect gate="G$1" pin="10*/TX2/CS" pad="10"/>
<connect gate="G$1" pin="11/DOUT" pad="11"/>
<connect gate="G$1" pin="12/DIN" pad="12"/>
<connect gate="G$1" pin="13/SCK" pad="13"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3*" pad="3"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="3V" pad="3V"/>
<connect gate="G$1" pin="4*" pad="4"/>
<connect gate="G$1" pin="5*" pad="5"/>
<connect gate="G$1" pin="6*" pad="6"/>
<connect gate="G$1" pin="7/RX3" pad="7"/>
<connect gate="G$1" pin="8/TX3" pad="8"/>
<connect gate="G$1" pin="9*/RX2" pad="9"/>
<connect gate="G$1" pin="A0/14" pad="14"/>
<connect gate="G$1" pin="A1/15" pad="15"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A11" pad="A11"/>
<connect gate="G$1" pin="A14/DAC" pad="A14/DAC"/>
<connect gate="G$1" pin="A2/16" pad="16"/>
<connect gate="G$1" pin="A3/17" pad="17"/>
<connect gate="G$1" pin="A4/18/SDA0" pad="18"/>
<connect gate="G$1" pin="A5/19/SCL0" pad="19"/>
<connect gate="G$1" pin="A6/20*" pad="20"/>
<connect gate="G$1" pin="A7/21*" pad="21"/>
<connect gate="G$1" pin="A8/22*" pad="22"/>
<connect gate="G$1" pin="A9/23*" pad="23"/>
<connect gate="G$1" pin="AGND" pad="AGND"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="PROG" pad="PROG"/>
<connect gate="G$1" pin="VBAT" pad="VBAT"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
<connect gate="G$1" pin="VUSB" pad="VUSB"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="DEV-12646"/>
</technology>
</technologies>
</device>
<device name="NOSILK" package="TEENSY-3.1_NOSILK">
<connects>
<connect gate="G$1" pin="0/RX1" pad="0"/>
<connect gate="G$1" pin="1/TX1" pad="1"/>
<connect gate="G$1" pin="10*/TX2/CS" pad="10"/>
<connect gate="G$1" pin="11/DOUT" pad="11"/>
<connect gate="G$1" pin="12/DIN" pad="12"/>
<connect gate="G$1" pin="13/SCK" pad="13"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3*" pad="3"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="3V" pad="3V"/>
<connect gate="G$1" pin="4*" pad="4"/>
<connect gate="G$1" pin="5*" pad="5"/>
<connect gate="G$1" pin="6*" pad="6"/>
<connect gate="G$1" pin="7/RX3" pad="7"/>
<connect gate="G$1" pin="8/TX3" pad="8"/>
<connect gate="G$1" pin="9*/RX2" pad="9"/>
<connect gate="G$1" pin="A0/14" pad="14"/>
<connect gate="G$1" pin="A1/15" pad="15"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A11" pad="A11"/>
<connect gate="G$1" pin="A14/DAC" pad="A14/DAC"/>
<connect gate="G$1" pin="A2/16" pad="16"/>
<connect gate="G$1" pin="A3/17" pad="17"/>
<connect gate="G$1" pin="A4/18/SDA0" pad="18"/>
<connect gate="G$1" pin="A5/19/SCL0" pad="19"/>
<connect gate="G$1" pin="A6/20*" pad="20"/>
<connect gate="G$1" pin="A7/21*" pad="21"/>
<connect gate="G$1" pin="A8/22*" pad="22"/>
<connect gate="G$1" pin="A9/23*" pad="23"/>
<connect gate="G$1" pin="AGND" pad="AGND"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="PROG" pad="PROG"/>
<connect gate="G$1" pin="VBAT" pad="VBAT"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
<connect gate="G$1" pin="VUSB" pad="VUSB"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="DEV-12646"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARKFUN_EDISON" prefix="B">
<description>&lt;h3&gt;SparkFun Edison &lt;/h3&gt;
&lt;p&gt;The Intel® Edison is an ultra small computing platform that will change the way you look at embedded electronics. Each Edison packs a huge amount of tech goodies into a tiny package while still providing the same robust strength of your go-to single board computer. Powered by the Intel® Atom™ SoC dual-core CPU and including an integrated WiFi, Bluetooth LE, and a 70-pin connector to attach a veritable slew of shield-like “Blocks” which can be stacked on top of each other.&lt;/p&gt;

&lt;p&gt;This device includes footprints for the Edison module itself, as well as the basic board outline used for our Edison blocks.&lt;/p&gt;


&lt;b&gt;&lt;p&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13024&gt;Intel Edison&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13039&gt;SparkFun Console Block&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13038&gt;SparkFun GPIO Block&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13037&gt;SparkFun Battery Block&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13045&gt;SparkFun Base Block&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13033&gt;SparkFun 9DOF Block&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13035&gt;SparkFun OLED Block&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13043&gt;SparkFun Dual H-Bridge Block&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13041&gt;SparkFun microSD Block&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13770&gt;SparkFun ADC Block&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13034&gt;SparkFun I2C Block&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13036&gt;SparkFun Arduino Block&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13727&gt;SparkFun Power Block&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13042&gt;SparkFun PWM Block&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13044&gt;SparkFun Raspberry Pi Block&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13040&gt;SparkFun UART Block&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="_BASIC" symbol="EDISON_CONNECTOR_BASE"/>
<gate name="_GPIO" symbol="EDISON_CONNECTOR_GPIO"/>
<gate name="_I2C_1" symbol="EDISON_CONNECTOR_I2C_1"/>
<gate name="_I2C_6" symbol="EDISON_CONNECTOR_I2C_6"/>
<gate name="_I2S" symbol="EDISON_CONNECTOR_I2S_2"/>
<gate name="_SD" symbol="EDISON_CONNECTOR_SD"/>
<gate name="_SPI" symbol="EDISON_CONNECTOR_SPI_2"/>
<gate name="_UART_1" symbol="EDISON_CONNECTOR_UART_1"/>
<gate name="_UART_2" symbol="EDISON_CONNECTOR_UART_2"/>
<gate name="_USB" symbol="EDISON_CONNECTOR_USB"/>
</gates>
<devices>
<device name="PCB" package="SPARKFUN_EDISON_PCB">
<connects>
<connect gate="_BASIC" pin="1.8V" pad="12"/>
<connect gate="_BASIC" pin="3.3V@1" pad="8"/>
<connect gate="_BASIC" pin="3.3V@2" pad="10"/>
<connect gate="_BASIC" pin="DCIN" pad="14"/>
<connect gate="_BASIC" pin="FW_RCVR" pad="69"/>
<connect gate="_BASIC" pin="GND@1" pad="1"/>
<connect gate="_BASIC" pin="GND@2" pad="5"/>
<connect gate="_BASIC" pin="GND@3" pad="9"/>
<connect gate="_BASIC" pin="GND@4" pad="11"/>
<connect gate="_BASIC" pin="GND@5" pad="13"/>
<connect gate="_BASIC" pin="GND@6" pad="15"/>
<connect gate="_BASIC" pin="MSIC_SLP_CLK" pad="7"/>
<connect gate="_BASIC" pin="OSC_CLK_OUT_0" pad="67"/>
<connect gate="_BASIC" pin="PWRBTN#" pad="17"/>
<connect gate="_BASIC" pin="RCVR_MODE" pad="31"/>
<connect gate="_BASIC" pin="RESET_OUT#" pad="36"/>
<connect gate="_BASIC" pin="VSYS@1" pad="2"/>
<connect gate="_BASIC" pin="VSYS@2" pad="4"/>
<connect gate="_BASIC" pin="VSYS@3" pad="6"/>
<connect gate="_BASIC" pin="V_VAT_BKUP" pad="23"/>
<connect gate="_GPIO" pin="GP12_PWM0" pad="35"/>
<connect gate="_GPIO" pin="GP13_PWM1" pad="33"/>
<connect gate="_GPIO" pin="GP14" pad="48"/>
<connect gate="_GPIO" pin="GP15" pad="42"/>
<connect gate="_GPIO" pin="GP165" pad="25"/>
<connect gate="_GPIO" pin="GP182_PWM2" pad="37"/>
<connect gate="_GPIO" pin="GP183_PWM3" pad="39"/>
<connect gate="_GPIO" pin="GP44" pad="24"/>
<connect gate="_GPIO" pin="GP45" pad="26"/>
<connect gate="_GPIO" pin="GP46" pad="28"/>
<connect gate="_GPIO" pin="GP47" pad="30"/>
<connect gate="_GPIO" pin="GP48" pad="32"/>
<connect gate="_GPIO" pin="GP49" pad="34"/>
<connect gate="_I2C_1" pin="GP19_I2C_1_SCL" pad="41"/>
<connect gate="_I2C_1" pin="GP20_I2C_1_SDA" pad="43"/>
<connect gate="_I2C_6" pin="GP27_I2C_6_SCL" pad="45"/>
<connect gate="_I2C_6" pin="GP28_I2C_6_SDA" pad="47"/>
<connect gate="_I2S" pin="GP40_I2S_2_CLK" pad="52"/>
<connect gate="_I2S" pin="GP41_I2S_2_FS" pad="54"/>
<connect gate="_I2S" pin="GP42_I2S_2_RXD" pad="50"/>
<connect gate="_I2S" pin="GP43_I2S_2_TXD" pad="56"/>
<connect gate="_SD" pin="!GP77_SD_0_CD#" pad="60"/>
<connect gate="_SD" pin="GP78_SD_0_CLK" pad="58"/>
<connect gate="_SD" pin="GP79_SD_0_CMD" pad="62"/>
<connect gate="_SD" pin="GP80_SD_0_DAT0" pad="66"/>
<connect gate="_SD" pin="GP81_SD_0_DAT1" pad="70"/>
<connect gate="_SD" pin="GP82_SD_0_DAT2" pad="64"/>
<connect gate="_SD" pin="GP83_SD_0_DAT3" pad="68"/>
<connect gate="_SD" pin="GP84_SD_0_CLK_FB" pad="44"/>
<connect gate="_SPI" pin="GP109_SPI_2_CLK" pad="55"/>
<connect gate="_SPI" pin="GP110_SPI_2_FS0" pad="53"/>
<connect gate="_SPI" pin="GP111_SPI_2_FS1" pad="51"/>
<connect gate="_SPI" pin="GP114_SPI_2_RXD" pad="59"/>
<connect gate="_SPI" pin="GP115_SPI_2_TXD" pad="57"/>
<connect gate="_UART_1" pin="GP128_UART_1_CTS" pad="65"/>
<connect gate="_UART_1" pin="GP129_UART_1_RTS" pad="63"/>
<connect gate="_UART_1" pin="GP130_UART_1_RX" pad="61"/>
<connect gate="_UART_1" pin="GP131_UART_1_TX" pad="46"/>
<connect gate="_UART_2" pin="GP134_UART_2_RX" pad="22"/>
<connect gate="_UART_2" pin="GP135_UART_2_TX" pad="27"/>
<connect gate="_USB" pin="FAULT" pad="19"/>
<connect gate="_USB" pin="PSW" pad="21"/>
<connect gate="_USB" pin="USB_DN" pad="18"/>
<connect gate="_USB" pin="USB_DP" pad="16"/>
<connect gate="_USB" pin="USB_ID" pad="3"/>
<connect gate="_USB" pin="USB_VBUS" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="SPARKFUN_EDISON_DAUGHTER">
<connects>
<connect gate="_BASIC" pin="1.8V" pad="12"/>
<connect gate="_BASIC" pin="3.3V@1" pad="8"/>
<connect gate="_BASIC" pin="3.3V@2" pad="10"/>
<connect gate="_BASIC" pin="DCIN" pad="14"/>
<connect gate="_BASIC" pin="FW_RCVR" pad="69"/>
<connect gate="_BASIC" pin="GND@1" pad="1"/>
<connect gate="_BASIC" pin="GND@2" pad="5"/>
<connect gate="_BASIC" pin="GND@3" pad="9"/>
<connect gate="_BASIC" pin="GND@4" pad="11"/>
<connect gate="_BASIC" pin="GND@5" pad="13"/>
<connect gate="_BASIC" pin="GND@6" pad="15"/>
<connect gate="_BASIC" pin="MSIC_SLP_CLK" pad="7"/>
<connect gate="_BASIC" pin="OSC_CLK_OUT_0" pad="67"/>
<connect gate="_BASIC" pin="PWRBTN#" pad="17"/>
<connect gate="_BASIC" pin="RCVR_MODE" pad="31"/>
<connect gate="_BASIC" pin="RESET_OUT#" pad="36"/>
<connect gate="_BASIC" pin="VSYS@1" pad="2"/>
<connect gate="_BASIC" pin="VSYS@2" pad="4"/>
<connect gate="_BASIC" pin="VSYS@3" pad="6"/>
<connect gate="_BASIC" pin="V_VAT_BKUP" pad="23"/>
<connect gate="_GPIO" pin="GP12_PWM0" pad="35"/>
<connect gate="_GPIO" pin="GP13_PWM1" pad="33"/>
<connect gate="_GPIO" pin="GP14" pad="48"/>
<connect gate="_GPIO" pin="GP15" pad="42"/>
<connect gate="_GPIO" pin="GP165" pad="25"/>
<connect gate="_GPIO" pin="GP182_PWM2" pad="37"/>
<connect gate="_GPIO" pin="GP183_PWM3" pad="39"/>
<connect gate="_GPIO" pin="GP44" pad="24"/>
<connect gate="_GPIO" pin="GP45" pad="26"/>
<connect gate="_GPIO" pin="GP46" pad="28"/>
<connect gate="_GPIO" pin="GP47" pad="30"/>
<connect gate="_GPIO" pin="GP48" pad="32"/>
<connect gate="_GPIO" pin="GP49" pad="34"/>
<connect gate="_I2C_1" pin="GP19_I2C_1_SCL" pad="41"/>
<connect gate="_I2C_1" pin="GP20_I2C_1_SDA" pad="43"/>
<connect gate="_I2C_6" pin="GP27_I2C_6_SCL" pad="45"/>
<connect gate="_I2C_6" pin="GP28_I2C_6_SDA" pad="47"/>
<connect gate="_I2S" pin="GP40_I2S_2_CLK" pad="52"/>
<connect gate="_I2S" pin="GP41_I2S_2_FS" pad="54"/>
<connect gate="_I2S" pin="GP42_I2S_2_RXD" pad="50"/>
<connect gate="_I2S" pin="GP43_I2S_2_TXD" pad="56"/>
<connect gate="_SD" pin="!GP77_SD_0_CD#" pad="60"/>
<connect gate="_SD" pin="GP78_SD_0_CLK" pad="58"/>
<connect gate="_SD" pin="GP79_SD_0_CMD" pad="62"/>
<connect gate="_SD" pin="GP80_SD_0_DAT0" pad="66"/>
<connect gate="_SD" pin="GP81_SD_0_DAT1" pad="70"/>
<connect gate="_SD" pin="GP82_SD_0_DAT2" pad="64"/>
<connect gate="_SD" pin="GP83_SD_0_DAT3" pad="68"/>
<connect gate="_SD" pin="GP84_SD_0_CLK_FB" pad="44"/>
<connect gate="_SPI" pin="GP109_SPI_2_CLK" pad="55"/>
<connect gate="_SPI" pin="GP110_SPI_2_FS0" pad="53"/>
<connect gate="_SPI" pin="GP111_SPI_2_FS1" pad="51"/>
<connect gate="_SPI" pin="GP114_SPI_2_RXD" pad="59"/>
<connect gate="_SPI" pin="GP115_SPI_2_TXD" pad="57"/>
<connect gate="_UART_1" pin="GP128_UART_1_CTS" pad="65"/>
<connect gate="_UART_1" pin="GP129_UART_1_RTS" pad="63"/>
<connect gate="_UART_1" pin="GP130_UART_1_RX" pad="61"/>
<connect gate="_UART_1" pin="GP131_UART_1_TX" pad="46"/>
<connect gate="_UART_2" pin="GP134_UART_2_RX" pad="22"/>
<connect gate="_UART_2" pin="GP135_UART_2_TX" pad="27"/>
<connect gate="_USB" pin="FAULT" pad="19"/>
<connect gate="_USB" pin="PSW" pad="21"/>
<connect gate="_USB" pin="USB_DN" pad="18"/>
<connect gate="_USB" pin="USB_DP" pad="16"/>
<connect gate="_USB" pin="USB_ID" pad="3"/>
<connect gate="_USB" pin="USB_VBUS" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RGB_LIGHT_SENSOR_ISL29125" prefix="B">
<description>&lt;h3&gt;SparkFun RGB Light Sensor - ISL29125&lt;/h3&gt;
&lt;p&gt;Mechanical footprint with connectors for ISL29125 RGB Light Sensor Breakout.&lt;/p&gt;

&lt;b&gt;&lt;p&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12829"&gt;SparkFun RGB Light Sensor - ISL29125&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RGB_LIGHT_SENSOR_ISL29125"/>
</gates>
<devices>
<device name="" package="ISL29125">
<connects>
<connect gate="G$1" pin="3.3V" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="INT" pad="5"/>
<connect gate="G$1" pin="SCL" pad="4"/>
<connect gate="G$1" pin="SDA" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO_UNO_R3_SHIELD_ICSP" prefix="B">
<description>&lt;h3&gt;Arduino R3 Shield Footprint with ICSP Header&lt;/h3&gt;

Includes pins for  6-pin (2x3) ICSP Header. Compatible with Leonardo boards that require SPI pin connections via this header. 

&lt;p&gt;SparkFun Products:
&lt;ul&gt;&lt;li&gt;&lt;a href=https://www.sparkfun.com/products/13183&gt;CryptoShield&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=https://www.sparkfun.com/products/12761&gt;microSD Shield&lt;/a&gt;
&lt;li&gt;&lt;a href=https://www.sparkfun.com/products/1417&gt;R3 Stackable Headers Kit&lt;/a&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ARDUINO_R3"/>
</gates>
<devices>
<device name="" package="UNO_R3_SHIELD_ICSP">
<connects>
<connect gate="G$1" pin="!RESET!@1" pad="RES"/>
<connect gate="G$1" pin="!RESET!@2" pad="RST_ICSP"/>
<connect gate="G$1" pin="*D10" pad="D10"/>
<connect gate="G$1" pin="*D11" pad="D11"/>
<connect gate="G$1" pin="*D3" pad="D3"/>
<connect gate="G$1" pin="*D5" pad="D5"/>
<connect gate="G$1" pin="*D6" pad="D6"/>
<connect gate="G$1" pin="*D9" pad="D9"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D0" pad="RX"/>
<connect gate="G$1" pin="D1" pad="TX"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="GND" pad="GND_ICSP"/>
<connect gate="G$1" pin="GND@0" pad="GND@0"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="IOREF" pad="IOREF"/>
<connect gate="G$1" pin="MISO" pad="MISO"/>
<connect gate="G$1" pin="MOSI" pad="MOSI"/>
<connect gate="G$1" pin="SCK" pad="SCK"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="VCC" pad="5V_ICSP"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-NO_LABELS" package="UNO_R3_SHIELD_ICSP_NOLABELS">
<connects>
<connect gate="G$1" pin="!RESET!@1" pad="RES"/>
<connect gate="G$1" pin="!RESET!@2" pad="RST_ICSP"/>
<connect gate="G$1" pin="*D10" pad="D10"/>
<connect gate="G$1" pin="*D11" pad="D11"/>
<connect gate="G$1" pin="*D3" pad="D3"/>
<connect gate="G$1" pin="*D5" pad="D5"/>
<connect gate="G$1" pin="*D6" pad="D6"/>
<connect gate="G$1" pin="*D9" pad="D9"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D0" pad="RX"/>
<connect gate="G$1" pin="D1" pad="TX"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="GND" pad="GND_ICSP"/>
<connect gate="G$1" pin="GND@0" pad="GND@0"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="IOREF" pad="IOREF"/>
<connect gate="G$1" pin="MISO" pad="MISO"/>
<connect gate="G$1" pin="MOSI" pad="MOSI"/>
<connect gate="G$1" pin="SCK" pad="SCK"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="VCC" pad="5V_ICSP"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BIG_RED_BOX-PCB" prefix="B">
<description>&lt;h3&gt;Big Red Box - Enclosure Footprint&lt;/h3&gt;

PCB footprint compatbile with Big Red Box Enclosure. 

&lt;p&gt;SparkFun Products:
&lt;ul&gt;&lt;li&gt;&lt;a href=https://www.sparkfun.com/products/11366&gt;Big Red Box - Enclosure&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=https://www.sparkfun.com/products/13899&gt;Stepoko&lt;/a&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BIG_RED_PCB"/>
</gates>
<devices>
<device name="DIMENSION" package="FLANGED_RED_ENCLOSURE-DIMENSION">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="REFERENCE" package="FLANGED_RED_ENCLOSURE-OUTLINE">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARKFUN_ESP8266_THING" prefix="B">
<description>&lt;h3&gt;SparkFun Thing Board&lt;/h3&gt;

&lt;p&gt; The SparkFun ESP8266 Thing is a breakout and development board for the ESP8266 WiFi SoC&lt;/p&gt;

&lt;p&gt;SparkFun Products:
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13231”&gt;SparkFun ESP8266 Thing&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ESP8266_THING"/>
</gates>
<devices>
<device name="" package="SPARKFUN_ESP8266_THING">
<connects>
<connect gate="G$1" pin="0" pad="0"/>
<connect gate="G$1" pin="12/MISO" pad="12"/>
<connect gate="G$1" pin="13/MOSI" pad="13"/>
<connect gate="G$1" pin="3.3V@1" pad="3.3V@1"/>
<connect gate="G$1" pin="3.3V@2" pad="3.3V@2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="ADC/A0" pad="ADC"/>
<connect gate="G$1" pin="DTR" pad="DTR"/>
<connect gate="G$1" pin="EN" pad="EN"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="GND@3" pad="GND@3"/>
<connect gate="G$1" pin="NC" pad="NC"/>
<connect gate="G$1" pin="RXI" pad="RXI"/>
<connect gate="G$1" pin="SCL/14/SCLK" pad="SCL"/>
<connect gate="G$1" pin="SDA/2" pad="SDA"/>
<connect gate="G$1" pin="TXO" pad="TXO"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
<connect gate="G$1" pin="XPD/16" pad="XPD"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="WRL-13231"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARKFUN_ESP8266_THING_DEV" prefix="B">
<description>&lt;h3&gt;SparkFun Thing -Dev Board&lt;/h3&gt;

&lt;p&gt; The SparkFun ESP8266 Thing Dev is a breakout and development board for the ESP8266 WiFi SoC, with an integrated FTDI USB-to-Serial chip.&lt;/p&gt;

&lt;p&gt;SparkFun Products:
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13711”&gt;SparkFun ESP8266 Thing-Dev Board&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ESP8266_THING_DEV"/>
</gates>
<devices>
<device name="" package="SPARKFUN_ESP8266_THING_DEV">
<connects>
<connect gate="G$1" pin="0" pad="0"/>
<connect gate="G$1" pin="12/MISO" pad="12"/>
<connect gate="G$1" pin="13/MOSI" pad="13"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="ADC/A0" pad="ADC"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="GND@3" pad="GND@3"/>
<connect gate="G$1" pin="NC" pad="NC"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="RXI/8" pad="RX"/>
<connect gate="G$1" pin="SCL/14/SCLK" pad="14"/>
<connect gate="G$1" pin="SDA/2" pad="2"/>
<connect gate="G$1" pin="TXO/7" pad="TX"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
<connect gate="G$1" pin="XPD/16" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="WRL-13711"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ELECTRIC_IMP_IMP002" prefix="U">
<description>&lt;h3&gt;Electric Imp Module&lt;/h3&gt;
&lt;p&gt;imp002&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Wireless/WiFi/imp002_specification.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12958"&gt;SparkFun Electric Imp imp002 Breakout&lt;/a&gt; (BOB-12958)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="ELECTRIC_IMP_IMP002"/>
</gates>
<devices>
<device name="" package="ELECTRIC_IMP_IMP002">
<connects>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@13" pad="13"/>
<connect gate="G$1" pin="GND@17" pad="17"/>
<connect gate="G$1" pin="GND@23" pad="23"/>
<connect gate="G$1" pin="GND@24" pad="24"/>
<connect gate="G$1" pin="GND@25" pad="25"/>
<connect gate="G$1" pin="GND@26" pad="26"/>
<connect gate="G$1" pin="GND@27" pad="27"/>
<connect gate="G$1" pin="GND@28" pad="28"/>
<connect gate="G$1" pin="GND@29" pad="29"/>
<connect gate="G$1" pin="GND@30" pad="30"/>
<connect gate="G$1" pin="GND@31" pad="31"/>
<connect gate="G$1" pin="GND@32" pad="32"/>
<connect gate="G$1" pin="GND@35" pad="35"/>
<connect gate="G$1" pin="GND@7" pad="7"/>
<connect gate="G$1" pin="LED_GREEN" pad="3"/>
<connect gate="G$1" pin="LED_RED" pad="4"/>
<connect gate="G$1" pin="OPTO_BIAS" pad="2"/>
<connect gate="G$1" pin="OPTO_IN" pad="6"/>
<connect gate="G$1" pin="PIN_1" pad="15"/>
<connect gate="G$1" pin="PIN_2" pad="16"/>
<connect gate="G$1" pin="PIN_5" pad="19"/>
<connect gate="G$1" pin="PIN_6" pad="20"/>
<connect gate="G$1" pin="PIN_7" pad="21"/>
<connect gate="G$1" pin="PIN_8" pad="22"/>
<connect gate="G$1" pin="PIN_9" pad="14"/>
<connect gate="G$1" pin="PIN_A" pad="8"/>
<connect gate="G$1" pin="PIN_B" pad="9"/>
<connect gate="G$1" pin="PIN_C" pad="10"/>
<connect gate="G$1" pin="PIN_D" pad="11"/>
<connect gate="G$1" pin="PIN_E" pad="12"/>
<connect gate="G$1" pin="POWER_EN" pad="5"/>
<connect gate="G$1" pin="VDD@18" pad="18"/>
<connect gate="G$1" pin="VDD@33" pad="33"/>
<connect gate="G$1" pin="VDDA" pad="34"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-12130"/>
<attribute name="VALUE" value="imp002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MBED_NXP_LPC1768">
<description>&lt;h3&gt;mbed LPC1768 board footprint&lt;/h3&gt;
&lt;h4&gt;Boards using this footprint:&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href=""&gt;mbed - LPC1768 (Cortex-M3)&lt;/a&gt; (DEV-09564)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="MBED_NXP_LPC1768"/>
</gates>
<devices>
<device name="" package="DIL40_0.9">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$10" pad="10"/>
<connect gate="G$1" pin="P$11" pad="11"/>
<connect gate="G$1" pin="P$12" pad="12"/>
<connect gate="G$1" pin="P$13" pad="13"/>
<connect gate="G$1" pin="P$14" pad="14"/>
<connect gate="G$1" pin="P$15" pad="15"/>
<connect gate="G$1" pin="P$16" pad="16"/>
<connect gate="G$1" pin="P$17" pad="17"/>
<connect gate="G$1" pin="P$18" pad="18"/>
<connect gate="G$1" pin="P$19" pad="19"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$20" pad="20"/>
<connect gate="G$1" pin="P$21" pad="21"/>
<connect gate="G$1" pin="P$22" pad="22"/>
<connect gate="G$1" pin="P$23" pad="23"/>
<connect gate="G$1" pin="P$24" pad="24"/>
<connect gate="G$1" pin="P$25" pad="25"/>
<connect gate="G$1" pin="P$26" pad="26"/>
<connect gate="G$1" pin="P$27" pad="27"/>
<connect gate="G$1" pin="P$28" pad="28"/>
<connect gate="G$1" pin="P$29" pad="29"/>
<connect gate="G$1" pin="P$3" pad="3"/>
<connect gate="G$1" pin="P$30" pad="30"/>
<connect gate="G$1" pin="P$31" pad="31"/>
<connect gate="G$1" pin="P$32" pad="32"/>
<connect gate="G$1" pin="P$33" pad="33"/>
<connect gate="G$1" pin="P$34" pad="34"/>
<connect gate="G$1" pin="P$35" pad="35"/>
<connect gate="G$1" pin="P$36" pad="36"/>
<connect gate="G$1" pin="P$37" pad="37"/>
<connect gate="G$1" pin="P$38" pad="38"/>
<connect gate="G$1" pin="P$39" pad="39"/>
<connect gate="G$1" pin="P$4" pad="4"/>
<connect gate="G$1" pin="P$40" pad="40"/>
<connect gate="G$1" pin="P$5" pad="5"/>
<connect gate="G$1" pin="P$6" pad="6"/>
<connect gate="G$1" pin="P$7" pad="7"/>
<connect gate="G$1" pin="P$8" pad="8"/>
<connect gate="G$1" pin="P$9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-12167"/>
<attribute name="VALUE" value="MBED1768"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="QDUINOMINI" prefix="BOARD">
<description>&lt;h3&gt;Qduino Mini Board Outline and Pins&lt;/h3&gt;
&lt;p&gt;Board outline for &lt;a href="https://www.sparkfun.com/products/13614"&gt;SparkFun Qduino Mini&lt;/a&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="QDUINOMINI"/>
</gates>
<devices>
<device name="" package="QDUINO_MINI_V15">
<connects>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="D0" pad="D0"/>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D10" pad="D10"/>
<connect gate="G$1" pin="D11" pad="D11"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D31"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D3" pad="D3"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D5" pad="D5"/>
<connect gate="G$1" pin="D6" pad="D6"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="D9" pad="D9"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="LIPO" pad="LIPO"/>
<connect gate="G$1" pin="MISO" pad="MISO"/>
<connect gate="G$1" pin="MOSI" pad="MOSI"/>
<connect gate="G$1" pin="RST" pad="RST"/>
<connect gate="G$1" pin="SCK" pad="SCK"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
<connect gate="G$1" pin="VUSB" pad="VUSB"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PARTICLE_PHOTON" prefix="JP">
<description>&lt;h3&gt;Particle Photon&lt;/h3&gt;
&lt;p&gt;Footprint of the Particle Photon that is used as a basis for many Photon shields. &lt;/p&gt;
&lt;p&gt;SparkFun Products:
&lt;ul&gt;&lt;li&gt;&lt;a href=https://www.sparkfun.com/products/13764”&gt;Particle Photon&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13598”&gt;SparkFun Photon ProtoShield&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13628"&gt;SparkFun Photon micro OLED Shield&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13629"&gt;SparkFun Photon IMU Shield&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13626"&gt;SparkFun Photon Battery Shield&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="PARTICLE_PHOTON"/>
</gates>
<devices>
<device name="" package="PARTICLE_PHOTON">
<connects>
<connect gate="G$1" pin="!RST!" pad="23"/>
<connect gate="G$1" pin="(JTAG_TCK)D6" pad="19"/>
<connect gate="G$1" pin="(JTAG_TDI)D5" pad="18"/>
<connect gate="G$1" pin="(JTAG_TDO)D4" pad="17"/>
<connect gate="G$1" pin="(JTAG_TMS)D7" pad="20"/>
<connect gate="G$1" pin="(JTAG_TRST)D3" pad="16"/>
<connect gate="G$1" pin="(SCL)D1" pad="14"/>
<connect gate="G$1" pin="(SDA)D0" pad="13"/>
<connect gate="G$1" pin="+3V3" pad="24"/>
<connect gate="G$1" pin="A0" pad="12"/>
<connect gate="G$1" pin="A1" pad="11"/>
<connect gate="G$1" pin="A2(SPI1_SS)" pad="10"/>
<connect gate="G$1" pin="A3(SPI1_SCK)" pad="9"/>
<connect gate="G$1" pin="A4(SPI1_MISO)" pad="8"/>
<connect gate="G$1" pin="A5(SPI1_MOSI)" pad="7"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="DAC" pad="6"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@21" pad="21"/>
<connect gate="G$1" pin="RX" pad="4"/>
<connect gate="G$1" pin="TX" pad="3"/>
<connect gate="G$1" pin="VBAT" pad="22"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="WKP" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TEMPLATE" package="PARTICLE_PHOTON_TEMPLATE">
<connects>
<connect gate="G$1" pin="!RST!" pad="23 RST"/>
<connect gate="G$1" pin="(JTAG_TCK)D6" pad="19 D6"/>
<connect gate="G$1" pin="(JTAG_TDI)D5" pad="18 D5"/>
<connect gate="G$1" pin="(JTAG_TDO)D4" pad="17 D4"/>
<connect gate="G$1" pin="(JTAG_TMS)D7" pad="20 D7"/>
<connect gate="G$1" pin="(JTAG_TRST)D3" pad="16 D3"/>
<connect gate="G$1" pin="(SCL)D1" pad="14 D1"/>
<connect gate="G$1" pin="(SDA)D0" pad="13 D0"/>
<connect gate="G$1" pin="+3V3" pad="3V3 24"/>
<connect gate="G$1" pin="A0" pad="12 A0"/>
<connect gate="G$1" pin="A1" pad="11 A1"/>
<connect gate="G$1" pin="A2(SPI1_SS)" pad="10 A2"/>
<connect gate="G$1" pin="A3(SPI1_SCK)" pad="9 A3"/>
<connect gate="G$1" pin="A4(SPI1_MISO)" pad="8 A4"/>
<connect gate="G$1" pin="A5(SPI1_MOSI)" pad="7 A5"/>
<connect gate="G$1" pin="D2" pad="15 D2"/>
<connect gate="G$1" pin="DAC" pad="6 DAC"/>
<connect gate="G$1" pin="GND@2" pad="2 GND@0"/>
<connect gate="G$1" pin="GND@21" pad="21 GND@2"/>
<connect gate="G$1" pin="RX" pad="4 RX"/>
<connect gate="G$1" pin="TX" pad="3 TX"/>
<connect gate="G$1" pin="VBAT" pad="22 VBAT"/>
<connect gate="G$1" pin="VIN" pad="1 VIN"/>
<connect gate="G$1" pin="WKP" pad="5 WKP"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TEMPLATE_WIDE" package="PARTICLE_PHOTON_TEMPLATE_WIDE">
<connects>
<connect gate="G$1" pin="!RST!" pad="23 RST"/>
<connect gate="G$1" pin="(JTAG_TCK)D6" pad="19 D6"/>
<connect gate="G$1" pin="(JTAG_TDI)D5" pad="18 D5"/>
<connect gate="G$1" pin="(JTAG_TDO)D4" pad="17 D4"/>
<connect gate="G$1" pin="(JTAG_TMS)D7" pad="20 D7"/>
<connect gate="G$1" pin="(JTAG_TRST)D3" pad="16 D3"/>
<connect gate="G$1" pin="(SCL)D1" pad="14 D1"/>
<connect gate="G$1" pin="(SDA)D0" pad="13 D0"/>
<connect gate="G$1" pin="+3V3" pad="3V3 24"/>
<connect gate="G$1" pin="A0" pad="12 A0"/>
<connect gate="G$1" pin="A1" pad="11 A1"/>
<connect gate="G$1" pin="A2(SPI1_SS)" pad="10 A2"/>
<connect gate="G$1" pin="A3(SPI1_SCK)" pad="9 A3"/>
<connect gate="G$1" pin="A4(SPI1_MISO)" pad="8 A4"/>
<connect gate="G$1" pin="A5(SPI1_MOSI)" pad="7 A5"/>
<connect gate="G$1" pin="D2" pad="15 D2"/>
<connect gate="G$1" pin="DAC" pad="6 DAC"/>
<connect gate="G$1" pin="GND@2" pad="2 GND@0"/>
<connect gate="G$1" pin="GND@21" pad="21 GND@2"/>
<connect gate="G$1" pin="RX" pad="4 RX"/>
<connect gate="G$1" pin="TX" pad="3 TX"/>
<connect gate="G$1" pin="VBAT" pad="22 VBAT"/>
<connect gate="G$1" pin="VIN" pad="1 VIN"/>
<connect gate="G$1" pin="WKP" pad="5 WKP"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TEMPLATE_NO_STANDOFF" package="PARTICLE_PHOTON_TEMPLATE_NO_STANDOFF">
<connects>
<connect gate="G$1" pin="!RST!" pad="23 RST"/>
<connect gate="G$1" pin="(JTAG_TCK)D6" pad="19 D6"/>
<connect gate="G$1" pin="(JTAG_TDI)D5" pad="18 D5"/>
<connect gate="G$1" pin="(JTAG_TDO)D4" pad="17 D4"/>
<connect gate="G$1" pin="(JTAG_TMS)D7" pad="20 D7"/>
<connect gate="G$1" pin="(JTAG_TRST)D3" pad="16 D3"/>
<connect gate="G$1" pin="(SCL)D1" pad="14 D1"/>
<connect gate="G$1" pin="(SDA)D0" pad="13 D0"/>
<connect gate="G$1" pin="+3V3" pad="3V3 24"/>
<connect gate="G$1" pin="A0" pad="12 A0"/>
<connect gate="G$1" pin="A1" pad="11 A1"/>
<connect gate="G$1" pin="A2(SPI1_SS)" pad="10 A2"/>
<connect gate="G$1" pin="A3(SPI1_SCK)" pad="9 A3"/>
<connect gate="G$1" pin="A4(SPI1_MISO)" pad="8 A4"/>
<connect gate="G$1" pin="A5(SPI1_MOSI)" pad="7 A5"/>
<connect gate="G$1" pin="D2" pad="15 D2"/>
<connect gate="G$1" pin="DAC" pad="6 DAC"/>
<connect gate="G$1" pin="GND@2" pad="2 GND@0"/>
<connect gate="G$1" pin="GND@21" pad="21 GND@2"/>
<connect gate="G$1" pin="RX" pad="4 RX"/>
<connect gate="G$1" pin="TX" pad="3 TX"/>
<connect gate="G$1" pin="VBAT" pad="22 VBAT"/>
<connect gate="G$1" pin="VIN" pad="1 VIN"/>
<connect gate="G$1" pin="WKP" pad="5 WKP"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARKFUN_MS5803-14BA_BREAKOUT" prefix="B">
<description>&lt;h3&gt;SparkFun MSP5803-14BA Breakout&lt;/h3&gt;
&lt;p&gt;I&lt;sup&gt;2&lt;/sup&gt;C compatible pressure sensor breakout&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12909”&gt;SparkFun MSP5803-14BA Breakout&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SPARKFUN_MS5803-14BA_BREAKOUT"/>
</gates>
<devices>
<device name="" package="SPARKFUN_MS5803-14BA_BREAKOUT">
<connects>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="AD/CS" pad="AD/CS"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="PS" pad="PS"/>
<connect gate="G$1" pin="SCL/SCLK" pad="SCL/SCLK"/>
<connect gate="G$1" pin="SDA/SDI" pad="SDA/SDI"/>
<connect gate="G$1" pin="SDO" pad="SDO"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="SEN-12909"/>
<attribute name="VALUE" value="Pressure Sensor"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARKFUN_NRF52832_BREAKOUT" prefix="B">
<description>&lt;h3&gt;SparkFun nRF52832 Breakout&lt;/h3&gt;
&lt;p&gt;SoC microcontroller with BLE, ANT, Nordic support, and 2.4Ghz multiprotocol radio&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13990”&gt;SparkFun nRF52832 Breakout&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SPARKFUN_NRF52832_BREAKOUT"/>
</gates>
<devices>
<device name="" package="SPARKFUN_NRF52832_BREAKOUT">
<connects>
<connect gate="G$1" pin="!RST" pad="!RST"/>
<connect gate="G$1" pin="00/X1" pad="00/X1"/>
<connect gate="G$1" pin="01/X2" pad="01/X2"/>
<connect gate="G$1" pin="02/A0" pad="02/A0"/>
<connect gate="G$1" pin="03/A1" pad="03/A1"/>
<connect gate="G$1" pin="04/A2" pad="04/A2"/>
<connect gate="G$1" pin="05/A3" pad="05/A3"/>
<connect gate="G$1" pin="08" pad="08"/>
<connect gate="G$1" pin="09" pad="09"/>
<connect gate="G$1" pin="1-NFC" pad="1-NFC"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2-NFC" pad="2-NFC"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26/RX" pad="26/RX"/>
<connect gate="G$1" pin="27/TX" pad="27/TX"/>
<connect gate="G$1" pin="28/A4" pad="28/A4"/>
<connect gate="G$1" pin="29/A5" pad="29/A5"/>
<connect gate="G$1" pin="3.3V" pad="3.3V 3.3V@1"/>
<connect gate="G$1" pin="30/A6" pad="30/A6"/>
<connect gate="G$1" pin="31/A7" pad="31/A7"/>
<connect gate="G$1" pin="GND" pad="GND GND1 GND2"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
<connect gate="G$1" pin="VIN" pad="VIN VIN1"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="WRL-13990"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ESP32_THING" prefix="B">
<description>&lt;h3&gt;SparkFun ESP32 Thing Board&lt;/h3&gt;
&lt;p&gt;Pins, silkscreen, and logos matching the layout of the &lt;a href=https://www.sparkfun.com/products/13907&gt;SparkFun ESP32 Thing&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Dimensions: 2.32" x 1.00"&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ESP32_THING"/>
</gates>
<devices>
<device name="_W_ANT_KEEPOUT" package="ESP32_THING">
<connects>
<connect gate="G$1" pin="!RST!" pad="6"/>
<connect gate="G$1" pin="0" pad="32"/>
<connect gate="G$1" pin="12" pad="8"/>
<connect gate="G$1" pin="13" pad="7"/>
<connect gate="G$1" pin="14" pad="9"/>
<connect gate="G$1" pin="15" pad="30"/>
<connect gate="G$1" pin="16" pad="35"/>
<connect gate="G$1" pin="17" pad="34"/>
<connect gate="G$1" pin="18" pad="28"/>
<connect gate="G$1" pin="19" pad="26"/>
<connect gate="G$1" pin="2" pad="31"/>
<connect gate="G$1" pin="21" pad="22"/>
<connect gate="G$1" pin="22" pad="25"/>
<connect gate="G$1" pin="23" pad="27"/>
<connect gate="G$1" pin="25" pad="12"/>
<connect gate="G$1" pin="26" pad="11"/>
<connect gate="G$1" pin="27" pad="10"/>
<connect gate="G$1" pin="32" pad="16"/>
<connect gate="G$1" pin="33" pad="15"/>
<connect gate="G$1" pin="34" pad="14"/>
<connect gate="G$1" pin="35" pad="13"/>
<connect gate="G$1" pin="36" pad="20"/>
<connect gate="G$1" pin="37" pad="19"/>
<connect gate="G$1" pin="38" pad="18"/>
<connect gate="G$1" pin="39" pad="17"/>
<connect gate="G$1" pin="3V3@36" pad="36"/>
<connect gate="G$1" pin="3V3@5" pad="5"/>
<connect gate="G$1" pin="4" pad="33"/>
<connect gate="G$1" pin="5" pad="29"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@21" pad="21"/>
<connect gate="G$1" pin="GND@37" pad="37"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="GND@40" pad="40"/>
<connect gate="G$1" pin="RX" pad="24"/>
<connect gate="G$1" pin="TX" pad="23"/>
<connect gate="G$1" pin="VBAT@3" pad="3"/>
<connect gate="G$1" pin="VBAT@38" pad="38"/>
<connect gate="G$1" pin="VUSB@2" pad="2"/>
<connect gate="G$1" pin="VUSB@39" pad="39"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="DEV-13907"/>
</technology>
</technologies>
</device>
<device name="_WO_ANT_KEEPOUT" package="ESP32_THING_NO_ANT">
<connects>
<connect gate="G$1" pin="!RST!" pad="6"/>
<connect gate="G$1" pin="0" pad="32"/>
<connect gate="G$1" pin="12" pad="8"/>
<connect gate="G$1" pin="13" pad="7"/>
<connect gate="G$1" pin="14" pad="9"/>
<connect gate="G$1" pin="15" pad="30"/>
<connect gate="G$1" pin="16" pad="35"/>
<connect gate="G$1" pin="17" pad="34"/>
<connect gate="G$1" pin="18" pad="28"/>
<connect gate="G$1" pin="19" pad="26"/>
<connect gate="G$1" pin="2" pad="31"/>
<connect gate="G$1" pin="21" pad="22"/>
<connect gate="G$1" pin="22" pad="25"/>
<connect gate="G$1" pin="23" pad="27"/>
<connect gate="G$1" pin="25" pad="12"/>
<connect gate="G$1" pin="26" pad="11"/>
<connect gate="G$1" pin="27" pad="10"/>
<connect gate="G$1" pin="32" pad="16"/>
<connect gate="G$1" pin="33" pad="15"/>
<connect gate="G$1" pin="34" pad="14"/>
<connect gate="G$1" pin="35" pad="13"/>
<connect gate="G$1" pin="36" pad="20"/>
<connect gate="G$1" pin="37" pad="19"/>
<connect gate="G$1" pin="38" pad="18"/>
<connect gate="G$1" pin="39" pad="17"/>
<connect gate="G$1" pin="3V3@36" pad="36"/>
<connect gate="G$1" pin="3V3@5" pad="5"/>
<connect gate="G$1" pin="4" pad="33"/>
<connect gate="G$1" pin="5" pad="29"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@21" pad="21"/>
<connect gate="G$1" pin="GND@37" pad="37"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="GND@40" pad="40"/>
<connect gate="G$1" pin="RX" pad="24"/>
<connect gate="G$1" pin="TX" pad="23"/>
<connect gate="G$1" pin="VBAT@3" pad="3"/>
<connect gate="G$1" pin="VBAT@38" pad="38"/>
<connect gate="G$1" pin="VUSB@2" pad="2"/>
<connect gate="G$1" pin="VUSB@39" pad="39"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEENSYVIEW" prefix="TV" uservalue="yes">
<gates>
<gate name="G1" symbol="TEENSYVIEW_1"/>
<gate name="G2" symbol="TEENSYVIEW_2"/>
</gates>
<devices>
<device name="" package="TEENSYVIEW">
<connects>
<connect gate="G1" pin="1" pad="1"/>
<connect gate="G1" pin="10" pad="10"/>
<connect gate="G1" pin="11" pad="11"/>
<connect gate="G1" pin="12" pad="12"/>
<connect gate="G1" pin="13" pad="13"/>
<connect gate="G1" pin="14" pad="14"/>
<connect gate="G1" pin="2" pad="2"/>
<connect gate="G1" pin="3" pad="3"/>
<connect gate="G1" pin="4" pad="4"/>
<connect gate="G1" pin="5" pad="5"/>
<connect gate="G1" pin="6" pad="6"/>
<connect gate="G1" pin="7" pad="7"/>
<connect gate="G1" pin="8" pad="8"/>
<connect gate="G1" pin="9" pad="9"/>
<connect gate="G2" pin="1" pad="15"/>
<connect gate="G2" pin="10" pad="24"/>
<connect gate="G2" pin="11" pad="25"/>
<connect gate="G2" pin="12" pad="26"/>
<connect gate="G2" pin="13" pad="27"/>
<connect gate="G2" pin="14" pad="28"/>
<connect gate="G2" pin="2" pad="16"/>
<connect gate="G2" pin="3" pad="17"/>
<connect gate="G2" pin="4" pad="18"/>
<connect gate="G2" pin="5" pad="19"/>
<connect gate="G2" pin="6" pad="20"/>
<connect gate="G2" pin="7" pad="21"/>
<connect gate="G2" pin="8" pad="22"/>
<connect gate="G2" pin="9" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAN485">
<gates>
<gate name="G$1" symbol="CAN485"/>
</gates>
<devices>
<device name="FULL_SOCKET" package="CAN485">
<connects>
<connect gate="G$1" pin="485A" pad="485A"/>
<connect gate="G$1" pin="485B" pad="485B"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="CANHI" pad="CANHI"/>
<connect gate="G$1" pin="CANLO" pad="CANLO"/>
<connect gate="G$1" pin="CTS" pad="CTS"/>
<connect gate="G$1" pin="D10" pad="10"/>
<connect gate="G$1" pin="D2/INT0/SCL" pad="2"/>
<connect gate="G$1" pin="D3/INT1/SDA" pad="3"/>
<connect gate="G$1" pin="D4" pad="4"/>
<connect gate="G$1" pin="D5" pad="5"/>
<connect gate="G$1" pin="D6" pad="6"/>
<connect gate="G$1" pin="D7" pad="7"/>
<connect gate="G$1" pin="D8" pad="8"/>
<connect gate="G$1" pin="D9" pad="9"/>
<connect gate="G$1" pin="DTR" pad="DTR"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="GND3" pad="GND3"/>
<connect gate="G$1" pin="GND4" pad="GND4"/>
<connect gate="G$1" pin="MISO/D12" pad="12"/>
<connect gate="G$1" pin="MOSI/D11" pad="11"/>
<connect gate="G$1" pin="RAW" pad="RAW"/>
<connect gate="G$1" pin="RESET" pad="RST"/>
<connect gate="G$1" pin="RESET1" pad="RST1"/>
<connect gate="G$1" pin="RXI" pad="RXI"/>
<connect gate="G$1" pin="RXI1" pad="RXI1"/>
<connect gate="G$1" pin="SCK/D13" pad="13"/>
<connect gate="G$1" pin="TXO" pad="TXO"/>
<connect gate="G$1" pin="TXO1" pad="TXO1"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
<connect gate="G$1" pin="VCC1" pad="VCC1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAN485_PRO_MINI">
<gates>
<gate name="G$1" symbol="CAN485_PRO_MINI"/>
</gates>
<devices>
<device name="PRO_MINI_COMPATIBLE" package="CAN485_PRO_MINI">
<connects>
<connect gate="G$1" pin="485A" pad="485A"/>
<connect gate="G$1" pin="485B" pad="485B"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4M" pad="A4M"/>
<connect gate="G$1" pin="A5M" pad="A5M"/>
<connect gate="G$1" pin="CANHI" pad="CANHI"/>
<connect gate="G$1" pin="CANLO" pad="CANLO"/>
<connect gate="G$1" pin="CTS" pad="CTS"/>
<connect gate="G$1" pin="D10" pad="10"/>
<connect gate="G$1" pin="D2/INT0/SCL" pad="2"/>
<connect gate="G$1" pin="D3/INT1/SDA" pad="3"/>
<connect gate="G$1" pin="D4" pad="4"/>
<connect gate="G$1" pin="D5" pad="5"/>
<connect gate="G$1" pin="D6" pad="6"/>
<connect gate="G$1" pin="D7" pad="7"/>
<connect gate="G$1" pin="D8" pad="8"/>
<connect gate="G$1" pin="D9" pad="9"/>
<connect gate="G$1" pin="DTR" pad="DTR"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="GND3" pad="GND3"/>
<connect gate="G$1" pin="GND4" pad="GND4"/>
<connect gate="G$1" pin="MISO/D12" pad="12"/>
<connect gate="G$1" pin="MOSI/D11" pad="11"/>
<connect gate="G$1" pin="RAW" pad="RAW"/>
<connect gate="G$1" pin="RESET" pad="RST"/>
<connect gate="G$1" pin="RESET1" pad="RST1"/>
<connect gate="G$1" pin="RXI" pad="RXI"/>
<connect gate="G$1" pin="RXI1" pad="RXI1"/>
<connect gate="G$1" pin="SCK/D13" pad="13"/>
<connect gate="G$1" pin="TXO" pad="TXO"/>
<connect gate="G$1" pin="TXO1" pad="TXO1"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
<connect gate="G$1" pin="VCC1" pad="VCC1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RFM69_BOB">
<gates>
<gate name="G$1" symbol="RFM69_BOB"/>
</gates>
<devices>
<device name="" package="RFM69_BOB">
<connects>
<connect gate="G$1" pin="0" pad="0"/>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="G" pad="G"/>
<connect gate="G$1" pin="G2" pad="G2"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="I" pad="I"/>
<connect gate="G$1" pin="O" pad="O"/>
<connect gate="G$1" pin="R" pad="R"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MICROSD-BREAKOUT" prefix="U">
<gates>
<gate name="G$1" symbol="MICROSD-BREAKOUT"/>
</gates>
<devices>
<device name="" package="MICROSD-BREAKOUT">
<connects>
<connect gate="G$1" pin="CD" pad="CD"/>
<connect gate="G$1" pin="CS" pad="CS"/>
<connect gate="G$1" pin="DI" pad="DI"/>
<connect gate="G$1" pin="DO" pad="DO"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="SCK" pad="SCK"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATLAS_CONDUCTIVITY" prefix="U">
<gates>
<gate name="G$1" symbol="ATLAS_CONDUCTIVITY"/>
</gates>
<devices>
<device name="" package="ATLAS_CONDUCTIVITY">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="PRB@1" pad="PRB@1"/>
<connect gate="G$1" pin="PRB@2" pad="PRB@2"/>
<connect gate="G$1" pin="RX/SCL" pad="RX/SCL"/>
<connect gate="G$1" pin="TX/SDA" pad="TX/SDA"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATLAS_BNC" prefix="U">
<gates>
<gate name="G$1" symbol="ATLAS_BNC"/>
</gates>
<devices>
<device name="" package="ATLAS_BNC">
<connects>
<connect gate="G$1" pin="@NC" pad="NC"/>
<connect gate="G$1" pin="CENTER" pad="CENTER"/>
<connect gate="G$1" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAN485_OUTER_PINS_ONLY">
<gates>
<gate name="G$1" symbol="CAN485_OUTER_ONLY"/>
</gates>
<devices>
<device name="" package="CAN485_OUTER_ONLY">
<connects>
<connect gate="G$1" pin="485A" pad="485A"/>
<connect gate="G$1" pin="485B" pad="485B"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="CANHI" pad="CANHI"/>
<connect gate="G$1" pin="CANLO" pad="CANLO"/>
<connect gate="G$1" pin="CTS" pad="CTS"/>
<connect gate="G$1" pin="D10" pad="10"/>
<connect gate="G$1" pin="D2/INT0/SCL" pad="2"/>
<connect gate="G$1" pin="D3/INT1/SDA" pad="3"/>
<connect gate="G$1" pin="D4" pad="4"/>
<connect gate="G$1" pin="D5" pad="5"/>
<connect gate="G$1" pin="D6" pad="6"/>
<connect gate="G$1" pin="D7" pad="7"/>
<connect gate="G$1" pin="D8" pad="8"/>
<connect gate="G$1" pin="D9" pad="9"/>
<connect gate="G$1" pin="DTR" pad="DTR"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="GND3" pad="GND3"/>
<connect gate="G$1" pin="GND4" pad="GND4"/>
<connect gate="G$1" pin="MISO/D12" pad="12"/>
<connect gate="G$1" pin="MOSI/D11" pad="11"/>
<connect gate="G$1" pin="RAW" pad="RAW"/>
<connect gate="G$1" pin="RESET" pad="RST"/>
<connect gate="G$1" pin="RESET1" pad="RST1"/>
<connect gate="G$1" pin="RXI" pad="RXI"/>
<connect gate="G$1" pin="RXI1" pad="RXI1"/>
<connect gate="G$1" pin="SCK/D13" pad="13"/>
<connect gate="G$1" pin="TXO" pad="TXO"/>
<connect gate="G$1" pin="TXO1" pad="TXO1"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
<connect gate="G$1" pin="VCC1" pad="VCC1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARKFUN_OPTOISOLATOR-BOB">
<gates>
<gate name="G$1" symbol="SPARKFUN_OPTOISOLATOR-BOB"/>
</gates>
<devices>
<device name="" package="SPARKFUN_OPTOISOLATOR-BOB">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="HV" pad="HV"/>
<connect gate="G$1" pin="HVG" pad="HVG"/>
<connect gate="G$1" pin="IN1" pad="IN1"/>
<connect gate="G$1" pin="IN2" pad="IN2"/>
<connect gate="G$1" pin="NC" pad="NC"/>
<connect gate="G$1" pin="OUT1" pad="OUT1"/>
<connect gate="G$1" pin="OUT2" pad="OUT2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
