<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.0">
<drawing>
<library>
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-2.54">
<description>2 PTH spaced 0.1" apart</description>
</package>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="CAP-PTH-LARGE">
</package>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="0402">
<description>&lt;p&gt;&lt;b&gt;Generic 1005 (0402) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="CAP-PTH-5MM">
<description>2 PTH spaced 5mm apart</description>
</package>
<package name="1206">
<description>&lt;p&gt;&lt;b&gt;Generic 3216 (1206) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="CAP-PTH-SMALL-KIT">
<description>&lt;h3&gt;CAP-PTH-SMALL-KIT&lt;/h3&gt;
Commonly used for small ceramic capacitors. Like our 0.1uF (http://www.sparkfun.com/products/8375) or 22pF caps (http://www.sparkfun.com/products/8571).&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.</description>
</package>
<package name="EIA3216">
<description>Generic EIA 3216 (1206) polarized tantalum capacitor</description>
</package>
<package name="EIA3528">
<description>Generic EIA 3528 polarized tantalum capacitor</description>
</package>
<package name="CPOL-RADIAL-2.5MM-6.5MM">
<description>2.5 mm spaced PTHs with 6.5 mm diameter outline</description>
</package>
<package name="CPOL-RADIAL-2.5MM-5MM">
<description>2.5 mm spaced PTHs with 5 mm diameter outline and standard solder mask</description>
</package>
<package name="EIA7343">
<description>EIA 7343 tantalum capacitor</description>
</package>
<package name="PANASONIC_G">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package G&lt;/b&gt;</description>
</package>
<package name="PANASONIC_C">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package E&lt;/b&gt;</description>
</package>
<package name="PANASONIC_D">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package E&lt;/b&gt;</description>
</package>
<package name="CPOL-RADIAL-5MM-10MM">
<description>5 mm spaced PTHs in 10 mm diameter silk ring</description>
</package>
<package name="1007">
<description>&lt;p&gt;&lt;b&gt;Generic 2518 (1007) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="CPOL-RADIAL-2.5MM-5MM-KIT">
<description>2.5 mm spaced PTHs with top copper masked</description>
</package>
<package name="CPOL-RADIAL-5MM-10MM-KIT">
<description>5 mm spaced PTHs, with 10 mm silk ring and no exposed copper on top</description>
</package>
<package name="NIC_10X10.5_CAP">
<description>Some old package in our library</description>
</package>
<package name="0603-POLAR">
<description>&lt;p&gt;&lt;b&gt;Polarized 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="CAP-PTH-10MM">
<description>2 PTH spaced 10mm apart</description>
</package>
<package name="1210">
<description>&lt;p&gt;&lt;b&gt;Generic 3225 (1210) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="EIA6032-NOM">
<description>Metric Size Code EIA 6032-25 Median (Nominal) Land Protrusion&lt;br /&gt;
http://www.kemet.com/Lists/ProductCatalog/Attachments/254/KEM_T2005_T491.pdf</description>
</package>
<package name="CAP-RADIAL-5MM-21.5MM">
<description>&lt;h3&gt;[Radial PTH Capacitor] - [5mm spaced leads, 21.5 mm OD]&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: [2]&lt;/li&gt;
&lt;li&gt;Pin pitch: [5mm]&lt;/li&gt;
&lt;li&gt;Area: [Circle: 21.5mm Outer Diameter]&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=http://www.cooperindustries.com/content/dam/public/bussmann/Electronics/Resources/product-datasheets/Bus_Elx_DS_4327_KR_Series.pdf&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="DSK-RADIAL-4.8MM">
<description>&lt;h3&gt;DSK-621 - 6.8mm Radial package for SuperCapacitor&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 10.15mm&lt;/li&gt;
&lt;li&gt;Area: 6.8mm x 11.7mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=https://media.digikey.com/pdf/Data%20Sheets/Elna%20America%20Inc/DS,DSK.pdf&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="0402-TIGHT">
</package>
<package name="0402_MURATA">
</package>
</packages>
<symbols>
<symbol name="CAP">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="CAP_ADJ">
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="CAP_POL">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="CAP-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="47UF-POLAR" prefix="C">
<description>&lt;h3&gt;47µF polarized capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP_POL"/>
</gates>
<devices>
<device name="-EIA3528-10V-10%" package="EIA3528">
<connects>
<connect gate="G$1" pin="+" pad="A"/>
<connect gate="G$1" pin="-" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08310"/>
<attribute name="VALUE" value="47uF"/>
</technology>
</technologies>
</device>
<device name="-PANASONIC_D-35V-20%" package="PANASONIC_D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08478"/>
<attribute name="VALUE" value="47uF"/>
</technology>
</technologies>
</device>
<device name="-PANASONIC_D-50V-20%" package="PANASONIC_D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="0.22UF" prefix="C">
<description>&lt;h3&gt;0.22µF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0603-25V-10%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-07822"/>
<attribute name="VALUE" value="0.22uF"/>
</technology>
</technologies>
</device>
<device name="-0603-50V-(-20/+80%)" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-09885"/>
<attribute name="VALUE" value="0.22uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1.0PF" prefix="C">
<description>&lt;h3&gt;1pF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0603-50V-25%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-07879"/>
<attribute name="VALUE" value="1.0pF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1.5PF" prefix="C">
<description>&lt;h3&gt;1.5pF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0603-50V-16.667%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08763"/>
<attribute name="VALUE" value="1.5pF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1000UF" prefix="C">
<description>&lt;h3&gt;1,000µF/1mF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;
CAP-08070</description>
<gates>
<gate name="G$1" symbol="CAP_POL"/>
</gates>
<devices>
<device name="-RADIAL-5MM-25V-20%" package="CPOL-RADIAL-5MM-10MM">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-09538"/>
<attribute name="VALUE" value="1mF"/>
</technology>
</technologies>
</device>
<device name="-RADIAL-5MM-35V-20%-KIT" package="CPOL-RADIAL-5MM-10MM-KIT">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-09538"/>
<attribute name="VALUE" value="1mf"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="100PF" prefix="C">
<description>&lt;h3&gt;100pF/0.1nF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0603-50V-5%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-07883"/>
<attribute name="VALUE" value="100pF"/>
</technology>
</technologies>
</device>
<device name="-0402-50V-5%" package="0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-13458"/>
<attribute name="VALUE" value="100PF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="100UF-POLAR" prefix="C">
<description>&lt;h3&gt;100µF polarized capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP_POL"/>
</gates>
<devices>
<device name="-EIA7343-10V-10%(TANT)" package="EIA7343">
<connects>
<connect gate="G$1" pin="+" pad="A"/>
<connect gate="G$1" pin="-" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-07890"/>
<attribute name="VALUE" value="100uF"/>
</technology>
</technologies>
</device>
<device name="-EIA7343-16V-10%(TANT)" package="EIA7343">
<connects>
<connect gate="G$1" pin="+" pad="A"/>
<connect gate="G$1" pin="-" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08702"/>
<attribute name="VALUE" value="100uF"/>
</technology>
</technologies>
</device>
<device name="-RADIAL-2.5MM-25V-20%" package="CPOL-RADIAL-2.5MM-6.5MM">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08439"/>
<attribute name="VALUE" value="100uF"/>
</technology>
</technologies>
</device>
<device name="-10X10.5-63V-20%" package="NIC_10X10.5_CAP">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08362"/>
<attribute name="VALUE" value="100uF"/>
</technology>
</technologies>
</device>
<device name="-25V-20%(ELEC)" package="PANASONIC_D">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-12547"/>
<attribute name="VALUE" value="100uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="10NF" prefix="C">
<description>&lt;h3&gt;0.01uF/10nF/10,000pF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;

CAP-09321</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-PTH-10MM-10000V-1-%" package="CAP-PTH-10MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-09321"/>
<attribute name="VALUE" value="10nF"/>
</technology>
</technologies>
</device>
<device name="-0603-50V-10%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-00867"/>
<attribute name="VALUE" value="10nF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="10UF-POLAR" prefix="C">
<description>&lt;h3&gt;10.0µF polarized capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP_POL"/>
</gates>
<devices>
<device name="-EIA3216-16V-10%(TANT)" package="EIA3216">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-00811"/>
<attribute name="VALUE" value="10uF"/>
</technology>
</technologies>
</device>
<device name="-0603-6.3V-20%(TANT)" package="0603-POLAR">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-13210"/>
<attribute name="VALUE" value="10uF"/>
</technology>
</technologies>
</device>
<device name="-EIA3528-20V-10%(TANT)" package="EIA3528">
<connects>
<connect gate="G$1" pin="+" pad="A"/>
<connect gate="G$1" pin="-" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08063"/>
<attribute name="VALUE" value="10uF"/>
</technology>
</technologies>
</device>
<device name="-RADIAL-2.5MM-25V-20%" package="CPOL-RADIAL-2.5MM-5MM">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08440"/>
<attribute name="VALUE" value="10uF"/>
</technology>
</technologies>
</device>
<device name="-RADIAL-2.5MM-KIT-25V-20%" package="CPOL-RADIAL-2.5MM-5MM-KIT">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08440"/>
<attribute name="VALUE" value="10uF"/>
</technology>
</technologies>
</device>
<device name="-EIA6032-25V-10%" package="EIA6032-NOM">
<connects>
<connect gate="G$1" pin="+" pad="A"/>
<connect gate="G$1" pin="-" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-12984"/>
<attribute name="VALUE" value="10µF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="10UF" prefix="C">
<description>&lt;h3&gt;10.0µF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0603-6.3V-20%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-11015"/>
<attribute name="VALUE" value="10uF"/>
</technology>
</technologies>
</device>
<device name="-1206-6.3V-20%" package="1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-10057"/>
<attribute name="VALUE" value="10uF"/>
</technology>
</technologies>
</device>
<device name="-0805-10V-10%" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-11330"/>
<attribute name="VALUE" value="10uF"/>
</technology>
</technologies>
</device>
<device name="-1210-50V-20%" package="1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-09824"/>
<attribute name="VALUE" value="10uF"/>
</technology>
</technologies>
</device>
<device name="-0805-25V-10%" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-14259"/>
<attribute name="VALUE" value="10uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="12PF" prefix="C" uservalue="yes">
<description>&lt;h3&gt;12pF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0603-50V-5%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-09137"/>
<attribute name="VALUE" value="12pF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="18PF" prefix="C">
<description>&lt;h3&gt;18pF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0603-50V-5%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08267"/>
<attribute name="VALUE" value="18pF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1.0NF/1000PF" prefix="C" uservalue="yes">
<description>&lt;h3&gt;1nF/1,000pF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0603-50V-10%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-07886"/>
<attribute name="VALUE" value="1nF"/>
</technology>
</technologies>
</device>
<device name="-0402_TIGHT-50V-10%" package="0402-TIGHT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-14280"/>
<attribute name="VALUE" value="1.0nF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2.2NF/2200PF" prefix="C">
<description>&lt;h3&gt;2.2nF/2,200pF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0603-50V-10%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-07877"/>
<attribute name="VALUE" value="2.2nF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2.2UF" prefix="C">
<description>&lt;h3&gt;2.2µF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0603-10V-20%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-07888"/>
<attribute name="VALUE" value="2.2uF"/>
</technology>
</technologies>
</device>
<device name="-0805-25V-(+80/-20%)" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-11624"/>
<attribute name="VALUE" value="2.2uF"/>
</technology>
</technologies>
</device>
<device name="-1206-50V-10%" package="1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-10009"/>
<attribute name="VALUE" value="2.2uF"/>
</technology>
</technologies>
</device>
<device name="-0402_TIGHT-10V-10%-X5R" package="0402-TIGHT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-14232"/>
<attribute name="VALUE" value="2.2uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="22NF/22,000PF" prefix="C">
<description>&lt;h3&gt;0.022uF/22nF/22,000pF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0603-50V-10%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-07885"/>
<attribute name="VALUE" value="22nF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="22PF" prefix="C">
<description>&lt;h3&gt;22pF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0603-50V-5%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-07876"/>
<attribute name="VALUE" value="22pF"/>
</technology>
</technologies>
</device>
<device name="-PTH-2.54MM-200V-5%" package="CAP-PTH-2.54">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-09128"/>
<attribute name="VALUE" value="22pF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="22UF" prefix="C">
<description>&lt;h3&gt;22µF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0805-6.3V-20%" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08402"/>
<attribute name="VALUE" value="22uF"/>
</technology>
</technologies>
</device>
<device name="-1210-16V-20%" package="1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0805-16V-20%" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-14260"/>
<attribute name="VALUE" value="22uF"/>
</technology>
</technologies>
</device>
<device name="-0603-6.3V-20%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-14464"/>
<attribute name="VALUE" value="22uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="27PF" prefix="C">
<description>&lt;h3&gt;27pF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0603-50V-5%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-09989"/>
<attribute name="VALUE" value="27pF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="3.3NF" prefix="C">
<description>&lt;h3&gt;3.3nF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0603-100V-10%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-09633"/>
<attribute name="VALUE" value="3.3nF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="33NF" prefix="C">
<description>&lt;h3&gt;33nF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0603-50V-10%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-07887"/>
<attribute name="VALUE" value="33nF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="33PF" prefix="C">
<description>&lt;h3&gt;33pF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0603-50V-5%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-10142"/>
<attribute name="VALUE" value="33pF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="390NF" prefix="C">
<description>&lt;h3&gt;0.39uF/390nF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0603-10V-10%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-10986"/>
<attribute name="VALUE" value="390nF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="4.7PF" prefix="C">
<description>&lt;h3&gt;4.7pF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0603-50V-5%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-07880"/>
<attribute name="VALUE" value="4.7pF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="4.7UF" prefix="C">
<description>&lt;h3&gt;4.7µF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0603-6.3V-(10%)" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08280"/>
<attribute name="VALUE" value="4.7uF"/>
</technology>
</technologies>
</device>
<device name="-1206-16V-(+80/-20%)" package="1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-10300"/>
<attribute name="VALUE" value="4.7uF"/>
</technology>
</technologies>
</device>
<device name="-0603-35V-(20%)" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-14106"/>
<attribute name="VALUE" value="4.7uF"/>
</technology>
</technologies>
</device>
<device name="-0402_TIGHT-6.3V-20%-X5R" package="0402-TIGHT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-14240"/>
<attribute name="VALUE" value="4.7uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="470NF" prefix="C">
<description>&lt;h3&gt;0.47uF/470nF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0402-16V-10%" package="0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-09041"/>
<attribute name="VALUE" value="470nF"/>
</technology>
</technologies>
</device>
<device name="-0603-10V-10%-X5R" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-13216"/>
<attribute name="VALUE" value="470nF"/>
</technology>
</technologies>
</device>
<device name="-0402_TIGHT-6.3V-10%-X5R" package="0402-TIGHT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-14242"/>
<attribute name="VALUE" value="0.47uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="470PF" prefix="C">
<description>&lt;h3&gt;470pF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0603-50V-5%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-07884"/>
<attribute name="VALUE" value="470pF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="47NF" prefix="C" uservalue="yes">
<description>&lt;h3&gt;47nF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0603-25V-5%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08605"/>
<attribute name="VALUE" value="47nF"/>
</technology>
</technologies>
</device>
<device name="-0402_TIGHT-25V-10%-X7R" package="0402-TIGHT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-14243"/>
<attribute name="VALUE" value="47nF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="47PF" prefix="C">
<description>&lt;h3&gt;47pF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0603-50V-5%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08913"/>
<attribute name="VALUE" value="47pF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="560PF" prefix="C">
<description>&lt;h3&gt;0.56nF/560pF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0603-50V-5%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08749"/>
<attribute name="VALUE" value="560pF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="560UF" prefix="C">
<description>&lt;h3&gt;560µF polarized capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP_POL"/>
</gates>
<devices>
<device name="-PANASONIC_G-25V-20%" package="PANASONIC_G">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-09983"/>
<attribute name="VALUE" value="560uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="680PF" prefix="C">
<description>&lt;h3&gt;680pF/0.68nF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0603-50V-10%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-09232"/>
<attribute name="VALUE" value="680pF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="68UF-POLAR" prefix="C">
<description>&lt;h3&gt;68µF polarized capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP_POL"/>
</gates>
<devices>
<device name="-EIA3528-10V-10%(TANT)" package="EIA3528">
<connects>
<connect gate="G$1" pin="+" pad="A"/>
<connect gate="G$1" pin="-" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-10790"/>
<attribute name="VALUE" value="68uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="9.0PF" prefix="C">
<description>&lt;h3&gt;9.0pF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0603-50V-10%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-09341"/>
<attribute name="VALUE" value="9.0pF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="10PF" prefix="C">
<description>&lt;h3&gt;10pF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0603-50V-5%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-11812"/>
<attribute name="VALUE" value="10pF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="0.18UF" prefix="C">
<description>&lt;h3&gt;0.18µF ceramic capacitor&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0603-10V-10%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-12380"/>
<attribute name="VALUE" value="0.18uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="15PF" prefix="C">
<description>&lt;h3&gt;15pF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0402-50V-5%" package="0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-13063"/>
<attribute name="VALUE" value="15pF"/>
</technology>
</technologies>
</device>
<device name="-0603-50V-5%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-07881"/>
<attribute name="VALUE" value="15pF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1.0UF" prefix="C">
<description>&lt;h3&gt;1µF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0603-16V-10%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-00868"/>
<attribute name="VALUE" value="1.0uF"/>
</technology>
</technologies>
</device>
<device name="-0402-16V-10%" package="0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-12417"/>
<attribute name="VALUE" value="1.0uF"/>
</technology>
</technologies>
</device>
<device name="-0805-25V-(+80/-20%)" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-11625"/>
<attribute name="VALUE" value="1.0uF"/>
</technology>
</technologies>
</device>
<device name="-1206-50V-10%" package="1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-09822"/>
<attribute name="VALUE" value="1.0uF"/>
</technology>
</technologies>
</device>
<device name="-0805-25V-10%" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08064"/>
<attribute name="VALUE" value="1.0uF"/>
</technology>
</technologies>
</device>
<device name="-0603-16V-10%-X7R" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-13930"/>
<attribute name="VALUE" value="1.0uF"/>
</technology>
</technologies>
</device>
<device name="-0402T-16V-10%" package="0402-TIGHT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-12417"/>
<attribute name="VALUE" value="1.0uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="0.1UF" prefix="C">
<description>&lt;h3&gt;0.1µF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0402-16V-10%" package="0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-12416"/>
<attribute name="VALUE" value="0.1uF"/>
</technology>
</technologies>
</device>
<device name="-0603-25V-(+80/-20%)" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="VALUE" value="0.1uF"/>
</technology>
</technologies>
</device>
<device name="-0603-25V-5%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="VALUE" value="0.1uF"/>
</technology>
</technologies>
</device>
<device name="-KIT-EZ-50V-20%" package="CAP-PTH-SMALL-KIT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08370"/>
<attribute name="VALUE" value="0.1uF"/>
</technology>
</technologies>
</device>
<device name="-0603-100V-10%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08390"/>
<attribute name="VALUE" value="0.1uF"/>
</technology>
</technologies>
</device>
<device name="-0402T-16V-10%" package="0402-TIGHT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-12416"/>
<attribute name="VALUE" value="0.1uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="22UF-POLAR" prefix="C">
<description>&lt;h3&gt;22µF polarized capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP_POL"/>
</gates>
<devices>
<device name="-PANASONIC_C-35V-20%" package="PANASONIC_C">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08618"/>
<attribute name="VALUE" value="22uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="0.33UF/330NF" prefix="C">
<description>&lt;h3&gt;0.33µF/330nF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0805-50V-10%" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08469"/>
<attribute name="VALUE" value="0.33µF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="0.8PF" prefix="C">
<description>&lt;h3&gt;0.8pF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0402-50V-0.1PF" package="0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-13456"/>
<attribute name="VALUE" value="0.8pF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="3.0NF" prefix="C">
<description>&lt;h3&gt;3.0nF (3nF, 3000pF) ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP-1"/>
</gates>
<devices>
<device name="-0603-50V-5%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-13515"/>
<attribute name="VALUE" value="3.0nF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6PF" prefix="C">
<description>&lt;h3&gt;6pF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0402-50V-0.5%" package="0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-13455"/>
<attribute name="VALUE" value="6pF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="5.6PF" prefix="C">
<description>&lt;h3&gt;5.6pF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0603-50V-5%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-12456"/>
<attribute name="VALUE" value="5.6PF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="180PF" prefix="C">
<description>&lt;h3&gt;180pF/0.18nF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0603-50V-5%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-11661"/>
<attribute name="VALUE" value="180pF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="270PF" prefix="C">
<description>&lt;h3&gt;270pF/0.27nF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0603-50V-5%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-13339"/>
<attribute name="VALUE" value="270PF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1F-EDLC" prefix="C">
<description>&lt;h3&gt;[Eaton] [KR-5R5C105-R] - [1F Electric Double Layer Capacitor (SuperCapacitor)]&lt;/h3&gt;
&lt;p&gt;This is a 21.5mm OD 1F SuperCapacitor.&lt;/p&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP_POL"/>
</gates>
<devices>
<device name="" package="CAP-RADIAL-5MM-21.5MM">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-13904"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name=".22F-SUPERCAP" prefix="C">
<description>&lt;h3&gt;ELNA DSK-621 - 220mF Electric Double Layer Capacitor (EDLC/SuperCapacitor)&lt;/h3&gt;
&lt;p&gt;A 220 mF SuperCapacitor. Used for backup power on devices with low standby current&lt;/p&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP_POL"/>
</gates>
<devices>
<device name="" package="DSK-RADIAL-4.8MM">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-13907"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="4.7UF-POLAR" prefix="C">
<gates>
<gate name="G$1" symbol="CAP_POL"/>
</gates>
<devices>
<device name="-EIA3528-35V-10%(TANT)" package="EIA3528">
<connects>
<connect gate="G$1" pin="+" pad="A"/>
<connect gate="G$1" pin="-" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-13916"/>
<attribute name="VALUE" value="4.7uF 35V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="47UF">
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-13854"/>
<attribute name="VALUE" value="47uF/6.3V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="330PF" prefix="C">
<description>&lt;h3&gt;330pF/0.33nF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0603-50V-5%" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-10108"/>
<attribute name="VALUE" value="330pF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="0.5PF" prefix="C">
<description>&lt;h3&gt;0.5pF ceramic capacitors&lt;/h3&gt;
&lt;p&gt;A capacitor is a passive two-terminal electrical component used to store electrical energy temporarily in an electric field.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0402_TIGHT-20V-PM0.05PF-NP0" package="0402-TIGHT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-14231"/>
<attribute name="VALUE" value="0.5pF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="5.0PF">
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0402" package="0402_MURATA">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-14350"/>
<attribute name="VALUE" value="5.0 pF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2.4PF">
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="-0402" package="0402_MURATA">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-14351"/>
<attribute name="VALUE" value="2.4 pF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
