<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.2">
<drawing>
<library>
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06-SMD_RA_MALE">
<description>&lt;h3&gt;SMD - 6 Pin Right Angle Male Header&lt;/h3&gt;
tDocu layer shows pin locations.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X06">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="MOLEX_1X6_RA_LOCK">
<description>&lt;h3&gt;Molex 6-Pin Plated Through-Hole Right Angle Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center to hold pins in place during soldering.  
tPlace shows location of connector.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/2pin_molex_set_19iv10.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X06_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin with Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X06_LOCK">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin with Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center, locking pins in place during soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X06-KIT">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin KIT&lt;/h3&gt;
&lt;p&gt;This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. 
&lt;br&gt;This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="ATX24_RIGHT_ANGLE">
<description>&lt;h3&gt;Molex Mini-Fit Jr. - 24 pin, Right Angle&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:24&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Connectors/ATX-RA.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;ATX24&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="AUDIO-JACK">
<description>&lt;h3&gt;3.5mm Stereo Audio Jack&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Audio-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Audio_Jack&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="STEREOJACK2.5MM_STEREOJACK2.5MM">
<description>&lt;h3&gt;2.5mm Stereo Audio Jack - PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/19726.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Audio_Jack_2.5MM&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="STEREOJACK2.5MM_SPECIAL_POGOPINS">
<description>&lt;h3&gt;2.5mm Stereo Audio Jack - PTH Pogo Pin Compatible&lt;/h3&gt;
Long pads to enable testing with pogo pins.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/19726.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Audio_Jack_2.5MM&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="STEREOJACK2.5MM_SPECIAL_HOLES-ONLY">
<description>&lt;h3&gt;2.5mm Stereo Audio Jack - PTH Holes Only&lt;/h3&gt;
No electrical connections. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/19726.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Audio_Jack_2.5MM&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="AUDIO-JACK-3.5MM-SMD">
<description>&lt;h3&gt;3.5mm Stereo Audio Jack - Surface Mount&lt;/h3&gt;
2.5mm Height. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/19269.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Audio_Jack&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X3">
<description>&lt;h3&gt;Plated Through Hole - 2x3&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X3-NS">
<description>&lt;h3&gt;Plated Through Hole - 2x3 No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X3_OFFSET">
<description>&lt;h3&gt;Plated Through Hole - 2x3 Long Pads w/ Offset Holes&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X3_LOCK">
<description>&lt;h3&gt;Plated Through Hole - 2x3 Locking Footprint&lt;/h3&gt;
Holes are offset from center 0.005", to hold pins in place while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X5">
<description>&lt;h3&gt;Plated Through Hole - 2x5&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X3-SHROUDED">
<description>&lt;h3&gt;Plated Through Hole - 2x3 Shrouded Header&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Shrouded-10pin.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X5-SHROUDED">
<description>&lt;h3&gt;Plated Through Hole - 2x5 Shrouded Header&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Shrouded-10pin.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X5-SHROUDED_LOCK">
<description>&lt;h3&gt;Plated Through Hole - 2x5 Shrouded Header Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center, to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Shrouded-10pin.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X5-SHROUDED_SMD">
<description>&lt;h3&gt;Surface Mount - 2x5 Shrouded Header&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Shrouded-10pin.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="BANANA_CONN">
<description>&lt;h3&gt;Banana Plug PTH&lt;/h3&gt;
0.2" diameter pad, 0.1" hole. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 1&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;BANANA_CONN&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="BC9VPC">
<description>&lt;h3&gt;9V Battery Holder (Open) - PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Area: 2.15"x1.20"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.memoryprotectiondevices.com/datasheets/BC9VPC-datasheet.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;BC9VPC&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="BNC">
<description>&lt;h3&gt;BNC Jack - Mouser Part#5227161 &lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 4&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.mouser.com/ds/2/418/NG_CS_1307191_BNC_Connectors_0307-561881.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;BNC&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="DB9">
<description>&lt;h3&gt;9 Pin Serial Connector - Female PCB Mount Right Angle&lt;/h3&gt;
0.318" style. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:11&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Connectors/DB9-PCB.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;DB9&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="DB9_MALE">
<description>&lt;h3&gt;9 Pin Serial Connector - Male PCB Mount Right Angle&lt;/h3&gt;
0.318" style. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:11&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/15944.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;DB9&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="DIN7">
<description>&lt;h3&gt;miniDIN Right Angle&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:7&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/mdn-s-07-x-mkt.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;DIN7&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="DS_TOUCH_CONNECTOR">
<description>&lt;h3&gt;4-pin DS touch screen connector&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/LCD/PSPTouchConnector.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;DS_TOUCH_CONNECTOR&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="EB-85A">
<description>&lt;h3&gt;EB-85A Connector&lt;/h3&gt;
Horizontal surface mount connector for the EB-85A/FV-M8 GPS receiver.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 10&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/GPS/EB-85A-Connector.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;EB-85A&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="FTDI_BASIC">
<description>&lt;h3&gt;FTDI Basic &lt;/h3&gt;
Includes tDocu labels for end pins that match the FTDI Basic connection.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 6&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;6_Pin_Serial_Cable&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X01_LONGPAD">
<description>&lt;h3&gt;Plated Through Hole - Long Pad&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:1&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X01">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:1&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X01_2MM">
<description>&lt;h3&gt;Plated Through Hole - 2mm&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:1&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X01_OFFSET">
<description>&lt;h3&gt;Plated Through Hole - Long Pad w/ Offset Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:1&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X01_POGOPIN_HOLE_0.061_DIA">
<description>&lt;h3&gt;Pogo Pin - 0.061"&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:1&lt;/li&gt;
&lt;li&gt;Pin pitch:0.061"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X01_POGOPIN_HOLE_0.58_DIA">
<description>&lt;h3&gt;Pogo Pin Hole - 0.58" &lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:1&lt;/li&gt;
&lt;li&gt;Pin pitch:0.58"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SNAP-FEMALE">
<description>&lt;h3&gt;Sew-On Fabric Snap - Female&lt;/h3&gt;
Equivalent to size #1/0 snap. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 1&lt;/li&gt;
&lt;li&gt;Area:8mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SNAP-MALE">
<description>&lt;h3&gt;Sew-On Fabric Snap - Male&lt;/h3&gt;
Equivalent to size #1/0 snap. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 1&lt;/li&gt;
&lt;li&gt;Area:8mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="MOLEX-1X2">
<description>&lt;h3&gt;Molex 2-Pin Plated Through-Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/2pin_molex_set_19iv10.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SCREWTERMINAL-3.5MM-2">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch - 2 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="JST-2-SMD">
<description>&lt;h3&gt;JST-Right Angle Male Header SMT&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/20404.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;li&gt;JST_2MM_MALE&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02_BIG">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.15"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="JST-2-SMD-VERT">
<description>&lt;h3&gt;JST-Vertical Male Header SMT &lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/20404.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SCREWTERMINAL-5MM-2">
<description>&lt;h3&gt;Screw Terminal  5mm Pitch -2 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 5mm/197mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02_LOCK">
<description>&lt;h3&gt;Plated Through Hole - Locking Footprint&lt;/h3&gt;
Holes are staggered by 0.005" from center to hold pins while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="MOLEX-1X2_LOCK">
<description>&lt;h3&gt;Molex 2-Pin Plated Through-Hole Locking Footprint&lt;/h3&gt;
Holes are offset from center by 0.005" to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/2pin_molex_set_19iv10.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02_LOCK_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - Long Pads with Locking Footprint&lt;/h3&gt;
Pins are staggered by 0.005" from center to hold pins in place while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SCREWTERMINAL-3.5MM-2_LOCK">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch - 2 Pin PTH Locking&lt;/h3&gt;
Holes are offset from center 0.005" to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - Long Pads without Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="JST-2-PTH">
<description>&lt;h3&gt;JST 2 Pin Right Angle Plated Through  Hole&lt;/h3&gt;
tDocu indicate polarity for connections that match SparkFun LiPo battery terminations. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch:2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Connectors/JST%282%29-01548.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02_XTRA_BIG">
<description>&lt;h3&gt;Plated Through Hole - 0.1" holes&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.2"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02_PP_HOLES_ONLY">
<description>&lt;h3&gt;Pogo Pins Connector - No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SCREWTERMINAL-3.5MM-2-NS">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch - 2 Pin PTH No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="JST-2-PTH-NS">
<description>&lt;h3&gt;JST 2 Pin Right Angle Plated Through  Hole- No Silk&lt;/h3&gt;
tDocu indicate polarity for connections that match SparkFun LiPo battery terminations. 
&lt;br&gt; No silk outline of connector. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch:2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Connectors/JST%282%29-01548.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="JST-2-PTH-KIT">
<description>&lt;h3&gt;JST 2 Pin Right Angle Plated Through  Hole - KIT&lt;/h3&gt;
tDocu indicate polarity for connections that match SparkFun LiPo battery terminations. 
&lt;br&gt; This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad.
&lt;br&gt; This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch:2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Connectors/JST%282%29-01548.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SPRINGTERMINAL-2.54MM-2">
<description>&lt;h3&gt;Spring Terminal- PCB Mount 2 Pin PTH&lt;/h3&gt;
tDocu marks the spring arms
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 4&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/SpringTerminal.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="MOLEX-1X3">
<description>&lt;h3&gt;PTH - 3 Pin Vertical Molex Polarized Header&lt;/h3&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt;&lt;a href="http://www.4uconnector.com/online/object/4udrawing/01932.pdf"&gt; 4UCONN part # 01932 &lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SCREWTERMINAL-3.5MM-3">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch -3 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 3&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03_LOCK">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin Locking Footprint&lt;/h3&gt;
Pins are staggered 0.005" off center to lock pins while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03_LOCK_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin Long Pad w/ Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center to lock pins in place while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="MOLEX-1X3_LOCK">
<description>&lt;h3&gt;PTH - 3 Pin Vertical Molex Polarized Header&lt;/h3&gt;
Pins are offset 0.005" from center to lock pins in place during soldering. 
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt;&lt;a href="http://www.4uconnector.com/online/object/4udrawing/01932.pdf"&gt; 4UCONN part # 01932 &lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SCREWTERMINAL-3.5MM-3_LOCK.007S">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch -3 Pin PTH Locking&lt;/h3&gt;
Holes are offset 0.007" from center to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 3&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="JST-3-PTH">
<description>&lt;h3&gt;JST 3 Pin Right Angle Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/ePH.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03_PP_HOLES_ONLY">
<description>&lt;h3&gt;Pogo Pins - 3 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SCREWTERMINAL-5MM-3">
<description>&lt;h3&gt;Screw Terminal  5mm Pitch -3 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 3&lt;/li&gt;
&lt;li&gt;Pin pitch: 5mm/197mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03_LOCK_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin Locking Footprint w/out Silk Outline&lt;/h3&gt;
Holes are offset from center 0.005" to lock pins in place while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="JST-3-SMD">
<description>&lt;h3&gt;JST 3 Pin Right Angle SMT&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03-1MM-RA">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin SMD&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X04">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="MOLEX-1X4">
<description>&lt;h3&gt;Molex 4-Pin Plated Through-Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/2pin_molex_set_19iv10.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SCREWTERMINAL-3.5MM-4">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch -4 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 4&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X04_1.27MM">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch: 1.27mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X04_LOCK">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin Locking Footprint&lt;/h3&gt;
Pins are offset 0.005" from center to lock pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X04_LOCK_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin Long Pads w/ Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center to lock pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="MOLEX-1X4_LOCK">
<description>&lt;h3&gt;Molex 4-Pin Plated Through-Hole Locking&lt;/h3&gt;
Holes are offset 0.005" from center to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/2pin_molex_set_19iv10.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X04_SMD_RA_MALE">
<description>&lt;h3&gt;SMD - 4 Pin Right Angle Male Header&lt;/h3&gt;
tDocu layer shows pin locations.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X04_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X04_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="JST-4-PTH">
<description>&lt;h3&gt;JST Right Angle 4 Pin Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 4&lt;/li&gt;
&lt;li&gt;Pin pitch: 2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/ePH.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SCREWTERMINAL-3.5MM-4_LOCK">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch -4 Pin PTH Locking&lt;/h3&gt;
Holes are offset 0.005" from center to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 4&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="JST04_1MM_RA">
<description>&lt;h3&gt;SMD- 4 Pin Right Angle &lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X4">
<description>&lt;h3&gt;Plated Through Hole - 2x4&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X05">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X05_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X05_1.27MM">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch: 1.27mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X05_LOCK">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin with Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center, locking pins in place during soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X05_LOCK_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin Long Pad with Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center, locking pins in place during soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X05_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X05_1MM">
<description>&lt;h3&gt;SMD - 5 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.sparkfun.com/datasheets/GPS/EM408-SMDConnector.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;li&gt;EM-408&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X05_1MM_RA">
<description>&lt;h3&gt;SMD - 5 Pin Right Angle&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X5-RA">
<description>&lt;h3&gt;Plated Through Hole - 2x5 Right Angle Male Headers&lt;/h3&gt;
tDocu shows pin location. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X5-RAF">
<description>&lt;h3&gt;Plated Through Hole - 2x5 Right Angle Female Header&lt;/h3&gt;
Silk outline of pins
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="MOLEX-1X6">
<description>&lt;h3&gt;Molex 6-Pin Plated Through-Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/2pin_molex_set_19iv10.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="MOLEX-1X6-RA">
<description>&lt;h3&gt;Molex 6-Pin Plated Through-Hole Right Angle&lt;/h3&gt;
tPlace shows angle of connector. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/2pin_molex_set_19iv10.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X06_LOCK_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin with Locking Footprint with Long Pads&lt;/h3&gt;
Holes are offset 0.005" from center, locking pins in place during soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="MOLEX-1X6_LOCK">
<description>&lt;h3&gt;Molex 6-Pin Plated Through-Hole Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center to hold pins in place during soldering.  
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/2pin_molex_set_19iv10.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X06_FEMALE_LOCK.010">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin Locking Header&lt;/h3&gt;
Includes silk outline for 6 pin female header
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://cdn.sparkfun.com/datasheets/Prototyping/SP-140520-XX-001.pdf”&gt;Datasheet referenced for footprint:&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SCREWTERMINAL-3.5MM-6">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch -6 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 6&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X06-SMD-FEMALE">
<description>&lt;h3&gt;Header - 6 pin Female SMD&lt;/h3&gt;
Right angle 0.1"
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Prototyping/19686.pdf”&gt;Datasheet referenced for footprint:&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X06_HOLES_ONLY">
<description>&lt;h3&gt; 6 Pin Holes&lt;/h3&gt;
No silk, no plating
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X06_SMD_STRAIGHT">
<description>&lt;h3&gt; 6 Pin SMD Female Header&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Prototyping/femaleSMDheader.pdf”&gt;Datasheet referenced for footprint:&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X06_SMD_STRAIGHT_ALT">
<description>&lt;h3&gt; 6 Pin SMD Female Header&lt;/h3&gt;
Alternate pin configuration
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Prototyping/femaleSMDheader.pdf”&gt;Datasheet referenced for footprint:&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X06_SMD_STRAIGHT_COMBO">
<description>&lt;h3&gt; 6 Pin SMD Female Header - Combined Footprint&lt;/h3&gt;

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Prototyping/femaleSMDheader.pdf”&gt;Datasheet referenced for footprint:&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X07">
<description>&lt;h3&gt;Plated Through Hole -7 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:7&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_07&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X07_LOCK">
<description>&lt;h3&gt;Plated Through Hole -7 Pin Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center, locking pins in place during soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:7&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_07&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X07_LOCK_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole -7 Pin Locking Footprint w/ Long Pads&lt;/h3&gt;
Holes are offset 0.005" from center, locking pins in place during soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:7&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_07&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X07_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole -7 Pin  Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:7&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_07&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X07_HOLES_ONLY">
<description>&lt;h3&gt; 7 Pin Holes&lt;/h3&gt;
No plating, no silk outline.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:7&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_07&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X08">
<description>&lt;h3&gt;Plated Through Hole -8 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X08_LOCK">
<description>&lt;h3&gt;Plated Through Hole -8 Pin Locking Footprint&lt;/h3&gt;
Holes are offset 0.005", to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X08_LOCK_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole -8 Pin Locking Footprint with Long Pads&lt;/h3&gt;
Holes are offset 0.005", to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X08_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole -8 Pin Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SCREWTERMINAL-3.5MM-8">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch -8 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 8&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X08_SMD">
<description>&lt;h3&gt;SMD -8 Pin Vertical Female&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Prototyping/femaleSMDheader.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X08_SMD_ALT">
<description>&lt;h3&gt;SMD -8 Pin Vertical Female&lt;/h3&gt;
Alternate pin configuration
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Prototyping/femaleSMDheader.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X08_SMD_COMBINED">
<description>&lt;h3&gt;SMD -8 Pin Vertical Female&lt;/h3&gt;
Combined footprint configuration
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Prototyping/femaleSMDheader.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="BM08B-SRSS-TB">
<description>&lt;h3&gt;JST Vertical Crimp Connect&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 8&lt;/li&gt;
&lt;li&gt;Pin pitch:1mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.jst-mfg.com/product/pdf/eng/eSR.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X8">
<description>&lt;h3&gt;Plated Through Hole - 2x8&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:16&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X09">
<description>&lt;h3&gt;Plated Through Hole -9 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:9&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_09&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X09_LOCK">
<description>&lt;h3&gt;Plated Through Hole -9 Pin Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" to lock pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:9&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_09&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X09_LOCK_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole -9 Pin Locking Footprint w/ Long Pads&lt;/h3&gt;
Holes are offset 0.005" to lock pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:9&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_09&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X09_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole -9 Pin Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:9&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_09&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X10">
<description>&lt;h3&gt;Plated Through Hole -10 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_10&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X10-2MM">
<description>&lt;h3&gt;Plated Through Hole -10 Pin 2mm&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/XBee-Connector.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_10&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X10-2MM-SMD">
<description>&lt;h3&gt;Plated Through Hole -10 Pin 2mm SMD&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Sockets/xbeeheadersmd.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_10&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X10_LOCK">
<description>&lt;h3&gt;Plated Through Hole -10 Pin Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" to hold pins in place while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_10&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X10_LOCK_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole -10 Pin Locking Footprint with Long Pads&lt;/h3&gt;
Holes are offset 0.005" to hold pins in place while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_10&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X10">
<description>&lt;h3&gt;Plated Through Hole - 2x10&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:20&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_10x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X10_LOCK">
<description>&lt;h3&gt;Plated Through Hole - 2x10 Locking Footprint&lt;/h3&gt;
Holes are offset 0.005", to hold pins in place while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:20&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_10x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X10_LOCK_SPECIAL">
<description>&lt;h3&gt;Plated Through Hole - 2x10 Locking Footprint Special&lt;/h3&gt;
Holes are offset 0.005", to hold pins in place while soldering. 
Pin rows are offset 5mm as well
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:20&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_10x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X10_NOSILK">
<description>&lt;h3&gt;Plated Through Hole - 2x10 No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:20&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_10x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X11">
<description>&lt;h3&gt;Plated Through Hole -11 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:11&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_11&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X11-1.27MM">
<description>&lt;h3&gt;Plated Through Hole -11 Pin 1.27mm&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:11&lt;/li&gt;
&lt;li&gt;Pin pitch:1.27mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_11&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X11_LOCK">
<description>&lt;h3&gt;Plated Through Hole -11 Pin Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" to hold pins in place while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:11&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_11&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X11_LOCK_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole -11 Pin Locking Footprint w/ Long Pads&lt;/h3&gt;
Holes are offset 0.005" to hold pins in place while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:11&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_11&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X11_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole -11 Pin w/ Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:11&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_11&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X11_HOLES_ONLY">
<description>&lt;h3&gt;11 pin holes&lt;/h3&gt;
No plating, no silk
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:11&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_11&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X12">
<description>&lt;h3&gt;Plated Through Hole -12 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:12&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_12&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X12_LOCK">
<description>&lt;h3&gt;Plated Through Hole -12 Pin Locking Footprint&lt;/h3&gt;
Holes are offset 0.005", to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:12&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_12&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X12_LOCK_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole -12 Pin Locking Footprint with Long Pads&lt;/h3&gt;
Holes are offset 0.005", to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:12&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_12&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X12_MACHINE-PIN-HEADER_LOCK.004">
<description>&lt;h3&gt;Plated Through Hole -12 Pin Machine Pin Headers&lt;/h3&gt;
Holes are offset 0.005", to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:12&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_12&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X12_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole -12 Pin Long Pads&lt;/h3&gt;
Holes are offset 0.005", to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:12&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_12&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X12_HOLES_ONLY">
<description>&lt;h3&gt;Holes -12 Pin&lt;/h3&gt;
No plating, no silk
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:12&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_12&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X13">
<description>&lt;h3&gt;Plated Through Hole -13 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:13&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_13&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X13-LONGPADS">
<description>&lt;h3&gt;Plated Through Hole -13 Pin Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:13&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_13&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X14">
<description>&lt;h3&gt;Plated Through Hole -14 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:14&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_14&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X14_LOCK">
<description>&lt;h3&gt;Plated Through Hole -14 Pin Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" to hold pins in place while soldering
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:14&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_14&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X14_LOCK_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole -14 Pin Locking Footprint w/ Long Pads&lt;/h3&gt;
Holes are offset 0.005" to hold pins in place during soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:14&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_14&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X14-LONGPADS">
<description>&lt;h3&gt;Plated Through Hole -14 Pin Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:14&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_14&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X15">
<description>&lt;h3&gt;Plated Through Hole -15 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:15&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_15&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X15_LOCK">
<description>&lt;h3&gt;Plated Through Hole -15 Pin Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" to hold pins in place while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:15&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_15&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X15_LOCK_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole -15 Pin Locking Footprint with Long Pads&lt;/h3&gt;
Holes are offset 0.005" to hold pins in place while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:15&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_15&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X16">
<description>&lt;h3&gt;Plated Through Hole -16 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:16&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_16&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X16_LOCK">
<description>&lt;h3&gt;Plated Through Hole -16 Pin Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" to hold pins in place while soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:16&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_16&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X16_LOCK_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole -16 Pin Locking Footprint w/ Long Pads&lt;/h3&gt;
Holes are offset 0.005" to hold pins in place while soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:16&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_16&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X16_MACHINE-PIN-HEADER_LOCK.004">
<description>&lt;h3&gt;Plated Through Hole -16 Pin Machine Pin Header Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" to hold pins in place while soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:16&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_16&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X16_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole -16 Pin Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:16&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_16&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X17">
<description>&lt;h3&gt;Plated Through Hole -17 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:17&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_17&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X18">
<description>&lt;h3&gt;Plated Through Hole -18 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:18&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_18&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X19">
<description>&lt;h3&gt;Plated Through Hole -19 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:19&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_19&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X20">
<description>&lt;h3&gt;Plated Through Hole -20 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:20&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_20&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X20_LOCK">
<description>&lt;h3&gt;Plated Through Hole -20 Pin Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center to hold pins in place while soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:20&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_20&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X20_LOCK_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole -20 Pin Locking Footprint Long Pads&lt;/h3&gt;
Holes are offset 0.005" from center to hold pins in place while soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:20&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_20&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X20_LOCK_SPECIAL">
<description>&lt;h3&gt;Plated Through Hole -20 Pin Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center to hold pins in place while soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:20&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_20&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X24">
<description>&lt;h3&gt;Plated Through Hole -24 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:24&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_24&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X24_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole -24 Pin Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:24&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_24&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X25">
<description>&lt;h3&gt;Plated Through Hole -25&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:25&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_25&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X25_LOCK">
<description>&lt;h3&gt;Plated Through Hole -25 pin Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center, to hold pins in place while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:25&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_25&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X25_LOCK_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole -25 pin Locking Footprint w/ Long Pads&lt;/h3&gt;
Holes are offset 0.005" from center, to hold pins in place while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:25&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_25&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X25_LONGPAD">
<description>&lt;h3&gt;Plated Through Hole -25 pin Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:25&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_25&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X27">
<description>&lt;h3&gt;Plated Through Hole -27 Pins&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:27&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_27&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X29">
<description>&lt;h3&gt;Plated Through Hole -29 Pins&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:29&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_29&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X29_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole -29 Pins No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:29&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_29&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X30">
<description>&lt;h3&gt;Plated Through Hole -30 Pins&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:30&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_30&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X30_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole -30 Pins No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:30&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_30&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X40_OFFSET">
<description>&lt;h3&gt;Plated Through Hole -40 Pins Offset&lt;/h3&gt;
Long Pads + offset holes
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:40&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_40&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X40">
<description>&lt;h3&gt;Plated Through Hole -40 Pins&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:40&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_40&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="MAGJACK">
<description>&lt;h3&gt;RJ45 Ethernet MagJack-Compatible&lt;/h3&gt;
tDocu shows where the cable plugs in
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 14&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/MagJack.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;MAGJACK&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="MAGJACK-POE">
<description>&lt;h3&gt;RJ45 PoE MagJack&lt;/h3&gt;
This RJ-45 jack with magnetics, gives you access to the unused twisted pair (10BASE-T, and 100BASE-T) which usually carries power in a power-over-ethernet system.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;MAGJACK-POE&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="OBDII">
<description>&lt;h3&gt;OBD-II Automotive Connector&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 16&lt;/li&gt;
&lt;li&gt;Pin pitch:0.15"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;OBD-II&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="PIC_ICSP_MINI_5_PIN">
<description>&lt;h3&gt;Mini ICSP Connector - 5 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch: 1.5mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.jst-mfg.com/product/pdf/eng/eZH.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;PIC_ICSP_MINI_5_PIN&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X12">
<description>&lt;h3&gt;Plated Through Hole - 2x12&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:24&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_12x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X26">
<description>&lt;h3&gt;Plated Through Hole - 2x26&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:52&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_26x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="POWER_JACK_SMD">
<description>&lt;h3&gt;DC Barrel Power Jack/Connector -SMD&lt;/h3&gt;
5.5mm jack, 2.1mm center pole diameter. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Prototyping/ADC-H-028-1.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;POWER_JACK&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="POWER_JACK_SLOT">
<description>&lt;h3&gt;DC Barrel Power Jack/Connector PTH Slot Pads&lt;/h3&gt;
Extended soldering pads. 
5.5mm jack, 2.1mm center pole diameter
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 3&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Barrel-Connector-PJ-202A.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;POWER_JACK&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="POWER_JACK_PTH">
<description>&lt;h3&gt;DC Barrel Power Jack/Connector PTH&lt;/h3&gt;
5.5mm jack, 2.1mm center pole diameter
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 3&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Barrel-Connector-PJ-202A.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;POWER_JACK&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="POWER_JACK_COMBO">
</package>
<package name="POWER_JACK_PTH_LOCK">
<description>&lt;h3&gt;DC Barrel Power Jack/Connector PTH Locking Footprint&lt;/h3&gt;
5.5mm jack, 2.1mm center pole diameter.
&lt;br&gt; Holes are offset from center 0.005" to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 3&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Barrel-Connector-PJ-202A.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;POWER_JACK&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="PSP_CONNECTOR">
<description>&lt;h3&gt;ZIF PSP Connector&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 42 &lt;/li&gt;
&lt;li&gt;Pin pitch:0.5mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/LCD/PSP-Connector.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;PSP_CONNECTOR&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="PSP_TOUCH_CONNECTOR">
<description>&lt;h3&gt;SMD PSP Touch Screen Connector&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 4&lt;/li&gt;
&lt;li&gt;Pin pitch: 1mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/LCD/PSPTouchConnector.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;PSP_TOUCH_CONNECTOR&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="RJ11-6">
<description>&lt;h3&gt;RJ11 6-Pin Socket with PCB Mounting Post&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 6&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Connectors/RJ11-Datasheet.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;RJ11-6&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="RJ45-8">
<description>&lt;h3&gt;RJ45 Socket with PCB Mounting Posts&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://cdn.sparkfun.com/datasheets/Prototyping/04908.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;RJ45-8&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SCREENKEY_MATING_CONNECTOR">
<description>&lt;h3&gt;FPC/FFC Locking Connector - SMD&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:14&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.5mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Connectors/PRT-09586-e58605370.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;SCREENKEY_CONNECTOR&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SIMHOLDER">
<description>&lt;h3&gt;SIM Card Socket SMT&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 6&lt;/li&gt;
&lt;li&gt;Pin pitch:2.54mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.morethanall.com/upload/products_pdf/144626051352e1f8ebd5c5c.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;SIMHOLDER&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="U.FL">
<description>&lt;h3&gt;U.FL SMD Antenna Connector&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;li&gt;Area: 3.0mm x 2.5mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Wireless/Antennas/RF-001001.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;U.FL&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="USB-A-H">
<description>&lt;h3&gt;USB Type 'A' Male Connector - PTH&lt;/h3&gt;
Shield pins may be grounded.
&lt;br&gt; tDocu shows plug end. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/10016.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;USB_A&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="USB-B-PTH">
<description>&lt;h3&gt;USB Type B Female PTH Mounted&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4 main, 2 shield&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/USB-B%20Connector.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;USB_B&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="USB-MINIB">
<description>&lt;h3&gt;USB Type Mini-B Surface Mounted&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 5 main, 4 shield pins&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/miniUSB-Dimensional.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;

&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;USB_Mini-B&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="USB-A-S-NOSILK-FEMALE">
<description>&lt;h3&gt;USB Type 'A' Female Connector - SMT No Silk&lt;/h3&gt;
Shield pins may be grounded.
&lt;br&gt; tDocu shows plug end. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=” https://www.sparkfun.com/datasheets/Prototyping/Connectors/USBFemaleTypeA.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;USB_A&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="USB-A-S-SILK-FEMALE">
<description>&lt;h3&gt;USB Type 'A' Female Connector - SMT Silk Outline&lt;/h3&gt;
Shield pins may be grounded.
&lt;br&gt; tDocu shows plug end. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=” https://www.sparkfun.com/datasheets/Prototyping/Connectors/USBFemaleTypeA.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;USB_A&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="USB-MICROB">
<description>&lt;h3&gt;USB Type microUSB Connector-No Bossed Pins&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5 pins, 4 shield connections&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;USB_Micro-B&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="USB_MICROB_VERTICAL">
<description>&lt;h3&gt;USB Micro-B Plug Connector&lt;/h3&gt;
Manufacturer part #: ZX80-B-5SA&lt;br&gt;
Manufacturer: Hirose&lt;br&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 5 main, 4 shield&lt;/li&gt;
&lt;p&gt;&lt;a href=”https://www.hirose.com/product/en/download_file/key_name/ZX/category/Catalog/doc_file_id/31704/?file_category_id=4&amp;item_id=13&amp;is_series=1”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;USB_Micro-B&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="MICRO-SD-SOCKET">
<description>&lt;h3&gt;microSD Socket SMD&lt;/h3&gt;
Puhs-Push type.
&lt;br&gt; tDocu shows location of uSD card in different positions.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:12&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/15882.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;MICRO-SD_CARD_SOCKET&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="DIL28-3-ZIF_SOCKET">
<description>&lt;h3&gt;ZIF Socket 28-Pin 0.3"&lt;/h3&gt;
tDocu shows location of lever when unlocked. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:28&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;ZIF_SOCKET_28-3&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="RCA">
<description>&lt;h3&gt;RCA Jack - Plated Through-Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Connectors/RCA-Jack.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;RCA&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="RCA_LOCK">
<description>&lt;h3&gt;RCA Jack - Plated Through-Hole Locking&lt;/h3&gt;
Holes are offset from center 0.005" to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Connectors/RCA-Jack.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;RCA&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X16_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole -16 Pin No Silk&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:16&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_16&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X19_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole -19 Pin No Silk&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:19&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_19&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X11_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole -11 Pin No Silk&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:11&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_11&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="6_PIN_SERIAL_TARGET_SIDE_W_SILK">
<description>&lt;h3&gt;6 pin Serial Target - Right Angle  SMT with Silk&lt;/h3&gt;
Package for devices meant to mate to an FTDI connector.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;6_Pin_Serial_Target&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="3.81MM_TERMINAL_BLOCK_FEMALE_LOCKING">
<description>&lt;h3&gt;MyDAQ Female Right Angle Terminal Block w/ Locking Footprint&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 40&lt;/li&gt;
&lt;li&gt;Pin pitch:3.18mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/10458.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;MyDAQ&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X04_SMD_VERTICAL_COMBO">
<description>&lt;h3&gt;SMD - 4 Pin Vertical Connector&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;SMD Pad count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="AUDIO_JACK_3.5MM_TRRS_SMD_RA">
<description>&lt;h3&gt;TRRS 3.5MM Right Angle Stereo Jack - SMT&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 4&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Prototyping/20153.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;AUDIO_JACK_TRRS&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03_SMD_RA_FEMALE">
<description>&lt;h3&gt;SMD - 3 Pin Right Angle Female Header&lt;/h3&gt;
Silk outline of pin location
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03_SMD_RA_MALE">
<description>&lt;h3&gt;SMD- 3 Pin Right Angle Male Headers&lt;/h3&gt;
No silk outline, but tDocu layer shows pin location. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X3_SMT_POSTS">
<description>&lt;h3&gt;Surface Mount - 2x3 Male Header with Keying Posts&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/15881.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X13">
</package>
<package name="USB-A-SMT-MALE">
<description>&lt;h3&gt;USB Type 'A' Male Connector - SMT&lt;/h3&gt;
Shield pins may be grounded.
&lt;br&gt; tDocu shows plug end. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=” http://www.molex.com/pdm_docs/sd/480371000_sd.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;USB_A&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X3_POGO">
<description>&lt;h3&gt;Plated Through Hole - 2x3 Pogo Pins&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X5_NOSILK">
<description>&lt;h3&gt;Plated Through Hole - 2x5 No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SPRING-CONNECTOR">
<description>&lt;h3&gt;Spring Connector&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 1&lt;/li&gt;
&lt;li&gt;Area:0.25"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02_2.54_SCREWTERM">
<description>&lt;h3&gt;2 Pin Screw Terminal - 2.54mm&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="BTA">
<description>&lt;h3&gt;British Telecom Connector - Analog Right Angle&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 6&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Prototyping/BTA-Connector%20Datasheet.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;VERNIER_ANALOG&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="BTD">
<description>&lt;h3&gt;British Telecom Connector - Right Angle Female Digital&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 6&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=””&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;VERNIER_DIGITAL&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X06_SMD_MALE">
<description>&lt;h3&gt; 6 Pin SMD Male Header&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Prototyping/maleSMDheader.pdf”&gt;Datasheet referenced for footprint:&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X10_SMD_MALE">
<description>&lt;h3&gt;SMD -10 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Prototyping/maleSMDheader.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_10&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X08_SMD_MALE">
<description>&lt;h3&gt;SMD -8 Pin Vertical Male&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Prototyping/maleSMDheader.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X10_SMD_COMBINED">
<description>&lt;h3&gt;SMD -10 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Prototyping/maleSMDheader.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_10&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03_SMD_RA_MALE_POST">
<description>&lt;h3&gt;SMD - 3 Pin Right Angle Male Header w/ Alignment Posts&lt;/h3&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt;&lt;a href="http://www.4uconnector.com/online/object/4udrawing/11026.pdf"&gt; 4UCONN part # 11026 &lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="USB-AB-MICRO-SMD">
<description>&lt;h3&gt;USB Type AB - SMT&lt;/h3&gt;
&lt;br&gt; Basic silk outline&lt;/br&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5 main, 3 shield&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint: http://www.morethanall.com//upload/products_pdf/87340574052ba5151280ca.pdf&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;USB AB&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X06-1MM">
<description>&lt;h3&gt;JST SH Vertical  6-Pin Connector -SMD&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:1mm&lt;/li&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="https://www.sparkfun.com/datasheets/GPS/EM406-SMDConnector-eSH.pdf"&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;li&gt;EM-406&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="USB-B-MICRO-SMD">
<description>&lt;h3&gt;USB - microB SMD&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Micro-USB.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;USB_MICRO-B&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X01NS_KIT">
<description>&lt;h3&gt;Plated Through Hole - No Silk Outline Kit Version&lt;/h3&gt;
&lt;p&gt; Mask on only one side to make soldering in kits easier.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:1&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="AUDIO-JACK-KIT">
<description>&lt;h3&gt;3.5mm Stereo Audio Jack -Kit Version&lt;/h3&gt;
Reduced openings in tStop, pins spread a tiny bit out to hold part on PCB during assembly
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Audio-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Audio_Jack&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X04_SMD_LONG">
<description>&lt;h3&gt;SMD - 4 Pin w/ Long Solder Pads&lt;/h3&gt;
No silk, but tDocu layer shows pin position. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="POWER_JACK_SMD_OVERPASTE_TOE">
<description>&lt;h3&gt;DC Barrel Power Jack/Connector -SMD Overpaste&lt;/h3&gt;
Over paste toe on each SMD pad to ease use of AOI. 
5.5mm jack, 2.1mm center pole diameter. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Prototyping/ADC-H-028-1.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;POWER_JACK&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X24_LOCK">
<description>&lt;h3&gt;Plated Through Hole -24 Pin Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center, to hold pins in place while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:24&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_24&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X11_NO_SILK_KIT">
<description>&lt;h3&gt;Plated Through Hole -11 Pin No Silk  Kit&lt;/h3&gt;
tMask is only on one layer. Designed for kits to prevent soldering on the wrong side. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:11&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_11&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="JST-6-SMD-VERT-1.0MM">
<description>&lt;h3&gt;JST SH Vertical 6-Pin SMT&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch: 1 mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/GPS/EM406-SMDConnector-eSH.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;JST_6PIN_VERTICAL&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X3_SMD">
<description>&lt;h3&gt;Surface Mount - 2x3&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:2.54mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="POWER_JACK_PTH_BREAD">
<description>&lt;h3&gt;DC Barrel Power Jack/Connector Breadboard Compatible&lt;/h3&gt;
Breadboard-friendly pins. 
5.5mm jack, 2.1mm center pole diameter
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 3&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Prototyping/18742.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;POWER_JACK&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X08_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole -8 Pin No Silk&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X10_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole -10 Pin No Silk&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_10&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X23">
<description>&lt;h3&gt;Plated Through Hole -23 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:23&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_23&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X23_LOCK">
<description>&lt;h3&gt;Plated Through Hole -23 Pin Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center, to hold pins in place while soldering
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:23&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_23&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X23_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole -23 Pin Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:23&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_23&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="JST-3-PTH-VERT">
<description>&lt;h3&gt;JST 3 Pin Vertical Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/ePH.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="JST-4-PTH-VERT">
<description>&lt;h3&gt;JST Vertical 4 Pin Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 4&lt;/li&gt;
&lt;li&gt;Pin pitch: 2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.jst-mfg.com/product/pdf/eng/ePH.pdf"&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="STEREOJACK2.5MM">
<description>&lt;h3&gt;2.5mm Stereo Audio Jack - SMT&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/19726.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Audio_Jack_2.5MM&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X12_NO_SILK_KIT">
<description>&lt;h3&gt;Plated Through Hole -12 Pin No Silk Kit&lt;/h3&gt;
Mask on one side only for soldering kits. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:12&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_12&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X06_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="BC9VPC_KIT">
<description>&lt;h3&gt;9V Battery Holder (Open) - PTH KIT&lt;/h3&gt;
Mask on one side for Kit soldering
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Area: 2.15"x1.20"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.memoryprotectiondevices.com/datasheets/BC9VPC-datasheet.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;BC9VPC&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SD">
<description>&lt;h3&gt;SD/MMC Socket&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:13&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://cdn.sparkfun.com/datasheets/Prototyping/19608.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;SD_CARD_SOCKET&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X3_TEST_POINTS">
<description>&lt;h3&gt;Plated Through Hole - 2x3 Test Point Header&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03_SMD_RA_MALE_POST_SMALLER">
<description>&lt;h3&gt;SMD - 3 Pin Right Angle Male Header w/ Alignment Posts&lt;/h3&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt;&lt;a href="http://www.4uconnector.com/online/object/4udrawing/11026.pdf"&gt; 4UCONN part # 11026 &lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03_SMD_RA_MALE_POST_SMALLEST">
</package>
<package name="1X13_LOCK">
<description>&lt;h3&gt;Plated Through Hole -13 Pin Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" to hold pins in place while soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:13&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_13&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="BINDING_POST">
<description>&lt;h3&gt;Insulated Binding Post&lt;/h3&gt;
Banana-jack compatible post
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;BINDING_POST&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X04_SMD_RA_FEMALE">
<description>&lt;h3&gt;SMD - 4 Pin Right-Angle Female Header&lt;/h3&gt;
Silk outline shows header location. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X17_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole -17 Pin No Silk&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:17&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_17&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X17_NO_SILK_KIT">
<description>&lt;h3&gt;Plated Through Hole -17 Pin No Silk Kit&lt;/h3&gt;
Mask on only one side for soldering kits. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:17&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_17&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="JST-5-PTH">
<description>&lt;h3&gt;JST 5 Pin Right Angle Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 5&lt;/li&gt;
&lt;li&gt;Pin pitch: 2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/ePH.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="JST-5-PTH-VERT">
<description>&lt;h3&gt;JST 5 Pin Vertical Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 5&lt;/li&gt;
&lt;li&gt;Pin pitch: 2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X12_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole -12 Pin No Silk&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:12&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_12&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X6_SMD">
<description>&lt;h3&gt;Surface Mount - 2x6&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:12&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X5_PTH_SILK_.05">
<description>&lt;h3&gt;Plated Through Hole - 2x5&lt;/h3&gt;
Holes are 0.05". 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X6">
<description>&lt;h3&gt;Plated Through Hole - 2x6&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:12&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X13_LOCK_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole -13 Pin Locking Footprint No Silk Outline&lt;/h3&gt;
Holes are offset 0.005" to hold pins in place while soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:13&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_13&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X15_LOCK_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole -15 Pin Locking Footprint No Silk Outline&lt;/h3&gt;
Holes are offset 0.005" to hold pins in place while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:15&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_15&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X08_LOCK_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole -8 Pin Locking Footprint No Silk&lt;/h3&gt;
Holes are offset 0.005", to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X09_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole -9 Pin No Silk&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:9&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_09&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X20_SHROUDED">
<description>&lt;h3&gt;Plated Through Hole - 2x20 Shrouded Header&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:40&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://cdn.sparkfun.com/datasheets/Dev/RaspberryPi/B-D-xx1X.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_20x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X20_NOSILK">
<description>&lt;h3&gt;Plated Through Hole - 2x20 No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:40&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_20x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X20">
<description>&lt;h3&gt;Plated Through Hole - 2x20&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:40&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_20x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X20_NO_SILK_KIT">
<description>&lt;h3&gt;Plated Through Hole -20 Pin No Silk Kit&lt;/h3&gt;
Mask on only one side for soldering kits.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:20&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_20&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X12_LOCK_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole -12 Pin Locking Footprint No Silk&lt;/h3&gt;
Holes are offset 0.005", to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:12&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_12&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="DEANS">
<description>&lt;h3&gt;Deans Connector&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Prototyping/deans_connector_PRT-11864.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;BATTERY_CONN&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X5-SHROUDED-NS">
<description>&lt;h3&gt;Plated Through Hole - 2x5 Shrouded Header No Silk&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Shrouded-10pin.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X20_LOCK_NOSILK">
<description>&lt;h3&gt;Plated Through Hole -20 Pin Locking Footprint No Silk &lt;/h3&gt;
Holes are offset 0.005" from center to hold pins in place while soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:20&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_20&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X01_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:1&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SCREWTERMINAL-3.5MM-5">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch -5 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 5&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X20_NOSILK">
<description>&lt;h3&gt;Plated Through Hole -20 Pin No Silk&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:20&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_20&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="6_PIN_SERIAL_TARGET_SIDE_RA_SMT">
<description>&lt;h3&gt;6 pin Serial Target - Right Angle  SMT&lt;/h3&gt;
Package for devices meant to mate to an FTDI connector. 
&lt;p&gt; tDocu shows pin location. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;6_Pin_Serial_Target&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X20_SHROUDED_SMT">
<description>&lt;h3&gt;Surface Mount - 2x20 Shrouded Header&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:40&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://sullinscorp.com/catalogs/145_PAGE118_.100_SBH11_SERIES_MALE_BOX_HDR_ST_RA_SMT.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_20x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SMTSO-256-ET-0.165DIA">
<description>&lt;h3&gt;SMTSO-256-ET Flush Mount Nut&lt;/h3&gt;
.165 drill
&lt;br&gt;
Fits 4-40 Screws. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 1&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X07_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole -7 Pin  No Silk&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:7&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_07&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X08_FEMALE_LOCK">
<description>&lt;h3&gt;Plated Through Hole -8 Pin Locking Female Headers&lt;/h3&gt;
Holes are offset 0.005" to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://cdn.sparkfun.com/datasheets/Prototyping/SP-140520-XX-001.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SAMTECH_FTSH-105-01">
<description>&lt;h3&gt;ARM Cortex Debug Connector (10-pin)&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.05"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.samtec.com/ftppub/cpdf/FTSH-1XX-XX-XXX-DV-XXX-MKT.pdf"&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CORTEX_DEBUG&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X5-PTH-1.27MM-NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - 2x5 ARM Cortex Debug Connector (10-pin)&lt;/h3&gt;
&lt;p&gt;tDoc (51) layer border represents maximum dimensions of plastic housing.&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:1.27mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://portal.fciconnect.com/Comergent//fci/drawing/20021111.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X06_1.27MM">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:1.27mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="PAD.02X.02">
<description>&lt;h3&gt;Electrically Conductive Pad 0.02" Square&lt;/h3&gt;
Used as a test point connection for pogo pins or other debugging tools. 
&lt;p&gt;Specifications:
&lt;li&gt;Area: 0.02" x 0.02"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;TEST_POINT&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="PAD.03X.03">
<description>&lt;h3&gt;Electrically Conductive Pad 0.03" Circle&lt;/h3&gt;
Used as a test point connection for pogo pins or other debugging tools. 
&lt;p&gt;Specifications:
&lt;li&gt;Area: 0.03" x 0.03"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;TEST_POINT&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="PAD.03X.05">
<description>&lt;h3&gt;Electrically Conductive Pad 0.05" Circle&lt;/h3&gt;
Used as a test point connection for pogo pins or other debugging tools. 
&lt;p&gt;Specifications:
&lt;li&gt;Area: 0.05" x 0.05"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;TEST_POINT&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="PAD.03X.04">
<description>&lt;h3&gt;Electrically Conductive Pad 0.04" Circle&lt;/h3&gt;
Used as a test point connection for pogo pins or other debugging tools. 
&lt;p&gt;Specifications:
&lt;li&gt;Area: 0.04" x 0.04"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;TEST_POINT&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="TP_15TH">
<description>&lt;h3&gt;Electrically Conductive Via 0.015" Drill&lt;/h3&gt;
Used as a test point connection for pogo pins or other debugging tools. 
&lt;p&gt;Specifications:
&lt;li&gt;Area:0.015"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;TEST_POINT&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="AUDIO_JACK_0.25&quot;_TRS_PTH_RA">
<description>&lt;h3&gt;Right Angle -1/4" Stereo Jack&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 6&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Components/General/JP-611%20DD.jpg”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;AUDIO_JACK_TRS_0.25"_PTH_RA&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="DIN5-RA-PTH">
<description>&lt;h3&gt;DIN5/180 Connector - Right Angle Female&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 5&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Connectors/MIDI-RA.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;DIN5&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X14_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole -14 Pin No Silk outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:14&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_14&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="EDISON_DAUGHTER">
<description>&lt;h3&gt;Hirose DF30C-70DP-0.4V(51) Receiver Footprint w/ Edison Outline&lt;/h3&gt;
Package can be used as basic guideline for creating Edison-mating daughter boards.
&lt;br&gt;Includes keepout area for antenna. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:70&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.4mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://media.digikey.com/pdf/Data%20Sheets/Hirose%20PDFs/DF40C-70DP-0.4V(51).pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;EDISON_FULL_CONNECTOR&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="DF40C-70DP-0.4(51)">
<description>&lt;h3&gt;Hirose DF30C-70DP-0.4V(51) Receiver&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:70&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.4mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://media.digikey.com/pdf/Data%20Sheets/Hirose%20PDFs/DF40C-70DP-0.4V(51).pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;EDISON_FULL_CONNECTOR&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="DF40-XC-(X.X)-70DS-0.4V(51)">
<description>&lt;h3&gt;Hirose DF40C-70DP-0.4V(51) Plug&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:70&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.4mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://media.digikey.com/pdf/Data%20Sheets/Hirose%20PDFs/DF40C-70DP-0.4V(51).pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;EDISON_FULL_CONNECTOR&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="MICRO-SD-SOCKET-SDIO">
</package>
<package name="1X02_POKEHOME">
<description>2 pin poke-home connector

part number 2062-2P from STA</description>
</package>
<package name="USB-B-MICRO-SMD_RED_PASTE">
<description>&lt;h3&gt;USB - microB SMD Reduced Paste&lt;/h3&gt;
 70% paste area under D+ D- USBID pins for applications where those pins aren't required, to reduce the likelihood of bridges.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Micro-USB.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;USB_MICRO-B&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X10_LOCK_NS">
<description>&lt;h3&gt;Plated Through Hole -10 Pin Locking Footprint - NO SILK&lt;/h3&gt;
Holes are offset 0.005" to hold pins in place while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_10&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="JST-3-PTH-NS">
<description>&lt;h3&gt;JST 3 Pin Right Angle Plated Through Hole &amp;ndash; NO SILK&lt;/h3&gt;
&lt;p&gt;No silkscreen outline. tDoc layer (51) indicates connector footprint.&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/ePH.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SCREWTERMINAL-3.5MM-3-NS">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch -3 Pin PTH &amp;ndash; NO SILK&lt;/h3&gt;
&lt;p&gt;No silkscreen outline. tDoc layer (51) indicates connector footprint.&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 3&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="USB-MICROB-PTH">
</package>
<package name="JST04_1MM_RA_STRESSRELIEF">
<description>Qwiic connector with milled cutout. Sliding the cable into this slot prevents the cable from coming unplugged.</description>
</package>
<package name="1X02_RA_PTH_FEMALE">
</package>
<package name="JST-6-SMD-HORI-1.0MM">
<description>&lt;h3&gt;JST SH Vertical 6-Pin SMT&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch: 1 mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/GPS/EM406-SMDConnector-eSH.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;JST_6PIN_VERTICAL&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X6_NOSILK">
</package>
<package name="USB_B_VERTICAL_PTH">
</package>
<package name="USB-B-MICRO-SMD_V04">
</package>
<package name="MICRO-B-TH">
<description>&lt;h3&gt;Micro B USB Plug Assembly - Straight Through-hole&lt;/h3&gt;
&lt;b&gt;**UNPROVEN**&lt;/b&gt;&lt;Br&gt;
See Digikey part #H11497-ND</description>
</package>
<package name="MICRO-B-SMT">
<description>&lt;h3&gt;USB Micro-B Plug Connector&lt;/h3&gt;
Manufacturer part #: ZX80-B-5SA&lt;br&gt;
Manufacturer: Hirose&lt;br&gt;&lt;br&gt;
&lt;b&gt;***Unproven***&lt;/b&gt; (Passed 1:1 printout test though!)</description>
</package>
<package name="USB-B-MICRO-SMD_V03">
</package>
<package name="USB-B-MICRO-SMD_VERT">
</package>
<package name="RASPBERRY_PI_SHIELD_HOLES">
<description>&lt;h3&gt;Surface Mount - 2x20 Header&lt;/h3&gt;

Reversed pinout to match Raspberry Pi male header pinout when coupled.</description>
</package>
<package name="RASPBERRY_PI_SHIELD_NOHOLES">
</package>
<package name="RASPBERRY_PI_SHIELD_BOTTOM_ENTRY_NOHOLES">
</package>
<package name="1X06_SCREW_TERMINAL_BLOCK">
</package>
<package name="MICROSD_TINY">
</package>
<package name="USB-MICROB-PTH-MILL">
</package>
<package name="2X8-SHROUDED_LOCK">
</package>
<package name="1X18_NO_SILK">
</package>
<package name="1X12_SM_SQ_NOSILK">
</package>
<package name="1X16_SM_SQ_NOSILK">
</package>
<package name="GATOR">
</package>
<package name="TAB_GATOR_MINI">
</package>
<package name="2X5-PTH-1.27MM">
<description>&lt;h3&gt;Plated Through Hole - 2x5 ARM Cortex Debug Connector (10-pin)&lt;/h3&gt;
&lt;p&gt;tDoc (51) layer border represents maximum dimensions of plastic housing.&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:1.27mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://portal.fciconnect.com/Comergent//fci/drawing/20021111.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X10-1.25MM-SMD">
</package>
<package name="SCREWTERMINAL-3.5MM-9">
</package>
<package name="SCREWTERMINAL-3.5MM-10">
</package>
<package name="SCREWTERMINAL-3.5MM-7">
</package>
<package name="SOLDER_PAD_2">
<description>&lt;h3&gt;LuMini Ring Solder Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: .8 in&lt;/li&gt;
&lt;li&gt;Area: .4 x 1 in.&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="CIRCULARPAD">
<description>LuMini Pad</description>
</package>
<package name="XLR-3_MALE">
<description>&lt;h3&gt;XLR-3 Connector - Package for the NC3MAAH-1 XLR-3 Connector&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 5&lt;/li&gt;
&lt;li&gt;Area: 1 x .7 in&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=http://www.neutrik.us/zoolu-website/media/download/1429/Drawing+NC3MAAH-1&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="XLR-3_FEMALE">
<description>&lt;h3&gt;XLR-3 Connector - Package for the NC3FAAH-1 XLR-3 Connector&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 5&lt;/li&gt;
&lt;li&gt;Area: 1 x .7 in&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=http://www.neutrik.us/zoolu-website/media/download/1389/Drawing+NC3FAAH1&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="USB-SOLDER-PADS">
</package>
<package name="USB-SOLDER-PADS-DATA_ONLY">
</package>
<package name="FPC05040-17204">
<description>This is a 40-pin FPC connector supplied by Atom. SparkFun SKU is 
CONN-14082</description>
</package>
<package name="1X16_LOCK_NO_SILK">
</package>
<package name="1X04_SPRING_TERMINAL">
</package>
<package name="GATOR_MINI">
</package>
<package name="FPC-24-AMPHENOL-SFV24R-1STE1HLF">
<description>&lt;h3&gt;24-Pin FPC/FFC Connector - 0.5mm pitch&lt;/h3&gt;
&lt;p&gt;Digikey: 609-4320-2-ND&lt;/p&gt;
&lt;p&gt;&lt;a href=https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/10112793.pdf&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="1X07_LOCK_NO_SILK">
</package>
<package name="1X04_UNITEST">
</package>
<package name="USB-C-16P-4LAYER-ISOLATED">
</package>
<package name="USB-C-16P">
</package>
<package name="2X5-SMD-1.27MM">
<description>Shrouded SMD connector for JTAG and SWD applications.</description>
</package>
<package name="1X08_SMD_COMBINED_NC">
</package>
<package name="JST04_1MM_VERT">
<description>&lt;h3&gt;Vertical Qwiic Connector&lt;/h3&gt;

&lt;p&gt;Physical and Electrical Charactersistics&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;Voltage Rating: 50V&lt;/li&gt;
&lt;li&gt;Current Rating 1.0A&lt;/li&gt;
&lt;li&gt;Contact Resistance: 20 milliohms&lt;/li&gt;
&lt;li&gt;ROHS Compliant&lt;/li&gt;
&lt;li&gt;SMD Pitch: 1mm&lt;/li&gt;
&lt;li&gt;Small pad size: .6mm x 1.55mm&lt;/li&gt;
&lt;li&gt;Large pad size: 1.2mm x 2.0mm&lt;/li&gt;
&lt;li&gt;&lt;/li&gt;
&lt;li&gt;&lt;/li&gt;
&lt;/ul&gt;</description>
</package>
<package name="1X04_1.27MM_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch: 1.27mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X13-SHROUDED">
</package>
</packages>
<symbols>
<symbol name="ARDUINO_SERIAL_PROGRAM">
<description>&lt;h3&gt;6-pin header connection for use with the "FTDI BASIC" pinout - TARGET SIDE.&lt;/h3&gt;
&lt;p&gt;&lt;/p&gt;

&lt;h3&gt;Also known as "Arduino Serial Program Header".&lt;/h3&gt;
&lt;p&gt;&lt;/p&gt;

It is used to mate with our FTDI Basic serial programmers using the Arduino IDE. 

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Note, this device has "TARGET" in the name.&lt;/b&gt; It is intended to be used on a design that contains a target micro-controller that you wish to program. 

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;The "sister" device, named "CABLE"&lt;/b&gt; is inteneded to be used on a design that usually lives on the end of your USB cable and prvides the converter chip (FTDI232 or FTDI231x) to commnicate serial RX/TX.</description>
<pin name="DTR" direction="pas"/>
<pin name="RXI" direction="pas"/>
<pin name="TXO" direction="pas"/>
<pin name="VCC" direction="pas"/>
<pin name="CTS" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="ATX24-1">
<description>&lt;h3&gt;ATX24 Pin Power Supply Connector&lt;/h3&gt;
&lt;p&gt;This is a good connector for connecting a computer power supply to a PCB. It's massive, but provides many amps of power at 5V and 12V.&lt;/p&gt;</description>
<pin name="-12V"/>
<pin name="3.3V@0"/>
<pin name="3.3V@1"/>
<pin name="3.3V@2"/>
<pin name="3.3V@3"/>
<pin name="5V@0"/>
<pin name="5V@1"/>
<pin name="5V@2"/>
<pin name="5V@3"/>
<pin name="5V@4"/>
<pin name="5V_STDBY"/>
<pin name="12V@0"/>
<pin name="12V@1"/>
<pin name="GND@0"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="GND@4"/>
<pin name="GND@5"/>
<pin name="GND@6"/>
<pin name="GND@7"/>
<pin name="NC"/>
<pin name="PS_ON"/>
<pin name="PWR_OK"/>
</symbol>
<symbol name="AUDIO-JACK">
<description>&lt;h3&gt; Audio Jack &lt;/h3&gt;
&lt;p&gt; 3 pin Basic Audio Jack&lt;/p&gt;</description>
<pin name="RIGHT"/>
<pin name="LEFT"/>
<pin name="SLEEVE"/>
</symbol>
<symbol name="AUDIO-JACK2">
<description>&lt;h3&gt; Audio Jack &lt;/h3&gt;
&lt;p&gt;  Basic Audio Jack with bypass switches&lt;/p&gt;</description>
<pin name="RING"/>
<pin name="TIP"/>
<pin name="SLEEVE"/>
<pin name="RSH"/>
<pin name="TSH"/>
</symbol>
<symbol name="AVR_SPI_PROGRAMMER_6">
<description>&lt;h3&gt;AVR ISP 6 Pin&lt;/h3&gt;
&lt;p&gt;This is the reduced ISP connector for AVR programming. Common on Arduino.</description>
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="AVR_SPI_PROGRAMMER">
<description>&lt;h3&gt;AVR 10-pin ICSP Header&lt;/h3&gt;
&lt;p&gt;This is the standard AVR In Circuit Serial Programming header. Minimal, but includes pin one indicator. Works with standard Olimex programmers. &lt;/p&gt;</description>
<pin name="MOSI" direction="pas" function="dot"/>
<pin name="VCC" direction="pwr" function="dot"/>
<pin name="NC" direction="nc" function="dot"/>
<pin name="GND@1" direction="pwr" function="dot"/>
<pin name="RESET" direction="pas" function="dot"/>
<pin name="GND@2" direction="pwr" function="dot"/>
<pin name="SCK" direction="pas" function="dot"/>
<pin name="GND@3" direction="pwr" function="dot"/>
<pin name="MISO" direction="pas" function="dot"/>
<pin name="GND@4" direction="pwr" function="dot"/>
</symbol>
<symbol name="BANANA_CONN">
<description>&lt;h3&gt;Through-hole Banana Jack&lt;/h3&gt;
&lt;p&gt;Basic PTH connection for banana jack plugs&lt;/p&gt;</description>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="BC9VPC">
<description>&lt;h3&gt;Battery&lt;/h3&gt;
&lt;p&gt;&lt;/p&gt;</description>
<pin name="V+"/>
<pin name="V-"/>
</symbol>
<symbol name="BNC">
<description>&lt;h3&gt;BNC Connector&lt;/h3&gt;
2 pin connection</description>
<pin name="OUT"/>
<pin name="GND"/>
</symbol>
<symbol name="F09G">
<description>&lt;h3&gt;DB9 Connector&lt;/h3&gt;
Standard DB9 (D-Sub 9) serial connector. Can be used for CAN bus as well as RS485 and RS232.</description>
<pin name="1" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="DIN7">
<description>&lt;h3&gt;Mini-DIN7 Connector&lt;/h3&gt;
Through-hole MiniDIN 7 connector. Commonly used with Roomba products. Don't confuse this with DIN-6, which is commonly used on oldschool keyboards and mice.</description>
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
</symbol>
<symbol name="DS_TOUCH_CONNECTOR">
<description>&lt;h3&gt;4-pin PSP touch screen connector&lt;/h3&gt;
This is the connector for the PSP touch screen. 

This connector is compatible with the PSP Touch Screen NOT the Sharp Color 24-Bit LCD.</description>
<pin name="X1"/>
<pin name="Y2"/>
<pin name="X2"/>
<pin name="Y1"/>
</symbol>
<symbol name="EB-85A">
<description>&lt;h3&gt;EB-85A Connector&lt;/h3&gt;
Connector for the EB-85A/FV-M8 GPS receiver.</description>
<pin name="GND" direction="pwr"/>
<pin name="TX2" direction="out"/>
<pin name="RX1" direction="in"/>
<pin name="TX1" direction="out"/>
<pin name="RX2" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="PPS" direction="out"/>
<pin name="BATT" direction="pwr"/>
</symbol>
<symbol name="EM406">
<description>&lt;h3&gt;EM406 GPS Connector&lt;/h3&gt;
Six pin connection for the EM406 GPS module.</description>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="1PPS"/>
<pin name="VCC"/>
</symbol>
<symbol name="EM408">
<description>&lt;h3&gt;EM-408 GPS receiver connector&lt;/h3&gt;
This is the  5 pin connector for the EM408 GPS receiver.</description>
<pin name="EN"/>
<pin name="GND" direction="pwr"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="CONN_06">
<description>&lt;h3&gt;6 Pin Connection&lt;/h3&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="CONN_01">
<description>&lt;h3&gt;1 Pin Connection&lt;/h3&gt;</description>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="CONN_02">
<description>&lt;h3&gt;2 Pin Connection&lt;/h3&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="CONN_03">
<description>&lt;h3&gt;3 Pin Connection&lt;/h3&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="CONN_04">
<description>&lt;h3&gt;4 Pin Connection&lt;/h3&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="CONN_04X2">
<description>&lt;h3&gt;8 Pin Connection&lt;/h3&gt;
4x2 pin layout</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="CONN_05">
<description>&lt;h3&gt;5 Pin Connection&lt;/h3&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="CONN_05X2">
<description>&lt;h3&gt;10 Pin Connection&lt;/h3&gt;
5x2 pin layout</description>
<pin name="10" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="CONN_07">
<description>&lt;h3&gt; 7 Pin Connection&lt;/h3&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="CONN_08">
<description>&lt;h3&gt; 8 Pin Connection&lt;/h3&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="CONN_2X8">
<description>&lt;h3&gt;16 Pin Connection&lt;/h3&gt;
2x8 pin layout</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="CONN_09">
<description>&lt;h3&gt; 9 Pin Connection&lt;/h3&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="CONN_10">
<description>&lt;h3&gt; 10 Pin Connection&lt;/h3&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="CONN_10X2">
<description>&lt;h3&gt; 20 Pin Connection&lt;/h3&gt;
10x2 pin layout</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="CONN_11">
<description>&lt;h3&gt; 11 Pin Connection&lt;/h3&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
<symbol name="CONN_12">
<description>&lt;h3&gt; 12 Pin Connection&lt;/h3&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="CONN_13">
<description>&lt;h3&gt; 13 Pin Connection&lt;/h3&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
</symbol>
<symbol name="CONN_14">
<description>&lt;h3&gt; 14 Pin Connection&lt;/h3&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="CONN_15">
<description>&lt;h3&gt; 15 Pin Connection&lt;/h3&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
</symbol>
<symbol name="CONN_16">
<description>&lt;h3&gt; 16 Pin Connection&lt;/h3&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="CONN_17">
<description>&lt;h3&gt; 17 Pin Connection&lt;/h3&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
</symbol>
<symbol name="CONN_18">
<description>&lt;h3&gt; 18 Pin Connection&lt;/h3&gt;</description>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="CONN_19">
<description>&lt;h3&gt; 19 Pin Connection&lt;/h3&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
</symbol>
<symbol name="CONN_20">
<description>&lt;h3&gt; 20 Pin Connection&lt;/h3&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
<symbol name="CONN_24">
<description>&lt;h3&gt; 24 Pin Connection&lt;/h3&gt;</description>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
</symbol>
<symbol name="CONN_25">
<description>&lt;h3&gt; 25 Pin Connection&lt;/h3&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
</symbol>
<symbol name="CONN_27">
<description>&lt;h3&gt; 27 Pin Connection&lt;/h3&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
</symbol>
<symbol name="CONN_29">
<description>&lt;h3&gt; 29 Pin Connection&lt;/h3&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
</symbol>
<symbol name="CONN_30">
<description>&lt;h3&gt; 30 Pin Connection&lt;/h3&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
</symbol>
<symbol name="CONN_40">
<description>&lt;h3&gt; 40 Pin Connection&lt;/h3&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
</symbol>
<symbol name="MAGJACK">
<pin name="YLED-"/>
<pin name="YLED+"/>
<pin name="GLED-"/>
<pin name="GLED+"/>
<pin name="RD-"/>
<pin name="RCT"/>
<pin name="RD+"/>
<pin name="TD-"/>
<pin name="TCT"/>
<pin name="TD+"/>
<pin name="SHIELD@0"/>
<pin name="SHIELD@1"/>
<pin name="NC@4"/>
<pin name="NC@5"/>
</symbol>
<symbol name="MAGJACK-POE">
<pin name="YLED-"/>
<pin name="YLED+"/>
<pin name="GLED-"/>
<pin name="GLED+"/>
<pin name="RD-"/>
<pin name="RCT"/>
<pin name="RD+"/>
<pin name="TD-"/>
<pin name="TCT"/>
<pin name="TD+"/>
<pin name="SHIELD@0"/>
<pin name="SHIELD@1"/>
<pin name="V+"/>
<pin name="V-"/>
</symbol>
<symbol name="OBDII">
<pin name="1"/>
<pin name="J1850BUS+"/>
<pin name="3"/>
<pin name="CHASGND"/>
<pin name="SIGGND"/>
<pin name="CANHIGH"/>
<pin name="ISOK-LINE"/>
<pin name="8"/>
<pin name="9"/>
<pin name="J1850BUS"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="CANLOW"/>
<pin name="ISOL-LINE"/>
<pin name="BATTPOWER"/>
</symbol>
<symbol name="ICSP-PIC">
<description>&lt;h3&gt;ISCP Programming connector for PICs&lt;/h3&gt;
This 6 pin header contains all the lines necessary for programming most PIC microcontrollers.</description>
<pin name="GND" direction="pwr"/>
<pin name="PGC"/>
<pin name="PGD"/>
<pin name="PGM"/>
<pin name="VCC" direction="pwr"/>
<pin name="VPP"/>
</symbol>
<symbol name="PIC-ISCP-MINI">
<pin name="VPP" direction="pas"/>
<pin name="VCC" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="PGD" direction="pas"/>
<pin name="PGC" direction="pas"/>
</symbol>
<symbol name="CONN_12X2">
<description>&lt;h3&gt; 24 Pin Connection&lt;/h3&gt;

12x2 pin layout</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="CONN_26X2">
<description>&lt;h3&gt; 52 Pin Connection&lt;/h3&gt;
26x2 pin layout</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="41" direction="pas"/>
<pin name="43" direction="pas"/>
<pin name="45" direction="pas"/>
<pin name="47" direction="pas"/>
<pin name="49" direction="pas"/>
<pin name="51" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="40" direction="pas"/>
<pin name="42" direction="pas"/>
<pin name="44" direction="pas"/>
<pin name="46" direction="pas"/>
<pin name="48" direction="pas"/>
<pin name="50" direction="pas"/>
<pin name="52" direction="pas"/>
</symbol>
<symbol name="POWERJACK">
<pin name="GNDBREAK"/>
<pin name="GND"/>
<pin name="PWR"/>
</symbol>
<symbol name="PSP_CONNECTOR">
<pin name="G7"/>
<pin name="G6"/>
<pin name="G5"/>
<pin name="G4"/>
<pin name="G3"/>
<pin name="G2"/>
<pin name="G1"/>
<pin name="G0"/>
<pin name="R7"/>
<pin name="R6"/>
<pin name="R5"/>
<pin name="R4"/>
<pin name="R3"/>
<pin name="R2"/>
<pin name="R1"/>
<pin name="R0"/>
<pin name="VCC2"/>
<pin name="VCC"/>
<pin name="GND2"/>
<pin name="GND"/>
<pin name="TEST3"/>
<pin name="TEST2"/>
<pin name="TEST1"/>
<pin name="NC2"/>
<pin name="AVDD2"/>
<pin name="AVDD"/>
<pin name="NC"/>
<pin name="VSYNC"/>
<pin name="HSYNC"/>
<pin name="DISP"/>
<pin name="CK"/>
<pin name="GND3"/>
<pin name="B7"/>
<pin name="B6"/>
<pin name="B5"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="B1"/>
<pin name="B0"/>
</symbol>
<symbol name="PSP_TOUCH_CONNECTOR">
<pin name="X1"/>
<pin name="Y2"/>
<pin name="X2"/>
<pin name="Y1"/>
</symbol>
<symbol name="RJ45-8">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="8"/>
<pin name="7"/>
<pin name="6"/>
<pin name="5"/>
</symbol>
<symbol name="SCREENKEYMATINGCONNECTOR">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
</symbol>
<symbol name="SIMHOLDER">
<pin name="VCC" direction="pwr"/>
<pin name="RST" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VPP" direction="in"/>
<pin name="I/O"/>
</symbol>
<symbol name="U.FL">
<pin name="GND@0"/>
<pin name="SIGNAL"/>
<pin name="GND@1"/>
</symbol>
<symbol name="USB">
<description>&lt;h3&gt;USB A/B - with Shield Pins&lt;/h3&gt;
&lt;p&gt;USB connector for type-A and type-B connectors. Includes shield pins broken out. &lt;/p&gt;</description>
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SHIELD"/>
</symbol>
<symbol name="USB-5PIN">
<description>&lt;h3&gt;USB - 5 pin&lt;/h3&gt;
&lt;p&gt;5 pin USB connector: VBUS, GND, D+, D-, ID &lt;/p&gt;
&lt;p&gt;Includes 4 pins for shield connections &lt;/p&gt;</description>
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="ID"/>
<pin name="SHIELD"/>
</symbol>
<symbol name="MICROB-PLUG">
<pin name="VCC"/>
<pin name="D-"/>
<pin name="D+"/>
<pin name="ID"/>
<pin name="GND"/>
<pin name="SHIELD"/>
</symbol>
<symbol name="DIL-28-3">
<description>&lt;h3&gt;ZIF Socket 28-Pin 0.3"&lt;/h3&gt;
&lt;p&gt;Lever-action ZIF socket for 28-pin ICs&lt;/p&gt;</description>
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
<pin name="P$11"/>
<pin name="P$12"/>
<pin name="P$13"/>
<pin name="P$14"/>
<pin name="P$15"/>
<pin name="P$16"/>
<pin name="P$17"/>
<pin name="P$18"/>
<pin name="P$19"/>
<pin name="P$20"/>
<pin name="P$21"/>
<pin name="P$22"/>
<pin name="P$23"/>
<pin name="P$24"/>
<pin name="P$25"/>
<pin name="P$26"/>
<pin name="P$27"/>
<pin name="P$28"/>
</symbol>
<symbol name="RCA">
<pin name="SWITCH"/>
<pin name="SHELL"/>
<pin name="PIN"/>
</symbol>
<symbol name="USB_AB">
<description>&lt;h3&gt;USB Type AB&lt;/h3&gt;
&lt;p&gt;Capable of OTG. 
&lt;br&gt;5-pins: USBVCC, GND, D+, D-, USBID&lt;/p&gt;</description>
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="USBID"/>
<pin name="SHIELD"/>
</symbol>
<symbol name="SDCARD-1">
<pin name="CD/DAT3"/>
<pin name="CMD"/>
<pin name="VSS1" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="CLK"/>
<pin name="VSS2" direction="pwr"/>
<pin name="DAT0"/>
<pin name="DAT1"/>
<pin name="DAT2"/>
<pin name="WP"/>
<pin name="CD"/>
<pin name="SH@1"/>
<pin name="SH@2"/>
</symbol>
<symbol name="MYDAQ_CONNECTOR">
<pin name="AN1-" direction="in"/>
<pin name="+15V" direction="pwr"/>
<pin name="-15V" direction="pwr"/>
<pin name="AGND_15V" direction="pwr"/>
<pin name="DIO2"/>
<pin name="DIO3"/>
<pin name="DIO4"/>
<pin name="DIO5"/>
<pin name="DIO6"/>
<pin name="DIO7"/>
<pin name="DGND" direction="pwr"/>
<pin name="DIO0"/>
<pin name="DIO1"/>
<pin name="5V" direction="pwr"/>
<pin name="AO0" direction="out"/>
<pin name="AO1" direction="out"/>
<pin name="AGND_IO" direction="pwr"/>
<pin name="AI0+" direction="in"/>
<pin name="AI0-" direction="in"/>
<pin name="AI1+" direction="in"/>
</symbol>
<symbol name="AUDIO-JACK3-TRRS">
<description>&lt;h3&gt; Audio Jack &lt;/h3&gt;
&lt;p&gt;   Audio Jack with TRRS&lt;/p&gt;</description>
<pin name="RING1"/>
<pin name="RING2"/>
<pin name="EARTH"/>
<pin name="TIP"/>
</symbol>
<symbol name="CONN_03X2">
<description>&lt;h3&gt;6 Pin Connection&lt;/h3&gt;
3x2 pin layout</description>
<pin name="1"/>
<pin name="3"/>
<pin name="5"/>
<pin name="6"/>
<pin name="4"/>
<pin name="2"/>
</symbol>
<symbol name="JST_2MM_MALE">
<pin name="-"/>
<pin name="+"/>
<pin name="PAD2"/>
<pin name="PAD1"/>
</symbol>
<symbol name="CONN_13X2">
<description>&lt;h3&gt; 26 Pin Connection&lt;/h3&gt;
13x2 pin layout</description>
<pin name="26" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="25" direction="pas"/>
</symbol>
<symbol name="JST_6_1MM_VERT">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
</symbol>
<symbol name="CONN_23">
<description>&lt;h3&gt; 23 Pin Connection&lt;/h3&gt;</description>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="BINDING_POST">
<description>&lt;h3&gt; Binding Post&lt;/h3&gt;
Single connection binding post</description>
<pin name="P$1"/>
</symbol>
<symbol name="CONN_06X2">
<description>&lt;h3&gt;12 Pin Connection&lt;/h3&gt;
6x2 pin layout</description>
<pin name="10" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="I2C_STANDARD">
<description>&lt;h3&gt;SparkFun I&lt;sup&gt;2&lt;/sup&gt;C Standard Pinout Header&lt;/h3&gt;
&lt;p&gt;SparkFun has standardized on a pinout for all I&lt;sup&gt;2&lt;/sup&gt;C based sensor breakouts.&lt;br&gt;</description>
<pin name="1" direction="pwr"/>
<pin name="2" direction="pwr"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="CONN_20X2">
<description>&lt;h3&gt; 40 Pin Connection&lt;/h3&gt;
20x2 pin layout</description>
<pin name="26" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
</symbol>
<symbol name="BATTERY_CONN">
<description>&lt;h3&gt;Battery Connection&lt;/h3&gt;
&lt;p&gt;&lt;/p&gt;</description>
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="CORTEX_DEBUG">
<description>&lt;h3&gt;Cortex Debug Connector&lt;/h3&gt;
&lt;p&gt;&lt;a href="http://infocenter.arm.com/help/topic/com.arm.doc.faqs/attached/13634/cortex_debug_connectors.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
<pin name="VCC"/>
<pin name="GND@3"/>
<pin name="GND@5"/>
<pin name="KEY"/>
<pin name="GNDDTCT"/>
<pin name="!RESET"/>
<pin name="NC/TDI"/>
<pin name="SWO/TDO"/>
<pin name="SWDCLK/TCK"/>
<pin name="SWDIO/TMS"/>
</symbol>
<symbol name="TEST-POINT">
<pin name="1"/>
</symbol>
<symbol name="VERNIER_ANALOG">
<pin name="AN1" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VRES" direction="pas"/>
<pin name="AUTOID" direction="pas"/>
<pin name="VCC" direction="pas"/>
<pin name="AN2" direction="pas"/>
</symbol>
<symbol name="VERNIER_DIGITAL">
<pin name="IO-0" direction="pas"/>
<pin name="IO-1" direction="pas"/>
<pin name="IO-2" direction="pas"/>
<pin name="VCC" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="IO-3" direction="pas"/>
</symbol>
<symbol name="AUDIO-JACK4-TRS-NORMALED-GND-1">
<description>&lt;h3&gt; Audio Jack &lt;/h3&gt;
&lt;p&gt; 1/4" TRS Jack - with normals on each conductor&lt;/p&gt;</description>
<pin name="EARTH"/>
<pin name="EARTH-NORM"/>
<pin name="RING"/>
<pin name="RING-NORM"/>
<pin name="TIP"/>
<pin name="TIP-NORM"/>
</symbol>
<symbol name="5-PIN-DIN">
<description>&lt;h3&gt;DIN5 Connector - Female Right Angle (frequently used as a MIDI Jack connector)&lt;/h3&gt;
This type of connector and cable is frequently used for transmitting midi data (musical instrument digital interface). It is what you usually see on a keyboard or set of electronic drums. Learn more &lt;a href="https://en.wikipedia.org/wiki/MIDI"&gt;here&lt;/a&gt;.</description>
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
</symbol>
<symbol name="EDISON_CONNECTOR">
<description>&lt;h3&gt;Intel &amp;reg; Edison Hirose Connectors &lt;/h3&gt;
&lt;p&gt;DF40 Series 70 pin connector used on the SparkFun Edison Blocks and the Intel &amp;reg; Edison.
&lt;p&gt;</description>
<pin name="VSYS@1"/>
<pin name="3.3V@1"/>
<pin name="1.8V"/>
<pin name="GND@1"/>
<pin name="MSIC_SLP_CLK"/>
<pin name="USB_ID"/>
<pin name="USB_DP"/>
<pin name="USB_DN"/>
<pin name="USB_VBUS"/>
<pin name="PWRBTN#"/>
<pin name="FAULT"/>
<pin name="PSW"/>
<pin name="V_VAT_BKUP"/>
<pin name="RESET_OUT#"/>
<pin name="GP44"/>
<pin name="GP165"/>
<pin name="GP45"/>
<pin name="GP46"/>
<pin name="GP47"/>
<pin name="GP48"/>
<pin name="GP49"/>
<pin name="GP15"/>
<pin name="GP14"/>
<pin name="GP12_PWM0"/>
<pin name="GP13_PWM1"/>
<pin name="GP182_PWM2"/>
<pin name="GP183_PWM3"/>
<pin name="GP19_I2C_1_SCL"/>
<pin name="GP20_I2C_1_SDA"/>
<pin name="GP27_I2C_6_SCL"/>
<pin name="GP28_I2C_6_SDA"/>
<pin name="GP42_I2S_2_RXD"/>
<pin name="GP40_I2S_2_CLK"/>
<pin name="GP41_I2S_2_FS"/>
<pin name="GP43_I2S_2_TXD"/>
<pin name="GP134_UART_2_RX"/>
<pin name="GP135_UART_2_TX"/>
<pin name="GP111_SPI_2_FS1"/>
<pin name="GP110_SPI_2_FS0"/>
<pin name="GP109_SPI_2_CLK"/>
<pin name="GP115_SPI_2_TXD"/>
<pin name="GP114_SPI_2_RXD"/>
<pin name="GP131_UART_1_TX"/>
<pin name="GP130_UART_1_RX"/>
<pin name="GP129_UART_1_RTS"/>
<pin name="GP128_UART_1_CTS"/>
<pin name="GP78_SD_0_CLK"/>
<pin name="GP77_SD_0_CD#"/>
<pin name="GP79_SD_0_CMD"/>
<pin name="GP80_SD_0_DAT0"/>
<pin name="GP81_SD_0_DAT1"/>
<pin name="GP82_SD_0_DAT2"/>
<pin name="GP83_SD_0_DAT3"/>
<pin name="OSC_CLK_OUT_0"/>
<pin name="3.3V@2"/>
<pin name="VSYS@2"/>
<pin name="VSYS@3"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="GND@4"/>
<pin name="GND@5"/>
<pin name="GND@6"/>
<pin name="RCVR_MODE"/>
<pin name="FW_RCVR"/>
<pin name="GP84_SD_CLK_FB"/>
<pin name="DCIN"/>
</symbol>
<symbol name="RASPBERRYPI_40_PIN_GPIO">
<pin name="3.3V" direction="pwr"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="GP4"/>
<pin name="GP17"/>
<pin name="GP27"/>
<pin name="GP22"/>
<pin name="MOSI" direction="out"/>
<pin name="MISO" direction="in"/>
<pin name="SCLK" direction="out"/>
<pin name="CE1" direction="out"/>
<pin name="CE0" direction="out"/>
<pin name="GP25"/>
<pin name="GP24"/>
<pin name="GP23"/>
<pin name="GP18#"/>
<pin name="RXI" direction="in"/>
<pin name="TXO" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="5V" direction="pwr"/>
<pin name="ID_SD"/>
<pin name="ID_SC"/>
<pin name="GP5"/>
<pin name="GP6"/>
<pin name="GP12"/>
<pin name="GP13"/>
<pin name="GP19"/>
<pin name="GP16"/>
<pin name="GP26"/>
<pin name="GP20"/>
<pin name="GP21"/>
</symbol>
<symbol name="U.FL-1">
<pin name="GND"/>
<pin name="SIGNAL"/>
</symbol>
<symbol name="MICROB-PLUG-1">
<pin name="D+"/>
<pin name="D-"/>
<pin name="GND"/>
<pin name="ID"/>
<pin name="SHIELD"/>
<pin name="VCC"/>
</symbol>
<symbol name="RASPBERRY_PI_HEADER-40-GROUPED">
<pin name="3.3V"/>
<pin name="SDA/D2"/>
<pin name="SCL/D3"/>
<pin name="D4"/>
<pin name="GND"/>
<pin name="D17"/>
<pin name="D27"/>
<pin name="D22"/>
<pin name="MOSI/D10"/>
<pin name="MISO/D9"/>
<pin name="SCK/D11"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D13"/>
<pin name="D19"/>
<pin name="D26"/>
<pin name="D21"/>
<pin name="D20"/>
<pin name="D16"/>
<pin name="D12"/>
<pin name="D7"/>
<pin name="CS/D8"/>
<pin name="D25"/>
<pin name="D24"/>
<pin name="D23"/>
<pin name="PCM_CLK/D18"/>
<pin name="RX/D15"/>
<pin name="TX/D14"/>
<pin name="5V"/>
<pin name="ID_SDA"/>
<pin name="ID_SCL"/>
</symbol>
<symbol name="CONN_24-1">
<description>&lt;h3&gt; 24 Pin Connection&lt;/h3&gt;</description>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="MICROSD">
<pin name="CS"/>
<pin name="DI"/>
<pin name="DO"/>
<pin name="GND"/>
<pin name="NC"/>
<pin name="RSV"/>
<pin name="SCK"/>
<pin name="SHIELD"/>
<pin name="VCC"/>
</symbol>
<symbol name="MICRO_BIT_GATOR_CLIP">
<pin name="P$1"/>
</symbol>
<symbol name="TAB_MICRO_BIT_GATOR_CLIP">
<pin name="P$1"/>
</symbol>
<symbol name="USB-C-MINIMUM">
<description>&lt;h3&gt;USB - C 16 Pin&lt;/h3&gt;
Exposes the minimal pins needed to implement a USB 2.x legacy device.</description>
<pin name="GND"/>
<pin name="VBUS"/>
<pin name="CC1"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="CC2"/>
<pin name="SHLD"/>
</symbol>
<symbol name="XLR-3">
<description>&lt;h3&gt;Neutrik XLR-3 Jack - XLR-3 Jack for DMX&lt;/h3&gt;
&lt;p&gt;Symbol for a horizontal, 3-pin DMX connector&lt;/p&gt;</description>
<pin name="GND"/>
<pin name="D+"/>
<pin name="D-"/>
</symbol>
<symbol name="CAMERA-OV7670-MODULE">
<pin name="SDA"/>
<pin name="AVDD"/>
<pin name="SCL"/>
<pin name="TRIG"/>
<pin name="LVLD"/>
<pin name="FVLD"/>
<pin name="INT"/>
<pin name="IOVDD"/>
<pin name="D7"/>
<pin name="MCLK"/>
<pin name="D6"/>
<pin name="GND"/>
<pin name="D5"/>
<pin name="PCLK"/>
<pin name="D4"/>
<pin name="D0"/>
<pin name="D3"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="MNT1"/>
<pin name="MNT2"/>
</symbol>
<symbol name="CORTEX_DEBUG_MINIMUM">
<pin name="VCC"/>
<pin name="GND"/>
<pin name="!RESET"/>
<pin name="SWO"/>
<pin name="SWDCLK"/>
<pin name="SWDIO"/>
</symbol>
<symbol name="RASPBERRYPI-26-PIN-GPIO">
<pin name="3.3V@1" direction="nc"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="GP4"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GP17"/>
<pin name="GP27"/>
<pin name="GP22"/>
<pin name="3.3V@17" direction="nc"/>
<pin name="MOSI" direction="out"/>
<pin name="MISO" direction="in"/>
<pin name="SCLK" direction="out"/>
<pin name="GND@25" direction="pwr"/>
<pin name="CE1" direction="out"/>
<pin name="CE0" direction="out"/>
<pin name="GP25"/>
<pin name="GND@20" direction="pwr"/>
<pin name="GP24"/>
<pin name="GP23"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GP18#"/>
<pin name="RXI" direction="in"/>
<pin name="TXO" direction="out"/>
<pin name="GND@6" direction="pwr"/>
<pin name="5V@4" direction="pwr"/>
<pin name="5V@2" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="6_PIN_SERIAL_TARGET" prefix="J" uservalue="yes">
<description>&lt;h3&gt;6-pin header connection for use with the "FTDI BASIC" pinout - TARGET SIDE.&lt;/h3&gt;
&lt;p&gt;&lt;/p&gt;

&lt;h3&gt;Also known as "Arduino Serial Program Header".&lt;/h3&gt;
&lt;p&gt;&lt;/p&gt;

It is used to mate with our FTDI Basic serial programmers using the Arduino IDE. 

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Note, this device has "TARGET" in the name.&lt;/b&gt; It is intended to be used on a design that contains a target micro-controller that you wish to program. 

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;The "sister" device, named "CABLE"&lt;/b&gt; is inteneded to be used on a design that usually lives on the end of your USB cable and prvides the converter chip (FTDI232 or FTDI231x) to commnicate serial RX/TX.

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;You can populate with some of these:&lt;/b&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/p&gt;
&lt;p&gt;&lt;/p&gt;
For reference (or to suit your programming needs) check out these designs:
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9716"&gt; SparkFun FTDI Basic Breakout - 5V&lt;/a&gt; (DEV-09716)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9873"&gt; SparkFun FTDI Basic Breakout - 3.3V&lt;/a&gt; (DEV-09873)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12935"&gt; SparkFun FTDI SmartBasic&lt;/a&gt; (DEV-12935)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13746"&gt; SparkFun Beefy 3 - FTDI Basic Breakout&lt;/a&gt; (DEV-13746)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="ARDUINO_SERIAL_PROGRAM"/>
</gates>
<devices>
<device name="SMD" package="1X06-SMD_RA_MALE">
<connects>
<connect gate="G$1" pin="CTS" pad="5"/>
<connect gate="G$1" pin="DTR" pad="1"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="RXI" pad="2"/>
<connect gate="G$1" pin="TXO" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08971"/>
</technology>
</technologies>
</device>
<device name="_SILK" package="1X06">
<connects>
<connect gate="G$1" pin="CTS" pad="5"/>
<connect gate="G$1" pin="DTR" pad="1"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="RXI" pad="2"/>
<connect gate="G$1" pin="TXO" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RA_LOCK" package="MOLEX_1X6_RA_LOCK">
<connects>
<connect gate="G$1" pin="CTS" pad="2"/>
<connect gate="G$1" pin="DTR" pad="6"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="RXI" pad="5"/>
<connect gate="G$1" pin="TXO" pad="4"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X06_LONGPADS">
<connects>
<connect gate="G$1" pin="CTS" pad="5"/>
<connect gate="G$1" pin="DTR" pad="1"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="RXI" pad="2"/>
<connect gate="G$1" pin="TXO" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X06_LOCK">
<connects>
<connect gate="G$1" pin="CTS" pad="5"/>
<connect gate="G$1" pin="DTR" pad="1"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="RXI" pad="2"/>
<connect gate="G$1" pin="TXO" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08437"/>
</technology>
</technologies>
</device>
<device name="PTH-KIT" package="1X06-KIT">
<connects>
<connect gate="G$1" pin="CTS" pad="5"/>
<connect gate="G$1" pin="DTR" pad="1"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="RXI" pad="2"/>
<connect gate="G$1" pin="TXO" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SILK" package="6_PIN_SERIAL_TARGET_SIDE_W_SILK">
<connects>
<connect gate="G$1" pin="CTS" pad="P$5"/>
<connect gate="G$1" pin="DTR" pad="P$1"/>
<connect gate="G$1" pin="GND" pad="P$6"/>
<connect gate="G$1" pin="RXI" pad="P$3"/>
<connect gate="G$1" pin="TXO" pad="P$2"/>
<connect gate="G$1" pin="VCC" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RA_SMT" package="6_PIN_SERIAL_TARGET_SIDE_RA_SMT">
<connects>
<connect gate="G$1" pin="CTS" pad="5"/>
<connect gate="G$1" pin="DTR" pad="1"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="RXI" pad="3"/>
<connect gate="G$1" pin="TXO" pad="2"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08971"/>
</technology>
</technologies>
</device>
<device name="_NO_SILK" package="1X06_NO_SILK">
<connects>
<connect gate="G$1" pin="CTS" pad="5"/>
<connect gate="G$1" pin="DTR" pad="1"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="RXI" pad="2"/>
<connect gate="G$1" pin="TXO" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATX24" prefix="J">
<description>&lt;h3&gt;ATX24 Pin Power Supply Connector - Right Angle PTH Mount&lt;/h3&gt;
&lt;p&gt;This is a good connector for connecting a computer power supply to a PCB. It's massive, but provides many amps of power at 5V and 12V.&lt;/p&gt;
&lt;p&gt;SparkFun Products:
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12867”&gt;SparkFun Benchtop Power Board Kit&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/10618”&gt;SparkFun Power Driver Shield Kit&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ATX24-1"/>
</gates>
<devices>
<device name="RH" package="ATX24_RIGHT_ANGLE">
<connects>
<connect gate="G$1" pin="-12V" pad="14"/>
<connect gate="G$1" pin="12V@0" pad="10"/>
<connect gate="G$1" pin="12V@1" pad="11"/>
<connect gate="G$1" pin="3.3V@0" pad="1"/>
<connect gate="G$1" pin="3.3V@1" pad="2"/>
<connect gate="G$1" pin="3.3V@2" pad="12"/>
<connect gate="G$1" pin="3.3V@3" pad="13"/>
<connect gate="G$1" pin="5V@0" pad="4"/>
<connect gate="G$1" pin="5V@1" pad="6"/>
<connect gate="G$1" pin="5V@2" pad="21"/>
<connect gate="G$1" pin="5V@3" pad="22"/>
<connect gate="G$1" pin="5V@4" pad="23"/>
<connect gate="G$1" pin="5V_STDBY" pad="9"/>
<connect gate="G$1" pin="GND@0" pad="3"/>
<connect gate="G$1" pin="GND@1" pad="5"/>
<connect gate="G$1" pin="GND@2" pad="7"/>
<connect gate="G$1" pin="GND@3" pad="15"/>
<connect gate="G$1" pin="GND@4" pad="17"/>
<connect gate="G$1" pin="GND@5" pad="18"/>
<connect gate="G$1" pin="GND@6" pad="19"/>
<connect gate="G$1" pin="GND@7" pad="24"/>
<connect gate="G$1" pin="NC" pad="20"/>
<connect gate="G$1" pin="PS_ON" pad="16"/>
<connect gate="G$1" pin="PWR_OK" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09674"/>
<attribute name="SF_ID" value="PRT-09498"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUDIO_JACK_2.5MM" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Audio Jack&lt;/h3&gt;
&lt;p&gt;2.5mm variants of PTH and SMT audio jacks.&lt;/p&gt;
&lt;p&gt;SparkFun Products:
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/11888”&gt;SparkFun PicoBoard&lt;/a&gt;- 2.5mm SMD&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="AUDIO-JACK"/>
</gates>
<devices>
<device name="_2.5MM" package="STEREOJACK2.5MM_STEREOJACK2.5MM">
<connects>
<connect gate="G$1" pin="LEFT" pad="SHIELD"/>
<connect gate="G$1" pin="RIGHT" pad="TIP"/>
<connect gate="G$1" pin="SLEEVE" pad="RING1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09878"/>
</technology>
</technologies>
</device>
<device name="SPECIAL_POGO_PINS" package="STEREOJACK2.5MM_SPECIAL_POGOPINS">
<connects>
<connect gate="G$1" pin="LEFT" pad="SHIELD"/>
<connect gate="G$1" pin="RIGHT" pad="TIP"/>
<connect gate="G$1" pin="SLEEVE" pad="RING1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_HOLESONLY" package="STEREOJACK2.5MM_SPECIAL_HOLES-ONLY">
<connects>
<connect gate="G$1" pin="LEFT" pad="SHIELD"/>
<connect gate="G$1" pin="RIGHT" pad="TIP"/>
<connect gate="G$1" pin="SLEEVE" pad="RING1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_2.5MM_SMD" package="STEREOJACK2.5MM">
<connects>
<connect gate="G$1" pin="LEFT" pad="1"/>
<connect gate="G$1" pin="RIGHT" pad="4"/>
<connect gate="G$1" pin="SLEEVE" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10062"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUDIO_JACK_3.5MM" prefix="J">
<description>&lt;h3&gt;Audio Jack&lt;/h3&gt;
&lt;p&gt; 3.5mm variants of PTH and SMT stereo audio jack with bypass switches.&lt;/p&gt;
&lt;p&gt;SparkFun Products:
&lt;ul&gt;&lt;li&gt;&lt;a href=”[https://www.sparkfun.com/products/11177]”&gt;SparkFun SparkPunk Sound Kit &lt;/a&gt; - PTH&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13720”&gt;MP3 Trigger&lt;/a&gt; -3.5mm SMD&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/11888”&gt;SparkFun PicoBoard&lt;/a&gt;- 2.5mm SMD&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="AUDIO-JACK2"/>
</gates>
<devices>
<device name="_PTH" package="AUDIO-JACK">
<connects>
<connect gate="G$1" pin="RING" pad="RING"/>
<connect gate="G$1" pin="RSH" pad="RSH"/>
<connect gate="G$1" pin="SLEEVE" pad="SLEEVE"/>
<connect gate="G$1" pin="TIP" pad="TIP"/>
<connect gate="G$1" pin="TSH" pad="TSH"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08774"/>
<attribute name="SF_ID" value="PRT-08032"/>
</technology>
</technologies>
</device>
<device name="_SMD" package="AUDIO-JACK-3.5MM-SMD">
<connects>
<connect gate="G$1" pin="RING" pad="RING"/>
<connect gate="G$1" pin="RSH" pad="RSH"/>
<connect gate="G$1" pin="SLEEVE" pad="SLEEVE"/>
<connect gate="G$1" pin="TIP" pad="TIP"/>
<connect gate="G$1" pin="TSH" pad="TSH"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10353"/>
</technology>
</technologies>
</device>
<device name="_KIT" package="AUDIO-JACK-KIT">
<connects>
<connect gate="G$1" pin="RING" pad="RING"/>
<connect gate="G$1" pin="RSH" pad="RSH"/>
<connect gate="G$1" pin="SLEEVE" pad="SLEEVE"/>
<connect gate="G$1" pin="TIP" pad="TIP"/>
<connect gate="G$1" pin="TSH" pad="TSH"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08774"/>
<attribute name="SF_ID" value="PRT-08032"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AVR_SPI_PROG_3X2" prefix="J">
<description>&lt;h3&gt;AVR ISP 6 Pin&lt;/h3&gt;
&lt;p&gt;This is the reduced ISP connector for AVR programming. Common on Arduino. This footprint will take up less PCB space and can be used with a 10-pin to 6-pin adapter such as SKU: BOB-08508&lt;/p&gt;

&lt;p&gt;&lt;b&gt;**Special note about "TEST_POINT" package.&lt;/b&gt; The stop mask is on the top side, so if you want your programming test points to be on the bottom of your board, make sure to place this package on the bottom side of the board. This also ensure that the orientation to program from the bottom side will be correct.&lt;/p&gt;

&lt;p&gt;SparkFun Products:
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11591"&gt;SparkFun ISP Pogo Adapter&lt;/a&gt; - NS&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11801"&gt;Tiny AVR Programmer&lt;/a&gt; -PTH&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="AVR_SPI_PROGRAMMER_6"/>
</gates>
<devices>
<device name="PTH" package="2X3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NS" package="2X3-NS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="OFFSET_PADS" package="2X3_OFFSET">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2X3_LOCK" package="2X3_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TESTPOINTS" package="2X3_TEST_POINTS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="2X3_SMT_POSTS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AVR_SPI_PROG_5X2" prefix="J">
<description>&lt;h3&gt;AVR 10-pin ICSP Header&lt;/h3&gt;
&lt;p&gt;This is the standard AVR In Circuit Serial Programming header. Minimal, but includes pin one indicator. Works with standard Olimex programmers. &lt;/p&gt;
&lt;p&gt;SparkFun Products:
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/778"&gt;2x5 AVR ICSP Male Header&lt;/a&gt; - PTH&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/8506”&gt;2x5 Pin Shrouded Header&lt;/a&gt; - PTH2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="AVR_SPI_PROGRAMMER"/>
</gates>
<devices>
<device name="PTH" package="2X5">
<connects>
<connect gate="G$1" pin="GND@1" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="6"/>
<connect gate="G$1" pin="GND@3" pad="8"/>
<connect gate="G$1" pin="GND@4" pad="10"/>
<connect gate="G$1" pin="MISO" pad="9"/>
<connect gate="G$1" pin="MOSI" pad="1"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="SCK" pad="7"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH2" package="2X5-SHROUDED">
<connects>
<connect gate="G$1" pin="GND@1" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="6"/>
<connect gate="G$1" pin="GND@3" pad="8"/>
<connect gate="G$1" pin="GND@4" pad="10"/>
<connect gate="G$1" pin="MISO" pad="9"/>
<connect gate="G$1" pin="MOSI" pad="1"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="SCK" pad="7"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08671"/>
<attribute name="SF_ID" value="PRT-08506"/>
</technology>
</technologies>
</device>
<device name="LOCK" package="2X5-SHROUDED_LOCK">
<connects>
<connect gate="G$1" pin="GND@1" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="6"/>
<connect gate="G$1" pin="GND@3" pad="8"/>
<connect gate="G$1" pin="GND@4" pad="10"/>
<connect gate="G$1" pin="MISO" pad="9"/>
<connect gate="G$1" pin="MOSI" pad="1"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="SCK" pad="7"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08671"/>
<attribute name="SF_ID" value="PRT-08506"/>
</technology>
</technologies>
</device>
<device name="SMD" package="2X5-SHROUDED_SMD">
<connects>
<connect gate="G$1" pin="GND@1" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="6"/>
<connect gate="G$1" pin="GND@3" pad="8"/>
<connect gate="G$1" pin="GND@4" pad="10"/>
<connect gate="G$1" pin="MISO" pad="9"/>
<connect gate="G$1" pin="MOSI" pad="1"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="SCK" pad="7"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BANANA_CONN" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Through-hole Banana Jack&lt;/h3&gt;
&lt;p&gt;Basic PTH connection for banana jack plugs&lt;/p&gt;
&lt;p&gt;SparkFun Products:
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/retired/10956"&gt;Multimeter Kit&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/retired/509"&gt;Banana to Alligator Cable&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/retired/508"&gt;Banana to Alligator Coax Cable&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/retired/507"&gt;Banana to Banana Cable&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/retired/506"&gt;Banana to IC Hook Cables&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BANANA_CONN"/>
</gates>
<devices>
<device name="" package="BANANA_CONN">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BC9VPC" prefix="J" uservalue="yes">
<description>&lt;h3&gt;9V Battery Holder - PC Mount&lt;/h3&gt;
&lt;p&gt;Standard and Kit footprints included&lt;/p&gt;
&lt;p&gt;SparkFun Products:
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11177"&gt;SparkFun SparkPunk Sound Kit&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12707”&gt;SparkFun SparkPunk Sequencer Kit&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BC9VPC"/>
</gates>
<devices>
<device name="" package="BC9VPC">
<connects>
<connect gate="G$1" pin="V+" pad="V+"/>
<connect gate="G$1" pin="V-" pad="V-"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="BATT-10855"/>
</technology>
</technologies>
</device>
<device name="_KIT" package="BC9VPC_KIT">
<connects>
<connect gate="G$1" pin="V+" pad="V+"/>
<connect gate="G$1" pin="V-" pad="V-"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="BATT-10855"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BNC" prefix="J">
<description>&lt;h3&gt;BNC Right Angle Connector&lt;/h3&gt;
&lt;p&gt;Mouser Part# 5227161&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/10550”&gt;BNC Connector - Right Angle&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BNC"/>
</gates>
<devices>
<device name="PTH" package="BNC">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="OUT" pad="S"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="LPA-12729"/>
<attribute name="SF_ID" value="PRT-10550"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DB9" prefix="J" uservalue="yes">
<description>&lt;h3&gt;DB9 Connector&lt;/h3&gt;
Standard DB9 (D-Sub 9) serial connector. Can be used for CAN bus as well as RS485 and RS232. Footprint production proven.

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Here is the female version connector we sell at SparkFun:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/429"&gt; 9 Pin Female Serial Connector - PCB Mount&lt;/a&gt; (PRT-00429)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This connector has been used on the following SparkFun products:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/449"&gt;SparkFun RS232 Shifter - SMD&lt;/a&gt; (PRT-00449)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8780"&gt; SparkFun RS232 Shifter SMD (No DB9)&lt;/a&gt; (PRT-08780)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="F09G"/>
</gates>
<devices>
<device name="FEMALE" package="DB9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08194"/>
</technology>
</technologies>
</device>
<device name="MALE" package="DB9_MALE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09904"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIN7" prefix="J">
<description>&lt;h3&gt;Mini-DIN7 Connector&lt;/h3&gt;
Through-hole MiniDIN 7 connector. Commonly used with Roomba products. Don't confuse this with DIN-6, which is commonly used on oldschool keyboards and mice.

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Here is the female version connector we sell at SparkFun:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/696"&gt; MiniDIN 7-Pin Connector&lt;/a&gt; (PRT-00696)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="DIN7"/>
</gates>
<devices>
<device name="" package="DIN7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08318"/>
<attribute name="SF_ID" value="PRT-00696"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS_TOUCH_CONNECTOR" prefix="J">
<description>&lt;h3&gt;4-pin PSP touch screen connector&lt;/h3&gt;
This is the SMD connector for the PSP touch screen. 4-pin right angle good, friction fit connector with 1 mm pitch.

This connector is compatible with the PSP Touch Screen NOT the Sharp Color 24-Bit LCD.

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Here is the connector we sell at SparkFun:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9104"&gt;Color 24-Bit LCD 4.3" PSP Touch Screen Connector&lt;/a&gt; (LCD-09104)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;It was also used on this SparkFun product:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13631"&gt;SparkFun Nintendo DS Screen Kit&lt;/a&gt; (LCD-13631)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="DS_TOUCH_CONNECTOR"/>
</gates>
<devices>
<device name="" package="DS_TOUCH_CONNECTOR">
<connects>
<connect gate="G$1" pin="X1" pad="1"/>
<connect gate="G$1" pin="X2" pad="3"/>
<connect gate="G$1" pin="Y1" pad="4"/>
<connect gate="G$1" pin="Y2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-0913"/>
<attribute name="SF_ID" value="LCD-09104"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EB-85A" prefix="J">
<description>&lt;h3&gt;EB-85A Connector&lt;/h3&gt;
Horizontal surface mount connector for the EB-85A/FV-M8 GPS receiver.

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Here is the connector we sell at SparkFun:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8297"&gt;Connector Horizontal SMD for EB-85A&lt;/a&gt; (GPS-08297)&lt;/li&gt;
&lt;li&gt;&lt;a href="http://www.sparkfun.com/datasheets/GPS/EB-85A-Connector.pdf"&gt;Datasheet&lt;/a&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;It was also used on this SparkFun product:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt; This connector is not on any currently live products, however it has been used on previously reitred products, so the package is proven.&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="EB-85A"/>
</gates>
<devices>
<device name="SMD" package="EB-85A">
<connects>
<connect gate="G$1" pin="BATT" pad="8"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="PPS" pad="7"/>
<connect gate="G$1" pin="RX1" pad="4"/>
<connect gate="G$1" pin="RX2" pad="6"/>
<connect gate="G$1" pin="TX1" pad="3"/>
<connect gate="G$1" pin="TX2" pad="5"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08435"/>
<attribute name="SF_ID" value="GPS-08297"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EM406" prefix="J">
<description>&lt;h3&gt;EM406 GPS Connector&lt;/h3&gt;
Here is a six pin vertical 1.0mm pitch connector. It is useful if you need something very tiny as a connection. These are not the standard JST type connectors we use on most of our boards, but are actually the much smaller JST-SH type.

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Here is the connector we sell at SparkFun:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/579"&gt;JST SH Vertical 6-Pin Connector - SMD&lt;/a&gt; (GPS-00579)&lt;/li&gt;
&lt;li&gt;&lt;a href="http://www.sparkfun.com/datasheets/GPS/EM406-SMDConnector-eSH.pdf"&gt;Datasheet&lt;/a&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;It was used on these SparkFun products:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11818"&gt;SparkFun GPS Breakout&lt;/a&gt; (BOB-11818)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12081"&gt;SparkFun Weather Shield&lt;/a&gt; (DEV-12081)&lt;/li&gt;
&lt;li&gt;And many, many other GPS related products.&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="EM406"/>
</gates>
<devices>
<device name="" package="1X06-1MM">
<connects>
<connect gate="G$1" pin="1PPS" pad="6"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="5"/>
<connect gate="G$1" pin="RX" pad="3"/>
<connect gate="G$1" pin="TX" pad="4"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08249"/>
<attribute name="SF_ID" value="GPS-00579"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EM408" prefix="J">
<description>&lt;h3&gt;EM-408 GPS receiver connector&lt;/h3&gt;
This is the mating connector for the EM408 GPS receiver. The EM408 connects to the board via a cable. Note, this connector footprint does not include the outline of the receiver.

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Here is the connector we sell at SparkFun:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8288"&gt;Connector Vertical SMD for EM408&lt;/a&gt; (GPS-08288)&lt;/li&gt;
&lt;li&gt;&lt;a href="http://www.sparkfun.com/datasheets/GPS/EM408-SMDConnector.pdf"&gt;Datasheet&lt;/a&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;It was also used on this SparkFun product:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt; This connector is not on any currently live products, however it has been used on previously reitred products, so the package is proven.&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special note:&lt;/b&gt; You should include the "EM408_Outline" device in your schematic if you are to use the EM408 in your design.</description>
<gates>
<gate name="G$1" symbol="EM408"/>
</gates>
<devices>
<device name="" package="1X05_1MM">
<connects>
<connect gate="G$1" pin="EN" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="RX" pad="3"/>
<connect gate="G$1" pin="TX" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08528"/>
<attribute name="SF_ID" value="GPS-08288"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6_PIN_SERIAL_CABLE" prefix="J">
<description>&lt;h3&gt;6-pin header connection for use with the "FTDI BASIC" pinout - CABLE SIDE.&lt;/h3&gt;
&lt;p&gt;&lt;/p&gt;

&lt;h3&gt;Also known as "Arduino Serial Program Header".&lt;/h3&gt;
&lt;p&gt;&lt;/p&gt;

This is used on a design to provide a 6-pin connection point for serial communication usually from a USB cable (D+/D-) to these headers (RX/TX). It also has the remaining pins necessary for programming in the Arduino evironment (DTR, GND, and sometimes VCC).

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Note, this device has "CABLE" in the name.&lt;/b&gt;  It is intended to be used on a design that usually lives on the end of your USB cable and prvides the converter chip (FTDI232 or FTDI231x) to commnicate serial RX/TX.
 
&lt;p&gt;&lt;/p&gt;
&lt;b&gt;The "sister" device, named "TARGET"&lt;/b&gt; is inteneded to be used on a design that contains a target micro-controller that you wish to program.
&lt;p&gt;&lt;/p&gt;
&lt;b&gt;You can populate with some of these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;&lt;/p&gt;
For reference (or to suit your programming needs) check out these designs:
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9716"&gt; SparkFun FTDI Basic Breakout - 5V&lt;/a&gt; (DEV-09716)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9873"&gt; SparkFun FTDI Basic Breakout - 3.3V&lt;/a&gt; (DEV-09873)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12935"&gt; SparkFun FTDI SmartBasic&lt;/a&gt; (DEV-12935)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13746"&gt; SparkFun Beefy 3 - FTDI Basic Breakout&lt;/a&gt; (DEV-13746)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="CONN_06"/>
</gates>
<devices>
<device name="PTH" package="FTDI_BASIC">
<connects>
<connect gate="G$1" pin="1" pad="DTR"/>
<connect gate="G$1" pin="2" pad="RXI"/>
<connect gate="G$1" pin="3" pad="TXO"/>
<connect gate="G$1" pin="4" pad="VCC"/>
<connect gate="G$1" pin="5" pad="CTS"/>
<connect gate="G$1" pin="6" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_01" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Single connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;
&lt;p&gt;&lt;/p&gt;

&lt;p&gt;&lt;/p&gt;
On any of the 0.1 inch spaced packages, you can populate with these:
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;
&lt;p&gt;&lt;/p&gt;
This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special notes:&lt;/b&gt;
&lt;p&gt; &lt;/p&gt;
SMTSO-256-ET is a "flush mount" nut for a 4-40 screw. We mostly use this on specialty testbeds; it is a nice way to connect hardware to your PCB at an adjustable hieght.
&lt;p&gt;&lt;/p&gt;
Also note, the SNAP packages are for using a snappable style connector. We sell a baggie of snaps and they are also used on two LilyPad designs:
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11347"&gt; Snap Assortment - 30 pack (male and female)&lt;/a&gt; (DEV-11347)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10941"&gt;LilyPad Arduino SimpleSnap&lt;/a&gt; (DEV-10941)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10940"&gt; LilyPad SimpleSnap Protoboard&lt;/a&gt; (DEV-10940)&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="CONN_01"/>
</gates>
<devices>
<device name="PTH_LONGPAD" package="1X01_LONGPAD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="1X01">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_2MM" package="1X01_2MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="OFFSET" package="1X01_OFFSET">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POGOPIN_HOLE_LARGE" package="1X01_POGOPIN_HOLE_0.061_DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POGOPIN_HOLE_0.58" package="1X01_POGOPIN_HOLE_0.58_DIA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SNAP-FEMALE" package="SNAP-FEMALE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SNAP-MALE" package="SNAP-MALE">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SPRING-CONN" package="SPRING-CONNECTOR">
<connects>
<connect gate="G$1" pin="1" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="PRT-11822"/>
</technology>
</technologies>
</device>
<device name="PTH_NO_SILK_KIT" package="1X01NS_KIT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_NO_SILK_YES_STOP" package="1X01_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMTSO-256-ET-0.165DIA" package="SMTSO-256-ET-0.165DIA">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="HW-08694"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_02" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special notes:&lt;/b&gt;

 Molex polarized connector foot print use with: PRT-08233 with associated crimp pins and housings.&lt;br&gt;&lt;br&gt;

2.54_SCREWTERM for use with  PRT-10571.&lt;br&gt;&lt;br&gt;

3.5mm Screw Terminal footprints for  PRT-08084&lt;br&gt;&lt;br&gt;

5mm Screw Terminal footprints for use with PRT-08432</description>
<gates>
<gate name="G$1" symbol="CONN_02"/>
</gates>
<devices>
<device name="" package="1X02">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR" package="MOLEX-1X2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="PRT-09918"/>
</technology>
</technologies>
</device>
<device name="3.5MM" package="SCREWTERMINAL-3.5MM-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08399"/>
</technology>
</technologies>
</device>
<device name="-JST-2MM-SMT" package="JST-2-SMD">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11443"/>
</technology>
</technologies>
</device>
<device name="PTH2" package="1X02_BIG">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="4UCON-15767" package="JST-2-SMD-VERT">
<connects>
<connect gate="G$1" pin="1" pad="GND"/>
<connect gate="G$1" pin="2" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="SCREWTERMINAL-5MM-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_SKU" value="PRT-08432"/>
</technology>
</technologies>
</device>
<device name="LOCK" package="1X02_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR_LOCK" package="MOLEX-1X2_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="PRT-09918"/>
</technology>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X02_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM_LOCK" package="SCREWTERMINAL-3.5MM-2_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08399"/>
</technology>
</technologies>
</device>
<device name="PTH3" package="1X02_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X02_NO_SILK" package="1X02_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PTH-2" package="JST-2-PTH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09863"/>
<attribute name="SKU" value="PRT-09914"/>
</technology>
</technologies>
</device>
<device name="PTH4" package="1X02_XTRA_BIG">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POGO_PIN_HOLES_ONLY" package="1X02_PP_HOLES_ONLY">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM-NO_SILK" package="SCREWTERMINAL-3.5MM-2-NS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08399"/>
</technology>
</technologies>
</device>
<device name="-JST-2-PTH-NO_SILK" package="JST-2-PTH-NS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PTH-2-KIT" package="JST-2-PTH-KIT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SPRING-2.54-RA" package="SPRINGTERMINAL-2.54MM-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2.54MM_SCREWTERM" package="1X02_2.54_SCREWTERM">
<connects>
<connect gate="G$1" pin="1" pad="P1"/>
<connect gate="G$1" pin="2" pad="P2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMALL_POKEHOME" package="1X02_POKEHOME">
<connects>
<connect gate="G$1" pin="1" pad="P1 P3"/>
<connect gate="G$1" pin="2" pad="P2 P4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-13512"/>
</technology>
</technologies>
</device>
<device name="PTH_RA_FEMALE" package="1X02_RA_PTH_FEMALE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-13700"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_03" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13875"&gt; Stackable Header - 3 Pin (Female, 0.1")&lt;/a&gt; (PRT-13875)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special notes:&lt;/b&gt;
&lt;p&gt; &lt;/p&gt;
&lt;p&gt; &lt;/p&gt; Molex polarized connector foot print use with SKU : PRT-08232 with associated crimp pins and housings.</description>
<gates>
<gate name="J$1" symbol="CONN_03"/>
</gates>
<devices>
<device name="" package="1X03">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="XXX-00000"/>
<attribute name="VALUE" value="455-1750-1-ND"/>
</technology>
</technologies>
</device>
<device name="POLAR" package="MOLEX-1X3">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08625"/>
<attribute name="SF_ID" value="PRT-08096"/>
</technology>
</technologies>
</device>
<device name="SCREW" package="SCREWTERMINAL-3.5MM-3">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08288"/>
<attribute name="SF_ID" value="PRT-08235"/>
</technology>
</technologies>
</device>
<device name="LOCK" package="1X03_LOCK">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X03_LOCK_LONGPADS">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR_LOCK" package="MOLEX-1X3_LOCK">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08625"/>
<attribute name="SF_ID" value="PRT-08096"/>
</technology>
</technologies>
</device>
<device name="SCREW_LOCK" package="SCREWTERMINAL-3.5MM-3_LOCK.007S">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08288"/>
<attribute name="SF_ID" value="PRT-08235"/>
</technology>
</technologies>
</device>
<device name="1X03_NO_SILK" package="1X03_NO_SILK">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X03_LONGPADS">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PTH" package="JST-3-PTH">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="WIRE-10037"/>
<attribute name="SF_ID" value="PRT-09915"/>
</technology>
</technologies>
</device>
<device name="POGO_PIN_HOLES_ONLY" package="1X03_PP_HOLES_ONLY">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SCREW-5MM" package="SCREWTERMINAL-5MM-3">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10134"/>
<attribute name="SF_SKU" value="PRT-08433"/>
</technology>
</technologies>
</device>
<device name="LOCK_NO_SILK" package="1X03_LOCK_NO_SILK">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-SMD" package="JST-3-SMD">
<connects>
<connect gate="J$1" pin="1" pad="3"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-12591"/>
<attribute name="VALUE" value="3-PIN SMD"/>
</technology>
</technologies>
</device>
<device name="SMD" package="1X03-1MM-RA">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD_RA_FEMALE" package="1X03_SMD_RA_FEMALE">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10926"/>
<attribute name="VALUE" value="1x3 RA Female .1&quot;"/>
</technology>
</technologies>
</device>
<device name="SMD_RA_MALE" package="1X03_SMD_RA_MALE">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10925"/>
</technology>
</technologies>
</device>
<device name="SMD_RA_MALE_POST" package="1X03_SMD_RA_MALE_POST">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PTH-VERT" package="JST-3-PTH-VERT">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-13230"/>
</technology>
</technologies>
</device>
<device name="1X03_SMD_RA_MALE_POST_SMALLER" package="1X03_SMD_RA_MALE_POST_SMALLER">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11912"/>
</technology>
</technologies>
</device>
<device name="1X03_SMD_RA_MALE_POST_SMALLEST" package="1X03_SMD_RA_MALE_POST_SMALLEST">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PTH-NS" package="JST-3-PTH-NS">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SCREW-NS" package="SCREWTERMINAL-3.5MM-3-NS">
<connects>
<connect gate="J$1" pin="1" pad="1"/>
<connect gate="J$1" pin="2" pad="2"/>
<connect gate="J$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_04X2" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="CONN_04X2"/>
</gates>
<devices>
<device name="" package="2X4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_05" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special notes:&lt;/b&gt;
&lt;p&gt; &lt;/p&gt; Molex polarized connector foot print use with SKU : PRT-08231 with associated crimp pins and housings. 1MM SMD Version SKU: PRT-10208</description>
<gates>
<gate name="G$1" symbol="CONN_05"/>
</gates>
<devices>
<device name="" package="1X05">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1.27MM" package="1X05_1.27MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X05_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X05_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_LONGPADS" package="1X05_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="1X05_1MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08528"/>
<attribute name="SF_ID" value="GPS-08288"/>
</technology>
</technologies>
</device>
<device name="SMD2" package="1X05_1MM_RA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NO_SILK" package="1X05_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST" package="JST-5-PTH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="PRT-09917"/>
</technology>
</technologies>
</device>
<device name="JST-VERT" package="JST-5-PTH-VERT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SCREW" package="SCREWTERMINAL-3.5MM-5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="Combine 8288+8399"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_05X2" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;h3&gt;For AVR SPI programming port, see special device with nice symbol: "AVR_SPI_PROG_5x2.dev"&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;You can populate with any combo of single row headers, but if you'd like an exact match, check these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/778"&gt; 2x5 AVR ICSP Male Header&lt;/a&gt; (PRT-00778)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8506"&gt; 2x5 Pin Shrouded Header&lt;/a&gt; (PRT-08506)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special note: the shrouded connector mates well with our 5x2 ribbon cables:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8535"&gt; 2x5 Pin IDC Ribbon Cable&lt;/a&gt; (PRT-08535)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="CONN_05X2"/>
</gates>
<devices>
<device name="PTH" package="2X5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08499"/>
<attribute name="SF_ID" value="PRT-0778"/>
</technology>
</technologies>
</device>
<device name="RA" package="2X5-RA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RAF" package="2X5-RAF">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SHD" package="2X5-SHROUDED">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08671"/>
<attribute name="SF_ID" value="PRT-08506"/>
</technology>
</technologies>
</device>
<device name="SHD_LOCK" package="2X5-SHROUDED_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08671"/>
<attribute name="SF_ID" value="PRT-08506"/>
</technology>
</technologies>
</device>
<device name="SHD_SMD" package="2X5-SHROUDED_SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09508"/>
</technology>
</technologies>
</device>
<device name="NO_SILK" package="2X5_NOSILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0.05_IN_PTH_SILK" package="2X5_PTH_SILK_.05">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SHD-NS" package="2X5-SHROUDED-NS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08671"/>
<attribute name="SF_ID" value="PRT-08506"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_06" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9280"&gt; Arduino Stackable Header - 6 Pin&lt;/a&gt; (PRT-09280)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="CONN_06"/>
</gates>
<devices>
<device name="SILK_FEMALE_PTH" package="1X06">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08437"/>
</technology>
</technologies>
</device>
<device name="POLAR" package="MOLEX-1X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RA" package="MOLEX-1X6-RA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="1X06-SMD_RA_MALE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08971"/>
<attribute name="VALUE" value="RA 6Pin SMD"/>
</technology>
</technologies>
</device>
<device name="LOCK" package="1X06_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X06_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR_LOCK" package="MOLEX-1X6_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RA_LOCK" package="MOLEX_1X6_RA_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FEMALE_LOCK" package="1X06_FEMALE_LOCK.010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X06_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM-6" package="SCREWTERMINAL-3.5MM-6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-FEMALE-V2" package="1X06-SMD-FEMALE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09668"/>
</technology>
</technologies>
</device>
<device name="POGOPIN_HOLES_ONLY" package="1X06_HOLES_ONLY">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08437"/>
</technology>
</technologies>
</device>
<device name="SMD-STRAIGHT-FEMALE" package="1X06_SMD_STRAIGHT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10203"/>
</technology>
</technologies>
</device>
<device name="SMD-STRAIGHT-ALT-FEMALE" package="1X06_SMD_STRAIGHT_ALT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10203"/>
</technology>
</technologies>
</device>
<device name="SMD-STRAIGHT-COMBO-FEMALE" package="1X06_SMD_STRAIGHT_COMBO">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10203"/>
</technology>
</technologies>
</device>
<device name="SMD_MALE" package="1X06_SMD_MALE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11293"/>
</technology>
</technologies>
</device>
<device name="SMD-1MM" package="1X06-1MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08249"/>
<attribute name="SF_ID" value="GPS-00579"/>
</technology>
</technologies>
</device>
<device name="NO_SILK_FEMALE_PTH" package="1X06_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08437"/>
</technology>
</technologies>
</device>
<device name="1.27MM" package="1X06_1.27MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NO_SILK_NO_POP" package="1X06_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2.5MM-6-90" package="1X06_SCREW_TERMINAL_BLOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_07" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special notes:&lt;/b&gt;
&lt;p&gt; &lt;/p&gt; Molex polarized connector foot print use with SKU : PRT-08231 with associated crimp pins and housings. 1MM SMD Version SKU: PRT-10208
&lt;p&gt;&lt;/p&gt;
NOTES ON THE VARIANTS LOCK and LOCK_LONGPADS...
This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place. You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers. Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,if you push a header all the way into place, it is covered up entirely on the bottom side.</description>
<gates>
<gate name="J1" symbol="CONN_07"/>
</gates>
<devices>
<device name="" package="1X07">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
<connect gate="J1" pin="5" pad="5"/>
<connect gate="J1" pin="6" pad="6"/>
<connect gate="J1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X07_LOCK">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
<connect gate="J1" pin="5" pad="5"/>
<connect gate="J1" pin="6" pad="6"/>
<connect gate="J1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X07_LOCK_LONGPADS">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
<connect gate="J1" pin="5" pad="5"/>
<connect gate="J1" pin="6" pad="6"/>
<connect gate="J1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X07_LONGPADS">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
<connect gate="J1" pin="5" pad="5"/>
<connect gate="J1" pin="6" pad="6"/>
<connect gate="J1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POGOPINS_HOLES_ONLY" package="1X07_HOLES_ONLY">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
<connect gate="J1" pin="5" pad="5"/>
<connect gate="J1" pin="6" pad="6"/>
<connect gate="J1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NO_SILK" package="1X07_NO_SILK">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
<connect gate="J1" pin="5" pad="5"/>
<connect gate="J1" pin="6" pad="6"/>
<connect gate="J1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM-7" package="SCREWTERMINAL-3.5MM-7">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
<connect gate="J1" pin="5" pad="5"/>
<connect gate="J1" pin="6" pad="6"/>
<connect gate="J1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_NO_SILK" package="1X07_LOCK_NO_SILK">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
<connect gate="J1" pin="5" pad="5"/>
<connect gate="J1" pin="6" pad="6"/>
<connect gate="J1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_08" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9279"&gt; Arduino Stackable Header - 8 Pin&lt;/a&gt; (PRT-09279)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special notes:&lt;/b&gt;
&lt;p&gt; &lt;/p&gt; Molex polarized connector foot print use with SKU : PRT-08231 with associated crimp pins and housings. 1MM SMD Version SKU: PRT-10208
&lt;p&gt;&lt;/p&gt;
NOTES ON THE VARIANTS LOCK and LOCK_LONGPADS...
This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place. You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers. Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,if you push a header all the way into place, it is covered up entirely on the bottom side.</description>
<gates>
<gate name="G$1" symbol="CONN_08"/>
</gates>
<devices>
<device name="&quot;" package="1X08">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08438"/>
</technology>
</technologies>
</device>
<device name="LOCK" package="1X08_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X08_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X08_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM-8" package="SCREWTERMINAL-3.5MM-8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-STRAIGHT-FEMALE" package="1X08_SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10204"/>
<attribute name="SF_ID" value="PRT-11543"/>
</technology>
</technologies>
</device>
<device name="SMD-STRAIGHT-ALT-FEMALE" package="1X08_SMD_ALT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10204"/>
<attribute name="SF_ID" value="PRT-11543"/>
</technology>
</technologies>
</device>
<device name="SMD-COMBO-FEMALE" package="1X08_SMD_COMBINED">
<connects>
<connect gate="G$1" pin="1" pad="1 1@2"/>
<connect gate="G$1" pin="2" pad="2 2@2"/>
<connect gate="G$1" pin="3" pad="3 3@2"/>
<connect gate="G$1" pin="4" pad="4 4@2"/>
<connect gate="G$1" pin="5" pad="5 5@2"/>
<connect gate="G$1" pin="6" pad="6 6@2"/>
<connect gate="G$1" pin="7" pad="7 7@2"/>
<connect gate="G$1" pin="8" pad="8 8@2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10204"/>
<attribute name="SF_ID" value="PRT-11543"/>
</technology>
</technologies>
</device>
<device name="BM08B-SRSS-TB" package="BM08B-SRSS-TB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10556"/>
</technology>
</technologies>
</device>
<device name="SMD-MALE" package="1X08_SMD_MALE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11292"/>
<attribute name="SF_ID" value="PRT-11541"/>
</technology>
</technologies>
</device>
<device name="NO_SILK_FEMALE_PTH" package="1X08_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08438"/>
</technology>
</technologies>
</device>
<device name="LOCK_NO_SILK" package="1X08_LOCK_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FEMALE_LOCK" package="1X08_FEMALE_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09233"/>
<attribute name="SF_ID" value="PRT-09279"/>
</technology>
</technologies>
</device>
<device name="SMD-COMBO-FEMALE_NC" package="1X08_SMD_COMBINED_NC">
<connects>
<connect gate="G$1" pin="1" pad="1 1@2"/>
<connect gate="G$1" pin="2" pad="2 2@2"/>
<connect gate="G$1" pin="3" pad="3 3@2"/>
<connect gate="G$1" pin="4" pad="4 4@2"/>
<connect gate="G$1" pin="5" pad="5 5@2"/>
<connect gate="G$1" pin="6" pad="6 6@2"/>
<connect gate="G$1" pin="7" pad="7 7@2"/>
<connect gate="G$1" pin="8" pad="8 8@2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10204"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_08X2" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;You can populate with any combo of single row headers, but if you'd like an exact match, check this:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13156"&gt; Header - 2x8 (Male, 0.1")&lt;/a&gt; (PRT-13156)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="J1" symbol="CONN_2X8"/>
</gates>
<devices>
<device name="_HEADER" package="2X8">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="10" pad="10"/>
<connect gate="J1" pin="11" pad="11"/>
<connect gate="J1" pin="12" pad="12"/>
<connect gate="J1" pin="13" pad="13"/>
<connect gate="J1" pin="14" pad="14"/>
<connect gate="J1" pin="15" pad="15"/>
<connect gate="J1" pin="16" pad="16"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
<connect gate="J1" pin="5" pad="5"/>
<connect gate="J1" pin="6" pad="6"/>
<connect gate="J1" pin="7" pad="7"/>
<connect gate="J1" pin="8" pad="8"/>
<connect gate="J1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_SHROUD" package="2X8-SHROUDED_LOCK">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="10" pad="10"/>
<connect gate="J1" pin="11" pad="11"/>
<connect gate="J1" pin="12" pad="12"/>
<connect gate="J1" pin="13" pad="13"/>
<connect gate="J1" pin="14" pad="14"/>
<connect gate="J1" pin="15" pad="15"/>
<connect gate="J1" pin="16" pad="16"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
<connect gate="J1" pin="5" pad="5"/>
<connect gate="J1" pin="6" pad="6"/>
<connect gate="J1" pin="7" pad="7"/>
<connect gate="J1" pin="8" pad="8"/>
<connect gate="J1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_09" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special notes:&lt;/b&gt;
&lt;p&gt; &lt;/p&gt; Molex polarized connector foot print use with SKU : PRT-08231 with associated crimp pins and housings. 1MM SMD Version SKU: PRT-10208
&lt;p&gt;&lt;/p&gt;
NOTES ON THE VARIANTS LOCK and LOCK_LONGPADS...
This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place. You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers. Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,if you push a header all the way into place, it is covered up entirely on the bottom side.</description>
<gates>
<gate name="J1" symbol="CONN_09"/>
</gates>
<devices>
<device name="" package="1X09">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
<connect gate="J1" pin="5" pad="5"/>
<connect gate="J1" pin="6" pad="6"/>
<connect gate="J1" pin="7" pad="7"/>
<connect gate="J1" pin="8" pad="8"/>
<connect gate="J1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X09_LOCK">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
<connect gate="J1" pin="5" pad="5"/>
<connect gate="J1" pin="6" pad="6"/>
<connect gate="J1" pin="7" pad="7"/>
<connect gate="J1" pin="8" pad="8"/>
<connect gate="J1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK-LONGPADS" package="1X09_LOCK_LONGPADS">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
<connect gate="J1" pin="5" pad="5"/>
<connect gate="J1" pin="6" pad="6"/>
<connect gate="J1" pin="7" pad="7"/>
<connect gate="J1" pin="8" pad="8"/>
<connect gate="J1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X09_LONGPADS">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
<connect gate="J1" pin="5" pad="5"/>
<connect gate="J1" pin="6" pad="6"/>
<connect gate="J1" pin="7" pad="7"/>
<connect gate="J1" pin="8" pad="8"/>
<connect gate="J1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NO_SILK" package="1X09_NO_SILK">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
<connect gate="J1" pin="5" pad="5"/>
<connect gate="J1" pin="6" pad="6"/>
<connect gate="J1" pin="7" pad="7"/>
<connect gate="J1" pin="8" pad="8"/>
<connect gate="J1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM-9" package="SCREWTERMINAL-3.5MM-9">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
<connect gate="J1" pin="5" pad="5"/>
<connect gate="J1" pin="6" pad="6"/>
<connect gate="J1" pin="7" pad="7"/>
<connect gate="J1" pin="8" pad="8"/>
<connect gate="J1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_10" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11376"&gt; Arduino Stackable Header - 10 Pin&lt;/a&gt; (PRT-11376)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special notes:&lt;/b&gt;
&lt;p&gt; &lt;/p&gt; Molex polarized connector foot print use with SKU : PRT-08231 with associated crimp pins and housings. 1MM SMD Version SKU: PRT-10208
&lt;p&gt;&lt;/p&gt;
NOTES ON THE VARIANTS LOCK and LOCK_LONGPADS...
This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place. You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers. Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,if you push a header all the way into place, it is covered up entirely on the bottom side.</description>
<gates>
<gate name="J1" symbol="CONN_10"/>
</gates>
<devices>
<device name="&quot;" package="1X10">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="10" pad="10"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
<connect gate="J1" pin="5" pad="5"/>
<connect gate="J1" pin="6" pad="6"/>
<connect gate="J1" pin="7" pad="7"/>
<connect gate="J1" pin="8" pad="8"/>
<connect gate="J1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11563"/>
</technology>
</technologies>
</device>
<device name="2MM" package="1X10-2MM">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="10" pad="10"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
<connect gate="J1" pin="5" pad="5"/>
<connect gate="J1" pin="6" pad="6"/>
<connect gate="J1" pin="7" pad="7"/>
<connect gate="J1" pin="8" pad="8"/>
<connect gate="J1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08875"/>
<attribute name="SF_ID" value="PRT-08272"/>
</technology>
</technologies>
</device>
<device name="2MMSMD" package="1X10-2MM-SMD">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="10" pad="10"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
<connect gate="J1" pin="5" pad="5"/>
<connect gate="J1" pin="6" pad="6"/>
<connect gate="J1" pin="7" pad="7"/>
<connect gate="J1" pin="8" pad="8"/>
<connect gate="J1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09042"/>
<attribute name="SF_ID" value="PRT-10030"/>
</technology>
</technologies>
</device>
<device name="LOCK" package="1X10_LOCK">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="10" pad="10"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
<connect gate="J1" pin="5" pad="5"/>
<connect gate="J1" pin="6" pad="6"/>
<connect gate="J1" pin="7" pad="7"/>
<connect gate="J1" pin="8" pad="8"/>
<connect gate="J1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X10_LOCK_LONGPADS">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="10" pad="10"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
<connect gate="J1" pin="5" pad="5"/>
<connect gate="J1" pin="6" pad="6"/>
<connect gate="J1" pin="7" pad="7"/>
<connect gate="J1" pin="8" pad="8"/>
<connect gate="J1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD_COMBO-FEMALE" package="1X10_SMD_COMBINED">
<connects>
<connect gate="J1" pin="1" pad="1A 1B"/>
<connect gate="J1" pin="10" pad="10A 10B"/>
<connect gate="J1" pin="2" pad="2A 2B"/>
<connect gate="J1" pin="3" pad="3A 3B"/>
<connect gate="J1" pin="4" pad="4A 4B"/>
<connect gate="J1" pin="5" pad="5A 5B"/>
<connect gate="J1" pin="6" pad="6A 6B"/>
<connect gate="J1" pin="7" pad="7A 7B"/>
<connect gate="J1" pin="8" pad="8A 8B"/>
<connect gate="J1" pin="9" pad="9A 9B"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11219"/>
</technology>
</technologies>
</device>
<device name="SMD_MALE" package="1X10_SMD_MALE">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="10" pad="10"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
<connect gate="J1" pin="5" pad="5"/>
<connect gate="J1" pin="6" pad="6"/>
<connect gate="J1" pin="7" pad="7"/>
<connect gate="J1" pin="8" pad="8"/>
<connect gate="J1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11291"/>
</technology>
</technologies>
</device>
<device name="NO_SILK_PTH_FEMALE" package="1X10_NO_SILK">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="10" pad="10"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
<connect gate="J1" pin="5" pad="5"/>
<connect gate="J1" pin="6" pad="6"/>
<connect gate="J1" pin="7" pad="7"/>
<connect gate="J1" pin="8" pad="8"/>
<connect gate="J1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11563"/>
</technology>
</technologies>
</device>
<device name="LOCK_NS" package="1X10_LOCK_NS">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="10" pad="10"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
<connect gate="J1" pin="5" pad="5"/>
<connect gate="J1" pin="6" pad="6"/>
<connect gate="J1" pin="7" pad="7"/>
<connect gate="J1" pin="8" pad="8"/>
<connect gate="J1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1.25MM_SMD" package="1X10-1.25MM-SMD">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="10" pad="10"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
<connect gate="J1" pin="5" pad="5"/>
<connect gate="J1" pin="6" pad="6"/>
<connect gate="J1" pin="7" pad="7"/>
<connect gate="J1" pin="8" pad="8"/>
<connect gate="J1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM-10" package="SCREWTERMINAL-3.5MM-10">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="10" pad="10"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
<connect gate="J1" pin="5" pad="5"/>
<connect gate="J1" pin="6" pad="6"/>
<connect gate="J1" pin="7" pad="7"/>
<connect gate="J1" pin="8" pad="8"/>
<connect gate="J1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_10X2" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special note about the "SPECIAL" package:&lt;/b&gt;
&lt;p&gt;&lt;/p&gt;
This was SPECIALLY designed to be used with our Graphic LCD Backpack.  Be sure you want to use this!  It is not only staggered on each line of header holes, but IT IS ALSO offset of the center point of the top and bottom lines by 5 mil.  This causes the headers to lock into place on the "standard" footprint on the LCD screen.  The extra squares on the tdocu layer are there simply to reference other pins (if you were to actually populate a longer header than ten long - this is what we do with the backpacks).</description>
<gates>
<gate name="G$1" symbol="CONN_10X2"/>
</gates>
<devices>
<device name="" package="2X10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2X10_LOCK" package="2X10_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SPECIAL" package="2X10_LOCK_SPECIAL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NOSILK" package="2X10_NOSILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_12" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special notes:&lt;/b&gt;
&lt;p&gt; &lt;/p&gt; Molex polarized connector foot print use with SKU : PRT-08231 with associated crimp pins and housings. 1MM SMD Version SKU: PRT-10208
&lt;p&gt;&lt;/p&gt;
NOTES ON THE VARIANTS LOCK and LOCK_LONGPADS...
This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place. You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers. Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,if you push a header all the way into place, it is covered up entirely on the bottom side.</description>
<gates>
<gate name="G$1" symbol="CONN_12"/>
</gates>
<devices>
<device name="" package="1X12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X12_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X12_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MACHINE-PIN_LOCK" package="1X12_MACHINE-PIN-HEADER_LOCK.004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09704"/>
</technology>
</technologies>
</device>
<device name="LONGPADS" package="1X12_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POGOPIN_HOLES_ONLY" package="1X12_HOLES_ONLY">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X12_NO_SILK_KIT" package="1X12_NO_SILK_KIT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NO_SILK" package="1X12_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_NO_SILK" package="1X12_LOCK_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SM_SQ_NO_SILK" package="1X12_SM_SQ_NOSILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_13" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special notes:&lt;/b&gt;
&lt;p&gt; &lt;/p&gt; Molex polarized connector foot print use with SKU : PRT-08231 with associated crimp pins and housings. 1MM SMD Version SKU: PRT-10208
&lt;p&gt;&lt;/p&gt;
NOTES ON THE VARIANTS LOCK and LOCK_LONGPADS...
This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place. You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers. Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,if you push a header all the way into place, it is covered up entirely on the bottom side.</description>
<gates>
<gate name="G$1" symbol="CONN_13"/>
</gates>
<devices>
<device name="" package="1X13">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X13-LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X13_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_NO_SILK" package="1X13_LOCK_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_14" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special notes:&lt;/b&gt;
&lt;p&gt; &lt;/p&gt; Molex polarized connector foot print use with SKU : PRT-08231 with associated crimp pins and housings. 1MM SMD Version SKU: PRT-10208
&lt;p&gt;&lt;/p&gt;
NOTES ON THE VARIANTS LOCK and LOCK_LONGPADS...
This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place. You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers. Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,if you push a header all the way into place, it is covered up entirely on the bottom side.</description>
<gates>
<gate name="G$1" symbol="CONN_14"/>
</gates>
<devices>
<device name="" package="1X14">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X14_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X14_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X14-LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NO_SILK" package="1X14_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_15" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special notes:&lt;/b&gt;
&lt;p&gt; &lt;/p&gt; Molex polarized connector foot print use with SKU : PRT-08231 with associated crimp pins and housings. 1MM SMD Version SKU: PRT-10208
&lt;p&gt;&lt;/p&gt;
NOTES ON THE VARIANTS LOCK and LOCK_LONGPADS...
This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place. You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers. Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,if you push a header all the way into place, it is covered up entirely on the bottom side.</description>
<gates>
<gate name="G$1" symbol="CONN_15"/>
</gates>
<devices>
<device name="" package="1X15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X15_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X15_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_NO_SILK" package="1X15_LOCK_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_17" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special notes:&lt;/b&gt;
&lt;p&gt; &lt;/p&gt; Molex polarized connector foot print use with SKU : PRT-08231 with associated crimp pins and housings. 1MM SMD Version SKU: PRT-10208
&lt;p&gt;&lt;/p&gt;
NOTES ON THE VARIANTS LOCK and LOCK_LONGPADS...
This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place. You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers. Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,if you push a header all the way into place, it is covered up entirely on the bottom side.</description>
<gates>
<gate name="G$1" symbol="CONN_17"/>
</gates>
<devices>
<device name="" package="1X17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NOSILK" package="1X17_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="KIT" package="1X17_NO_SILK_KIT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-12294"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_18" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special notes:&lt;/b&gt;
&lt;p&gt; &lt;/p&gt; Molex polarized connector foot print use with SKU : PRT-08231 with associated crimp pins and housings. 1MM SMD Version SKU: PRT-10208
&lt;p&gt;&lt;/p&gt;
NOTES ON THE VARIANTS LOCK and LOCK_LONGPADS...
This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place. You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers. Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,if you push a header all the way into place, it is covered up entirely on the bottom side.</description>
<gates>
<gate name="G$1" symbol="CONN_18"/>
</gates>
<devices>
<device name="SILK" package="1X18">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="1X18_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_20" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special notes:&lt;/b&gt;
&lt;p&gt; &lt;/p&gt; Molex polarized connector foot print use with SKU : PRT-08231 with associated crimp pins and housings. 1MM SMD Version SKU: PRT-10208
&lt;p&gt;&lt;/p&gt;
NOTES ON THE VARIANTS LOCK and LOCK_LONGPADS...
This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place. You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers. Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,if you push a header all the way into place, it is covered up entirely on the bottom side.
&lt;p&gt;&lt;/p&gt;
&lt;b&gt; Note about LOCK SPECIAL package:&lt;/b&gt;
&lt;p&gt;&lt;/p&gt;
This is just like the LOCK variant in that the holes are staggared by 5 mil, but except for the last two holes.  They are not altered from the "standard" footprint layout.  This is used for a special purpose on the layout of our Graphic LCD Backpack.  Make sure you want to use this device before selecting it for you project!</description>
<gates>
<gate name="G$1" symbol="CONN_20"/>
</gates>
<devices>
<device name="" package="1X20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X20_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X20_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SPECIAL" package="1X20_LOCK_SPECIAL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NO_SILK_KIT" package="1X20_NO_SILK_KIT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_NOSILK" package="1X20_LOCK_NOSILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09864"/>
</technology>
</technologies>
</device>
<device name="NOSILK" package="1X20_NOSILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_25" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special notes:&lt;/b&gt;
&lt;p&gt; &lt;/p&gt; Molex polarized connector foot print use with SKU : PRT-08231 with associated crimp pins and housings. 1MM SMD Version SKU: PRT-10208
&lt;p&gt;&lt;/p&gt;
NOTES ON THE VARIANTS LOCK and LOCK_LONGPADS...
This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place. You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers. Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,if you push a header all the way into place, it is covered up entirely on the bottom side.</description>
<gates>
<gate name="G$1" symbol="CONN_25"/>
</gates>
<devices>
<device name="" package="1X25">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X25_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X25_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_LONGPADS" package="1X25_LONGPAD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_27" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special notes:&lt;/b&gt;
&lt;p&gt; &lt;/p&gt; Molex polarized connector foot print use with SKU : PRT-08231 with associated crimp pins and housings. 1MM SMD Version SKU: PRT-10208
&lt;p&gt;&lt;/p&gt;
NOTES ON THE VARIANTS LOCK and LOCK_LONGPADS...
This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place. You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers. Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,if you push a header all the way into place, it is covered up entirely on the bottom side.</description>
<gates>
<gate name="G$1" symbol="CONN_27"/>
</gates>
<devices>
<device name="" package="1X27">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_29" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special notes:&lt;/b&gt;
&lt;p&gt; &lt;/p&gt; Molex polarized connector foot print use with SKU : PRT-08231 with associated crimp pins and housings. 1MM SMD Version SKU: PRT-10208
&lt;p&gt;&lt;/p&gt;
NOTES ON THE VARIANTS LOCK and LOCK_LONGPADS...
This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place. You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers. Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,if you push a header all the way into place, it is covered up entirely on the bottom side.</description>
<gates>
<gate name="G$1" symbol="CONN_29"/>
</gates>
<devices>
<device name="NO_SILK" package="1X29_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="1X29">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_30" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special notes:&lt;/b&gt;
&lt;p&gt; &lt;/p&gt; Molex polarized connector foot print use with SKU : PRT-08231 with associated crimp pins and housings. 1MM SMD Version SKU: PRT-10208
&lt;p&gt;&lt;/p&gt;
NOTES ON THE VARIANTS LOCK and LOCK_LONGPADS...
This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place. You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers. Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,if you push a header all the way into place, it is covered up entirely on the bottom side.</description>
<gates>
<gate name="G$1" symbol="CONN_30"/>
</gates>
<devices>
<device name="" package="1X30">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NO_SILK" package="1X30_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_40" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special notes:&lt;/b&gt;
&lt;p&gt; &lt;/p&gt; Molex polarized connector foot print use with SKU : PRT-08231 with associated crimp pins and housings. 1MM SMD Version SKU: PRT-10208
&lt;p&gt;&lt;/p&gt;
NOTES ON THE VARIANTS LOCK and LOCK_LONGPADS...
This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place. You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers. Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,if you push a header all the way into place, it is covered up entirely on the bottom side.</description>
<gates>
<gate name="G$1" symbol="CONN_40"/>
</gates>
<devices>
<device name="OFFSET" package="1X40_OFFSET">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="1X40">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-FPC" package="FPC05040-17204">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="10" pad="P$10"/>
<connect gate="G$1" pin="11" pad="P$11"/>
<connect gate="G$1" pin="12" pad="P$12"/>
<connect gate="G$1" pin="13" pad="P$13"/>
<connect gate="G$1" pin="14" pad="P$14"/>
<connect gate="G$1" pin="15" pad="P$15"/>
<connect gate="G$1" pin="16" pad="P$16"/>
<connect gate="G$1" pin="17" pad="P$17"/>
<connect gate="G$1" pin="18" pad="P$18"/>
<connect gate="G$1" pin="19" pad="P$19"/>
<connect gate="G$1" pin="2" pad="P$2"/>
<connect gate="G$1" pin="20" pad="P$20"/>
<connect gate="G$1" pin="21" pad="P$21"/>
<connect gate="G$1" pin="22" pad="P$22"/>
<connect gate="G$1" pin="23" pad="P$23"/>
<connect gate="G$1" pin="24" pad="P$24"/>
<connect gate="G$1" pin="25" pad="P$25"/>
<connect gate="G$1" pin="26" pad="P$26"/>
<connect gate="G$1" pin="27" pad="P$27"/>
<connect gate="G$1" pin="28" pad="P$28"/>
<connect gate="G$1" pin="29" pad="P$29"/>
<connect gate="G$1" pin="3" pad="P$3"/>
<connect gate="G$1" pin="30" pad="P$30"/>
<connect gate="G$1" pin="31" pad="P$31"/>
<connect gate="G$1" pin="32" pad="P$32"/>
<connect gate="G$1" pin="33" pad="P$33"/>
<connect gate="G$1" pin="34" pad="P$34"/>
<connect gate="G$1" pin="35" pad="P$35"/>
<connect gate="G$1" pin="36" pad="P$36"/>
<connect gate="G$1" pin="37" pad="P$37"/>
<connect gate="G$1" pin="38" pad="P$38"/>
<connect gate="G$1" pin="39" pad="P$39"/>
<connect gate="G$1" pin="4" pad="P$4"/>
<connect gate="G$1" pin="40" pad="P$40"/>
<connect gate="G$1" pin="5" pad="P$5"/>
<connect gate="G$1" pin="6" pad="P$6"/>
<connect gate="G$1" pin="7" pad="P$7"/>
<connect gate="G$1" pin="8" pad="P$8"/>
<connect gate="G$1" pin="9" pad="P$9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-14082"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAGJACK" prefix="J">
<description>&lt;h3&gt;MAGJACK: RJ-45 with LEDs&lt;/h3&gt;
This is a single port, RJ45 ethernet jacks with built in transformer (magnetics), status LEDs, and shielding.

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Here is the connector we sell at SparkFun:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8534"&gt;RJ45 Ethernet MagJack-Compatible&lt;/a&gt; (PRT-08534)&lt;/li&gt;
&lt;li&gt;&lt;a href="http://www.sparkfun.com/datasheets/Prototyping/MagJack.pdf"&gt;Datasheet&lt;/a&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;It is used on this SparkFun product:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13021"&gt;SparkFun RJ45 MagJack Breakout&lt;/a&gt; (BOB-13021)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="MAGJACK"/>
</gates>
<devices>
<device name="" package="MAGJACK">
<connects>
<connect gate="G$1" pin="GLED+" pad="11"/>
<connect gate="G$1" pin="GLED-" pad="12"/>
<connect gate="G$1" pin="NC@4" pad="4"/>
<connect gate="G$1" pin="NC@5" pad="5"/>
<connect gate="G$1" pin="RCT" pad="3"/>
<connect gate="G$1" pin="RD+" pad="1"/>
<connect gate="G$1" pin="RD-" pad="2"/>
<connect gate="G$1" pin="SHIELD@0" pad="M1"/>
<connect gate="G$1" pin="SHIELD@1" pad="M2"/>
<connect gate="G$1" pin="TCT" pad="6"/>
<connect gate="G$1" pin="TD+" pad="7"/>
<connect gate="G$1" pin="TD-" pad="8"/>
<connect gate="G$1" pin="YLED+" pad="9"/>
<connect gate="G$1" pin="YLED-" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09556"/>
<attribute name="SF_ID" value="PRT-08534"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAGJACK-POE" prefix="J">
<description>&lt;h3&gt;PoE compatible MagJack&lt;/h3&gt;
This is a simple RJ45 PoEthernet MagJack connector that can help connect you to the Internet with the ability to provide power. 

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Here is the connector we sell at SparkFun:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13606"&gt;RJ45 PoE MagJack&lt;/a&gt; (PRT-13606)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Note:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt; This connector is not on any currently live SparkFun products, however it has been used on previously reitred products, so the package is proven.&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="MAGJACK-POE"/>
</gates>
<devices>
<device name="" package="MAGJACK-POE">
<connects>
<connect gate="G$1" pin="GLED+" pad="13"/>
<connect gate="G$1" pin="GLED-" pad="14"/>
<connect gate="G$1" pin="RCT" pad="3"/>
<connect gate="G$1" pin="RD+" pad="1"/>
<connect gate="G$1" pin="RD-" pad="2"/>
<connect gate="G$1" pin="SHIELD@0" pad="GND0"/>
<connect gate="G$1" pin="SHIELD@1" pad="GND1"/>
<connect gate="G$1" pin="TCT" pad="4"/>
<connect gate="G$1" pin="TD+" pad="5"/>
<connect gate="G$1" pin="TD-" pad="6"/>
<connect gate="G$1" pin="V+" pad="9"/>
<connect gate="G$1" pin="V-" pad="10"/>
<connect gate="G$1" pin="YLED+" pad="11"/>
<connect gate="G$1" pin="YLED-" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10659"/>
<attribute name="SF_ID" value="PRT-13606"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OBDII" prefix="J">
<description>&lt;h3&gt;OBD-II Connector&lt;/h3&gt;
OBDII is an on board diagnostics standard that is used on a large variety of cars. 

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Here is the connector we sell at SparkFun:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9911"&gt;OBD-II connector&lt;/a&gt; (DEV-09911)&lt;/li&gt;
&lt;li&gt;&lt;a href="http://pinoutsguide.com/CarElectronics/car_obd2_pinout.shtml"&gt;Info and Pinout&lt;/a&gt; (sorry, no datasheet)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;We do not use this connector on any active designs, however, if you're looking for OBDII tech, please check out these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=obd"&gt;SparkFun OBD related products&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="OBDII"/>
</gates>
<devices>
<device name="" package="OBDII">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="BATTPOWER" pad="16"/>
<connect gate="G$1" pin="CANHIGH" pad="6"/>
<connect gate="G$1" pin="CANLOW" pad="14"/>
<connect gate="G$1" pin="CHASGND" pad="4"/>
<connect gate="G$1" pin="ISOK-LINE" pad="7"/>
<connect gate="G$1" pin="ISOL-LINE" pad="15"/>
<connect gate="G$1" pin="J1850BUS" pad="10"/>
<connect gate="G$1" pin="J1850BUS+" pad="2"/>
<connect gate="G$1" pin="SIGGND" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="DEV-09911"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC_ICSP_6_PIN" prefix="J">
<description>&lt;h3&gt;ISCP Programming connector for PICs&lt;/h3&gt;
This 6 pin header contains all the lines necessary for programming most PIC microcontrollers.

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Here is the connector we sell at SparkFun:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8094"&gt;Polarized Connectors - Header (6-Pin)&lt;/a&gt; (PRT-08094)&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;&lt;/p&gt;
&lt;b&gt;It is used on this SparkFun product:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11703"&gt;SparkFun UDB5 - PIC UAV Development Board&lt;/a&gt; (DEV-11703)&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Also, if you need a nice PIC programmer, please check these out:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9973"&gt;MPLAB PICkit 3&lt;/a&gt; (PGM-09973)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="ICSP-PIC"/>
</gates>
<devices>
<device name="" package="MOLEX-1X6">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PGC" pad="2"/>
<connect gate="G$1" pin="PGD" pad="3"/>
<connect gate="G$1" pin="PGM" pad="1"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VPP" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08046"/>
<attribute name="SF_ID" value="PRT-08094"/>
</technology>
</technologies>
</device>
<device name="POLAR_LOCK" package="MOLEX-1X6_LOCK">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PGC" pad="2"/>
<connect gate="G$1" pin="PGD" pad="3"/>
<connect gate="G$1" pin="PGM" pad="1"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VPP" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC_ICSP_MINI_5_PIN" prefix="J">
<description>&lt;b&gt;PIC-ICSP-Mini&lt;/b&gt;
Miniature 5-pin connection for temporary programming of PICs. Use this device in your design to save space.


&lt;h3&gt;Miniature ISCP Programming connector for PICs&lt;/h3&gt;
This 5 pin header contains all the lines necessary for programming most PIC microcontrollers. Use this device in your design to save space.

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Here is the connector we sell at SparkFun:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11264"&gt;5-Pin Mini ICSP Connector&lt;/a&gt; (PRT-11264)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;It is used on these SparkFun products:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/762"&gt;USB Bit Whacker - 18F2553 Development Board&lt;/a&gt; (DEV-00762)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/258"&gt;SparkFun Serial Enabled LCD Backpack&lt;/a&gt; (LCD-00258)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Also, if you need a nice PIC programmer, please check these out:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9973"&gt;MPLAB PICkit 3&lt;/a&gt; (PGM-09973)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="PIC-ISCP-MINI"/>
</gates>
<devices>
<device name="" package="PIC_ICSP_MINI_5_PIN">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="PGC" pad="5"/>
<connect gate="G$1" pin="PGD" pad="4"/>
<connect gate="G$1" pin="VCC" pad="2"/>
<connect gate="G$1" pin="VPP" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08314"/>
<attribute name="SF_ID" value="PRT-11264"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_12X2" prefix="J">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="CONN_12X2"/>
</gates>
<devices>
<device name="" package="2X12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_26X2" prefix="J">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="CONN_26X2"/>
</gates>
<devices>
<device name="" package="2X26">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="POWER_JACK" prefix="J">
<description>&lt;h3&gt;Power Jack Connector&lt;/h3&gt;
This is the standard 5.5mm barrel jack for power.&lt;br&gt;
The PTH is the most common, proven, reliable, footprint.&lt;br&gt;
The Slot footprint only works if the mill layer is transmitted to the PCB fab house so be warned.&lt;br&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Here are the connectors we sell at SparkFun:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/119"&gt;DC Barrel Power Jack/Connector&lt;/a&gt; (PRT-00119)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12748"&gt;DC Barrel Power Jack/Connector (SMD)&lt;/a&gt; (PRT-12748)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10811"&gt;DC Barrel Jack Adapter - Breadboard Compatible&lt;/a&gt; (PRT-10811)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;It is used on this SparkFun product (and many, many others):&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12757"&gt;SparkFun RedBoard - Programmed with Arduino&lt;/a&gt; (DEV-12757)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Also, if you need a mating power supply or connector, please check these out:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/298"&gt;Wall Adapter Power Supply - 9VDC 650mA&lt;/a&gt; (TOL-00298)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10287"&gt;DC Barrel Jack Adapter - Male&lt;/a&gt; (PRT-10287)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="POWERJACK"/>
</gates>
<devices>
<device name="SMD" package="POWER_JACK_SMD">
<connects>
<connect gate="G$1" pin="GND" pad="P$4"/>
<connect gate="G$1" pin="GNDBREAK" pad="GND"/>
<connect gate="G$1" pin="PWR" pad="VIN0"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08106"/>
<attribute name="SF_ID" value="PRT-12748"/>
<attribute name="VALUE" value="5.5x2.1mm Barrel"/>
</technology>
</technologies>
</device>
<device name="SLT" package="POWER_JACK_SLOT">
<connects>
<connect gate="G$1" pin="GND" pad="GND@2"/>
<connect gate="G$1" pin="GNDBREAK" pad="GND@1"/>
<connect gate="G$1" pin="PWR" pad="PWR"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="PRT-00119"/>
</technology>
</technologies>
</device>
<device name="" package="POWER_JACK_PTH">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GNDBREAK" pad="GNDBREAK"/>
<connect gate="G$1" pin="PWR" pad="PWR"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08197"/>
</technology>
</technologies>
</device>
<device name="PTH_SMD_COMBO" package="POWER_JACK_COMBO">
<connects>
<connect gate="G$1" pin="GND" pad="GND@1"/>
<connect gate="G$1" pin="GNDBREAK" pad="GND"/>
<connect gate="G$1" pin="PWR" pad="POWER"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_LOCK" package="POWER_JACK_PTH_LOCK">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GNDBREAK" pad="GNDBREAK"/>
<connect gate="G$1" pin="PWR" pad="PWR"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08197"/>
<attribute name="SF_ID" value="PRT-00119"/>
</technology>
</technologies>
</device>
<device name="TOE" package="POWER_JACK_SMD_OVERPASTE_TOE">
<connects>
<connect gate="G$1" pin="GND" pad="P$4"/>
<connect gate="G$1" pin="GNDBREAK" pad="GND"/>
<connect gate="G$1" pin="PWR" pad="VIN0"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08106"/>
<attribute name="SF_ID" value="PRT-12748"/>
</technology>
</technologies>
</device>
<device name="PTH_BREAD" package="POWER_JACK_PTH_BREAD">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GNDBREAK" pad="GNDBREAK"/>
<connect gate="G$1" pin="PWR" pad="PWR"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="PRT-10811"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PSP_CONNECTOR" prefix="J">
<description>&lt;h3&gt;Connector for the PlayStation Portable (PSP) screen ribbon cable&lt;/h3&gt;
We no longer sell the &lt;a href="https://www.sparkfun.com/products/retired/8335"&gt;screens&lt;/a&gt;, however we do still sell the connector.

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Here is the connector we sell at SparkFun:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8355"&gt;Color 24-Bit LCD 4.3" PSP Connector&lt;/a&gt; (LCD-08355)&lt;/li&gt;
&lt;li&gt;&lt;a href="http://www.sparkfun.com/datasheets/LCD/PSP-Connector.pdf"&gt;Datasheet&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="PSP_CONNECTOR"/>
</gates>
<devices>
<device name="" package="PSP_CONNECTOR">
<connects>
<connect gate="G$1" pin="AVDD" pad="AVDD"/>
<connect gate="G$1" pin="AVDD2" pad="AVDD2"/>
<connect gate="G$1" pin="B0" pad="B0"/>
<connect gate="G$1" pin="B1" pad="B1"/>
<connect gate="G$1" pin="B2" pad="B2"/>
<connect gate="G$1" pin="B3" pad="B3"/>
<connect gate="G$1" pin="B4" pad="B4"/>
<connect gate="G$1" pin="B5" pad="B5"/>
<connect gate="G$1" pin="B6" pad="B6"/>
<connect gate="G$1" pin="B7" pad="B7"/>
<connect gate="G$1" pin="CK" pad="CK"/>
<connect gate="G$1" pin="DISP" pad="DISP"/>
<connect gate="G$1" pin="G0" pad="G0"/>
<connect gate="G$1" pin="G1" pad="G1"/>
<connect gate="G$1" pin="G2" pad="G2"/>
<connect gate="G$1" pin="G3" pad="G3"/>
<connect gate="G$1" pin="G4" pad="G4"/>
<connect gate="G$1" pin="G5" pad="G5"/>
<connect gate="G$1" pin="G6" pad="G6"/>
<connect gate="G$1" pin="G7" pad="G7"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="GND3" pad="GND3"/>
<connect gate="G$1" pin="HSYNC" pad="HSYNC"/>
<connect gate="G$1" pin="NC" pad="NC"/>
<connect gate="G$1" pin="NC2" pad="NC2"/>
<connect gate="G$1" pin="R0" pad="R0"/>
<connect gate="G$1" pin="R1" pad="R1"/>
<connect gate="G$1" pin="R2" pad="R2"/>
<connect gate="G$1" pin="R3" pad="R3"/>
<connect gate="G$1" pin="R4" pad="R4"/>
<connect gate="G$1" pin="R5" pad="R5"/>
<connect gate="G$1" pin="R6" pad="R6"/>
<connect gate="G$1" pin="R7" pad="R7"/>
<connect gate="G$1" pin="TEST1" pad="TEST1"/>
<connect gate="G$1" pin="TEST2" pad="TEST2"/>
<connect gate="G$1" pin="TEST3" pad="TEST3"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
<connect gate="G$1" pin="VCC2" pad="VCC2"/>
<connect gate="G$1" pin="VSYNC" pad="VSYNC"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="LCD-08355"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PSP_TOUCH_CONNECTOR" prefix="J">
<description>&lt;h3&gt;4 pin Connector for the Color 24-Bit LCD 4.3" Play Station Portable (PSP) Touch Screen&lt;/h3&gt;
We no longer sell the &lt;a href="https://www.sparkfun.com/products/retired/8448"&gt;screens&lt;/a&gt;, however we do still sell the connector.

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Here is the connector we sell at SparkFun:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9104"&gt;Color 24-Bit LCD 4.3" PSP Touch Screen Connector&lt;/a&gt; (LCD-09104)&lt;/li&gt;
&lt;li&gt;&lt;a href="http://www.sparkfun.com/datasheets/LCD/PSPTouchConnector.pdf"&gt;Datasheet&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="PSP_TOUCH_CONNECTOR"/>
</gates>
<devices>
<device name="" package="PSP_TOUCH_CONNECTOR">
<connects>
<connect gate="G$1" pin="X1" pad="X1"/>
<connect gate="G$1" pin="X2" pad="X2"/>
<connect gate="G$1" pin="Y1" pad="Y1"/>
<connect gate="G$1" pin="Y2" pad="Y2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09139"/>
<attribute name="SF_ID" value="LCD-09104"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RJ11-6" prefix="J">
<description>&lt;h3&gt;RJ11 Jack - 6 pin&lt;/h3&gt;
Commonly found on CAT3 devices and some Microchip programmers.

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Here is the connector we sell at SparkFun:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/132"&gt;RJ11 6-Pin Connector&lt;/a&gt; (PRT-00132)&lt;/li&gt;
&lt;li&gt;&lt;a href="http://www.sparkfun.com/datasheets/Prototyping/Connectors/RJ11-Datasheet.pdf"&gt;Datasheet&lt;/a&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;It is used on this SparkFun product:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12081"&gt;SparkFun Weather Shield&lt;/a&gt; (DEV-12081)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8942"&gt;Weather Meters&lt;/a&gt; (SEN-08942)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="CONN_06"/>
</gates>
<devices>
<device name="" package="RJ11-6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08590"/>
<attribute name="SF_ID" value="PRT-00132"/>
<attribute name="VALUE" value="RJ11"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RJ45-8" prefix="J">
<description>&lt;h3&gt;RJ45 Jack - 8 pin&lt;/h3&gt;
Simple RJ45, 8-pin connection. Commonly used for Cat5, Cat5e, and Cat6 Ethernet cables.

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Here is the connector we sell at SparkFun:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/643"&gt;RJ45 8-Pin Connector&lt;/a&gt; (PRT-00643)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Prototyping/04908.pdf"&gt;Datasheet&lt;/a&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;It is used on this SparkFun product:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/716"&gt;SparkFun RJ45 Breakout&lt;/a&gt; (BOB-00716)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;br&gt;&lt;/br&gt;
Note, you may also be interested in the "MAGJACK" version of this. It is basically a RJ45 connector, but also has some status LEDs built into the connector housing. You can check that out in this library at the device named "MAGJACK.dev" and see these products online:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8534"&gt;RJ45 Ethernet MagJack-Compatible&lt;/a&gt; (PRT-08534)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13021"&gt;SparkFun RJ45 MagJack Breakout&lt;/a&gt; (BOB-13021)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="JP1" symbol="RJ45-8"/>
</gates>
<devices>
<device name="" package="RJ45-8">
<connects>
<connect gate="JP1" pin="1" pad="1"/>
<connect gate="JP1" pin="2" pad="2"/>
<connect gate="JP1" pin="3" pad="3"/>
<connect gate="JP1" pin="4" pad="4"/>
<connect gate="JP1" pin="5" pad="5"/>
<connect gate="JP1" pin="6" pad="6"/>
<connect gate="JP1" pin="7" pad="7"/>
<connect gate="JP1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08506"/>
<attribute name="SF_ID" value="PRT-00643"/>
<attribute name="VALUE" value="RJ45"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SCREENKEY_CONNECTOR" prefix="J">
<description>&lt;h3&gt;Connector for the ScreenKey&lt;/h3&gt;
This is a tiny, locking 14-pin FPC/FFC connector that mates with the TFT ScreenKeys and their displays. These connectors require a really minimal amount of force to close, which is great for the delicate wires they’re designed for. 
&lt;br&gt;&lt;/br&gt;
&lt;br&gt;&lt;/br&gt;
Unfortunately, we no longer sell the &lt;a href="https://www.sparkfun.com/products/retired/9366"&gt;ScreenKey TFT128&lt;/a&gt; or the  &lt;a href="https://www.sparkfun.com/products/retired/9380"&gt;TFT128 Display&lt;/a&gt;, however we do still sell the connector.


&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Here is the connector we sell at SparkFun:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9586"&gt;ScreenKey Mating Connector&lt;/a&gt; (PRT-09586)&lt;/li&gt;
&lt;li&gt;&lt;a href="hhttp://www.sparkfun.com/datasheets/Prototyping/Connectors/PRT-09586-e58605370.pdf"&gt;Datasheet&lt;/a&gt; (FH12-14S-0.5SH)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="SCREENKEYMATINGCONNECTOR"/>
</gates>
<devices>
<device name="" package="SCREENKEY_MATING_CONNECTOR">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09581"/>
<attribute name="SF_ID" value="PRT-09586"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SIMHOLDER" prefix="J" uservalue="yes">
<description>&lt;h3&gt;SIM Cellular Card Socket&lt;/h3&gt;
&lt;p&gt;SMT 6 pin standard connection. &lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/548”&gt;SIM Socket&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13120"&gt;SparkFun Cellular Shield - MG2639&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/573”&gt;SparkFun SIM Card Socket Breakout&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="J1" symbol="SIMHOLDER"/>
</gates>
<devices>
<device name="SIM" package="SIMHOLDER">
<connects>
<connect gate="J1" pin="CLK" pad="C3"/>
<connect gate="J1" pin="GND" pad="C5"/>
<connect gate="J1" pin="I/O" pad="C7"/>
<connect gate="J1" pin="RST" pad="C2"/>
<connect gate="J1" pin="VCC" pad="C1"/>
<connect gate="J1" pin="VPP" pad="C6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08536"/>
<attribute name="SF_ID" value="PRT-00548"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="U.FL" prefix="J" uservalue="yes">
<description>&lt;h3&gt;SMD Antenna Connector - U.FL&lt;/h3&gt;
&lt;p&gt;2mm height, 3.0mm x 3.0mm receptacle size. &lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13287"&gt;SparkFun WiFi Shield - ESP8266&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13231”&gt;SparkFun ESP8266 Thing&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/11420”&gt;SparkFun MiniGen - Pro Mini Signal Generator Shield&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="U.FL"/>
</gates>
<devices>
<device name="" package="U.FL">
<connects>
<connect gate="G$1" pin="GND@0" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="SIGNAL" pad="FEED"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09193"/>
<attribute name="SF_ID" value="WRL-09144"/>
<attribute name="VALUE" value="U.FL"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB_MINI-B" prefix="J">
<description>&lt;h3&gt;USB type Mini-B Connector&lt;/h3&gt;
&lt;p&gt;Breaks out 5th pin, and includes shield pins if needed.&lt;/p&gt;
&lt;p&gt;SparkFun Products:
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9716”&gt;SparkFun FTDI Basic Breakout&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11812”&gt;SparkFun XBee Explorer USB&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12757”&gt;SparkFun Redboard&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="USB-5PIN"/>
</gates>
<devices>
<device name="_SMT" package="USB-MINIB">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="ID" pad="ID"/>
<connect gate="G$1" pin="SHIELD" pad="S1 S2 S3 S4"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08193"/>
<attribute name="SF_ID" value="PRT-00587"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB_MICRO-B" prefix="J" uservalue="yes">
<description>&lt;h3&gt;USB Type Micro-B Connector&lt;/h3&gt;
&lt;p&gt;Male/female and PTH/SMT variants&lt;/p&gt;
&lt;p&gt;SparkFun Products:
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12035”&gt;SparkFun microB USB Breakout&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/10031”&gt;SparkFun USB microB Plug Breakout&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13231”&gt;SparkFun ESP8266 Thing&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="J1" symbol="USB-5PIN"/>
</gates>
<devices>
<device name="_MALE-VERT" package="USB_MICROB_VERTICAL">
<connects>
<connect gate="J1" pin="D+" pad="D+"/>
<connect gate="J1" pin="D-" pad="D-"/>
<connect gate="J1" pin="GND" pad="GND"/>
<connect gate="J1" pin="ID" pad="ID"/>
<connect gate="J1" pin="SHIELD" pad="SHLD1 SHLD2 SHLD3 SHLD4"/>
<connect gate="J1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09900"/>
</technology>
</technologies>
</device>
<device name="_FEMALE-SMT" package="USB-B-MICRO-SMD">
<connects>
<connect gate="J1" pin="D+" pad="D+"/>
<connect gate="J1" pin="D-" pad="D-"/>
<connect gate="J1" pin="GND" pad="GND"/>
<connect gate="J1" pin="ID" pad="ID"/>
<connect gate="J1" pin="SHIELD" pad="SHIELD1 SHIELD2 SHIELD3"/>
<connect gate="J1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11752"/>
</technology>
</technologies>
</device>
<device name="_SMT" package="USB-MICROB">
<connects>
<connect gate="J1" pin="D+" pad="D+"/>
<connect gate="J1" pin="D-" pad="D-"/>
<connect gate="J1" pin="GND" pad="GND"/>
<connect gate="J1" pin="ID" pad="ID"/>
<connect gate="J1" pin="SHIELD" pad="MT1 MT2 P$1 P$2"/>
<connect gate="J1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09505"/>
<attribute name="SF_ID" value="PRT-08533"/>
</technology>
</technologies>
</device>
<device name="REDUCED_PASTE" package="USB-B-MICRO-SMD_RED_PASTE">
<connects>
<connect gate="J1" pin="D+" pad="D+"/>
<connect gate="J1" pin="D-" pad="D-"/>
<connect gate="J1" pin="GND" pad="GND"/>
<connect gate="J1" pin="ID" pad="ID"/>
<connect gate="J1" pin="SHIELD" pad="SHIELD1 SHIELD2 SHIELD3"/>
<connect gate="J1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11752"/>
</technology>
</technologies>
</device>
<device name="_FEMALE-SMT-VERT" package="USB-B-MICRO-SMD_VERT">
<connects>
<connect gate="J1" pin="D+" pad="D+"/>
<connect gate="J1" pin="D-" pad="D-"/>
<connect gate="J1" pin="GND" pad="GND"/>
<connect gate="J1" pin="ID" pad="ID"/>
<connect gate="J1" pin="SHIELD" pad="P1 P2 P3"/>
<connect gate="J1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-13534"/>
<attribute name="VALUE" value="WM9734TR-ND "/>
</technology>
</technologies>
</device>
<device name="_HALF_PTH_MILL" package="USB-MICROB-PTH-MILL">
<connects>
<connect gate="J1" pin="D+" pad="D+"/>
<connect gate="J1" pin="D-" pad="D-"/>
<connect gate="J1" pin="GND" pad="GND"/>
<connect gate="J1" pin="ID" pad="ID"/>
<connect gate="J1" pin="SHIELD" pad="SHIELD SHIELD2 SHIELD3 SHIELD4 SHIELD5 SHIELD6 SHIELD7 SHIELD8 SHIELD9 SHIELD10"/>
<connect gate="J1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-13711"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ZIFSOCKET-28-3" prefix="J">
<description>&lt;h3&gt;ZIF Socket 28-Pin 0.3"&lt;/h3&gt;
&lt;p&gt;Lever-action ZIF socket for 28-pin ICs&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9175"&gt;ZIF Socket 28-Pin&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DIL-28-3"/>
</gates>
<devices>
<device name="&quot;" package="DIL28-3-ZIF_SOCKET">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$10" pad="10"/>
<connect gate="G$1" pin="P$11" pad="11"/>
<connect gate="G$1" pin="P$12" pad="12"/>
<connect gate="G$1" pin="P$13" pad="13"/>
<connect gate="G$1" pin="P$14" pad="14"/>
<connect gate="G$1" pin="P$15" pad="15"/>
<connect gate="G$1" pin="P$16" pad="16"/>
<connect gate="G$1" pin="P$17" pad="17"/>
<connect gate="G$1" pin="P$18" pad="18"/>
<connect gate="G$1" pin="P$19" pad="19"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$20" pad="20"/>
<connect gate="G$1" pin="P$21" pad="21"/>
<connect gate="G$1" pin="P$22" pad="22"/>
<connect gate="G$1" pin="P$23" pad="23"/>
<connect gate="G$1" pin="P$24" pad="24"/>
<connect gate="G$1" pin="P$25" pad="25"/>
<connect gate="G$1" pin="P$26" pad="26"/>
<connect gate="G$1" pin="P$27" pad="27"/>
<connect gate="G$1" pin="P$28" pad="28"/>
<connect gate="G$1" pin="P$3" pad="3"/>
<connect gate="G$1" pin="P$4" pad="4"/>
<connect gate="G$1" pin="P$5" pad="5"/>
<connect gate="G$1" pin="P$6" pad="6"/>
<connect gate="G$1" pin="P$7" pad="7"/>
<connect gate="G$1" pin="P$8" pad="8"/>
<connect gate="G$1" pin="P$9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10960"/>
<attribute name="SF_ID" value="PRT-09175"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RCA" prefix="J">
<description>&lt;h3&gt;RCA Jack connector&lt;/h3&gt;
This is a right angle RCA jack connecotr. Commonly used for video or audio.

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Here is the connector we sell at SparkFun:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8631"&gt;RCA Jack&lt;/a&gt; (PRT-08631)&lt;/li&gt;
&lt;li&gt;&lt;a href="http://www.sparkfun.com/datasheets/Prototyping/Connectors/RCA-Jack.pdf"&gt;Datasheet&lt;/a&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;It is not used on any active designs, however it was used on a couple retired products:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8826"&gt;RCA Jack Breakout [RETIRED]&lt;/a&gt; (PRT-08826)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9168"&gt;SparkFun On Screen Display Breakout - MAX7456 [RETIRED]&lt;/a&gt; (BOB-09168)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;You may also be interested in a cable:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11573"&gt;RCA Video Cable - 6'&lt;/a&gt; (CAB-11573)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="RCA"/>
</gates>
<devices>
<device name="" package="RCA">
<connects>
<connect gate="G$1" pin="PIN" pad="PIN"/>
<connect gate="G$1" pin="SHELL" pad="SHELL"/>
<connect gate="G$1" pin="SWITCH" pad="SWITCH"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09081"/>
<attribute name="SF_ID" value="PRT-08631"/>
</technology>
</technologies>
</device>
<device name="LOCK" package="RCA_LOCK">
<connects>
<connect gate="G$1" pin="PIN" pad="PIN"/>
<connect gate="G$1" pin="SHELL" pad="SHELL"/>
<connect gate="G$1" pin="SWITCH" pad="SWITCH"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_16" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special notes:&lt;/b&gt;
&lt;p&gt; &lt;/p&gt; Molex polarized connector foot print use with SKU : PRT-08231 with associated crimp pins and housings. 1MM SMD Version SKU: PRT-10208
&lt;p&gt;&lt;/p&gt;
NOTES ON THE VARIANTS LOCK and LOCK_LONGPADS...
This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place. You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers. Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,if you push a header all the way into place, it is covered up entirely on the bottom side.</description>
<gates>
<gate name="G$1" symbol="CONN_16"/>
</gates>
<devices>
<device name="" package="1X16">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X16_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X16_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MACHIINE-PIN_LOCK" package="1X16_MACHINE-PIN-HEADER_LOCK.004">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X16_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X16_NO_SILK" package="1X16_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X16_SM_SQ_NOSILK" package="1X16_SM_SQ_NOSILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_NO_SILK" package="1X16_LOCK_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_19" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special notes:&lt;/b&gt;
&lt;p&gt; &lt;/p&gt; Molex polarized connector foot print use with SKU : PRT-08231 with associated crimp pins and housings. 1MM SMD Version SKU: PRT-10208
&lt;p&gt;&lt;/p&gt;
NOTES ON THE VARIANTS LOCK and LOCK_LONGPADS...
This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place. You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers. Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,if you push a header all the way into place, it is covered up entirely on the bottom side.</description>
<gates>
<gate name="G$1" symbol="CONN_19"/>
</gates>
<devices>
<device name="" package="1X19">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X19_NO_SILK" package="1X19_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_11" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="CONN_11"/>
</gates>
<devices>
<device name="" package="1X11">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_1.27MM" package="1X11-1.27MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X11_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X11_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X11_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POGOPIN_HOLES_ONLY" package="1X11_HOLES_ONLY">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X11_NO_SILK" package="1X11_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X11_NO_SILK_KIT" package="1X11_NO_SILK_KIT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SD_CARD_SOCKET" prefix="J">
<description>&lt;h3&gt;SD Memory Card Connector (standard "large" size)&lt;/h3&gt;
Push-push normal type, CD enable, WP enable.

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Here is the connector we sell at SparkFun:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12769"&gt;SD/MMC Socket&lt;/a&gt; (PRT-12769)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Prototyping/19608.pdf"&gt;Datasheet&lt;/a&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;It is used on these SparkFun products:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12941"&gt;SparkFun SD/MMC Card Breakout&lt;/a&gt; (BOB-12941)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11468"&gt;SD Sniffer&lt;/a&gt; (TOL-11468)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="SDCARD-1"/>
</gates>
<devices>
<device name="" package="SD">
<connects>
<connect gate="G$1" pin="CD" pad="CD"/>
<connect gate="G$1" pin="CD/DAT3" pad="1"/>
<connect gate="G$1" pin="CLK" pad="5"/>
<connect gate="G$1" pin="CMD" pad="2"/>
<connect gate="G$1" pin="DAT0" pad="7"/>
<connect gate="G$1" pin="DAT1" pad="8"/>
<connect gate="G$1" pin="DAT2" pad="9"/>
<connect gate="G$1" pin="SH@1" pad="SH@1"/>
<connect gate="G$1" pin="SH@2" pad="SH@2"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS1" pad="3"/>
<connect gate="G$1" pin="VSS2" pad="6"/>
<connect gate="G$1" pin="WP" pad="WP"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11976"/>
<attribute name="SF_ID" value="PRT-12769"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MYDAQ" prefix="J">
<description>&lt;h3&gt;myDAQ&lt;/h3&gt;
This connecotr is used in the National Instruments myDAQ measurement and control tool ecosystem. Learn more at the &lt;a href="http://www.ni.com/mydaq/"&gt;myDAQ website&lt;/a&gt;. The connector is a 20pin 3.81mm spaced Female Right Angle Terminal Block (PTH).

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Sorry, we do not sell the connector as an individual part at SparkFun, howere here is a link to the datasheet:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="http://www.4uconnector.com/online/object/4udrawing/10458.pdf"&gt;Datasheet&lt;/a&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;It is used on this SparkFun product:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10705"&gt;SparkFun myDAQ Protoboard Kit&lt;/a&gt; (DEV-10705)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="MYDAQ_CONNECTOR"/>
</gates>
<devices>
<device name="" package="3.81MM_TERMINAL_BLOCK_FEMALE_LOCKING">
<connects>
<connect gate="G$1" pin="+15V" pad="1"/>
<connect gate="G$1" pin="-15V" pad="2"/>
<connect gate="G$1" pin="5V" pad="20"/>
<connect gate="G$1" pin="AGND_15V" pad="3"/>
<connect gate="G$1" pin="AGND_IO" pad="6"/>
<connect gate="G$1" pin="AI0+" pad="7"/>
<connect gate="G$1" pin="AI0-" pad="8"/>
<connect gate="G$1" pin="AI1+" pad="9"/>
<connect gate="G$1" pin="AN1-" pad="10"/>
<connect gate="G$1" pin="AO0" pad="4"/>
<connect gate="G$1" pin="AO1" pad="5"/>
<connect gate="G$1" pin="DGND" pad="19"/>
<connect gate="G$1" pin="DIO0" pad="11"/>
<connect gate="G$1" pin="DIO1" pad="12"/>
<connect gate="G$1" pin="DIO2" pad="13"/>
<connect gate="G$1" pin="DIO3" pad="14"/>
<connect gate="G$1" pin="DIO4" pad="15"/>
<connect gate="G$1" pin="DIO5" pad="16"/>
<connect gate="G$1" pin="DIO6" pad="17"/>
<connect gate="G$1" pin="DIO7" pad="18"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10450"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB_AB" prefix="J" uservalue="yes">
<description>&lt;h3&gt;USB Type AB Micro Connector&lt;/h3&gt;
&lt;p&gt;OTG-compatible. 5 pins, 3 shield pins&lt;/p&gt;
&lt;p&gt;SparkFun Products:
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13613”&gt;IOIO-OTG&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13664”&gt;SparkFun SAMD21 Mini Breakout&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="USB_AB"/>
</gates>
<devices>
<device name="_SMT" package="USB-AB-MICRO-SMD">
<connects>
<connect gate="G$1" pin="D+" pad="D+1"/>
<connect gate="G$1" pin="D-" pad="D-1"/>
<connect gate="G$1" pin="GND" pad="GND1"/>
<connect gate="G$1" pin="SHIELD" pad="SHLD1 SHLD2 SHLD3"/>
<connect gate="G$1" pin="USBID" pad="ID1"/>
<connect gate="G$1" pin="VBUS" pad="VBUS1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11794"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_03X2" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;You can populate with any combo of single row headers, but if you'd like an exact match, check these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12807"&gt; Header - 2x3 (Male, 0.1")&lt;/a&gt; (PRT-12807)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13010"&gt; Header - 2x3 (Female, 0.1")&lt;/a&gt; (PRT-13010)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10877"&gt; 2x3 Pin Shrouded Header&lt;/a&gt; (PRT-10877)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special note: the shrouded connector mates well with our 3x2 ribbon cables:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10651"&gt; Ribbon Crimp Connector - 6-pin (2x3, Female)&lt;/a&gt; (PRT-10651)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10646"&gt; Ribbon Cable - 6 wire (15ft)&lt;/a&gt; (PRT-10646)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="CONN_03X2"/>
</gates>
<devices>
<device name="SHROUD" package="2X3-SHROUDED">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10681"/>
<attribute name="SF_ID" value="PRT_10877"/>
</technology>
</technologies>
</device>
<device name="SMT" package="2X3_SMT_POSTS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11415"/>
</technology>
</technologies>
</device>
<device name="POGO_PINS" package="2X3_POGO">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
<connect gate="G$1" pin="3" pad="P$3"/>
<connect gate="G$1" pin="4" pad="P$4"/>
<connect gate="G$1" pin="5" pad="P$5"/>
<connect gate="G$1" pin="6" pad="P$6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="HW-11044"/>
</technology>
</technologies>
</device>
<device name="2X3_SILK_MALE_PTH" package="2X3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09701"/>
</technology>
</technologies>
</device>
<device name="NO_SILK" package="2X3-NS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FEMALE_SMD" package="2X3_SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11290"/>
</technology>
</technologies>
</device>
<device name="FEMALE" package="2X3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11566"/>
<attribute name="VALUE" value="FEMALE 2x3"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUDIO_JACK_TRRS" prefix="J">
<description>&lt;h3&gt;Audio Jack - 3.5mm TRRS (SMD)&lt;/h3&gt;
&lt;p&gt;This is a 3.5mm TRRS SMD audio jack. 
&lt;br&gt;TRRS connectors are the audio-style connectors that you see on some phones, MP3 players and development boards. 
&lt;br&gt;TRRS stands for “tip, ring, ring, sleeve,” which reflects that this  has three conductors and a ground. &lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12639”&gt;Audio Jack&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12968"&gt;mbed Starter Kit&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/11570&gt;SparkFun TRRS 3.5mm Jack Breakout&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="AUDIO-JACK3-TRRS"/>
</gates>
<devices>
<device name="SMD_RA" package="AUDIO_JACK_3.5MM_TRRS_SMD_RA">
<connects>
<connect gate="G$1" pin="EARTH" pad="EARTH"/>
<connect gate="G$1" pin="RING1" pad="RING1"/>
<connect gate="G$1" pin="RING2" pad="RING2"/>
<connect gate="G$1" pin="TIP" pad="TIP"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10676"/>
<attribute name="SF_ID" value="PRT-12639"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JST_2MM_MALE" prefix="J" uservalue="yes">
<description>&lt;h3&gt;JST 2MM MALE RA CONNECTOR&lt;/h3&gt;
Two pin, compact surface mount connector. Commonly used as a battery input connection point. We really like the solid locking feeling and high current rating on these small connectors. We use these all the time as battery connectors. Mates to single-cell LiPo batteries.

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Here is the connector we sell at SparkFun:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8612"&gt;JST Right Angle Connector - White&lt;/a&gt; (PRT-08612)&lt;/li&gt;
&lt;li&gt;&lt;a href="http://www.sparkfun.com/datasheets/Prototyping/Connectors/JST-Horizontal.pdf"&gt;Datasheet&lt;/a&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;It was used on these SparkFun products:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11214"&gt;SparkFun MOSFET Power Controller&lt;/a&gt; (PRT-11214)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13777"&gt;SparkFun Battery Babysitter - LiPo Battery Manager&lt;/a&gt; (PRT-13777)&lt;/li&gt;
&lt;li&gt;And many, many others that required a lipo battery connection.&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="JST_2MM_MALE"/>
</gates>
<devices>
<device name="" package="JST-2-SMD">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
<connect gate="G$1" pin="PAD1" pad="NC1"/>
<connect gate="G$1" pin="PAD2" pad="NC2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11443"/>
<attribute name="SF_ID" value="PRT-08612"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_13X2" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="CONN_13X2"/>
</gates>
<devices>
<device name="2X13" package="2X13">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JST_6_PIN_VERTICAL" prefix="J">
<description>&lt;h3&gt;JST 6 pin vertical connector&lt;/h3&gt;
Here is a six pin vertical 1.0mm pitch connector. It is useful if you need something very tiny as a connection. These are not the standard JST type connectors we use on most of our boards, but are actually the much smaller JST-SH type.

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Here is the connector we sell at SparkFun:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/579"&gt;JST SH Vertical 6-Pin Connector - SMD&lt;/a&gt; (GPS-00579)&lt;/li&gt;
&lt;li&gt;&lt;a href="http://www.sparkfun.com/datasheets/GPS/EM406-SMDConnector-eSH.pdf"&gt;Datasheet&lt;/a&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;It was used on these SparkFun products:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11818"&gt;SparkFun GPS Breakout&lt;/a&gt; (BOB-11818)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12081"&gt;SparkFun Weather Shield&lt;/a&gt; (DEV-12081)&lt;/li&gt;
&lt;li&gt;And many, many other GPS related products.&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="JST_6_1MM_VERT"/>
</gates>
<devices>
<device name="" package="JST-6-SMD-VERT-1.0MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08249"/>
<attribute name="SF_ID" value="GPS-00579"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_23" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special notes:&lt;/b&gt;
&lt;p&gt; &lt;/p&gt; Molex polarized connector foot print use with SKU : PRT-08231 with associated crimp pins and housings. 1MM SMD Version SKU: PRT-10208
&lt;p&gt;&lt;/p&gt;
NOTES ON THE VARIANTS LOCK and LOCK_LONGPADS...
This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place. You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers. Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,if you push a header all the way into place, it is covered up entirely on the bottom side.</description>
<gates>
<gate name="G$1" symbol="CONN_23"/>
</gates>
<devices>
<device name="" package="1X23">
<connects>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X23_LOCK">
<connects>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X23_LONGPADS">
<connects>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BINDING_POST" prefix="J">
<description>&lt;h3&gt;Binding Post&lt;/h3&gt;
&lt;p&gt;The component itself has an threaded, insulated body that goes through the board, with a small threaded metal stud coming off the back. 
&lt;p&gt; The intent of this package is that the post goes through a milled obling hole, and a small wire would be used to connect from the PCB pad to the metal contact on the post.
&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13006”&gt;SparkFun Decade Resistance Box&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12867”&gt;SparkFun Benchtop Power Board Kit&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/9739”&gt;Binding Post - Red&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/9740”&gt;Binding Post - Black&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BINDING_POST"/>
</gates>
<devices>
<device name="" package="BINDING_POST">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09675"/>
<attribute name="SF_ID" value="PRT-09740"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_06X2" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="CONN_06X2"/>
</gates>
<devices>
<device name="SMD_FEMALE" package="2X6_SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_FEMALE" package="2X6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-12423"/>
<attribute name="VALUE" value="2X6 FEMALE"/>
</technology>
</technologies>
</device>
<device name="NO_SILK" package="2X6_NOSILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="I2C_STANDARD" prefix="J" uservalue="yes">
<description>&lt;h3&gt;SparkFun I&lt;sup&gt;2&lt;/sup&gt;C Standard Pinout Header&lt;/h3&gt;
&lt;p&gt;SparkFun has standardized on a pinout for all I&lt;sup&gt;2&lt;/sup&gt;C based sensor breakouts.&lt;br&gt;
&lt;br&gt;
This pinout allows I&lt;sup&gt;2&lt;/sup&gt;C boards to be plugged directly into the headers on Arduino Uno compatible boards, and
to be daisy chained easily.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Example SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13676"&gt;SparkFun Atmospheric Sensor Breakout - BME280&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/11084”&gt;SparkFun Altitude/Pressure Sensor Breakout - MPL3115A2&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12785”&gt;SparkFun TOF Range Finder Sensor - VL6180&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="I2C_STANDARD"/>
</gates>
<devices>
<device name="" package="1X04">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_NO_SILK" package="1X04_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="QWIIC" package="JST04_1MM_RA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-13694"/>
<attribute name="VALUE" value="Qwiic Right Angle"/>
</technology>
</technologies>
</device>
<device name="UNITEST" package="1X04_UNITEST">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_20X2" prefix="J">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="CONN_20X2"/>
</gates>
<devices>
<device name="" package="2X20">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NOSILK" package="2X20_NOSILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SHROUDED" package="2X20_SHROUDED">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-12263"/>
<attribute name="SF_ID" value="CONN-12263"/>
</technology>
</technologies>
</device>
<device name="SHROUDED_SMT" package="2X20_SHROUDED_SMT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-13143"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BATTERY_CONN" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Battery Connectors&lt;/h3&gt;
&lt;p&gt;Various footprints for battery connections&lt;/p&gt;
&lt;p&gt;SparkFun Products:
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11864"&gt;Deans Connector -M/F Pair&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BATTERY_CONN"/>
</gates>
<devices>
<device name="_DEANS" package="DEANS">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="PRT-11864"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MICRO-SD_CARD_SOCKET" prefix="J">
<description>&lt;h3&gt;microSD Socket for Transflash&lt;/h3&gt;
&lt;p&gt;Push-push type µSD socket.  tDoc lines correctly indicate media card edge positions when inserting (unlocked, locked, depressed).
&lt;br&gt;
&lt;br&gt;&lt;b&gt;NOTE:&lt;/b&gt; CD1 and CD2 are connected internally, and the default detect state of the socket is detect pin to ground.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13660”&gt;WAV Trigger&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13262”&gt;CAN-Bus Shield&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13743”&gt;SparkFun Level Shifing microSD Breakout&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="J1" symbol="MICROSD"/>
</gates>
<devices>
<device name="PUSH-PUSH" package="MICRO-SD-SOCKET">
<connects>
<connect gate="J1" pin="CS" pad="CS"/>
<connect gate="J1" pin="DI" pad="DI"/>
<connect gate="J1" pin="DO" pad="DO"/>
<connect gate="J1" pin="GND" pad="GND"/>
<connect gate="J1" pin="NC" pad="RSV2"/>
<connect gate="J1" pin="RSV" pad="RSV1"/>
<connect gate="J1" pin="SCK" pad="SCLK"/>
<connect gate="J1" pin="SHIELD" pad="CD1"/>
<connect gate="J1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-07820"/>
</technology>
</technologies>
</device>
<device name="TINY" package="MICROSD_TINY">
<connects>
<connect gate="J1" pin="CS" pad="2"/>
<connect gate="J1" pin="DI" pad="3"/>
<connect gate="J1" pin="DO" pad="7"/>
<connect gate="J1" pin="GND" pad="6"/>
<connect gate="J1" pin="NC" pad="9"/>
<connect gate="J1" pin="RSV" pad="1 8"/>
<connect gate="J1" pin="SCK" pad="5"/>
<connect gate="J1" pin="SHIELD" pad="GND1 GND2 GND3 GND4 GND5 GND6"/>
<connect gate="J1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-13500"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEST-POINT" prefix="TP">
<description>&lt;h3&gt;SparkFun Test Points&lt;/h3&gt;
&lt;p&gt;Bare copper test points for troubleshooting or In-Circuit-Testing. These are used by our Production team for verifying production board runs using pogo-pins on test beds.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13284”&gt;SparkFun LSM9DS1 Breakout&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13714”&gt;SparkFun PSOC&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13879"&gt;SparkFun Load Cell Amplifier&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TEST-POINT"/>
</gates>
<devices>
<device name="2" package="PAD.02X.02">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3" package="PAD.03X.03">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3X5" package="PAD.03X.05">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3X4" package="PAD.03X.04">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TP_15TH_THRU" package="TP_15TH">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POGO_PTH" package="1X01_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CORTEX_JTAG_DEBUG" prefix="J">
<description>&lt;h3&gt;Cortex Debug Connector - 10 pin&lt;/h3&gt;
&lt;p&gt;Supports JTAG debug, Serial Wire debug, and Serial Wire Viewer.
PTH and SMD connector options available.&lt;/p&gt;
&lt;p&gt; &lt;ul&gt;&lt;a href=”http://infocenter.arm.com/help/topic/com.arm.doc.faqs/attached/13634/cortex_debug_connectors.pdf”&gt;General Connector Information&lt;/a&gt;
&lt;p&gt;&lt;b&gt; Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”http://www.digikey.com/product-detail/en/cnc-tech/3220-10-0100-00/1175-1627-ND/3883661”&gt;PTH Connector&lt;/a&gt; -via Digi-Key&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13229”&gt;SparkFun PSoc&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13810”&gt;SparkFun T&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="J1" symbol="CORTEX_DEBUG"/>
</gates>
<devices>
<device name="_PTH_NS" package="2X5-PTH-1.27MM-NO_SILK">
<connects>
<connect gate="J1" pin="!RESET" pad="10"/>
<connect gate="J1" pin="GND@3" pad="3"/>
<connect gate="J1" pin="GND@5" pad="5"/>
<connect gate="J1" pin="GNDDTCT" pad="9"/>
<connect gate="J1" pin="KEY" pad="7"/>
<connect gate="J1" pin="NC/TDI" pad="8"/>
<connect gate="J1" pin="SWDCLK/TCK" pad="4"/>
<connect gate="J1" pin="SWDIO/TMS" pad="2"/>
<connect gate="J1" pin="SWO/TDO" pad="6"/>
<connect gate="J1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_PTH" package="2X5-PTH-1.27MM">
<connects>
<connect gate="J1" pin="!RESET" pad="10"/>
<connect gate="J1" pin="GND@3" pad="3"/>
<connect gate="J1" pin="GND@5" pad="5"/>
<connect gate="J1" pin="GNDDTCT" pad="9"/>
<connect gate="J1" pin="KEY" pad="7"/>
<connect gate="J1" pin="NC/TDI" pad="8"/>
<connect gate="J1" pin="SWDCLK/TCK" pad="4"/>
<connect gate="J1" pin="SWDIO/TMS" pad="2"/>
<connect gate="J1" pin="SWO/TDO" pad="6"/>
<connect gate="J1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_SMD" package="2X5-SMD-1.27MM">
<connects>
<connect gate="J1" pin="!RESET" pad="10"/>
<connect gate="J1" pin="GND@3" pad="3"/>
<connect gate="J1" pin="GND@5" pad="5"/>
<connect gate="J1" pin="GNDDTCT" pad="9"/>
<connect gate="J1" pin="KEY" pad="7"/>
<connect gate="J1" pin="NC/TDI" pad="8"/>
<connect gate="J1" pin="SWDCLK/TCK" pad="4"/>
<connect gate="J1" pin="SWDIO/TMS" pad="2"/>
<connect gate="J1" pin="SWO/TDO" pad="6"/>
<connect gate="J1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-14503"/>
<attribute name="VALUE" value="JTAG"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VERNIER_ANALOG" prefix="J">
<description>&lt;h3&gt;British Telecom Connector - BTA (female)&lt;/h3&gt;
&lt;p&gt;This device is useful when designing a project that uses any of the analog sensors in the Vernier ecosystem (sensors and/or controllers)&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12858"&gt; SparkFun Vernier Interface Shield&lt;/a&gt; (DEV-12858)&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12753”&gt;British Telecom Connector - BTA (female)&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="VERNIER_ANALOG"/>
</gates>
<devices>
<device name="" package="BTA">
<connects>
<connect gate="G$1" pin="AN1" pad="1"/>
<connect gate="G$1" pin="AN2" pad="6"/>
<connect gate="G$1" pin="AUTOID" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VRES" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11653"/>
<attribute name="SF_ID" value="PRT-12753"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VERNIER_DIGITAL" prefix="J">
<description>&lt;h3&gt;British Telecom Connector - BTD Digital (female)&lt;/h3&gt;
&lt;p&gt;This device is useful when designing a project that uses any of the analog sensors in the Vernier ecosystem (sensors and/or controllers)&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12858"&gt; SparkFun Vernier Interface Shield&lt;/a&gt; (DEV-12858)&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12754”&gt;British Telecom Connector - BTD (female)&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;


&lt;p&gt;&lt;/p&gt;
&lt;b&gt; More information about the Vernier ecosystem can be found here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="http://www.vernier.com/engineering/arduino/"&gt; http://www.vernier.com/engineering/arduino/&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="VERNIER_DIGITAL"/>
</gates>
<devices>
<device name="" package="BTD">
<connects>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IO-0" pad="1"/>
<connect gate="G$1" pin="IO-1" pad="2"/>
<connect gate="G$1" pin="IO-2" pad="3"/>
<connect gate="G$1" pin="IO-3" pad="6"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11654"/>
<attribute name="SF_ID" value="PRT-12754"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUDIO_JACK_TRS_0.25&quot;_PTH_RA" prefix="J">
<description>&lt;h3&gt;Audio Jack, 1/4" TRS jack, horizontal, PTH, aka "Phono jack"&lt;/h3&gt;
&lt;p&gt;&lt;/p&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Find the connector here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11144"&gt; Audio Jack - 1/4" Stereo (right angle)&lt;/a&gt; (COM-11144)&lt;/li&gt;
&lt;li&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/General/JP-611%20DD.jpg"&gt;Datasheet&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;Note, although the datasheet and physical part are slightly different, this footprint was proven to mate well on the Proto Pedal.&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;
&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is used on these SparkFun Products: &lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13005"&gt;SparkFun TRS Jack Breakout - 1/4" Stereo&lt;/a&gt; (BOB-13005 )&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13124"&gt; SparkFun Proto Pedal - sorry bad link - product comming soon!&lt;/a&gt; (PRT-13124)&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="AUDIO-JACK4-TRS-NORMALED-GND-1"/>
</gates>
<devices>
<device name="" package="AUDIO_JACK_0.25&quot;_TRS_PTH_RA">
<connects>
<connect gate="G$1" pin="EARTH" pad="SLEEVE"/>
<connect gate="G$1" pin="EARTH-NORM" pad="SLEEVE-NORM"/>
<connect gate="G$1" pin="RING" pad="RING"/>
<connect gate="G$1" pin="RING-NORM" pad="RING-NORM"/>
<connect gate="G$1" pin="TIP" pad="TIP"/>
<connect gate="G$1" pin="TIP-NORM" pad="TIP-NORM"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-12339"/>
<attribute name="SF_ID" value="COM-11144"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIN5" prefix="J">
<description>&lt;h3&gt;DIN5 Connector - Female Right Angle (frequently used as a MIDI Jack connector)&lt;/h3&gt;
This type of connector and cable is frequently used for transmitting midi data (musical instrument digital interface). It is what you usually see on a keyboard or set of electronic drums. Learn more &lt;a href="https://en.wikipedia.org/wiki/MIDI"&gt;here&lt;/a&gt;.
&lt;br&gt;&lt;/br&gt;
&lt;br&gt;&lt;/br&gt;

For more information on the pinout and electrical specifications of MIDI communications, please see the following resource:

&lt;a href="https://www.midi.org/specifications/item/midi-din-electrical-specification"&gt;https://www.midi.org/specifications/item/midi-din-electrical-specification&lt;/a&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Here is the connector we sell at SparkFun:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9536"&gt;MIDI Connector - Female Right Angle&lt;/a&gt; (PRT-09536)&lt;/li&gt;
&lt;li&gt;&lt;a href="hhttp://www.sparkfun.com/datasheets/Prototyping/Connectors/MIDI-RA.pdf"&gt;Datasheet&lt;/a&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;It is used on this SparkFun product:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12898"&gt;SparkFun MIDI Shield&lt;/a&gt; (DEV-12898)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="5-PIN-DIN"/>
</gates>
<devices>
<device name="" package="DIN5-RA-PTH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09481"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB_A" prefix="J">
<description>&lt;h3&gt;USB-A Connector&lt;/h3&gt;
&lt;p&gt;Male and female variants, as well as PTH and SMT variants&lt;/p&gt;
&lt;p&gt;SparkFun Products:
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/11697”&gt;SparkFun XBee Explorer Dongle&lt;/a&gt; PTH Male&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12924”&gt;SparkFun MicroView-USB Programmer&lt;/a&gt; SMT Male&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12700”&gt;SparkFun USB Type A Female Breakout&lt;/a&gt; SMT Female&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="USB"/>
</gates>
<devices>
<device name="_PTH_MALE" package="USB-A-H">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="SHIELD" pad="SHLD1 SHLD2"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08367"/>
<attribute name="SF_ID" value="PRT-00437"/>
</technology>
</technologies>
</device>
<device name="_SMT_FEMALE_NS" package="USB-A-S-NOSILK-FEMALE">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="SHIELD" pad="SHLD1 SHLD2"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09520"/>
<attribute name="SF_ID" value="PRT-09011"/>
</technology>
</technologies>
</device>
<device name="_SMT_MALE" package="USB-A-SMT-MALE">
<connects>
<connect gate="G$1" pin="D+" pad="D+1"/>
<connect gate="G$1" pin="D-" pad="D-1"/>
<connect gate="G$1" pin="GND" pad="GND1"/>
<connect gate="G$1" pin="SHIELD" pad="SHLD1 SHLD2"/>
<connect gate="G$1" pin="VBUS" pad="VBUS1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11499"/>
</technology>
</technologies>
</device>
<device name="_SMT_FEMALE" package="USB-A-S-SILK-FEMALE">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="SHIELD" pad="SHLD1 SHLD2"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09520"/>
<attribute name="SF_ID" value="PRT-09011"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB_B" prefix="J">
<description>&lt;h3&gt;USB Type B Connector&lt;/h3&gt;
&lt;p&gt;&lt;/p&gt;
&lt;p&gt;SparkFun Products:
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13899”&gt;SparkFun Stepoko&lt;/a&gt; PTH&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="USB"/>
</gates>
<devices>
<device name="_PTH" package="USB-B-PTH">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="SHIELD" pad="SHLD1 SHLD2"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08278"/>
<attribute name="SF_ID" value="PRT-00139"/>
</technology>
</technologies>
</device>
<device name="_VERTICAL" package="USB_B_VERTICAL_PTH">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SHIELD" pad="5 6"/>
<connect gate="G$1" pin="VBUS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EDISON_CONNECTOR_FULL" prefix="J">
<description>&lt;h3&gt;Intel &amp;reg; Edison Hirose Connectors &lt;/h3&gt;
&lt;p&gt;DF40 Series 70 pin connector 3mm headers and sockets used on the SparkFun Edison Blocks.
&lt;p&gt;
Edison Daughter package includes layout for the Edison module itself, including mounting holes and antenna area marked.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13770”&gt;SparkFun ADC Edison Block&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13727”&gt;SparkFun Power Edison Block&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13045”&gt;SparkFun Base Edison Block&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13043”&gt;SparkFun Dual H-Bridge Edison Block&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13041”&gt;SparkFun microSD Edison Block&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="EDISON_CONNECTOR"/>
</gates>
<devices>
<device name="_MOUNTING_HOLES" package="EDISON_DAUGHTER">
<connects>
<connect gate="G$1" pin="1.8V" pad="12"/>
<connect gate="G$1" pin="3.3V@1" pad="8"/>
<connect gate="G$1" pin="3.3V@2" pad="10"/>
<connect gate="G$1" pin="DCIN" pad="14"/>
<connect gate="G$1" pin="FAULT" pad="19"/>
<connect gate="G$1" pin="FW_RCVR" pad="69"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="GND@3" pad="9"/>
<connect gate="G$1" pin="GND@4" pad="11"/>
<connect gate="G$1" pin="GND@5" pad="13"/>
<connect gate="G$1" pin="GND@6" pad="15"/>
<connect gate="G$1" pin="GP109_SPI_2_CLK" pad="55"/>
<connect gate="G$1" pin="GP110_SPI_2_FS0" pad="53"/>
<connect gate="G$1" pin="GP111_SPI_2_FS1" pad="51"/>
<connect gate="G$1" pin="GP114_SPI_2_RXD" pad="59"/>
<connect gate="G$1" pin="GP115_SPI_2_TXD" pad="57"/>
<connect gate="G$1" pin="GP128_UART_1_CTS" pad="65"/>
<connect gate="G$1" pin="GP129_UART_1_RTS" pad="63"/>
<connect gate="G$1" pin="GP12_PWM0" pad="35"/>
<connect gate="G$1" pin="GP130_UART_1_RX" pad="61"/>
<connect gate="G$1" pin="GP131_UART_1_TX" pad="46"/>
<connect gate="G$1" pin="GP134_UART_2_RX" pad="22"/>
<connect gate="G$1" pin="GP135_UART_2_TX" pad="27"/>
<connect gate="G$1" pin="GP13_PWM1" pad="33"/>
<connect gate="G$1" pin="GP14" pad="48"/>
<connect gate="G$1" pin="GP15" pad="42"/>
<connect gate="G$1" pin="GP165" pad="25"/>
<connect gate="G$1" pin="GP182_PWM2" pad="37"/>
<connect gate="G$1" pin="GP183_PWM3" pad="39"/>
<connect gate="G$1" pin="GP19_I2C_1_SCL" pad="41"/>
<connect gate="G$1" pin="GP20_I2C_1_SDA" pad="43"/>
<connect gate="G$1" pin="GP27_I2C_6_SCL" pad="45"/>
<connect gate="G$1" pin="GP28_I2C_6_SDA" pad="47"/>
<connect gate="G$1" pin="GP40_I2S_2_CLK" pad="52"/>
<connect gate="G$1" pin="GP41_I2S_2_FS" pad="54"/>
<connect gate="G$1" pin="GP42_I2S_2_RXD" pad="50"/>
<connect gate="G$1" pin="GP43_I2S_2_TXD" pad="56"/>
<connect gate="G$1" pin="GP44" pad="24"/>
<connect gate="G$1" pin="GP45" pad="26"/>
<connect gate="G$1" pin="GP46" pad="28"/>
<connect gate="G$1" pin="GP47" pad="30"/>
<connect gate="G$1" pin="GP48" pad="32"/>
<connect gate="G$1" pin="GP49" pad="34"/>
<connect gate="G$1" pin="GP77_SD_0_CD#" pad="60"/>
<connect gate="G$1" pin="GP78_SD_0_CLK" pad="58"/>
<connect gate="G$1" pin="GP79_SD_0_CMD" pad="62"/>
<connect gate="G$1" pin="GP80_SD_0_DAT0" pad="66"/>
<connect gate="G$1" pin="GP81_SD_0_DAT1" pad="70"/>
<connect gate="G$1" pin="GP82_SD_0_DAT2" pad="64"/>
<connect gate="G$1" pin="GP83_SD_0_DAT3" pad="68"/>
<connect gate="G$1" pin="GP84_SD_CLK_FB" pad="44"/>
<connect gate="G$1" pin="MSIC_SLP_CLK" pad="7"/>
<connect gate="G$1" pin="OSC_CLK_OUT_0" pad="67"/>
<connect gate="G$1" pin="PSW" pad="21"/>
<connect gate="G$1" pin="PWRBTN#" pad="17"/>
<connect gate="G$1" pin="RCVR_MODE" pad="31"/>
<connect gate="G$1" pin="RESET_OUT#" pad="36"/>
<connect gate="G$1" pin="USB_DN" pad="18"/>
<connect gate="G$1" pin="USB_DP" pad="16"/>
<connect gate="G$1" pin="USB_ID" pad="3"/>
<connect gate="G$1" pin="USB_VBUS" pad="20"/>
<connect gate="G$1" pin="VSYS@1" pad="2"/>
<connect gate="G$1" pin="VSYS@2" pad="4"/>
<connect gate="G$1" pin="VSYS@3" pad="6"/>
<connect gate="G$1" pin="V_VAT_BKUP" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_HEADER" package="DF40C-70DP-0.4(51)">
<connects>
<connect gate="G$1" pin="1.8V" pad="12"/>
<connect gate="G$1" pin="3.3V@1" pad="8"/>
<connect gate="G$1" pin="3.3V@2" pad="10"/>
<connect gate="G$1" pin="DCIN" pad="14"/>
<connect gate="G$1" pin="FAULT" pad="19"/>
<connect gate="G$1" pin="FW_RCVR" pad="69"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="GND@3" pad="9"/>
<connect gate="G$1" pin="GND@4" pad="11"/>
<connect gate="G$1" pin="GND@5" pad="13"/>
<connect gate="G$1" pin="GND@6" pad="15"/>
<connect gate="G$1" pin="GP109_SPI_2_CLK" pad="55"/>
<connect gate="G$1" pin="GP110_SPI_2_FS0" pad="53"/>
<connect gate="G$1" pin="GP111_SPI_2_FS1" pad="51"/>
<connect gate="G$1" pin="GP114_SPI_2_RXD" pad="59"/>
<connect gate="G$1" pin="GP115_SPI_2_TXD" pad="57"/>
<connect gate="G$1" pin="GP128_UART_1_CTS" pad="65"/>
<connect gate="G$1" pin="GP129_UART_1_RTS" pad="63"/>
<connect gate="G$1" pin="GP12_PWM0" pad="35"/>
<connect gate="G$1" pin="GP130_UART_1_RX" pad="61"/>
<connect gate="G$1" pin="GP131_UART_1_TX" pad="46"/>
<connect gate="G$1" pin="GP134_UART_2_RX" pad="22"/>
<connect gate="G$1" pin="GP135_UART_2_TX" pad="27"/>
<connect gate="G$1" pin="GP13_PWM1" pad="33"/>
<connect gate="G$1" pin="GP14" pad="48"/>
<connect gate="G$1" pin="GP15" pad="42"/>
<connect gate="G$1" pin="GP165" pad="25"/>
<connect gate="G$1" pin="GP182_PWM2" pad="37"/>
<connect gate="G$1" pin="GP183_PWM3" pad="39"/>
<connect gate="G$1" pin="GP19_I2C_1_SCL" pad="41"/>
<connect gate="G$1" pin="GP20_I2C_1_SDA" pad="43"/>
<connect gate="G$1" pin="GP27_I2C_6_SCL" pad="45"/>
<connect gate="G$1" pin="GP28_I2C_6_SDA" pad="47"/>
<connect gate="G$1" pin="GP40_I2S_2_CLK" pad="52"/>
<connect gate="G$1" pin="GP41_I2S_2_FS" pad="54"/>
<connect gate="G$1" pin="GP42_I2S_2_RXD" pad="50"/>
<connect gate="G$1" pin="GP43_I2S_2_TXD" pad="56"/>
<connect gate="G$1" pin="GP44" pad="24"/>
<connect gate="G$1" pin="GP45" pad="26"/>
<connect gate="G$1" pin="GP46" pad="28"/>
<connect gate="G$1" pin="GP47" pad="30"/>
<connect gate="G$1" pin="GP48" pad="32"/>
<connect gate="G$1" pin="GP49" pad="34"/>
<connect gate="G$1" pin="GP77_SD_0_CD#" pad="60"/>
<connect gate="G$1" pin="GP78_SD_0_CLK" pad="58"/>
<connect gate="G$1" pin="GP79_SD_0_CMD" pad="62"/>
<connect gate="G$1" pin="GP80_SD_0_DAT0" pad="66"/>
<connect gate="G$1" pin="GP81_SD_0_DAT1" pad="70"/>
<connect gate="G$1" pin="GP82_SD_0_DAT2" pad="64"/>
<connect gate="G$1" pin="GP83_SD_0_DAT3" pad="68"/>
<connect gate="G$1" pin="GP84_SD_CLK_FB" pad="44"/>
<connect gate="G$1" pin="MSIC_SLP_CLK" pad="7"/>
<connect gate="G$1" pin="OSC_CLK_OUT_0" pad="67"/>
<connect gate="G$1" pin="PSW" pad="21"/>
<connect gate="G$1" pin="PWRBTN#" pad="17"/>
<connect gate="G$1" pin="RCVR_MODE" pad="31"/>
<connect gate="G$1" pin="RESET_OUT#" pad="36"/>
<connect gate="G$1" pin="USB_DN" pad="18"/>
<connect gate="G$1" pin="USB_DP" pad="16"/>
<connect gate="G$1" pin="USB_ID" pad="3"/>
<connect gate="G$1" pin="USB_VBUS" pad="20"/>
<connect gate="G$1" pin="VSYS@1" pad="2"/>
<connect gate="G$1" pin="VSYS@2" pad="4"/>
<connect gate="G$1" pin="VSYS@3" pad="6"/>
<connect gate="G$1" pin="V_VAT_BKUP" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-12248"/>
</technology>
</technologies>
</device>
<device name="_SOCKET" package="DF40-XC-(X.X)-70DS-0.4V(51)">
<connects>
<connect gate="G$1" pin="1.8V" pad="12"/>
<connect gate="G$1" pin="3.3V@1" pad="8"/>
<connect gate="G$1" pin="3.3V@2" pad="10"/>
<connect gate="G$1" pin="DCIN" pad="14"/>
<connect gate="G$1" pin="FAULT" pad="19"/>
<connect gate="G$1" pin="FW_RCVR" pad="69"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="GND@3" pad="9"/>
<connect gate="G$1" pin="GND@4" pad="11"/>
<connect gate="G$1" pin="GND@5" pad="13"/>
<connect gate="G$1" pin="GND@6" pad="15"/>
<connect gate="G$1" pin="GP109_SPI_2_CLK" pad="55"/>
<connect gate="G$1" pin="GP110_SPI_2_FS0" pad="53"/>
<connect gate="G$1" pin="GP111_SPI_2_FS1" pad="51"/>
<connect gate="G$1" pin="GP114_SPI_2_RXD" pad="59"/>
<connect gate="G$1" pin="GP115_SPI_2_TXD" pad="57"/>
<connect gate="G$1" pin="GP128_UART_1_CTS" pad="65"/>
<connect gate="G$1" pin="GP129_UART_1_RTS" pad="63"/>
<connect gate="G$1" pin="GP12_PWM0" pad="35"/>
<connect gate="G$1" pin="GP130_UART_1_RX" pad="61"/>
<connect gate="G$1" pin="GP131_UART_1_TX" pad="46"/>
<connect gate="G$1" pin="GP134_UART_2_RX" pad="22"/>
<connect gate="G$1" pin="GP135_UART_2_TX" pad="27"/>
<connect gate="G$1" pin="GP13_PWM1" pad="33"/>
<connect gate="G$1" pin="GP14" pad="48"/>
<connect gate="G$1" pin="GP15" pad="42"/>
<connect gate="G$1" pin="GP165" pad="25"/>
<connect gate="G$1" pin="GP182_PWM2" pad="37"/>
<connect gate="G$1" pin="GP183_PWM3" pad="39"/>
<connect gate="G$1" pin="GP19_I2C_1_SCL" pad="41"/>
<connect gate="G$1" pin="GP20_I2C_1_SDA" pad="43"/>
<connect gate="G$1" pin="GP27_I2C_6_SCL" pad="45"/>
<connect gate="G$1" pin="GP28_I2C_6_SDA" pad="47"/>
<connect gate="G$1" pin="GP40_I2S_2_CLK" pad="52"/>
<connect gate="G$1" pin="GP41_I2S_2_FS" pad="54"/>
<connect gate="G$1" pin="GP42_I2S_2_RXD" pad="50"/>
<connect gate="G$1" pin="GP43_I2S_2_TXD" pad="56"/>
<connect gate="G$1" pin="GP44" pad="24"/>
<connect gate="G$1" pin="GP45" pad="26"/>
<connect gate="G$1" pin="GP46" pad="28"/>
<connect gate="G$1" pin="GP47" pad="30"/>
<connect gate="G$1" pin="GP48" pad="32"/>
<connect gate="G$1" pin="GP49" pad="34"/>
<connect gate="G$1" pin="GP77_SD_0_CD#" pad="60"/>
<connect gate="G$1" pin="GP78_SD_0_CLK" pad="58"/>
<connect gate="G$1" pin="GP79_SD_0_CMD" pad="62"/>
<connect gate="G$1" pin="GP80_SD_0_DAT0" pad="66"/>
<connect gate="G$1" pin="GP81_SD_0_DAT1" pad="70"/>
<connect gate="G$1" pin="GP82_SD_0_DAT2" pad="64"/>
<connect gate="G$1" pin="GP83_SD_0_DAT3" pad="68"/>
<connect gate="G$1" pin="GP84_SD_CLK_FB" pad="44"/>
<connect gate="G$1" pin="MSIC_SLP_CLK" pad="7"/>
<connect gate="G$1" pin="OSC_CLK_OUT_0" pad="67"/>
<connect gate="G$1" pin="PSW" pad="21"/>
<connect gate="G$1" pin="PWRBTN#" pad="17"/>
<connect gate="G$1" pin="RCVR_MODE" pad="31"/>
<connect gate="G$1" pin="RESET_OUT#" pad="36"/>
<connect gate="G$1" pin="USB_DN" pad="18"/>
<connect gate="G$1" pin="USB_DP" pad="16"/>
<connect gate="G$1" pin="USB_ID" pad="3"/>
<connect gate="G$1" pin="USB_VBUS" pad="20"/>
<connect gate="G$1" pin="VSYS@1" pad="2"/>
<connect gate="G$1" pin="VSYS@2" pad="4"/>
<connect gate="G$1" pin="VSYS@3" pad="6"/>
<connect gate="G$1" pin="V_VAT_BKUP" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-12247"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RASPBERRYPI-40-PIN-GPIO" prefix="J">
<description>&lt;h3&gt;Raspberry Pi GPIO Header&lt;/h3&gt;
&lt;p&gt;2x20 pin connector, as found on B, B+, A+ models. Both shrouded PTH and SMT versions available.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13054”&gt;GPIO Shrouded Header&lt;/a&gt;- PTH&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13717”&gt;SparkFun Pi Wedge (Preassembled)&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RASPBERRYPI_40_PIN_GPIO"/>
</gates>
<devices>
<device name="_PTH" package="2X20_SHROUDED">
<connects>
<connect gate="G$1" pin="3.3V" pad="1 17"/>
<connect gate="G$1" pin="5V" pad="2 4"/>
<connect gate="G$1" pin="CE0" pad="24"/>
<connect gate="G$1" pin="CE1" pad="26"/>
<connect gate="G$1" pin="GND" pad="6 9 14 20 25 30 34 39"/>
<connect gate="G$1" pin="GP12" pad="32"/>
<connect gate="G$1" pin="GP13" pad="33"/>
<connect gate="G$1" pin="GP16" pad="36"/>
<connect gate="G$1" pin="GP17" pad="11"/>
<connect gate="G$1" pin="GP18#" pad="12"/>
<connect gate="G$1" pin="GP19" pad="35"/>
<connect gate="G$1" pin="GP20" pad="38"/>
<connect gate="G$1" pin="GP21" pad="40"/>
<connect gate="G$1" pin="GP22" pad="15"/>
<connect gate="G$1" pin="GP23" pad="16"/>
<connect gate="G$1" pin="GP24" pad="18"/>
<connect gate="G$1" pin="GP25" pad="22"/>
<connect gate="G$1" pin="GP26" pad="37"/>
<connect gate="G$1" pin="GP27" pad="13"/>
<connect gate="G$1" pin="GP4" pad="7"/>
<connect gate="G$1" pin="GP5" pad="29"/>
<connect gate="G$1" pin="GP6" pad="31"/>
<connect gate="G$1" pin="ID_SC" pad="28"/>
<connect gate="G$1" pin="ID_SD" pad="27"/>
<connect gate="G$1" pin="MISO" pad="21"/>
<connect gate="G$1" pin="MOSI" pad="19"/>
<connect gate="G$1" pin="RXI" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SCLK" pad="23"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="TXO" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-12263"/>
<attribute name="SF_ID" value="PRT-13054"/>
</technology>
</technologies>
</device>
<device name="_SMT" package="2X20_SHROUDED_SMT">
<connects>
<connect gate="G$1" pin="3.3V" pad="1 17"/>
<connect gate="G$1" pin="5V" pad="2 4"/>
<connect gate="G$1" pin="CE0" pad="24"/>
<connect gate="G$1" pin="CE1" pad="26"/>
<connect gate="G$1" pin="GND" pad="6 9 14 20 25 30 34 39"/>
<connect gate="G$1" pin="GP12" pad="32"/>
<connect gate="G$1" pin="GP13" pad="33"/>
<connect gate="G$1" pin="GP16" pad="36"/>
<connect gate="G$1" pin="GP17" pad="11"/>
<connect gate="G$1" pin="GP18#" pad="12"/>
<connect gate="G$1" pin="GP19" pad="35"/>
<connect gate="G$1" pin="GP20" pad="38"/>
<connect gate="G$1" pin="GP21" pad="40"/>
<connect gate="G$1" pin="GP22" pad="15"/>
<connect gate="G$1" pin="GP23" pad="16"/>
<connect gate="G$1" pin="GP24" pad="18"/>
<connect gate="G$1" pin="GP25" pad="22"/>
<connect gate="G$1" pin="GP26" pad="37"/>
<connect gate="G$1" pin="GP27" pad="13"/>
<connect gate="G$1" pin="GP4" pad="7"/>
<connect gate="G$1" pin="GP5" pad="29"/>
<connect gate="G$1" pin="GP6" pad="31"/>
<connect gate="G$1" pin="ID_SC" pad="28"/>
<connect gate="G$1" pin="ID_SD" pad="27"/>
<connect gate="G$1" pin="MISO" pad="21"/>
<connect gate="G$1" pin="MOSI" pad="19"/>
<connect gate="G$1" pin="RXI" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SCLK" pad="23"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="TXO" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-13143"/>
</technology>
</technologies>
</device>
<device name="_PTH_NO_SHROUD" package="2X20">
<connects>
<connect gate="G$1" pin="3.3V" pad="1 17"/>
<connect gate="G$1" pin="5V" pad="2 4"/>
<connect gate="G$1" pin="CE0" pad="24"/>
<connect gate="G$1" pin="CE1" pad="26"/>
<connect gate="G$1" pin="GND" pad="6 9 14 20 25 30 34 39"/>
<connect gate="G$1" pin="GP12" pad="32"/>
<connect gate="G$1" pin="GP13" pad="33"/>
<connect gate="G$1" pin="GP16" pad="36"/>
<connect gate="G$1" pin="GP17" pad="11"/>
<connect gate="G$1" pin="GP18#" pad="12"/>
<connect gate="G$1" pin="GP19" pad="35"/>
<connect gate="G$1" pin="GP20" pad="38"/>
<connect gate="G$1" pin="GP21" pad="40"/>
<connect gate="G$1" pin="GP22" pad="15"/>
<connect gate="G$1" pin="GP23" pad="16"/>
<connect gate="G$1" pin="GP24" pad="18"/>
<connect gate="G$1" pin="GP25" pad="22"/>
<connect gate="G$1" pin="GP26" pad="37"/>
<connect gate="G$1" pin="GP27" pad="13"/>
<connect gate="G$1" pin="GP4" pad="7"/>
<connect gate="G$1" pin="GP5" pad="29"/>
<connect gate="G$1" pin="GP6" pad="31"/>
<connect gate="G$1" pin="ID_SC" pad="28"/>
<connect gate="G$1" pin="ID_SD" pad="27"/>
<connect gate="G$1" pin="MISO" pad="21"/>
<connect gate="G$1" pin="MOSI" pad="19"/>
<connect gate="G$1" pin="RXI" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SCLK" pad="23"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="TXO" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="QWIIC_CONNECTOR" prefix="J" uservalue="yes">
<description>&lt;h3&gt;SparkFun I&lt;sup&gt;2&lt;/sup&gt;C Standard Qwiic Connector&lt;/h3&gt;
An SMD 1mm pitch JST connector makes it easy and quick (get it? Qwiic?) to connect I&lt;sup&gt;2&lt;/sup&gt;C devices to each other. The &lt;a href=”http://www.sparkfun.com/qwiic”&gt;Qwiic system&lt;/a&gt; enables fast and solderless connection between popular platforms and various sensors and actuators.

&lt;br&gt;&lt;br&gt;

We carry &lt;a href=”https://www.sparkfun.com/products/14204”&gt;200mm&lt;/a&gt;, &lt;a href=”https://www.sparkfun.com/products/14205”&gt;100mm&lt;/a&gt;, &lt;a href=”https://www.sparkfun.com/products/14206”&gt;50mm&lt;/a&gt;, and &lt;a href=”https://www.sparkfun.com/products/14207”&gt;breadboard friendly&lt;/a&gt; Qwiic cables. We also offer &lt;a href=”https://www.sparkfun.com/products/14323”&gt;10 pcs strips&lt;/a&gt; the SMD connectors.</description>
<gates>
<gate name="G$1" symbol="I2C_STANDARD"/>
</gates>
<devices>
<device name="JS-1MM" package="JST04_1MM_RA">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-13694"/>
<attribute name="VALUE" value=""/>
</technology>
</technologies>
</device>
<device name="SR" package="JST04_1MM_RA_STRESSRELIEF">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="JST04_1MM_VERT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-14483"/>
<attribute name="VALUE" value="Vertical Qwiic Connector"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="U.FL2PIN" prefix="J" uservalue="yes">
<description>&lt;h3&gt;SMD Antenna Connector - U.FL&lt;/h3&gt;
&lt;p&gt;2mm height, 3.0mm x 3.0mm receptacle size. &lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13287"&gt;SparkFun WiFi Shield - ESP8266&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13231”&gt;SparkFun ESP8266 Thing&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/11420”&gt;SparkFun MiniGen - Pro Mini Signal Generator Shield&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="U.FL-1"/>
</gates>
<devices>
<device name="" package="U.FL">
<connects>
<connect gate="G$1" pin="GND" pad="1 2"/>
<connect gate="G$1" pin="SIGNAL" pad="FEED"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09193"/>
<attribute name="SF_ID" value="WRL-09144"/>
<attribute name="VALUE" value="U.FL"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JST_6_PIN_HORIZONTAL" prefix="J">
<description>&lt;h3&gt;JST 6 pin horizontal connector&lt;/h3&gt;
JST-SH type.

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Here is the connector we sell at SparkFun:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="link"&gt;name&lt;/a&gt; (XXX-00000)&lt;/li&gt;
&lt;li&gt;&lt;a href="http://www.sparkfun.com/datasheets/GPS/EM406-SMDConnector-eSH.pdf"&gt;Datasheet&lt;/a&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;It was used on these SparkFun products:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="link"&gt;name&lt;/a&gt; (XXX-00000)&lt;/li&gt;
&lt;li&gt;&lt;a href="link"&gt;name&lt;/a&gt; (XXX-00000)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="A" symbol="CONN_06"/>
<gate name="B" symbol="CONN_02"/>
</gates>
<devices>
<device name="" package="JST-6-SMD-HORI-1.0MM">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="B" pin="1" pad="M1"/>
<connect gate="B" pin="2" pad="M2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="XXX-00000"/>
<attribute name="VALUE" value="BM06B-SRSS-TB"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RASPBERRY_PI_40" prefix="U">
<gates>
<gate name="U1" symbol="RASPBERRY_PI_HEADER-40-GROUPED"/>
</gates>
<devices>
<device name="SMD" package="RASPBERRY_PI_SHIELD_HOLES">
<connects>
<connect gate="U1" pin="3.3V" pad="1 17"/>
<connect gate="U1" pin="5V" pad="2 4"/>
<connect gate="U1" pin="CS/D8" pad="24"/>
<connect gate="U1" pin="D12" pad="32"/>
<connect gate="U1" pin="D13" pad="33"/>
<connect gate="U1" pin="D16" pad="36"/>
<connect gate="U1" pin="D17" pad="11"/>
<connect gate="U1" pin="D19" pad="35"/>
<connect gate="U1" pin="D20" pad="38"/>
<connect gate="U1" pin="D21" pad="40"/>
<connect gate="U1" pin="D22" pad="15"/>
<connect gate="U1" pin="D23" pad="16"/>
<connect gate="U1" pin="D24" pad="18"/>
<connect gate="U1" pin="D25" pad="22"/>
<connect gate="U1" pin="D26" pad="37"/>
<connect gate="U1" pin="D27" pad="13"/>
<connect gate="U1" pin="D4" pad="7"/>
<connect gate="U1" pin="D5" pad="29"/>
<connect gate="U1" pin="D6" pad="31"/>
<connect gate="U1" pin="D7" pad="26"/>
<connect gate="U1" pin="GND" pad="6 9 14 20 25 30 34 39"/>
<connect gate="U1" pin="ID_SCL" pad="28"/>
<connect gate="U1" pin="ID_SDA" pad="27"/>
<connect gate="U1" pin="MISO/D9" pad="21"/>
<connect gate="U1" pin="MOSI/D10" pad="19"/>
<connect gate="U1" pin="PCM_CLK/D18" pad="12"/>
<connect gate="U1" pin="RX/D15" pad="10"/>
<connect gate="U1" pin="SCK/D11" pad="23"/>
<connect gate="U1" pin="SCL/D3" pad="5"/>
<connect gate="U1" pin="SDA/D2" pad="3"/>
<connect gate="U1" pin="TX/D14" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NOHOLES" package="RASPBERRY_PI_SHIELD_NOHOLES">
<connects>
<connect gate="U1" pin="3.3V" pad="1 17"/>
<connect gate="U1" pin="5V" pad="2 4"/>
<connect gate="U1" pin="CS/D8" pad="24"/>
<connect gate="U1" pin="D12" pad="32"/>
<connect gate="U1" pin="D13" pad="33"/>
<connect gate="U1" pin="D16" pad="36"/>
<connect gate="U1" pin="D17" pad="11"/>
<connect gate="U1" pin="D19" pad="35"/>
<connect gate="U1" pin="D20" pad="38"/>
<connect gate="U1" pin="D21" pad="40"/>
<connect gate="U1" pin="D22" pad="15"/>
<connect gate="U1" pin="D23" pad="16"/>
<connect gate="U1" pin="D24" pad="18"/>
<connect gate="U1" pin="D25" pad="22"/>
<connect gate="U1" pin="D26" pad="37"/>
<connect gate="U1" pin="D27" pad="13"/>
<connect gate="U1" pin="D4" pad="7"/>
<connect gate="U1" pin="D5" pad="29"/>
<connect gate="U1" pin="D6" pad="31"/>
<connect gate="U1" pin="D7" pad="26"/>
<connect gate="U1" pin="GND" pad="6 9 14 20 25 30 34 39"/>
<connect gate="U1" pin="ID_SCL" pad="28"/>
<connect gate="U1" pin="ID_SDA" pad="27"/>
<connect gate="U1" pin="MISO/D9" pad="21"/>
<connect gate="U1" pin="MOSI/D10" pad="19"/>
<connect gate="U1" pin="PCM_CLK/D18" pad="12"/>
<connect gate="U1" pin="RX/D15" pad="10"/>
<connect gate="U1" pin="SCK/D11" pad="23"/>
<connect gate="U1" pin="SCL/D3" pad="5"/>
<connect gate="U1" pin="SDA/D2" pad="3"/>
<connect gate="U1" pin="TX/D14" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BTM-NOHOLES" package="RASPBERRY_PI_SHIELD_BOTTOM_ENTRY_NOHOLES">
<connects>
<connect gate="U1" pin="3.3V" pad="1 17"/>
<connect gate="U1" pin="5V" pad="2 4"/>
<connect gate="U1" pin="CS/D8" pad="24"/>
<connect gate="U1" pin="D12" pad="32"/>
<connect gate="U1" pin="D13" pad="33"/>
<connect gate="U1" pin="D16" pad="36"/>
<connect gate="U1" pin="D17" pad="11"/>
<connect gate="U1" pin="D19" pad="35"/>
<connect gate="U1" pin="D20" pad="38"/>
<connect gate="U1" pin="D21" pad="40"/>
<connect gate="U1" pin="D22" pad="15"/>
<connect gate="U1" pin="D23" pad="16"/>
<connect gate="U1" pin="D24" pad="18"/>
<connect gate="U1" pin="D25" pad="22"/>
<connect gate="U1" pin="D26" pad="37"/>
<connect gate="U1" pin="D27" pad="13"/>
<connect gate="U1" pin="D4" pad="7"/>
<connect gate="U1" pin="D5" pad="29"/>
<connect gate="U1" pin="D6" pad="31"/>
<connect gate="U1" pin="D7" pad="26"/>
<connect gate="U1" pin="GND" pad="6 9 14 20 25 30 34 39"/>
<connect gate="U1" pin="ID_SCL" pad="28"/>
<connect gate="U1" pin="ID_SDA" pad="27"/>
<connect gate="U1" pin="MISO/D9" pad="21"/>
<connect gate="U1" pin="MOSI/D10" pad="19"/>
<connect gate="U1" pin="PCM_CLK/D18" pad="12"/>
<connect gate="U1" pin="RX/D15" pad="10"/>
<connect gate="U1" pin="SCK/D11" pad="23"/>
<connect gate="U1" pin="SCL/D3" pad="5"/>
<connect gate="U1" pin="SDA/D2" pad="3"/>
<connect gate="U1" pin="TX/D14" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-13790"/>
<attribute name="VALUE" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_24" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special notes:&lt;/b&gt;
&lt;p&gt; &lt;/p&gt; Molex polarized connector foot print use with SKU : PRT-08231 with associated crimp pins and housings. 1MM SMD Version SKU: PRT-10208
&lt;p&gt;&lt;/p&gt;
NOTES ON THE VARIANTS LOCK and LOCK_LONGPADS...
This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place. You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers. Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,if you push a header all the way into place, it is covered up entirely on the bottom side.</description>
<gates>
<gate name="G$1" symbol="CONN_24-1"/>
</gates>
<devices>
<device name="" package="1X24">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="1X24_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X24_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GATOR" prefix="J">
<gates>
<gate name="G$1" symbol="MICRO_BIT_GATOR_CLIP"/>
</gates>
<devices>
<device name="" package="GATOR">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1 P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GATOR_MINI" package="GATOR_MINI">
<connects>
<connect gate="G$1" pin="P$1" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TAB_GATOR_MINI">
<gates>
<gate name="G$1" symbol="TAB_MICRO_BIT_GATOR_CLIP"/>
</gates>
<devices>
<device name="" package="TAB_GATOR_MINI">
<connects>
<connect gate="G$1" pin="P$1" pad="P1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOLDER_PAD_2" prefix="J">
<description>Solder Pad for LuMini Rings</description>
<gates>
<gate name="G$1" symbol="CONN_02"/>
</gates>
<devices>
<device name="" package="SOLDER_PAD_2">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED_PAD" prefix="J">
<description>LuMini 8X8 Solder Pad</description>
<gates>
<gate name="G$1" symbol="CONN_01"/>
</gates>
<devices>
<device name="" package="CIRCULARPAD">
<connects>
<connect gate="G$1" pin="1" pad="P$1 P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB_C" prefix="J" uservalue="yes">
<description>&lt;h3&gt;USB Type C 16Pin Connector&lt;/h3&gt;

Super Speed pins not available on the 16-pin purely SMD connector so this part is best for USB 2.0 implementations. D1 and D2 are tied together enabling D+/- no matter which way the cable is plugged into the connector. The two channel configuration pins (CC1/2) are exposed. These are normally connected to ground via 5.1k resistors but can be reconfigured for high current/high power applications.</description>
<gates>
<gate name="J1" symbol="USB-C-MINIMUM"/>
</gates>
<devices>
<device name="4-LAYER-ISOLATED" package="USB-C-16P-4LAYER-ISOLATED">
<connects>
<connect gate="J1" pin="CC1" pad="A5"/>
<connect gate="J1" pin="CC2" pad="B5"/>
<connect gate="J1" pin="D+" pad="A6 B6"/>
<connect gate="J1" pin="D-" pad="A7 B7"/>
<connect gate="J1" pin="GND" pad="GND GND2"/>
<connect gate="J1" pin="SHLD" pad="SHLD1 SHLD2 SHLD3 SHLD4 SHLD5 SHLD6 SHLD7 SHLD8"/>
<connect gate="J1" pin="VBUS" pad="VBUS1 VBUS2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-14122"/>
<attribute name="VALUE" value="USB Female Type C Connector"/>
</technology>
</technologies>
</device>
<device name="2-LAYER" package="USB-C-16P">
<connects>
<connect gate="J1" pin="CC1" pad="A5"/>
<connect gate="J1" pin="CC2" pad="B5"/>
<connect gate="J1" pin="D+" pad="A6 B6"/>
<connect gate="J1" pin="D-" pad="A7 B7"/>
<connect gate="J1" pin="GND" pad="GND GND2"/>
<connect gate="J1" pin="SHLD" pad="SHLD1 SHLD2 SHLD3 SHLD4 SHLD5 SHLD6 SHLD7 SHLD8"/>
<connect gate="J1" pin="VBUS" pad="VBUS1 VBUS2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-14122"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XLR-3" prefix="J">
<description>&lt;h3&gt;Neutrik XLR-3 Jack - XLR-3 Jack for DMX&lt;/h3&gt;
&lt;p&gt;Symbol for a horizontal, 3-pin DMX connector&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="XLR-3"/>
</gates>
<devices>
<device name="-MALE" package="XLR-3_MALE">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-14141"/>
</technology>
</technologies>
</device>
<device name="-FEMALE" package="XLR-3_FEMALE">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-14142"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB_SOLDER_PADS_DATA_ONLY" prefix="JP">
<description>Solder pad access to USB pins. Helpful to expose on PCBs so user can attach external USB connector if necessary.</description>
<gates>
<gate name="JP1" symbol="CONN_02"/>
</gates>
<devices>
<device name="" package="USB-SOLDER-PADS-DATA_ONLY">
<connects>
<connect gate="JP1" pin="1" pad="D+"/>
<connect gate="JP1" pin="2" pad="D-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB_SOLDER_PADS" prefix="JP">
<description>Solder pad access to USB pins. Helpful to expose on PCBs so user can attach external USB connector if necessary.</description>
<gates>
<gate name="JP1" symbol="CONN_04"/>
</gates>
<devices>
<device name="" package="USB-SOLDER-PADS">
<connects>
<connect gate="JP1" pin="1" pad="VBUS"/>
<connect gate="JP1" pin="2" pad="D-"/>
<connect gate="JP1" pin="3" pad="D+"/>
<connect gate="JP1" pin="4" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_04" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special notes:&lt;/b&gt;
&lt;p&gt; &lt;/p&gt; Molex polarized connector foot print use with SKU : PRT-08231 with associated crimp pins and housings. 1MM SMD Version SKU: PRT-10208</description>
<gates>
<gate name="J1" symbol="CONN_04"/>
</gates>
<devices>
<device name="PTH" package="1X04">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09696"/>
</technology>
</technologies>
</device>
<device name="POLAR" package="MOLEX-1X4">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08186"/>
<attribute name="SF_ID" value="PRT-08231"/>
</technology>
</technologies>
</device>
<device name="SCREW" package="SCREWTERMINAL-3.5MM-4">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-14485"/>
</technology>
</technologies>
</device>
<device name="1.27MM" package="1X04_1.27MM">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X04_LOCK">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09696"/>
</technology>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X04_LOCK_LONGPADS">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09696"/>
</technology>
</technologies>
</device>
<device name="POLAR_LOCK" package="MOLEX-1X4_LOCK">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08186"/>
<attribute name="SF_ID" value="PRT-08231"/>
</technology>
</technologies>
</device>
<device name="SMD" package="1X04_SMD_RA_MALE">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09140"/>
<attribute name="SF_ID" value="PRT-12638"/>
</technology>
</technologies>
</device>
<device name="LONGPADS" package="1X04_LONGPADS">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09696"/>
</technology>
</technologies>
</device>
<device name="1X04_NO_SILK" package="1X04_NO_SILK">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09696"/>
</technology>
</technologies>
</device>
<device name="JST-PTH" package="JST-4-PTH">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="WIRE-13531"/>
<attribute name="SF_ID" value="PRT-09916"/>
</technology>
</technologies>
</device>
<device name="SCREW_LOCK" package="SCREWTERMINAL-3.5MM-4_LOCK">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD2" package="JST04_1MM_RA">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10310"/>
<attribute name="SF_ID" value="PRT-10208"/>
</technology>
</technologies>
</device>
<device name="SMD_STRAIGHT_COMBO" package="1X04_SMD_VERTICAL_COMBO">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08511"/>
<attribute name="VALUE" value="1X04_SMD_STRAIGHT_COMBO"/>
</technology>
</technologies>
</device>
<device name="SMD_LONG" package="1X04_SMD_LONG">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09140"/>
<attribute name="SF_ID" value="PRT-12638"/>
</technology>
</technologies>
</device>
<device name="JST-PTH-VERT" package="JST-4-PTH-VERT">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-13251"/>
</technology>
</technologies>
</device>
<device name="SMD_RA_FEMALE" package="1X04_SMD_RA_FEMALE">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-12382"/>
</technology>
</technologies>
</device>
<device name="SPRING" package="1X04_SPRING_TERMINAL">
<connects>
<connect gate="J1" pin="1" pad="1 5"/>
<connect gate="J1" pin="2" pad="2 6"/>
<connect gate="J1" pin="3" pad="3 7"/>
<connect gate="J1" pin="4" pad="4 8"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="PRT-08075"/>
</technology>
</technologies>
</device>
<device name="1.27MM_NO_SILK" package="1X04_1.27MM_NO_SILK">
<connects>
<connect gate="J1" pin="1" pad="1"/>
<connect gate="J1" pin="2" pad="2"/>
<connect gate="J1" pin="3" pad="3"/>
<connect gate="J1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAMERA-HIMAX" prefix="J">
<gates>
<gate name="G$1" symbol="CAMERA-OV7670-MODULE"/>
</gates>
<devices>
<device name="" package="FPC-24-AMPHENOL-SFV24R-1STE1HLF">
<connects>
<connect gate="G$1" pin="AVDD" pad="4 11"/>
<connect gate="G$1" pin="D0" pad="14"/>
<connect gate="G$1" pin="D1" pad="3"/>
<connect gate="G$1" pin="D2" pad="9"/>
<connect gate="G$1" pin="D3" pad="5"/>
<connect gate="G$1" pin="D4" pad="12"/>
<connect gate="G$1" pin="D5" pad="20"/>
<connect gate="G$1" pin="D6" pad="19"/>
<connect gate="G$1" pin="D7" pad="13"/>
<connect gate="G$1" pin="FVLD" pad="6"/>
<connect gate="G$1" pin="GND" pad="2 15"/>
<connect gate="G$1" pin="INT" pad="18"/>
<connect gate="G$1" pin="IOVDD" pad="10"/>
<connect gate="G$1" pin="LVLD" pad="16"/>
<connect gate="G$1" pin="MCLK" pad="8"/>
<connect gate="G$1" pin="MNT1" pad="MNT1@0 MNT1@1"/>
<connect gate="G$1" pin="MNT2" pad="MNT2@0 MNT2@1"/>
<connect gate="G$1" pin="PCLK" pad="17"/>
<connect gate="G$1" pin="SCL" pad="21"/>
<connect gate="G$1" pin="SDA" pad="22"/>
<connect gate="G$1" pin="TRIG" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIGIKEY" value="609-4320-2-ND"/>
<attribute name="PROD_ID" value="CONN-14233"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CORTEX_JTAG_DEBUG_MINIMUM" prefix="J">
<description>&lt;h3&gt;Cortex Debug Connector - 10 pin&lt;/h3&gt;
&lt;p&gt;Supports JTAG debug, Serial Wire debug, and Serial Wire Viewer.
PTH and SMD connector options available.&lt;/p&gt;
&lt;p&gt; &lt;ul&gt;&lt;a href=”http://infocenter.arm.com/help/topic/com.arm.doc.faqs/attached/13634/cortex_debug_connectors.pdf”&gt;General Connector Information&lt;/a&gt;
&lt;p&gt;&lt;b&gt; Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”http://www.digikey.com/product-detail/en/cnc-tech/3220-10-0100-00/1175-1627-ND/3883661”&gt;PTH Connector&lt;/a&gt; -via Digi-Key&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13229”&gt;SparkFun PSoc&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13810”&gt;SparkFun T&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CORTEX_DEBUG_MINIMUM"/>
</gates>
<devices>
<device name="_PTH_NS" package="2X5-PTH-1.27MM-NO_SILK">
<connects>
<connect gate="G$1" pin="!RESET" pad="10"/>
<connect gate="G$1" pin="GND" pad="3 5 9"/>
<connect gate="G$1" pin="SWDCLK" pad="4"/>
<connect gate="G$1" pin="SWDIO" pad="2"/>
<connect gate="G$1" pin="SWO" pad="6"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_PTH" package="2X5-PTH-1.27MM">
<connects>
<connect gate="G$1" pin="!RESET" pad="10"/>
<connect gate="G$1" pin="GND" pad="3 5 9"/>
<connect gate="G$1" pin="SWDCLK" pad="4"/>
<connect gate="G$1" pin="SWDIO" pad="2"/>
<connect gate="G$1" pin="SWO" pad="6"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_SMD" package="2X5-SMD-1.27MM">
<connects>
<connect gate="G$1" pin="!RESET" pad="10"/>
<connect gate="G$1" pin="GND" pad="3 5 9"/>
<connect gate="G$1" pin="SWDCLK" pad="4"/>
<connect gate="G$1" pin="SWDIO" pad="2"/>
<connect gate="G$1" pin="SWO" pad="6"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-14468"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RASPBERRYPI-26-PIN-GPIO" prefix="J">
<description>&lt;h3&gt;RASPBERRY PI I/O HEADER&lt;/h3&gt;

&lt;p&gt;As defined for the Revistion 2 Pi. The 40 pin header is backwards compatible with this smaller more compact footprint.&lt;/p&gt;</description>
<gates>
<gate name="JP1" symbol="RASPBERRYPI-26-PIN-GPIO"/>
</gates>
<devices>
<device name="PTH" package="2X13-SHROUDED">
<connects>
<connect gate="JP1" pin="3.3V@1" pad="1"/>
<connect gate="JP1" pin="3.3V@17" pad="17"/>
<connect gate="JP1" pin="5V@2" pad="2"/>
<connect gate="JP1" pin="5V@4" pad="4"/>
<connect gate="JP1" pin="CE0" pad="24"/>
<connect gate="JP1" pin="CE1" pad="26"/>
<connect gate="JP1" pin="GND@14" pad="14"/>
<connect gate="JP1" pin="GND@20" pad="20"/>
<connect gate="JP1" pin="GND@25" pad="25"/>
<connect gate="JP1" pin="GND@6" pad="6"/>
<connect gate="JP1" pin="GND@9" pad="9"/>
<connect gate="JP1" pin="GP17" pad="11"/>
<connect gate="JP1" pin="GP18#" pad="12"/>
<connect gate="JP1" pin="GP22" pad="15"/>
<connect gate="JP1" pin="GP23" pad="16"/>
<connect gate="JP1" pin="GP24" pad="18"/>
<connect gate="JP1" pin="GP25" pad="22"/>
<connect gate="JP1" pin="GP27" pad="13"/>
<connect gate="JP1" pin="GP4" pad="7"/>
<connect gate="JP1" pin="MISO" pad="21"/>
<connect gate="JP1" pin="MOSI" pad="19"/>
<connect gate="JP1" pin="RXI" pad="10"/>
<connect gate="JP1" pin="SCL" pad="5"/>
<connect gate="JP1" pin="SCLK" pad="23"/>
<connect gate="JP1" pin="SDA" pad="3"/>
<connect gate="JP1" pin="TXO" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIST" value="sparkfun"/>
<attribute name="DIST_ID" value="PRT-11490"/>
</technology>
</technologies>
</device>
<device name="" package="2X13">
<connects>
<connect gate="JP1" pin="3.3V@1" pad="1"/>
<connect gate="JP1" pin="3.3V@17" pad="17"/>
<connect gate="JP1" pin="5V@2" pad="2"/>
<connect gate="JP1" pin="5V@4" pad="4"/>
<connect gate="JP1" pin="CE0" pad="24"/>
<connect gate="JP1" pin="CE1" pad="26"/>
<connect gate="JP1" pin="GND@14" pad="14"/>
<connect gate="JP1" pin="GND@20" pad="20"/>
<connect gate="JP1" pin="GND@25" pad="25"/>
<connect gate="JP1" pin="GND@6" pad="6"/>
<connect gate="JP1" pin="GND@9" pad="9"/>
<connect gate="JP1" pin="GP17" pad="11"/>
<connect gate="JP1" pin="GP18#" pad="12"/>
<connect gate="JP1" pin="GP22" pad="15"/>
<connect gate="JP1" pin="GP23" pad="16"/>
<connect gate="JP1" pin="GP24" pad="18"/>
<connect gate="JP1" pin="GP25" pad="22"/>
<connect gate="JP1" pin="GP27" pad="13"/>
<connect gate="JP1" pin="GP4" pad="7"/>
<connect gate="JP1" pin="MISO" pad="21"/>
<connect gate="JP1" pin="MOSI" pad="19"/>
<connect gate="JP1" pin="RXI" pad="10"/>
<connect gate="JP1" pin="SCL" pad="5"/>
<connect gate="JP1" pin="SCLK" pad="23"/>
<connect gate="JP1" pin="SDA" pad="3"/>
<connect gate="JP1" pin="TXO" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
