<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.0">
<drawing>
<library>
<description>&lt;h3&gt;SparkFun Electromechanical Parts&lt;/h3&gt;
This library contains electromechanical devices, like motors, speakers,servos, and relays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BUZZER-12MM">
<description>&lt;h3&gt;12mm Buzzer - PTH&lt;/h3&gt;
&lt;p&gt;This is a small 12mm round speaker that operates around the audible 2kHz range. You can use these speakers to create simple music or user interfaces.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/General/cem-1203-42-.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BUZZER&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="BUZZER-CCV">
<description>&lt;h3&gt;9mm Buzzer - SMD&lt;/h3&gt;
&lt;p&gt;This is a small 9mm round speaker that operates around the audible 2kHz range. You can use these speakers to create simple music or user interfaces.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.challengeelectronics.com/downloads/sound_transducers/electromagnetic_smd/CEET105A025-16-2545-27MLR.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BUZZER&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="BUZZER-12MM-NS">
<description>&lt;h3&gt;12mm Buzzer - PTH (No silkscreent variant)&lt;/h3&gt;
&lt;p&gt;This is a small 12mm round speaker that operates around the audible 2kHz range. You can use these speakers to create simple music or user interfaces.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/General/cem-1203-42-.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BUZZER&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="BUZZER-12MM-NS-KIT">
<description>&lt;h3&gt;12mm Buzzer - PTH (KIT, No-Silkscreen VARIANT)&lt;/h3&gt;
&lt;p&gt;This is a small 12mm round speaker that operates around the audible 2kHz range. You can use these speakers to create simple music or user interfaces.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/General/cem-1203-42-.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BUZZER&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="BUZZER-CCV-KIT">
<description>&lt;h3&gt;9mm Buzzer - SMD (KIT variant)&lt;/h3&gt;
&lt;p&gt;This is a small 9mm round speaker that operates around the audible 2kHz range. You can use these speakers to create simple music or user interfaces.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has longer pads to aid in hand soldering.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.challengeelectronics.com/downloads/sound_transducers/electromagnetic_smd/CEET105A025-16-2545-27MLR.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BUZZER&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="VIBE-MOTOR-10MM">
<description>&lt;h3&gt;Vibration Motor&lt;/h3&gt;
&lt;p&gt;10mm vibration motor terminated with tinned wires.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Robotics/B1034.FL45-00-015.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;MOTOR&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="RELAY-JZC">
<description>&lt;h3&gt;Relay SPDT Sealed (JZC-11F-5V-1Z)&lt;/h3&gt;
&lt;p&gt;These are high quality Single Pole - Double Throw (SPDT) sealed relays. Use them to switch high voltage, and/or high current devices.&lt;/p&gt;
&lt;p&gt;This relay’s coil is rated up to 12V, with a minimum switching voltage of 5V. The contacts are rated up to 5A (@250VAC, 30VDC).&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.sparkfun.com/datasheets/Components/General/JZC-11F-05VDC-1Z%20EN.pdf"&gt;Datasheet&lt;/a&gt; (JZC-11F-5V-1Z)&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Note&lt;/b&gt;: The datasheet specifies a 5.04mm (.2 inch) gap between pins two and three. This does not reflect the &lt;i&gt;actual&lt;/i&gt; gap between the two pins which is .17 inches. Furthermore the gap is not split into an equidistant Y-offset with pin four. Instead, pin 3 is 2.54mm (.1 inch) in the Y-direction from center of pin four and pin 4 is .07 inches in the negative Y direction. &lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;RELAY-SPDT&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="PCB_MOUNT_SPEAKER">
<description>&lt;h3&gt;Speaker - PCB Mount&lt;/h3&gt;
&lt;p&gt;PTH speaker. 30mm diameter.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/General/PCBspeaker.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;SPEAKER&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="1X03">
<description>&lt;h3&gt;3-Pin Header&lt;/h3&gt;
&lt;p&gt;0.1"-spaced 3-pin header. 
&lt;ul&gt;&lt;li&gt;Drill diameter: 40 mil&lt;/li&gt;
&lt;li&gt;Copper diameter: 74 mil&lt;/li&gt;&lt;/ul&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;SERVO&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="BUZZER-12MM-KIT">
<description>&lt;h3&gt;12mm Buzzer - PTH (KIT VARIANT)&lt;/h3&gt;
&lt;p&gt;This is a small 12mm round speaker that operates around the audible 2kHz range. You can use these speakers to create simple music or user interfaces.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/General/cem-1203-42-.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BUZZER&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="RELAY-T90">
<description>&lt;h3&gt;Relay SPDT Sealed - 20A (JQX-15F/005)&lt;/h3&gt;
&lt;p&gt;These are massive single pole - double throw (SPDT) sealed relays. This means that when current is applied to the coil it throws a simple changeover switch, terminating the connection from the NC contact to ground and closing the NO contact. Use them to switch high voltage/high current devices.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/General/Relay.JQX-15F.pdf"&gt;Datasheet&lt;/a&gt; (JQX-15F/005)&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;RELAY-SPDT&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="HEATSINK_PRT-9576">
</package>
<package name="RELAY_G5LE">
</package>
</packages>
<symbols>
<symbol name="BUZZER">
<description>&lt;h3&gt;Buzzer&lt;/h3&gt;</description>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="MOTOR">
<description>&lt;h3&gt;Motor (Single-Phase, Two-Terminal)&lt;/h3&gt;</description>
<pin name="+"/>
<pin name="-"/>
</symbol>
<symbol name="RELAY-SPDT">
<description>&lt;h3&gt;Relay (SPDT) (1 Common Pin)&lt;/h3&gt;</description>
<pin name="COIL2"/>
<pin name="MAIN"/>
<pin name="NO"/>
<pin name="NC"/>
<pin name="COIL1"/>
</symbol>
<symbol name="SPEAKER">
<description>&lt;h3&gt;Loudspeaker&lt;/h3&gt;</description>
<pin name="+"/>
<pin name="-"/>
</symbol>
<symbol name="SMALL_SERVO_MOTOR">
<description>&lt;h3&gt;Servo Motor&lt;/h3&gt;</description>
<pin name="SIG"/>
<pin name="V+"/>
<pin name="GND"/>
</symbol>
<symbol name="HEATSINK">
</symbol>
</symbols>
<devicesets>
<deviceset name="BUZZER" prefix="LS">
<description>&lt;h3&gt;Buzzer&lt;/h3&gt;
&lt;p&gt;Small round buzzers that operate around the audible 2kHz range. You can use these as speakers to create simple music or user interfaces.&lt;/p&gt;
&lt;p&gt;Variant Overview:
&lt;ul&gt;
&lt;li&gt;&lt;b&gt;PTH - &lt;/b&gt; &lt;a href="https://www.sparkfun.com/products/7950"&gt;Mini Speaker - PC Mount 12mm 2.048kHz&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;b&gt;PTH_KIT - &lt;/b&gt; &lt;a href="https://www.sparkfun.com/products/7950"&gt;Mini Speaker - PC Mount 12mm 2.048kHz&lt;/a&gt;&lt;/li&gt;&lt;ul&gt;&lt;li&gt; KIT simplifies soldering by adding stop mask to one side of the pads.&lt;/li&gt;&lt;/ul&gt;
&lt;li&gt;&lt;b&gt;PTH_NO_SILK - &lt;/b&gt; &lt;a href="https://www.sparkfun.com/products/7950"&gt;Mini Speaker - PC Mount 12mm 2.048kHz&lt;/a&gt;&lt;/li&gt;&lt;ul&gt;&lt;li&gt; No silkscreen indicator of buzzer outline.&lt;/li&gt;&lt;/ul&gt;
&lt;li&gt;&lt;b&gt;PTH_KIT_NO_SILK - &lt;/b&gt; &lt;a href="https://www.sparkfun.com/products/7950"&gt;Mini Speaker - PC Mount 12mm 2.048kHz&lt;/a&gt;&lt;/li&gt;&lt;ul&gt;&lt;li&gt; KIT package w/o silkscreen&lt;/li&gt;&lt;/ul&gt;
&lt;li&gt;&lt;b&gt;SMD - &lt;/b&gt; Buzzer Audio Magnetic (CCV-084B16)&lt;/li&gt; &lt;ul&gt;&lt;li&gt;SMD buzzer used on, e.g. the &lt;a href="https://www.sparkfun.com/products/8463"&gt;LilyPad Buzzer&lt;/a&gt; and &lt;a href="https://www.sparkfun.com/products/9963"&gt;RFID USB Reader&lt;/a&gt;.&lt;/li&gt;&lt;/ul&gt;&lt;li&gt;&lt;b&gt;SMD_KIT - &lt;/b&gt; Buzzer Audio Magnetic (CCV-084B16)&lt;/li&gt;&lt;ul&gt;&lt;li&gt;SMD Buzzer with elongated pins to make soldering easier. Used on the &lt;a href="https://www.sparkfun.com/products/10935"&gt;SparkFun Simon Says - Surface Mount Soldering Kit&lt;/a&gt;.&lt;/li&gt;&lt;/ul&gt;
&lt;/ul&gt;
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BUZZER"/>
</gates>
<devices>
<device name="-PTH" package="BUZZER-12MM">
<connects>
<connect gate="G$1" pin="1" pad="+"/>
<connect gate="G$1" pin="2" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-08253"/>
<attribute name="SF_SKU" value="COM-07950"/>
</technology>
</technologies>
</device>
<device name="-SMD" package="BUZZER-CCV">
<connects>
<connect gate="G$1" pin="1" pad="+"/>
<connect gate="G$1" pin="2" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-08568"/>
</technology>
</technologies>
</device>
<device name="-PTH_NO_SILK" package="BUZZER-12MM-NS">
<connects>
<connect gate="G$1" pin="1" pad="+"/>
<connect gate="G$1" pin="2" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-08253"/>
<attribute name="SF_SKU" value="COM-07950"/>
</technology>
</technologies>
</device>
<device name="-PTH_KIT_NO_SILK" package="BUZZER-12MM-NS-KIT">
<connects>
<connect gate="G$1" pin="1" pad="+"/>
<connect gate="G$1" pin="2" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-08253"/>
<attribute name="SF_SKU" value="COM-07950"/>
</technology>
</technologies>
</device>
<device name="-SMD_KIT" package="BUZZER-CCV-KIT">
<connects>
<connect gate="G$1" pin="1" pad="+"/>
<connect gate="G$1" pin="2" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-08568"/>
</technology>
</technologies>
</device>
<device name="-PTH_KIT" package="BUZZER-12MM-KIT">
<connects>
<connect gate="G$1" pin="1" pad="+"/>
<connect gate="G$1" pin="2" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-08253"/>
<attribute name="SF_SKU" value="COM-07950"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOTOR" prefix="M">
<description>&lt;h3&gt;Motor (Single-Phase)&lt;/h3&gt;
&lt;p&gt;Two-terminal, single-phase motors.&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8449"&gt;Vibration Motor&lt;/a&gt; (ROB-08449)
&lt;br&gt;Physical dimension and wire connections for this powerful vibration motor. Motor has a self adhesive backing.&lt;/li&gt;&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="MOTOR"/>
</gates>
<devices>
<device name="10MM" package="VIBE-MOTOR-10MM">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-08572"/>
<attribute name="SF_SKU" value="ROB-08449"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RELAY-SPDT" prefix="K">
<description>&lt;h3&gt;SPDT Electromechanical Relay&lt;/h3&gt;
&lt;p&gt;Single-pole, double-throw sealed relays. When current is applied to the coil, it throws a simple changeover switch, terminating the connection from the NC contact to ground and closing the NO contact. Use them to switch high voltage/high current devices.&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;JQX-15F: &lt;a href="https://www.sparkfun.com/products/10924"&gt;Relay SPDT Sealed - 20A&lt;/a&gt; (COM-10924)&lt;/li&gt;
&lt;li&gt;JZC-11F: &lt;a href="https://www.sparkfun.com/products/100"&gt;Relay SPDT Sealed&lt;/a&gt; (COM-00100)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="K$1" symbol="RELAY-SPDT"/>
</gates>
<devices>
<device name="-JZC-11F" package="RELAY-JZC">
<connects>
<connect gate="K$1" pin="COIL1" pad="5"/>
<connect gate="K$1" pin="COIL2" pad="1"/>
<connect gate="K$1" pin="MAIN" pad="4"/>
<connect gate="K$1" pin="NC" pad="2"/>
<connect gate="K$1" pin="NO" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-09533"/>
<attribute name="SF_SKU" value="COM-00100"/>
</technology>
</technologies>
</device>
<device name="-JQX-15F" package="RELAY-T90">
<connects>
<connect gate="K$1" pin="COIL1" pad="COIL1"/>
<connect gate="K$1" pin="COIL2" pad="COIL2"/>
<connect gate="K$1" pin="MAIN" pad="MAIN"/>
<connect gate="K$1" pin="NC" pad="NC"/>
<connect gate="K$1" pin="NO" pad="NO"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-10736"/>
<attribute name="SF_SKU" value="COM-10924"/>
</technology>
</technologies>
</device>
<device name="" package="RELAY_G5LE">
<connects>
<connect gate="K$1" pin="COIL1" pad="2"/>
<connect gate="K$1" pin="COIL2" pad="5"/>
<connect gate="K$1" pin="MAIN" pad="1"/>
<connect gate="K$1" pin="NC" pad="4"/>
<connect gate="K$1" pin="NO" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-14214"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPEAKER" prefix="LS">
<description>&lt;h3&gt;Speaker&lt;/h3&gt;
&lt;p&gt;Generic 2-terminal loudspeakers&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11089"&gt;Speaker - PCB Mount&lt;/a&gt; (COM-11089)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="SPEAKER"/>
</gates>
<devices>
<device name="" package="PCB_MOUNT_SPEAKER">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-11789"/>
<attribute name="SF_SKU" value="COM-11089"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SERVO" prefix="M">
<description>&lt;h3&gt;Servo Motor&lt;/h3&gt;
&lt;p&gt;3-pin connector for a standard servo motor (voltage supply, ground, and control signal.)&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9065"&gt;Servo - Generic (Sub-Micro Size)&lt;/a&gt; (ROB-09065)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9347"&gt;Servo - Generic High Torque Continuous Rotation (Standard Size)&lt;/a&gt; (ROB-09347)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11965"&gt;Servo - Generic High Torque (Standard Size)&lt;/a&gt; (ROB-11965)&lt;/li&gt;</description>
<gates>
<gate name="G$1" symbol="SMALL_SERVO_MOTOR"/>
</gates>
<devices>
<device name="" package="1X03">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="SIG" pad="1"/>
<connect gate="G$1" pin="V+" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEATSINK" prefix="HS" uservalue="yes">
<gates>
<gate name="G$1" symbol="HEATSINK"/>
</gates>
<devices>
<device name="PRT-9576" package="HEATSINK_PRT-9576">
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-9537"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
