<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<library>
<description>&lt;h3&gt;SparkFun Conversion ICs&lt;/h3&gt;
This library is for ICs that perform analog to digital conversion, as well as digital to analog.  This includes not only strict ADCs, but audio in and out converters, decoders, thermocouple measurement ics the like.  Anything that is a single part that works between the two domains goes here.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08">
<description>SOIC, 0.15 inch width</description>
</package>
<package name="LQFP-48">
<description>&lt;h3&gt;LQFP -48&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 48&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;VS1000&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SSOP_20">
<description>20-pin .65mm pitch/5.2mm body SMT</description>
</package>
<package name="SSOP20">
<description>&lt;b&gt;Shrink Small Outline Package&lt;/b&gt;&lt;p&gt;
package type SS</description>
</package>
<package name="MSOP10">
<description>&lt;b&gt;10 Lead Platic MSOP&lt;/b&gt;&lt;p&gt;
Source: http://www.linear.com .. LT1996</description>
</package>
<package name="SOT23-6">
<description>&lt;h3&gt;SOT23-6&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 6&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;MCP4725&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SO16A">
<description>&lt;h3&gt;SOP-16L&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 16&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://cdn.sparkfun.com/datasheets/Sensors/ForceFlex/hx711_english.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;HX711&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SO16">
<description>&lt;h3&gt;SOIC -16&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 16&lt;/li&gt;
&lt;li&gt;Area: 0.15 width&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;HX711&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
<symbols>
<symbol name="VS1000">
<pin name="XRESET"/>
<pin name="TEST"/>
<pin name="XTAL1"/>
<pin name="XTAL0"/>
<pin name="NFDIO0/IO0_0"/>
<pin name="NFDIO1/IO0_1"/>
<pin name="NFDIO2/IO0_2"/>
<pin name="NFDIO3/IO0_3"/>
<pin name="NFDIO4/IO0_4"/>
<pin name="NFDIO5/IO0_5"/>
<pin name="NFDIO6/IO0_6"/>
<pin name="NFDIO7/IO0_7"/>
<pin name="NFRDY/GPIO0_8"/>
<pin name="NFRD/GPIO0_9"/>
<pin name="CS1/GPIO0_10"/>
<pin name="NFCLE/GPIO0_12"/>
<pin name="NFALE/GPIO0_13"/>
<pin name="NFWR/GPIO0_11"/>
<pin name="CS2/GPIO0_14"/>
<pin name="DGND2"/>
<pin name="DGND3"/>
<pin name="AGND1"/>
<pin name="AGND2"/>
<pin name="AGND3"/>
<pin name="AGND4"/>
<pin name="DGND1"/>
<pin name="VHIGH"/>
<pin name="POWBTN"/>
<pin name="LEFT"/>
<pin name="RIGHT"/>
<pin name="GBUF"/>
<pin name="RCAP"/>
<pin name="XCS/GPIO1_0"/>
<pin name="SCLK/GPIO1_1"/>
<pin name="SI/GPIO1_2"/>
<pin name="SO/GPIO1_3"/>
<pin name="RX/GPIO1_4"/>
<pin name="TX/GPIO1_5"/>
<pin name="USBN"/>
<pin name="USBP"/>
<pin name="CVDD"/>
<pin name="IOVDD2"/>
<pin name="AVDD1"/>
<pin name="AVDD2"/>
<pin name="AVDD3"/>
<pin name="AVDD4"/>
<pin name="IOVDD3"/>
<pin name="IOVDD1"/>
</symbol>
<symbol name="VS1033D">
<pin name="S0"/>
<pin name="SI"/>
<pin name="SCLK"/>
<pin name="XCS"/>
<pin name="XDCS/BSYNC"/>
<pin name="DREQ"/>
<pin name="XRESET"/>
<pin name="TEST"/>
<pin name="XTAL1/MCLK"/>
<pin name="XTAL2"/>
<pin name="VCO"/>
<pin name="GPIO0/I2S_SCLK"/>
<pin name="GPIO1/I2S_SDATA"/>
<pin name="GPIO2/DCLK"/>
<pin name="GPIO3/SDATA"/>
<pin name="GPIO4/I2S_LROUT"/>
<pin name="GPIO5/I2C_MCLK"/>
<pin name="GPIO6"/>
<pin name="GPIO7"/>
<pin name="IOVDD1"/>
<pin name="IOVDD2"/>
<pin name="IOVDD3"/>
<pin name="CVDD1"/>
<pin name="CVDD2"/>
<pin name="CVDD3"/>
<pin name="AVDD1"/>
<pin name="AVDD2"/>
<pin name="AVDD3"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="LEFT"/>
<pin name="RIGHT"/>
<pin name="GBUF"/>
<pin name="MICP"/>
<pin name="MICN"/>
<pin name="LINEIN"/>
<pin name="RCAP"/>
<pin name="DGND6"/>
<pin name="DGND1"/>
<pin name="DGND2"/>
<pin name="DGND3"/>
<pin name="DGND4"/>
<pin name="DGND5"/>
<pin name="AGND4"/>
<pin name="CVDD4"/>
<pin name="AGND1"/>
<pin name="AGND2"/>
<pin name="AGND3"/>
</symbol>
<symbol name="WTV020SD-20S">
<pin name="P03"/>
<pin name="P04"/>
<pin name="P05"/>
<pin name="P06"/>
<pin name="P07"/>
<pin name="VCC"/>
<pin name="SPK_P"/>
<pin name="SPK_N"/>
<pin name="NC"/>
<pin name="PAD_EQO"/>
<pin name="PAD_EQI"/>
<pin name="GND"/>
<pin name="VPP"/>
<pin name="VDD"/>
<pin name="OSCI/P10"/>
<pin name="OSCO/P11"/>
<pin name="RESET"/>
<pin name="P00"/>
<pin name="P01"/>
<pin name="P02"/>
</symbol>
<symbol name="ADS1015">
<pin name="AIN0"/>
<pin name="AIN1"/>
<pin name="AIN2"/>
<pin name="AIN3"/>
<pin name="ALERT/RDY"/>
<pin name="ADDR"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="VSS"/>
<pin name="VDD"/>
</symbol>
<symbol name="MAX31855K">
<pin name="GND"/>
<pin name="T-"/>
<pin name="T+"/>
<pin name="VCC"/>
<pin name="(MI)SO"/>
<pin name="!CS"/>
<pin name="SCK"/>
</symbol>
<symbol name="MCP4725">
<pin name="VOUT"/>
<pin name="VSS"/>
<pin name="VDD"/>
<pin name="AO"/>
<pin name="SCL"/>
<pin name="SDA"/>
</symbol>
<symbol name="PCM1803A">
<pin name="VINL"/>
<pin name="VINR"/>
<pin name="VREF1"/>
<pin name="VREF2"/>
<pin name="VCCA"/>
<pin name="GNDA"/>
<pin name="PDWN"/>
<pin name="BPAS"/>
<pin name="TEST"/>
<pin name="LRCK"/>
<pin name="BCK"/>
<pin name="DOUT"/>
<pin name="GNDD"/>
<pin name="VDD"/>
<pin name="SCK"/>
<pin name="OSR"/>
<pin name="FMT0"/>
<pin name="FMT1"/>
<pin name="MD0"/>
<pin name="MD1"/>
</symbol>
<symbol name="HX711">
<description>&lt;h3&gt;HX711 ADC 24-bit Weight Sensor&lt;/h3&gt;</description>
<pin name="AGND"/>
<pin name="AVDD"/>
<pin name="BASE"/>
<pin name="DOUT"/>
<pin name="DVDD"/>
<pin name="INA+"/>
<pin name="INA-"/>
<pin name="INB+"/>
<pin name="INB-"/>
<pin name="PD_SCK"/>
<pin name="RATE"/>
<pin name="VBG"/>
<pin name="VFB"/>
<pin name="VSUP"/>
<pin name="XI"/>
<pin name="XO"/>
</symbol>
<symbol name="NAU7802">
<pin name="VIN2P"/>
<pin name="VIN1P"/>
<pin name="VIN1N"/>
<pin name="DRDY"/>
<pin name="AVDD"/>
<pin name="AVSS"/>
<pin name="REFN"/>
<pin name="XIN"/>
<pin name="DVSS"/>
<pin name="XOUT"/>
<pin name="DVDD"/>
<pin name="VBG"/>
<pin name="VIN2N"/>
<pin name="REFP"/>
<pin name="SDIO"/>
<pin name="SCLK"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="VS1000">
<description>&lt;h3&gt;VS1000D&lt;/h3&gt;
&lt;p&gt;Ogg Vorbis Player IC with USB and NAND FLASH Interface 12 MHz LQFP-48&lt;/p&gt;
&lt;h3&gt;&lt;/h3&gt;
&lt;p&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=""&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8300"&gt;Storefront component: Ogg Vorbis Codec IC - VS1000D&lt;/a&gt; (COM-08300)&lt;/li&gt;

&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="VS1000"/>
</gates>
<devices>
<device name="" package="LQFP-48">
<connects>
<connect gate="G$1" pin="AGND1" pad="38"/>
<connect gate="G$1" pin="AGND2" pad="41"/>
<connect gate="G$1" pin="AGND3" pad="42"/>
<connect gate="G$1" pin="AGND4" pad="48"/>
<connect gate="G$1" pin="AVDD1" pad="34"/>
<connect gate="G$1" pin="AVDD2" pad="39"/>
<connect gate="G$1" pin="AVDD3" pad="44"/>
<connect gate="G$1" pin="AVDD4" pad="46"/>
<connect gate="G$1" pin="CS1/GPIO0_10" pad="15"/>
<connect gate="G$1" pin="CS2/GPIO0_14" pad="21"/>
<connect gate="G$1" pin="CVDD" pad="32"/>
<connect gate="G$1" pin="DGND1" pad="6"/>
<connect gate="G$1" pin="DGND2" pad="18"/>
<connect gate="G$1" pin="DGND3" pad="31"/>
<connect gate="G$1" pin="GBUF" pad="43"/>
<connect gate="G$1" pin="IOVDD1" pad="30"/>
<connect gate="G$1" pin="IOVDD2" pad="19"/>
<connect gate="G$1" pin="IOVDD3" pad="7"/>
<connect gate="G$1" pin="LEFT" pad="47"/>
<connect gate="G$1" pin="NFALE/GPIO0_13" pad="17"/>
<connect gate="G$1" pin="NFCLE/GPIO0_12" pad="16"/>
<connect gate="G$1" pin="NFDIO0/IO0_0" pad="2"/>
<connect gate="G$1" pin="NFDIO1/IO0_1" pad="3"/>
<connect gate="G$1" pin="NFDIO2/IO0_2" pad="4"/>
<connect gate="G$1" pin="NFDIO3/IO0_3" pad="5"/>
<connect gate="G$1" pin="NFDIO4/IO0_4" pad="9"/>
<connect gate="G$1" pin="NFDIO5/IO0_5" pad="10"/>
<connect gate="G$1" pin="NFDIO6/IO0_6" pad="11"/>
<connect gate="G$1" pin="NFDIO7/IO0_7" pad="12"/>
<connect gate="G$1" pin="NFRD/GPIO0_9" pad="14"/>
<connect gate="G$1" pin="NFRDY/GPIO0_8" pad="13"/>
<connect gate="G$1" pin="NFWR/GPIO0_11" pad="20"/>
<connect gate="G$1" pin="POWBTN" pad="37"/>
<connect gate="G$1" pin="RCAP" pad="45"/>
<connect gate="G$1" pin="RIGHT" pad="40"/>
<connect gate="G$1" pin="RX/GPIO1_4" pad="27"/>
<connect gate="G$1" pin="SCLK/GPIO1_1" pad="23"/>
<connect gate="G$1" pin="SI/GPIO1_2" pad="24"/>
<connect gate="G$1" pin="SO/GPIO1_3" pad="25"/>
<connect gate="G$1" pin="TEST" pad="8"/>
<connect gate="G$1" pin="TX/GPIO1_5" pad="26"/>
<connect gate="G$1" pin="USBN" pad="36"/>
<connect gate="G$1" pin="USBP" pad="35"/>
<connect gate="G$1" pin="VHIGH" pad="33"/>
<connect gate="G$1" pin="XCS/GPIO1_0" pad="22"/>
<connect gate="G$1" pin="XRESET" pad="1"/>
<connect gate="G$1" pin="XTAL0" pad="29"/>
<connect gate="G$1" pin="XTAL1" pad="28"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="LPA-12743 "/>
<attribute name="VALUE" value="VS1000D"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VS1033/1053" prefix="U">
<description>&lt;h3&gt;VS1053B MP3 and MIDI Codec&lt;/h3&gt;
&lt;p&gt;AAC/MP3/WMA/MIDI/Ogg Audio Player and Ogg Recording Device LQFP-48 7x7x1.4 mm&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.sparkfun.com/datasheets/Components/SMD/vs1053.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8892"&gt;Storefront component: MP3 and MIDI Codec - VS1053B&lt;/a&gt; (COM-08892)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12660"&gt;SparkFun MP3 Player Shield&lt;/a&gt; (DEV-12660)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11013"&gt;LilyPad MP3&lt;/a&gt; (DEV-11013)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10587"&gt;SparkFun Music Instrument Shield&lt;/a&gt; (DEV-10587)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="VS1033D"/>
</gates>
<devices>
<device name="SMD" package="LQFP-48">
<connects>
<connect gate="G$1" pin="AGND1" pad="37"/>
<connect gate="G$1" pin="AGND2" pad="40"/>
<connect gate="G$1" pin="AGND3" pad="41"/>
<connect gate="G$1" pin="AGND4" pad="47"/>
<connect gate="G$1" pin="AVDD1" pad="38"/>
<connect gate="G$1" pin="AVDD2" pad="43"/>
<connect gate="G$1" pin="AVDD3" pad="45"/>
<connect gate="G$1" pin="CVDD1" pad="5"/>
<connect gate="G$1" pin="CVDD2" pad="7"/>
<connect gate="G$1" pin="CVDD3" pad="24"/>
<connect gate="G$1" pin="CVDD4" pad="31"/>
<connect gate="G$1" pin="DGND1" pad="4"/>
<connect gate="G$1" pin="DGND2" pad="16"/>
<connect gate="G$1" pin="DGND3" pad="20"/>
<connect gate="G$1" pin="DGND4" pad="21"/>
<connect gate="G$1" pin="DGND5" pad="22"/>
<connect gate="G$1" pin="DGND6" pad="35"/>
<connect gate="G$1" pin="DREQ" pad="8"/>
<connect gate="G$1" pin="GBUF" pad="42"/>
<connect gate="G$1" pin="GPIO0/I2S_SCLK" pad="33"/>
<connect gate="G$1" pin="GPIO1/I2S_SDATA" pad="34"/>
<connect gate="G$1" pin="GPIO2/DCLK" pad="9"/>
<connect gate="G$1" pin="GPIO3/SDATA" pad="10"/>
<connect gate="G$1" pin="GPIO4/I2S_LROUT" pad="36"/>
<connect gate="G$1" pin="GPIO5/I2C_MCLK" pad="25"/>
<connect gate="G$1" pin="GPIO6" pad="11"/>
<connect gate="G$1" pin="GPIO7" pad="12"/>
<connect gate="G$1" pin="IOVDD1" pad="6"/>
<connect gate="G$1" pin="IOVDD2" pad="14"/>
<connect gate="G$1" pin="IOVDD3" pad="19"/>
<connect gate="G$1" pin="LEFT" pad="46"/>
<connect gate="G$1" pin="LINEIN" pad="48"/>
<connect gate="G$1" pin="MICN" pad="2"/>
<connect gate="G$1" pin="MICP" pad="1"/>
<connect gate="G$1" pin="RCAP" pad="44"/>
<connect gate="G$1" pin="RIGHT" pad="39"/>
<connect gate="G$1" pin="RX" pad="26"/>
<connect gate="G$1" pin="S0" pad="30"/>
<connect gate="G$1" pin="SCLK" pad="28"/>
<connect gate="G$1" pin="SI" pad="29"/>
<connect gate="G$1" pin="TEST" pad="32"/>
<connect gate="G$1" pin="TX" pad="27"/>
<connect gate="G$1" pin="VCO" pad="15"/>
<connect gate="G$1" pin="XCS" pad="23"/>
<connect gate="G$1" pin="XDCS/BSYNC" pad="13"/>
<connect gate="G$1" pin="XRESET" pad="3"/>
<connect gate="G$1" pin="XTAL1/MCLK" pad="18"/>
<connect gate="G$1" pin="XTAL2" pad="17"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-12665"/>
<attribute name="VALUE" value="VS1053B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VS1063">
<description>&lt;h3&gt;MP3 and MIDI Codec - VS1063&lt;/h3&gt;
&lt;p&gt;AAC/MP3/WMA/MIDI/Ogg Audio Player and Ogg Recording Device LQFP-48 7x7x1.4 mm&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Widgets/vs1063ds.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11025"&gt;Storefront component:  MP3 and MIDI Codec - VS1063&lt;/a&gt; (COM-11025)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="VS1033D"/>
</gates>
<devices>
<device name="SMD" package="LQFP-48">
<connects>
<connect gate="G$1" pin="AGND1" pad="37"/>
<connect gate="G$1" pin="AGND2" pad="40"/>
<connect gate="G$1" pin="AGND3" pad="41"/>
<connect gate="G$1" pin="AGND4" pad="47"/>
<connect gate="G$1" pin="AVDD1" pad="38"/>
<connect gate="G$1" pin="AVDD2" pad="43"/>
<connect gate="G$1" pin="AVDD3" pad="45"/>
<connect gate="G$1" pin="CVDD1" pad="5"/>
<connect gate="G$1" pin="CVDD2" pad="7"/>
<connect gate="G$1" pin="CVDD3" pad="24"/>
<connect gate="G$1" pin="CVDD4" pad="31"/>
<connect gate="G$1" pin="DGND1" pad="4"/>
<connect gate="G$1" pin="DGND2" pad="16"/>
<connect gate="G$1" pin="DGND3" pad="20"/>
<connect gate="G$1" pin="DGND4" pad="21"/>
<connect gate="G$1" pin="DGND5" pad="22"/>
<connect gate="G$1" pin="DGND6" pad="35"/>
<connect gate="G$1" pin="DREQ" pad="8"/>
<connect gate="G$1" pin="GBUF" pad="42"/>
<connect gate="G$1" pin="GPIO0/I2S_SCLK" pad="33"/>
<connect gate="G$1" pin="GPIO1/I2S_SDATA" pad="34"/>
<connect gate="G$1" pin="GPIO2/DCLK" pad="9"/>
<connect gate="G$1" pin="GPIO3/SDATA" pad="10"/>
<connect gate="G$1" pin="GPIO4/I2S_LROUT" pad="36"/>
<connect gate="G$1" pin="GPIO5/I2C_MCLK" pad="25"/>
<connect gate="G$1" pin="GPIO6" pad="11"/>
<connect gate="G$1" pin="GPIO7" pad="12"/>
<connect gate="G$1" pin="IOVDD1" pad="6"/>
<connect gate="G$1" pin="IOVDD2" pad="14"/>
<connect gate="G$1" pin="IOVDD3" pad="19"/>
<connect gate="G$1" pin="LEFT" pad="46"/>
<connect gate="G$1" pin="LINEIN" pad="48"/>
<connect gate="G$1" pin="MICN" pad="2"/>
<connect gate="G$1" pin="MICP" pad="1"/>
<connect gate="G$1" pin="RCAP" pad="44"/>
<connect gate="G$1" pin="RIGHT" pad="39"/>
<connect gate="G$1" pin="RX" pad="26"/>
<connect gate="G$1" pin="S0" pad="30"/>
<connect gate="G$1" pin="SCLK" pad="28"/>
<connect gate="G$1" pin="SI" pad="29"/>
<connect gate="G$1" pin="TEST" pad="32"/>
<connect gate="G$1" pin="TX" pad="27"/>
<connect gate="G$1" pin="VCO" pad="15"/>
<connect gate="G$1" pin="XCS" pad="23"/>
<connect gate="G$1" pin="XDCS/BSYNC" pad="13"/>
<connect gate="G$1" pin="XRESET" pad="3"/>
<connect gate="G$1" pin="XTAL1/MCLK" pad="18"/>
<connect gate="G$1" pin="XTAL2" pad="17"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-10870"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WTV020SD" prefix="IC" uservalue="yes">
<description>&lt;h3&gt;WTV020SD Audio Module&lt;/h3&gt;
&lt;p&gt;SD audio playback IC&lt;br&gt;
Can play back .wav or .ad4 files from an SD card&lt;br&gt;
SPI control or digital input trigger control&lt;br&gt;
available in SSOP-20 or DIP-20&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Widgets/WTV020SD.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11125"&gt;SparkFun Audio-Sound Breakout - WTV020SD&lt;/a&gt; (WIG-11125)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="WTV020SD-20S"/>
</gates>
<devices>
<device name="" package="SSOP_20">
<connects>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="NC" pad="9"/>
<connect gate="G$1" pin="OSCI/P10" pad="15"/>
<connect gate="G$1" pin="OSCO/P11" pad="16"/>
<connect gate="G$1" pin="P00" pad="18"/>
<connect gate="G$1" pin="P01" pad="19"/>
<connect gate="G$1" pin="P02" pad="20"/>
<connect gate="G$1" pin="P03" pad="1"/>
<connect gate="G$1" pin="P04" pad="2"/>
<connect gate="G$1" pin="P05" pad="3"/>
<connect gate="G$1" pin="P06" pad="4"/>
<connect gate="G$1" pin="P07" pad="5"/>
<connect gate="G$1" pin="PAD_EQI" pad="11"/>
<connect gate="G$1" pin="PAD_EQO" pad="10"/>
<connect gate="G$1" pin="RESET" pad="17"/>
<connect gate="G$1" pin="SPK_N" pad="8"/>
<connect gate="G$1" pin="SPK_P" pad="7"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VPP" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11012"/>
<attribute name="VALUE" value="WTV020SD-20S"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS1015" prefix="U" uservalue="yes">
<description>&lt;h3&gt;ADS1015 12-BIT ADC&lt;/h3&gt;
&lt;p&gt;12-Bit Del-Sig ADC&lt;br&gt;
Four single-ended inputs or two differential inputs&lt;br&gt;
Internal PGA&lt;br&gt;
I&lt;sup&gt;2&lt;/sup&gt;C interface&lt;br&gt;
2.0-5.5V
&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13770"&gt;SparkFun Block for Intel Edison - ADC&lt;/a&gt; (DEV-13770)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="ADS1015"/>
</gates>
<devices>
<device name="" package="MSOP10">
<connects>
<connect gate="G$1" pin="ADDR" pad="1"/>
<connect gate="G$1" pin="AIN0" pad="4"/>
<connect gate="G$1" pin="AIN1" pad="5"/>
<connect gate="G$1" pin="AIN2" pad="6"/>
<connect gate="G$1" pin="AIN3" pad="7"/>
<connect gate="G$1" pin="ALERT/RDY" pad="2"/>
<connect gate="G$1" pin="SCL" pad="10"/>
<connect gate="G$1" pin="SDA" pad="9"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VSS" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-12270"/>
<attribute name="VALUE" value="ADS1015"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX31855K" prefix="U">
<description>&lt;h3&gt;Cold-Junction-Compensated K-Thermocoupleto-Digital
Converter (-270°C to +1800°C)&lt;/h3&gt;
&lt;p&gt;The MAX31855K performs cold-junction compensation
and digitizes the signal from a type-K thermocouple.&lt;br&gt;
The data is output in a 14-bit resolution, SPI™-compatible,
read-only format.&lt;br&gt;
This converter resolves temperatures to 0.25°C, allows readings as high as +1800°C and as low as -270°C, and exhibits thermocouple accuracy of ±2°C for temperatures ranging from -200°C to +700°C for K-type thermocouples.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Sensors/Temp/MAX31855K.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13266"&gt;SparkFun Thermocouple Breakout - MAX31855K&lt;/a&gt; (SEN-13266)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="MAX31855K"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="!CS" pad="6"/>
<connect gate="G$1" pin="(MI)SO" pad="7"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="SCK" pad="5"/>
<connect gate="G$1" pin="T+" pad="3"/>
<connect gate="G$1" pin="T-" pad="2"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-12578"/>
<attribute name="VALUE" value="MAX31855K"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP4725" prefix="U">
<description>&lt;h3&gt;MCP4725 DAC&lt;/h3&gt;
&lt;p&gt;Microchip 12-bit I2C DAC, SOT23-6&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/BreakoutBoards/MCP4725_2009.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12918"&gt;SparkFun I2C DAC Breakout - MCP4725&lt;/a&gt; (BOB-12918)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="U1" symbol="MCP4725"/>
</gates>
<devices>
<device name="SOT-23" package="SOT23-6">
<connects>
<connect gate="U1" pin="AO" pad="6"/>
<connect gate="U1" pin="SCL" pad="5"/>
<connect gate="U1" pin="SDA" pad="4"/>
<connect gate="U1" pin="VDD" pad="3"/>
<connect gate="U1" pin="VOUT" pad="1"/>
<connect gate="U1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-08886"/>
<attribute name="VALUE" value="MCP4725"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCM1803" prefix="U">
<description>&lt;h3&gt;PCM1803ADB STEREO ADC&lt;/h3&gt;
&lt;p&gt;24-bit&lt;/p&gt;
&lt;p&gt;&lt;a href=""&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;none&lt;/li&gt;
&lt;/ul&gt;
stock = 62</description>
<gates>
<gate name="G$1" symbol="PCM1803A"/>
</gates>
<devices>
<device name="SMD" package="SSOP20">
<connects>
<connect gate="G$1" pin="BCK" pad="11"/>
<connect gate="G$1" pin="BPAS" pad="8"/>
<connect gate="G$1" pin="DOUT" pad="12"/>
<connect gate="G$1" pin="FMT0" pad="17"/>
<connect gate="G$1" pin="FMT1" pad="18"/>
<connect gate="G$1" pin="GNDA" pad="6"/>
<connect gate="G$1" pin="GNDD" pad="13"/>
<connect gate="G$1" pin="LRCK" pad="10"/>
<connect gate="G$1" pin="MD0" pad="19"/>
<connect gate="G$1" pin="MD1" pad="20"/>
<connect gate="G$1" pin="OSR" pad="16"/>
<connect gate="G$1" pin="PDWN" pad="7"/>
<connect gate="G$1" pin="SCK" pad="15"/>
<connect gate="G$1" pin="TEST" pad="9"/>
<connect gate="G$1" pin="VCCA" pad="5"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VINL" pad="1"/>
<connect gate="G$1" pin="VINR" pad="2"/>
<connect gate="G$1" pin="VREF1" pad="3"/>
<connect gate="G$1" pin="VREF2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09251"/>
<attribute name="VALUE" value="PCM1803"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HX711" prefix="U">
<description>&lt;h3&gt;AVIA Semiconductor HX711 - ADC&lt;/h3&gt;
&lt;p&gt;24-Bit Analog-to-Digital Converter for Weigh Scales
&lt;li&gt;&lt;a href=”https://cdn.sparkfun.com/datasheets/Sensors/ForceFlex/hx711_english.pdf”&gt;Datasheet&lt;/a&gt;&lt;/li&gt;
&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13879”&gt;SparkFun Load Cell Amplifier - HX711 &lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="U1" symbol="HX711"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="U1" pin="AGND" pad="5"/>
<connect gate="U1" pin="AVDD" pad="3"/>
<connect gate="U1" pin="BASE" pad="2"/>
<connect gate="U1" pin="DOUT" pad="12"/>
<connect gate="U1" pin="DVDD" pad="16"/>
<connect gate="U1" pin="INA+" pad="8"/>
<connect gate="U1" pin="INA-" pad="7"/>
<connect gate="U1" pin="INB+" pad="10"/>
<connect gate="U1" pin="INB-" pad="9"/>
<connect gate="U1" pin="PD_SCK" pad="11"/>
<connect gate="U1" pin="RATE" pad="15"/>
<connect gate="U1" pin="VBG" pad="6"/>
<connect gate="U1" pin="VFB" pad="4"/>
<connect gate="U1" pin="VSUP" pad="1"/>
<connect gate="U1" pin="XI" pad="14"/>
<connect gate="U1" pin="XO" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-12445"/>
<attribute name="VALUE" value="HX711"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NAU7802" prefix="U">
<description>24-bit load cell conversion IC with I2C interface in SOIC-16 package. Similar to HX711 but with true I2C interface.</description>
<gates>
<gate name="U1" symbol="NAU7802"/>
</gates>
<devices>
<device name="SOIC" package="SO16">
<connects>
<connect gate="U1" pin="AVDD" pad="16"/>
<connect gate="U1" pin="AVSS" pad="8"/>
<connect gate="U1" pin="DRDY" pad="12"/>
<connect gate="U1" pin="DVDD" pad="15"/>
<connect gate="U1" pin="DVSS" pad="9"/>
<connect gate="U1" pin="REFN" pad="7"/>
<connect gate="U1" pin="REFP" pad="1"/>
<connect gate="U1" pin="SCLK" pad="13"/>
<connect gate="U1" pin="SDIO" pad="14"/>
<connect gate="U1" pin="VBG" pad="6"/>
<connect gate="U1" pin="VIN1N" pad="2"/>
<connect gate="U1" pin="VIN1P" pad="3"/>
<connect gate="U1" pin="VIN2N" pad="4"/>
<connect gate="U1" pin="VIN2P" pad="5"/>
<connect gate="U1" pin="XIN" pad="10"/>
<connect gate="U1" pin="XOUT" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-14299"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
