<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<library>
<description>&lt;h3&gt;SparkFun Logic ICs&lt;/h3&gt;
This library contains parts which fit into the standard logic IC families.&lt;br&gt;&lt;br&gt;
This library is special as the devices are most generalized, with manufacturer specific variants stemming from the generalized numbers.  It also uses individual gates for common parts with a power consort.  Place the gates in a schematic such that they are easy to see in the circuit, and apply power to the power symbol for multigate packages. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="SOT353">
<description>&lt;h3&gt;SOT353 aka SC70-5&lt;/h3&gt;
Used on single circuit logic gates</description>
</package>
<package name="LCC20">
<description>&lt;b&gt;Leadless Chip Carrier&lt;/b&gt;&lt;p&gt; Ceramic Package</description>
</package>
<package name="TSSOP16">
<description>&lt;b&gt;TSOP16&lt;/b&gt;&lt;p&gt;
thin small outline package</description>
</package>
<package name="SSOP24">
</package>
<package name="SO14">
</package>
<package name="SO16">
<description>SOIC, 0.15 inch width</description>
</package>
<package name="DIP14-KIT">
</package>
<package name="DIP16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIP16-KIT">
</package>
<package name="DHVQFN-16-2.5X3.5MM">
<description>&lt;h3&gt;16-Pin DHVQFN (SOT763-1) - 2.5 x 3.5 x 0.85 mm&lt;/h3&gt;
&lt;p&gt;Package used by NXP 74HC4051BQ 8-channel analog mux/demux.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cache.nxp.com/documents/reflow_soldering/sot763-1_fr.pdf"&gt;NXP Footprint for reflow soldering&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.nxp.com/documents/data_sheet/74HC_HCT4051.pdf"&gt;Example Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="TSSOP28">
<description>&lt;h3&gt;TSSOP-28 - [Package Short Description]&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 28&lt;/li&gt;
&lt;li&gt;Pin pitch: .65 mm&lt;/li&gt;
&lt;li&gt;Area: 6.6 mm x 7.9 mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=http://www.ti.com/lit/ds/symlink/pca9548a.pdf&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
<symbols>
<symbol name="74595">
<pin name="QB" direction="hiz"/>
<pin name="QC" direction="hiz"/>
<pin name="QD" direction="hiz"/>
<pin name="QE" direction="hiz"/>
<pin name="QF" direction="hiz"/>
<pin name="QG" direction="hiz"/>
<pin name="QH" direction="hiz"/>
<pin name="SCL" direction="in" function="dot"/>
<pin name="SCK" direction="in" function="clk"/>
<pin name="RCK" direction="in" function="clk"/>
<pin name="G" direction="in" function="dot"/>
<pin name="SER" direction="in"/>
<pin name="QA" direction="hiz"/>
<pin name="QH*" direction="hiz"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="74165">
<pin name="B" direction="hiz"/>
<pin name="C" direction="hiz"/>
<pin name="D" direction="hiz"/>
<pin name="E" direction="hiz"/>
<pin name="F" direction="hiz"/>
<pin name="G" direction="hiz"/>
<pin name="H" direction="hiz"/>
<pin name="!QH" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="CLK_INH" direction="in"/>
<pin name="SH/!LD" direction="in"/>
<pin name="SER" direction="in"/>
<pin name="A" direction="hiz"/>
<pin name="QH" direction="hiz"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="CD4013">
<pin name="Q" direction="out"/>
<pin name="!Q" direction="out"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="R" direction="in"/>
<pin name="D" direction="in"/>
<pin name="S" direction="in"/>
</symbol>
<symbol name="CD4017">
<pin name="Q5" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q0" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q8" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q9" direction="out"/>
<pin name="CO" direction="out"/>
<pin name="ENA" direction="in" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="RES" direction="in"/>
</symbol>
<symbol name="TPIC6C595">
<pin name="!CLR" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="RCK" direction="in"/>
<pin name="SER_IN" direction="in"/>
<pin name="SER_OUT" direction="out"/>
<pin name="SRCK" direction="in"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="74HC4052">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="INH" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="VEE" direction="pwr"/>
<pin name="X"/>
<pin name="X0"/>
<pin name="X1"/>
<pin name="X2"/>
<pin name="X3"/>
<pin name="Y"/>
<pin name="Y0"/>
<pin name="Y1"/>
<pin name="Y2"/>
<pin name="Y3"/>
</symbol>
<symbol name="CD74HC4067">
<pin name="COM"/>
<pin name="CHAN7"/>
<pin name="CHAN6"/>
<pin name="CHAN5"/>
<pin name="CHAN4"/>
<pin name="CHAN3"/>
<pin name="CHAN2"/>
<pin name="CHAN1"/>
<pin name="CHAN0"/>
<pin name="S0" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="GND"/>
<pin name="S3" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="EN" direction="in" function="dot"/>
<pin name="CHAN15"/>
<pin name="CHAN14"/>
<pin name="CHAN13"/>
<pin name="CHAN12"/>
<pin name="CHAN11"/>
<pin name="CHAN10"/>
<pin name="CHAN9"/>
<pin name="CHAN8"/>
<pin name="VCC"/>
</symbol>
<symbol name="GATE_OR_2">
<pin name="B"/>
<pin name="A"/>
<pin name="Y"/>
</symbol>
<symbol name="GATE_AND_2">
<pin name="B"/>
<pin name="A"/>
<pin name="Y"/>
</symbol>
<symbol name="GATE_INVERTER">
<pin name="Y"/>
<pin name="A"/>
</symbol>
<symbol name="GATE_INVERTER_WITH_ENABLE">
<pin name="Y"/>
<pin name="A"/>
<pin name="!EN"/>
</symbol>
<symbol name="GATE_INVERTER_SCHMITT_TRIGGER">
<pin name="Y"/>
<pin name="A"/>
</symbol>
<symbol name="POWER_CONSORT">
<pin name="P$V+"/>
<pin name="P$V-"/>
</symbol>
<symbol name="74HC4051">
<description>&lt;h3&gt;NXP 74HC4051 8-Channel Analog Multiplexer/Demultiplexer&lt;/h3&gt;
&lt;p&gt;The 74HC4051; 74HCT4051 is a single-pole octal-throw analog switch (SP8T) suitable for use in analog or digital 8:1 multiplexer/demultiplexer applications. The switch features three digital select inputs (S0, S1 and S2), eight independent inputs/outputs (Yn), a common input/output (Z) and a digital enable input (E). When E is HIGH, the switches are turned off. Inputs include clamp diodes. This enables the use of current limiting resistors to interface inputs to voltages in excess of VCC.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.nxp.com/documents/data_sheet/74HC_HCT4051.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
<pin name="S0"/>
<pin name="S1"/>
<pin name="S2"/>
<pin name="VEE"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="Y0"/>
<pin name="Y1"/>
<pin name="Y2"/>
<pin name="Y3"/>
<pin name="Y4"/>
<pin name="Y5"/>
<pin name="Y6"/>
<pin name="Y7"/>
<pin name="Z"/>
<pin name="!E!"/>
</symbol>
<symbol name="SN74LVC1G66_SPST_AMUX">
<pin name="A_IN"/>
<pin name="CTRL_IN"/>
<pin name="A_OUT"/>
<pin name="VSS"/>
<pin name="VCC"/>
</symbol>
<symbol name="TCA9548A">
<description>&lt;h3&gt;Texas Instruments PCA9548A - I2C Multiplexer&lt;/h3&gt;
&lt;p&gt;The PCA9548A device has eight bidirectional
translating switches that can be controlled through
the I2C bus. The SCL/SDA upstream pair fans out to
eight downstream pairs, or channels. Any individual
SCn/SDn channel or combination of channels can be
selected, determined by the contents of the
programmable control register. These downstream
channels can be used to resolve I2C slave address
conflicts.&lt;/p&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<pin name="SD0"/>
<pin name="A1"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="A0"/>
<pin name="VCC"/>
<pin name="A2"/>
<pin name="!RST"/>
<pin name="GND"/>
<pin name="SD3"/>
<pin name="SD5"/>
<pin name="SC5"/>
<pin name="SC2"/>
<pin name="SC4"/>
<pin name="SD4"/>
<pin name="SC3"/>
<pin name="SD2"/>
<pin name="SD1"/>
<pin name="SD7"/>
<pin name="SC7"/>
<pin name="SC0"/>
<pin name="SC6"/>
<pin name="SD6"/>
<pin name="SC1"/>
</symbol>
<symbol name="MUX_1:1_X4">
<pin name="1Y"/>
<pin name="1E"/>
<pin name="2Y"/>
<pin name="2E"/>
<pin name="3Y"/>
<pin name="3E"/>
<pin name="4Y"/>
<pin name="4E"/>
<pin name="1Z"/>
<pin name="2Z"/>
<pin name="3Z"/>
<pin name="4Z"/>
<pin name="VCC"/>
<pin name="GND"/>
</symbol>
<symbol name="GATE_BUFFER_WITH_ENABLE">
<pin name="Y"/>
<pin name="A"/>
<pin name="!EN"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="74*08" prefix="U" uservalue="yes">
<description>&lt;h3&gt;Single AND gate&lt;/h3&gt;
&lt;p&gt;IC GATE AND SNGL 2INPUT SOT353&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11006"&gt;SparkFun LogicBlocks Kit&lt;/a&gt; (KIT-11006)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12097"&gt;SparkFun RedBot Mainboard&lt;/a&gt; (ROB-12097)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G1" symbol="GATE_AND_2"/>
<gate name="G2" symbol="POWER_CONSORT"/>
</gates>
<devices>
<device name="SE" package="SOT23-5">
<connects>
<connect gate="G1" pin="A" pad="1"/>
<connect gate="G1" pin="B" pad="2"/>
<connect gate="G1" pin="Y" pad="4"/>
<connect gate="G2" pin="P$V+" pad="5"/>
<connect gate="G2" pin="P$V-" pad="3"/>
</connects>
<technologies>
<technology name="LVC">
<attribute name="PROD_ID" value="IC-10841"/>
<attribute name="VALUE" value="74LVC1G08SE"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*32" prefix="U" uservalue="yes">
<description>&lt;h3&gt;Single OR gate&lt;/h3&gt;
&lt;p&gt;IC POSITIVE-OR GATE 2-IN SC-70&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13899"&gt;SparkFun Stepoko&lt;/a&gt; (ROB-13899)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11006"&gt;SparkFun LogicBlocks Kit&lt;/a&gt; (KIT-11006)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G1" symbol="GATE_OR_2"/>
<gate name="G2" symbol="POWER_CONSORT"/>
</gates>
<devices>
<device name="" package="SOT353">
<connects>
<connect gate="G1" pin="A" pad="1"/>
<connect gate="G1" pin="B" pad="2"/>
<connect gate="G1" pin="Y" pad="4"/>
<connect gate="G2" pin="P$V+" pad="5"/>
<connect gate="G2" pin="P$V-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-10842"/>
<attribute name="VALUE" value="SN74LVC1G32DCKR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*125" prefix="U" uservalue="yes">
<description>&lt;h3&gt;Quad inverter with enable&lt;/h3&gt;
&lt;p&gt;BUFF TRI-ST QD N-INV 14SOIC&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9825"&gt;Pocket AVR Programmer&lt;/a&gt; (PGM-09825)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13582"&gt;SparkFun Line Follower Array&lt;/a&gt; (SEN-13582)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G0" symbol="GATE_INVERTER_WITH_ENABLE"/>
<gate name="G1" symbol="GATE_INVERTER_WITH_ENABLE"/>
<gate name="G2" symbol="GATE_INVERTER_WITH_ENABLE"/>
<gate name="G3" symbol="GATE_INVERTER_WITH_ENABLE"/>
<gate name="PWR" symbol="POWER_CONSORT"/>
</gates>
<devices>
<device name="DG" package="SO14">
<connects>
<connect gate="G0" pin="!EN" pad="1"/>
<connect gate="G0" pin="A" pad="2"/>
<connect gate="G0" pin="Y" pad="3"/>
<connect gate="G1" pin="!EN" pad="4"/>
<connect gate="G1" pin="A" pad="5"/>
<connect gate="G1" pin="Y" pad="6"/>
<connect gate="G2" pin="!EN" pad="13"/>
<connect gate="G2" pin="A" pad="12"/>
<connect gate="G2" pin="Y" pad="11"/>
<connect gate="G3" pin="!EN" pad="10"/>
<connect gate="G3" pin="A" pad="9"/>
<connect gate="G3" pin="Y" pad="8"/>
<connect gate="PWR" pin="P$V+" pad="14"/>
<connect gate="PWR" pin="P$V-" pad="7"/>
</connects>
<technologies>
<technology name="AC">
<attribute name="PROD_ID" value="IC-08880"/>
<attribute name="VALUE" value="MC74AC125DG"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*1G04" prefix="U" uservalue="yes">
<description>&lt;h3&gt;Single Inverter&lt;/h3&gt;
&lt;p&gt;IC NOT GATE INVERTER SNGL 1IN SOT353&lt;br&gt;
Supply: 1.65V to 5.5V
&lt;/p&gt;
&lt;p&gt;&lt;a href="http://diodes.com/datasheets/74LVC1G04.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13899"&gt;SparkFun Stepoko&lt;/a&gt; (ROB-13899)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13183"&gt;SparkFun CryptoShield&lt;/a&gt; (DEV-13183)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11006"&gt;SparkFun LogicBlocks Kit&lt;/a&gt; (KIT-11006)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9815"&gt;SparkFun ArduMoto&lt;/a&gt; (DEV-09815)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G1" symbol="GATE_INVERTER"/>
<gate name="G2" symbol="POWER_CONSORT"/>
</gates>
<devices>
<device name="SE" package="SOT353">
<connects>
<connect gate="G1" pin="A" pad="2"/>
<connect gate="G1" pin="Y" pad="4"/>
<connect gate="G2" pin="P$V+" pad="5"/>
<connect gate="G2" pin="P$V-" pad="3"/>
</connects>
<technologies>
<technology name="LVC">
<attribute name="PROD_ID" value="IC-10843"/>
<attribute name="VALUE" value="74LVC1G04SE"/>
</technology>
</technologies>
</device>
<device name="" package="SOT353">
<connects>
<connect gate="G1" pin="A" pad="2"/>
<connect gate="G1" pin="Y" pad="4"/>
<connect gate="G2" pin="P$V+" pad="5"/>
<connect gate="G2" pin="P$V-" pad="3"/>
</connects>
<technologies>
<technology name="HC">
<attribute name="PROD_ID" value="COMP-08268"/>
<attribute name="VALUE" value="74HC1G04"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*1G125" prefix="U" uservalue="yes">
<description>&lt;h3&gt;Single buffer&lt;/h3&gt;
&lt;p&gt;Buffers &amp; Line Drivers Tri-State Single Bus SOT-23-5&lt;/p&gt;
&lt;p&gt;&lt;a href=""&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13664"&gt;SparkFun SAMD21 Mini Breakout&lt;/a&gt; (DEV-13664)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13672"&gt;SparkFun SAMD21 Dev Breakout&lt;/a&gt; (DEV-13672)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12898"&gt;SparkFun MIDI Shield&lt;/a&gt; (DEV-12898)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12071"&gt;SparkFun WiFi Shield - CC3000&lt;/a&gt; (DEV-12071)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G2" symbol="POWER_CONSORT"/>
<gate name="G$1" symbol="GATE_BUFFER_WITH_ENABLE"/>
</gates>
<devices>
<device name="D" package="SOT23-5">
<connects>
<connect gate="G$1" pin="!EN" pad="1"/>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="Y" pad="4"/>
<connect gate="G2" pin="P$V+" pad="5"/>
<connect gate="G2" pin="P$V-" pad="3"/>
</connects>
<technologies>
<technology name="AHC">
<attribute name="PROD_ID" value="IC-11920"/>
<attribute name="VALUE" value="SN74AHC1G125"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*165" prefix="U" uservalue="yes">
<description>&lt;h3&gt;8-Bit Shift Register (Parallel to Serial)&lt;/h3&gt;
&lt;p&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/BreakoutBoards/sn54hc165.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11733"&gt;SparkFun Shift-In Breakout - SN74HC165&lt;/a&gt; (BOB-11733)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="U1" symbol="74165"/>
</gates>
<devices>
<device name="D" package="SO16">
<connects>
<connect gate="U1" pin="!QH" pad="7"/>
<connect gate="U1" pin="A" pad="11"/>
<connect gate="U1" pin="B" pad="12"/>
<connect gate="U1" pin="C" pad="13"/>
<connect gate="U1" pin="CLK" pad="2"/>
<connect gate="U1" pin="CLK_INH" pad="15"/>
<connect gate="U1" pin="D" pad="14"/>
<connect gate="U1" pin="E" pad="3"/>
<connect gate="U1" pin="F" pad="4"/>
<connect gate="U1" pin="G" pad="5"/>
<connect gate="U1" pin="GND" pad="8"/>
<connect gate="U1" pin="H" pad="6"/>
<connect gate="U1" pin="QH" pad="9"/>
<connect gate="U1" pin="SER" pad="10"/>
<connect gate="U1" pin="SH/!LD" pad="1"/>
<connect gate="U1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="HC">
<attribute name="PROD_ID" value="IC-11325"/>
<attribute name="VALUE" value="SN74HC165DR"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*595" prefix="U" uservalue="yes">
<description>&lt;h3&gt;8-Bit Shift Register (Serial to Parallel)&lt;/h3&gt;
&lt;p&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/BreakoutBoards/MM74HC595.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10680"&gt;SparkFun Shift Register Breakout - 74HC595&lt;/a&gt; (BOB-10680)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="U1" symbol="74595"/>
</gates>
<devices>
<device name="N" package="DIP16">
<connects>
<connect gate="U1" pin="G" pad="13"/>
<connect gate="U1" pin="GND" pad="8"/>
<connect gate="U1" pin="QA" pad="15"/>
<connect gate="U1" pin="QB" pad="1"/>
<connect gate="U1" pin="QC" pad="2"/>
<connect gate="U1" pin="QD" pad="3"/>
<connect gate="U1" pin="QE" pad="4"/>
<connect gate="U1" pin="QF" pad="5"/>
<connect gate="U1" pin="QG" pad="6"/>
<connect gate="U1" pin="QH" pad="7"/>
<connect gate="U1" pin="QH*" pad="9"/>
<connect gate="U1" pin="RCK" pad="12"/>
<connect gate="U1" pin="SCK" pad="11"/>
<connect gate="U1" pin="SCL" pad="10"/>
<connect gate="U1" pin="SER" pad="14"/>
<connect gate="U1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="HC">
<attribute name="PROD_ID" value="IC-13123"/>
<attribute name="VALUE" value="SN74HC595N "/>
</technology>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="U1" pin="G" pad="13"/>
<connect gate="U1" pin="GND" pad="8"/>
<connect gate="U1" pin="QA" pad="15"/>
<connect gate="U1" pin="QB" pad="1"/>
<connect gate="U1" pin="QC" pad="2"/>
<connect gate="U1" pin="QD" pad="3"/>
<connect gate="U1" pin="QE" pad="4"/>
<connect gate="U1" pin="QF" pad="5"/>
<connect gate="U1" pin="QG" pad="6"/>
<connect gate="U1" pin="QH" pad="7"/>
<connect gate="U1" pin="QH*" pad="9"/>
<connect gate="U1" pin="RCK" pad="12"/>
<connect gate="U1" pin="SCK" pad="11"/>
<connect gate="U1" pin="SCL" pad="10"/>
<connect gate="U1" pin="SER" pad="14"/>
<connect gate="U1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="HC">
<attribute name="PROD_ID" value="IC-07875"/>
<attribute name="VALUE" value="SN74HC595D"/>
</technology>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="U1" pin="G" pad="17"/>
<connect gate="U1" pin="GND" pad="10"/>
<connect gate="U1" pin="QA" pad="19"/>
<connect gate="U1" pin="QB" pad="2"/>
<connect gate="U1" pin="QC" pad="3"/>
<connect gate="U1" pin="QD" pad="4"/>
<connect gate="U1" pin="QE" pad="5"/>
<connect gate="U1" pin="QF" pad="7"/>
<connect gate="U1" pin="QG" pad="8"/>
<connect gate="U1" pin="QH" pad="9"/>
<connect gate="U1" pin="QH*" pad="12"/>
<connect gate="U1" pin="RCK" pad="15"/>
<connect gate="U1" pin="SCK" pad="14"/>
<connect gate="U1" pin="SCL" pad="13"/>
<connect gate="U1" pin="SER" pad="18"/>
<connect gate="U1" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="" package="TSSOP16">
<connects>
<connect gate="U1" pin="G" pad="13"/>
<connect gate="U1" pin="GND" pad="8"/>
<connect gate="U1" pin="QA" pad="15"/>
<connect gate="U1" pin="QB" pad="1"/>
<connect gate="U1" pin="QC" pad="2"/>
<connect gate="U1" pin="QD" pad="3"/>
<connect gate="U1" pin="QE" pad="4"/>
<connect gate="U1" pin="QF" pad="5"/>
<connect gate="U1" pin="QG" pad="6"/>
<connect gate="U1" pin="QH" pad="7"/>
<connect gate="U1" pin="QH*" pad="9"/>
<connect gate="U1" pin="RCK" pad="12"/>
<connect gate="U1" pin="SCK" pad="11"/>
<connect gate="U1" pin="SCL" pad="10"/>
<connect gate="U1" pin="SER" pad="14"/>
<connect gate="U1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*4052" prefix="U" uservalue="yes">
<description>&lt;h3&gt;Dual 4:1 Analog Mux&lt;/h3&gt;
&lt;p&gt;Dual four-channel analog MULTIPLEXER / DEMULTIPLEXER&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12858"&gt;SparkFun Vernier Interface Shield&lt;/a&gt; (DEV-12858)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="U1" symbol="74HC4052"/>
</gates>
<devices>
<device name="D" package="SO16">
<connects>
<connect gate="U1" pin="A" pad="10"/>
<connect gate="U1" pin="B" pad="9"/>
<connect gate="U1" pin="GND" pad="8"/>
<connect gate="U1" pin="INH" pad="6"/>
<connect gate="U1" pin="VCC" pad="16"/>
<connect gate="U1" pin="VEE" pad="7"/>
<connect gate="U1" pin="X" pad="13"/>
<connect gate="U1" pin="X0" pad="12"/>
<connect gate="U1" pin="X1" pad="14"/>
<connect gate="U1" pin="X2" pad="15"/>
<connect gate="U1" pin="X3" pad="11"/>
<connect gate="U1" pin="Y" pad="3"/>
<connect gate="U1" pin="Y0" pad="1"/>
<connect gate="U1" pin="Y1" pad="5"/>
<connect gate="U1" pin="Y2" pad="2"/>
<connect gate="U1" pin="Y3" pad="4"/>
</connects>
<technologies>
<technology name="HC">
<attribute name="PROD_ID" value="IC-13103"/>
<attribute name="VALUE" value="74HC4052D"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*4067" prefix="U" uservalue="yes">
<description>&lt;h3&gt;16-channel analog MUX&lt;/h3&gt;
&lt;p&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.sparkfun.com/datasheets/IC/cd74hc4067.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13720"&gt;MP3 Trigger&lt;/a&gt; (WIG-13720)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9056"&gt;SparkFun Analog/Digital MUX Breakout - CD74HC4067&lt;/a&gt; (BOB-09056)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="U1" symbol="CD74HC4067"/>
</gates>
<devices>
<device name="SM96" package="SSOP24">
<connects>
<connect gate="U1" pin="CHAN0" pad="9"/>
<connect gate="U1" pin="CHAN1" pad="8"/>
<connect gate="U1" pin="CHAN10" pad="21"/>
<connect gate="U1" pin="CHAN11" pad="20"/>
<connect gate="U1" pin="CHAN12" pad="19"/>
<connect gate="U1" pin="CHAN13" pad="18"/>
<connect gate="U1" pin="CHAN14" pad="17"/>
<connect gate="U1" pin="CHAN15" pad="16"/>
<connect gate="U1" pin="CHAN2" pad="7"/>
<connect gate="U1" pin="CHAN3" pad="6"/>
<connect gate="U1" pin="CHAN4" pad="5"/>
<connect gate="U1" pin="CHAN5" pad="4"/>
<connect gate="U1" pin="CHAN6" pad="3"/>
<connect gate="U1" pin="CHAN7" pad="2"/>
<connect gate="U1" pin="CHAN8" pad="23"/>
<connect gate="U1" pin="CHAN9" pad="22"/>
<connect gate="U1" pin="COM" pad="1"/>
<connect gate="U1" pin="EN" pad="15"/>
<connect gate="U1" pin="GND" pad="12"/>
<connect gate="U1" pin="S0" pad="10"/>
<connect gate="U1" pin="S1" pad="11"/>
<connect gate="U1" pin="S2" pad="14"/>
<connect gate="U1" pin="S3" pad="13"/>
<connect gate="U1" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="HC">
<attribute name="PROD_ID" value="IC-08252"/>
<attribute name="VALUE" value="CD74HC4067SM96"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*7014" prefix="U" uservalue="yes">
<description>&lt;h3&gt;Schmitt-trigger Hex Buffer&lt;/h3&gt;
&lt;p&gt;The 74HC7014 is a hex buffer with precision Schmitt-trigger inputs. The precisely defined&lt;br&gt;
trigger levels are lying in a window between (0.55 x VCC) and (0.65 x VCC). It makes the&lt;br&gt;
circuit suitable to operate in a highly noisy environment. Input shorts are allowed to -1.5 V&lt;br&gt;
and +16 V without disturbing other channels. Inputs include clamp diodes that enable the&lt;br&gt;
use of current limiting resistors to interface inputs to voltages in excess of VCC. Schmitt&lt;br&gt;
trigger inputs transform slowly changing input signals into sharply defined jitter-free output&lt;br&gt;
signals.
&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13899"&gt;SparkFun Stepoko&lt;/a&gt; (ROB-13899)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G1" symbol="GATE_INVERTER_SCHMITT_TRIGGER"/>
<gate name="G2" symbol="GATE_INVERTER_SCHMITT_TRIGGER"/>
<gate name="G3" symbol="GATE_INVERTER_SCHMITT_TRIGGER"/>
<gate name="G4" symbol="GATE_INVERTER_SCHMITT_TRIGGER"/>
<gate name="G5" symbol="GATE_INVERTER_SCHMITT_TRIGGER"/>
<gate name="G6" symbol="GATE_INVERTER_SCHMITT_TRIGGER"/>
<gate name="G7" symbol="POWER_CONSORT"/>
</gates>
<devices>
<device name="D" package="SO14">
<connects>
<connect gate="G1" pin="A" pad="1"/>
<connect gate="G1" pin="Y" pad="2"/>
<connect gate="G2" pin="A" pad="3"/>
<connect gate="G2" pin="Y" pad="4"/>
<connect gate="G3" pin="A" pad="5"/>
<connect gate="G3" pin="Y" pad="6"/>
<connect gate="G4" pin="A" pad="9"/>
<connect gate="G4" pin="Y" pad="8"/>
<connect gate="G5" pin="A" pad="11"/>
<connect gate="G5" pin="Y" pad="10"/>
<connect gate="G6" pin="A" pad="13"/>
<connect gate="G6" pin="Y" pad="12"/>
<connect gate="G7" pin="P$V+" pad="14"/>
<connect gate="G7" pin="P$V-" pad="7"/>
</connects>
<technologies>
<technology name="HC">
<attribute name="PROD_ID" value=" IC-12527"/>
<attribute name="VALUE" value="74HC7014D"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CD4013" prefix="U" uservalue="yes">
<description>&lt;h3&gt;Dual D-type Flip-Flop&lt;/h3&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Kits/CD4013B.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11177"&gt;SparkFun SparkPunk Sound Kit&lt;/a&gt; (KIT-11177)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12707"&gt;SparkFun SparkPunk Sequencer Kit&lt;/a&gt; (KIT-12707)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G1" symbol="CD4013"/>
<gate name="G2" symbol="CD4013"/>
<gate name="G3" symbol="POWER_CONSORT"/>
</gates>
<devices>
<device name="" package="DIP14-KIT">
<connects>
<connect gate="G1" pin="!Q" pad="2"/>
<connect gate="G1" pin="CLK" pad="3"/>
<connect gate="G1" pin="D" pad="5"/>
<connect gate="G1" pin="Q" pad="1"/>
<connect gate="G1" pin="R" pad="4"/>
<connect gate="G1" pin="S" pad="6"/>
<connect gate="G2" pin="!Q" pad="12"/>
<connect gate="G2" pin="CLK" pad="11"/>
<connect gate="G2" pin="D" pad="9"/>
<connect gate="G2" pin="Q" pad="13"/>
<connect gate="G2" pin="R" pad="10"/>
<connect gate="G2" pin="S" pad="8"/>
<connect gate="G3" pin="P$V+" pad="14"/>
<connect gate="G3" pin="P$V-" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11896"/>
<attribute name="VALUE" value="CD4013B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CD4017" prefix="U" uservalue="yes">
<description>&lt;h3&gt;10-Out Decade Counter&lt;/h3&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Kits/cd4022b.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12707"&gt;SparkFun SparkPunk Sequencer Kit&lt;/a&gt; (KIT-12707)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G1" symbol="CD4017"/>
<gate name="G2" symbol="POWER_CONSORT"/>
</gates>
<devices>
<device name="" package="DIP16">
<connects>
<connect gate="G1" pin="CLK" pad="14"/>
<connect gate="G1" pin="CO" pad="12"/>
<connect gate="G1" pin="ENA" pad="13"/>
<connect gate="G1" pin="Q0" pad="3"/>
<connect gate="G1" pin="Q1" pad="2"/>
<connect gate="G1" pin="Q2" pad="4"/>
<connect gate="G1" pin="Q3" pad="7"/>
<connect gate="G1" pin="Q4" pad="10"/>
<connect gate="G1" pin="Q5" pad="1"/>
<connect gate="G1" pin="Q6" pad="5"/>
<connect gate="G1" pin="Q7" pad="6"/>
<connect gate="G1" pin="Q8" pad="9"/>
<connect gate="G1" pin="Q9" pad="11"/>
<connect gate="G1" pin="RES" pad="15"/>
<connect gate="G2" pin="P$V+" pad="16"/>
<connect gate="G2" pin="P$V-" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11929"/>
<attribute name="VALUE" value="CD4017"/>
</technology>
</technologies>
</device>
<device name="KIT" package="DIP16-KIT">
<connects>
<connect gate="G1" pin="CLK" pad="14"/>
<connect gate="G1" pin="CO" pad="12"/>
<connect gate="G1" pin="ENA" pad="13"/>
<connect gate="G1" pin="Q0" pad="3"/>
<connect gate="G1" pin="Q1" pad="2"/>
<connect gate="G1" pin="Q2" pad="4"/>
<connect gate="G1" pin="Q3" pad="7"/>
<connect gate="G1" pin="Q4" pad="10"/>
<connect gate="G1" pin="Q5" pad="1"/>
<connect gate="G1" pin="Q6" pad="5"/>
<connect gate="G1" pin="Q7" pad="6"/>
<connect gate="G1" pin="Q8" pad="9"/>
<connect gate="G1" pin="Q9" pad="11"/>
<connect gate="G1" pin="RES" pad="15"/>
<connect gate="G2" pin="P$V+" pad="16"/>
<connect gate="G2" pin="P$V-" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11929"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPIC6C596" prefix="U" uservalue="yes">
<description>&lt;h3&gt;Serial in shift register with open collector outputs&lt;/h3&gt;
&lt;p&gt;This can sink up to 100mA per channel&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Widgets/TPIC6C596.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13279"&gt;SparkFun Large Digit Driver&lt;/a&gt; (WIG-13279)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="U1" symbol="TPIC6C595"/>
</gates>
<devices>
<device name="SOIC" package="SO16">
<connects>
<connect gate="U1" pin="!CLR" pad="7"/>
<connect gate="U1" pin="!G" pad="8"/>
<connect gate="U1" pin="D0" pad="3"/>
<connect gate="U1" pin="D1" pad="4"/>
<connect gate="U1" pin="D2" pad="5"/>
<connect gate="U1" pin="D3" pad="6"/>
<connect gate="U1" pin="D4" pad="11"/>
<connect gate="U1" pin="D5" pad="12"/>
<connect gate="U1" pin="D6" pad="13"/>
<connect gate="U1" pin="D7" pad="14"/>
<connect gate="U1" pin="GND" pad="16"/>
<connect gate="U1" pin="RCK" pad="10"/>
<connect gate="U1" pin="SER_IN" pad="2"/>
<connect gate="U1" pin="SER_OUT" pad="9"/>
<connect gate="U1" pin="SRCK" pad="15"/>
<connect gate="U1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-12522"/>
<attribute name="VALUE" value="TPIC6C596"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*4051" prefix="U" uservalue="yes">
<description>&lt;h3&gt;NXP 74HC4051 8-Channel Analog Multiplexer/Demultiplexer&lt;/h3&gt;
&lt;p&gt;The 74HC4051; 74HCT4051 is a single-pole octal-throw analog switch (SP8T) suitable for use in analog or digital 8:1 multiplexer/demultiplexer applications. The switch features three digital select inputs (S0, S1 and S2), eight independent inputs/outputs (Yn), a common input/output (Z) and a digital enable input (E). When E is HIGH, the switches are turned off. Inputs include clamp diodes. This enables the use of current limiting resistors to interface inputs to voltages in excess of VCC.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.nxp.com/documents/data_sheet/74HC_HCT4051.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="74HC4051"/>
</gates>
<devices>
<device name="BQ" package="DHVQFN-16-2.5X3.5MM">
<connects>
<connect gate="G$1" pin="!E!" pad="6"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="S0" pad="11"/>
<connect gate="G$1" pin="S1" pad="10"/>
<connect gate="G$1" pin="S2" pad="9"/>
<connect gate="G$1" pin="VCC" pad="16 EP"/>
<connect gate="G$1" pin="VEE" pad="7"/>
<connect gate="G$1" pin="Y0" pad="13"/>
<connect gate="G$1" pin="Y1" pad="14"/>
<connect gate="G$1" pin="Y2" pad="15"/>
<connect gate="G$1" pin="Y3" pad="12"/>
<connect gate="G$1" pin="Y4" pad="1"/>
<connect gate="G$1" pin="Y5" pad="5"/>
<connect gate="G$1" pin="Y6" pad="2"/>
<connect gate="G$1" pin="Y7" pad="4"/>
<connect gate="G$1" pin="Z" pad="3"/>
</connects>
<technologies>
<technology name="HC">
<attribute name="PROD_ID" value="IC-13334"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*1G66" prefix="U" uservalue="yes">
<description>&lt;h3&gt;SN74LVC1G66 - SPST NO Analog Switch&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;10-Ohm on resistance&lt;/li&gt;
&lt;li&gt;1.65-5.5V&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;

&lt;p&gt;&lt;a href=”http://www.ti.com/lit/ds/symlink/sn74lvc1g66.pdf”&gt;TI Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Spectacle&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SN74LVC1G66_SPST_AMUX"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="A_IN" pad="1"/>
<connect gate="G$1" pin="A_OUT" pad="2"/>
<connect gate="G$1" pin="CTRL_IN" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VSS" pad="3"/>
</connects>
<technologies>
<technology name="LVC">
<attribute name="PROD_ID" value="IC-13549"/>
<attribute name="VALUE" value="SN74LVC1G66"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCA9548A" prefix="U">
<description>&lt;h3&gt;Texas Instruments PCA9548A - I2C Multiplexer&lt;/h3&gt;
&lt;p&gt;The PCA9548A device has eight bidirectional
translating switches that can be controlled through
the I2C bus. The SCL/SDA upstream pair fans out to
eight downstream pairs, or channels. Any individual
SCn/SDn channel or combination of channels can be
selected, determined by the contents of the
programmable control register. These downstream
channels can be used to resolve I2C slave address
conflicts.&lt;/p&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="U1" symbol="TCA9548A"/>
</gates>
<devices>
<device name="" package="TSSOP28">
<connects>
<connect gate="U1" pin="!RST" pad="3"/>
<connect gate="U1" pin="A0" pad="1"/>
<connect gate="U1" pin="A1" pad="2"/>
<connect gate="U1" pin="A2" pad="21"/>
<connect gate="U1" pin="GND" pad="12"/>
<connect gate="U1" pin="SC0" pad="5"/>
<connect gate="U1" pin="SC1" pad="7"/>
<connect gate="U1" pin="SC2" pad="9"/>
<connect gate="U1" pin="SC3" pad="11"/>
<connect gate="U1" pin="SC4" pad="14"/>
<connect gate="U1" pin="SC5" pad="16"/>
<connect gate="U1" pin="SC6" pad="18"/>
<connect gate="U1" pin="SC7" pad="20"/>
<connect gate="U1" pin="SCL" pad="22"/>
<connect gate="U1" pin="SD0" pad="4"/>
<connect gate="U1" pin="SD1" pad="6"/>
<connect gate="U1" pin="SD2" pad="8"/>
<connect gate="U1" pin="SD3" pad="10"/>
<connect gate="U1" pin="SD4" pad="13"/>
<connect gate="U1" pin="SD5" pad="15"/>
<connect gate="U1" pin="SD6" pad="17"/>
<connect gate="U1" pin="SD7" pad="19"/>
<connect gate="U1" pin="SDA" pad="23"/>
<connect gate="U1" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-13948"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74LVC4066D_QUAD_BILATERAL_SWITCH">
<description>&lt;h3&gt;Nexperia Quad Bilateral Switch&lt;/h3&gt;
&lt;p&gt;The 74LVC4066 is a high-speed Si-gate CMOS device.
The 74LVC4066 provides four single pole, single-throw analog switch functions. Each
switch has two input/output terminals (nY and nZ) and an active HIGH enable input (nE).
When nE is LOW, the analog switch is turned off.
Schmitt-trigger action at the enable inputs makes the circuit tolerant of slower input rise
and fall times across the entire VCC range from 1.65 V to 5.5 V.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://assets.nexperia.com/documents/data-sheet/74LVC4066.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MUX_1:1_X4"/>
</gates>
<devices>
<device name="" package="SO14">
<connects>
<connect gate="G$1" pin="1E" pad="13"/>
<connect gate="G$1" pin="1Y" pad="1"/>
<connect gate="G$1" pin="1Z" pad="2"/>
<connect gate="G$1" pin="2E" pad="5"/>
<connect gate="G$1" pin="2Y" pad="4"/>
<connect gate="G$1" pin="2Z" pad="3"/>
<connect gate="G$1" pin="3E" pad="6"/>
<connect gate="G$1" pin="3Y" pad="8"/>
<connect gate="G$1" pin="3Z" pad="9"/>
<connect gate="G$1" pin="4E" pad="12"/>
<connect gate="G$1" pin="4Y" pad="11"/>
<connect gate="G$1" pin="4Z" pad="10"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-13944"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
