<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.2">
<drawing>
<library>
<description>&lt;h3&gt;SparkFun Memory ICs&lt;/h3&gt;
This library contains memory ICs.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08">
<description>SOIC, 0.15 inch width</description>
</package>
<package name="SO08-EIAJ">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
<package name="WSON8-6X5MM">
</package>
<package name="SOIC-8">
<description>8-Pin SOIC 208-mil</description>
</package>
</packages>
<symbols>
<symbol name="EEPROM-I2C">
<pin name="GND" direction="pwr"/>
<pin name="WP"/>
<pin name="VCC" direction="pwr"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="A2"/>
<pin name="A0"/>
<pin name="A1"/>
</symbol>
<symbol name="SPI_FLASH">
<description>&lt;h3&gt; Flash &lt;/h3&gt;</description>
<pin name="CS"/>
<pin name="MISO"/>
<pin name="WP"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="HOLD"/>
<pin name="SCK"/>
<pin name="MOSI"/>
</symbol>
<symbol name="W25Q32FV">
<pin name="!CS!"/>
<pin name="!HOLD!(D3)"/>
<pin name="!WP!(D2)"/>
<pin name="GND"/>
<pin name="SCK"/>
<pin name="SI(D0)"/>
<pin name="SO(D1)"/>
<pin name="VCC"/>
</symbol>
<symbol name="SPI_FLASH_DUAL/QUAD">
<description>&lt;h3&gt;SPI Flash Memory - Dual/Quad&lt;/h3&gt;</description>
<pin name="!CS"/>
<pin name="!WP"/>
<pin name="GND"/>
<pin name="SO"/>
<pin name="VCC"/>
<pin name="!HOLD"/>
<pin name="SCK"/>
<pin name="SI"/>
</symbol>
<symbol name="QSPI_FLASH">
<description>&lt;h3&gt;Integrated Silicon Solution Inc. - IS25LP032D-JBLE - 32 MB QSPI Flash&lt;/h3&gt;
&lt;p&gt;The IS25LP032D and IS25WP032D Serial Flash memory offers a versatile storage solution with high flexibility and
performance in a simplified pin count package. ISSI’s “Industry Standard Serial Interface” Flash is for systems that
require limited space, a low pin count, and low power consumption. The device is accessed through a 4-wire SPI
Interface consisting of a Serial Data Input (SI), Serial Data Output (SO), Serial Clock (SCK), and Chip Enable
(CE#) pins, which can also be configured to serve as multi-I/O (see pin descriptions).&lt;/p&gt;</description>
<pin name="SCK"/>
<pin name="MOSI/IO0"/>
<pin name="MISO/IO1"/>
<pin name="WP#/IO2"/>
<pin name="HOLD#/IO3"/>
<pin name="CE#"/>
<pin name="VCC"/>
<pin name="GND"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="EEPROM-I2C" prefix="U">
<description>&lt;h3&gt;I2C EEPROMs, 24LC256 and others&lt;/h3&gt;
&lt;p&gt;24LC256 Series 256 kb I2C 2 Wire (32 k x 8 Bit) 2.5 V Serial EEPROM SMD - SOIC-8
&lt;/p&gt;
&lt;p&gt;&lt;a href=""&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11703"&gt;SparkFun UDB5 - PIC UAV Development Board&lt;/a&gt; (GPS-11703)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="EEPROM-I2C"/>
</gates>
<devices>
<device name="SMD" package="SO08">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09714"/>
<attribute name="VALUE" value="24LC256"/>
</technology>
</technologies>
</device>
<device name="EIAJ" package="SO08-EIAJ">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NA-XXXXX"/>
<attribute name="VALUE" value="I2C EEPROM"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPI_FLASH-X25XX" prefix="U">
<description>&lt;h3&gt;32M Serial Flash Memory&lt;/h3&gt;
&lt;p&gt;8pin SPI Flash series x25xx. Works with devices like W25X32 and BR25L32&lt;/p&gt;
&lt;li&gt;&lt;a href="http://www.macronix.com/Lists/Datasheet/Attachments/5031/MX25L3206E,%203V,%2032Mb,%20v1.5.pdf"&gt;Datasheet&lt;/a&gt;&lt;/li&gt;
&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10920"&gt;SparkFun Venus GPS Logger&lt;/a&gt; (GPS-10920)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="SPI_FLASH"/>
</gates>
<devices>
<device name="SMD" package="SO08">
<connects>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="HOLD" pad="7"/>
<connect gate="G$1" pin="MISO" pad="2"/>
<connect gate="G$1" pin="MOSI" pad="5"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="N/A"/>
<attribute name="VALUE" value="32M SPI Flash"/>
</technology>
</technologies>
</device>
<device name="SMD1" package="SO08-EIAJ">
<connects>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="HOLD" pad="7"/>
<connect gate="G$1" pin="MISO" pad="2"/>
<connect gate="G$1" pin="MOSI" pad="5"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09109"/>
<attribute name="VALUE" value="25F32006WSOI"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="W25Q32FV" prefix="U">
<description>&lt;h3&gt;W25Q32FV 32Mb (4MB) Serial Flash Memory&lt;/h3&gt;
&lt;p&gt;The W25Q32FV support the standard Serial Peripheral Interface (SPI), Dual/Quad I/O SPI as  well as 2-clocks instruction cycle Quad Peripheral Interface (QPI).&lt;/p&gt;
&lt;p&gt;104MHz, SPI, 8-SOIC-EIAJ&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.winbond.com/resource-files/w25q32fv%20revh%20091613.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13794"&gt;SparkFun Blynk Board - ESP8266&lt;/a&gt; (WRL-13794)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="W25Q32FV"/>
</gates>
<devices>
<device name="ZP" package="WSON8-6X5MM">
<connects>
<connect gate="G$1" pin="!CS!" pad="1"/>
<connect gate="G$1" pin="!HOLD!(D3)" pad="7"/>
<connect gate="G$1" pin="!WP!(D2)" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="SI(D0)" pad="5"/>
<connect gate="G$1" pin="SO(D1)" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NA-XXXXX"/>
<attribute name="VALUE" value="W25Q32FV"/>
</technology>
</technologies>
</device>
<device name="SS" package="SOIC-8">
<connects>
<connect gate="G$1" pin="!CS!" pad="1"/>
<connect gate="G$1" pin="!HOLD!(D3)" pad="7"/>
<connect gate="G$1" pin="!WP!(D2)" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="SI(D0)" pad="5"/>
<connect gate="G$1" pin="SO(D1)" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-13229"/>
<attribute name="VALUE" value="W25Q32FV"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT25SF041" prefix="U">
<description>&lt;h3&gt;AT25SF041 4Mb Serial Flash Memory&lt;/h3&gt;
&lt;p&gt;104MHz, SPI, 8-SOIC
&lt;li&gt;&lt;a href=”http://www.adestotech.com/wp-content/uploads/DS-AT25SF041_044.pdf”&gt;Datasheet&lt;/a&gt;&lt;/li&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13231”&gt;SparkFun ESP8266 Thing&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13711”&gt;SparkFun ESP8266 Thing - Dev Board&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SPI_FLASH_DUAL/QUAD"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="!CS" pad="1"/>
<connect gate="G$1" pin="!HOLD" pad="7"/>
<connect gate="G$1" pin="!WP" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="SI" pad="5"/>
<connect gate="G$1" pin="SO" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-12455"/>
<attribute name="VALUE" value="4MB Flash"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="QSPI32MBIT" prefix="U">
<description>&lt;h3&gt;Integrated Silicon Solution Inc. IS25LP032D&lt;/h3&gt;
&lt;p&gt;The IS25LP032D Serial Flash memory offers a versatile storage solution with high flexibility and
performance in a simplified pin count package. ISSI’s “Industry Standard Serial Interface” Flash is for systems that
require limited space, a low pin count, and low power consumption. The device is accessed through a 4-wire SPI
Interface consisting of a Serial Data Input (SI), Serial Data Output (SO), Serial Clock (SCK), and Chip Enable
(CE#) pins, which can also be configured to serve as multi-I/O (see pin descriptions). &lt;/p&gt;
&lt;p&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="http://www.issi.com/WW/pdf/25LP-WP032D.pdf"&gt;Datasheet&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="QSPI_FLASH"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="CE#" pad="1"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="HOLD#/IO3" pad="6"/>
<connect gate="G$1" pin="MISO/IO1" pad="2"/>
<connect gate="G$1" pin="MOSI/IO0" pad="8"/>
<connect gate="G$1" pin="SCK" pad="7"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="WP#/IO2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-14501"/>
<attribute name="VALUE" value="32MB"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
