<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<library>
<description>&lt;h3&gt;SparkFun Special Function ICs&lt;/h3&gt;
This library contains ICs that do not really fit into the other, more generic categories.  Basically, anything that serves some function but has a bunch of brains or special bias circuitry that prevents it from being used as a general part qualifies for this category.
&lt;p&gt;Contents:
&lt;ul&gt;&lt;li&gt;555 timers&lt;/li&gt;
&lt;li&gt;LED drivers&lt;/li&gt;
&lt;li&gt;H-Bridge drivers&lt;/li&gt;
&lt;li&gt;Motor drivers&lt;/li&gt;
&lt;li&gt;Waveform generators&lt;/li&gt;
&lt;li&gt;Crypto&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08">
<description>SOIC, 0.15 inch width</description>
</package>
<package name="DIP08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIP08-KIT">
</package>
<package name="DIP14">
</package>
<package name="DIP14-KIT">
</package>
<package name="SSOP16">
</package>
<package name="AD9837">
</package>
<package name="SOT23-3">
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="QFN-10-RSE">
</package>
<package name="TSSOP-28_4MM">
</package>
<package name="QFN-28">
</package>
<package name="DIP18">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;&lt;p&gt;
 package type P</description>
</package>
<package name="SOIC-18">
</package>
<package name="DIL18">
<description>&lt;h3&gt;Dual In Line Package - 18 Pin &lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 18&lt;/li&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LM391&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="PLCC20S">
<description>&lt;h3&gt;PLCC 20 Pin Square&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 20&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=” http://focus.ti.com/en/download/qlty/LAND_PATTERN_RECOMMENDATIONS-MISC.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LM391&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="WQFN-24">
<description>&lt;h3&gt;WQFN - 24 Pin &lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 24&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.ti.com/lit/ds/symlink/lp55231.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LP55231&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="QFN-28-5MM-1:1">
</package>
<package name="QFN-28-5MM_ALT1">
</package>
<package name="QFN-28-5MM_ALT2">
</package>
<package name="QFN-28-5MM_ALT1_REDUCED_PASTE">
</package>
<package name="QFN-28-5MM">
</package>
<package name="HTSSOP28">
</package>
<package name="VSSOP-10">
</package>
<package name="WSON-12">
<description>&lt;h3&gt;WSON-12&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 12&lt;/li&gt;
&lt;li&gt;Area:2mmx3mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.ti.com/lit/ds/symlink/drv8835.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;DRV883X&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="MULTIWATT15">
<description>Multiwatt15V package for the L298 dual full bridge driver</description>
</package>
<package name="MULTIWATT15_6400BGHEATSINK">
</package>
<package name="MULTIWATT15_YB324GHEATSINK">
</package>
<package name="MULTIWATT15_6400BGHEATSINK_2">
</package>
<package name="POWERSO20">
</package>
<package name="SSOP24">
</package>
<package name="VNH2SP30">
</package>
<package name="SO018">
</package>
<package name="SO18L">
</package>
<package name="POWERSO20_L298_PAD">
</package>
<package name="HTSSOP32">
<description>&lt;h3&gt;[HTSSOP-32] - [Package for the TLC5947 PWM driver]&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: [32]&lt;/li&gt;
&lt;li&gt;Pin pitch: [0.65 mm]&lt;/li&gt;
&lt;li&gt;Area: [11.00 mm x 6.20 mm]&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=http://www.ti.com/lit/ds/symlink/tlc5947.pdf&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;[TLC5947]&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="LGA-28">
<description>&lt;h3&gt;LGA-28 - LGA-28 package for the BNO080 IMU&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 28&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.5mm&lt;/li&gt;
&lt;li&gt;Area: 3.8mm X 5.2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.hillcrestlabs.com/download/5a05f340566d07c196001ec1”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/14618”&gt;BNO080&lt;/a&gt;&lt;/li&gt;

&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="MLX90540_MLX90640">
<description>&lt;h3&gt;Melexis MLX90640 Infrared Array&lt;/h3&gt;
&lt;p&gt;
The MLX90640 is a fully calibrated 32x24 pixels
thermal IR array in an industry standard 4-lead TO39
package with digital interface.&lt;/p&gt;
&lt;p&gt;&lt;a href=https://cdn.sparkfun.com/assets/7/b/f/2/d/MLX90640-Datasheet-Melexis.pdf&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="14_PIN_OESIP">
<description>&lt;h3&gt;MAX30101 14 Pin OESIP&lt;/h3&gt;

&lt;p&gt;Phycial Characteristics:&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;3.3 X 5.6 X 1.55 mm&lt;/li&gt;
&lt;li&gt;14 pin - 8mm Pitch&lt;/li&gt;
&lt;li&gt;OESIP&lt;/li&gt;
&lt;/ul&gt;</description>
</package>
<package name="16_PIN_WLP">
<description>&lt;h3&gt;16_PIN_WLP&lt;/h3&gt;

Physical Characteristics
&lt;ul&gt;
&lt;li&gt;1.554 X 1.572 X .64mm &lt;/li&gt;
&lt;li&gt;16 Pins&lt;/li&gt;
&lt;li&gt;.35mm pitch&lt;/li&gt;
&lt;li&gt;WLP Package&lt;/li&gt;
&lt;/ul&gt;</description>
</package>
</packages>
<symbols>
<symbol name="AD5262">
<pin name="A1" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="B1" direction="pas"/>
<pin name="B2" direction="pas"/>
<pin name="CLK" direction="in"/>
<pin name="CS_N" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="PR_N" direction="in"/>
<pin name="SDI" direction="in"/>
<pin name="SDO" direction="out"/>
<pin name="SHDN_N" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="VL" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="W1" direction="pas"/>
<pin name="W2" direction="pas"/>
</symbol>
<symbol name="556_TIMER_DUAL">
<pin name="GND"/>
<pin name="TRIG"/>
<pin name="OUT"/>
<pin name="CV"/>
<pin name="RST"/>
<pin name="THR"/>
<pin name="DIS"/>
<pin name="TRIG2"/>
<pin name="OUT2"/>
<pin name="RST2"/>
<pin name="CV2"/>
<pin name="THR2"/>
<pin name="DIS2"/>
<pin name="VCC"/>
</symbol>
<symbol name="AD9837">
<pin name="SCLK"/>
<pin name="SDATA"/>
<pin name="FSYNC"/>
<pin name="MCLK"/>
<pin name="DGND"/>
<pin name="AGND"/>
<pin name="VOUT"/>
<pin name="COMP"/>
<pin name="VDD"/>
<pin name="CAP/2.5V"/>
</symbol>
<symbol name="INA169">
<pin name="VIN+"/>
<pin name="VIN-"/>
<pin name="V+"/>
<pin name="GND"/>
<pin name="OUT"/>
</symbol>
<symbol name="MCP41XXX">
<pin name="VCC"/>
<pin name="CS"/>
<pin name="SCK"/>
<pin name="DI"/>
<pin name="A"/>
<pin name="W"/>
<pin name="B"/>
<pin name="GND"/>
</symbol>
<symbol name="MSGEQ7">
<pin name="DCOUT"/>
<pin name="CG"/>
<pin name="CKIN"/>
<pin name="GND"/>
<pin name="RESET" direction="in"/>
<pin name="STROBE" direction="in"/>
<pin name="AUDIO_IN" direction="in"/>
<pin name="VDD" direction="in"/>
</symbol>
<symbol name="NE555">
<pin name="TRE" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="DIS" direction="in"/>
<pin name="TRI" direction="in"/>
<pin name="VCC+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="CON" direction="in"/>
<pin name="/RES" direction="in"/>
</symbol>
<symbol name="TS3USB221A">
<pin name="D-"/>
<pin name="D+"/>
<pin name="2D+"/>
<pin name="1D+"/>
<pin name="1D-"/>
<pin name="2D-"/>
<pin name="!OE"/>
<pin name="S"/>
<pin name="VCC"/>
<pin name="VSS"/>
</symbol>
<symbol name="ATAES132">
<pin name="AUTHO"/>
<pin name="GND" direction="pwr"/>
<pin name="NC1" direction="nc"/>
<pin name="NC3" direction="nc"/>
<pin name="NC7" direction="nc"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="ATECC108">
<description>ATECC108</description>
<pin name="GND" direction="pwr"/>
<pin name="NC1"/>
<pin name="NC2" direction="nc"/>
<pin name="NC3" direction="nc"/>
<pin name="NC7" direction="nc"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="ATSHA204-1">
<description>ATSHA204 I2C 8-Lead SOIC</description>
<pin name="GND" direction="pwr"/>
<pin name="NC1" direction="nc"/>
<pin name="NC2" direction="nc"/>
<pin name="NC3" direction="nc"/>
<pin name="NC7" direction="nc"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="ATSHA204">
<pin name="SDA"/>
<pin name="VCC"/>
<pin name="GND"/>
</symbol>
<symbol name="PCA9685">
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="CH0"/>
<pin name="CH1"/>
<pin name="CH2"/>
<pin name="CH3"/>
<pin name="CH4"/>
<pin name="CH5"/>
<pin name="CH6"/>
<pin name="CH7"/>
<pin name="VSS"/>
<pin name="CH8"/>
<pin name="CH9"/>
<pin name="CH10"/>
<pin name="CH11"/>
<pin name="CH12"/>
<pin name="CH13"/>
<pin name="CH14"/>
<pin name="CH15"/>
<pin name="!OE"/>
<pin name="A5"/>
<pin name="EXTCLK"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="VDD"/>
</symbol>
<symbol name="SX1509">
<description>&lt;h3&gt;Semtech SX1509&lt;/h3&gt;
Level Shifting GPIO Expander w/ LED Driver and Keypad Engine</description>
<pin name="VDDM"/>
<pin name="!RESET"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="!INT"/>
<pin name="GND"/>
<pin name="VCC1"/>
<pin name="I/O[0]"/>
<pin name="I/O[1]"/>
<pin name="I/O[2]"/>
<pin name="I/O[3]"/>
<pin name="I/O[4]"/>
<pin name="I/O[5]"/>
<pin name="I/O[6]"/>
<pin name="I/O[7]"/>
<pin name="VCC2"/>
<pin name="I/O[8]"/>
<pin name="I/O[9]"/>
<pin name="I/O[10]"/>
<pin name="I/O[11]"/>
<pin name="I/O[12]"/>
<pin name="I/O[13]"/>
<pin name="I/O[14]"/>
<pin name="I/O[15]"/>
<pin name="OSCIO"/>
<pin name="ADDR0"/>
<pin name="ADDR1"/>
</symbol>
<symbol name="SPEAKJET">
<pin name="E0"/>
<pin name="E1"/>
<pin name="E2"/>
<pin name="E3"/>
<pin name="E4"/>
<pin name="E5"/>
<pin name="E6/RC0"/>
<pin name="E7/RC1"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="RX"/>
<pin name="RST"/>
<pin name="M0"/>
<pin name="M1"/>
<pin name="D0/RDY"/>
<pin name="D1/SPK"/>
<pin name="D2/BHF"/>
<pin name="VOICE"/>
</symbol>
<symbol name="LM3915">
<description>&lt;h3&gt;[Manufacturer (if applicable)] [General Part Number (if applicable)] [Short Part Description (required)]&lt;/h3&gt;
&lt;p&gt;[Few-sentence description of part(s)&lt;/p&gt;</description>
<pin name="LED1" direction="out"/>
<pin name="LED2" direction="out"/>
<pin name="LED3" direction="out"/>
<pin name="LED4" direction="out"/>
<pin name="LED5" direction="out"/>
<pin name="LED6" direction="out"/>
<pin name="LED7" direction="out"/>
<pin name="LED8" direction="out"/>
<pin name="LED9" direction="out"/>
<pin name="LED10" direction="out"/>
<pin name="MODE" direction="in"/>
<pin name="REFADJ" direction="pas"/>
<pin name="REFOUT" direction="out"/>
<pin name="RHI" direction="in"/>
<pin name="RLO" direction="in"/>
<pin name="SIGIN" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="LP55231">
<description>&lt;h3&gt;LP55231 Nine-channel LED Driver&lt;/h3&gt;</description>
<pin name="GND"/>
<pin name="VDD"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="EN"/>
<pin name="CLK"/>
<pin name="!INT"/>
<pin name="!TRIG"/>
<pin name="ASEL0"/>
<pin name="ASEL1"/>
<pin name="B3/D6"/>
<pin name="G3/D5"/>
<pin name="R3/D9"/>
<pin name="B2/D4"/>
<pin name="G2/D3"/>
<pin name="R2/D8"/>
<pin name="B1/D2"/>
<pin name="G1/D1"/>
<pin name="R1/D7"/>
<pin name="VOUT"/>
<pin name="C1+"/>
<pin name="C1-"/>
<pin name="C2+"/>
<pin name="C2-"/>
</symbol>
<symbol name="A4983">
<pin name="CP1"/>
<pin name="CP2"/>
<pin name="DIR" direction="in"/>
<pin name="ENABLE" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND_PAD" direction="pwr"/>
<pin name="MS1" direction="in"/>
<pin name="MS2" direction="in"/>
<pin name="MS3" direction="in"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="OUT1A"/>
<pin name="OUT1B"/>
<pin name="OUT2A"/>
<pin name="OUT2B"/>
<pin name="REF"/>
<pin name="RESET" direction="in"/>
<pin name="ROSC"/>
<pin name="SENSE1"/>
<pin name="SENSE2"/>
<pin name="SLEEP" direction="in"/>
<pin name="STEP" direction="in"/>
<pin name="VBB1"/>
<pin name="VBB2"/>
<pin name="VCP"/>
<pin name="VDD" direction="pwr"/>
<pin name="VREG"/>
</symbol>
<symbol name="DRV8835">
<description>&lt;h3&gt;DRV8835 Dual Channel Motor Driver&lt;/h3&gt;</description>
<pin name="AIN1/PH"/>
<pin name="AIN2/EN"/>
<pin name="AOUT1"/>
<pin name="AOUT2"/>
<pin name="BIN1/PH"/>
<pin name="BIN2/EN"/>
<pin name="BOUT1"/>
<pin name="BOUT2"/>
<pin name="MODE"/>
<pin name="VCC"/>
<pin name="VM"/>
<pin name="VSS"/>
</symbol>
<symbol name="DRV2605L">
<pin name="REG"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="IN/TRIG"/>
<pin name="EN"/>
<pin name="VDD/NC"/>
<pin name="OUT+"/>
<pin name="GND"/>
<pin name="OUT-"/>
<pin name="VDD"/>
</symbol>
<symbol name="DRV8811">
<pin name="VCC"/>
<pin name="VMB"/>
<pin name="VMA"/>
<pin name="ISENA"/>
<pin name="ISENB"/>
<pin name="USM0"/>
<pin name="USM1"/>
<pin name="RCA"/>
<pin name="RCB"/>
<pin name="RESETN"/>
<pin name="ENABLEN"/>
<pin name="SLEEPN"/>
<pin name="DIR"/>
<pin name="DECAY"/>
<pin name="STEP"/>
<pin name="VREF"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="PAD"/>
<pin name="HOME"/>
<pin name="BOUT1"/>
<pin name="BOUT2"/>
<pin name="AOUT1"/>
<pin name="AOUT2"/>
<pin name="VCP"/>
<pin name="VGD"/>
<pin name="CP1"/>
<pin name="CP2"/>
<pin name="SRN"/>
</symbol>
<symbol name="L298">
<pin name="OUT1"/>
<pin name="VS"/>
<pin name="ENA"/>
<pin name="GND"/>
<pin name="IN3"/>
<pin name="IN4"/>
<pin name="OUT4"/>
<pin name="CSA"/>
<pin name="OUT2"/>
<pin name="IN1"/>
<pin name="IN2"/>
<pin name="VLS"/>
<pin name="ENB"/>
<pin name="OUT3"/>
<pin name="CSB"/>
</symbol>
<symbol name="L298_BRIDGE_DRIVER">
<pin name="GND@1"/>
<pin name="SENSE_A"/>
<pin name="NC@3"/>
<pin name="OUT1"/>
<pin name="OUT2"/>
<pin name="VS"/>
<pin name="IN1"/>
<pin name="ENA"/>
<pin name="IN2"/>
<pin name="GND@10"/>
<pin name="GND@11"/>
<pin name="VSS"/>
<pin name="IN3"/>
<pin name="ENB"/>
<pin name="IN4"/>
<pin name="OUT3"/>
<pin name="OUT4"/>
<pin name="NC@18"/>
<pin name="SENSE_B"/>
<pin name="GND@20"/>
</symbol>
<symbol name="STA540">
<pin name="IN1"/>
<pin name="IN2"/>
<pin name="IN3"/>
<pin name="SVR"/>
<pin name="IN4"/>
<pin name="P-GND"/>
<pin name="S-GND"/>
<pin name="DIAG"/>
<pin name="OUT4"/>
<pin name="OUT3"/>
<pin name="OUT2"/>
<pin name="OUT1"/>
<pin name="VCC1"/>
<pin name="VCC2"/>
<pin name="STBY"/>
</symbol>
<symbol name="L6470">
<pin name="BUSYN/SYNC"/>
<pin name="DGND"/>
<pin name="PGNDB"/>
<pin name="PGNDA"/>
<pin name="AGND"/>
<pin name="OSCOUT"/>
<pin name="OSCIN"/>
<pin name="FLAGN"/>
<pin name="STCK"/>
<pin name="STBYN/RESETN"/>
<pin name="CSN"/>
<pin name="CK"/>
<pin name="SDI"/>
<pin name="SDO"/>
<pin name="VSA"/>
<pin name="VSB"/>
<pin name="OUT1A"/>
<pin name="OUT2A"/>
<pin name="OUT1B"/>
<pin name="OUT2B"/>
<pin name="VDD"/>
<pin name="CP"/>
<pin name="VBOOT"/>
<pin name="VREG"/>
<pin name="SW"/>
<pin name="ADCIN"/>
<pin name="VSB2"/>
<pin name="VSA2"/>
<pin name="EPAD"/>
</symbol>
<symbol name="TB6612FNG">
<pin name="A01@1"/>
<pin name="A01@2"/>
<pin name="PGND1@3"/>
<pin name="PGND1@4"/>
<pin name="A02@5"/>
<pin name="A02@6"/>
<pin name="B02@7"/>
<pin name="B02@8"/>
<pin name="PGND2@9"/>
<pin name="PGND2@10"/>
<pin name="B01@11"/>
<pin name="B01@12"/>
<pin name="VM2"/>
<pin name="VM3"/>
<pin name="PWMB"/>
<pin name="BIN2"/>
<pin name="BIN1"/>
<pin name="GND"/>
<pin name="STBY"/>
<pin name="VCC"/>
<pin name="AIN1"/>
<pin name="AIN2"/>
<pin name="PWMA"/>
<pin name="VM1"/>
</symbol>
<symbol name="VNH2SP30">
<pin name="OUTB@15"/>
<pin name="INB"/>
<pin name="VCC@13"/>
<pin name="EN/DIAB"/>
<pin name="CS"/>
<pin name="PWM"/>
<pin name="EN/DIAA"/>
<pin name="INA"/>
<pin name="VCC@3"/>
<pin name="OUTA@1"/>
<pin name="OUTA@30"/>
<pin name="GNDA@28"/>
<pin name="GNDA@27"/>
<pin name="GNDA@26"/>
<pin name="OUTA@25"/>
<pin name="VCC@23"/>
<pin name="OUTB@21"/>
<pin name="GNDB@20"/>
<pin name="GNDB@19"/>
<pin name="GNDB@18"/>
<pin name="OUTB@16"/>
<pin name="VCC@SLUG1"/>
<pin name="OUTA@SLUG3"/>
<pin name="OUTB@SLUG2"/>
</symbol>
<symbol name="AL8805">
<pin name="SW"/>
<pin name="GND"/>
<pin name="CTRL"/>
<pin name="VIN"/>
<pin name="SET"/>
</symbol>
<symbol name="ULN2803">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
</symbol>
<symbol name="L298_SMD_W_PAD">
<pin name="GND@1"/>
<pin name="SENSE_A"/>
<pin name="NC@3"/>
<pin name="OUT1"/>
<pin name="OUT2"/>
<pin name="VS"/>
<pin name="IN1"/>
<pin name="ENA"/>
<pin name="IN2"/>
<pin name="GND@10"/>
<pin name="GND@11"/>
<pin name="VSS"/>
<pin name="IN3"/>
<pin name="ENB"/>
<pin name="IN4"/>
<pin name="OUT3"/>
<pin name="OUT4"/>
<pin name="NC@18"/>
<pin name="SENSE_B"/>
<pin name="GND@20"/>
<pin name="GND@PAD"/>
</symbol>
<symbol name="TLC5947">
<description>&lt;h3&gt;[Texas Instruments] [TLC5947] [24-Channel 12-bit PWM driver]&lt;/h3&gt;
&lt;h3&gt;TI TLC5947 24-channel 12-bit constant current PWM driver&lt;/h3&gt;
&lt;p&gt;The TLC5947 is a 24-channel, constant-current sink LED driver. Each channel is individually adjustable with 4096 pulse-width modulated (PWM) steps. PWM control is repeated automatically with the programmed grayscale (GS) data. GS data are written via a serial interface port. The current value of all 24 channels is set by a single external resistor.&lt;/p&gt;

The TLC5947 has a thermal shutdown (TSD) function that turns off all output drivers during an over-temperature condition. All of the output drivers automatically restart when the temperature returns to normal conditions. &lt;/p&gt;</description>
<pin name="OUT23" direction="out"/>
<pin name="OUT6" direction="out"/>
<pin name="OUT5" direction="out"/>
<pin name="OUT4" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT0" direction="out"/>
<pin name="!BLANK"/>
<pin name="XLAT"/>
<pin name="SOUT"/>
<pin name="SIN"/>
<pin name="SCLK"/>
<pin name="IREF"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="OUT22" direction="out"/>
<pin name="OUT21" direction="out"/>
<pin name="OUT20" direction="out"/>
<pin name="OUT19" direction="out"/>
<pin name="OUT18" direction="out"/>
<pin name="OUT17" direction="out"/>
<pin name="OUT16" direction="out"/>
<pin name="OUT15" direction="out"/>
<pin name="OUT14" direction="out"/>
<pin name="OUT13" direction="out"/>
<pin name="OUT12" direction="out"/>
<pin name="OUT11" direction="out"/>
<pin name="OUT10" direction="out"/>
<pin name="OUT9" direction="out"/>
<pin name="OUT8" direction="out"/>
<pin name="OUT7" direction="out"/>
</symbol>
<symbol name="BNO080-IMU">
<description>&lt;h3&gt;Hillcrest Labs BNO080 - High Precision IMU&lt;/h3&gt;
&lt;p&gt;The BNO080/BNO085 IMU has a combination triple axis accelerometer/gyro/magnetometer packaged with an ARM Cortex M0+ running powerful algorithms. This enables the BNO080 Inertial Measurement Unit (IMU) to produce accurate rotation vector headings with an error of 5 degrees or less. It's what we've been waiting for: all the sensor data is combined into meaningful, accurate IMU information. &lt;/p&gt;</description>
<pin name="GND"/>
<pin name="!RST"/>
<pin name="CAP"/>
<pin name="VDD"/>
<pin name="XIN32"/>
<pin name="CLKSEL1"/>
<pin name="S_SDA"/>
<pin name="S_SCL"/>
<pin name="!BOOT"/>
<pin name="!H_INT"/>
<pin name="H_SCL/SCLK/RX"/>
<pin name="H_SDA/MISO/TX"/>
<pin name="H_SA0/MOSI"/>
<pin name="VDDIO"/>
<pin name="GNDIO"/>
<pin name="!H_CS"/>
<pin name="CLKSEL0"/>
<pin name="PS0/WAKE"/>
<pin name="PS1"/>
</symbol>
<symbol name="MLX90540_MLX90640">
<pin name="GND"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="VDD"/>
</symbol>
<symbol name="MAX30101">
<description>&lt;h3&gt;MAX30101 Heart Rate Sensor and Oximeter&lt;/h3&gt;
&lt;p&gt;&lt;/p&gt;</description>
<pin name="NC" direction="nc"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="!INT"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="VDD_LED" direction="pwr"/>
</symbol>
<symbol name="MAX32664">
<description>&lt;h3&gt;MAX32644 Version A Biometric Sensor Hub&lt;/h3&gt;</description>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VCORE" direction="pwr"/>
<pin name="OSC_OUT"/>
<pin name="OSC_IN"/>
<pin name="SNSR_SDA"/>
<pin name="SNSR_SCL"/>
<pin name="SLAVE_SDA"/>
<pin name="SLAVE_SCL"/>
<pin name="!RST"/>
<pin name="!MFIO"/>
<pin name="ACCEL_INT"/>
<pin name="HR_INT"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="AD5262">
<description>&lt;h3&gt;Digital Potentiometer IC&lt;/h3&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/assets/learn_tutorials/1/8/8/AD5262BRU_datasheet.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13144"&gt;SparkFun Touch Potentiometer&lt;/a&gt; (PRT-13144)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="1" symbol="AD5262"/>
</gates>
<devices>
<device name="" package="SSOP16">
<connects>
<connect gate="1" pin="A1" pad="2"/>
<connect gate="1" pin="A2" pad="16"/>
<connect gate="1" pin="B1" pad="4"/>
<connect gate="1" pin="B2" pad="14"/>
<connect gate="1" pin="CLK" pad="7"/>
<connect gate="1" pin="CS_N" pad="9"/>
<connect gate="1" pin="GND" pad="11"/>
<connect gate="1" pin="PR_N" pad="10"/>
<connect gate="1" pin="SDI" pad="8"/>
<connect gate="1" pin="SDO" pad="1"/>
<connect gate="1" pin="SHDN_N" pad="6"/>
<connect gate="1" pin="VDD" pad="5"/>
<connect gate="1" pin="VL" pad="13"/>
<connect gate="1" pin="VSS" pad="12"/>
<connect gate="1" pin="W1" pad="3"/>
<connect gate="1" pin="W2" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-12358"/>
<attribute name="VALUE" value="AD5262BRU"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="556" prefix="IC" uservalue="yes">
<description>&lt;h3&gt;556 Dual 555 timer&lt;/h3&gt;
&lt;p&gt;2 555 timers in one package&lt;br&gt;
1MHZ 14DIP&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Kits/icm7555-56.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11177"&gt;SparkFun SparkPunk Sound Kit&lt;/a&gt; (KIT-11177)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="556_TIMER_DUAL"/>
</gates>
<devices>
<device name="" package="DIP14">
<connects>
<connect gate="G$1" pin="CV" pad="3"/>
<connect gate="G$1" pin="CV2" pad="11"/>
<connect gate="G$1" pin="DIS" pad="1"/>
<connect gate="G$1" pin="DIS2" pad="13"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="OUT2" pad="9"/>
<connect gate="G$1" pin="RST" pad="4"/>
<connect gate="G$1" pin="RST2" pad="10"/>
<connect gate="G$1" pin="THR" pad="2"/>
<connect gate="G$1" pin="THR2" pad="12"/>
<connect gate="G$1" pin="TRIG" pad="6"/>
<connect gate="G$1" pin="TRIG2" pad="8"/>
<connect gate="G$1" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11898"/>
<attribute name="VALUE" value="556"/>
</technology>
</technologies>
</device>
<device name="KIT" package="DIP14-KIT">
<connects>
<connect gate="G$1" pin="CV" pad="3"/>
<connect gate="G$1" pin="CV2" pad="11"/>
<connect gate="G$1" pin="DIS" pad="1"/>
<connect gate="G$1" pin="DIS2" pad="13"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="OUT2" pad="9"/>
<connect gate="G$1" pin="RST" pad="4"/>
<connect gate="G$1" pin="RST2" pad="10"/>
<connect gate="G$1" pin="THR" pad="2"/>
<connect gate="G$1" pin="THR2" pad="12"/>
<connect gate="G$1" pin="TRIG" pad="6"/>
<connect gate="G$1" pin="TRIG2" pad="8"/>
<connect gate="G$1" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11898"/>
<attribute name="VALUE" value="556"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD9837">
<description>&lt;h3&gt;Programmable waveform generator&lt;/h3&gt;
&lt;p&gt;Sine, triangular, and square wave outputs&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/BreakoutBoards/AD9837.PDF"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11420"&gt;SparkFun MiniGen - Pro Mini Signal Generator Shield&lt;/a&gt; (BOB-11420)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G1" symbol="AD9837"/>
</gates>
<devices>
<device name="" package="AD9837">
<connects>
<connect gate="G1" pin="AGND" pad="P$9"/>
<connect gate="G1" pin="CAP/2.5V" pad="P$3"/>
<connect gate="G1" pin="COMP" pad="P$1"/>
<connect gate="G1" pin="DGND" pad="P$0 P$4"/>
<connect gate="G1" pin="FSYNC" pad="P$8"/>
<connect gate="G1" pin="MCLK" pad="P$5"/>
<connect gate="G1" pin="SCLK" pad="P$7"/>
<connect gate="G1" pin="SDATA" pad="P$6"/>
<connect gate="G1" pin="VDD" pad="P$2"/>
<connect gate="G1" pin="VOUT" pad="P$10"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11223"/>
<attribute name="VALUE" value="AD9837BCPZ"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA169" prefix="U">
<description>&lt;h3&gt;Current Output Current Shunt Monitor&lt;/h3&gt;
&lt;p&gt;0.5%, SOT23-5&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Sensors/Current/ina169.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12040"&gt;SparkFun Current Sensor Breakout - INA169&lt;/a&gt; (SEN-12040)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="INA169"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="VIN+" pad="3"/>
<connect gate="G$1" pin="VIN-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11776"/>
<attribute name="VALUE" value="INA169"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP41XXX" prefix="U">
<description>&lt;h3&gt;Digital Potentiometer - 10K&lt;/h3&gt;
&lt;p&gt;SPI controlled single digital potentiometer by Microchip&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/General%20IC/22060b.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10613"&gt;Storefront component: Digital Potentiometer - 10K&lt;/a&gt; (COM-10613)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="MCP41XXX"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="A" pad="5"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCK" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="W" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NA-XXXXX"/>
<attribute name="VALUE" value="MCP41XXX"/>
</technology>
</technologies>
</device>
<device name="DIL" package="DIP08">
<connects>
<connect gate="G$1" pin="A" pad="5"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCK" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="W" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-13155"/>
<attribute name="VALUE" value="MCP41XXX"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MSGEQ7" prefix="IC">
<description>&lt;h3&gt;7-band graphic equalizer&lt;/h3&gt;
&lt;p&gt;This IC is for making a 7 band/channel audio spectrometer.&lt;br&gt;
There are two versions of this part.  The DIP available on the storefront, and the SO used in product.
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/General/MSGEQ7.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10468"&gt;Storefront component: Graphic Equalizer Display Filter - MSGEQ7&lt;/a&gt; (COM-10468)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13116"&gt;SparkFun Spectrum Shield&lt;/a&gt; (DEV-13116)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="MSGEQ7"/>
</gates>
<devices>
<device name="SOIC" package="SO08">
<connects>
<connect gate="G$1" pin="AUDIO_IN" pad="5"/>
<connect gate="G$1" pin="CG" pad="6"/>
<connect gate="G$1" pin="CKIN" pad="8"/>
<connect gate="G$1" pin="DCOUT" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="RESET" pad="7"/>
<connect gate="G$1" pin="STROBE" pad="4"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-10141"/>
<attribute name="VALUE" value="MSGEQ7N"/>
</technology>
</technologies>
</device>
<device name="DIL" package="DIP08">
<connects>
<connect gate="G$1" pin="AUDIO_IN" pad="5"/>
<connect gate="G$1" pin="CG" pad="6"/>
<connect gate="G$1" pin="CKIN" pad="8"/>
<connect gate="G$1" pin="DCOUT" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="RESET" pad="7"/>
<connect gate="G$1" pin="STROBE" pad="4"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-12196"/>
<attribute name="VALUE" value="MSGEQ7P"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="555" prefix="IC" uservalue="yes">
<description>&lt;h3&gt;General purpose bipolar Timer&lt;/h3&gt;
&lt;p&gt;&lt;a href="http://www.sparkfun.com/datasheets/Components/General/ne555.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12707"&gt;SparkFun SparkPunk Sequencer Kit&lt;/a&gt; (KIT-12707)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9273"&gt;Storefront Component: 555 Timer&lt;/a&gt; (COM-09273)&lt;/li&gt;
&lt;/ul&gt;

Two parts valid for production:&lt;br&gt;
&lt;br&gt;
VFP: IC-11930 (M7555 PTH)&lt;br&gt;
VFP: IC-09173 (555 PTH) - &lt;b&gt;Preferred&lt;/b&gt;&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="NE555"/>
</gates>
<devices>
<device name="P" package="DIP08">
<connects>
<connect gate="G$1" pin="/RES" pad="4"/>
<connect gate="G$1" pin="CON" pad="5"/>
<connect gate="G$1" pin="DIS" pad="7"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="TRE" pad="6"/>
<connect gate="G$1" pin="TRI" pad="2"/>
<connect gate="G$1" pin="VCC+" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09173"/>
<attribute name="PROD_ID_ALT" value="IC-09173"/>
<attribute name="VALUE" value="555"/>
</technology>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="G$1" pin="/RES" pad="4"/>
<connect gate="G$1" pin="CON" pad="5"/>
<connect gate="G$1" pin="DIS" pad="7"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="TRE" pad="6"/>
<connect gate="G$1" pin="TRI" pad="2"/>
<connect gate="G$1" pin="VCC+" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NA-XXXXX"/>
<attribute name="VALUE" value="555"/>
</technology>
</technologies>
</device>
<device name="KIT" package="DIP08-KIT">
<connects>
<connect gate="G$1" pin="/RES" pad="4"/>
<connect gate="G$1" pin="CON" pad="5"/>
<connect gate="G$1" pin="DIS" pad="7"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="TRE" pad="6"/>
<connect gate="G$1" pin="TRI" pad="2"/>
<connect gate="G$1" pin="VCC+" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09173"/>
<attribute name="PROD_ID_ALT" value="IC-11930"/>
<attribute name="VALUE" value="555"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TS3USB221A" prefix="U" uservalue="yes">
<description>&lt;h3&gt;DPDT Analog Mux&lt;/h3&gt;
&lt;p&gt;DPDT Analog Mux&lt;br&gt;
Vcc 2.5 to 3.3V&lt;br&gt;
Passes up to 5.5V at 3.3V supply&lt;br&gt;
900MHz BW, 6&amp;#8486; switch resistance&lt;br&gt;
&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12935"&gt;SparkFun FTDI SmartBasic&lt;/a&gt; (DEV-12935)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="TS3USB221A"/>
</gates>
<devices>
<device name="" package="QFN-10-RSE">
<connects>
<connect gate="G$1" pin="!OE" pad="6"/>
<connect gate="G$1" pin="1D+" pad="1"/>
<connect gate="G$1" pin="1D-" pad="2"/>
<connect gate="G$1" pin="2D+" pad="3"/>
<connect gate="G$1" pin="2D-" pad="4"/>
<connect gate="G$1" pin="D+" pad="8"/>
<connect gate="G$1" pin="D-" pad="7"/>
<connect gate="G$1" pin="S" pad="9"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-12115"/>
<attribute name="VALUE" value="TS3USB221A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATAES132" prefix="AES">
<description>&lt;h3&gt;Crypto 32Kb Serial EEPROM&lt;/h3&gt;
&lt;p&gt;AES-128-CCM&lt;br&gt;
MAC&lt;br&gt;
Secure Storage for 128-bit keys&lt;br&gt;
Encrypted User Memory Readn and Write&lt;br&gt;
HWRNG&lt;br&gt;
2.5V to 5.5V&lt;br&gt;
&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Dev/Beagle/Atmel-8760-CryptoAuth-ATAES132-Datasheet.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12773"&gt;CryptoCape&lt;/a&gt; (DEV-12773)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13183"&gt;SparkFun CryptoShield&lt;/a&gt; (DEV-13183)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="ATAES132"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="AUTHO" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC3" pad="3"/>
<connect gate="G$1" pin="NC7" pad="7"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11983"/>
<attribute name="VALUE" value="ATAES132"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATECC108" prefix="ECC">
<description>&lt;h3&gt;ATECC108 ECDSA with NIST&lt;/h3&gt;
&lt;p&gt;ATECC108: Provides ECDSA with NIST curves P256, B283, and K283.  Also, a RNG, 8.5Kb EEPROM.  2.0V - 5.5V.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Dev/Beagle/Atmel-8873S-CryptoAuth-ATECC108-Datasheet-Summary.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12773"&gt;CryptoCape&lt;/a&gt; (DEV-12773)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13183"&gt;SparkFun CryptoShield&lt;/a&gt; (DEV-13183)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="ATECC108"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC2" pad="2"/>
<connect gate="G$1" pin="NC3" pad="3"/>
<connect gate="G$1" pin="NC7" pad="7"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11982"/>
<attribute name="VALUE" value="ATECC108"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATSHA204_SOIC8" prefix="U">
<description>&lt;h3&gt;Crypto 4.5KB I2C&lt;/h3&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Dev/Beagle/Atmel-8740-CryptoAuth-ATSHA204-Datasheet.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12773"&gt;CryptoCape&lt;/a&gt; (DEV-12773)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13183"&gt;SparkFun CryptoShield&lt;/a&gt; (DEV-13183)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="ATSHA204-1"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC2" pad="2"/>
<connect gate="G$1" pin="NC3" pad="3"/>
<connect gate="G$1" pin="NC7" pad="7"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11981"/>
<attribute name="VALUE" value="ATSHA204"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATSHA204" prefix="U">
<description>&lt;h3&gt;Atmel ATSHA204&lt;/h3&gt;
&lt;p&gt;The Atmel ATSHA204 is an optimized authentication chip that includes a 4.5Kb EEPROM. This array can be used for storage of keys, miscellaneous read/write, read-only, password or secret data, and consumption tracking. Access to the various sections of memory can be restricted in a variety of ways and then the configuration locked to prevent changes.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.atmel.com/Images/Atmel-8740-CryptoAuth-ATSHA204-Datasheet.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12887"&gt;SparkFun Electric Imp Shield&lt;/a&gt; &lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12886"&gt; SparkFun Electric Imp Breakout&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="ATSHA204"/>
</gates>
<devices>
<device name="-TSU" package="SOT23-3">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="SDA" pad="1"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11208"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCA9685" prefix="U" uservalue="yes">
<description>&lt;h3&gt;16-channel 12-bit PWM&lt;/h3&gt;
&lt;p&gt;I&lt;sup&gt;2&lt;/sup&gt;C interface&lt;br&gt;
Internal Oscillator 40Hz to 1kHz&lt;br&gt;
Can be totem pole or open collector&lt;br&gt;
2.3V to 5.5V
&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13042"&gt;SparkFun Block for Intel® Edison - PWM&lt;/a&gt; (DEV-13042)&lt;/li&gt;
&lt;/ul&gt;
PROTO: IC-12240&lt;br&gt;
PROD_ID: IC-12271</description>
<gates>
<gate name="G$1" symbol="PCA9685"/>
</gates>
<devices>
<device name="" package="TSSOP-28_4MM">
<connects>
<connect gate="G$1" pin="!OE" pad="23"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="A5" pad="24"/>
<connect gate="G$1" pin="CH0" pad="6"/>
<connect gate="G$1" pin="CH1" pad="7"/>
<connect gate="G$1" pin="CH10" pad="17"/>
<connect gate="G$1" pin="CH11" pad="18"/>
<connect gate="G$1" pin="CH12" pad="19"/>
<connect gate="G$1" pin="CH13" pad="20"/>
<connect gate="G$1" pin="CH14" pad="21"/>
<connect gate="G$1" pin="CH15" pad="22"/>
<connect gate="G$1" pin="CH2" pad="8"/>
<connect gate="G$1" pin="CH3" pad="9"/>
<connect gate="G$1" pin="CH4" pad="10"/>
<connect gate="G$1" pin="CH5" pad="11"/>
<connect gate="G$1" pin="CH6" pad="12"/>
<connect gate="G$1" pin="CH7" pad="13"/>
<connect gate="G$1" pin="CH8" pad="15"/>
<connect gate="G$1" pin="CH9" pad="16"/>
<connect gate="G$1" pin="EXTCLK" pad="25"/>
<connect gate="G$1" pin="SCL" pad="26"/>
<connect gate="G$1" pin="SDA" pad="27"/>
<connect gate="G$1" pin="VDD" pad="28"/>
<connect gate="G$1" pin="VSS" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-12271"/>
<attribute name="VALUE" value="PCA9685"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SX1509" prefix="U" uservalue="yes">
<description>&lt;h3&gt;Semtech SX1509&lt;/h3&gt;
&lt;p&gt;The SX1509 is a complete ultra low voltage 1.2V to 3.6V General Purpose parallel Input/Output (GPIO) expanders ideal for low power handheld battery powered equipment. This version comes in a 16-channel configuration and allows easy serial expansion of I/O through a standard 400kHz I2C interface. GPIO devices can provide additional control and monitoring when the microcontroller or chipset has insufficient I/O ports, or in systems where serial communication and control from a remote location is advantageous.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/BreakoutBoards/sx1509.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13601"&gt;SparkFun 16 Output I/O Expander Breakout - SX1509&lt;/a&gt; (BOB-13601)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13582"&gt;SparkFun Line Follower Array&lt;/a&gt; (SEN-13582)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="SX1509"/>
</gates>
<devices>
<device name="" package="QFN-28">
<connects>
<connect gate="G$1" pin="!INT" pad="9"/>
<connect gate="G$1" pin="!RESET" pad="23"/>
<connect gate="G$1" pin="ADDR0" pad="26"/>
<connect gate="G$1" pin="ADDR1" pad="10"/>
<connect gate="G$1" pin="GND" pad="3 17 29"/>
<connect gate="G$1" pin="I/O[0]" pad="27"/>
<connect gate="G$1" pin="I/O[10]" pad="15"/>
<connect gate="G$1" pin="I/O[11]" pad="16"/>
<connect gate="G$1" pin="I/O[12]" pad="19"/>
<connect gate="G$1" pin="I/O[13]" pad="20"/>
<connect gate="G$1" pin="I/O[14]" pad="21"/>
<connect gate="G$1" pin="I/O[15]" pad="22"/>
<connect gate="G$1" pin="I/O[1]" pad="28"/>
<connect gate="G$1" pin="I/O[2]" pad="1"/>
<connect gate="G$1" pin="I/O[3]" pad="2"/>
<connect gate="G$1" pin="I/O[4]" pad="5"/>
<connect gate="G$1" pin="I/O[5]" pad="6"/>
<connect gate="G$1" pin="I/O[6]" pad="7"/>
<connect gate="G$1" pin="I/O[7]" pad="8"/>
<connect gate="G$1" pin="I/O[8]" pad="13"/>
<connect gate="G$1" pin="I/O[9]" pad="14"/>
<connect gate="G$1" pin="OSCIO" pad="11"/>
<connect gate="G$1" pin="SCL" pad="25"/>
<connect gate="G$1" pin="SDA" pad="24"/>
<connect gate="G$1" pin="VCC1" pad="4"/>
<connect gate="G$1" pin="VCC2" pad="18"/>
<connect gate="G$1" pin="VDDM" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11311"/>
<attribute name="VALUE" value="SX1509"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPEAKJET" prefix="U">
<description>&lt;h3&gt;Speech synthesis chip&lt;/h3&gt;
&lt;p&gt;&lt;a href="http://www.sparkfun.com/datasheets/Components/General/speakjet-usermanual.pdf"&gt;User Manual&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9578"&gt;SpeakJet&lt;/a&gt; (COM-09578)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="SPEAKJET"/>
</gates>
<devices>
<device name="DIP" package="DIP18">
<connects>
<connect gate="G$1" pin="D0/RDY" pad="17"/>
<connect gate="G$1" pin="D1/SPK" pad="16"/>
<connect gate="G$1" pin="D2/BHF" pad="15"/>
<connect gate="G$1" pin="E0" pad="9"/>
<connect gate="G$1" pin="E1" pad="8"/>
<connect gate="G$1" pin="E2" pad="7"/>
<connect gate="G$1" pin="E3" pad="6"/>
<connect gate="G$1" pin="E4" pad="4"/>
<connect gate="G$1" pin="E5" pad="3"/>
<connect gate="G$1" pin="E6/RC0" pad="2"/>
<connect gate="G$1" pin="E7/RC1" pad="1"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="M0" pad="13"/>
<connect gate="G$1" pin="M1" pad="12"/>
<connect gate="G$1" pin="RST" pad="11"/>
<connect gate="G$1" pin="RX" pad="10"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="VOICE" pad="18"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09512"/>
<attribute name="VALUE" value="SPEAKJET"/>
</technology>
</technologies>
</device>
<device name="SMD" package="SOIC-18">
<connects>
<connect gate="G$1" pin="D0/RDY" pad="17"/>
<connect gate="G$1" pin="D1/SPK" pad="16"/>
<connect gate="G$1" pin="D2/BHF" pad="15"/>
<connect gate="G$1" pin="E0" pad="9"/>
<connect gate="G$1" pin="E1" pad="8"/>
<connect gate="G$1" pin="E2" pad="7"/>
<connect gate="G$1" pin="E3" pad="6"/>
<connect gate="G$1" pin="E4" pad="4"/>
<connect gate="G$1" pin="E5" pad="3"/>
<connect gate="G$1" pin="E6/RC0" pad="2"/>
<connect gate="G$1" pin="E7/RC1" pad="1"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="M0" pad="13"/>
<connect gate="G$1" pin="M1" pad="12"/>
<connect gate="G$1" pin="RST" pad="11"/>
<connect gate="G$1" pin="RX" pad="10"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="VOICE" pad="18"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-XXXXX"/>
<attribute name="VALUE" value="SPEAKJET"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM391" prefix="U">
<description>&lt;h3&gt;LM3914 Dot/Bar Display Driver&lt;/h3&gt;
&lt;p&gt;TTL/CMOS Logic
&lt;br&gt;Drives LEDs, LCDs, Vacuum Fluorecents
&lt;br&gt;
Source:&lt;br&gt;
&lt;a href="http://www.national.com/ds/LM/LM3915.pdf"&gt; Data sheet LM3915&lt;/a&gt;&lt;br&gt;
&lt;a href="http://www.national.com/ds/LM/LM3914.pdf"&gt; Data sheet LM3914 &lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13688”&gt;MyoWare LED Shield&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12694”&gt;Dot/Bar Display Driver - LM3914&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LM3915"/>
</gates>
<devices>
<device name="N" package="DIL18">
<connects>
<connect gate="G$1" pin="LED1" pad="1"/>
<connect gate="G$1" pin="LED10" pad="10"/>
<connect gate="G$1" pin="LED2" pad="18"/>
<connect gate="G$1" pin="LED3" pad="17"/>
<connect gate="G$1" pin="LED4" pad="16"/>
<connect gate="G$1" pin="LED5" pad="15"/>
<connect gate="G$1" pin="LED6" pad="14"/>
<connect gate="G$1" pin="LED7" pad="13"/>
<connect gate="G$1" pin="LED8" pad="12"/>
<connect gate="G$1" pin="LED9" pad="11"/>
<connect gate="G$1" pin="MODE" pad="9"/>
<connect gate="G$1" pin="REFADJ" pad="8"/>
<connect gate="G$1" pin="REFOUT" pad="7"/>
<connect gate="G$1" pin="RHI" pad="6"/>
<connect gate="G$1" pin="RLO" pad="4"/>
<connect gate="G$1" pin="SIGIN" pad="5"/>
<connect gate="G$1" pin="V+" pad="3"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="COM-12694"/>
</technology>
<technology name="4">
<attribute name="SF_ID" value=""/>
</technology>
<technology name="5">
<attribute name="SF_ID" value=""/>
</technology>
</technologies>
</device>
<device name="V" package="PLCC20S">
<connects>
<connect gate="G$1" pin="LED1" pad="1"/>
<connect gate="G$1" pin="LED10" pad="12"/>
<connect gate="G$1" pin="LED2" pad="20"/>
<connect gate="G$1" pin="LED3" pad="19"/>
<connect gate="G$1" pin="LED4" pad="18"/>
<connect gate="G$1" pin="LED5" pad="17"/>
<connect gate="G$1" pin="LED6" pad="16"/>
<connect gate="G$1" pin="LED7" pad="15"/>
<connect gate="G$1" pin="LED8" pad="14"/>
<connect gate="G$1" pin="LED9" pad="13"/>
<connect gate="G$1" pin="MODE" pad="11"/>
<connect gate="G$1" pin="REFADJ" pad="10"/>
<connect gate="G$1" pin="REFOUT" pad="8"/>
<connect gate="G$1" pin="RHI" pad="6"/>
<connect gate="G$1" pin="RLO" pad="4"/>
<connect gate="G$1" pin="SIGIN" pad="5"/>
<connect gate="G$1" pin="V+" pad="3"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value=""/>
</technology>
<technology name="4">
<attribute name="PROD_ID" value="IC-13110"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP55231" prefix="U">
<description>&lt;h3&gt;LP55231 Programmable 9-Output LED Driver&lt;/h3&gt;
&lt;p&gt;&lt;li&gt;&lt;a href=”http://www.ti.com/lit/ds/symlink/lp55231.pdf”&gt;Datasheet&lt;/a&gt;&lt;/li&gt;
&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href='https://www.sparkfun.com/products/13884'&gt;SparkFun LED Driver Breakout - LP55231&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LP55231"/>
</gates>
<devices>
<device name="WQFN" package="WQFN-24">
<connects>
<connect gate="G$1" pin="!INT" pad="7"/>
<connect gate="G$1" pin="!TRIG" pad="10"/>
<connect gate="G$1" pin="ASEL0" pad="20"/>
<connect gate="G$1" pin="ASEL1" pad="21"/>
<connect gate="G$1" pin="B1/D2" pad="18"/>
<connect gate="G$1" pin="B2/D4" pad="16"/>
<connect gate="G$1" pin="B3/D6" pad="14"/>
<connect gate="G$1" pin="C1+" pad="2"/>
<connect gate="G$1" pin="C1-" pad="24"/>
<connect gate="G$1" pin="C2+" pad="1"/>
<connect gate="G$1" pin="C2-" pad="23"/>
<connect gate="G$1" pin="CLK" pad="6"/>
<connect gate="G$1" pin="EN" pad="5"/>
<connect gate="G$1" pin="G1/D1" pad="19"/>
<connect gate="G$1" pin="G2/D3" pad="17"/>
<connect gate="G$1" pin="G3/D5" pad="15"/>
<connect gate="G$1" pin="GND" pad="4 EP"/>
<connect gate="G$1" pin="R1/D7" pad="13"/>
<connect gate="G$1" pin="R2/D8" pad="12"/>
<connect gate="G$1" pin="R3/D9" pad="11"/>
<connect gate="G$1" pin="SCL" pad="9"/>
<connect gate="G$1" pin="SDA" pad="8"/>
<connect gate="G$1" pin="VDD" pad="3"/>
<connect gate="G$1" pin="VOUT" pad="22"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-13302"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="A4988" prefix="U">
<description>DMOS Microstepping Driver with Translator(IC-11483)</description>
<gates>
<gate name="G$1" symbol="A4983"/>
</gates>
<devices>
<device name="5MM" package="QFN-28-5MM">
<connects>
<connect gate="G$1" pin="CP1" pad="P$4"/>
<connect gate="G$1" pin="CP2" pad="P$5"/>
<connect gate="G$1" pin="DIR" pad="P$19"/>
<connect gate="G$1" pin="ENABLE" pad="P$2"/>
<connect gate="G$1" pin="GND@1" pad="P$3"/>
<connect gate="G$1" pin="GND@2" pad="P$18"/>
<connect gate="G$1" pin="GND_PAD" pad="P$29"/>
<connect gate="G$1" pin="MS1" pad="P$9"/>
<connect gate="G$1" pin="MS2" pad="P$10"/>
<connect gate="G$1" pin="MS3" pad="P$11"/>
<connect gate="G$1" pin="NC@1" pad="P$7"/>
<connect gate="G$1" pin="NC@2" pad="P$20"/>
<connect gate="G$1" pin="NC@3" pad="P$25"/>
<connect gate="G$1" pin="OUT1A" pad="P$24"/>
<connect gate="G$1" pin="OUT1B" pad="P$21"/>
<connect gate="G$1" pin="OUT2A" pad="P$26"/>
<connect gate="G$1" pin="OUT2B" pad="P$1"/>
<connect gate="G$1" pin="REF" pad="P$17"/>
<connect gate="G$1" pin="RESET" pad="P$12"/>
<connect gate="G$1" pin="ROSC" pad="P$13"/>
<connect gate="G$1" pin="SENSE1" pad="P$23"/>
<connect gate="G$1" pin="SENSE2" pad="P$27"/>
<connect gate="G$1" pin="SLEEP" pad="P$14"/>
<connect gate="G$1" pin="STEP" pad="P$16"/>
<connect gate="G$1" pin="VBB1" pad="P$22"/>
<connect gate="G$1" pin="VBB2" pad="P$28"/>
<connect gate="G$1" pin="VCP" pad="P$6"/>
<connect gate="G$1" pin="VDD" pad="P$15"/>
<connect gate="G$1" pin="VREG" pad="P$8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ALT1" package="QFN-28-5MM_ALT1">
<connects>
<connect gate="G$1" pin="CP1" pad="P$4"/>
<connect gate="G$1" pin="CP2" pad="P$5"/>
<connect gate="G$1" pin="DIR" pad="P$19"/>
<connect gate="G$1" pin="ENABLE" pad="P$2"/>
<connect gate="G$1" pin="GND@1" pad="P$3"/>
<connect gate="G$1" pin="GND@2" pad="P$18"/>
<connect gate="G$1" pin="GND_PAD" pad="P$29"/>
<connect gate="G$1" pin="MS1" pad="P$9"/>
<connect gate="G$1" pin="MS2" pad="P$10"/>
<connect gate="G$1" pin="MS3" pad="P$11"/>
<connect gate="G$1" pin="NC@1" pad="P$7"/>
<connect gate="G$1" pin="NC@2" pad="P$20"/>
<connect gate="G$1" pin="NC@3" pad="P$25"/>
<connect gate="G$1" pin="OUT1A" pad="P$24"/>
<connect gate="G$1" pin="OUT1B" pad="P$21"/>
<connect gate="G$1" pin="OUT2A" pad="P$26"/>
<connect gate="G$1" pin="OUT2B" pad="P$1"/>
<connect gate="G$1" pin="REF" pad="P$17"/>
<connect gate="G$1" pin="RESET" pad="P$12"/>
<connect gate="G$1" pin="ROSC" pad="P$13"/>
<connect gate="G$1" pin="SENSE1" pad="P$23"/>
<connect gate="G$1" pin="SENSE2" pad="P$27"/>
<connect gate="G$1" pin="SLEEP" pad="P$14"/>
<connect gate="G$1" pin="STEP" pad="P$16"/>
<connect gate="G$1" pin="VBB1" pad="P$22"/>
<connect gate="G$1" pin="VBB2" pad="P$28"/>
<connect gate="G$1" pin="VCP" pad="P$6"/>
<connect gate="G$1" pin="VDD" pad="P$15"/>
<connect gate="G$1" pin="VREG" pad="P$8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11483"/>
</technology>
</technologies>
</device>
<device name="ALT2" package="QFN-28-5MM_ALT2">
<connects>
<connect gate="G$1" pin="CP1" pad="P$4"/>
<connect gate="G$1" pin="CP2" pad="P$5"/>
<connect gate="G$1" pin="DIR" pad="P$19"/>
<connect gate="G$1" pin="ENABLE" pad="P$2"/>
<connect gate="G$1" pin="GND@1" pad="P$3"/>
<connect gate="G$1" pin="GND@2" pad="P$18"/>
<connect gate="G$1" pin="GND_PAD" pad="P$29"/>
<connect gate="G$1" pin="MS1" pad="P$9"/>
<connect gate="G$1" pin="MS2" pad="P$10"/>
<connect gate="G$1" pin="MS3" pad="P$11"/>
<connect gate="G$1" pin="NC@1" pad="P$7"/>
<connect gate="G$1" pin="NC@2" pad="P$20"/>
<connect gate="G$1" pin="NC@3" pad="P$25"/>
<connect gate="G$1" pin="OUT1A" pad="P$24"/>
<connect gate="G$1" pin="OUT1B" pad="P$21"/>
<connect gate="G$1" pin="OUT2A" pad="P$26"/>
<connect gate="G$1" pin="OUT2B" pad="P$1"/>
<connect gate="G$1" pin="REF" pad="P$17"/>
<connect gate="G$1" pin="RESET" pad="P$12"/>
<connect gate="G$1" pin="ROSC" pad="P$13"/>
<connect gate="G$1" pin="SENSE1" pad="P$23"/>
<connect gate="G$1" pin="SENSE2" pad="P$27"/>
<connect gate="G$1" pin="SLEEP" pad="P$14"/>
<connect gate="G$1" pin="STEP" pad="P$16"/>
<connect gate="G$1" pin="VBB1" pad="P$22"/>
<connect gate="G$1" pin="VBB2" pad="P$28"/>
<connect gate="G$1" pin="VCP" pad="P$6"/>
<connect gate="G$1" pin="VDD" pad="P$15"/>
<connect gate="G$1" pin="VREG" pad="P$8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1:1" package="QFN-28-5MM-1:1">
<connects>
<connect gate="G$1" pin="CP1" pad="P$4"/>
<connect gate="G$1" pin="CP2" pad="P$5"/>
<connect gate="G$1" pin="DIR" pad="P$19"/>
<connect gate="G$1" pin="ENABLE" pad="P$2"/>
<connect gate="G$1" pin="GND@1" pad="P$3"/>
<connect gate="G$1" pin="GND@2" pad="P$18"/>
<connect gate="G$1" pin="GND_PAD" pad="P$29"/>
<connect gate="G$1" pin="MS1" pad="P$9"/>
<connect gate="G$1" pin="MS2" pad="P$10"/>
<connect gate="G$1" pin="MS3" pad="P$11"/>
<connect gate="G$1" pin="NC@1" pad="P$7"/>
<connect gate="G$1" pin="NC@2" pad="P$20"/>
<connect gate="G$1" pin="NC@3" pad="P$25"/>
<connect gate="G$1" pin="OUT1A" pad="P$24"/>
<connect gate="G$1" pin="OUT1B" pad="P$21"/>
<connect gate="G$1" pin="OUT2A" pad="P$26"/>
<connect gate="G$1" pin="OUT2B" pad="P$1"/>
<connect gate="G$1" pin="REF" pad="P$17"/>
<connect gate="G$1" pin="RESET" pad="P$12"/>
<connect gate="G$1" pin="ROSC" pad="P$13"/>
<connect gate="G$1" pin="SENSE1" pad="P$23"/>
<connect gate="G$1" pin="SENSE2" pad="P$27"/>
<connect gate="G$1" pin="SLEEP" pad="P$14"/>
<connect gate="G$1" pin="STEP" pad="P$16"/>
<connect gate="G$1" pin="VBB1" pad="P$22"/>
<connect gate="G$1" pin="VBB2" pad="P$28"/>
<connect gate="G$1" pin="VCP" pad="P$6"/>
<connect gate="G$1" pin="VDD" pad="P$15"/>
<connect gate="G$1" pin="VREG" pad="P$8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ALT1_REDUCED_PASTE" package="QFN-28-5MM_ALT1_REDUCED_PASTE">
<connects>
<connect gate="G$1" pin="CP1" pad="P$4"/>
<connect gate="G$1" pin="CP2" pad="P$5"/>
<connect gate="G$1" pin="DIR" pad="P$19"/>
<connect gate="G$1" pin="ENABLE" pad="P$2"/>
<connect gate="G$1" pin="GND@1" pad="P$3"/>
<connect gate="G$1" pin="GND@2" pad="P$18"/>
<connect gate="G$1" pin="GND_PAD" pad="P$29"/>
<connect gate="G$1" pin="MS1" pad="P$9"/>
<connect gate="G$1" pin="MS2" pad="P$10"/>
<connect gate="G$1" pin="MS3" pad="P$11"/>
<connect gate="G$1" pin="NC@1" pad="P$7"/>
<connect gate="G$1" pin="NC@2" pad="P$20"/>
<connect gate="G$1" pin="NC@3" pad="P$25"/>
<connect gate="G$1" pin="OUT1A" pad="P$24"/>
<connect gate="G$1" pin="OUT1B" pad="P$21"/>
<connect gate="G$1" pin="OUT2A" pad="P$26"/>
<connect gate="G$1" pin="OUT2B" pad="P$1"/>
<connect gate="G$1" pin="REF" pad="P$17"/>
<connect gate="G$1" pin="RESET" pad="P$12"/>
<connect gate="G$1" pin="ROSC" pad="P$13"/>
<connect gate="G$1" pin="SENSE1" pad="P$23"/>
<connect gate="G$1" pin="SENSE2" pad="P$27"/>
<connect gate="G$1" pin="SLEEP" pad="P$14"/>
<connect gate="G$1" pin="STEP" pad="P$16"/>
<connect gate="G$1" pin="VBB1" pad="P$22"/>
<connect gate="G$1" pin="VBB2" pad="P$28"/>
<connect gate="G$1" pin="VCP" pad="P$6"/>
<connect gate="G$1" pin="VDD" pad="P$15"/>
<connect gate="G$1" pin="VREG" pad="P$8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11483"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DRV8811" prefix="U">
<gates>
<gate name="G$1" symbol="DRV8811"/>
</gates>
<devices>
<device name="" package="HTSSOP28">
<connects>
<connect gate="G$1" pin="AOUT1" pad="4"/>
<connect gate="G$1" pin="AOUT2" pad="25"/>
<connect gate="G$1" pin="BOUT1" pad="11"/>
<connect gate="G$1" pin="BOUT2" pad="18"/>
<connect gate="G$1" pin="CP1" pad="23"/>
<connect gate="G$1" pin="CP2" pad="24"/>
<connect gate="G$1" pin="DECAY" pad="5"/>
<connect gate="G$1" pin="DIR" pad="3"/>
<connect gate="G$1" pin="ENABLEN" pad="26"/>
<connect gate="G$1" pin="GND@1" pad="7"/>
<connect gate="G$1" pin="GND@2" pad="21"/>
<connect gate="G$1" pin="HOME" pad="2"/>
<connect gate="G$1" pin="ISENA" pad="1"/>
<connect gate="G$1" pin="ISENB" pad="14"/>
<connect gate="G$1" pin="PAD" pad="GND@10 GND@11 GND@12 GND@13 GND@14 GND@15 GND@16 GND@17 GND@18 GND@19 GND@20 GND@21 GND@22 GND@23 GND@24 GND@25 GND@26 GND@27 GND@28 GND@29 GND@30 GND@PAD"/>
<connect gate="G$1" pin="RCA" pad="6"/>
<connect gate="G$1" pin="RCB" pad="9"/>
<connect gate="G$1" pin="RESETN" pad="17"/>
<connect gate="G$1" pin="SLEEPN" pad="27"/>
<connect gate="G$1" pin="SRN" pad="16"/>
<connect gate="G$1" pin="STEP" pad="19"/>
<connect gate="G$1" pin="USM0" pad="13"/>
<connect gate="G$1" pin="USM1" pad="12"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="VCP" pad="22"/>
<connect gate="G$1" pin="VGD" pad="20"/>
<connect gate="G$1" pin="VMA" pad="28"/>
<connect gate="G$1" pin="VMB" pad="15"/>
<connect gate="G$1" pin="VREF" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-12375"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DRV2605L">
<gates>
<gate name="DRV2605" symbol="DRV2605L"/>
</gates>
<devices>
<device name="" package="VSSOP-10">
<connects>
<connect gate="DRV2605" pin="EN" pad="P$5"/>
<connect gate="DRV2605" pin="GND" pad="P$8"/>
<connect gate="DRV2605" pin="IN/TRIG" pad="P$4"/>
<connect gate="DRV2605" pin="OUT+" pad="P$7"/>
<connect gate="DRV2605" pin="OUT-" pad="P$9"/>
<connect gate="DRV2605" pin="REG" pad="P$1"/>
<connect gate="DRV2605" pin="SCL" pad="P$2"/>
<connect gate="DRV2605" pin="SDA" pad="P$3"/>
<connect gate="DRV2605" pin="VDD" pad="P$10"/>
<connect gate="DRV2605" pin="VDD/NC" pad="P$6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-13504"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DRV883X" prefix="U" uservalue="yes">
<description>&lt;h3&gt;DRV8835 2 Channel Motor Driver&lt;/h3&gt;
&lt;p&gt;Dual 1.5A H-bridge, 2-11V
&lt;li&gt;&lt;a href=”http://www.ti.com/lit/ds/symlink/drv8835.pdf”&gt;Datasheet&lt;/a&gt;&lt;/li&gt;
&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13911”&gt;SparkFun Serial Controlled Motor Driver&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DRV8835"/>
</gates>
<devices>
<device name="" package="WSON-12">
<connects>
<connect gate="G$1" pin="AIN1/PH" pad="10"/>
<connect gate="G$1" pin="AIN2/EN" pad="9"/>
<connect gate="G$1" pin="AOUT1" pad="2"/>
<connect gate="G$1" pin="AOUT2" pad="3"/>
<connect gate="G$1" pin="BIN1/PH" pad="8"/>
<connect gate="G$1" pin="BIN2/EN" pad="7"/>
<connect gate="G$1" pin="BOUT1" pad="4"/>
<connect gate="G$1" pin="BOUT2" pad="5"/>
<connect gate="G$1" pin="MODE" pad="11"/>
<connect gate="G$1" pin="VCC" pad="12"/>
<connect gate="G$1" pin="VM" pad="1"/>
<connect gate="G$1" pin="VSS" pad="6 PAD"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-13342"/>
<attribute name="VALUE" value="DRV8835"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L6470" prefix="U" uservalue="yes">
<description>3A RMS/7A peak bipolar stepper motor driver with SPI control&lt;br&gt;
and step input in HTSSOP-28 package.&lt;br&gt;
IC-10648</description>
<gates>
<gate name="G$1" symbol="L6470"/>
</gates>
<devices>
<device name="" package="HTSSOP28">
<connects>
<connect gate="G$1" pin="ADCIN" pad="5"/>
<connect gate="G$1" pin="AGND" pad="9"/>
<connect gate="G$1" pin="BUSYN/SYNC" pad="22"/>
<connect gate="G$1" pin="CK" pad="19"/>
<connect gate="G$1" pin="CP" pad="10"/>
<connect gate="G$1" pin="CSN" pad="23"/>
<connect gate="G$1" pin="DGND" pad="21"/>
<connect gate="G$1" pin="EPAD" pad="GND@PAD"/>
<connect gate="G$1" pin="FLAGN" pad="24"/>
<connect gate="G$1" pin="OSCIN" pad="7"/>
<connect gate="G$1" pin="OSCOUT" pad="8"/>
<connect gate="G$1" pin="OUT1A" pad="1"/>
<connect gate="G$1" pin="OUT1B" pad="14"/>
<connect gate="G$1" pin="OUT2A" pad="28"/>
<connect gate="G$1" pin="OUT2B" pad="15"/>
<connect gate="G$1" pin="PGNDA" pad="27"/>
<connect gate="G$1" pin="PGNDB" pad="13"/>
<connect gate="G$1" pin="SDI" pad="20"/>
<connect gate="G$1" pin="SDO" pad="18"/>
<connect gate="G$1" pin="STBYN/RESETN" pad="3"/>
<connect gate="G$1" pin="STCK" pad="25"/>
<connect gate="G$1" pin="SW" pad="4"/>
<connect gate="G$1" pin="VBOOT" pad="11"/>
<connect gate="G$1" pin="VDD" pad="17"/>
<connect gate="G$1" pin="VREG" pad="6"/>
<connect gate="G$1" pin="VSA" pad="2"/>
<connect gate="G$1" pin="VSA2" pad="26"/>
<connect gate="G$1" pin="VSB" pad="12"/>
<connect gate="G$1" pin="VSB2" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-10648"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L298" prefix="U">
<description>L298 Dual Full Bridge Driver</description>
<gates>
<gate name="G$1" symbol="L298"/>
</gates>
<devices>
<device name="" package="MULTIWATT15">
<connects>
<connect gate="G$1" pin="CSA" pad="1"/>
<connect gate="G$1" pin="CSB" pad="15"/>
<connect gate="G$1" pin="ENA" pad="6"/>
<connect gate="G$1" pin="ENB" pad="11"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="IN1" pad="5"/>
<connect gate="G$1" pin="IN2" pad="7"/>
<connect gate="G$1" pin="IN3" pad="10"/>
<connect gate="G$1" pin="IN4" pad="12"/>
<connect gate="G$1" pin="OUT1" pad="2"/>
<connect gate="G$1" pin="OUT2" pad="3"/>
<connect gate="G$1" pin="OUT3" pad="13"/>
<connect gate="G$1" pin="OUT4" pad="14"/>
<connect gate="G$1" pin="VLS" pad="9"/>
<connect gate="G$1" pin="VS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HEATSINK" package="MULTIWATT15_6400BGHEATSINK">
<connects>
<connect gate="G$1" pin="CSA" pad="1"/>
<connect gate="G$1" pin="CSB" pad="15"/>
<connect gate="G$1" pin="ENA" pad="6"/>
<connect gate="G$1" pin="ENB" pad="11"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="IN1" pad="5"/>
<connect gate="G$1" pin="IN2" pad="7"/>
<connect gate="G$1" pin="IN3" pad="10"/>
<connect gate="G$1" pin="IN4" pad="12"/>
<connect gate="G$1" pin="OUT1" pad="2"/>
<connect gate="G$1" pin="OUT2" pad="3"/>
<connect gate="G$1" pin="OUT3" pad="13"/>
<connect gate="G$1" pin="OUT4" pad="14"/>
<connect gate="G$1" pin="VLS" pad="9"/>
<connect gate="G$1" pin="VS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L298_BRIDGE_DRIVER">
<description>Full-bridge power driver IC</description>
<gates>
<gate name="G$1" symbol="L298_BRIDGE_DRIVER"/>
</gates>
<devices>
<device name="" package="POWERSO20">
<connects>
<connect gate="G$1" pin="ENA" pad="8"/>
<connect gate="G$1" pin="ENB" pad="14"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@10" pad="10"/>
<connect gate="G$1" pin="GND@11" pad="11"/>
<connect gate="G$1" pin="GND@20" pad="20"/>
<connect gate="G$1" pin="IN1" pad="7"/>
<connect gate="G$1" pin="IN2" pad="9"/>
<connect gate="G$1" pin="IN3" pad="13"/>
<connect gate="G$1" pin="IN4" pad="15"/>
<connect gate="G$1" pin="NC@18" pad="18"/>
<connect gate="G$1" pin="NC@3" pad="3"/>
<connect gate="G$1" pin="OUT1" pad="4"/>
<connect gate="G$1" pin="OUT2" pad="5"/>
<connect gate="G$1" pin="OUT3" pad="16"/>
<connect gate="G$1" pin="OUT4" pad="17"/>
<connect gate="G$1" pin="SENSE_A" pad="2"/>
<connect gate="G$1" pin="SENSE_B" pad="19"/>
<connect gate="G$1" pin="VS" pad="6"/>
<connect gate="G$1" pin="VSS" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09133"/>
<attribute name="VALUE" value="L298P013"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STA540">
<description>Multiwatt package for L298 bridge driver</description>
<gates>
<gate name="G$1" symbol="STA540"/>
</gates>
<devices>
<device name="" package="MULTIWATT15">
<connects>
<connect gate="G$1" pin="DIAG" pad="10"/>
<connect gate="G$1" pin="IN1" pad="4"/>
<connect gate="G$1" pin="IN2" pad="5"/>
<connect gate="G$1" pin="IN3" pad="12"/>
<connect gate="G$1" pin="IN4" pad="11"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="2"/>
<connect gate="G$1" pin="OUT3" pad="15"/>
<connect gate="G$1" pin="OUT4" pad="14"/>
<connect gate="G$1" pin="P-GND" pad="8"/>
<connect gate="G$1" pin="S-GND" pad="9"/>
<connect gate="G$1" pin="STBY" pad="7"/>
<connect gate="G$1" pin="SVR" pad="6"/>
<connect gate="G$1" pin="VCC1" pad="3"/>
<connect gate="G$1" pin="VCC2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="W/6400BG_HEATSINK" package="MULTIWATT15_6400BGHEATSINK">
<connects>
<connect gate="G$1" pin="DIAG" pad="10"/>
<connect gate="G$1" pin="IN1" pad="4"/>
<connect gate="G$1" pin="IN2" pad="5"/>
<connect gate="G$1" pin="IN3" pad="12"/>
<connect gate="G$1" pin="IN4" pad="11"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="2"/>
<connect gate="G$1" pin="OUT3" pad="15"/>
<connect gate="G$1" pin="OUT4" pad="14"/>
<connect gate="G$1" pin="P-GND" pad="8"/>
<connect gate="G$1" pin="S-GND" pad="9"/>
<connect gate="G$1" pin="STBY" pad="7"/>
<connect gate="G$1" pin="SVR" pad="6"/>
<connect gate="G$1" pin="VCC1" pad="3"/>
<connect gate="G$1" pin="VCC2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="W/YB324G_HEATSINK" package="MULTIWATT15_YB324GHEATSINK">
<connects>
<connect gate="G$1" pin="DIAG" pad="10"/>
<connect gate="G$1" pin="IN1" pad="4"/>
<connect gate="G$1" pin="IN2" pad="5"/>
<connect gate="G$1" pin="IN3" pad="12"/>
<connect gate="G$1" pin="IN4" pad="11"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="2"/>
<connect gate="G$1" pin="OUT3" pad="15"/>
<connect gate="G$1" pin="OUT4" pad="14"/>
<connect gate="G$1" pin="P-GND" pad="8"/>
<connect gate="G$1" pin="S-GND" pad="9"/>
<connect gate="G$1" pin="STBY" pad="7"/>
<connect gate="G$1" pin="SVR" pad="6"/>
<connect gate="G$1" pin="VCC1" pad="3"/>
<connect gate="G$1" pin="VCC2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="6400BG_W/SOLDERPOSTS" package="MULTIWATT15_6400BGHEATSINK_2">
<connects>
<connect gate="G$1" pin="DIAG" pad="10"/>
<connect gate="G$1" pin="IN1" pad="4"/>
<connect gate="G$1" pin="IN2" pad="5"/>
<connect gate="G$1" pin="IN3" pad="12"/>
<connect gate="G$1" pin="IN4" pad="11"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="2"/>
<connect gate="G$1" pin="OUT3" pad="15"/>
<connect gate="G$1" pin="OUT4" pad="14"/>
<connect gate="G$1" pin="P-GND" pad="8"/>
<connect gate="G$1" pin="S-GND" pad="9"/>
<connect gate="G$1" pin="STBY" pad="7"/>
<connect gate="G$1" pin="SVR" pad="6"/>
<connect gate="G$1" pin="VCC1" pad="3"/>
<connect gate="G$1" pin="VCC2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TB6612FNG">
<description>Toshiba 1A dual motor driver
IC-09363</description>
<gates>
<gate name="G$1" symbol="TB6612FNG"/>
</gates>
<devices>
<device name="" package="SSOP24">
<connects>
<connect gate="G$1" pin="A01@1" pad="1"/>
<connect gate="G$1" pin="A01@2" pad="2"/>
<connect gate="G$1" pin="A02@5" pad="5"/>
<connect gate="G$1" pin="A02@6" pad="6"/>
<connect gate="G$1" pin="AIN1" pad="21"/>
<connect gate="G$1" pin="AIN2" pad="22"/>
<connect gate="G$1" pin="B01@11" pad="11"/>
<connect gate="G$1" pin="B01@12" pad="12"/>
<connect gate="G$1" pin="B02@7" pad="7"/>
<connect gate="G$1" pin="B02@8" pad="8"/>
<connect gate="G$1" pin="BIN1" pad="17"/>
<connect gate="G$1" pin="BIN2" pad="16"/>
<connect gate="G$1" pin="GND" pad="18"/>
<connect gate="G$1" pin="PGND1@3" pad="3"/>
<connect gate="G$1" pin="PGND1@4" pad="4"/>
<connect gate="G$1" pin="PGND2@10" pad="10"/>
<connect gate="G$1" pin="PGND2@9" pad="9"/>
<connect gate="G$1" pin="PWMA" pad="23"/>
<connect gate="G$1" pin="PWMB" pad="15"/>
<connect gate="G$1" pin="STBY" pad="19"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="VM1" pad="24"/>
<connect gate="G$1" pin="VM2" pad="13"/>
<connect gate="G$1" pin="VM3" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09363"/>
<attribute name="VALUE" value="TB6612FNG"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VNH2SP30">
<description>30A motor driver IC(IC-10030,moster moto)</description>
<gates>
<gate name="G$1" symbol="VNH2SP30"/>
</gates>
<devices>
<device name="" package="VNH2SP30">
<connects>
<connect gate="G$1" pin="CS" pad="9"/>
<connect gate="G$1" pin="EN/DIAA" pad="6"/>
<connect gate="G$1" pin="EN/DIAB" pad="10"/>
<connect gate="G$1" pin="GNDA@26" pad="26"/>
<connect gate="G$1" pin="GNDA@27" pad="27"/>
<connect gate="G$1" pin="GNDA@28" pad="28"/>
<connect gate="G$1" pin="GNDB@18" pad="18"/>
<connect gate="G$1" pin="GNDB@19" pad="19"/>
<connect gate="G$1" pin="GNDB@20" pad="20"/>
<connect gate="G$1" pin="INA" pad="5"/>
<connect gate="G$1" pin="INB" pad="11"/>
<connect gate="G$1" pin="OUTA@1" pad="1"/>
<connect gate="G$1" pin="OUTA@25" pad="25"/>
<connect gate="G$1" pin="OUTA@30" pad="30"/>
<connect gate="G$1" pin="OUTA@SLUG3" pad="SLUG3"/>
<connect gate="G$1" pin="OUTB@15" pad="15"/>
<connect gate="G$1" pin="OUTB@16" pad="16"/>
<connect gate="G$1" pin="OUTB@21" pad="21"/>
<connect gate="G$1" pin="OUTB@SLUG2" pad="SLUG2"/>
<connect gate="G$1" pin="PWM" pad="8"/>
<connect gate="G$1" pin="VCC@13" pad="13"/>
<connect gate="G$1" pin="VCC@23" pad="23"/>
<connect gate="G$1" pin="VCC@3" pad="3"/>
<connect gate="G$1" pin="VCC@SLUG1" pad="SLUG1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AL8805" prefix="U" uservalue="yes">
<description>&lt;h3&gt;Constant current LED driver&lt;/h3&gt;&lt;p&gt;
PWM-able 1MHz switch freq 6V-36V&lt;br&gt;
Up to 1A LED current</description>
<gates>
<gate name="G$1" symbol="AL8805"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="CTRL" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SET" pad="4"/>
<connect gate="G$1" pin="SW" pad="1"/>
<connect gate="G$1" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11626"/>
<attribute name="VALUE" value="AL8805WS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ULN2803" prefix="ULN2803" uservalue="yes">
<description>&lt;b&gt;Darlington Driver(IC-07959, low stock)&lt;/b&gt;
ULN2803 Darlington array. 500mA max per channel, 8-channel package. Spark Fun Electronics SKU : COM-00312</description>
<gates>
<gate name="G$1" symbol="ULN2803"/>
</gates>
<devices>
<device name="DIP" package="DIL18">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOIC" package="SO018">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOICW" package="SO18L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L298_SMD_W_PAD">
<description>Full-bridge power driver IC

This device uses the ground pad under the IC</description>
<gates>
<gate name="G$1" symbol="L298_SMD_W_PAD"/>
</gates>
<devices>
<device name="" package="POWERSO20_L298_PAD">
<connects>
<connect gate="G$1" pin="ENA" pad="8"/>
<connect gate="G$1" pin="ENB" pad="14"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@10" pad="10"/>
<connect gate="G$1" pin="GND@11" pad="11"/>
<connect gate="G$1" pin="GND@20" pad="20"/>
<connect gate="G$1" pin="GND@PAD" pad="PAD"/>
<connect gate="G$1" pin="IN1" pad="7"/>
<connect gate="G$1" pin="IN2" pad="9"/>
<connect gate="G$1" pin="IN3" pad="13"/>
<connect gate="G$1" pin="IN4" pad="15"/>
<connect gate="G$1" pin="NC@18" pad="18"/>
<connect gate="G$1" pin="NC@3" pad="3"/>
<connect gate="G$1" pin="OUT1" pad="4"/>
<connect gate="G$1" pin="OUT2" pad="5"/>
<connect gate="G$1" pin="OUT3" pad="16"/>
<connect gate="G$1" pin="OUT4" pad="17"/>
<connect gate="G$1" pin="SENSE_A" pad="2"/>
<connect gate="G$1" pin="SENSE_B" pad="19"/>
<connect gate="G$1" pin="VS" pad="6"/>
<connect gate="G$1" pin="VSS" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09133"/>
<attribute name="VALUE" value="L298"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLC5947">
<description>&lt;h3&gt;TI TLC5947 24-channel 12-bit constant current PWM driver&lt;/h3&gt;
&lt;p&gt;The TLC5947 is a 24-channel, constant-current sink LED driver. Each channel is individually adjustable with 4096 pulse-width modulated (PWM) steps. PWM control is repeated automatically with the programmed grayscale (GS) data. GS data are written via a serial interface port. The current value of all 24 channels is set by a single external resistor.&lt;/p&gt;

The TLC5947 has a thermal shutdown (TSD) function that turns off all output drivers during an over-temperature condition. All of the output drivers automatically restart when the temperature returns to normal conditions.
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”[PRODUCT1LINK]”&gt;[PRODUCT 1]&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TLC5947"/>
</gates>
<devices>
<device name="" package="HTSSOP32">
<connects>
<connect gate="G$1" pin="!BLANK" pad="BLANK"/>
<connect gate="G$1" pin="GND" pad="EPAD GND P$1 P$2 P$3 P$4 P$5 P$6 P$7 P$8 P$9 P$10 P$11 P$12 P$13 P$14 P$15 P$16 P$17 P$18 P$19 P$20 P$21 P$22 P$23 P$24 P$25 P$26 P$27 P$28 P$29 P$30 P$31 P$32"/>
<connect gate="G$1" pin="IREF" pad="IREF"/>
<connect gate="G$1" pin="OUT0" pad="OUT0"/>
<connect gate="G$1" pin="OUT1" pad="OUT1"/>
<connect gate="G$1" pin="OUT10" pad="OUT10"/>
<connect gate="G$1" pin="OUT11" pad="OUT11"/>
<connect gate="G$1" pin="OUT12" pad="OUT12"/>
<connect gate="G$1" pin="OUT13" pad="OUT13"/>
<connect gate="G$1" pin="OUT14" pad="OUT14"/>
<connect gate="G$1" pin="OUT15" pad="OUT15"/>
<connect gate="G$1" pin="OUT16" pad="OUT16"/>
<connect gate="G$1" pin="OUT17" pad="OUT17"/>
<connect gate="G$1" pin="OUT18" pad="OUT18"/>
<connect gate="G$1" pin="OUT19" pad="OUT19"/>
<connect gate="G$1" pin="OUT2" pad="OUT2"/>
<connect gate="G$1" pin="OUT20" pad="OUT20"/>
<connect gate="G$1" pin="OUT21" pad="OUT21"/>
<connect gate="G$1" pin="OUT22" pad="OUT22"/>
<connect gate="G$1" pin="OUT23" pad="OUT23"/>
<connect gate="G$1" pin="OUT3" pad="OUT3"/>
<connect gate="G$1" pin="OUT4" pad="OUT4"/>
<connect gate="G$1" pin="OUT5" pad="OUT5"/>
<connect gate="G$1" pin="OUT6" pad="OUT6"/>
<connect gate="G$1" pin="OUT7" pad="OUT7"/>
<connect gate="G$1" pin="OUT8" pad="OUT8"/>
<connect gate="G$1" pin="OUT9" pad="OUT9"/>
<connect gate="G$1" pin="SCLK" pad="SCLK"/>
<connect gate="G$1" pin="SIN" pad="SIN"/>
<connect gate="G$1" pin="SOUT" pad="SOUT"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
<connect gate="G$1" pin="XLAT" pad="XLAT"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-13817"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BNO080" prefix="U">
<description>&lt;h3&gt;Hillcrest Labs BNO080 - High Precision IMU (VR)&lt;/h3&gt;
&lt;p&gt;The VR IMU uses the impressive BNO080 IMU. This IC has a combination triple axis accelerometer/gyro/magnetometer packaged with an ARM Cortex M0+ running powerful algorithms. The BNO080 Inertial Measurement Unit (IMU) produces accurate rotation vector headings, excellently suited for VR and other heading applications with a static rotation error of 2 degrees or less. It’s what we’ve been waiting for: all the sensor data is combined and drift corrected into meaningful, accurate IMU information.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/14618”&gt;VR IMU (BNO080)&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="U1" symbol="BNO080-IMU"/>
</gates>
<devices>
<device name="" package="LGA-28">
<connects>
<connect gate="U1" pin="!BOOT" pad="4"/>
<connect gate="U1" pin="!H_CS" pad="18"/>
<connect gate="U1" pin="!H_INT" pad="14"/>
<connect gate="U1" pin="!RST" pad="11"/>
<connect gate="U1" pin="CAP" pad="9"/>
<connect gate="U1" pin="CLKSEL0" pad="10"/>
<connect gate="U1" pin="CLKSEL1" pad="26"/>
<connect gate="U1" pin="GND" pad="2"/>
<connect gate="U1" pin="GNDIO" pad="25"/>
<connect gate="U1" pin="H_SA0/MOSI" pad="17"/>
<connect gate="U1" pin="H_SCL/SCLK/RX" pad="19"/>
<connect gate="U1" pin="H_SDA/MISO/TX" pad="20"/>
<connect gate="U1" pin="PS0/WAKE" pad="6"/>
<connect gate="U1" pin="PS1" pad="5"/>
<connect gate="U1" pin="S_SCL" pad="15"/>
<connect gate="U1" pin="S_SDA" pad="16"/>
<connect gate="U1" pin="VDD" pad="3"/>
<connect gate="U1" pin="VDDIO" pad="28"/>
<connect gate="U1" pin="XIN32" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SEN-13947"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MLX90540_MLX90640" prefix="U">
<description>&lt;h3&gt;Melexis MLX90640 Infrared Array&lt;/h3&gt;
&lt;p&gt;
The MLX90640 is a fully calibrated 32x24 pixels
thermal IR array in an industry standard 4-lead TO39
package with digital interface.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MLX90540_MLX90640"/>
</gates>
<devices>
<device name="" package="MLX90540_MLX90640">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="SCL" pad="SCL"/>
<connect gate="G$1" pin="SDA" pad="SDA"/>
<connect gate="G$1" pin="VDD" pad="VDD"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-14042"/>
<attribute name="VALUE" value="55DEG"/>
</technology>
<technology name="4">
<attribute name="PROD_ID" value="IC-14041"/>
<attribute name="VALUE" value="110DEG"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX30101EFD" prefix="U">
<description>&lt;h3&gt;MAX30101 High-Sensitivity Pulse Oximeter and
Heart-Rate Sensor&lt;/h3&gt;

&lt;p&gt;The MAX30101 is an integrated pulse oximetry and
heart-rate monitor module. It includes internal LEDs,
photodetectors, optical elements, and low-noise electronics
with ambient light rejection. The MAX30101 provides a
complete system solution to ease the design-in process
for mobile and wearable devices.
&lt;/p&gt;
&lt;p&gt;
The MAX30101 operates on a single 1.8V power supply
and a separate 5.0V power supply for the internal LEDs.
Communication is through a standard I2C-compatible
interface. The module can be shut down through software
with zero standby current, allowing the power rails to
remain powered at all times&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MAX30101"/>
</gates>
<devices>
<device name="" package="14_PIN_OESIP">
<connects>
<connect gate="G$1" pin="!INT" pad="P13"/>
<connect gate="G$1" pin="GND" pad="P4 P12"/>
<connect gate="G$1" pin="NC" pad="P1 P5 P6 P7 P8 P14"/>
<connect gate="G$1" pin="SCL" pad="P2"/>
<connect gate="G$1" pin="SDA" pad="P3"/>
<connect gate="G$1" pin="VDD" pad="P11"/>
<connect gate="G$1" pin="VDD_LED" pad="P9 P10"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-14270"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX32664GWEA" prefix="U">
<description>&lt;h3&gt;Maxim MAX32664 Biometric Sensor Hub&lt;/h3&gt;
&lt;p&gt;he MAX32664 is a sensor hub family with embedded
firmware and algorithms for wearables. It seamlessly
enables customer-desired sensor functionality, including
communication with Maxim’s optical sensor solutions and
delivering raw or calculated data to the outside world. This
is achieved while keeping overall system power consumption in check.
&lt;/p&gt;
&lt;p&gt;
The MAX32664 Version A supports the MAX30101/
MAX30102 high-sensitivity pulse oximeter and heart rate
sensor for wearable health for finger-based applications.
&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MAX32664"/>
</gates>
<devices>
<device name="" package="16_PIN_WLP">
<connects>
<connect gate="G$1" pin="!MFIO" pad="16"/>
<connect gate="G$1" pin="!RST" pad="12"/>
<connect gate="G$1" pin="ACCEL_INT" pad="15"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="HR_INT" pad="6"/>
<connect gate="G$1" pin="NC" pad="7 8 11"/>
<connect gate="G$1" pin="OSC_IN" pad="2"/>
<connect gate="G$1" pin="OSC_OUT" pad="1"/>
<connect gate="G$1" pin="SLAVE_SCL" pad="10"/>
<connect gate="G$1" pin="SLAVE_SDA" pad="9"/>
<connect gate="G$1" pin="SNSR_SCL" pad="5"/>
<connect gate="G$1" pin="SNSR_SDA" pad="14"/>
<connect gate="G$1" pin="VCORE" pad="4"/>
<connect gate="G$1" pin="VDD" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-14271"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
