<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.3">
<drawing>
<library>
<description>&lt;h3&gt;SparkFun Jumpers&lt;/h3&gt;
In this library you'll find jumpers, or other semipermanent means of changing current paths. The least permanent form is the solder jumper. These can be changed by adding, removing, or moving solder. In cases that are less likely to be changed we have jumpers that are connected with traces. These can be cut with a razor, or reconnected with solder. Reference designator JP.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMT-JUMPER_3_NO_SILK">
</package>
<package name="SMT-JUMPER_3_1-NC_TRACE_SILK">
</package>
<package name="SMT-JUMPER_3_1-NC_PASTE_SILK">
</package>
<package name="SMT-JUMPER_3_2-NC_TRACE_SILK">
</package>
<package name="SMT-JUMPER_3_2-NC_PASTE_SILK">
</package>
<package name="SMT-JUMPER_3_2-NC_PASTE_NO-SILK">
</package>
<package name="SMT-JUMPER_3_1-NC_PASTE_NO-SILK">
</package>
<package name="SMT-JUMPER_3_1-NC_TRACE_NO-SILK">
</package>
<package name="SMT-JUMPER_3_2-NC_TRACE_NO-SILK">
</package>
<package name="SMT-JUMPER_3_NO_NO-SILK">
</package>
<package name="SMT-JUMPER_2_NO_SILK_ROUND">
</package>
<package name="SMT-JUMPER_2_NO_NO-SILK_ROUND">
</package>
<package name="SMT-JUMPER_2_NC_TRACE_SILK">
</package>
<package name="SMT-JUMPER_2_NC_TRACE_NO-SILK">
</package>
<package name="SMT-JUMPER_2_NC_PASTE_SILK">
</package>
<package name="SMT-JUMPER_2_NC_PASTE_NO-SILK">
</package>
<package name="SMT-JUMPER_2_NO_SILK">
</package>
<package name="SMT-JUMPER_2_NO_NO-SILK">
</package>
<package name="SMT-JUMPER_3_0-NO_TRACE_NO-SILK">
</package>
</packages>
<symbols>
<symbol name="SMT-JUMPER_2_NC_PASTE">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="SMT-JUMPER_2_NC_TRACE">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="SMT-JUMPER_2_NO">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="SMT-JUMPER_3_1-NC_PASTE">
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="SMT-JUMPER_3_1-NC_TRACE">
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="SMT-JUMPER_3_2-NC_PASTE">
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="SMT-JUMPER_3_2-NC_TRACE">
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="SMT-JUMPER_3_NO">
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="JUMPER-SMT_2_NO" prefix="JP">
<description>&lt;h3&gt;Normally open jumper&lt;/h3&gt;
&lt;p&gt;This jumper has two pads in close proximity to each other. Apply solder to close the connection.&lt;/p&gt;

&lt;p&gt;Round pads are easier to solder for beginners, but are a lot larger.&lt;/p&gt;
&lt;p&gt;SparkFun Product that uses the round pads:
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12781"&gt;SparkFun EL Sequencer&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SMT-JUMPER_2_NO"/>
</gates>
<devices>
<device name="_NO-SILK" package="SMT-JUMPER_2_NO_NO-SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_NO-SILK_ROUND" package="SMT-JUMPER_2_NO_NO-SILK_ROUND">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_SILK" package="SMT-JUMPER_2_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_SILK_ROUND" package="SMT-JUMPER_2_NO_SILK_ROUND">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JUMPER-SMT_2_NC_TRACE" prefix="JP">
<description>&lt;h3&gt;Normally closed trace jumper&lt;/h3&gt;
&lt;p&gt;This jumper has a trace between two pads so it's normally closed (NC). Use a razor knife to open the connection. For best results follow the IPC guidelines for cutting traces:&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;Cutout at least 0.063 mm (0.005 in).&lt;/li&gt;
&lt;li&gt;Remove all loose material to clean up the cut area.&lt;/li&gt;
&lt;li&gt;Seal the cut with an approved epoxy.&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;Reapply solder to reclose the connection.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SMT-JUMPER_2_NC_TRACE"/>
</gates>
<devices>
<device name="_NO-SILK" package="SMT-JUMPER_2_NC_TRACE_NO-SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_SILK" package="SMT-JUMPER_2_NC_TRACE_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JUMPER-SMT_2_NC_PASTE" prefix="JP">
<description>&lt;h3&gt;Normally closed solder jumper&lt;/h3&gt;
&lt;p&gt;This jumper has an aperture in the stencil to allow solder paste to bridge the split in the wire so it's normally closed (NC). Wick off the solder to open the connection. Reapply solder to reclose the connection.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SMT-JUMPER_2_NC_PASTE"/>
</gates>
<devices>
<device name="_NO-SILK" package="SMT-JUMPER_2_NC_PASTE_NO-SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_SILK" package="SMT-JUMPER_2_NC_PASTE_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JUMPER-SMT_3_NO" prefix="JP">
<description>&lt;h3&gt;Normally open jumper&lt;/h3&gt;
&lt;p&gt;This jumper has three pads in close proximity to each other. Apply solder to close the connection(s).&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SMT-JUMPER_3_NO"/>
</gates>
<devices>
<device name="_NO-SILK" package="SMT-JUMPER_3_NO_NO-SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_SILK" package="SMT-JUMPER_3_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_NO_SILK" package="SMT-JUMPER_3_0-NO_TRACE_NO-SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JUMPER-SMT_3_1-NC_TRACE" prefix="JP">
<description>&lt;h3&gt;Normally closed trace jumper (1 of 2 connections)&lt;/h3&gt;
&lt;p&gt;This jumper has a trace between two pads so it's normally closed (NC). The other connection is normally open (NO). Use a razor knife to open the connection. For best results follow the IPC guidelines for cutting traces:&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;Cutout at least 0.063 mm (0.005 in).&lt;/li&gt;
&lt;li&gt;Remove all loose material to clean up the cut area.&lt;/li&gt;
&lt;li&gt;Seal the cut with an approved epoxy.&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;Reapply solder to reclose the connection, or to close the NO connection.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SMT-JUMPER_3_1-NC_TRACE"/>
</gates>
<devices>
<device name="_SILK" package="SMT-JUMPER_3_1-NC_TRACE_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_NO-SILK" package="SMT-JUMPER_3_1-NC_TRACE_NO-SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JUMPER-SMT_3_2-NC_TRACE" prefix="JP">
<description>&lt;h3&gt;Normally closed trace jumper (2 of 2 connections)&lt;/h3&gt;
&lt;p&gt;This jumper has a trace between all three pads so they are normally closed (NC). Use a razor knife to open the connection(s). For best results follow the IPC guidelines for cutting traces:&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;Cutout at least 0.063 mm (0.005 in).&lt;/li&gt;
&lt;li&gt;Remove all loose material to clean up the cut area.&lt;/li&gt;
&lt;li&gt;Seal the cut with an approved epoxy.&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;Reapply solder to reclose the connection(s).&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SMT-JUMPER_3_2-NC_TRACE"/>
</gates>
<devices>
<device name="_NO-SILK" package="SMT-JUMPER_3_2-NC_TRACE_NO-SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_SILK" package="SMT-JUMPER_3_2-NC_TRACE_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JUMPER-SMT_3_2-NC_PASTE" prefix="JP">
<description>&lt;h3&gt;Normally closed solder jumper (2 of 2 connections)&lt;/h3&gt;
&lt;p&gt;This jumper has an aperture in the stencil to allow solder paste to bridge both connections. Both connections are normally closed (NC). Wick off the solder to open the connection(s). Reapply solder to reclose the connection(s).&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SMT-JUMPER_3_2-NC_PASTE"/>
</gates>
<devices>
<device name="_SILK" package="SMT-JUMPER_3_2-NC_PASTE_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_NO-SILK" package="SMT-JUMPER_3_2-NC_PASTE_NO-SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JUMPER-SMT_3_1-NC_PASTE" prefix="JP">
<description>&lt;h3&gt;Normally closed solder jumper (1 of 2 connections)&lt;/h3&gt;
&lt;p&gt;This jumper has an aperture in the stencil to allow solder paste to bridge one of the two connections. One connection is normally closed (NC), while the other is normally open (NO). Wick off the solder to open the connection. Reapply solder to reclose the connection. Apply solder to the other side instead to change the current path.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SMT-JUMPER_3_1-NC_PASTE"/>
</gates>
<devices>
<device name="_NO-SILK" package="SMT-JUMPER_3_1-NC_PASTE_NO-SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_SILK" package="SMT-JUMPER_3_1-NC_PASTE_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
