<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.2">
<drawing>
<library>
<description>&lt;h3&gt;SparkFun RF, WiFi, Cellular, and Bluetooth&lt;/h3&gt;
In this library you'll find things that send or receive RF-- cellular modules, Bluetooth, WiFi, etc.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ANT-2.4GHZ-9.5X2.0MM">
<description>&lt;h3&gt;2.4GHz Chip Antenna - 9.5 x 2.0 x 1.2 mm&lt;/h3&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Wireless/General/SPK-AT9520-B2R4HAA.pdf"&gt;Example Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="ANT-2.4GHZ-6.5X2.2MM">
<description>&lt;h3&gt;2.45GHz Chip Antenna - 6.5 x 2.2 x 1.0 mm&lt;/h3&gt;
&lt;p&gt; 6.5 x 2.2 x 1.0 mm package&lt;/p&gt;
&lt;p&gt;Package used for Linx ANT-2.45-CHIP-x antenna&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/chip-antenna-2.4ghz.pdf"&gt;Example Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="QFN-64-9X9MM">
<description>&lt;h3&gt;64-pin QFN 9x9mm, 0.5mm pitch&lt;/h3&gt;
&lt;p&gt;Package used by ATmega128RFA1&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.atmel.com/Images/Atmel-8266-MCU_Wireless-ATmega128RFA1_Datasheet.pdf"&gt;Example Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="BALUN-0805">
<description>&lt;h3&gt;Balun - 0805 Package&lt;/h3&gt;
&lt;p&gt;Transformer to convert an unbalanced signal to a balenced one, or vice-versa.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://katalog.we-online.de/pbs/datasheet/748421245.pdf"&gt;Example Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="RN41">
<description>&lt;h3&gt;Roving Networks RN-41 Bluetooth Module&lt;/h3&gt;
&lt;p&gt;13.4x25.8x2mm module&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Wireless/Bluetooth/rn-41-ds-v3.41r.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="BTM182">
<description>&lt;h3&gt;Rayson BTM-182 Bluetooth Module&lt;/h3&gt;
&lt;p&gt;BTM-182 Class2 Bluetooth Module from Rayson&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Wireless/Bluetooth/BTM182.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="ID-12">
<description>&lt;h3&gt;ID-2, ID-12, and ID-20 Low-voltage RFID Readers&lt;/h3&gt;
&lt;p&gt;Footprint works for ID-2LA, ID-12LA, and ID-20LA modules&lt;/p&gt;
&lt;p&gt;Dimensions of RFID readers vary, but the pin-out remains the same.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Sensors/ID/ID-2LA,%20ID-12LA,%20ID-20LA2013-4-10.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="ID-12_LOCK">
<description>&lt;h3&gt;ID-2, ID-12, and ID-20 Low-voltage RFID Readers&lt;/h3&gt;
&lt;p&gt;&lt;b&gt;Locking PTH footprint!&lt;/b&gt; Adjacent holes are offset.
&lt;p&gt;Footprint works for ID-2LA, ID-12LA, and ID-20LA modules&lt;/p&gt;
&lt;p&gt;Dimensions of RFID readers vary, but the pin-out remains the same.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Sensors/ID/ID-2LA,%20ID-12LA,%20ID-20LA2013-4-10.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="ID-12_SMD">
<description>&lt;h3&gt;ID-2, ID-12, and ID-20 Low-voltage RFID Readers - SMD Footprint&lt;/h3&gt;
&lt;p&gt;Footprint works for ID-2LA, ID-12LA, and ID-20LA modules&lt;/p&gt;
&lt;p&gt;Dimensions of RFID readers vary, but the pin-out remains the same.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Sensors/ID/ID-2LA,%20ID-12LA,%20ID-20LA2013-4-10.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="QFN20-4X4MM">
<description>&lt;h3&gt;QFN 20-pin, 4x4mm&lt;/h3&gt;
&lt;p&gt;Used by nRF24L01&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/SMD/nRF24L01Pluss_Preliminary_Product_Specification_v1_0.pdf"&gt;Datasheet Example&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="QFN-32-5X5MM">
<description>&lt;h3&gt;QFN 32-Pin w/ Thermal Pad - 5.0 x 5.0 mm&lt;/h3&gt;
&lt;p&gt;Used by nRF24LU1 and nRF24LE1&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Wireless/Nordic/nRF24LU1P_1_0.pdf"&gt;Datasheet Example&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="RF-LINK_RX">
<description>&lt;h3&gt;RF Link Receiver, PTH Package&lt;/h3&gt;
&lt;p&gt;These RF receivers easily fit into a breadboard and work well with microcontrollers to create a very simple wireless data link.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/products/10532"&gt;SparkFun Product&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Wireless/General/RWS-371-6_433.92MHz_ASK_RF_Receiver_Module_Data_Sheet.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="RF-LINK_TX">
<description>&lt;h3&gt;RF Link Transmitter, PTH Package&lt;/h3&gt;
&lt;p&gt;These RF transmitter easily fit into a breadboard and work well with microcontrollers to create a very simple wireless data link.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/products/10534"&gt;SparkFun Product&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Wireless/General/TWS-BS-3_433.92MHz_ASK_RF_Transmitter_Module_Data_Sheet.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="RFM22-XXX-S2">
<description>&lt;h3&gt;Hope RF RFM22 RF Transceiver&lt;/h3&gt;
&lt;p&gt;Package for Hope RF s RFM22-xxx-S2 SMD wireless transciever, xxx is module s frequency band.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/products/12030"&gt;SparkFun Link (915MHz)&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/products/12770"&gt;SparkFun Link (433 MHz)&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Wireless/General/RFM22.PDF"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="RMCM01">
<description>&lt;h3&gt;Polar RMCM-01 Heart Rate Receiver Module&lt;/h3&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Wireless/General/RMCM01.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="RN171">
<description>&lt;h3&gt;Roving Networks RN-171 Wi-Fi Module&lt;/h3&gt;
&lt;p&gt;26.67 x 17.78 x 3.18 mm module&lt;/p&gt;
&lt;p&gt;&lt;a href="http://ww1.microchip.com/downloads/en/DeviceDoc/70005171A.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="QFN-20-3X3MM">
<description>&lt;h3&gt;20-Pin QFN Package 3 x 3 mm&lt;/h3&gt;
&lt;p&gt;Used by Silicon Labs Si470x (Si4703, Si4707, etc.) FM Recievier&lt;/p&gt;

&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/assets/learn_tutorials/2/7/4/Si4703_datasheet.pdf"&gt;Example Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="SM130">
<description>&lt;h3&gt;SM130 13.56 MHz RFID Mifare(R) R/W Module&lt;/h3&gt;
&lt;p&gt;30-pin DIL with 100mil spacing between headers&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Sensors/ID/SM130.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="SM5100B">
<description>&lt;h3&gt;SM5100B GSM/GPRS Module - 60-pin 0.5mm-pitch board-to-board connector&lt;/h3&gt;
&lt;p&gt;Mill layers define four shielding GND tabs.&lt;/p&gt;
&lt;p&gt;The SM5100B GSM/GPRS module interfaces with a board via a 60-pin board-to-board connector.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Prototyping/Connectors/CEL-09535-p5kf.pdf"&gt;Connector Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Cellular/SM5100B-D_HW_spec_V1.0.0.pdf"&gt;SM5100B Hardware Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="WIFLY_GSX">
<description>&lt;h3&gt;Roving Networks RN-131C (WiFly GSX) 802.11b/g Module&lt;/h3&gt;
&lt;p&gt;Wi-Fi module with a 37 x 28.5 x 3.5 mm footprint.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Wireless/WiFi/rn-131-ds.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/products/10004"&gt;SparkFun Product Link&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="XBEE">
<description>&lt;h3&gt;Digi XBee and XBee-PRO RF Modules&lt;/h3&gt;
&lt;p&gt;20-pin 2mm PTH headers.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Wireless/Zigbee/XBee-Dimensional.pdf"&gt;XBee Mechanical Drawings&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.sparkfun.com/datasheets/Prototyping/XBee-Connector.pdf"&gt;Header Mechanical Drawing&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/products/8272"&gt;Header SparkFun Product Link&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="XBEE-SILK">
<description>&lt;h3&gt;Digi XBee and XBee-PRO RF Modules (Silkscreen Dimension Indicators)&lt;/h3&gt;
&lt;p&gt;20-pin 2mm PTH headers. Silkscreen to indicate polarity and dimensions of XBee (non-Pro's)&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Wireless/Zigbee/XBee-Dimensional.pdf"&gt;XBee Mechanical Drawings&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.sparkfun.com/datasheets/Prototyping/XBee-Connector.pdf"&gt;Header Mechanical Drawing&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/products/8272"&gt;Header SparkFun Product Link&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="XBEE-SMD">
<description>&lt;h3&gt;Digi XBee and XBee-PRO RF Modules (SMD pads)&lt;/h3&gt;
&lt;p&gt;20-pin 2mm SMD headers.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Wireless/Zigbee/XBee-Dimensional.pdf"&gt;XBee Mechanical Drawings&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Prototyping/Sockets/xbeeheadersmd2.pdf"&gt;Header Mechanical Drawing&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/products/10030"&gt;Header SparkFun Product Link&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="XBEE-LOCK">
<description>&lt;h3&gt;Digi XBee and XBee-PRO RF Modules (Locking footprint)&lt;/h3&gt;
&lt;p&gt;20-pin 2mm PTH headers - offset to "lock" headers in place for soldering.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Wireless/Zigbee/XBee-Dimensional.pdf"&gt;XBee Mechanical Drawings&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.sparkfun.com/datasheets/Prototyping/XBee-Connector.pdf"&gt;Header Mechanical Drawing&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/products/8272"&gt;Header SparkFun Product Link&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="XTEND-DIGI-MODEM">
<description>&lt;h3&gt;Digi XTend 900 1W RF Module&lt;/h3&gt;
&lt;p&gt;Module dimensions: 6.05 x 3.65 x 0.51 cm&lt;br&gt;
Package for the Xtend Digi Modem 40 mile range.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Wireless/Zigbee/xtend-mechanical.pdf"&gt;Dimensional Drawing&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/products/9411"&gt;SparkFun Product Link&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="BLUERADIO_BR-LE4.0-S2">
<description>&lt;h3&gt;BlueRadio BR-LE4.0-S2 Bluetooth 4.0 Module&lt;/h3&gt;
&lt;p&gt;11.8x17.6x1.9mm&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.blueradios.com/nBlue%20BR-LE4.0-S2%20Summary%20Datasheet.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="RN-52">
<description>&lt;h3&gt;Roving Networks RN-52 Bluetooth Audio Module&lt;/h3&gt;
&lt;p&gt;13.5x26.0x2.7mm module&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Wireless/Bluetooth/rn-52-ds-1.1r.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="QFN-46-13.5X16.3MM">
<description>&lt;h3&gt;Texas Instruments CC3000 Wi-Fi Module&lt;/h3&gt;
&lt;p&gt;Size: 16.3 x 13.5 x 2.0 mm&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.ti.com/lit/ds/symlink/cc3000.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="ANT-2.4GHZ-8.0X1.0MM">
<description>&lt;h3&gt;2.4GHz Chip Antenna - 8.0x1.0mm&lt;/h3&gt;
&lt;p&gt;Package for Johanson Technology 2500AT44M0400E - 2.4GHz SMD antenna.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.mouser.com/ds/2/611/antenna_2500at44m0400-242425.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="BC127">
<description>&lt;h3&gt;BC127 Bluetooth 4.0 Audio Module&lt;/h3&gt;
&lt;p&gt;11.8x18mm module.&lt;/p&gt;
&lt;p&gt; Extra tCream on pads.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.bluecreation.com/userfiles/DataSheet-BC127-latest3.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="RFM69HCW-XXXS2">
<description>&lt;h3&gt;Hope RF RFM69HCW RF Transciever&lt;/h3&gt;
&lt;p&gt;&lt;a href="http://www.orcam.eu/res/Datablad/rfm69hcwv11.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="RFM69W-XXXS2">
<description>&lt;h3&gt;Hope RF RFM69HW RF Transceiver&lt;/h3&gt;
&lt;p&gt;&lt;a href="http://www.hoperf.com/upload/rf/RFM69HW-V1.3.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="RFM69CW-XXXS2">
<description>&lt;h3&gt;Hope RF RFM69CW RF Transciever&lt;/h3&gt;
&lt;p&gt;&lt;a href="http://www.hoperf.com/upload/rf/RFM69CW-V1.1.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="BC118">
<description>&lt;h3&gt;Blue Creation BC118 Bluetooth 4.0 Audio Module&lt;/h3&gt;
&lt;p&gt;14.4x19.3mm&lt;/p&gt;
&lt;p&gt;&lt;a href="http://media.digikey.com/pdf/Data%20Sheets/BlueCreation%20PDFs/BC118_DS.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="SD-CARD">
<description>&lt;h3&gt;SD Card Socket&lt;/h3&gt;
&lt;p&gt;The  4UCONN part number is &lt;a href="http://www.4uconnector.com/online/Itemadrawing.asp?fldseries=19646&amp;seriesno_a=12"&gt;19646&lt;/a&gt;.&lt;/p&gt;
&lt;p&gt;See this part in action on the &lt;a href="https://www.sparkfun.com/products/11400"&gt;Electric Imp Breakout&lt;/a&gt;.&lt;/p&gt;</description>
</package>
<package name="XBEE-LONGPAD">
<description>&lt;h3&gt;Digi XBee and XBee-PRO RF Modules (Long pads)&lt;/h3&gt;
&lt;p&gt;20-pin 2mm PTH headers. Elongated annular rings to make soldering easier.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Wireless/Zigbee/XBee-Dimensional.pdf"&gt;XBee Mechanical Drawings&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.sparkfun.com/datasheets/Prototyping/XBee-Connector.pdf"&gt;Header Mechanical Drawing&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/products/8272"&gt;Header SparkFun Product Link&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="QFN32-5X5MM">
<description>&lt;h3&gt;32-pin QFN 5.0 x 5.0 mm, 0.5mm pitch&lt;/h3&gt;
&lt;p&gt;Used by ESP8266&lt;/p&gt;
&lt;p&gt;&lt;a href="http://espressif.com/sites/default/files/documentation/0a-esp8266_datasheet_en_v4.4.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="TRACE_ANTENNA_2.4GHZ_25.7MM">
<description>&lt;h3&gt;2.4GHz Inverted F PCB Trace Antenna&lt;/h3&gt;
&lt;p&gt;PCB trace antenna with a 25.7 x 7.5 mm footprint.&lt;/p&gt;
&lt;p&gt;Based on layout from &lt;a href="http://www.ti.com/lit/an/swru120b/swru120b.pdf"&gt;TI design note DN0007&lt;/a&gt;.&lt;/p&gt;</description>
</package>
<package name="TRACE_ANTENNA_2.4GHZ_15.2MM">
<description>&lt;h3&gt;2.4GHz Meander PCB Trace Antenna&lt;/h3&gt;
&lt;p&gt;PCB trace antenna with a 15.2 x 5.7mm footprint.&lt;/p&gt;
&lt;p&gt;Based on layout from &lt;a href="http://www.ti.com/lit/an/swra117d/swra117d.pdf"&gt;TI app note AN043&lt;/a&gt;.&lt;/p&gt;</description>
</package>
<package name="QFN48-0.4MM">
<description>&lt;h3&gt;QFN 48 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 48&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.4mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://cdn.sparkfun.com/datasheets/IoT/esp32_datasheet_en.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;ESP32&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="QFN48-6X6MM">
<description>&lt;h3&gt;QFN-48 pin 6x6mm&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 48&lt;/li&gt;
&lt;li&gt;Area: 6x6mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://cdn.sparkfun.com/datasheets/Wireless/Bluetooth/nRF52832_PS_v1.0.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;nRF52832&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="RFD77101">
<description>&lt;h3&gt;Simblee  BLE Module RFD77101&lt;/h3&gt;
&lt;p&gt;© 2015 RF Digital Corporation&lt;br/&gt; 
&lt;a href="http://www.RFDigital.com"&gt;www.RFDigital.com&lt;/a&gt;&lt;br/&gt;
&lt;a href="http://www.Simblee.com"&gt;www.Simblee.com&lt;/a&gt;&lt;br/&gt;
PATENTS PENDING 04.01.2015&lt;br/&gt;&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 45&lt;/li&gt;
&lt;li&gt;Pin pitch:0.5mm&lt;/li&gt;
&lt;li&gt;Area:7mmx10mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://cdn.sparkfun.com/datasheets/IoT/Simblee%20RFD77101%20Datasheet%20v1.0.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;RFD77101&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="ESP07">
</package>
<package name="ESP-WROOM-32">
</package>
<package name="ESP-WROOM-32-NARROW">
</package>
<package name="RFM95/96/97/98W">
<description>&lt;h3&gt;RFM95/96/97/98&lt;/h3&gt;

&lt;p&gt;The RFM95/96/97/98(W) transceivers feature the
LoRaTM    long range modem that provides ultra-long range
spread spectrum communication and high interference
immunity whilst minimising current consumption. &lt;/p&gt;

&lt;p&gt;&lt;a href="http://www.hoperf.com/upload/rf/RFM95_96_97_98W.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="1X10-1.25MM-SMD">
</package>
<package name="ESP-12S">
</package>
<package name="ESP8266_ESP-01">
<description>&lt;h3&gt;ESP8266 ESP-01 Module&lt;/h3&gt;</description>
</package>
<package name="E19-915MS1W">
<description>&lt;h3&gt;E19-915M30S - 1W 915M TRX Using SX1276&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 22&lt;/li&gt;
&lt;li&gt;Pin pitch: Varies&lt;/li&gt;
&lt;li&gt;Area: 1.15 in x 1.65 in&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://cdn.sparkfun.com/assets/d/8/3/6/e/E19__915M30S__Datasheet_EN_v1.0.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s): 
&lt;ul&gt;&lt;li&gt;SAMD21 ProRF 1W&lt;/li&gt;
&lt;li&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="ANT-2.4GHZ-3.2X1.6X1.2MM">
<description>&lt;h3&gt;SMD WiFi/Bluetooth (2.4GHz) Antenna -- 3.2x1.6x1.2mm&lt;/h3&gt;
&lt;p&gt;Features:
&lt;ul&gt;
&lt;li&gt;2450MHz, Bandwidth ≥90MHz&lt;/li&gt;
&lt;li&gt;Suitable for RoHS compliant reflow&lt;/li&gt;
&lt;li&gt;Gain 0.5dBi (Peak) / -1dBi (Average)&lt;/li&gt;
&lt;li&gt;VSWR &lt;2:1&lt;/li&gt;
&lt;li&gt;Small size – 3.2 x 1.6 x 1.2mm (0.125 x 0.62 x 0.047 inch)&lt;/li&gt;
&lt;li&gt;Non Ground Mounting type.&lt;/li&gt;
&lt;li&gt;Power Handling 3W Max&lt;/li&gt;
&lt;li&gt;Matched to 50 Ohm.&lt;/li&gt;
&lt;/ul&gt;
&lt;/p&gt;

&lt;p&gt;&lt;a href=https://abracon.com/chip-antenna/AMCA31-2R450G-S1F-T.pdf&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="ANT-2.4GHZ-3.2X1.6X1.2MM-REDUCED_KEEPOUT">
</package>
<package name="ESP-WROVER-32">
</package>
<package name="XBEE3-SMD">
</package>
<package name="SMA-EDGE">
<description>&lt;b&gt;SMA Antenna Connector&lt;/b&gt;&lt;p&gt;
This is a footprint for an edge mount RF antenna. Works pretty well with SMA type connectors but may also work with other edge mount RF connectors. Keep in mind, these edge mount connectors assume you are using a 0.062" PCB thickness.</description>
</package>
</packages>
<symbols>
<symbol name="ANTENNA-GROUNDED">
<description>&lt;h3&gt;Antenna (with ground termination)&lt;/h3&gt;</description>
<pin name="GND"/>
<pin name="SIGNAL"/>
</symbol>
<symbol name="ANTENNA">
<description>&lt;h3&gt;Antenna&lt;/h3&gt;</description>
<pin name="SIGNAL"/>
</symbol>
<symbol name="ATMEGA128RFA1">
<description>&lt;h3&gt;Atmel ATmega128RFA1 8-Bit AVR Microcontroller w/ Low-Power 2.4GHz RF Transceiver&lt;/h3&gt;
&lt;p&gt;The  ATmega128RFA1  is  a  low-power  CMOS  8-bit  microcontroller  based  on  the  AVR enhanced RISC architecture combined with a high data rate transceiver for the 2.4 GHz ISM band. By   executing   powerful   instructions   in   a   single   clock   cycle,   the   device   achieves  throughputs  approaching  1  MIPS  per  MHz  allowing  the  system  designer  to  optimize power consumption versus processing speed. The  radio  transceiver  provides  high  data  rates  from  250 kb/s  up  to  2 Mb/s,  frame handling,  outstanding receiver  sensitivity  and  high transmit  output  power  enabling  a very robust wireless communication. &lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.atmel.com/Images/Atmel-8266-MCU_Wireless-ATmega128RFA1_Datasheet.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/products/11197"&gt;SparkFun ATmega128RFA1 Development Board&lt;/a&gt;&lt;/p&gt;</description>
<pin name="EVDD"/>
<pin name="DEVDD@23"/>
<pin name="AVDD"/>
<pin name="DVDD@21"/>
<pin name="AVSS@58"/>
<pin name="DVSS@20"/>
<pin name="PB0"/>
<pin name="PB1/SCK"/>
<pin name="PB2/PDI"/>
<pin name="PB3/PDO"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="PE7"/>
<pin name="PF7"/>
<pin name="PF6"/>
<pin name="PF5"/>
<pin name="PF4"/>
<pin name="PF3"/>
<pin name="PF2"/>
<pin name="PF1"/>
<pin name="PF0"/>
<pin name="PG0"/>
<pin name="PG1"/>
<pin name="PG2"/>
<pin name="PG3"/>
<pin name="PG4"/>
<pin name="PG5"/>
<pin name="AVSS_RFN"/>
<pin name="AVSS_RFP"/>
<pin name="RFP"/>
<pin name="RFN"/>
<pin name="RSTN"/>
<pin name="RSTON"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="AREF"/>
<pin name="TST"/>
<pin name="CLKI"/>
<pin name="DVDD@22"/>
<pin name="DVSS@24"/>
<pin name="DVSS@35"/>
<pin name="DVSS@45"/>
<pin name="DVSS@55"/>
<pin name="DEVDD@34"/>
<pin name="DEVDD@44"/>
<pin name="DEVDD@54"/>
<pin name="AVSS@61"/>
</symbol>
<symbol name="BALUN">
<pin name="IN"/>
<pin name="OUT1"/>
<pin name="GND@5"/>
<pin name="OUT2"/>
<pin name="GND@2"/>
</symbol>
<symbol name="RN41">
<pin name="GND"/>
<pin name="SPIMOSI"/>
<pin name="PIO6"/>
<pin name="PIO7"/>
<pin name="RESET"/>
<pin name="SPICLK"/>
<pin name="PCMCLK"/>
<pin name="PCMSYNC"/>
<pin name="PCMIN"/>
<pin name="PCMOUT"/>
<pin name="VDD"/>
<pin name="GND1"/>
<pin name="UARTRX"/>
<pin name="UARTTX"/>
<pin name="UARTRTS"/>
<pin name="UARTCTS"/>
<pin name="USBD+"/>
<pin name="USBD-"/>
<pin name="PIO2"/>
<pin name="PIO3"/>
<pin name="PIO5"/>
<pin name="PIO4"/>
<pin name="SPICSB"/>
<pin name="SPIMISO"/>
<pin name="PIO9"/>
<pin name="GND2"/>
<pin name="PIO8"/>
<pin name="PIO10"/>
<pin name="PIO11"/>
<pin name="AIO0"/>
<pin name="AIO1"/>
<pin name="GND3"/>
</symbol>
<symbol name="BTM182">
<pin name="VDD"/>
<pin name="VDD_USB"/>
<pin name="USB_DP"/>
<pin name="USB_DN"/>
<pin name="PCM_OUT"/>
<pin name="PCM_CLK"/>
<pin name="PCM_SYNC"/>
<pin name="PCM_IN"/>
<pin name="UART_CTS"/>
<pin name="UART_TX"/>
<pin name="UART_RX"/>
<pin name="UART_RTS"/>
<pin name="SPI_MOSI"/>
<pin name="SPI_CSB"/>
<pin name="SPI_MISO"/>
<pin name="SPI_CLK"/>
<pin name="GND"/>
<pin name="RESET"/>
<pin name="AIO1"/>
<pin name="AIO0"/>
<pin name="PIO11"/>
<pin name="PIO10"/>
<pin name="PIO9"/>
<pin name="PIO8"/>
<pin name="PIO7"/>
<pin name="PIO6"/>
<pin name="PIO5"/>
<pin name="PIO4"/>
<pin name="PIO3"/>
<pin name="PIO2"/>
<pin name="PIO1"/>
<pin name="PIO0"/>
</symbol>
<symbol name="ID-12">
<description>&lt;h3&gt;ID2-LA, ID12-LA and the ID20-LA&lt;/h3&gt;
&lt;p&gt;RFID modules in a small footprint that work at 2.8-5V  and support ASCII, Wiegand26 and Magnetic ABA Track2 data formats. The&lt;/p&gt;</description>
<pin name="GND"/>
<pin name="RES"/>
<pin name="ANT1"/>
<pin name="ANT2"/>
<pin name="CP"/>
<pin name="TINRANGE"/>
<pin name="FS"/>
<pin name="D1"/>
<pin name="DATA"/>
<pin name="LED"/>
<pin name="VCC"/>
</symbol>
<symbol name="NRF24L01-1">
<pin name="VDD@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="CE" direction="in"/>
<pin name="MOSI" direction="in"/>
<pin name="MISO" direction="out"/>
<pin name="SCK" direction="in"/>
<pin name="VSS@20" direction="pwr"/>
<pin name="IRQ" direction="out" function="dot"/>
<pin name="DVDD" direction="pwr"/>
<pin name="XC2" direction="in"/>
<pin name="XC1" direction="in"/>
<pin name="VDD_PA" direction="pwr"/>
<pin name="ANT1" direction="out"/>
<pin name="ANT2" direction="out"/>
<pin name="VDD@15" direction="pwr"/>
<pin name="IREF" direction="in"/>
<pin name="VDD@18" direction="pwr"/>
<pin name="CSN" direction="in"/>
<pin name="VSS@17" direction="pwr"/>
<pin name="VSS@14" direction="pwr"/>
<pin name="VSS@0" direction="pwr"/>
</symbol>
<symbol name="NRF24LE1">
<description>&lt;h3&gt;Nordic nRF24LE1 Ultra-low Power Wireless System on Chip&lt;/h3&gt;
&lt;p&gt;The Nordic Semiconductor nRF24LE1 is a 2.4GHz ISM band radio with emhanced 8051 MCU, up to 2Mbps on air data rate, 1.9 to 3.6V supply range, 16-32-bit multiplication-division co-processor (MDU), 16 kBytes of on-chip Flash, 1 kBytes on SRAM, 1 kBytes NV data memory, 512 Bytes NV data memory (extended endurance), Interrupt controller with 18 sources and 4 priority levels, 1 Analog comparator, 10 Bit ADC, Hardware SPI slave and master, UART, three 16-bit timers/counters, AES encryption/decryption co-processor, Random number generator, 2-Wire interface, 2 Channel PWM, 7, 15, or 31 GPIO lines, On-chip hardware debug support for a JTAG debugger.&lt;/p&gt;</description>
<pin name="P0.1"/>
<pin name="VDD1"/>
<pin name="DEC1"/>
<pin name="DEC2"/>
<pin name="P0.2"/>
<pin name="PROG"/>
<pin name="P0.3"/>
<pin name="VSS1"/>
<pin name="VDD2"/>
<pin name="P0.4"/>
<pin name="P0.5"/>
<pin name="P0.6"/>
<pin name="P0.7"/>
<pin name="P1.0"/>
<pin name="P1.1"/>
<pin name="P1.2"/>
<pin name="P1.3"/>
<pin name="P1.4"/>
<pin name="RESET"/>
<pin name="VDD_PA"/>
<pin name="ANT1"/>
<pin name="ANT2"/>
<pin name="VSS2"/>
<pin name="VDD3"/>
<pin name="IREF"/>
<pin name="VSS3"/>
<pin name="VDD4"/>
<pin name="P1.5"/>
<pin name="P1.6"/>
<pin name="XC2"/>
<pin name="XC1"/>
<pin name="P0.0"/>
</symbol>
<symbol name="NRF24LU1">
<description>&lt;h3&gt;Nordic nRF24LU1+ Single-Chip 2.4GHz Transceiver w/ USB Microcontroller and Flash&lt;/h3&gt;
&lt;p&gt;Nordic’s nRF24LU1+ is a complete system-on-chip wireless transceiver. The nRF24LU1+ features a fully integrated USB 2.0 compliant device controller, which makes this chip a great choice for a compact wireless USB dongle. The nRF24LU1+ is compatible with our nRF24L01+ 2.4GHz RF transceivers as well. Additional features include an 8-bit application microcontroller, 32 kB flash memory, 6 GPIO pins, SPI and UART support, and up to 2Mbps on air data rates.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/products/retired/9525"&gt;2.4GHz Transceiver IC - nRF24LU1+ (COM-09525)&lt;/a&gt;&lt;/p&gt;</description>
<pin name="VDD3"/>
<pin name="P0.0"/>
<pin name="P0.1"/>
<pin name="VSS2"/>
<pin name="P0.2"/>
<pin name="P0.3"/>
<pin name="P0.4"/>
<pin name="P0.5"/>
<pin name="/RESET"/>
<pin name="PROG"/>
<pin name="VSS1"/>
<pin name="D-"/>
<pin name="D+"/>
<pin name="VDD2"/>
<pin name="VBUS"/>
<pin name="VDD1"/>
<pin name="XC1"/>
<pin name="XC2"/>
<pin name="VSS7"/>
<pin name="DEC2"/>
<pin name="DEC1"/>
<pin name="VDD6"/>
<pin name="VSS6"/>
<pin name="IREF"/>
<pin name="VDD5"/>
<pin name="VSS5"/>
<pin name="ANT2"/>
<pin name="ANT1"/>
<pin name="VDD_PA"/>
<pin name="VDD4"/>
<pin name="VSS4"/>
<pin name="VSS3"/>
</symbol>
<symbol name="RF-LINK_RX">
<description>&lt;h3&gt;RF Link Receiver (434 MHz, 315 MHz)&lt;/h3&gt;
&lt;p&gt;These wireless receivers work with equivalent transmitters. They can easily fit into a breadboard and work well with microcontrollers to create a very simple wireless data link. Since these are only receivers, they will only work communicating data one-way, you would need two pairs (of different frequencies) to act as a transmitter/receiver pair..&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/products/10532"&gt;RF Link Receiver - 4800bps (434 MHz) (WRL-10532)&lt;/a&gt;&lt;/p&gt;</description>
<pin name="GND" direction="pwr"/>
<pin name="ANT" direction="pas"/>
<pin name="+5V" direction="pwr"/>
<pin name="DATA" direction="in"/>
</symbol>
<symbol name="RF-LINK_TX">
<description>&lt;h3&gt;RF Link Transmitter (434 MHz, 315 MHz)&lt;/h3&gt;
&lt;p&gt;These wireless transmitters work with equivalent receivers. They can easily fit into a breadboard and work well with microcontrollers to create a very simple wireless data link. Since these are only transmitters, they will only work communicating data one-way, you would need two pairs (of different frequencies) to act as a transmitter/receiver pair.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/products/10534"&gt;RF Link Transmitter - 434MHz (WRL-10534)&lt;/a&gt;&lt;/p&gt;</description>
<pin name="GND" direction="pwr"/>
<pin name="DATA" direction="in"/>
<pin name="ANT" direction="pas"/>
<pin name="+5V" direction="pwr"/>
</symbol>
<symbol name="RFM22">
<description>&lt;h3&gt;Hope RF RFM22 ISM Transciever Module&lt;/h3&gt;

&lt;p&gt;The RFM22 is a low-power, low cost radio that is capable of operating in the 434MHz and 900MHz open bands. It's frequency is software defined and there are some very good libraries written for it.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/products/11018"&gt;SparkFun RFM22 Shield - 434MHz (DEV-11018)&lt;/a&gt;&lt;/p&gt;</description>
<pin name="ANT"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GPIO0"/>
<pin name="GPIO1"/>
<pin name="GPIO2"/>
<pin name="NIRQ" direction="out"/>
<pin name="NSEL" direction="in"/>
<pin name="RXANT" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="SDI" direction="in"/>
<pin name="SDN" direction="in"/>
<pin name="SDO" direction="out"/>
<pin name="TXANT" direction="in"/>
<pin name="VCC"/>
</symbol>
<symbol name="RMCM01">
<description>&lt;h3&gt;Polar RMCM01 Heart Rate Monitor Receiver&lt;/h3&gt; 
&lt;p&gt;The Polar heart rate receiver component receiver
wirelessly receives the heart rate signal from Polar
transmitter belt. The complete heart rate measurement
system consists of three different parts; transmitter,
receiver and electronics and/or display device that is
outputting the heart rate value.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/products/8661"&gt;Polar Heart Rate Monitor Interface (SEN-08661)&lt;/a&gt;&lt;/p&gt;</description>
<pin name="FPLS"/>
<pin name="HR"/>
<pin name="OSC"/>
<pin name="F32KIN"/>
<pin name="OSC_ON"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="LX1"/>
<pin name="LX2"/>
<pin name="WIDB_DET"/>
<pin name="RESET"/>
</symbol>
<symbol name="RN171">
<description>&lt;h3&gt;Roving Networks RN-171 802.11b/g WiFi Serial Module&lt;/h3&gt; 
&lt;p&gt;The RN-171 is a small form factor, ultra-low power embedded TCP/IP module. The RN-171 is a standalone, complete TCP/IP wireless networking module. Due to its small form factor and extremely low power consumption, it is perfect for mobile wireless applications such as asset monitoring, sensors, and portable battery operated devices.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/products/retired/11049"&gt;WiFly RN-171 802.11b/g Serial Module (WRL-11049)&lt;/a&gt;&lt;/p&gt;</description>
<pin name="GND@1"/>
<pin name="CLK"/>
<pin name="CS"/>
<pin name="GPIO7"/>
<pin name="INT/GPIO6"/>
<pin name="MISO"/>
<pin name="MOSI"/>
<pin name="VDD"/>
<pin name="GPIO3"/>
<pin name="GPIO2"/>
<pin name="GPIO1"/>
<pin name="GND@14"/>
<pin name="GND@20"/>
<pin name="GND@21"/>
<pin name="GND@22"/>
<pin name="GND@23"/>
<pin name="ANT"/>
<pin name="GND@25"/>
<pin name="GND@26"/>
<pin name="GND@27"/>
<pin name="GND@28"/>
<pin name="SEN0"/>
<pin name="SEN1"/>
<pin name="SEN2"/>
<pin name="SEN3"/>
<pin name="SPOWER"/>
<pin name="VDD_RF"/>
<pin name="SEN4"/>
<pin name="SEN5"/>
<pin name="SEN6"/>
<pin name="SEN7"/>
<pin name="GND@39"/>
<pin name="RESET"/>
<pin name="AWAKE"/>
<pin name="GPIO14"/>
<pin name="RTS"/>
<pin name="CTS"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="GND@47"/>
<pin name="SREG"/>
<pin name="VDD_BATT"/>
</symbol>
<symbol name="SI470X">
<description>&lt;h3&gt;Silicon Labs Si4703 FM Tuner&lt;/h3&gt;
&lt;p&gt;Beyond enabling you to tune in to FM radio stations, the Si4703 is also capable of detecting and processing both Radio Data Service (RDS) and Radio Broadcast Data Service (RBDS) information. The Si4703 even does a very good job of filtering and carrier detection. It also enables data such as the station ID and song name to be displayed to the user.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/products/12938"&gt;SparkFun FM Tuner Evaluation Board - Si4703 (WRL-12938)&lt;/a&gt;&lt;/p&gt;</description>
<pin name="!RST"/>
<pin name="!SEN"/>
<pin name="DOUT"/>
<pin name="FMIP"/>
<pin name="GND@12"/>
<pin name="GND@PAD"/>
<pin name="GPIO1"/>
<pin name="GPIO2"/>
<pin name="GPIO3"/>
<pin name="LOUT"/>
<pin name="LPI"/>
<pin name="RCLK"/>
<pin name="RFGND"/>
<pin name="ROUT"/>
<pin name="SCLK"/>
<pin name="SDIO"/>
<pin name="VA"/>
<pin name="VD"/>
<pin name="VIO"/>
</symbol>
<symbol name="SM130">
<description>&lt;h3&gt;SonMicro SMB130 - 13.56 MHz RFID Mifare Read/Write Module&lt;/h3&gt;
&lt;p&gt;The SMB130 is a 28 pin DIP module that includes all necessary components for a 13.56 MHz RFID MIFARE®, aside from a PCB antenna.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/products/10126"&gt;SparkFun Product Link&lt;/a&gt;&lt;/p&gt;</description>
<pin name="VCC"/>
<pin name="RFVCC"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="OK"/>
<pin name="ERROR"/>
<pin name="RESET"/>
<pin name="I1"/>
<pin name="I2"/>
<pin name="GND"/>
<pin name="RFGND@23"/>
<pin name="RFGND@25"/>
<pin name="RFGND@27"/>
<pin name="ANT2"/>
<pin name="ANT1"/>
<pin name="O2"/>
<pin name="O1"/>
<pin name="RX-I"/>
<pin name="TX-O"/>
</symbol>
<symbol name="SM5100B">
<description>&lt;h3&gt;LinkSprite SM5100B GSM/GPRS Module&lt;/h3&gt;
&lt;p&gt;The SM5100B is a miniature, quad-band GSM 850/EGSM 900/DCS 1800/PCS 1900 module, which can be integrated into a great number of wireless projects. You can use this module to accomplish almost anything a normal cell phone can - SMS text messages, GSM/GPRS, TCP/IP, and more!&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/products/9533"&gt;SparkFun Product Link&lt;/a&gt;&lt;/p&gt;</description>
<pin name="VBAT@0"/>
<pin name="VCHG@0"/>
<pin name="VBAT@1"/>
<pin name="VCHG@1"/>
<pin name="VBAT@2"/>
<pin name="ADIN1"/>
<pin name="VBAT@3"/>
<pin name="ADIN2"/>
<pin name="GND@0"/>
<pin name="GPIO_19"/>
<pin name="GND@1"/>
<pin name="EAR_MICN"/>
<pin name="GND@2"/>
<pin name="EAR_MICP"/>
<pin name="GND@3"/>
<pin name="EAR_SPKN"/>
<pin name="GND@4"/>
<pin name="EAR_SPKP"/>
<pin name="TXD0"/>
<pin name="RXD0"/>
<pin name="SIM_RST"/>
<pin name="GPIO_17"/>
<pin name="KEY_DRV3"/>
<pin name="KEY_DRV0"/>
<pin name="KEY_DRV4"/>
<pin name="KEY_DRV2"/>
<pin name="SIM_CLK"/>
<pin name="KEY_DRV1"/>
<pin name="SIM_DA"/>
<pin name="KEY_DRV5"/>
<pin name="KEY_SEN2"/>
<pin name="KEY_SEN1"/>
<pin name="GPO42/NBOOT"/>
<pin name="RESET"/>
<pin name="GPIO_4"/>
<pin name="KEY_SEN0"/>
<pin name="GPIO_10"/>
<pin name="GPIO_6"/>
<pin name="GPIO_1"/>
<pin name="KEY_SEN3"/>
<pin name="GPIO_9"/>
<pin name="AUX_MICP"/>
<pin name="RXD1"/>
<pin name="AUX_SPKP"/>
<pin name="GPIO_18"/>
<pin name="TXD1"/>
<pin name="VCC@0"/>
<pin name="RTC_BATT"/>
<pin name="GPIO_26"/>
<pin name="AUX_MICN"/>
<pin name="SIM_VCC"/>
<pin name="GPIO_16"/>
<pin name="GPO_11"/>
<pin name="GPIO_8"/>
<pin name="GPIO_3"/>
<pin name="GPIO_20"/>
<pin name="GPIO_46"/>
<pin name="AUX_SPKN"/>
<pin name="POWER_ON"/>
<pin name="VCC@1"/>
</symbol>
<symbol name="WIFLY_GSX">
<description>&lt;h3&gt;Roving Networks WiFly GSX (RN-131C) Wi-Fi Module&lt;/h3&gt;
&lt;p&gt;The WiFly GSX (RN-131C) module is a complete ultra low power embedded TCP/IP solution. The WiFly GSX module is a stand alone, embedded wireless 802.11b/g networking module.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/products/10004"&gt;SparkFun Product Link&lt;/a&gt;&lt;/p&gt;</description>
<pin name="EPCB"/>
<pin name="EPCA"/>
<pin name="FORCE_WAKE"/>
<pin name="RESET_L"/>
<pin name="SPI_MOSI"/>
<pin name="SPI_CLK"/>
<pin name="SPI_MISO"/>
<pin name="GPIO9"/>
<pin name="GPIO8"/>
<pin name="GPIO7"/>
<pin name="GPIO6"/>
<pin name="GPIO5"/>
<pin name="GPIO4"/>
<pin name="GPIO_13"/>
<pin name="GPIO_12"/>
<pin name="URX"/>
<pin name="UTX"/>
<pin name="VD_BAT"/>
<pin name="VD_3V_IN"/>
<pin name="SENS0"/>
<pin name="SENS1"/>
<pin name="SENS2"/>
<pin name="SENS3"/>
<pin name="SENS4"/>
<pin name="SENS5"/>
<pin name="SENS6"/>
<pin name="SENS7"/>
<pin name="SENSPWR"/>
<pin name="DMA_RX"/>
<pin name="DMA_TX"/>
<pin name="SUPCAP"/>
<pin name="3V3_OUT"/>
<pin name="3V3_IN"/>
<pin name="G9"/>
<pin name="G8"/>
<pin name="G7"/>
<pin name="G6"/>
<pin name="G5"/>
<pin name="G4"/>
<pin name="G3"/>
<pin name="G2"/>
<pin name="G1"/>
<pin name="G10"/>
<pin name="NC"/>
</symbol>
<symbol name="XTEND-DIGI-MODEM">
<description>&lt;h3&gt;Digi XTend 900 1W RF Transceiver&lt;/h3&gt;
&lt;p&gt;The XTend Modem packs a ton of RF punch into a small, low-power, easy-to-use, and reliable module. Outdoors, with line-of-sight, this module can communicate at up to 40 miles; indoors it can still do up to 3000ft. The module transfers a standard asynchronous serial data stream, operates within the ISM 900MHz frequency band and sustains up to 115.2kbps data throughput. The module comes with an attached RPSMA antenna connector.&lt;/p&gt;</description>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="GPO2"/>
<pin name="TX_PWR"/>
<pin name="DI"/>
<pin name="DO"/>
<pin name="SHDN"/>
<pin name="SLEEP"/>
<pin name="CTS"/>
<pin name="RTS"/>
<pin name="CONFIG"/>
</symbol>
<symbol name="BLUERADIO_BR-LE4.0-S2">
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="VCC(2.0-3.6V)" direction="pwr"/>
<pin name="SPI_CSB"/>
<pin name="SPI_CLK"/>
<pin name="SPI_MOSI"/>
<pin name="SPI_MISO"/>
<pin name="PIO_2"/>
<pin name="PIO_3/INT"/>
<pin name="PIO_4"/>
<pin name="PIO_5"/>
<pin name="PIO_6"/>
<pin name="PIO_7"/>
<pin name="USB_VBUS"/>
<pin name="USB_GND"/>
<pin name="USB_DP"/>
<pin name="USB_DM"/>
<pin name="UART_RX" direction="in"/>
<pin name="UART_TX" direction="out"/>
<pin name="UART_RTS" direction="out" function="dot"/>
<pin name="UART_CTS" direction="in" function="dot"/>
<pin name="RESET" direction="in"/>
<pin name="PIO_9"/>
<pin name="PIO_14"/>
<pin name="ADC_0" direction="in"/>
<pin name="ADC_1" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="PIO_8"/>
</symbol>
<symbol name="ELECTRIC_IMP">
<description>&lt;h3&gt;Electric Imp&lt;/h3&gt;

A wi-fi enabled microcontroller, in an SD card package.</description>
<pin name="1(CLK2/CTS1/TX3/SCL2)"/>
<pin name="2(MISO1/MOSI2/RTS1/RX3/SDA2)"/>
<pin name="5(SCLK1/SCLK2/TX2)"/>
<pin name="7(MOSI1/MISO2/RX2)"/>
<pin name="8(MOSI2/TX1/SCL1)"/>
<pin name="9(MISO2/RX1/SDA1)"/>
<pin name="CD"/>
<pin name="WP"/>
<pin name="VDD"/>
<pin name="ID"/>
<pin name="GND"/>
<pin name="S1"/>
<pin name="S2"/>
</symbol>
<symbol name="BC127_GPIO">
<pin name="PIO_0"/>
<pin name="PIO_1"/>
<pin name="PIO_2"/>
<pin name="PIO_3"/>
<pin name="PIO_4"/>
<pin name="PIO_5"/>
<pin name="PIO_6"/>
<pin name="PIO_7"/>
<pin name="AIO_1"/>
<pin name="CAP_SENSE_1"/>
<pin name="CAP_SENSE_2"/>
<pin name="CAP_SENSE_3"/>
<pin name="CAP_SENSE_4"/>
<pin name="LED_0"/>
<pin name="LED_1"/>
<pin name="LED_2"/>
</symbol>
<symbol name="BC127_POWER">
<pin name="GND"/>
<pin name="VDD_PADS"/>
<pin name="VBAT"/>
<pin name="VBAT_SENSE"/>
<pin name="VCHG"/>
<pin name="CHG_EXT"/>
<pin name="VREGEN"/>
<pin name="3V3_USB"/>
<pin name="!RESET"/>
</symbol>
<symbol name="BC127_DATA_PORTS">
<pin name="USB_N"/>
<pin name="USB_P"/>
<pin name="UART_TX"/>
<pin name="UART_RX"/>
<pin name="UART_CTS"/>
<pin name="UART_RTS"/>
<pin name="SPI_!PCM"/>
<pin name="PCM_OUT/MISO"/>
<pin name="PCM_IN/MOSI"/>
<pin name="PCM_SYNC/CSB"/>
<pin name="PCM_CLK/CLK"/>
</symbol>
<symbol name="BC127_ANALOG_AUDIO">
<pin name="SPKR_LN"/>
<pin name="SPKR_LP"/>
<pin name="SPKR_RN"/>
<pin name="SPKR_RP"/>
<pin name="MIC_BIAS_A"/>
<pin name="MIC_RN"/>
<pin name="MIC_RP"/>
<pin name="MIC_LN"/>
<pin name="MIC_LP"/>
</symbol>
<symbol name="RN-52">
<pin name="AGND"/>
<pin name="AIC0"/>
<pin name="GND"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="GND3"/>
<pin name="GND4"/>
<pin name="GND5"/>
<pin name="GND6"/>
<pin name="GND7"/>
<pin name="GND8"/>
<pin name="GND9"/>
<pin name="GPIO2"/>
<pin name="GPIO3"/>
<pin name="GPIO4"/>
<pin name="GPIO5"/>
<pin name="GPIO6"/>
<pin name="GPIO7"/>
<pin name="GPIO9"/>
<pin name="GPIO10"/>
<pin name="GPIO11"/>
<pin name="GPIO12"/>
<pin name="GPIO13"/>
<pin name="LED0"/>
<pin name="LED1"/>
<pin name="MIC_BIAS"/>
<pin name="MIC_L+"/>
<pin name="MIC_L-"/>
<pin name="MIC_R+"/>
<pin name="MIC_R-"/>
<pin name="PCM_CLK"/>
<pin name="PCM_IN"/>
<pin name="PCM_OUT"/>
<pin name="PCM_SYNC"/>
<pin name="PWREN"/>
<pin name="SPI_CLK"/>
<pin name="SPI_MISO"/>
<pin name="SPI_MOSI"/>
<pin name="SPI_SS"/>
<pin name="SPKR_L+"/>
<pin name="SPKR_L-"/>
<pin name="SPKR_R+"/>
<pin name="SPKR_R-"/>
<pin name="UART_CTS"/>
<pin name="UART_RTS"/>
<pin name="UART_RX"/>
<pin name="UART_TX"/>
<pin name="USBD+"/>
<pin name="USBD-"/>
<pin name="VDD"/>
</symbol>
<symbol name="CC3000">
<pin name="GND@1"/>
<pin name="RESERVED_1"/>
<pin name="NC"/>
<pin name="RESERVED_2"/>
<pin name="WL_EN2"/>
<pin name="WL_RS232_TX"/>
<pin name="WL_EN1"/>
<pin name="WL_RS232_RX"/>
<pin name="GND@9"/>
<pin name="GND@10"/>
<pin name="GND@11"/>
<pin name="SPI_CS"/>
<pin name="SPI_DOUT"/>
<pin name="SPI_IRQ"/>
<pin name="SPI_DIN"/>
<pin name="GND@16"/>
<pin name="SPI_CLK"/>
<pin name="GND@18"/>
<pin name="VBAT_IN"/>
<pin name="GND@20"/>
<pin name="EXT_32K"/>
<pin name="GND@22"/>
<pin name="VIO_HOST"/>
<pin name="RESERVED_3"/>
<pin name="GND@25"/>
<pin name="VBAT_SW_EN"/>
<pin name="SDA_EEPROM"/>
<pin name="SDA_CC3000"/>
<pin name="SCL_EEPROM"/>
<pin name="SCL_CC3000"/>
<pin name="GND@31"/>
<pin name="GND@32"/>
<pin name="GND@33"/>
<pin name="GND@34"/>
<pin name="RF_ANT"/>
<pin name="GND@36"/>
<pin name="GND@37"/>
<pin name="GND@38"/>
<pin name="GND@39"/>
<pin name="GND@40"/>
<pin name="GND@41"/>
<pin name="GND@42"/>
<pin name="GND@43"/>
<pin name="GND@44"/>
<pin name="GND@45"/>
<pin name="GND@46"/>
</symbol>
<symbol name="RFM69H">
<description>&lt;h3&gt;Hope RF RFM69H ISM Transceiver Module&lt;/h3&gt; 
&lt;p&gt;The RFM69H is a transceiver module capable of operation 
over a wide frequency range, including the 
315,433,868 and 
915MHz license-free ISM (Industry Scientific and Medical) 
frequency bands. All major RF communication parameters 
are programmable and most of them  can  be  dynamically 
set.  The  RFM69H  offers  the unique advantage of 
programmable narrow-band and wide- band  communication 
modes. The RFM69H is optimized for low power 
consumption while offering high RF output power and 
channelized operation.
Compliance  ETSI and FCC 
regulations. &lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.hoperf.cn/upload/docs/RF/SX/RFM69H_DataSheet_v1.3.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
<pin name="RST" direction="in"/>
<pin name="IO0/INT"/>
<pin name="IO1"/>
<pin name="IO2"/>
<pin name="IO3"/>
<pin name="IO4"/>
<pin name="IO5"/>
<pin name="VCC" direction="pwr"/>
<pin name="ANT" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="SCK" direction="in"/>
<pin name="MISO"/>
<pin name="MOSI" direction="in"/>
<pin name="!CS" direction="in"/>
</symbol>
<symbol name="RFM69">
<description>&lt;h3&gt;Hope RF RFM69CW ISM Transceiver Module&lt;/h3&gt; 
&lt;p&gt;The RFM69CW radio module by HopeRF is a compact, powerful radio transceiver module for swapping data packets in the 868 MHz ISM band, using standard and enhanced FSK modulation. The radio is great for sub-compact designs; just 4mm of mounted height from using an SMD precision crystal.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.hoperf.com/upload/rf/RFM69CW-V1.1.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
<pin name="RESET" direction="in"/>
<pin name="DIO0"/>
<pin name="DIO1"/>
<pin name="DIO2"/>
<pin name="DIO3"/>
<pin name="DIO5"/>
<pin name="3.3V" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="ANT" direction="pas"/>
<pin name="GND@2" direction="pwr"/>
<pin name="SCK" direction="in"/>
<pin name="MISO"/>
<pin name="MOSI" direction="in"/>
<pin name="NSS" direction="in"/>
</symbol>
<symbol name="BC118_POWER">
<pin name="GND"/>
<pin name="VDD"/>
<pin name="VBAT"/>
<pin name="WAKE"/>
</symbol>
<symbol name="BC118_PIO">
<pin name="AIO_0"/>
<pin name="AIO_1"/>
<pin name="AIO_2"/>
<pin name="PIO_3"/>
<pin name="PIO_4"/>
<pin name="PIO_5/SPI_CLK"/>
<pin name="PIO_6/SPI_CSB"/>
<pin name="PIO_7/SPI_MOSI"/>
<pin name="PIO_8/SPI_MISO"/>
<pin name="SPI/!PCM"/>
<pin name="PIO_2"/>
<pin name="PIO_9"/>
<pin name="PIO_10"/>
<pin name="PIO_11"/>
</symbol>
<symbol name="BC118_COMMS">
<pin name="I2C_SDA"/>
<pin name="I2C_SCL"/>
<pin name="UART_RX"/>
<pin name="UART_TX"/>
</symbol>
<symbol name="XBEE">
<description>&lt;h3&gt;Digi XBee and XBee Pro&lt;/h3&gt;
&lt;p&gt;XBees are tiny blue chips that can communicate wirelessly with each other. They can do simple things, like replacing a couple of wires in serial communication, which is nice when you want to make a remote for your paintball vehicle.&lt;/p&gt;</description>
<pin name="CTS" direction="out" function="dot"/>
<pin name="DIN" direction="in"/>
<pin name="DIO0"/>
<pin name="DIO1"/>
<pin name="DIO2"/>
<pin name="DIO3"/>
<pin name="DIO4"/>
<pin name="DIO5"/>
<pin name="DIO9"/>
<pin name="DIO11"/>
<pin name="DIO12"/>
<pin name="DOUT" direction="out"/>
<pin name="DTR" function="dot"/>
<pin name="GND" direction="pwr"/>
<pin name="RES@8"/>
<pin name="RES@14"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="RSSI"/>
<pin name="RTS" direction="in" function="dot"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="ESP8266">
<description>&lt;h3&gt;ESP8266 WiFi Smart Module&lt;/h3&gt;</description>
<pin name="VDDA@1"/>
<pin name="LNA"/>
<pin name="VDD3P3@3"/>
<pin name="VDD3P3@4"/>
<pin name="VDD_RTC"/>
<pin name="TOUT/ADC"/>
<pin name="CHIP_EN"/>
<pin name="XPD_DCDC/GPIO16"/>
<pin name="MTMS/SPICLK/GPIO14"/>
<pin name="MTDI/SPIQ/GPIO12"/>
<pin name="VDDPST@11"/>
<pin name="MTCK/SPID/GPIO13"/>
<pin name="MTDO/SPICS/GPIO15"/>
<pin name="GPIO2"/>
<pin name="SPICS2/GPIO0"/>
<pin name="GPIO4"/>
<pin name="VDDPST@17"/>
<pin name="SPIHD/SD_DATA_2"/>
<pin name="SPIWP/SD_DATA_3"/>
<pin name="SPICS0/SD_CMD"/>
<pin name="SPICLK/SD_CLK"/>
<pin name="SPIQ/SD_DATA_0"/>
<pin name="SPID/SD_DATA_1"/>
<pin name="GPIO5"/>
<pin name="U0RXD"/>
<pin name="U0TXD"/>
<pin name="XTAL_OUT"/>
<pin name="XTAL_IN"/>
<pin name="VDDD"/>
<pin name="VDDA@30"/>
<pin name="RES12K"/>
<pin name="EXT_RSTB"/>
<pin name="GND"/>
</symbol>
<symbol name="ESP32">
<pin name="SENSOR_CAPP(GPI37/ADC1:1/RTC1)"/>
<pin name="SENSOR_VP(GPI36/ADC1:0/RTC0)"/>
<pin name="VDDA3P3"/>
<pin name="LNA_IN"/>
<pin name="SENSOR_CAPN(GPI38/ADC1:2/RTC2)"/>
<pin name="SENSOR_VN(GPI39/ADC1:3/RTC3)"/>
<pin name="CHIP_PU"/>
<pin name="VDET_1(GPI34/ADC1:6)"/>
<pin name="VDET_2(GPI35/ADC1:7)"/>
<pin name="32K_XP(GPIO32/ADC1:4/TOUCH9/RTC9)"/>
<pin name="32K_XN(GPIO33/ADC1:5/TOUCH8/RTC8)"/>
<pin name="(DAC2/ADC2:9/RTC7)GPIO26"/>
<pin name="(DAC1/ADC2:8/RTC6)GPIO25"/>
<pin name="(ADC2:7/TOUCH7/RTC17)GPIO27"/>
<pin name="(GPIO14/ADC2:6/TOUCH6/RTC16/SPICLK)MTMS"/>
<pin name="(GPIO12/ADC2:5/TOUCH5/RTC15/SPIQ)MTDI"/>
<pin name="VDD3P3_RTC"/>
<pin name="(GPIO13/ADC2:4/TOUCH4/RTC14/SPID/U0CTS)MTCK"/>
<pin name="(GPIO15/ADC2:3/TOUCH3/RTC13/SPICSO/U0RTS)MTDO"/>
<pin name="(ADC2:2/TOUCH2/RTC12/SPIWP)GPIO2"/>
<pin name="(ADC2:1/TOUCH1/RTC11/CLK_OUT1)GPIO0"/>
<pin name="(ADC2:0/TOUCH0/RTC10/SPIHD)GPIO4"/>
<pin name="VDD3P3_SDIO"/>
<pin name="(HS1_DATA4)GPIO16"/>
<pin name="(HS1_DATA5)GPIO17"/>
<pin name="(GPIO9/SPIHD/HS1_DATA2/U1RX)SD_DATA2"/>
<pin name="(GPIO10/SPIWP/HS1_DATA3/U1TX)SD_DATA3"/>
<pin name="(GPIO11/SPICSO/HS1_CMD/U1RTS)SD_CMD"/>
<pin name="(GPIO6/SPICLK/HS1_CLK/U1CTS)SD_CLK"/>
<pin name="(GPIO7/SPI1/HS1_DATA0)SD_DATA0"/>
<pin name="(GPIO8/SPID/HS1_DATA1)SD_DATA1"/>
<pin name="(VSPICS0/HS1_DATA6)GPIO5"/>
<pin name="(VSPICLK/HS1_DATA7)GPIO18"/>
<pin name="(GPIO1/CLK_OUT3/HS2_DATA1)U0TXD"/>
<pin name="(GPIO3/CLK_OUT2/HS2_DATA0)U0RXD"/>
<pin name="GPIO23"/>
<pin name="(VSPIWP/HS2_CLK)GPIO22"/>
<pin name="(VSPIQ/HS2_DATA2)GPIO19"/>
<pin name="VDD3P3_CPU"/>
<pin name="XTAL_N"/>
<pin name="XTAL_P"/>
<pin name="VDDA"/>
<pin name="CAP2"/>
<pin name="CAP1"/>
<pin name="GND"/>
<pin name="(VSPIHD/HS2_CMD)GPIO21"/>
</symbol>
<symbol name="NRF52832">
<description>&lt;h3&gt;Nordic nRF52832 Bluetooth Smart/ANT/2.4GHz RF SoC&lt;/h3&gt;
&lt;p&gt;The nRF52832 SoC is a powerful, highly flexible ultra-low power multiprotocol SoC ideally suited for Bluetooth® Smart ANT and 2.4GHz ultra low-power wireless applications. The nRF52832 SoC is built around a 32-bit ARM® Cortex™-M4F CPU with 512kB + 64kB RAM. The embedded 2.4GHz transceiver supports Bluetooth Smart, ANT and proprietary 2.4 GHz protocol stack. It is on air compatible with the nRF51 Series, nRF24L and nRF24AP Series products from Nordic Semiconductor.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.nordicsemi.com/eng/Products/Bluetooth-low-energy2/nRF52832"&gt;Product Page&lt;/a&gt;&lt;/p&gt;</description>
<pin name="DEC1"/>
<pin name="P0.00/XL1"/>
<pin name="P0.01/XL2"/>
<pin name="P0.02/AIN0"/>
<pin name="P0.03/AIN1"/>
<pin name="P0.04/AIN2"/>
<pin name="P0.05/AIN3"/>
<pin name="P0.06"/>
<pin name="P0.07"/>
<pin name="P0.08"/>
<pin name="P0.09/NFC1"/>
<pin name="VDD"/>
<pin name="P0.10/NFC2"/>
<pin name="P0.11"/>
<pin name="P0.12"/>
<pin name="P0.13"/>
<pin name="P0.14"/>
<pin name="P0.15"/>
<pin name="P0.16"/>
<pin name="P0.17"/>
<pin name="P0.18"/>
<pin name="P0.19"/>
<pin name="P0.20"/>
<pin name="P0.21/RESET"/>
<pin name="SWDCLK"/>
<pin name="SWDIO"/>
<pin name="P0.22"/>
<pin name="P0.23"/>
<pin name="P0.24"/>
<pin name="ANT"/>
<pin name="VSS"/>
<pin name="DEC2"/>
<pin name="DEC3"/>
<pin name="XC1(32MHZ)"/>
<pin name="XC2(32MHZ)"/>
<pin name="P0.25"/>
<pin name="P0.26"/>
<pin name="P0.27"/>
<pin name="P0.29/AIN5"/>
<pin name="P0.28/AIN4"/>
<pin name="P0.30/AIN6"/>
<pin name="P0.31/AIN7"/>
<pin name="DEC4"/>
<pin name="DCC"/>
<pin name="NC"/>
</symbol>
<symbol name="RFD77101">
<description>&lt;p&gt;&lt;strong&gt;Simblee  BLE Module RFD77101&lt;/strong&gt;&lt;/p&gt;
&lt;p&gt;© 2015 RF Digital Corporation&lt;br/&gt; 
&lt;a href="http://www.RFDigital.com"&gt;www.RFDigital.com&lt;/a&gt;&lt;br/&gt;
&lt;a href="http://www.Simblee.com"&gt;www.Simblee.com&lt;/a&gt;&lt;br/&gt;
PATENTS PENDING 04.01.2015&lt;br/&gt;&lt;/p&gt;</description>
<pin name="!RESET!" direction="in"/>
<pin name="DNC@3" direction="nc"/>
<pin name="DNC@5" direction="nc"/>
<pin name="DNC@10" direction="nc"/>
<pin name="FACTORY" direction="nc"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@19" direction="pwr"/>
<pin name="GND@30" direction="pwr"/>
<pin name="GND@42" direction="pwr"/>
<pin name="GND@43" direction="pwr"/>
<pin name="GND@44" direction="pwr"/>
<pin name="GND@45" direction="pwr"/>
<pin name="P0.00/AREF0"/>
<pin name="P0.01/AIN2"/>
<pin name="P0.02/AIN3"/>
<pin name="P0.03/AIN4"/>
<pin name="P0.04/AIN5"/>
<pin name="P0.05/AIN6"/>
<pin name="P0.06/AREF1/AIN7"/>
<pin name="P0.07"/>
<pin name="P0.08"/>
<pin name="P0.09"/>
<pin name="P0.10"/>
<pin name="P0.11"/>
<pin name="P0.12"/>
<pin name="P0.13"/>
<pin name="P0.14"/>
<pin name="P0.15"/>
<pin name="P0.16"/>
<pin name="P0.17"/>
<pin name="P0.18"/>
<pin name="P0.19"/>
<pin name="P0.20"/>
<pin name="P0.21"/>
<pin name="P0.22"/>
<pin name="P0.23"/>
<pin name="P0.24"/>
<pin name="P0.25"/>
<pin name="P0.28"/>
<pin name="P0.29"/>
<pin name="P0.30"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="ESP07-16PIN">
<pin name="ADC"/>
<pin name="CH_PD"/>
<pin name="GND"/>
<pin name="GPIO0"/>
<pin name="GPIO2"/>
<pin name="GPIO4"/>
<pin name="GPIO5"/>
<pin name="GPIO12"/>
<pin name="GPIO13"/>
<pin name="GPIO14"/>
<pin name="GPIO15"/>
<pin name="GPIO16"/>
<pin name="RESET"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="VCC"/>
</symbol>
<symbol name="ESP-WROOM-32">
<pin name="GND@1"/>
<pin name="3V3"/>
<pin name="EN"/>
<pin name="SENSOR_VP/I36"/>
<pin name="SENSOR_VN/I39"/>
<pin name="IO34"/>
<pin name="IO35"/>
<pin name="XTAL_P/IO32"/>
<pin name="XTAL_N/IO33"/>
<pin name="IO25"/>
<pin name="IO26"/>
<pin name="IO27"/>
<pin name="SCK_H/IO14"/>
<pin name="MISO_H/IO12"/>
<pin name="GND@15"/>
<pin name="MOSI_H/IO13"/>
<pin name="SHD/IO9"/>
<pin name="SWP/IO10"/>
<pin name="SCS/IO11"/>
<pin name="GND@38"/>
<pin name="MOSI_V/IO23"/>
<pin name="IO22"/>
<pin name="TXD"/>
<pin name="RXD"/>
<pin name="IO21"/>
<pin name="NC"/>
<pin name="MISO_V/IO19"/>
<pin name="SCK_V/IO18"/>
<pin name="CS0_V/IO5"/>
<pin name="IO17"/>
<pin name="IO16"/>
<pin name="IO4"/>
<pin name="IO0"/>
<pin name="IO2"/>
<pin name="CS0_H/IO15"/>
<pin name="SDI/IO8"/>
<pin name="SDO/IO7"/>
<pin name="SCK/IO6"/>
<pin name="GND"/>
</symbol>
<symbol name="RFM95W">
<description>&lt;h3&gt;RFM95/96/97/98&lt;/h3&gt;

&lt;p&gt;The RFM95/96/97/98(W) transceivers feature the
LoRaTM    long range modem that provides ultra-long range
spread spectrum communication and high interference
immunity whilst minimising current consumption. &lt;/p&gt;

&lt;p&gt;&lt;a href="http://www.hoperf.com/upload/rf/RFM95_96_97_98W.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
<pin name="!RESET"/>
<pin name="3.3V"/>
<pin name="ANT"/>
<pin name="DIO0"/>
<pin name="DIO1"/>
<pin name="DIO2"/>
<pin name="DIO3"/>
<pin name="DIO4"/>
<pin name="DIO5"/>
<pin name="GND"/>
<pin name="MISO"/>
<pin name="MOSI"/>
<pin name="NSS"/>
<pin name="SCK"/>
</symbol>
<symbol name="ROCKBLOCK_9603">
<pin name="GND"/>
<pin name="LI-ION"/>
<pin name="5V"/>
<pin name="ON/!OFF!"/>
<pin name="!RI!"/>
<pin name="NETAV"/>
<pin name="RTS" direction="in"/>
<pin name="CTS" direction="out"/>
<pin name="TX-I"/>
<pin name="RX-O" direction="out"/>
</symbol>
<symbol name="ESP-12S">
<pin name="RST"/>
<pin name="ADC"/>
<pin name="EN"/>
<pin name="IO16"/>
<pin name="IO14"/>
<pin name="IO12"/>
<pin name="IO13"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="IO15"/>
<pin name="IO2"/>
<pin name="IO0"/>
<pin name="IO4"/>
<pin name="IO5"/>
<pin name="RXD0"/>
<pin name="TXD0"/>
</symbol>
<symbol name="ESP8266_ESP-01">
<description>&lt;h3&gt;ESP8266 ESP-01 Module&lt;/h3&gt;
ESP8266 WiFi module pre-programmed with an AT command interface.</description>
<pin name="GND"/>
<pin name="GPIO2"/>
<pin name="GPIO0"/>
<pin name="RXD"/>
<pin name="VCC"/>
<pin name="RST"/>
<pin name="CH_PD"/>
<pin name="TXD"/>
</symbol>
<symbol name="ESP-WROOM-32-IMPORT">
<pin name="3V3"/>
<pin name="EN"/>
<pin name="GND"/>
<pin name="GND@1"/>
<pin name="GND@15"/>
<pin name="GND@38"/>
<pin name="IO0"/>
<pin name="IO2"/>
<pin name="IO4"/>
<pin name="CS0_V/IO5"/>
<pin name="MISO_H/IO12"/>
<pin name="MOSI_HIO13"/>
<pin name="SCK_HIO14"/>
<pin name="CS0_H/IO15"/>
<pin name="IO16"/>
<pin name="IO17"/>
<pin name="SCK_V/IO18"/>
<pin name="MISO_V/IO19"/>
<pin name="NC"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="MOSI_V/IO23"/>
<pin name="IO25"/>
<pin name="IO26"/>
<pin name="IO27"/>
<pin name="XTAL_P/IO32"/>
<pin name="XTAL_N/IO33"/>
<pin name="I34"/>
<pin name="I35"/>
<pin name="RXD"/>
<pin name="SCK/IO6"/>
<pin name="SCS/IO11"/>
<pin name="SDI/IO8"/>
<pin name="SDO/IO7"/>
<pin name="SENSOR_VN/I39"/>
<pin name="SENSOR_VP/I36"/>
<pin name="SHD/IO9"/>
<pin name="SWP/IO10"/>
<pin name="TXD"/>
</symbol>
<symbol name="E19-915MS1W">
<description>&lt;h3&gt;Chengdu Ebyte E19-915M30S - 915M TRX 1W Using SX1276, LoRa&lt;/h3&gt;
&lt;p&gt;This is a 915 MHz LoRa (or optionally FSK) modulated transciver bassed on the Semtech SX1276. It has a high ouput power of 1W an a pre-installed U.FL connector. Can be used with LoRa WAN with DIO0, DIO1, and DIO2 hooked up to controller interrupt inputs&lt;/p&gt;</description>
<pin name="RXEN"/>
<pin name="TXEN"/>
<pin name="!NSS"/>
<pin name="MOSI"/>
<pin name="MISO"/>
<pin name="SCK"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="!RST"/>
<pin name="DIO0"/>
<pin name="DIO1"/>
<pin name="DIO2"/>
<pin name="DIO3"/>
<pin name="DIO4"/>
<pin name="DIO5"/>
<pin name="ANT"/>
</symbol>
<symbol name="ESP-WROVER-32">
<pin name="GND@1"/>
<pin name="3V3"/>
<pin name="EN"/>
<pin name="SENSOR_VP/I36"/>
<pin name="SENSOR_VN/I39"/>
<pin name="IO34"/>
<pin name="IO35"/>
<pin name="XTAL_P/IO32"/>
<pin name="XTAL_N/IO33"/>
<pin name="IO25"/>
<pin name="IO26"/>
<pin name="IO27"/>
<pin name="SCK_H/IO14"/>
<pin name="MISO_H/IO12"/>
<pin name="GND@15"/>
<pin name="MOSI_H/IO13"/>
<pin name="SHD/IO9"/>
<pin name="SWP/IO10"/>
<pin name="SCS/IO11"/>
<pin name="GND@38"/>
<pin name="MOSI_V/IO23"/>
<pin name="IO22"/>
<pin name="TXD"/>
<pin name="RXD"/>
<pin name="IO21"/>
<pin name="NC"/>
<pin name="MISO_V/IO19"/>
<pin name="SCK_V/IO18"/>
<pin name="CS0_V/IO5"/>
<pin name="IO4"/>
<pin name="IO0"/>
<pin name="IO2"/>
<pin name="CS0_H/IO15"/>
<pin name="SDI/IO8"/>
<pin name="SDO/IO7"/>
<pin name="SCK/IO6"/>
<pin name="GND"/>
</symbol>
<symbol name="XBEE3">
<pin name="GND"/>
<pin name="VCC"/>
<pin name="!RST" direction="in"/>
<pin name="D13/DOUT"/>
<pin name="D14/DIN"/>
<pin name="D12"/>
<pin name="D10/PWM0/RSSI"/>
<pin name="D11/PWM1/SDA"/>
<pin name="D8/!DTR!/SLP_RQ"/>
<pin name="D19/!ATNN!/!BT_MODE"/>
<pin name="D18/SCK"/>
<pin name="D17/!SS"/>
<pin name="D16/MOSI"/>
<pin name="D15/MISO"/>
<pin name="D4"/>
<pin name="D9/ON/!SLP"/>
<pin name="D5/ASSOCIATE"/>
<pin name="D6/!RTS"/>
<pin name="D3/A3"/>
<pin name="D2/A2"/>
<pin name="D1/A1/SCL"/>
<pin name="D0/A0"/>
<pin name="RF"/>
<pin name="D7/!CTS"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ANTENNA" prefix="A">
<description>&lt;h3&gt;Single-ended Antennae&lt;/h3&gt;
&lt;p&gt;2.4GHz and antennae with just one terminal. These are all chip antennae.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;2.4GHz (WiFi/BT/ZigBee) Antennae&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;b&gt;ANT-2.4GHZ-6.5X2.2MM&lt;/b&gt; - 6.5 x 2.2 mm chip antenna. (&lt;a href="https://www.sparkfun.com/products/144"&gt;SparkFun Product&lt;/a&gt;)&lt;/li&gt;
&lt;li&gt;&lt;b&gt;ANT-2.4GHZ8.0X1.0MM&lt;/b&gt; -  8.0 x 1.0 mm chip antenna. (&lt;a href="http://www.mouser.com/ds/2/611/antenna_2500at44m0400-242425.pdf"&gt;Datasheet&lt;/a&gt;)&lt;/li&gt;
&lt;li&gt;&lt;b&gt;ANT-2.4GHZ9.5X2.0MM&lt;/b&gt; - 9.5 x 2.0 mm chip antenna. (&lt;a href="https://www.sparkfun.com/products/9025"&gt;SparkFun Product&lt;/a&gt;)&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ANTENNA"/>
</gates>
<devices>
<device name="2.4GHZ-9.5X2.0MM" package="ANT-2.4GHZ-9.5X2.0MM">
<connects>
<connect gate="G$1" pin="SIGNAL" pad="FEED"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="ANT-09067"/>
<attribute name="SF_ID" value="WRL-09025"/>
</technology>
</technologies>
</device>
<device name="2.4GHZ-6.5X2.2MM" package="ANT-2.4GHZ-6.5X2.2MM">
<connects>
<connect gate="G$1" pin="SIGNAL" pad="FEED"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="ANT-08187"/>
<attribute name="SF_ID" value="WRL-00144"/>
<attribute name="VALUE" value="2.45GHz"/>
</technology>
</technologies>
</device>
<device name="2.4GHZ-8.0X1.0MM" package="ANT-2.4GHZ-8.0X1.0MM">
<connects>
<connect gate="G$1" pin="SIGNAL" pad="FEED"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="ANT-14377"/>
</technology>
</technologies>
</device>
<device name="-2.4GHZ-3.2X1.6MM" package="ANT-2.4GHZ-3.2X1.6X1.2MM">
<connects>
<connect gate="G$1" pin="SIGNAL" pad="FEED"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="ANT-14235"/>
</technology>
</technologies>
</device>
<device name="-2.4GHZ-3.2X1.6MM-REDUCED" package="ANT-2.4GHZ-3.2X1.6X1.2MM-REDUCED_KEEPOUT">
<connects>
<connect gate="G$1" pin="SIGNAL" pad="FEED"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="ANT-14235"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA128RFA1" prefix="U" uservalue="yes">
<description>&lt;h3&gt;Atmel ATmega128RFA1 8-Bit AVR Microcontroller w/ Low-Power 2.4GHz RF Transceiver&lt;/h3&gt;
&lt;p&gt;The  ATmega128RFA1  is  a  low-power  CMOS  8-bit  microcontroller  based  on  the  AVR enhanced RISC architecture combined with a high data rate transceiver for the 2.4 GHz ISM band. By   executing   powerful   instructions   in   a   single   clock   cycle,   the   device   achieves  throughputs  approaching  1  MIPS  per  MHz  allowing  the  system  designer  to  optimize power consumption versus processing speed. The  radio  transceiver  provides  high  data  rates  from  250 kb/s  up  to  2 Mb/s,  frame handling,  outstanding receiver  sensitivity  and  high transmit  output  power  enabling  a very robust wireless communication. &lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.atmel.com/Images/Atmel-8266-MCU_Wireless-ATmega128RFA1_Datasheet.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/products/11197"&gt;SparkFun ATmega128RFA1 Development Board&lt;/a&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ATMEGA128RFA1"/>
</gates>
<devices>
<device name="" package="QFN-64-9X9MM">
<connects>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVDD" pad="60"/>
<connect gate="G$1" pin="AVSS@58" pad="58"/>
<connect gate="G$1" pin="AVSS@61" pad="61"/>
<connect gate="G$1" pin="AVSS_RFN" pad="10"/>
<connect gate="G$1" pin="AVSS_RFP" pad="7"/>
<connect gate="G$1" pin="CLKI" pad="33"/>
<connect gate="G$1" pin="DEVDD@23" pad="23"/>
<connect gate="G$1" pin="DEVDD@34" pad="34"/>
<connect gate="G$1" pin="DEVDD@44" pad="44"/>
<connect gate="G$1" pin="DEVDD@54" pad="54"/>
<connect gate="G$1" pin="DVDD@21" pad="21"/>
<connect gate="G$1" pin="DVDD@22" pad="22"/>
<connect gate="G$1" pin="DVSS@20" pad="20"/>
<connect gate="G$1" pin="DVSS@24" pad="24"/>
<connect gate="G$1" pin="DVSS@35" pad="35"/>
<connect gate="G$1" pin="DVSS@45" pad="45"/>
<connect gate="G$1" pin="DVSS@55" pad="55"/>
<connect gate="G$1" pin="EVDD" pad="59"/>
<connect gate="G$1" pin="PB0" pad="36"/>
<connect gate="G$1" pin="PB1/SCK" pad="37"/>
<connect gate="G$1" pin="PB2/PDI" pad="38"/>
<connect gate="G$1" pin="PB3/PDO" pad="39"/>
<connect gate="G$1" pin="PB4" pad="40"/>
<connect gate="G$1" pin="PB5" pad="41"/>
<connect gate="G$1" pin="PB6" pad="42"/>
<connect gate="G$1" pin="PB7" pad="43"/>
<connect gate="G$1" pin="PD0" pad="25"/>
<connect gate="G$1" pin="PD1" pad="26"/>
<connect gate="G$1" pin="PD2" pad="27"/>
<connect gate="G$1" pin="PD3" pad="28"/>
<connect gate="G$1" pin="PD4" pad="29"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PD6" pad="31"/>
<connect gate="G$1" pin="PD7" pad="32"/>
<connect gate="G$1" pin="PE0" pad="46"/>
<connect gate="G$1" pin="PE1" pad="47"/>
<connect gate="G$1" pin="PE2" pad="48"/>
<connect gate="G$1" pin="PE3" pad="49"/>
<connect gate="G$1" pin="PE4" pad="50"/>
<connect gate="G$1" pin="PE5" pad="51"/>
<connect gate="G$1" pin="PE6" pad="52"/>
<connect gate="G$1" pin="PE7" pad="53"/>
<connect gate="G$1" pin="PF0" pad="63"/>
<connect gate="G$1" pin="PF1" pad="64"/>
<connect gate="G$1" pin="PF2" pad="1"/>
<connect gate="G$1" pin="PF3" pad="2"/>
<connect gate="G$1" pin="PF4" pad="3"/>
<connect gate="G$1" pin="PF5" pad="4"/>
<connect gate="G$1" pin="PF6" pad="5"/>
<connect gate="G$1" pin="PF7" pad="6"/>
<connect gate="G$1" pin="PG0" pad="14"/>
<connect gate="G$1" pin="PG1" pad="15"/>
<connect gate="G$1" pin="PG2" pad="16"/>
<connect gate="G$1" pin="PG3" pad="17"/>
<connect gate="G$1" pin="PG4" pad="18"/>
<connect gate="G$1" pin="PG5" pad="19"/>
<connect gate="G$1" pin="RFN" pad="9"/>
<connect gate="G$1" pin="RFP" pad="8"/>
<connect gate="G$1" pin="RSTN" pad="12"/>
<connect gate="G$1" pin="RSTON" pad="13"/>
<connect gate="G$1" pin="TST" pad="11"/>
<connect gate="G$1" pin="XTAL1" pad="57"/>
<connect gate="G$1" pin="XTAL2" pad="56"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09639"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BALUN" prefix="B">
<description>&lt;h3&gt;Balun&lt;/h3&gt;
&lt;p&gt;Transformer to convert an unbalanced signal to a balenced one, or vice-versa.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://katalog.we-online.de/pbs/datasheet/748421245.pdf"&gt;Example Datasheet&lt;/a&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BALUN"/>
</gates>
<devices>
<device name="0805" package="BALUN-0805">
<connects>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT1" pad="3"/>
<connect gate="G$1" pin="OUT2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-09637"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BLUETOOTH-RN-41" prefix="U">
<description>&lt;h3&gt;Roving Networks RN-41 Bluetooth Module&lt;/h3&gt;
&lt;p&gt;The RN-41 module is a small form factor, low power, class 1 Bluetooth radio that is ideal for designers who want to add wireless capability to their products without spending significant time and money developing Bluetooth-specific hardware and software. The RN-41 supports multiple interface protocols, is simple to design in, and is fully certified, making it a complete embedded Bluetooth solution.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products&lt;/b&gt;:
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12575"&gt;Bluetooth SMD Module - RN-41&lt;/a&gt; (WRL-12575)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12579"&gt;Bluetooth Module Breakout - Roving Networks (RN-41 v6.15)&lt;/a&gt; (WRL-12579)&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RN41"/>
</gates>
<devices>
<device name="" package="RN41">
<connects>
<connect gate="G$1" pin="AIO0" pad="30"/>
<connect gate="G$1" pin="AIO1" pad="35"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND1" pad="12"/>
<connect gate="G$1" pin="GND2" pad="28"/>
<connect gate="G$1" pin="GND3" pad="29"/>
<connect gate="G$1" pin="PCMCLK" pad="7"/>
<connect gate="G$1" pin="PCMIN" pad="9"/>
<connect gate="G$1" pin="PCMOUT" pad="10"/>
<connect gate="G$1" pin="PCMSYNC" pad="8"/>
<connect gate="G$1" pin="PIO10" pad="33"/>
<connect gate="G$1" pin="PIO11" pad="34"/>
<connect gate="G$1" pin="PIO2" pad="19"/>
<connect gate="G$1" pin="PIO3" pad="20"/>
<connect gate="G$1" pin="PIO4" pad="22"/>
<connect gate="G$1" pin="PIO5" pad="21"/>
<connect gate="G$1" pin="PIO6" pad="3"/>
<connect gate="G$1" pin="PIO7" pad="4"/>
<connect gate="G$1" pin="PIO8" pad="31"/>
<connect gate="G$1" pin="PIO9" pad="32"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="SPICLK" pad="6"/>
<connect gate="G$1" pin="SPICSB" pad="23"/>
<connect gate="G$1" pin="SPIMISO" pad="24"/>
<connect gate="G$1" pin="SPIMOSI" pad="2"/>
<connect gate="G$1" pin="UARTCTS" pad="16"/>
<connect gate="G$1" pin="UARTRTS" pad="15"/>
<connect gate="G$1" pin="UARTRX" pad="13"/>
<connect gate="G$1" pin="UARTTX" pad="14"/>
<connect gate="G$1" pin="USBD+" pad="17"/>
<connect gate="G$1" pin="USBD-" pad="18"/>
<connect gate="G$1" pin="VDD" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11844"/>
<attribute name="SF_ID" value="WRL-12575"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BTM-182" prefix="U">
<description>&lt;h3&gt;Rayson BTM-182 Bluetooth Module&lt;/h3&gt;
&lt;p&gt;The BTM-182  is an easy to use Bluetooth SPP (Serial Port Protocol) module, designed for transparent wireless serial connection setup. This is a fully qualified Bluetooth V2.0+EDR (Enhanced Data Rate) 3Mbps modulation with complete 2.4GHz radio transceiver. It uses CSR Bluecore 04 external single chip Bluetooth system with CMOS technology and with AFH (Adaptive Frequency Hopping).&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products&lt;/b&gt;:
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/retired/9977"&gt;Bluetooth DIP Module - Rayson BTM-182&lt;/a&gt; (WRL-9977)&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BTM182"/>
</gates>
<devices>
<device name="_" package="BTM182">
<connects>
<connect gate="G$1" pin="AIO0" pad="2"/>
<connect gate="G$1" pin="AIO1" pad="3"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="PCM_CLK" pad="5"/>
<connect gate="G$1" pin="PCM_IN" pad="7"/>
<connect gate="G$1" pin="PCM_OUT" pad="4"/>
<connect gate="G$1" pin="PCM_SYNC" pad="6"/>
<connect gate="G$1" pin="PIO0" pad="31"/>
<connect gate="G$1" pin="PIO1" pad="32"/>
<connect gate="G$1" pin="PIO10" pad="30"/>
<connect gate="G$1" pin="PIO11" pad="1"/>
<connect gate="G$1" pin="PIO2" pad="27"/>
<connect gate="G$1" pin="PIO3" pad="26"/>
<connect gate="G$1" pin="PIO4" pad="25"/>
<connect gate="G$1" pin="PIO5" pad="24"/>
<connect gate="G$1" pin="PIO6" pad="23"/>
<connect gate="G$1" pin="PIO7" pad="22"/>
<connect gate="G$1" pin="PIO8" pad="28"/>
<connect gate="G$1" pin="PIO9" pad="29"/>
<connect gate="G$1" pin="RESET" pad="21"/>
<connect gate="G$1" pin="SPI_CLK" pad="20"/>
<connect gate="G$1" pin="SPI_CSB" pad="18"/>
<connect gate="G$1" pin="SPI_MISO" pad="19"/>
<connect gate="G$1" pin="SPI_MOSI" pad="17"/>
<connect gate="G$1" pin="UART_CTS" pad="8"/>
<connect gate="G$1" pin="UART_RTS" pad="11"/>
<connect gate="G$1" pin="UART_RX" pad="10"/>
<connect gate="G$1" pin="UART_TX" pad="9"/>
<connect gate="G$1" pin="USB_DN" pad="13"/>
<connect gate="G$1" pin="USB_DP" pad="12"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VDD_USB" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09842"/>
<attribute name="SF_ID" value="WRL-09913"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ID-12/20" prefix="U">
<description>&lt;h3&gt;ID Innovations 125kHz RFID Reader (ID2, ID3, ID12, and ID20)&lt;/h3&gt;
&lt;p&gt;The IDS, ID3, ID12, and ID20 are very simple to use RFID reader modules. Power the module, hold up a 125kHz card, and get a serial string output containing the unique ID of the card.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11862"&gt;RFID Reader ID-3LA (125 kHz)&lt;/a&gt; (SEN-11862)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11827"&gt;RFID Reader ID-12LA (125 kHz)&lt;/a&gt; (SEN-11827)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11828"&gt;RFID Reader ID-20LA (125 kHz)&lt;/a&gt; (SEN-11828)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9963"&gt;SparkFun RFID USB Reader&lt;/a&gt; (SEN-9963)&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ID-12"/>
</gates>
<devices>
<device name="" package="ID-12">
<connects>
<connect gate="G$1" pin="ANT1" pad="3"/>
<connect gate="G$1" pin="ANT2" pad="4"/>
<connect gate="G$1" pin="CP" pad="5"/>
<connect gate="G$1" pin="D1" pad="8"/>
<connect gate="G$1" pin="DATA" pad="9"/>
<connect gate="G$1" pin="FS" pad="7"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="LED" pad="10"/>
<connect gate="G$1" pin="RES" pad="2"/>
<connect gate="G$1" pin="TINRANGE" pad="6"/>
<connect gate="G$1" pin="VCC" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08875"/>
</technology>
</technologies>
</device>
<device name="ID-12_LOCK" package="ID-12_LOCK">
<connects>
<connect gate="G$1" pin="ANT1" pad="3"/>
<connect gate="G$1" pin="ANT2" pad="4"/>
<connect gate="G$1" pin="CP" pad="5"/>
<connect gate="G$1" pin="D1" pad="8"/>
<connect gate="G$1" pin="DATA" pad="9"/>
<connect gate="G$1" pin="FS" pad="7"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="LED" pad="10"/>
<connect gate="G$1" pin="RES" pad="2"/>
<connect gate="G$1" pin="TINRANGE" pad="6"/>
<connect gate="G$1" pin="VCC" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08875"/>
</technology>
</technologies>
</device>
<device name="SMD" package="ID-12_SMD">
<connects>
<connect gate="G$1" pin="ANT1" pad="3"/>
<connect gate="G$1" pin="ANT2" pad="4"/>
<connect gate="G$1" pin="CP" pad="5"/>
<connect gate="G$1" pin="D1" pad="8"/>
<connect gate="G$1" pin="DATA" pad="9"/>
<connect gate="G$1" pin="FS" pad="7"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="LED" pad="10"/>
<connect gate="G$1" pin="RES" pad="2"/>
<connect gate="G$1" pin="TINRANGE" pad="6"/>
<connect gate="G$1" pin="VCC" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09345, CONN-09344"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NRF24L01">
<description>&lt;h3&gt;Nordic nrf24L01 2.4GHz Low-power Transceiver&lt;/h3&gt;
&lt;p&gt;This is the very popular, low cost, very low power RF transceiver from Nordic Semiconductor. Simple SPI interface.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/690"&gt;2.4GHz Transceiver IC - nRF24L01+&lt;/a&gt; (COM-00690)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/705"&gt;SparkFun Transceiver Breakout - nRF24L01+ (RP-SMA)&lt;/a&gt; (WRL-00705)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/691"&gt;SparkFun Transceiver Breakout - nRF24L01+&lt;/a&gt; (COM-00691)&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="NRF24L01-1"/>
</gates>
<devices>
<device name="SMD" package="QFN20-4X4MM">
<connects>
<connect gate="G$1" pin="ANT1" pad="12"/>
<connect gate="G$1" pin="ANT2" pad="13"/>
<connect gate="G$1" pin="CE" pad="1"/>
<connect gate="G$1" pin="CSN" pad="2"/>
<connect gate="G$1" pin="DVDD" pad="19"/>
<connect gate="G$1" pin="IREF" pad="16"/>
<connect gate="G$1" pin="IRQ" pad="6"/>
<connect gate="G$1" pin="MISO" pad="5"/>
<connect gate="G$1" pin="MOSI" pad="4"/>
<connect gate="G$1" pin="SCK" pad="3"/>
<connect gate="G$1" pin="VDD@15" pad="15"/>
<connect gate="G$1" pin="VDD@18" pad="18"/>
<connect gate="G$1" pin="VDD@7" pad="7"/>
<connect gate="G$1" pin="VDD_PA" pad="11"/>
<connect gate="G$1" pin="VSS@0" pad="0"/>
<connect gate="G$1" pin="VSS@14" pad="14"/>
<connect gate="G$1" pin="VSS@17" pad="17"/>
<connect gate="G$1" pin="VSS@20" pad="20"/>
<connect gate="G$1" pin="VSS@8" pad="8"/>
<connect gate="G$1" pin="XC1" pad="10"/>
<connect gate="G$1" pin="XC2" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-08950"/>
<attribute name="SF_ID" value="COM-00690"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NRF24LE1">
<description>&lt;h3&gt;Nordic nRF24LE1 Ultra-low Power Wireless System on Chip&lt;/h3&gt;
&lt;p&gt;The Nordic Semiconductor nRF24LE1 is a 2.4GHz ISM band radio with emhanced 8051 MCU, up to 2Mbps on air data rate, 1.9 to 3.6V supply range, 16-32-bit multiplication-division co-processor (MDU), 16 kBytes of on-chip Flash, 1 kBytes on SRAM, 1 kBytes NV data memory, 512 Bytes NV data memory (extended endurance), Interrupt controller with 18 sources and 4 priority levels, 1 Analog comparator, 10 Bit ADC, Hardware SPI slave and master, UART, three 16-bit timers/counters, AES encryption/decryption co-processor, Random number generator, 2-Wire interface, 2 Channel PWM, 7, 15, or 31 GPIO lines, On-chip hardware debug support for a JTAG debugger.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="NRF24LE1"/>
</gates>
<devices>
<device name="" package="QFN-32-5X5MM">
<connects>
<connect gate="G$1" pin="ANT1" pad="21"/>
<connect gate="G$1" pin="ANT2" pad="22"/>
<connect gate="G$1" pin="DEC1" pad="3"/>
<connect gate="G$1" pin="DEC2" pad="4"/>
<connect gate="G$1" pin="IREF" pad="25"/>
<connect gate="G$1" pin="P0.0" pad="32"/>
<connect gate="G$1" pin="P0.1" pad="1"/>
<connect gate="G$1" pin="P0.2" pad="5"/>
<connect gate="G$1" pin="P0.3" pad="7"/>
<connect gate="G$1" pin="P0.4" pad="10"/>
<connect gate="G$1" pin="P0.5" pad="11"/>
<connect gate="G$1" pin="P0.6" pad="12"/>
<connect gate="G$1" pin="P0.7" pad="13"/>
<connect gate="G$1" pin="P1.0" pad="14"/>
<connect gate="G$1" pin="P1.1" pad="15"/>
<connect gate="G$1" pin="P1.2" pad="16"/>
<connect gate="G$1" pin="P1.3" pad="17"/>
<connect gate="G$1" pin="P1.4" pad="18"/>
<connect gate="G$1" pin="P1.5" pad="28"/>
<connect gate="G$1" pin="P1.6" pad="29"/>
<connect gate="G$1" pin="PROG" pad="6"/>
<connect gate="G$1" pin="RESET" pad="19"/>
<connect gate="G$1" pin="VDD1" pad="2"/>
<connect gate="G$1" pin="VDD2" pad="9"/>
<connect gate="G$1" pin="VDD3" pad="24"/>
<connect gate="G$1" pin="VDD4" pad="27"/>
<connect gate="G$1" pin="VDD_PA" pad="20"/>
<connect gate="G$1" pin="VSS1" pad="8"/>
<connect gate="G$1" pin="VSS2" pad="23"/>
<connect gate="G$1" pin="VSS3" pad="26"/>
<connect gate="G$1" pin="XC1" pad="31"/>
<connect gate="G$1" pin="XC2" pad="30"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09044"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NRF24LU1">
<description>&lt;h3&gt;Nordic nRF24LU1+ Single-Chip 2.4GHz Transceiver w/ USB Microcontroller and Flash&lt;/h3&gt;
&lt;p&gt;Nordic’s nRF24LU1+ is a complete system-on-chip wireless transceiver. The nRF24LU1+ features a fully integrated USB 2.0 compliant device controller, which makes this chip a great choice for a compact wireless USB dongle. The nRF24LU1+ is compatible with our nRF24L01+ 2.4GHz RF transceivers as well. Additional features include an 8-bit application microcontroller, 32 kB flash memory, 6 GPIO pins, SPI and UART support, and up to 2Mbps on air data rates.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9525"&gt;2.4GHz Transceiver IC - nRF24LU1+&lt;/a&gt; (COM-09525)&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="NRF24LU1"/>
</gates>
<devices>
<device name="" package="QFN-32-5X5MM">
<connects>
<connect gate="G$1" pin="/RESET" pad="8"/>
<connect gate="G$1" pin="ANT1" pad="21"/>
<connect gate="G$1" pin="ANT2" pad="22"/>
<connect gate="G$1" pin="D+" pad="4"/>
<connect gate="G$1" pin="D-" pad="5"/>
<connect gate="G$1" pin="DEC1" pad="28"/>
<connect gate="G$1" pin="DEC2" pad="29"/>
<connect gate="G$1" pin="IREF" pad="25"/>
<connect gate="G$1" pin="P0.0" pad="10"/>
<connect gate="G$1" pin="P0.1" pad="11"/>
<connect gate="G$1" pin="P0.2" pad="13"/>
<connect gate="G$1" pin="P0.3" pad="14"/>
<connect gate="G$1" pin="P0.4" pad="15"/>
<connect gate="G$1" pin="P0.5" pad="16"/>
<connect gate="G$1" pin="PROG" pad="7"/>
<connect gate="G$1" pin="VBUS" pad="2"/>
<connect gate="G$1" pin="VDD1" pad="1"/>
<connect gate="G$1" pin="VDD2" pad="3"/>
<connect gate="G$1" pin="VDD3" pad="9"/>
<connect gate="G$1" pin="VDD4" pad="19"/>
<connect gate="G$1" pin="VDD5" pad="24"/>
<connect gate="G$1" pin="VDD6" pad="27"/>
<connect gate="G$1" pin="VDD_PA" pad="20"/>
<connect gate="G$1" pin="VSS1" pad="6"/>
<connect gate="G$1" pin="VSS2" pad="12"/>
<connect gate="G$1" pin="VSS3" pad="17"/>
<connect gate="G$1" pin="VSS4" pad="18"/>
<connect gate="G$1" pin="VSS5" pad="23"/>
<connect gate="G$1" pin="VSS6" pad="26"/>
<connect gate="G$1" pin="VSS7" pad="30"/>
<connect gate="G$1" pin="XC1" pad="32"/>
<connect gate="G$1" pin="XC2" pad="31"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09045"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RF-LINK_RX">
<description>&lt;h3&gt;RF Link Receiver (434 MHz, 315 MHz)&lt;/h3&gt;
&lt;p&gt;These wireless receivers work with equivalent transmitters. They can easily fit into a breadboard and work well with microcontrollers to create a very simple wireless data link. Since these are only receivers, they will only work communicating data one-way, you would need two pairs (of different frequencies) to act as a transmitter/receiver pair..&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10532"&gt;RF Link Receiver - 4800bps (434 MHz)&lt;/a&gt;(WRL-10532)&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RF-LINK_RX"/>
</gates>
<devices>
<device name="" package="RF-LINK_RX">
<connects>
<connect gate="G$1" pin="+5V" pad="+5V@1"/>
<connect gate="G$1" pin="ANT" pad="ANT"/>
<connect gate="G$1" pin="DATA" pad="DATA@1"/>
<connect gate="G$1" pin="GND" pad="GND@1"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="WRL-10533"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RF-LINK_TX">
<description>&lt;h3&gt;RF Link Transmitter (434 MHz, 315 MHz)&lt;/h3&gt;
&lt;p&gt;These wireless transmitters work with equivalent receivers. They can easily fit into a breadboard and work well with microcontrollers to create a very simple wireless data link. Since these are only transmitters, they will only work communicating data one-way, you would need two pairs (of different frequencies) to act as a transmitter/receiver pair.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10534"&gt;RF Link Transmitter - 434MHz&lt;/a&gt; (WRL-10534)&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RF-LINK_TX"/>
</gates>
<devices>
<device name="" package="RF-LINK_TX">
<connects>
<connect gate="G$1" pin="+5V" pad="VCC"/>
<connect gate="G$1" pin="ANT" pad="ANT"/>
<connect gate="G$1" pin="DATA" pad="DATA"/>
<connect gate="G$1" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="WRL-10534"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RFM22">
<description>&lt;h3&gt;Hope RF RFM22 ISM Transciever Module&lt;/h3&gt;

&lt;p&gt;The RFM22 is a low-power, low cost radio that is capable of operating in the 434MHz and 900MHz open bands. It's frequency is software defined and there are some very good libraries written for it.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11018"&gt;SparkFun RFM22 Shield - 434MHz&lt;/a&gt; (DEV-11018)&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RFM22"/>
</gates>
<devices>
<device name="434MHZ" package="RFM22-XXX-S2">
<connects>
<connect gate="G$1" pin="ANT" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="GND@2" pad="9"/>
<connect gate="G$1" pin="GND@3" pad="16"/>
<connect gate="G$1" pin="GPIO0" pad="6"/>
<connect gate="G$1" pin="GPIO1" pad="7"/>
<connect gate="G$1" pin="GPIO2" pad="8"/>
<connect gate="G$1" pin="NIRQ" pad="14"/>
<connect gate="G$1" pin="NSEL" pad="13"/>
<connect gate="G$1" pin="RXANT" pad="3"/>
<connect gate="G$1" pin="SCLK" pad="12"/>
<connect gate="G$1" pin="SDI" pad="11"/>
<connect gate="G$1" pin="SDN" pad="15"/>
<connect gate="G$1" pin="SDO" pad="10"/>
<connect gate="G$1" pin="TXANT" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-10007"/>
<attribute name="SF_ID" value="WRL-10153"/>
<attribute name="VALUE" value="434MHz"/>
</technology>
</technologies>
</device>
<device name="915MHZ" package="RFM22-XXX-S2">
<connects>
<connect gate="G$1" pin="ANT" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="GND@2" pad="9"/>
<connect gate="G$1" pin="GND@3" pad="16"/>
<connect gate="G$1" pin="GPIO0" pad="6"/>
<connect gate="G$1" pin="GPIO1" pad="7"/>
<connect gate="G$1" pin="GPIO2" pad="8"/>
<connect gate="G$1" pin="NIRQ" pad="14"/>
<connect gate="G$1" pin="NSEL" pad="13"/>
<connect gate="G$1" pin="RXANT" pad="3"/>
<connect gate="G$1" pin="SCLK" pad="12"/>
<connect gate="G$1" pin="SDI" pad="11"/>
<connect gate="G$1" pin="SDN" pad="15"/>
<connect gate="G$1" pin="SDO" pad="10"/>
<connect gate="G$1" pin="TXANT" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11750"/>
<attribute name="SF_ID" value="WRL-12030"/>
<attribute name="VALUE" value="915MHz"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RMCM01">
<description>&lt;h3&gt;Polar RMCM01 Heart Rate Monitor Receiver&lt;/h3&gt; 
&lt;p&gt;The Polar heart rate receiver component receiver
wirelessly receives the heart rate signal from Polar
transmitter belt. The complete heart rate measurement
system consists of three different parts; transmitter,
receiver and electronics and/or display device that is
outputting the heart rate value.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8661"&gt;Polar Heart Rate Monitor Interface&lt;/a&gt; (SEN-08661)&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RMCM01"/>
</gates>
<devices>
<device name="" package="RMCM01">
<connects>
<connect gate="G$1" pin="F32KIN" pad="3"/>
<connect gate="G$1" pin="FPLS" pad="6"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="HR" pad="5"/>
<connect gate="G$1" pin="LX1" pad="10"/>
<connect gate="G$1" pin="LX2" pad="9"/>
<connect gate="G$1" pin="OSC" pad="4"/>
<connect gate="G$1" pin="OSC_ON" pad="2"/>
<connect gate="G$1" pin="RESET" pad="7"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="WIDB_DET" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-08853"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RN171" prefix="U">
<description>&lt;h3&gt;Roving Networks RN-171 802.11b/g WiFi Serial Module&lt;/h3&gt; 
&lt;p&gt;The RN-171 is a small form factor, ultra-low power embedded TCP/IP module. The RN-171 is a standalone, complete TCP/IP wireless networking module. Due to its small form factor and extremely low power consumption, it is perfect for mobile wireless applications such as asset monitoring, sensors, and portable battery operated devices.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/retired/11049"&gt;WiFly RN-171 802.11b/g Serial Module&lt;/a&gt; (WRL-11049)&lt;/li&gt;

&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RN171"/>
</gates>
<devices>
<device name="" package="RN171">
<connects>
<connect gate="G$1" pin="ANT" pad="24"/>
<connect gate="G$1" pin="AWAKE" pad="41"/>
<connect gate="G$1" pin="CLK" pad="4"/>
<connect gate="G$1" pin="CS" pad="5"/>
<connect gate="G$1" pin="CTS" pad="44"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@14" pad="14"/>
<connect gate="G$1" pin="GND@20" pad="20"/>
<connect gate="G$1" pin="GND@21" pad="21"/>
<connect gate="G$1" pin="GND@22" pad="22"/>
<connect gate="G$1" pin="GND@23" pad="23"/>
<connect gate="G$1" pin="GND@25" pad="25"/>
<connect gate="G$1" pin="GND@26" pad="26"/>
<connect gate="G$1" pin="GND@27" pad="27"/>
<connect gate="G$1" pin="GND@28" pad="28"/>
<connect gate="G$1" pin="GND@39" pad="39"/>
<connect gate="G$1" pin="GND@47" pad="47"/>
<connect gate="G$1" pin="GPIO1" pad="13"/>
<connect gate="G$1" pin="GPIO14" pad="42"/>
<connect gate="G$1" pin="GPIO2" pad="12"/>
<connect gate="G$1" pin="GPIO3" pad="11"/>
<connect gate="G$1" pin="GPIO7" pad="6"/>
<connect gate="G$1" pin="INT/GPIO6" pad="7"/>
<connect gate="G$1" pin="MISO" pad="8"/>
<connect gate="G$1" pin="MOSI" pad="9"/>
<connect gate="G$1" pin="RESET" pad="40"/>
<connect gate="G$1" pin="RTS" pad="43"/>
<connect gate="G$1" pin="RX" pad="45"/>
<connect gate="G$1" pin="SEN0" pad="29"/>
<connect gate="G$1" pin="SEN1" pad="30"/>
<connect gate="G$1" pin="SEN2" pad="31"/>
<connect gate="G$1" pin="SEN3" pad="32"/>
<connect gate="G$1" pin="SEN4" pad="35"/>
<connect gate="G$1" pin="SEN5" pad="36"/>
<connect gate="G$1" pin="SEN6" pad="37"/>
<connect gate="G$1" pin="SEN7" pad="38"/>
<connect gate="G$1" pin="SPOWER" pad="33"/>
<connect gate="G$1" pin="SREG" pad="48"/>
<connect gate="G$1" pin="TX" pad="46"/>
<connect gate="G$1" pin="VDD" pad="10"/>
<connect gate="G$1" pin="VDD_BATT" pad="49"/>
<connect gate="G$1" pin="VDD_RF" pad="34"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11000"/>
<attribute name="SF_ID" value="WRL-11049"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SI4703" prefix="U">
<description>&lt;h3&gt;Silicon Labs Si4703 FM Tuner&lt;/h3&gt;
&lt;p&gt;Beyond enabling you to tune in to FM radio stations, the Si4703 is also capable of detecting and processing both Radio Data Service (RDS) and Radio Broadcast Data Service (RBDS) information. The Si4703 even does a very good job of filtering and carrier detection. It also enables data such as the station ID and song name to be displayed to the user.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12938"&gt;SparkFun FM Tuner Evaluation Board - Si4703&lt;/a&gt; (WRL-12938)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11083"&gt;SparkFun FM Tuner Basic Breakout - Si4703&lt;/a&gt; (WRL-11083)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11043"&gt;FabFM Radio Kit &lt;/a&gt; (KIT-11043)&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SI470X"/>
</gates>
<devices>
<device name="" package="QFN-20-3X3MM">
<connects>
<connect gate="G$1" pin="!RST" pad="5"/>
<connect gate="G$1" pin="!SEN" pad="6"/>
<connect gate="G$1" pin="DOUT" pad="15"/>
<connect gate="G$1" pin="FMIP" pad="2"/>
<connect gate="G$1" pin="GND@12" pad="12"/>
<connect gate="G$1" pin="GND@PAD" pad="21"/>
<connect gate="G$1" pin="GPIO1" pad="19"/>
<connect gate="G$1" pin="GPIO2" pad="18"/>
<connect gate="G$1" pin="GPIO3" pad="17"/>
<connect gate="G$1" pin="LOUT" pad="14"/>
<connect gate="G$1" pin="LPI" pad="4"/>
<connect gate="G$1" pin="RCLK" pad="9"/>
<connect gate="G$1" pin="RFGND" pad="3"/>
<connect gate="G$1" pin="ROUT" pad="13"/>
<connect gate="G$1" pin="SCLK" pad="7"/>
<connect gate="G$1" pin="SDIO" pad="8"/>
<connect gate="G$1" pin="VA" pad="16"/>
<connect gate="G$1" pin="VD" pad="11"/>
<connect gate="G$1" pin="VIO" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-10150"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SM130" prefix="U">
<description>&lt;h3&gt;SonMicro SMB130 - 13.56 MHz RFID Mifare Read/Write Module&lt;/h3&gt;
&lt;p&gt;The SMB130 is a 28 pin DIP module that includes all necessary components for a 13.56 MHz RFID MIFARE®, aside from a PCB antenna.&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10126"&gt;RFID Module - SM130 MIFARE® (13.56 MHz) &lt;/a&gt; (SEN-10126)&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SM130"/>
</gates>
<devices>
<device name="" package="SM130">
<connects>
<connect gate="G$1" pin="ANT1" pad="24"/>
<connect gate="G$1" pin="ANT2" pad="26"/>
<connect gate="G$1" pin="ERROR" pad="17"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="I1" pad="19"/>
<connect gate="G$1" pin="I2" pad="20"/>
<connect gate="G$1" pin="O1" pad="21"/>
<connect gate="G$1" pin="O2" pad="22"/>
<connect gate="G$1" pin="OK" pad="16"/>
<connect gate="G$1" pin="RESET" pad="18"/>
<connect gate="G$1" pin="RFGND@23" pad="23"/>
<connect gate="G$1" pin="RFGND@25" pad="25"/>
<connect gate="G$1" pin="RFGND@27" pad="27"/>
<connect gate="G$1" pin="RFVCC" pad="1"/>
<connect gate="G$1" pin="RX-I" pad="11"/>
<connect gate="G$1" pin="SCL" pad="9"/>
<connect gate="G$1" pin="SDA" pad="10"/>
<connect gate="G$1" pin="TX-O" pad="12"/>
<connect gate="G$1" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="LPA-12905"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SM5100B">
<description>&lt;h3&gt;LinkSprite SM5100B GSM/GPRS Module&lt;/h3&gt;
&lt;p&gt;The SM5100B is a miniature, quad-band GSM 850/EGSM 900/DCS 1800/PCS 1900 module, which can be integrated into a great number of wireless projects. You can use this module to accomplish almost anything a normal cell phone can - SMS text messages, GSM/GPRS, TCP/IP, and more!&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9533"&gt;GSM/GPRS Module - SM5100B&lt;/a&gt; (CEL-09533)&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SM5100B"/>
</gates>
<devices>
<device name="" package="SM5100B">
<connects>
<connect gate="G$1" pin="ADIN1" pad="6"/>
<connect gate="G$1" pin="ADIN2" pad="8"/>
<connect gate="G$1" pin="AUX_MICN" pad="50"/>
<connect gate="G$1" pin="AUX_MICP" pad="42"/>
<connect gate="G$1" pin="AUX_SPKN" pad="58"/>
<connect gate="G$1" pin="AUX_SPKP" pad="44"/>
<connect gate="G$1" pin="EAR_MICN" pad="12"/>
<connect gate="G$1" pin="EAR_MICP" pad="14"/>
<connect gate="G$1" pin="EAR_SPKN" pad="16"/>
<connect gate="G$1" pin="EAR_SPKP" pad="18"/>
<connect gate="G$1" pin="GND@0" pad="13"/>
<connect gate="G$1" pin="GND@1" pad="15"/>
<connect gate="G$1" pin="GND@2" pad="17"/>
<connect gate="G$1" pin="GND@3" pad="9"/>
<connect gate="G$1" pin="GND@4" pad="11"/>
<connect gate="G$1" pin="GPIO_1" pad="39"/>
<connect gate="G$1" pin="GPIO_10" pad="37"/>
<connect gate="G$1" pin="GPIO_16" pad="52"/>
<connect gate="G$1" pin="GPIO_17" pad="22"/>
<connect gate="G$1" pin="GPIO_18" pad="45"/>
<connect gate="G$1" pin="GPIO_19" pad="10"/>
<connect gate="G$1" pin="GPIO_20" pad="56"/>
<connect gate="G$1" pin="GPIO_26" pad="49"/>
<connect gate="G$1" pin="GPIO_3" pad="55"/>
<connect gate="G$1" pin="GPIO_4" pad="35"/>
<connect gate="G$1" pin="GPIO_46" pad="57"/>
<connect gate="G$1" pin="GPIO_6" pad="38"/>
<connect gate="G$1" pin="GPIO_8" pad="54"/>
<connect gate="G$1" pin="GPIO_9" pad="41"/>
<connect gate="G$1" pin="GPO42/NBOOT" pad="33"/>
<connect gate="G$1" pin="GPO_11" pad="53"/>
<connect gate="G$1" pin="KEY_DRV0" pad="24"/>
<connect gate="G$1" pin="KEY_DRV1" pad="28"/>
<connect gate="G$1" pin="KEY_DRV2" pad="26"/>
<connect gate="G$1" pin="KEY_DRV3" pad="23"/>
<connect gate="G$1" pin="KEY_DRV4" pad="25"/>
<connect gate="G$1" pin="KEY_DRV5" pad="30"/>
<connect gate="G$1" pin="KEY_SEN0" pad="36"/>
<connect gate="G$1" pin="KEY_SEN1" pad="32"/>
<connect gate="G$1" pin="KEY_SEN2" pad="31"/>
<connect gate="G$1" pin="KEY_SEN3" pad="40"/>
<connect gate="G$1" pin="POWER_ON" pad="59"/>
<connect gate="G$1" pin="RESET" pad="34"/>
<connect gate="G$1" pin="RTC_BATT" pad="48"/>
<connect gate="G$1" pin="RXD0" pad="20"/>
<connect gate="G$1" pin="RXD1" pad="43"/>
<connect gate="G$1" pin="SIM_CLK" pad="27"/>
<connect gate="G$1" pin="SIM_DA" pad="29"/>
<connect gate="G$1" pin="SIM_RST" pad="21"/>
<connect gate="G$1" pin="SIM_VCC" pad="51"/>
<connect gate="G$1" pin="TXD0" pad="19"/>
<connect gate="G$1" pin="TXD1" pad="46"/>
<connect gate="G$1" pin="VBAT@0" pad="7"/>
<connect gate="G$1" pin="VBAT@1" pad="1"/>
<connect gate="G$1" pin="VBAT@2" pad="3"/>
<connect gate="G$1" pin="VBAT@3" pad="5"/>
<connect gate="G$1" pin="VCC@0" pad="47"/>
<connect gate="G$1" pin="VCC@1" pad="60"/>
<connect gate="G$1" pin="VCHG@0" pad="2"/>
<connect gate="G$1" pin="VCHG@1" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09315"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WIFLY_GSX">
<description>&lt;h3&gt;Roving Networks WiFly GSX (RN-131C) Wi-Fi Module&lt;/h3&gt;
&lt;p&gt;The WiFly GSX (RN-131C) module is a complete ultra low power embedded TCP/IP solution. The WiFly GSX module is a stand alone, embedded wireless 802.11b/g networking module.&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;p&gt;&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10004"&gt;WiFly GSX 802.11b/g Serial Module - Roving Networks&lt;/a&gt; (WRL-10004)&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="WIFLY_GSX"/>
</gates>
<devices>
<device name="" package="WIFLY_GSX">
<connects>
<connect gate="G$1" pin="3V3_IN" pad="18"/>
<connect gate="G$1" pin="3V3_OUT" pad="17"/>
<connect gate="G$1" pin="DMA_RX" pad="23"/>
<connect gate="G$1" pin="DMA_TX" pad="22"/>
<connect gate="G$1" pin="EPCA" pad="6"/>
<connect gate="G$1" pin="EPCB" pad="7"/>
<connect gate="G$1" pin="FORCE_WAKE" pad="9"/>
<connect gate="G$1" pin="G1" pad="19"/>
<connect gate="G$1" pin="G10" pad="44"/>
<connect gate="G$1" pin="G2" pad="36"/>
<connect gate="G$1" pin="G3" pad="37"/>
<connect gate="G$1" pin="G4" pad="38"/>
<connect gate="G$1" pin="G5" pad="39"/>
<connect gate="G$1" pin="G6" pad="40"/>
<connect gate="G$1" pin="G7" pad="41"/>
<connect gate="G$1" pin="G8" pad="42"/>
<connect gate="G$1" pin="G9" pad="43"/>
<connect gate="G$1" pin="GPIO4" pad="29"/>
<connect gate="G$1" pin="GPIO5" pad="28"/>
<connect gate="G$1" pin="GPIO6" pad="27"/>
<connect gate="G$1" pin="GPIO7" pad="26"/>
<connect gate="G$1" pin="GPIO8" pad="25"/>
<connect gate="G$1" pin="GPIO9" pad="24"/>
<connect gate="G$1" pin="GPIO_12" pad="11"/>
<connect gate="G$1" pin="GPIO_13" pad="10"/>
<connect gate="G$1" pin="NC" pad="35"/>
<connect gate="G$1" pin="RESET_L" pad="5"/>
<connect gate="G$1" pin="SENS0" pad="34"/>
<connect gate="G$1" pin="SENS1" pad="30"/>
<connect gate="G$1" pin="SENS2" pad="31"/>
<connect gate="G$1" pin="SENS3" pad="32"/>
<connect gate="G$1" pin="SENS4" pad="2"/>
<connect gate="G$1" pin="SENS5" pad="3"/>
<connect gate="G$1" pin="SENS6" pad="1"/>
<connect gate="G$1" pin="SENS7" pad="4"/>
<connect gate="G$1" pin="SENSPWR" pad="33"/>
<connect gate="G$1" pin="SPI_CLK" pad="15"/>
<connect gate="G$1" pin="SPI_MISO" pad="16"/>
<connect gate="G$1" pin="SPI_MOSI" pad="14"/>
<connect gate="G$1" pin="SUPCAP" pad="8"/>
<connect gate="G$1" pin="URX" pad="12"/>
<connect gate="G$1" pin="UTX" pad="13"/>
<connect gate="G$1" pin="VD_3V_IN" pad="21"/>
<connect gate="G$1" pin="VD_BAT" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-12671"/>
<attribute name="SF_ID" value="WRL-13525"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XTEND-DIGI-MODEM">
<description>&lt;h3&gt;Digi XTend 900 1W RF Transceiver&lt;/h3&gt;
&lt;p&gt;The XTend Modem packs a ton of RF punch into a small, low-power, easy-to-use, and reliable module. Outdoors, with line-of-sight, this module can communicate at up to 40 miles; indoors it can still do up to 3000ft. The module transfers a standard asynchronous serial data stream, operates within the ISM 900MHz frequency band and sustains up to 115.2kbps data throughput. The module comes with an attached RPSMA antenna connector.&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9411"&gt;XTend 900 1W RPSMA - 40 Mile Range&lt;/a&gt; (WRL-09411)&lt;/li&gt;&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="XTEND-DIGI-MODEM"/>
</gates>
<devices>
<device name="" package="XTEND-DIGI-MODEM">
<connects>
<connect gate="G$1" pin="CONFIG" pad="11"/>
<connect gate="G$1" pin="CTS" pad="9"/>
<connect gate="G$1" pin="DI" pad="5"/>
<connect gate="G$1" pin="DO" pad="6"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GPO2" pad="3"/>
<connect gate="G$1" pin="RTS" pad="10"/>
<connect gate="G$1" pin="SHDN" pad="7"/>
<connect gate="G$1" pin="SLEEP" pad="8"/>
<connect gate="G$1" pin="TX_PWR" pad="4"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="WRL-09411"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BLUERADIO_BR-LE4.0-S2" uservalue="yes">
<description>&lt;H3&gt;Blue Radios BR-LE4.0-S2A BlueTooth 4.0 Module&lt;/H3&gt;
&lt;p&gt;The BR-LE4.0-S2A is a standalone Class 1 Bluetooth 4.0 module that requires no firmware or external components. Custom client applications can be written directly onto the module, which supports both analog and digital peripherals, eliminating the need for a second microprocessor. Alternately, the BR-LE4.0-S2A can be integrated into an existing design as a HCI network processor device, with a host processor running the core application and the BR-LE4.0-S2A providing Bluetooth low energy communications.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products&lt;/b&gt;:
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12991"&gt;Bluetooth 4.0 Module - BR-LE 4.0-S2A&lt;/a&gt; (WRL-12991)&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BLUERADIO_BR-LE4.0-S2"/>
</gates>
<devices>
<device name="" package="BLUERADIO_BR-LE4.0-S2">
<connects>
<connect gate="G$1" pin="ADC_0" pad="21"/>
<connect gate="G$1" pin="ADC_1" pad="4"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="10"/>
<connect gate="G$1" pin="GND@2" pad="20"/>
<connect gate="G$1" pin="GND@3" pad="30"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="PIO_14" pad="19"/>
<connect gate="G$1" pin="PIO_2" pad="23"/>
<connect gate="G$1" pin="PIO_3/INT" pad="26"/>
<connect gate="G$1" pin="PIO_4" pad="28"/>
<connect gate="G$1" pin="PIO_5" pad="24"/>
<connect gate="G$1" pin="PIO_6" pad="25"/>
<connect gate="G$1" pin="PIO_7" pad="29"/>
<connect gate="G$1" pin="PIO_8" pad="27"/>
<connect gate="G$1" pin="PIO_9" pad="22"/>
<connect gate="G$1" pin="RESET" pad="3"/>
<connect gate="G$1" pin="SPI_CLK" pad="7"/>
<connect gate="G$1" pin="SPI_CSB" pad="6"/>
<connect gate="G$1" pin="SPI_MISO" pad="5"/>
<connect gate="G$1" pin="SPI_MOSI" pad="8"/>
<connect gate="G$1" pin="UART_CTS" pad="11"/>
<connect gate="G$1" pin="UART_RTS" pad="12"/>
<connect gate="G$1" pin="UART_RX" pad="14"/>
<connect gate="G$1" pin="UART_TX" pad="13"/>
<connect gate="G$1" pin="USB_DM" pad="18"/>
<connect gate="G$1" pin="USB_DP" pad="17"/>
<connect gate="G$1" pin="USB_GND" pad="16"/>
<connect gate="G$1" pin="USB_VBUS" pad="15"/>
<connect gate="G$1" pin="VCC(2.0-3.6V)" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11328"/>
<attribute name="VALUE" value="BR-LE4.0-S2A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ELECTRIC_IMP" prefix="U">
<description>&lt;h3&gt;Electric Imp SD Socket&lt;/h3&gt;
&lt;p&gt;The Electric Imp provides an easy, integrated way to connect almost any hardware device both to other devices and to internet services. It’s more than just a WiFi card, or even a WiFi module with processing built in - it’s an integrated platform that deals with the drudgery of connectivity, allowing you to concentrate on the application instead of the mechanics.
&lt;p&gt;This device matches the &lt;a href="https://www.sparkfun.com/products/11395"&gt;Electric Imp&lt;/a&gt; pinout to a 4UCONN SD MMC connector. The 4UCONN part number for the connector is &lt;a href="http://www.4uconnector.com/online/Itemadrawing.asp?fldseries=19646&amp;seriesno_a=12"&gt;19646&lt;/a&gt;.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products&lt;/b&gt;:
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12886"&gt;Electric Imp Breakout&lt;/a&gt; (WRL-12886)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12887"&gt;SparkFun Electric Imp Shield&lt;/a&gt; (WRL-12887)&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ELECTRIC_IMP"/>
</gates>
<devices>
<device name="" package="SD-CARD">
<connects>
<connect gate="G$1" pin="1(CLK2/CTS1/TX3/SCL2)" pad="1"/>
<connect gate="G$1" pin="2(MISO1/MOSI2/RTS1/RX3/SDA2)" pad="2"/>
<connect gate="G$1" pin="5(SCLK1/SCLK2/TX2)" pad="5"/>
<connect gate="G$1" pin="7(MOSI1/MISO2/RX2)" pad="7"/>
<connect gate="G$1" pin="8(MOSI2/TX1/SCL1)" pad="8"/>
<connect gate="G$1" pin="9(MISO2/RX1/SDA1)" pad="9"/>
<connect gate="G$1" pin="CD" pad="CD"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="ID" pad="6"/>
<connect gate="G$1" pin="S1" pad="SH@1"/>
<connect gate="G$1" pin="S2" pad="SH@2"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="WP" pad="WP"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11976"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BC127" prefix="U" uservalue="yes">
<description>&lt;H3&gt;Blue Creations BC127 BLE module&lt;/H3&gt;
&lt;p&gt;The BC127 is a highly flexible, low power, small form factor Bluetooth Version 4.0 Certified Audio module. It comes preloaded with BlueCreation Melody software, and is ideal for developers who want to quickly and cost effectively integrate Bluetooth functionality into their products.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products&lt;/b&gt;:
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12819"&gt;Bluetooth SMD Module - BC127&lt;/a&gt; (WRL-12819)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11927"&gt;Bluetooth Audio Breakout - BC127&lt;/a&gt; (WRL-11927)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11924"&gt;Purpletooth Jamboree - BC127 Development Board&lt;/a&gt; (WRL-11924)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name=".ANALOG_AUDIO" symbol="BC127_ANALOG_AUDIO"/>
<gate name=".GPIO" symbol="BC127_GPIO"/>
<gate name=".POWER" symbol="BC127_POWER"/>
<gate name=".DATA_PORTS" symbol="BC127_DATA_PORTS"/>
</gates>
<devices>
<device name="&quot;" package="BC127">
<connects>
<connect gate=".ANALOG_AUDIO" pin="MIC_BIAS_A" pad="17"/>
<connect gate=".ANALOG_AUDIO" pin="MIC_LN" pad="20"/>
<connect gate=".ANALOG_AUDIO" pin="MIC_LP" pad="21"/>
<connect gate=".ANALOG_AUDIO" pin="MIC_RN" pad="18"/>
<connect gate=".ANALOG_AUDIO" pin="MIC_RP" pad="19"/>
<connect gate=".ANALOG_AUDIO" pin="SPKR_LN" pad="13"/>
<connect gate=".ANALOG_AUDIO" pin="SPKR_LP" pad="14"/>
<connect gate=".ANALOG_AUDIO" pin="SPKR_RN" pad="15"/>
<connect gate=".ANALOG_AUDIO" pin="SPKR_RP" pad="16"/>
<connect gate=".DATA_PORTS" pin="PCM_CLK/CLK" pad="47"/>
<connect gate=".DATA_PORTS" pin="PCM_IN/MOSI" pad="49"/>
<connect gate=".DATA_PORTS" pin="PCM_OUT/MISO" pad="48"/>
<connect gate=".DATA_PORTS" pin="PCM_SYNC/CSB" pad="46"/>
<connect gate=".DATA_PORTS" pin="SPI_!PCM" pad="45"/>
<connect gate=".DATA_PORTS" pin="UART_CTS" pad="40"/>
<connect gate=".DATA_PORTS" pin="UART_RTS" pad="43"/>
<connect gate=".DATA_PORTS" pin="UART_RX" pad="42"/>
<connect gate=".DATA_PORTS" pin="UART_TX" pad="41"/>
<connect gate=".DATA_PORTS" pin="USB_N" pad="35"/>
<connect gate=".DATA_PORTS" pin="USB_P" pad="36"/>
<connect gate=".GPIO" pin="AIO_1" pad="12"/>
<connect gate=".GPIO" pin="CAP_SENSE_1" pad="7"/>
<connect gate=".GPIO" pin="CAP_SENSE_2" pad="10"/>
<connect gate=".GPIO" pin="CAP_SENSE_3" pad="9"/>
<connect gate=".GPIO" pin="CAP_SENSE_4" pad="8"/>
<connect gate=".GPIO" pin="LED_0" pad="37"/>
<connect gate=".GPIO" pin="LED_1" pad="38"/>
<connect gate=".GPIO" pin="LED_2" pad="39"/>
<connect gate=".GPIO" pin="PIO_0" pad="23"/>
<connect gate=".GPIO" pin="PIO_1" pad="24"/>
<connect gate=".GPIO" pin="PIO_2" pad="50"/>
<connect gate=".GPIO" pin="PIO_3" pad="51"/>
<connect gate=".GPIO" pin="PIO_4" pad="26"/>
<connect gate=".GPIO" pin="PIO_5" pad="25"/>
<connect gate=".GPIO" pin="PIO_6" pad="5"/>
<connect gate=".GPIO" pin="PIO_7" pad="6"/>
<connect gate=".POWER" pin="!RESET" pad="44"/>
<connect gate=".POWER" pin="3V3_USB" pad="34"/>
<connect gate=".POWER" pin="CHG_EXT" pad="29"/>
<connect gate=".POWER" pin="GND" pad="1 2 3 4 11 22 27"/>
<connect gate=".POWER" pin="VBAT" pad="32"/>
<connect gate=".POWER" pin="VBAT_SENSE" pad="31"/>
<connect gate=".POWER" pin="VCHG" pad="30"/>
<connect gate=".POWER" pin="VDD_PADS" pad="33"/>
<connect gate=".POWER" pin="VREGEN" pad="28"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11659"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BLUETOOTH-RN-52">
<description>&lt;h3&gt;Roving Networks RN-52 Bluetooth Audio Module&lt;/h3&gt;
&lt;p&gt;The RN-52 is an audio module that provides a highly integrated solution for delivering high quality stereo audio in a small form factor with little difficulty. This module is perfect for a project involving hands free audio for your car, remote controlling your media center, or streaming 2-channel audio.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products&lt;/b&gt;:
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11678"&gt;RN-52 - Bluetooth Audio Module&lt;/a&gt; (WRL-11678)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12849"&gt;Audio Bluetooth Breakout - RN-52&lt;/a&gt; (WRL-12849)&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RN-52"/>
</gates>
<devices>
<device name="" package="RN-52">
<connects>
<connect gate="G$1" pin="AGND" pad="36"/>
<connect gate="G$1" pin="AIC0" pad="3"/>
<connect gate="G$1" pin="GND" pad="RFG1"/>
<connect gate="G$1" pin="GND1" pad="RFG2"/>
<connect gate="G$1" pin="GND2" pad="RFG3"/>
<connect gate="G$1" pin="GND3" pad="RFG4"/>
<connect gate="G$1" pin="GND4" pad="RFG5"/>
<connect gate="G$1" pin="GND5" pad="RFG6"/>
<connect gate="G$1" pin="GND6" pad="G4"/>
<connect gate="G$1" pin="GND7" pad="G3"/>
<connect gate="G$1" pin="GND8" pad="G2"/>
<connect gate="G$1" pin="GND9" pad="G1"/>
<connect gate="G$1" pin="GPIO10" pad="9"/>
<connect gate="G$1" pin="GPIO11" pad="8"/>
<connect gate="G$1" pin="GPIO12" pad="6"/>
<connect gate="G$1" pin="GPIO13" pad="7"/>
<connect gate="G$1" pin="GPIO2" pad="2"/>
<connect gate="G$1" pin="GPIO3" pad="1"/>
<connect gate="G$1" pin="GPIO4" pad="4"/>
<connect gate="G$1" pin="GPIO5" pad="5"/>
<connect gate="G$1" pin="GPIO6" pad="18"/>
<connect gate="G$1" pin="GPIO7" pad="17"/>
<connect gate="G$1" pin="GPIO9" pad="10"/>
<connect gate="G$1" pin="LED0" pad="30"/>
<connect gate="G$1" pin="LED1" pad="29"/>
<connect gate="G$1" pin="MIC_BIAS" pad="31"/>
<connect gate="G$1" pin="MIC_L+" pad="32"/>
<connect gate="G$1" pin="MIC_L-" pad="34"/>
<connect gate="G$1" pin="MIC_R+" pad="33"/>
<connect gate="G$1" pin="MIC_R-" pad="35"/>
<connect gate="G$1" pin="PCM_CLK" pad="24"/>
<connect gate="G$1" pin="PCM_IN" pad="21"/>
<connect gate="G$1" pin="PCM_OUT" pad="22"/>
<connect gate="G$1" pin="PCM_SYNC" pad="23"/>
<connect gate="G$1" pin="PWREN" pad="19"/>
<connect gate="G$1" pin="SPI_CLK" pad="27"/>
<connect gate="G$1" pin="SPI_MISO" pad="26"/>
<connect gate="G$1" pin="SPI_MOSI" pad="28"/>
<connect gate="G$1" pin="SPI_SS" pad="25"/>
<connect gate="G$1" pin="SPKR_L+" pad="40"/>
<connect gate="G$1" pin="SPKR_L-" pad="38"/>
<connect gate="G$1" pin="SPKR_R+" pad="39"/>
<connect gate="G$1" pin="SPKR_R-" pad="37"/>
<connect gate="G$1" pin="UART_CTS" pad="14"/>
<connect gate="G$1" pin="UART_RTS" pad="13"/>
<connect gate="G$1" pin="UART_RX" pad="16"/>
<connect gate="G$1" pin="UART_TX" pad="15"/>
<connect gate="G$1" pin="USBD+" pad="12"/>
<connect gate="G$1" pin="USBD-" pad="11"/>
<connect gate="G$1" pin="VDD" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11569"/>
<attribute name="SF_ID" value="WRL-11678"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CC3000">
<description>&lt;h3&gt;Texas Instruments CC3000 WiFi Module&lt;/h3&gt;
&lt;p&gt;The CC3000 from TI (Texas Instruments) is a self-contained wireless network processor that makes incorporating internet connectivity into your project simple. Instead of the more standard UART communication method, the CC3000 module utilizes an SPI interface allowing you, the user, to control the flow of data as you please.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12820"&gt;WiFi SMD Module - CC3000&lt;/a&gt; (WRL-12820)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12072"&gt;SparkFun WiFi Breakout - CC3000&lt;/a&gt; (WRL-12072)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12071"&gt;SparkFun WiFi Shield - CC3000&lt;/a&gt; (WRL-12071)&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CC3000"/>
</gates>
<devices>
<device name="" package="QFN-46-13.5X16.3MM">
<connects>
<connect gate="G$1" pin="EXT_32K" pad="P$21"/>
<connect gate="G$1" pin="GND@1" pad="P$1"/>
<connect gate="G$1" pin="GND@10" pad="P$10"/>
<connect gate="G$1" pin="GND@11" pad="P$11"/>
<connect gate="G$1" pin="GND@16" pad="P$16"/>
<connect gate="G$1" pin="GND@18" pad="P$18"/>
<connect gate="G$1" pin="GND@20" pad="P$20"/>
<connect gate="G$1" pin="GND@22" pad="P$22"/>
<connect gate="G$1" pin="GND@25" pad="P$25"/>
<connect gate="G$1" pin="GND@31" pad="P$31"/>
<connect gate="G$1" pin="GND@32" pad="P$32"/>
<connect gate="G$1" pin="GND@33" pad="P$33"/>
<connect gate="G$1" pin="GND@34" pad="P$34"/>
<connect gate="G$1" pin="GND@36" pad="P$36"/>
<connect gate="G$1" pin="GND@37" pad="GND@37"/>
<connect gate="G$1" pin="GND@38" pad="GND@38"/>
<connect gate="G$1" pin="GND@39" pad="GND@39"/>
<connect gate="G$1" pin="GND@40" pad="GND@40"/>
<connect gate="G$1" pin="GND@41" pad="GND@41"/>
<connect gate="G$1" pin="GND@42" pad="GND@42"/>
<connect gate="G$1" pin="GND@43" pad="GND@43"/>
<connect gate="G$1" pin="GND@44" pad="GND@44"/>
<connect gate="G$1" pin="GND@45" pad="GND@45"/>
<connect gate="G$1" pin="GND@46" pad="GND@46"/>
<connect gate="G$1" pin="GND@9" pad="P$9"/>
<connect gate="G$1" pin="NC" pad="P$3"/>
<connect gate="G$1" pin="RESERVED_1" pad="P$2"/>
<connect gate="G$1" pin="RESERVED_2" pad="P$4"/>
<connect gate="G$1" pin="RESERVED_3" pad="P$24"/>
<connect gate="G$1" pin="RF_ANT" pad="P$35"/>
<connect gate="G$1" pin="SCL_CC3000" pad="P$30"/>
<connect gate="G$1" pin="SCL_EEPROM" pad="P$29"/>
<connect gate="G$1" pin="SDA_CC3000" pad="P$28"/>
<connect gate="G$1" pin="SDA_EEPROM" pad="P$27"/>
<connect gate="G$1" pin="SPI_CLK" pad="P$17"/>
<connect gate="G$1" pin="SPI_CS" pad="P$12"/>
<connect gate="G$1" pin="SPI_DIN" pad="P$15"/>
<connect gate="G$1" pin="SPI_DOUT" pad="P$13"/>
<connect gate="G$1" pin="SPI_IRQ" pad="P$14"/>
<connect gate="G$1" pin="VBAT_IN" pad="P$19"/>
<connect gate="G$1" pin="VBAT_SW_EN" pad="P$26"/>
<connect gate="G$1" pin="VIO_HOST" pad="P$23"/>
<connect gate="G$1" pin="WL_EN1" pad="P$7"/>
<connect gate="G$1" pin="WL_EN2" pad="P$5"/>
<connect gate="G$1" pin="WL_RS232_RX" pad="P$8"/>
<connect gate="G$1" pin="WL_RS232_TX" pad="P$6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-12643"/>
<attribute name="SF_ID" value="WRL-13444"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RFM69H" prefix="U">
<description>&lt;h3&gt;Hope RF RFM69H ISM Transceiver Module&lt;/h3&gt; 
&lt;p&gt;The RFM69H is a transceiver module capable of operation over a wide frequency range, including the 315,433,868 and 915MHz license-free ISM (Industry Scientific and Medical) frequency bands. All major RF communication parameters are programmable and most of them  can  be  dynamically set.  The  RFM69H  offers  the unique advantage of programmable narrow-band and wide- band  communication modes. The RFM69H is optimized for low power consumption while offering high RF output power and channelized operation.Compliance  ETSI and FCC regulations. &lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.hoperf.cn/upload/docs/RF/SX/RFM69H_DataSheet_v1.3.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13909"&gt;RFM69HCW Wireless Transceiver - 915MHz&lt;/a&gt; (COM-13909)&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13910"&gt;RFM69HCW Wireless Transceiver - 434MHz&lt;/a&gt; (COM-13910)&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12775"&gt;SparkFun RFM69 Breakout (915MHz)&lt;/a&gt; (WRL-12775)&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12823"&gt;SparkFun RFM69 Breakout (434MHz)&lt;/a&gt; (WRL-12823)&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="U1" symbol="RFM69H"/>
</gates>
<devices>
<device name="CW-915" package="RFM69HCW-XXXS2">
<connects>
<connect gate="U1" pin="!CS" pad="5"/>
<connect gate="U1" pin="ANT" pad="9"/>
<connect gate="U1" pin="GND" pad="1 8 10"/>
<connect gate="U1" pin="IO0/INT" pad="14"/>
<connect gate="U1" pin="IO1" pad="15"/>
<connect gate="U1" pin="IO2" pad="16"/>
<connect gate="U1" pin="IO3" pad="11"/>
<connect gate="U1" pin="IO4" pad="12"/>
<connect gate="U1" pin="IO5" pad="7"/>
<connect gate="U1" pin="MISO" pad="2"/>
<connect gate="U1" pin="MOSI" pad="3"/>
<connect gate="U1" pin="RST" pad="6"/>
<connect gate="U1" pin="SCK" pad="4"/>
<connect gate="U1" pin="VCC" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11997"/>
<attribute name="VALUE" value="915MHz"/>
</technology>
</technologies>
</device>
<device name="W" package="RFM69W-XXXS2">
<connects>
<connect gate="U1" pin="!CS" pad="15"/>
<connect gate="U1" pin="ANT" pad="10"/>
<connect gate="U1" pin="GND" pad="9 11"/>
<connect gate="U1" pin="IO0/INT" pad="2"/>
<connect gate="U1" pin="IO1" pad="3"/>
<connect gate="U1" pin="IO2" pad="4"/>
<connect gate="U1" pin="IO3" pad="5"/>
<connect gate="U1" pin="IO4" pad="6"/>
<connect gate="U1" pin="IO5" pad="7"/>
<connect gate="U1" pin="MISO" pad="13"/>
<connect gate="U1" pin="MOSI" pad="14"/>
<connect gate="U1" pin="RST" pad="1"/>
<connect gate="U1" pin="SCK" pad="12"/>
<connect gate="U1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CW-433" package="RFM69HCW-XXXS2">
<connects>
<connect gate="U1" pin="!CS" pad="5"/>
<connect gate="U1" pin="ANT" pad="9"/>
<connect gate="U1" pin="GND" pad="1 8 10"/>
<connect gate="U1" pin="IO0/INT" pad="14"/>
<connect gate="U1" pin="IO1" pad="15"/>
<connect gate="U1" pin="IO2" pad="16"/>
<connect gate="U1" pin="IO3" pad="11"/>
<connect gate="U1" pin="IO4" pad="12"/>
<connect gate="U1" pin="IO5" pad="7"/>
<connect gate="U1" pin="MISO" pad="2"/>
<connect gate="U1" pin="MOSI" pad="3"/>
<connect gate="U1" pin="RST" pad="6"/>
<connect gate="U1" pin="SCK" pad="4"/>
<connect gate="U1" pin="VCC" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-12053"/>
<attribute name="VALUE" value="433MHz"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RFM69" prefix="U">
<description>&lt;h3&gt;Hope RF RFM69CW ISM Transceiver Module&lt;/h3&gt; 
&lt;p&gt;The RFM69CW radio module by HopeRF is a compact, powerful radio transceiver module for swapping data packets in the 868 MHz ISM band, using standard and enhanced FSK modulation. The radio is great for sub-compact designs; just 4mm of mounted height from using an SMD precision crystal.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.hoperf.com/upload/rf/RFM69CW-V1.1.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RFM69"/>
</gates>
<devices>
<device name="CW-915MHZ" package="RFM69CW-XXXS2">
<connects>
<connect gate="G$1" pin="3.3V" pad="2"/>
<connect gate="G$1" pin="ANT" pad="1"/>
<connect gate="G$1" pin="DIO0" pad="9"/>
<connect gate="G$1" pin="DIO1" pad="11"/>
<connect gate="G$1" pin="DIO2" pad="10"/>
<connect gate="G$1" pin="DIO3" pad="4"/>
<connect gate="G$1" pin="DIO5" pad="12"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="14"/>
<connect gate="G$1" pin="MISO" pad="8"/>
<connect gate="G$1" pin="MOSI" pad="5"/>
<connect gate="G$1" pin="NSS" pad="7"/>
<connect gate="G$1" pin="RESET" pad="13"/>
<connect gate="G$1" pin="SCK" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11996"/>
<attribute name="VALUE" value="915MHz"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BC118" prefix="U" uservalue="yes">
<description>&lt;h3&gt;Blue Creation BC118 Bluetooth 4.0 Audio Module&lt;/h3&gt;
&lt;p&gt;BC118 consists of a Bluetooth Smart (Bluetooth 4.0) radio, a microprocessor running an embedded protocol stack. The
module is controlled by high level UART instructions or GPIOs. B118 supports UART and I2C Transparent mode for
cable replacement, standard/custom profiles, central and peripheral modes. It can connect to any Android, iOS or
Windows Mobile Smartphone that is Bluetooth smart capable. The firmware can be upgraded using an App provided by
BlueCreation. BC118 can run standalone, with a host processor or controlled by an App.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://media.digikey.com/pdf/Data%20Sheets/BlueCreation%20PDFs/BC118_DS.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products&lt;/b&gt;:
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13019"&gt;BLE Mate 2&lt;/a&gt; (WRL-13019)
&lt;/li&gt;&lt;/ul&gt;</description>
<gates>
<gate name="G1" symbol="BC118_POWER"/>
<gate name="G2" symbol="BC118_PIO"/>
<gate name="G3" symbol="BC118_COMMS"/>
</gates>
<devices>
<device name="" package="BC118">
<connects>
<connect gate="G1" pin="GND" pad="1 2 12 13 15 16 18 23 24 31 32 33 34 35"/>
<connect gate="G1" pin="VBAT" pad="27"/>
<connect gate="G1" pin="VDD" pad="17"/>
<connect gate="G1" pin="WAKE" pad="30"/>
<connect gate="G2" pin="AIO_0" pad="5"/>
<connect gate="G2" pin="AIO_1" pad="4"/>
<connect gate="G2" pin="AIO_2" pad="3"/>
<connect gate="G2" pin="PIO_10" pad="28"/>
<connect gate="G2" pin="PIO_11" pad="29"/>
<connect gate="G2" pin="PIO_2" pad="21"/>
<connect gate="G2" pin="PIO_3" pad="8"/>
<connect gate="G2" pin="PIO_4" pad="9"/>
<connect gate="G2" pin="PIO_5/SPI_CLK" pad="10"/>
<connect gate="G2" pin="PIO_6/SPI_CSB" pad="11"/>
<connect gate="G2" pin="PIO_7/SPI_MOSI" pad="14"/>
<connect gate="G2" pin="PIO_8/SPI_MISO" pad="19"/>
<connect gate="G2" pin="PIO_9" pad="26"/>
<connect gate="G2" pin="SPI/!PCM" pad="20"/>
<connect gate="G3" pin="I2C_SCL" pad="22"/>
<connect gate="G3" pin="I2C_SDA" pad="25"/>
<connect gate="G3" pin="UART_RX" pad="7"/>
<connect gate="G3" pin="UART_TX" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="WRL-12203"/>
<attribute name="VALUE" value="BC118"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XBEE" prefix="JP" uservalue="yes">
<description>&lt;h3&gt;Digi XBee and XBee Pro&lt;/h3&gt;
&lt;p&gt;XBees are tiny blue chips that can communicate wirelessly with each other. They can do simple things, like replacing a couple of wires in serial communication, which is nice when you want to make a remote for your paintball vehicle.&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/pages/xbee_guide"&gt;SparkFun XBee Buying Guide&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11812"&gt;SparkFun XBee Explorer USB&lt;/a&gt; (WRL-11812)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8276"&gt;Breakout Board for XBee Module&lt;/a&gt; (WRL-8276)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11373"&gt;SparkFun XBee Explorer Regulated&lt;/a&gt; (WRL-11373)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11697"&gt;SparkFun XBee Explorer Dongle&lt;/a&gt; (WRL-11697)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12847"&gt;SparkFun XBee Shield&lt;/a&gt; (WRL-12847)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13225"&gt;SparkFun XBee Explorer Serial&lt;/a&gt; (WRL-13225)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="XBEE"/>
</gates>
<devices>
<device name="SILK" package="XBEE-SILK">
<connects>
<connect gate="G$1" pin="CTS" pad="12"/>
<connect gate="G$1" pin="DIN" pad="3"/>
<connect gate="G$1" pin="DIO0" pad="20"/>
<connect gate="G$1" pin="DIO1" pad="19"/>
<connect gate="G$1" pin="DIO11" pad="7"/>
<connect gate="G$1" pin="DIO12" pad="4"/>
<connect gate="G$1" pin="DIO2" pad="18"/>
<connect gate="G$1" pin="DIO3" pad="17"/>
<connect gate="G$1" pin="DIO4" pad="11"/>
<connect gate="G$1" pin="DIO5" pad="15"/>
<connect gate="G$1" pin="DIO9" pad="13"/>
<connect gate="G$1" pin="DOUT" pad="2"/>
<connect gate="G$1" pin="DTR" pad="9"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="RES@14" pad="14"/>
<connect gate="G$1" pin="RES@8" pad="8"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="RSSI" pad="6"/>
<connect gate="G$1" pin="RTS" pad="16"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="XBEE-SMD">
<connects>
<connect gate="G$1" pin="CTS" pad="12"/>
<connect gate="G$1" pin="DIN" pad="3"/>
<connect gate="G$1" pin="DIO0" pad="20"/>
<connect gate="G$1" pin="DIO1" pad="19"/>
<connect gate="G$1" pin="DIO11" pad="7"/>
<connect gate="G$1" pin="DIO12" pad="4"/>
<connect gate="G$1" pin="DIO2" pad="18"/>
<connect gate="G$1" pin="DIO3" pad="17"/>
<connect gate="G$1" pin="DIO4" pad="11"/>
<connect gate="G$1" pin="DIO5" pad="15"/>
<connect gate="G$1" pin="DIO9" pad="13"/>
<connect gate="G$1" pin="DOUT" pad="2"/>
<connect gate="G$1" pin="DTR" pad="9"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="RES@14" pad="14"/>
<connect gate="G$1" pin="RES@8" pad="8"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="RSSI" pad="6"/>
<connect gate="G$1" pin="RTS" pad="16"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09042"/>
</technology>
</technologies>
</device>
<device name="LONGPAD" package="XBEE-LONGPAD">
<connects>
<connect gate="G$1" pin="CTS" pad="12"/>
<connect gate="G$1" pin="DIN" pad="3"/>
<connect gate="G$1" pin="DIO0" pad="20"/>
<connect gate="G$1" pin="DIO1" pad="19"/>
<connect gate="G$1" pin="DIO11" pad="7"/>
<connect gate="G$1" pin="DIO12" pad="4"/>
<connect gate="G$1" pin="DIO2" pad="18"/>
<connect gate="G$1" pin="DIO3" pad="17"/>
<connect gate="G$1" pin="DIO4" pad="11"/>
<connect gate="G$1" pin="DIO5" pad="15"/>
<connect gate="G$1" pin="DIO9" pad="13"/>
<connect gate="G$1" pin="DOUT" pad="2"/>
<connect gate="G$1" pin="DTR" pad="9"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="RES@14" pad="14"/>
<connect gate="G$1" pin="RES@8" pad="8"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="RSSI" pad="6"/>
<connect gate="G$1" pin="RTS" pad="16"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="XBEE-LOCK">
<connects>
<connect gate="G$1" pin="CTS" pad="12"/>
<connect gate="G$1" pin="DIN" pad="3"/>
<connect gate="G$1" pin="DIO0" pad="20"/>
<connect gate="G$1" pin="DIO1" pad="19"/>
<connect gate="G$1" pin="DIO11" pad="7"/>
<connect gate="G$1" pin="DIO12" pad="4"/>
<connect gate="G$1" pin="DIO2" pad="18"/>
<connect gate="G$1" pin="DIO3" pad="17"/>
<connect gate="G$1" pin="DIO4" pad="11"/>
<connect gate="G$1" pin="DIO5" pad="15"/>
<connect gate="G$1" pin="DIO9" pad="13"/>
<connect gate="G$1" pin="DOUT" pad="2"/>
<connect gate="G$1" pin="DTR" pad="9"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="RES@14" pad="14"/>
<connect gate="G$1" pin="RES@8" pad="8"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="RSSI" pad="6"/>
<connect gate="G$1" pin="RTS" pad="16"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="XBEE">
<connects>
<connect gate="G$1" pin="CTS" pad="12"/>
<connect gate="G$1" pin="DIN" pad="3"/>
<connect gate="G$1" pin="DIO0" pad="20"/>
<connect gate="G$1" pin="DIO1" pad="19"/>
<connect gate="G$1" pin="DIO11" pad="7"/>
<connect gate="G$1" pin="DIO12" pad="4"/>
<connect gate="G$1" pin="DIO2" pad="18"/>
<connect gate="G$1" pin="DIO3" pad="17"/>
<connect gate="G$1" pin="DIO4" pad="11"/>
<connect gate="G$1" pin="DIO5" pad="15"/>
<connect gate="G$1" pin="DIO9" pad="13"/>
<connect gate="G$1" pin="DOUT" pad="2"/>
<connect gate="G$1" pin="DTR" pad="9"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="RES@14" pad="14"/>
<connect gate="G$1" pin="RES@8" pad="8"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="RSSI" pad="6"/>
<connect gate="G$1" pin="RTS" pad="16"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ESP8266" prefix="U">
<description>&lt;h3&gt;Espressif ESP8266 WiFi/Microcontroller SoC&lt;/h3&gt;
&lt;p&gt;The ESP8266 WiFi Module is a self contained SOC with integrated TCP/IP protocol stack that can give any microcontroller access to your WiFi network. The ESP8266 is capable of either hosting an application or offloading all Wi-Fi networking functions from another application processor.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13678"&gt;WiFi Module ESP8266&lt;/a&gt; (WRL-13678)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13231"&gt;SparkFun ESP8266 Thing&lt;/a&gt; (WRL-13231)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13287"&gt;SparkFun WiFi Shield - ESP8266&lt;/a&gt; (WRL-13287)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13711"&gt;SparkFun ESP8266 Thing - Dev Board&lt;/a&gt; (WRL-13711)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13794"&gt;SparkFun Blynk Board - ESP8266&lt;/a&gt; (WRL-13794)&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ESP8266"/>
</gates>
<devices>
<device name="" package="QFN32-5X5MM">
<connects>
<connect gate="G$1" pin="CHIP_EN" pad="7"/>
<connect gate="G$1" pin="EXT_RSTB" pad="32"/>
<connect gate="G$1" pin="GND" pad="EP"/>
<connect gate="G$1" pin="GPIO2" pad="14"/>
<connect gate="G$1" pin="GPIO4" pad="16"/>
<connect gate="G$1" pin="GPIO5" pad="24"/>
<connect gate="G$1" pin="LNA" pad="2"/>
<connect gate="G$1" pin="MTCK/SPID/GPIO13" pad="12"/>
<connect gate="G$1" pin="MTDI/SPIQ/GPIO12" pad="10"/>
<connect gate="G$1" pin="MTDO/SPICS/GPIO15" pad="13"/>
<connect gate="G$1" pin="MTMS/SPICLK/GPIO14" pad="9"/>
<connect gate="G$1" pin="RES12K" pad="31"/>
<connect gate="G$1" pin="SPICLK/SD_CLK" pad="21"/>
<connect gate="G$1" pin="SPICS0/SD_CMD" pad="20"/>
<connect gate="G$1" pin="SPICS2/GPIO0" pad="15"/>
<connect gate="G$1" pin="SPID/SD_DATA_1" pad="23"/>
<connect gate="G$1" pin="SPIHD/SD_DATA_2" pad="18"/>
<connect gate="G$1" pin="SPIQ/SD_DATA_0" pad="22"/>
<connect gate="G$1" pin="SPIWP/SD_DATA_3" pad="19"/>
<connect gate="G$1" pin="TOUT/ADC" pad="6"/>
<connect gate="G$1" pin="U0RXD" pad="25"/>
<connect gate="G$1" pin="U0TXD" pad="26"/>
<connect gate="G$1" pin="VDD3P3@3" pad="3"/>
<connect gate="G$1" pin="VDD3P3@4" pad="4"/>
<connect gate="G$1" pin="VDDA@1" pad="1"/>
<connect gate="G$1" pin="VDDA@30" pad="30"/>
<connect gate="G$1" pin="VDDD" pad="29"/>
<connect gate="G$1" pin="VDDPST@11" pad="11"/>
<connect gate="G$1" pin="VDDPST@17" pad="17"/>
<connect gate="G$1" pin="VDD_RTC" pad="5"/>
<connect gate="G$1" pin="XPD_DCDC/GPIO16" pad="8"/>
<connect gate="G$1" pin="XTAL_IN" pad="28"/>
<connect gate="G$1" pin="XTAL_OUT" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-12452"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ANTENNA-GROUNDED" prefix="E">
<description>&lt;h3&gt;Antenna w/ Ground Connection&lt;/h3&gt;
&lt;p&gt;2.4GHz antennae with signal and ground terminals.&lt;/p&gt;
&lt;p&gt;&lt;ul&gt;
&lt;li&gt;&lt;b&gt;TRACE_ANTENNA_2.4GHZ_15.2MM&lt;/b&gt; - Meander Trace antenna
&lt;ul&gt;&lt;li&gt;15.2 x 5.7mm footprint&lt;/li&gt;
&lt;li&gt;Based on layout from &lt;a href="http://www.ti.com/lit/an/swra117d/swra117d.pdf"&gt;TI app note AN043&lt;/a&gt;.&lt;/li&gt;&lt;/ul&gt;
&lt;/li&gt;
&lt;li&gt;&lt;b&gt;TRACE_ANTENNA_2.4GHZ_25.7MM&lt;/b&gt; - Inverted F trace antenna
&lt;ul&gt;&lt;li&gt;25.7 x 7.5 mm footprint.&lt;/li&gt;
&lt;li&gt;Based on layout from &lt;a href="http://www.ti.com/lit/an/swru120b/swru120b.pdf"&gt;TI design note DN0007&lt;/a&gt;.&lt;/li&gt;&lt;/ul&gt;
&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ANTENNA-GROUNDED"/>
</gates>
<devices>
<device name="TRACE-25.7MM" package="TRACE_ANTENNA_2.4GHZ_25.7MM">
<connects>
<connect gate="G$1" pin="GND" pad="GND GND2"/>
<connect gate="G$1" pin="SIGNAL" pad="ANT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TRACE-15.2MM" package="TRACE_ANTENNA_2.4GHZ_15.2MM">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="SIGNAL" pad="ANT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EDGE_SMA" package="SMA-EDGE">
<connects>
<connect gate="G$1" pin="GND" pad="GND@0 GND@1 GND@2 GND@3"/>
<connect gate="G$1" pin="SIGNAL" pad="SIG"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ESP32" prefix="U">
<description>&lt;h3&gt;Espressif ESP32&lt;/h3&gt;
&lt;p&gt;
&lt;li&gt;WiFi-compatible SoC microcontroller.&lt;/li&gt;
&lt;li&gt; Bluetooth Low energy support (BLE, BT4.0, Bluetooth Smart)&lt;/li&gt;
&lt;li&gt;28 GPIO pins&lt;/li&gt;
&lt;li&gt;Dual-core Tensilica LX6 microprocessor&lt;/li&gt;
&lt;li&gt;Hardware accelerated encryption (AES, SHA2, ECC, RSA-4096)&lt;/li&gt;
&lt;li&gt;4MB Flash memory&lt;/li&gt;
&lt;li&gt;520kB internal SRAM&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://cdn.sparkfun.com/datasheets/IoT/esp32_datasheet_en.pdf”&gt;Datasheet&lt;/a&gt;&lt;/li&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href='https://www.sparkfun.com/products/13907'&gt;SparkFun ESP32 Thing&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ESP32"/>
</gates>
<devices>
<device name="" package="QFN48-0.4MM">
<connects>
<connect gate="G$1" pin="(ADC2:0/TOUCH0/RTC10/SPIHD)GPIO4" pad="24"/>
<connect gate="G$1" pin="(ADC2:1/TOUCH1/RTC11/CLK_OUT1)GPIO0" pad="23"/>
<connect gate="G$1" pin="(ADC2:2/TOUCH2/RTC12/SPIWP)GPIO2" pad="22"/>
<connect gate="G$1" pin="(ADC2:7/TOUCH7/RTC17)GPIO27" pad="16"/>
<connect gate="G$1" pin="(DAC1/ADC2:8/RTC6)GPIO25" pad="14"/>
<connect gate="G$1" pin="(DAC2/ADC2:9/RTC7)GPIO26" pad="15"/>
<connect gate="G$1" pin="(GPIO1/CLK_OUT3/HS2_DATA1)U0TXD" pad="41"/>
<connect gate="G$1" pin="(GPIO10/SPIWP/HS1_DATA3/U1TX)SD_DATA3" pad="29"/>
<connect gate="G$1" pin="(GPIO11/SPICSO/HS1_CMD/U1RTS)SD_CMD" pad="30"/>
<connect gate="G$1" pin="(GPIO12/ADC2:5/TOUCH5/RTC15/SPIQ)MTDI" pad="18"/>
<connect gate="G$1" pin="(GPIO13/ADC2:4/TOUCH4/RTC14/SPID/U0CTS)MTCK" pad="20"/>
<connect gate="G$1" pin="(GPIO14/ADC2:6/TOUCH6/RTC16/SPICLK)MTMS" pad="17"/>
<connect gate="G$1" pin="(GPIO15/ADC2:3/TOUCH3/RTC13/SPICSO/U0RTS)MTDO" pad="21"/>
<connect gate="G$1" pin="(GPIO3/CLK_OUT2/HS2_DATA0)U0RXD" pad="40"/>
<connect gate="G$1" pin="(GPIO6/SPICLK/HS1_CLK/U1CTS)SD_CLK" pad="31"/>
<connect gate="G$1" pin="(GPIO7/SPI1/HS1_DATA0)SD_DATA0" pad="32"/>
<connect gate="G$1" pin="(GPIO8/SPID/HS1_DATA1)SD_DATA1" pad="33"/>
<connect gate="G$1" pin="(GPIO9/SPIHD/HS1_DATA2/U1RX)SD_DATA2" pad="28"/>
<connect gate="G$1" pin="(HS1_DATA4)GPIO16" pad="25"/>
<connect gate="G$1" pin="(HS1_DATA5)GPIO17" pad="27"/>
<connect gate="G$1" pin="(VSPICLK/HS1_DATA7)GPIO18" pad="35"/>
<connect gate="G$1" pin="(VSPICS0/HS1_DATA6)GPIO5" pad="34"/>
<connect gate="G$1" pin="(VSPIHD/HS2_CMD)GPIO21" pad="42"/>
<connect gate="G$1" pin="(VSPIQ/HS2_DATA2)GPIO19" pad="38"/>
<connect gate="G$1" pin="(VSPIWP/HS2_CLK)GPIO22" pad="39"/>
<connect gate="G$1" pin="32K_XN(GPIO33/ADC1:5/TOUCH8/RTC8)" pad="13"/>
<connect gate="G$1" pin="32K_XP(GPIO32/ADC1:4/TOUCH9/RTC9)" pad="12"/>
<connect gate="G$1" pin="CAP1" pad="48"/>
<connect gate="G$1" pin="CAP2" pad="47"/>
<connect gate="G$1" pin="CHIP_PU" pad="9"/>
<connect gate="G$1" pin="GND" pad="EP"/>
<connect gate="G$1" pin="GPIO23" pad="36"/>
<connect gate="G$1" pin="LNA_IN" pad="2"/>
<connect gate="G$1" pin="SENSOR_CAPN(GPI38/ADC1:2/RTC2)" pad="7"/>
<connect gate="G$1" pin="SENSOR_CAPP(GPI37/ADC1:1/RTC1)" pad="6"/>
<connect gate="G$1" pin="SENSOR_VN(GPI39/ADC1:3/RTC3)" pad="8"/>
<connect gate="G$1" pin="SENSOR_VP(GPI36/ADC1:0/RTC0)" pad="5"/>
<connect gate="G$1" pin="VDD3P3_CPU" pad="37"/>
<connect gate="G$1" pin="VDD3P3_RTC" pad="19"/>
<connect gate="G$1" pin="VDD3P3_SDIO" pad="26"/>
<connect gate="G$1" pin="VDDA" pad="1 43 46"/>
<connect gate="G$1" pin="VDDA3P3" pad="3 4"/>
<connect gate="G$1" pin="VDET_1(GPI34/ADC1:6)" pad="10"/>
<connect gate="G$1" pin="VDET_2(GPI35/ADC1:7)" pad="11"/>
<connect gate="G$1" pin="XTAL_N" pad="44"/>
<connect gate="G$1" pin="XTAL_P" pad="45"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-13338"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NRF52832" prefix="U">
<description>&lt;h3&gt;Nordic nRF52832 Bluetooth Smart/ANT/2.4GHz RF SoC&lt;/h3&gt;
&lt;p&gt;The nRF52832 SoC is a powerful, highly flexible ultra-low power multiprotocol SoC ideally suited for Bluetooth® Smart ANT and 2.4GHz ultra low-power wireless applications.
&lt;br&gt;The nRF52832 SoC is built around a 32-bit ARM® Cortex™-M4F CPU with 512kB + 64kB RAM. The embedded 2.4GHz transceiver supports Bluetooth Smart, ANT and proprietary 2.4 GHz protocol stack. 
&lt;br&gt;It is on air compatible with the nRF51 Series, nRF24L and nRF24AP Series products from Nordic Semiconductor.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Wireless/Bluetooth/nRF52832_PS_v1.0.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13990”&gt;SparkFun nRF52832 Breakout&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="NRF52832"/>
</gates>
<devices>
<device name="" package="QFN48-6X6MM">
<connects>
<connect gate="G$1" pin="ANT" pad="30"/>
<connect gate="G$1" pin="DCC" pad="47"/>
<connect gate="G$1" pin="DEC1" pad="1"/>
<connect gate="G$1" pin="DEC2" pad="32"/>
<connect gate="G$1" pin="DEC3" pad="33"/>
<connect gate="G$1" pin="DEC4" pad="46"/>
<connect gate="G$1" pin="NC" pad="44"/>
<connect gate="G$1" pin="P0.00/XL1" pad="2"/>
<connect gate="G$1" pin="P0.01/XL2" pad="3"/>
<connect gate="G$1" pin="P0.02/AIN0" pad="4"/>
<connect gate="G$1" pin="P0.03/AIN1" pad="5"/>
<connect gate="G$1" pin="P0.04/AIN2" pad="6"/>
<connect gate="G$1" pin="P0.05/AIN3" pad="7"/>
<connect gate="G$1" pin="P0.06" pad="8"/>
<connect gate="G$1" pin="P0.07" pad="9"/>
<connect gate="G$1" pin="P0.08" pad="10"/>
<connect gate="G$1" pin="P0.09/NFC1" pad="11"/>
<connect gate="G$1" pin="P0.10/NFC2" pad="12"/>
<connect gate="G$1" pin="P0.11" pad="14"/>
<connect gate="G$1" pin="P0.12" pad="15"/>
<connect gate="G$1" pin="P0.13" pad="16"/>
<connect gate="G$1" pin="P0.14" pad="17"/>
<connect gate="G$1" pin="P0.15" pad="18"/>
<connect gate="G$1" pin="P0.16" pad="19"/>
<connect gate="G$1" pin="P0.17" pad="20"/>
<connect gate="G$1" pin="P0.18" pad="21"/>
<connect gate="G$1" pin="P0.19" pad="22"/>
<connect gate="G$1" pin="P0.20" pad="23"/>
<connect gate="G$1" pin="P0.21/RESET" pad="24"/>
<connect gate="G$1" pin="P0.22" pad="27"/>
<connect gate="G$1" pin="P0.23" pad="28"/>
<connect gate="G$1" pin="P0.24" pad="29"/>
<connect gate="G$1" pin="P0.25" pad="37"/>
<connect gate="G$1" pin="P0.26" pad="38"/>
<connect gate="G$1" pin="P0.27" pad="39"/>
<connect gate="G$1" pin="P0.28/AIN4" pad="40"/>
<connect gate="G$1" pin="P0.29/AIN5" pad="41"/>
<connect gate="G$1" pin="P0.30/AIN6" pad="42"/>
<connect gate="G$1" pin="P0.31/AIN7" pad="43"/>
<connect gate="G$1" pin="SWDCLK" pad="25"/>
<connect gate="G$1" pin="SWDIO" pad="26"/>
<connect gate="G$1" pin="VDD" pad="13 36 48"/>
<connect gate="G$1" pin="VSS" pad="31 45 EP"/>
<connect gate="G$1" pin="XC1(32MHZ)" pad="34"/>
<connect gate="G$1" pin="XC2(32MHZ)" pad="35"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-13460"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RFD77101" prefix="U">
<description>&lt;p&gt;&lt;strong&gt;Simblee  BLE Module RFD77101&lt;/strong&gt;&lt;/p&gt;
&lt;p&gt;© 2015 RF Digital Corporation&lt;br/&gt; 
&lt;a href="https://cdn.sparkfun.com/datasheets/IoT/Simblee%20RFD77101%20Datasheet%20v1.0.pdf"&gt;Datasheet&lt;/a&gt;&lt;br/&gt;
PATENTS PENDING 04.01.2015
&lt;br&gt;
&lt;br&gt;
Bluetooth Smart radio transceiver, ARM Cortex M0 microcontroller.
&lt;br&gt; 128kB Flash, 24kB RAM, no EEPROM
&lt;br&gt; Arduino-compatible. 

&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13808”&gt;Simblee BLE Module - RFD77101&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13632”&gt;SparkFun Simblee BLE Breakout - RFD77101&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RFD77101"/>
</gates>
<devices>
<device name="" package="RFD77101">
<connects>
<connect gate="G$1" pin="!RESET!" pad="8"/>
<connect gate="G$1" pin="DNC@10" pad="10"/>
<connect gate="G$1" pin="DNC@3" pad="3"/>
<connect gate="G$1" pin="DNC@5" pad="5"/>
<connect gate="G$1" pin="FACTORY" pad="9"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@19" pad="19"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@30" pad="30"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="GND@42" pad="42"/>
<connect gate="G$1" pin="GND@43" pad="43"/>
<connect gate="G$1" pin="GND@44" pad="44"/>
<connect gate="G$1" pin="GND@45" pad="45"/>
<connect gate="G$1" pin="GND@6" pad="6"/>
<connect gate="G$1" pin="P0.00/AREF0" pad="25"/>
<connect gate="G$1" pin="P0.01/AIN2" pad="23"/>
<connect gate="G$1" pin="P0.02/AIN3" pad="24"/>
<connect gate="G$1" pin="P0.03/AIN4" pad="22"/>
<connect gate="G$1" pin="P0.04/AIN5" pad="32"/>
<connect gate="G$1" pin="P0.05/AIN6" pad="21"/>
<connect gate="G$1" pin="P0.06/AREF1/AIN7" pad="31"/>
<connect gate="G$1" pin="P0.07" pad="26"/>
<connect gate="G$1" pin="P0.08" pad="20"/>
<connect gate="G$1" pin="P0.09" pad="18"/>
<connect gate="G$1" pin="P0.10" pad="27"/>
<connect gate="G$1" pin="P0.11" pad="17"/>
<connect gate="G$1" pin="P0.12" pad="16"/>
<connect gate="G$1" pin="P0.13" pad="28"/>
<connect gate="G$1" pin="P0.14" pad="29"/>
<connect gate="G$1" pin="P0.15" pad="15"/>
<connect gate="G$1" pin="P0.16" pad="14"/>
<connect gate="G$1" pin="P0.17" pad="12"/>
<connect gate="G$1" pin="P0.18" pad="13"/>
<connect gate="G$1" pin="P0.19" pad="11"/>
<connect gate="G$1" pin="P0.20" pad="33"/>
<connect gate="G$1" pin="P0.21" pad="36"/>
<connect gate="G$1" pin="P0.22" pad="37"/>
<connect gate="G$1" pin="P0.23" pad="34"/>
<connect gate="G$1" pin="P0.24" pad="35"/>
<connect gate="G$1" pin="P0.25" pad="38"/>
<connect gate="G$1" pin="P0.28" pad="39"/>
<connect gate="G$1" pin="P0.29" pad="40"/>
<connect gate="G$1" pin="P0.30" pad="41"/>
<connect gate="G$1" pin="VDD" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-13237"/>
<attribute name="SF_ID" value="WRL-13808"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ESP07-16PIN">
<description>&lt;h3&gt;Espressif ESP-07S&lt;/h3&gt;
&lt;p&gt;
&lt;li&gt;WiFi-compatible SoC microcontroller.&lt;/li&gt;
&lt;li&gt;16 GPIO pins&lt;/li&gt;

&lt;li&gt;&lt;a href=”https://www.tinyosshop.com/datasheet/ESP-07S_User_Manual.pdf”&gt;User Guide&lt;/a&gt;&lt;/li&gt;&lt;/p&gt;</description>
<gates>
<gate name="A" symbol="ESP07-16PIN"/>
</gates>
<devices>
<device name="" package="ESP07">
<connects>
<connect gate="A" pin="ADC" pad="ADC"/>
<connect gate="A" pin="CH_PD" pad="CH_PD"/>
<connect gate="A" pin="GND" pad="GND"/>
<connect gate="A" pin="GPIO0" pad="GPIO0"/>
<connect gate="A" pin="GPIO12" pad="GPIO12"/>
<connect gate="A" pin="GPIO13" pad="GPIO13"/>
<connect gate="A" pin="GPIO14" pad="GPIO14"/>
<connect gate="A" pin="GPIO15" pad="GPIO15"/>
<connect gate="A" pin="GPIO16" pad="GPIO16"/>
<connect gate="A" pin="GPIO2" pad="GPIO2"/>
<connect gate="A" pin="GPIO4" pad="GPIO4"/>
<connect gate="A" pin="GPIO5" pad="GPIO5"/>
<connect gate="A" pin="RESET" pad="REST"/>
<connect gate="A" pin="RX" pad="RX"/>
<connect gate="A" pin="TX" pad="TX"/>
<connect gate="A" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-13915"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ESP-WROOM-32" prefix="U">
<gates>
<gate name="G$1" symbol="ESP-WROOM-32"/>
</gates>
<devices>
<device name="" package="ESP-WROOM-32">
<connects>
<connect gate="G$1" pin="3V3" pad="2"/>
<connect gate="G$1" pin="CS0_H/IO15" pad="23"/>
<connect gate="G$1" pin="CS0_V/IO5" pad="29"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@38" pad="38"/>
<connect gate="G$1" pin="IO0" pad="25"/>
<connect gate="G$1" pin="IO16" pad="27"/>
<connect gate="G$1" pin="IO17" pad="28"/>
<connect gate="G$1" pin="IO2" pad="24"/>
<connect gate="G$1" pin="IO21" pad="33"/>
<connect gate="G$1" pin="IO22" pad="36"/>
<connect gate="G$1" pin="IO25" pad="10"/>
<connect gate="G$1" pin="IO26" pad="11"/>
<connect gate="G$1" pin="IO27" pad="12"/>
<connect gate="G$1" pin="IO34" pad="6"/>
<connect gate="G$1" pin="IO35" pad="7"/>
<connect gate="G$1" pin="IO4" pad="26"/>
<connect gate="G$1" pin="MISO_H/IO12" pad="14"/>
<connect gate="G$1" pin="MISO_V/IO19" pad="31"/>
<connect gate="G$1" pin="MOSI_H/IO13" pad="16"/>
<connect gate="G$1" pin="MOSI_V/IO23" pad="37"/>
<connect gate="G$1" pin="NC" pad="32"/>
<connect gate="G$1" pin="RXD" pad="34"/>
<connect gate="G$1" pin="SCK/IO6" pad="20"/>
<connect gate="G$1" pin="SCK_H/IO14" pad="13"/>
<connect gate="G$1" pin="SCK_V/IO18" pad="30"/>
<connect gate="G$1" pin="SCS/IO11" pad="19"/>
<connect gate="G$1" pin="SDI/IO8" pad="22"/>
<connect gate="G$1" pin="SDO/IO7" pad="21"/>
<connect gate="G$1" pin="SENSOR_VN/I39" pad="5"/>
<connect gate="G$1" pin="SENSOR_VP/I36" pad="4"/>
<connect gate="G$1" pin="SHD/IO9" pad="17"/>
<connect gate="G$1" pin="SWP/IO10" pad="18"/>
<connect gate="G$1" pin="TXD" pad="35"/>
<connect gate="G$1" pin="XTAL_N/IO33" pad="9"/>
<connect gate="G$1" pin="XTAL_P/IO32" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-13849"/>
</technology>
</technologies>
</device>
<device name="NARROW" package="ESP-WROOM-32-NARROW">
<connects>
<connect gate="G$1" pin="3V3" pad="2"/>
<connect gate="G$1" pin="CS0_H/IO15" pad="23"/>
<connect gate="G$1" pin="CS0_V/IO5" pad="29"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@38" pad="38"/>
<connect gate="G$1" pin="IO0" pad="25"/>
<connect gate="G$1" pin="IO16" pad="27"/>
<connect gate="G$1" pin="IO17" pad="28"/>
<connect gate="G$1" pin="IO2" pad="24"/>
<connect gate="G$1" pin="IO21" pad="33"/>
<connect gate="G$1" pin="IO22" pad="36"/>
<connect gate="G$1" pin="IO25" pad="10"/>
<connect gate="G$1" pin="IO26" pad="11"/>
<connect gate="G$1" pin="IO27" pad="12"/>
<connect gate="G$1" pin="IO34" pad="6"/>
<connect gate="G$1" pin="IO35" pad="7"/>
<connect gate="G$1" pin="IO4" pad="26"/>
<connect gate="G$1" pin="MISO_H/IO12" pad="14"/>
<connect gate="G$1" pin="MISO_V/IO19" pad="31"/>
<connect gate="G$1" pin="MOSI_H/IO13" pad="16"/>
<connect gate="G$1" pin="MOSI_V/IO23" pad="37"/>
<connect gate="G$1" pin="NC" pad="32"/>
<connect gate="G$1" pin="RXD" pad="34"/>
<connect gate="G$1" pin="SCK/IO6" pad="20"/>
<connect gate="G$1" pin="SCK_H/IO14" pad="13"/>
<connect gate="G$1" pin="SCK_V/IO18" pad="30"/>
<connect gate="G$1" pin="SCS/IO11" pad="19"/>
<connect gate="G$1" pin="SDI/IO8" pad="22"/>
<connect gate="G$1" pin="SDO/IO7" pad="21"/>
<connect gate="G$1" pin="SENSOR_VN/I39" pad="5"/>
<connect gate="G$1" pin="SENSOR_VP/I36" pad="4"/>
<connect gate="G$1" pin="SHD/IO9" pad="17"/>
<connect gate="G$1" pin="SWP/IO10" pad="18"/>
<connect gate="G$1" pin="TXD" pad="35"/>
<connect gate="G$1" pin="XTAL_N/IO33" pad="9"/>
<connect gate="G$1" pin="XTAL_P/IO32" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-13849"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RFM95W" prefix="U">
<description>&lt;h3&gt;RFM95/96/97/98&lt;/h3&gt;

&lt;p&gt;The RFM95/96/97/98(W) transceivers feature the
LoRaTM    long range modem that provides ultra-long range
spread spectrum communication and high interference
immunity whilst minimising current consumption. &lt;/p&gt;

&lt;p&gt;These devices also support high performance (G)FSK
modes for systems including WMBus, IEEE802.15.4g. The
RFM95/96/97/98(W) deliver exceptional phase noise,
selectivity, receiver linearity and IIP3 for significantly
lower current consumption than competing devices&lt;/p&gt;

&lt;p&gt;&lt;a href="http://www.hoperf.com/upload/rf/RFM95_96_97_98W.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RFM95W"/>
</gates>
<devices>
<device name="" package="RFM95/96/97/98W">
<connects>
<connect gate="G$1" pin="!RESET" pad="!RESET"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="ANT" pad="ANT"/>
<connect gate="G$1" pin="DIO0" pad="DIO0"/>
<connect gate="G$1" pin="DIO1" pad="DIO1"/>
<connect gate="G$1" pin="DIO2" pad="DIO2"/>
<connect gate="G$1" pin="DIO3" pad="DIO3"/>
<connect gate="G$1" pin="DIO4" pad="DIO4"/>
<connect gate="G$1" pin="DIO5" pad="DIO5"/>
<connect gate="G$1" pin="GND" pad="GND@1 GND@2 GND@3"/>
<connect gate="G$1" pin="MISO" pad="MISO"/>
<connect gate="G$1" pin="MOSI" pad="MOSI"/>
<connect gate="G$1" pin="NSS" pad="NSS"/>
<connect gate="G$1" pin="SCK" pad="SCK"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-13959"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ROCKBLOCK_9603" prefix="U1">
<description>Designed to work with SMD connector 53398-1071 from Molex.</description>
<gates>
<gate name="U1" symbol="ROCKBLOCK_9603"/>
</gates>
<devices>
<device name="SMD" package="1X10-1.25MM-SMD">
<connects>
<connect gate="U1" pin="!RI!" pad="5"/>
<connect gate="U1" pin="5V" pad="8"/>
<connect gate="U1" pin="CTS" pad="2"/>
<connect gate="U1" pin="GND" pad="10"/>
<connect gate="U1" pin="LI-ION" pad="9"/>
<connect gate="U1" pin="NETAV" pad="4"/>
<connect gate="U1" pin="ON/!OFF!" pad="7"/>
<connect gate="U1" pin="RTS" pad="3"/>
<connect gate="U1" pin="RX-O" pad="1"/>
<connect gate="U1" pin="TX-I" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ESP-12S" prefix="U">
<description>&lt;h3&gt;AI-Thinker ESP-12S&lt;/h3&gt;
&lt;p&gt;ESP-12S WiFi module is developed by AI-Thinker Co.,Ltd, core processor ESP8266 in smaller sizes of the module
encapsulates Tensilica L106 integrates industry-leading ultra low power 32-bit MCU micro, with the 16-bit short mode,
clock speed support 80 MHz, 160 MHz, supports the RTOS, integrated Wi-Fi MAC/BB/RF/PA/LNA, on-board antennas.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ESP-12S"/>
</gates>
<devices>
<device name="" package="ESP-12S">
<connects>
<connect gate="G$1" pin="ADC" pad="2"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="9 P$1"/>
<connect gate="G$1" pin="IO0" pad="12"/>
<connect gate="G$1" pin="IO12" pad="6"/>
<connect gate="G$1" pin="IO13" pad="7"/>
<connect gate="G$1" pin="IO14" pad="5"/>
<connect gate="G$1" pin="IO15" pad="10"/>
<connect gate="G$1" pin="IO16" pad="4"/>
<connect gate="G$1" pin="IO2" pad="11"/>
<connect gate="G$1" pin="IO4" pad="13"/>
<connect gate="G$1" pin="IO5" pad="14"/>
<connect gate="G$1" pin="RST" pad="1"/>
<connect gate="G$1" pin="RXD0" pad="15"/>
<connect gate="G$1" pin="TXD0" pad="16"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-14115"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ESP8266_ESP-01" prefix="U">
<description>&lt;h3&gt;ESP8266 ESP-01 Module&lt;/h3&gt;

&lt;p&gt;The ESP8266 WiFi Module is a self contained SOC with integrated TCP/IP protocol stack that can give any microcontroller access to your WiFi network. The ESP8266 is capable of either hosting an application or offloading all Wi-Fi networking functions from another application processor. Each ESP8266 module comes pre-programmed with an AT command set firmware, meaning, you can simply hook this up to your Arduino device and get about as much WiFi-ability as a WiFi Shield offers (and that’s just out of the box)! The ESP8266 module is an extremely cost effective board with a huge, and ever growing, community.&lt;/p&gt;

&lt;p&gt;This module has a powerful enough on-board processing and storage capability that allows it to be integrated with the sensors and other application specific devices through its GPIOs with minimal development up-front and minimal loading during runtime. Its high degree of on-chip integration allows for minimal external circuitry, including the front-end module, is designed to occupy minimal PCB area. The ESP8266 supports APSD for VoIP applications and Bluetooth co-existance interfaces, it contains a self-calibrated RF allowing it to work under all operating conditions, and requires no external RF parts.&lt;/p&gt;

&lt;p&gt;&lt;a href=https://www.sparkfun.com/products/13678&gt;SparkFun Product Page&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="ESP8266_ESP-01"/>
</gates>
<devices>
<device name="" package="ESP8266_ESP-01">
<connects>
<connect gate="G$1" pin="CH_PD" pad="2"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="GPIO0" pad="6"/>
<connect gate="G$1" pin="GPIO2" pad="7"/>
<connect gate="G$1" pin="RST" pad="3"/>
<connect gate="G$1" pin="RXD" pad="5"/>
<connect gate="G$1" pin="TXD" pad="1"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="WRL-13678"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="E19-915MS1W" prefix="U" uservalue="yes">
<description>&lt;h3&gt;Chengdu Ebyte E19-915M30S - 915M LoRa (FSK) TRX Using SX1276&lt;/h3&gt;
&lt;p&gt;This is a 915 MHz LoRa (or optionally FSK) modulated transciver bassed on the Semtech SX1276. It has a high ouput power of 1W an a pre-installed U.FL connector. Can be used with LoRa WAN with DIO0, DIO1, and DIO2 hooked up to controller interrupt inputs&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/15034”&gt;SAMD21 Pro RF 1W&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="E19-915MS1W"/>
</gates>
<devices>
<device name="" package="E19-915MS1W">
<connects>
<connect gate="G$1" pin="!NSS" pad="P$15"/>
<connect gate="G$1" pin="!RST" pad="P$8"/>
<connect gate="G$1" pin="ANT" pad="P$19"/>
<connect gate="G$1" pin="DIO0" pad="P$7"/>
<connect gate="G$1" pin="DIO1" pad="P$6"/>
<connect gate="G$1" pin="DIO2" pad="P$5"/>
<connect gate="G$1" pin="DIO3" pad="P$4"/>
<connect gate="G$1" pin="DIO4" pad="P$3"/>
<connect gate="G$1" pin="DIO5" pad="P$2"/>
<connect gate="G$1" pin="GND" pad="P$1 P$9 P$10 P$18 P$20 P$21 P$22"/>
<connect gate="G$1" pin="MISO" pad="P$13"/>
<connect gate="G$1" pin="MOSI" pad="P$14"/>
<connect gate="G$1" pin="RXEN" pad="P$17"/>
<connect gate="G$1" pin="SCK" pad="P$12"/>
<connect gate="G$1" pin="TXEN" pad="P$16"/>
<connect gate="G$1" pin="VCC" pad="P$11"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-14076"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ESP-WROVER-32" prefix="U">
<gates>
<gate name="G$1" symbol="ESP-WROVER-32"/>
</gates>
<devices>
<device name="ESP-WROVER-32" package="ESP-WROVER-32">
<connects>
<connect gate="G$1" pin="3V3" pad="P$2"/>
<connect gate="G$1" pin="CS0_H/IO15" pad="P$23"/>
<connect gate="G$1" pin="CS0_V/IO5" pad="P$29"/>
<connect gate="G$1" pin="EN" pad="P$3"/>
<connect gate="G$1" pin="GND" pad="P$39"/>
<connect gate="G$1" pin="GND@1" pad="P$1"/>
<connect gate="G$1" pin="GND@15" pad="P$15"/>
<connect gate="G$1" pin="GND@38" pad="P$38"/>
<connect gate="G$1" pin="IO0" pad="P$25"/>
<connect gate="G$1" pin="IO2" pad="P$24"/>
<connect gate="G$1" pin="IO21" pad="P$33"/>
<connect gate="G$1" pin="IO22" pad="P$36"/>
<connect gate="G$1" pin="IO25" pad="P$10"/>
<connect gate="G$1" pin="IO26" pad="P$11"/>
<connect gate="G$1" pin="IO27" pad="P$12"/>
<connect gate="G$1" pin="IO34" pad="P$6"/>
<connect gate="G$1" pin="IO35" pad="P$7"/>
<connect gate="G$1" pin="IO4" pad="P$26"/>
<connect gate="G$1" pin="MISO_H/IO12" pad="P$14"/>
<connect gate="G$1" pin="MISO_V/IO19" pad="P$31"/>
<connect gate="G$1" pin="MOSI_H/IO13" pad="P$16"/>
<connect gate="G$1" pin="MOSI_V/IO23" pad="P$37"/>
<connect gate="G$1" pin="NC" pad="P$27 P$28 P$32"/>
<connect gate="G$1" pin="RXD" pad="P$34"/>
<connect gate="G$1" pin="SCK/IO6" pad="P$20"/>
<connect gate="G$1" pin="SCK_H/IO14" pad="P$13"/>
<connect gate="G$1" pin="SCK_V/IO18" pad="P$30"/>
<connect gate="G$1" pin="SCS/IO11" pad="P$19"/>
<connect gate="G$1" pin="SDI/IO8" pad="P$22"/>
<connect gate="G$1" pin="SDO/IO7" pad="P$21"/>
<connect gate="G$1" pin="SENSOR_VN/I39" pad="P$5"/>
<connect gate="G$1" pin="SENSOR_VP/I36" pad="P$4"/>
<connect gate="G$1" pin="SHD/IO9" pad="P$17"/>
<connect gate="G$1" pin="SWP/IO10" pad="P$18"/>
<connect gate="G$1" pin="TXD" pad="P$35"/>
<connect gate="G$1" pin="XTAL_N/IO33" pad="P$9"/>
<connect gate="G$1" pin="XTAL_P/IO32" pad="P$8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XBEE3" prefix="U">
<gates>
<gate name="G$1" symbol="XBEE3"/>
</gates>
<devices>
<device name="" package="XBEE3-SMD">
<connects>
<connect gate="G$1" pin="!RST" pad="P$6"/>
<connect gate="G$1" pin="D0/A0" pad="P$31"/>
<connect gate="G$1" pin="D1/A1/SCL" pad="P$30"/>
<connect gate="G$1" pin="D10/PWM0/RSSI" pad="P$7"/>
<connect gate="G$1" pin="D11/PWM1/SDA" pad="P$8"/>
<connect gate="G$1" pin="D12" pad="P$5"/>
<connect gate="G$1" pin="D13/DOUT" pad="P$3"/>
<connect gate="G$1" pin="D14/DIN" pad="P$4"/>
<connect gate="G$1" pin="D15/MISO" pad="P$16"/>
<connect gate="G$1" pin="D16/MOSI" pad="P$15"/>
<connect gate="G$1" pin="D17/!SS" pad="P$14"/>
<connect gate="G$1" pin="D18/SCK" pad="P$13"/>
<connect gate="G$1" pin="D19/!ATNN!/!BT_MODE" pad="P$11"/>
<connect gate="G$1" pin="D2/A2" pad="P$29"/>
<connect gate="G$1" pin="D3/A3" pad="P$28"/>
<connect gate="G$1" pin="D4" pad="P$23"/>
<connect gate="G$1" pin="D5/ASSOCIATE" pad="P$26"/>
<connect gate="G$1" pin="D6/!RTS" pad="P$27"/>
<connect gate="G$1" pin="D7/!CTS" pad="P$24"/>
<connect gate="G$1" pin="D8/!DTR!/SLP_RQ" pad="P$9"/>
<connect gate="G$1" pin="D9/ON/!SLP" pad="P$25"/>
<connect gate="G$1" pin="GND" pad="P$1 P$10 P$12 P$21 P$32 P$34"/>
<connect gate="G$1" pin="RF" pad="P$33"/>
<connect gate="G$1" pin="VCC" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="WRL-14444/ WRL-14467"/>
<attribute name="VALUE" value="XBEE3_Micro"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
