<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.1">
<drawing>
<library>
<description>&lt;h3&gt;SparkFun Electronics' Retired foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are &lt;b&gt; no longer used&lt;/b&gt; in our catalog.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ANDROID-ELECTRIC_SHEEP_LOGO">
</package>
<package name="ANDROID-ELECTRIC_SHEEP_LOGO_SMALL">
</package>
<package name="CREATIVE_COMMONS">
</package>
<package name="SFE-LOGO">
</package>
<package name="SFE-NEW-WEBLOGO">
</package>
<package name="SFE-LOGO-FLAME-COPPER">
</package>
<package name="SFE-LOGO-FLAME">
</package>
<package name="SFE-NEW-WEB">
</package>
<package name="SFE-NEW-WEB-SOLDERMASK">
</package>
<package name="STARBOARD_LOGO">
</package>
<package name="STARBOARD_LOGO_TEXT">
</package>
<package name="FIDUCIAL-1.5X3">
</package>
<package name="FIDUCIAL-1X2.5">
</package>
<package name="FRIST_LOGO">
</package>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="1206">
</package>
<package name="EIA3216">
</package>
<package name="HSMC-C265">
</package>
<package name="SO014">
</package>
<package name="SPARKFUN-DIGITALIC_QFN-44">
</package>
<package name="SPARKFUN-DIGITALIC_QFN-44-NOPAD">
</package>
<package name="SPARKFUN-DIGITALIC_TQFP44">
</package>
<package name="QFN-44-NOPAD_1:1">
</package>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SJ_2S">
<description>Small solder jumper with big paste layer so it will short during reflow.</description>
</package>
<package name="1X02_LOCK">
<description>&lt;h3&gt;Plated Through Hole - Locking Footprint&lt;/h3&gt;
Holes are staggered by 0.005" from center to hold pins while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SJ_2S-NO">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
<package name="SJ_2S-NO-NS">
</package>
<package name="SJ_3">
</package>
<package name="1X03">
</package>
<package name="SJ_3_PASTE1&amp;2">
</package>
<package name="SJ_3_PASTE2&amp;3">
</package>
<package name="SJ_2S-TRACE">
<description>Solder jumper, small, shorted with trace. No paste layer. Trace is cuttable.</description>
</package>
<package name="SJ_2S-NOTRACE">
</package>
<package name="SJ_2S-TRACE-PTH">
</package>
<package name="SJ_2S-PTH">
</package>
<package name="SJ_ROUND">
</package>
<package name="SJ_2W">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
<package name="SJ_2">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
<package name="SJ_3_PASTE1&amp;2&amp;3">
</package>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="KSA_SEALED_TAC_SWITCH">
</package>
<package name="TACTILE-SWITCH-SMD">
</package>
<package name="PIC24FXXX_TQFP64">
<description>64-Lead TQFP Plastic Thin Quad Flatpack - 10x10x1mm Body, 2mmFP</description>
</package>
<package name="LED-1206">
<description>&lt;h3&gt;LED 1206 SMT&lt;/h3&gt;

1206, surface mount. 

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: &lt;/li&gt;
&lt;li&gt;Area: &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;[]&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="SIMPLE_HOLE">
<description>&lt;h3&gt;Simple Hole&lt;/h3&gt;
Sew hole
&lt;p&gt;Specifications:
&lt;li&gt;Drill: 0.1in&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;SEW_HOLE&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SIMPLE_HOLE_SM">
<description>&lt;h3&gt;Simple Hole - Small&lt;/h3&gt;
Sew hole small diameter
&lt;p&gt;Specifications:
&lt;li&gt;Drill: 0.07in&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;SEW_HOLE&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="BLE112-A">
<description>&lt;h3&gt;BLE112-A Bluetooth Smart Module&lt;/h3&gt;
&lt;p&gt;Bluetooth 4.0 module with built-in chip antenna.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.mouser.com/ds/2/368/Bluegiga_Technologies_BLE112_Datasheet-558666.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="RN-131G">
</package>
<package name="RS9110-N-11-22-SHORT">
<description>Redpine WiFi module: short FP (doesn't include the NC pads around the antenna)</description>
</package>
<package name="BADGER_HACK">
<description>&lt;h3&gt;BadgerStick Logo and Tutorial URL&lt;/h3&gt;
&lt;p&gt;&lt;a href="https://learn.sparkfun.com/tutorials/badgerhack"&gt;Tutorial Link&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;BADGERHACK_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="DUMMY">
<description>&lt;h3&gt;Dummy Footprint&lt;/h3&gt;
&lt;p&gt;NOTHING HERE!!! For when you want a symbol with no package as an option against symbols with a package.&lt;/p&gt;

&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;BADGERHACK_LOGO&lt;/li&gt;
&lt;li&gt;FRAME-LETTER&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="FKIT-LOGO_MEDIUM">
</package>
<package name="FKIT-LOGO_SMALL">
</package>
<package name="FKIT-LOGO_VERY_SMALL">
</package>
<package name="FKIT-LOGOTYPE_SMALL">
</package>
<package name="FKIT-LOGOTYPE_VERY_SMALL">
</package>
<package name="FKIT-LOGOTYPE_MEDIUM">
</package>
<package name="OVERTONE_LOGO">
</package>
<package name="LOGO-LILYPAD">
</package>
<package name="LOGO-LPA">
</package>
<package name="LOGO-L">
</package>
<package name="LOGO-L-TINY">
</package>
<package name="LOGO-A">
</package>
<package name="2X30-BERGSTAK-0.8MM-F">
<description>96BOARDS High Speed connector
&lt;br&gt;
For video &amp; camera interfaces
&lt;br&gt;
Part as drawn in the for the part:
&lt;br&gt;- FCI 61083-063402PLF for 7mm stack height or
&lt;br&gt;- FCI 61083-064402PLF for 8mm stack</description>
</package>
<package name="2X30-BERGSTAK-0.8MM-M">
</package>
<package name="2X20-2MM-SHROUDED-PTH">
</package>
<package name="2X20-SHROUDED">
</package>
<package name="2X20-2MM-SMT-F">
<description>E.G. Molex 87832-4072</description>
</package>
<package name="2X20-2MM-SHROUDED-SMT-BOTTOM-M">
<description>&lt;B&gt;Warning! this is for the BOTTOM of a 96-boards Layout&lt;/b&gt;&lt;br&gt;&lt;br&gt;
Pin 1 is not in the right place for ordinary usage!!

&lt;BR&gt;&lt;BR&gt;
Candidate parts:&lt;BR&gt;
Molex 87832-4072 - shrouded&lt;BR&gt;
Molex 87759-4050 - unshrouded</description>
</package>
<package name="2X20-2MM-SHROUDED-RA-PTH">
<description>2x20, 2mm pitch, shrouded, right-angle header. &lt;br&gt;&lt;br&gt;


Candidate parts:
Molex  87833-4019 
Samtec LTMM-120-02-F-D-RA</description>
</package>
<package name="2X20-2MM-SHROUDED-SMT-TOP-M">
<description>96-boards lo-spped male on top of board.&lt;BR&gt;&lt;BR&gt;

This is the 96-boards lo-speed connector, rearranged to put a male header on the top of the board.
&lt;BR&gt;&lt;BR&gt;
Candidate parts:&lt;BR&gt;
Molex 87832-4072 - shrouded&lt;BR&gt;
Molex 87759-4050 - unshrouded</description>
</package>
<package name="2X20-2MM-SHROUDED-SMT-RIBBON-M">
</package>
<package name="DUEMILANOVE_SHIELD">
</package>
<package name="DUEMILANOVE_VIAS">
</package>
<package name="DUEMILANOVE_SHIELD_NOHOLES">
</package>
<package name="DUEMILANOVE_SHIELD_LONGPADS">
</package>
<package name="DUEMILANOVE_SHIELD_NOLABELS">
</package>
<package name="DUEMILANOVE_SHIELD_NOHOLES_NOLABELS">
</package>
<package name="ARDUINO_MINI">
</package>
<package name="DP6037_V1">
</package>
<package name="XPORT">
</package>
<package name="XPORT_DIRECT_MODULE">
</package>
<package name="XPORT_DIRECT_MODULE-SMD">
</package>
<package name="LIGHTPIPE-7511">
</package>
<package name="APA3010SF4C">
</package>
<package name="LUXEON">
</package>
<package name="LUXEON-REBEL">
</package>
<package name="ATARI_CONNECTOR">
</package>
<package name="DB15">
</package>
<package name="F25D">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="F25H">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="F25HP">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="F25V">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="F25VP">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="F25VB">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="M25D">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="M25H">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="M25HP">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="M25V">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="M25VP">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="M25VB">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="IPOD_FEMALE_CONNECTOR">
</package>
<package name="IPOD_MALE_CONNECTOR">
</package>
<package name="FFC_16">
</package>
<package name="LITTLE_BITS_FEMALE">
</package>
<package name="LITTLE_BITS_MALE">
</package>
<package name="LITTLEBITS">
</package>
<package name="LCD_CFAX">
<description>&lt;h3&gt;CFAX LCD (crystalfontz)&lt;/h3&gt;
&lt;p&gt;For 128x64 LCDs.&lt;/p&gt;

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 16&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;li&gt;Area: &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Example device(s): 
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/retired/257"&gt;CrystalFontz LCD&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="DIL28-3">
<description>Standard 28-pin DIP package.&lt;br&gt;
IC needs to have legs bent before insertion.</description>
</package>
<package name="LQFP-32">
<description>&lt;b&gt;Quad Flat Package&lt;/b&gt; 32 LD LQFP&lt;p&gt;
Source: ds232b12.pdf&lt;br&gt;
http://www.ftdichip.com</description>
</package>
<package name="QFN-24">
</package>
<package name="QFN-24_ALT1.PAC">
</package>
<package name="QFN-32">
<description>&lt;h3&gt;QFN 32-Pin package w/ Thermal Pad&lt;/h3&gt;
&lt;b&gt;***Unproven***&lt;/b&gt;
&lt;br&gt;&lt;br&gt;
&lt;B&gt;Applicable Parts:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;TLC5940&lt;/ul&gt;</description>
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="DIL24">
</package>
<package name="TSSOP28">
</package>
<package name="TSSOP28-GROUNDPAD">
</package>
<package name="SOT23-3">
</package>
<package name="SOT143">
<description>&lt;h3&gt;SOT143&lt;/h3&gt;
Package is used for the STM811 (also APX811)&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Proven&lt;/b&gt;</description>
</package>
<package name="SOT23-6">
</package>
<package name="SSOP28DB">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="LQFP-48">
</package>
<package name="QFN-24-USB">
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="SO08">
<description>SOIC, 0.15 inch width</description>
</package>
<package name="SO-28W">
<description>&lt;B&gt;Small Outline Wide Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
300-mil body, package type SO</description>
</package>
<package name="TSSOP30">
</package>
<package name="SC70-6">
</package>
<package name="SO08WIDE">
</package>
<package name="SO08-EIAJ">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
<package name="TSOP48">
</package>
<package name="MLP28">
<description>&lt;b&gt;MLP 28&lt;/b&gt;&lt;p&gt;
Source: www.silabs.com .. CP2101.pdf</description>
</package>
<package name="SO16L">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; .300 SIOC&lt;p&gt;
Source: http://www.maxim-ic.com/cgi-bin/packages?pkg=16%2FSOIC%2E300&amp;Type=Max</description>
</package>
<package name="TSSOP20">
</package>
<package name="TSSOP16">
<description>&lt;b&gt;TSOP16&lt;/b&gt;&lt;p&gt;
thin small outline package</description>
</package>
<package name="SOIC-14">
</package>
<package name="TSSOP-16">
</package>
<package name="SO08-EPAD">
</package>
<package name="QFN-24_ALT2">
<description>&lt;h3&gt;24-pin QFN with Exposed Thermal pad&lt;/h3&gt;
Parts that use this package:
&lt;ul&gt;
&lt;li&gt;A6282&lt;/li&gt;
&lt;/ul&gt;
Last modified: 8/20/10&lt;br&gt;
&lt;br&gt;
&lt;b&gt;***UNPROVEN***&lt;/b&gt;&lt;BR&gt;</description>
</package>
<package name="DIL18">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="MSOP8">
<description>&lt;b&gt;8M, 8-Lead, 0.118" Wide, Miniature Small Outline Package&lt;/b&gt;&lt;p&gt;
MSOP&lt;br&gt;
8M-Package doc1097.pdf</description>
</package>
<package name="SOIC8">
</package>
<package name="SO16">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
<package name="TQFP32-5MM">
</package>
<package name="SO08-UNIVERSAL">
<description>SOIC-08 footprint wth long lands.&lt;br&gt;

To fit both narrow and wide SOICs - for SOIC-to-DIP adapter board.
&lt;br&gt;&lt;br&gt;
Not recommended if you're trying to fit a specific chip.</description>
</package>
<package name="PQFP208">
</package>
<package name="DIP16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SO-24DW">
<description>300-mil body, package type SO</description>
</package>
<package name="SOP-14">
<description>&lt;h3&gt;14-pin SOP-14 package&lt;/h3&gt;
Used on WS2801 RGB controller</description>
</package>
<package name="PQ208">
</package>
<package name="SQFP-S-10X10-64-XS1">
</package>
<package name="TSSOP-24">
<description>&lt;h3&gt;24-pin TSSOP with Exposed Thermal Pad&lt;/h3&gt;
Used on: &lt;ul&gt;
&lt;li&gt;Allegro A6282 16-bit LED driver&lt;/li&gt;
&lt;/ul&gt;
Last modified: 8/21/10&lt;br&gt;
&lt;b&gt;***Unproven***&lt;/b&gt;&lt;br&gt;</description>
</package>
<package name="TSSOP14">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 14&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="LCC20">
<description>&lt;b&gt;Leadless Chip Carrier&lt;/b&gt;&lt;p&gt; Ceramic Package</description>
</package>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="1210">
<description>&lt;p&gt;&lt;b&gt;Generic 3225 (1210) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="ALPHANUMERIC">
</package>
<package name="7-SEGMENT-DISPLAY">
</package>
<package name="7-SEGMENT-4DIGIT">
</package>
<package name="7-SEGMENT-4DIGIT-YOUNGSUN">
<description>This is a package for the 4-digit 7-segment RED LED from Young Sun.</description>
</package>
<package name="7-SEGMENT-4DIGIT_LONGPADS_FOR_POGOBED">
</package>
<package name="BATTERY">
<description>&lt;B&gt;BATTERY&lt;/B&gt;&lt;p&gt;
22 mm</description>
</package>
<package name="BATTCON_24.5MM">
</package>
<package name="LIPO-1100MAH">
</package>
<package name="BATTERY-AA-PANEL">
</package>
<package name="BATTERY_20MM_PTH_COMPACT">
</package>
<package name="LIPO-110-TABS">
</package>
<package name="BUTTON-CONDUCTIVE-0.1">
</package>
<package name="BUTTON-CONDUCTIVE-MINI">
</package>
<package name="BUTTON-10MM">
</package>
<package name="CAPSENSE_PAD">
</package>
<package name="DIPSWITCH-02">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;</description>
</package>
<package name="DIPSWITCH-08-50MIL">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;
&lt;p&gt;Half-size SMT DIP switch, 1.27 mm / 0.05" pitch. For example the following:&lt;/p&gt;
&lt;ul&gt;
  &lt;li&gt;Omron A6H series; &lt;a href="http://www.omron.com/ecb/products/pdf/en-a6h.pdf"&gt;Datasheet&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;</description>
</package>
<package name="FKIT-LIR2450-H">
</package>
<package name="FKIT-RIBBON_CONNECTOR_03_2MM_L">
</package>
<package name="FKIT-RIBBON_CONNECTOR_03_2MM_R">
</package>
<package name="FKIT-SNAP_FEMALE">
</package>
<package name="FKIT-SNAP_MALE">
</package>
<package name="G3VM-61E1">
</package>
<package name="AAVID_573400">
</package>
<package name="N35P112">
</package>
<package name="TRIM_POT">
</package>
<package name="3362U">
</package>
<package name="POT_ALPHA_RV16AF-20">
<description>Package for Alpha RV16AF-20 potentiometer</description>
</package>
<package name="POT_MAMMOTH">
</package>
<package name="POT_PTH">
</package>
<package name="RELAY-S108T02">
</package>
<package name="RELAY-G5Q">
<description>G5Q-1A DC12</description>
</package>
<package name="RELAY-T9A">
<description>Big relay. 220V/30A. SparkFun SKU: COM-00101</description>
</package>
<package name="RELAY-T9A-2">
</package>
<package name="RELAY-G5V">
<description>G5Q SPDT Relay (SparkFun SKU: COM-00100). Footprint should also work with SPST-NO relay.</description>
</package>
<package name="SWITCH-4PDT-CNK">
</package>
<package name="MSS22">
<description>MSS22 DPDT Switch</description>
</package>
<package name="MS">
<description>Series S Slide Switch</description>
</package>
<package name="ES">
<description>Right Angle Slide Switch. Works with part#ES21MABE</description>
</package>
<package name="OS">
</package>
<package name="EG2211">
</package>
<package name="STOMP-SWITCH-DPDT">
<description>Stomp switch

COM-11151

Footprint unproven</description>
</package>
<package name="TACTILE-PTH-12MM">
</package>
<package name="TACTILE_SWITCH_SMD-3">
</package>
<package name="SWITCH-DPDT">
</package>
<package name="R_SW_TH">
</package>
<package name="SWITCH_SPDT_SMD">
</package>
<package name="SWITCH-SPST-VERTICAL">
</package>
<package name="KPS-1290">
</package>
<package name="1X01_TURRET">
<description>0.08" Drill, 0.13" tDoc</description>
</package>
<package name="TRIMPOT_TC33">
</package>
<package name="3362U-2">
</package>
<package name="TRIM_POT_PTH">
</package>
<package name="TRIMPOT-3MM">
</package>
<package name="TRIMPOT-5MM">
</package>
<package name="TRIMPOT_PTH_S3_LOCK">
</package>
<package name="TRIMPOT-5MM-V2">
</package>
<package name="SMARTCARD">
<description>&lt;b&gt;Description:&lt;/b&gt; S..m..r..t. I am so smrt!</description>
</package>
<package name="SMA-EDGE">
<description>&lt;b&gt;SMA Antenna Connector&lt;/b&gt;&lt;p&gt;
This is a footprint for an edge mount RF antenna. Works pretty well with SMA type connectors but may also work with other edge mount RF connectors. Keep in mind, these edge mount connectors assume you are using a 0.062" PCB thickness.</description>
</package>
<package name="TOUCH-SCREEN">
</package>
<package name="DIL40-6-ZIF_SOCKET">
</package>
<package name="ZUNE_CONNECTOR_MALE">
</package>
<package name="TQFP32-08_MCU">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="TQFP64_MCU">
<description>64-Lead TQFP Plastic Thin Quad Flatpack - 10x10x1mm Body, 2mmFP</description>
</package>
<package name="TQFP64_14X14MM_MCU">
<description>64-Lead TQFP Plastic Thin Quad Flatpack - 14x14x1mm Body</description>
</package>
<package name="MLF32_MCU">
<description>&lt;b&gt;32M1-A&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="QFN20_MCU">
</package>
<package name="SSOP28DB_MCU">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="TQFP44_MCU">
</package>
<package name="TQFP-100-12X12MM_MCU">
</package>
<package name="LQFP-48_MCU">
</package>
<package name="SO-28W_MCU">
<description>&lt;B&gt;Small Outline Wide Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
300-mil body, package type SO</description>
</package>
<package name="SQFP-S-10X10-64_MCU">
<description>&lt;b&gt;QFP64&lt;/b&gt;&lt;p&gt;
shrink quad flat pack, square</description>
</package>
<package name="P8X32A-Q44_MCU">
</package>
<package name="PIC24FXXX_TQFP64_MCU">
<description>64-Lead TQFP Plastic Thin Quad Flatpack - 10x10x1mm Body, 2mmFP</description>
</package>
<package name="UBW32_TQFP100_MCU">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="TQFP-100-14X14MM_MCU">
</package>
<package name="LQFP-10X10-64_MCU">
<description>&lt;b&gt;LQFP64&lt;/b&gt;&lt;p&gt;
shrink quad flat pack, square</description>
</package>
<package name="SO08_MCU">
<description>SOIC, 0.15 inch width</description>
</package>
<package name="SO08-EIAJ_MCU">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
<package name="SO14_MCU">
<description>SOIC, 0.15 inch width</description>
</package>
<package name="DIP08_MCU">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIP28_MCU">
<description>Standard 28-pin DIP package.&lt;br&gt;
IC needs to have legs bent before insertion.</description>
</package>
<package name="DIP28-KIT_MCU">
</package>
<package name="DIL28-ZIF_SOCKET_MCU">
</package>
<package name="DIP40_MCU">
<description>Dual In Line Package: 40-pin PDIP</description>
</package>
<package name="USB-B-PTH">
<description>&lt;h3&gt;USB Type B PTH Mounted&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4 main, 2 shield&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;USB_B&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="USB-MB-H">
<description>&lt;b&gt;USB Series Mini-B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-MINIB-OLD">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
<package name="S4B-PH">
</package>
<package name="USB-MINIB">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
<package name="USB-MINIB-NOSTOP">
</package>
<package name="USB-MICROB">
<description>Micro USB Package</description>
</package>
<package name="MINI-DIN6">
</package>
<package name="RJ9">
<description>Footprint for RJ9 simple connector. Common with telephone handsets. SparkFun SKU: PRT-08694</description>
</package>
<package name="COMPUTER-PERIPHERAL-POWER-RA">
</package>
<package name="COMPUTER-PERIPHERAL-POWER">
</package>
<package name="2X12">
</package>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X10">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X26">
</package>
<package name="2X13-SHROUDED">
</package>
<package name="AUDIO_JACK_0.25&quot;_TRS_PTH_VERTICAL">
</package>
<package name="USD-SOCKET-PP">
<description>OLD Production Socket. DO NOT USE for production boards.</description>
</package>
<package name="MICRO-SD-SOCKET-PP">
</package>
<package name="MICROSD_1:1">
</package>
<package name="MICRO-SD-SOCKET-SDIO">
</package>
<package name="MSOP-10-GNDPAD">
<description>10-lead MSOP w/ center GND pad</description>
</package>
<package name="SC-70">
</package>
<package name="TO-PMOD-7">
<description>7-Lead package for National voltage switchers (LMZ14203)</description>
</package>
<package name="Q5-DD">
<description>&lt;b&gt;Q5-DD&lt;/b&gt;</description>
</package>
<package name="QFN16-3X3MM_TI">
</package>
<package name="QFN16-4X4">
<description>&lt;b&gt;16-Lead Plastic Quad Flat, No Lead Package (ML) - 4x4x0.9mm Body [QFN]&lt;/b&gt;&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/41203E.pdf</description>
</package>
<package name="QFN16-3X3MM">
<description>3mm x 3mm QFN 16 pin</description>
</package>
<package name="QFN-28-5MM-1:1">
</package>
<package name="QFN-28-5MM_ALT1">
</package>
<package name="QFN-28-5MM_ALT2">
</package>
<package name="QFN-28-5MM_ALT1_REDUCED_PASTE">
</package>
<package name="QFN-28-5MM">
</package>
<package name="TO-220-11LEAD">
<description>TO-220 11 Pin Package</description>
</package>
<package name="SO-24W">
</package>
<package name="MICROPHONE-PTH-9.7MM">
<description>&lt;h3&gt;Microphone - 9.7 mm Diameter, PTH&lt;/h3&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Sensors/Sound/CEM-C9745JAD462P2.54R.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;
&lt;li&gt;Pin Count: 2&lt;/li&gt;
&lt;li&gt;Diameter: 9.7 mm&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;Devices Using:&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;MIC&lt;/li&gt;
&lt;/ul&gt;</description>
</package>
<package name="MICROPHONE-SMD-6MM">
<description>&lt;h3&gt;SMD Omni-Directional Condenser Microphone&lt;/h3&gt;
&lt;p&gt;&lt;a href="http://www.challengeelectronics.com/downloads/microphones/omni_directional/CEM-OB6018-3EAD443C43MR.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;
&lt;li&gt;Pin Count: 2&lt;/li&gt;
&lt;li&gt;Diameter: 6.0 mm&lt;/li&gt;
&lt;li&gt;Height: 1.8 mm&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;Devices Using:&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;MIC&lt;/li&gt;
&lt;/ul&gt;</description>
</package>
<package name="MOLEX-1X2">
<description>&lt;h3&gt;Molex 2-Pin Plated Through-Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/2pin_molex_set_19iv10.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SCREWTERMINAL-3.5MM-2">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch - 2 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="JST-2-SMD">
<description>&lt;h3&gt;JST-Right Angle Male Header SMT&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/20404.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;li&gt;JST_2MM_MALE&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02_BIG">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.15"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="JST-2-SMD-VERT">
<description>&lt;h3&gt;JST-Vertical Male Header SMT &lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/20404.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SCREWTERMINAL-5MM-2">
<description>&lt;h3&gt;Screw Terminal  5mm Pitch -2 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 5mm/197mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="MOLEX-1X2_LOCK">
<description>&lt;h3&gt;Molex 2-Pin Plated Through-Hole Locking Footprint&lt;/h3&gt;
Holes are offset from center by 0.005" to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/2pin_molex_set_19iv10.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02_LOCK_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - Long Pads with Locking Footprint&lt;/h3&gt;
Pins are staggered by 0.005" from center to hold pins in place while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SCREWTERMINAL-3.5MM-2_LOCK">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch - 2 Pin PTH Locking&lt;/h3&gt;
Holes are offset from center 0.005" to hold pins in place during soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - Long Pads without Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="JST-2-PTH">
<description>&lt;h3&gt;JST 2 Pin Right Angle Plated Through  Hole&lt;/h3&gt;
tDocu indicate polarity for connections that match SparkFun LiPo battery terminations. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch:2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Connectors/JST%282%29-01548.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02_XTRA_BIG">
<description>&lt;h3&gt;Plated Through Hole - 0.1" holes&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.2"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02_PP_HOLES_ONLY">
<description>&lt;h3&gt;Pogo Pins Connector - No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SCREWTERMINAL-3.5MM-2-NS">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch - 2 Pin PTH No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="JST-2-PTH-NS">
<description>&lt;h3&gt;JST 2 Pin Right Angle Plated Through  Hole- No Silk&lt;/h3&gt;
tDocu indicate polarity for connections that match SparkFun LiPo battery terminations. 
&lt;br&gt; No silk outline of connector. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch:2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Connectors/JST%282%29-01548.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="JST-2-PTH-KIT">
<description>&lt;h3&gt;JST 2 Pin Right Angle Plated Through  Hole - KIT&lt;/h3&gt;
tDocu indicate polarity for connections that match SparkFun LiPo battery terminations. 
&lt;br&gt; This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad.
&lt;br&gt; This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch:2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Connectors/JST%282%29-01548.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SPRINGTERMINAL-2.54MM-2">
<description>&lt;h3&gt;Spring Terminal- PCB Mount 2 Pin PTH&lt;/h3&gt;
tDocu marks the spring arms
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 4&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/SpringTerminal.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02_2.54_SCREWTERM">
<description>&lt;h3&gt;2 Pin Screw Terminal - 2.54mm&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="JST-2-PTH-VERT">
<description>&lt;h3&gt;JST -XH Male 2.5mm Vertical Plated-Through-Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.jst-mfg.com/product/pdf/eng/eXH.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02_POKEHOME">
<description>2 pin poke-home connector

part number 2062-2P from STA</description>
</package>
<package name="INDUCTOR_2.2UH">
</package>
</packages>
<symbols>
<symbol name="ANDROID-ELECTRIC_SHEEP_LOGO">
</symbol>
<symbol name="CREATIVE_COMMONS">
</symbol>
<symbol name="A3L-LOC">
</symbol>
<symbol name="LOGO1">
</symbol>
<symbol name="STARBOARD_LOGO">
</symbol>
<symbol name="FIDUCIAL">
</symbol>
<symbol name="SPARKFUN-EAGLE-RULES">
</symbol>
<symbol name="FIRST">
</symbol>
<symbol name="CAP">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="CAP_POL">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="LED">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="74ACT125D">
<pin name="VCC"/>
<pin name="A0"/>
<pin name="B0"/>
<pin name="A1"/>
<pin name="B1"/>
<pin name="A2"/>
<pin name="B2"/>
<pin name="GND"/>
<pin name="B3"/>
<pin name="A3"/>
<pin name="O3"/>
<pin name="O2"/>
<pin name="O1"/>
<pin name="O0"/>
</symbol>
<symbol name="SPARKFUN-DIGITALIC_ATMEGA32U4">
<pin name="!RESET"/>
<pin name="AREF"/>
<pin name="AVCC@24"/>
<pin name="AVCC@44"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="GND@15"/>
<pin name="GND@23"/>
<pin name="GND@35"/>
<pin name="GND@43"/>
<pin name="PB0(SS)"/>
<pin name="PB1(SCK)"/>
<pin name="PB2(MOSI)"/>
<pin name="PB3(MISO)"/>
<pin name="PB4(ADC11)"/>
<pin name="PB5(ADC12)"/>
<pin name="PB6(ADC13)"/>
<pin name="PB7"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PD0(SCL)"/>
<pin name="PD1(SDA)"/>
<pin name="PD2(RX)"/>
<pin name="PD3(TX)"/>
<pin name="PD4(ADC8)"/>
<pin name="PD5"/>
<pin name="PD6(ADC9)"/>
<pin name="PD7(ADC10)"/>
<pin name="PE2/!HWB"/>
<pin name="PE6"/>
<pin name="PF0(ADC0)"/>
<pin name="PF1(ADC1)"/>
<pin name="PF4(ADC4)"/>
<pin name="PF5(ADC5)"/>
<pin name="PF6(ADC6)"/>
<pin name="PF7(ADC7)"/>
<pin name="UCAP"/>
<pin name="UGND"/>
<pin name="UVCC"/>
<pin name="VBUS"/>
<pin name="VCC@14"/>
<pin name="VCC@34"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
</symbol>
<symbol name="JUMPER-2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="JUMPER-3">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="SJ">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="SJ_2">
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="LETTER_L">
</symbol>
<symbol name="DOCFIELD">
</symbol>
<symbol name="SWITCH-MOMENTARY">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="PIC24FJXXXDAX06">
<pin name="!MCLR" direction="in"/>
<pin name="AN2/C2INB/VMIO/RP13/CN4/RB2"/>
<pin name="AN3/C2INA/VPIO/CN5/RB3"/>
<pin name="AN8/RP8/CN26/RB8"/>
<pin name="AN9/RP9/CN27/RB9"/>
<pin name="AN14/CTPLS/RP14/CN32/RB14"/>
<pin name="AN15/RP29/REFO/CN12/RB15"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="C1INC/RP26/CN9/RG7"/>
<pin name="C1IND/RP21/CN8/RG6"/>
<pin name="C2INC/RP27/GD15/CN11/RG9"/>
<pin name="C2IND/RP19/GD14/CN10/RG8"/>
<pin name="C3INA/SESSEND/CN16/RD7"/>
<pin name="C3INB/CN15/RD6"/>
<pin name="D+/CN83/RG2"/>
<pin name="D-/CN84/RG3"/>
<pin name="DMH/RP11/INT0/CN49/RD0"/>
<pin name="DPH/RP23/CN51/RD2"/>
<pin name="DPLN/SDA1/RP4/GD8/CN54/RD9"/>
<pin name="ENVREG" direction="in"/>
<pin name="GD0/CN58/RE0"/>
<pin name="GD1/CN59/RE1"/>
<pin name="GD2/CN60/RE2"/>
<pin name="GD3/CN61/RE3"/>
<pin name="GD10/VBUSST/VCMPST1/VBUSVLD/CN68/RF0"/>
<pin name="GD11/VCMPST2/SESSVLD/CN69/RF1"/>
<pin name="GD12/SCL3/CN64/RE6"/>
<pin name="GD13/SDA3/CN65/RE7"/>
<pin name="HSYNC/CN62/RE4"/>
<pin name="OSCI/CLKI/CN23/RC12"/>
<pin name="OSCO/CLKO/CN22/RC15"/>
<pin name="PGEC1/AN1/VREF-/RP1/CN3/RB1"/>
<pin name="PGEC2/AN6/RP6/CN24/RB6"/>
<pin name="PGEC3/AN5/C1INA/VBUSON/RP18/CN7/RB5"/>
<pin name="PGED1/AN0/VREF+/RP0/CN2/RB0"/>
<pin name="PGED2/AN7/RP7/RCV/CN25/RB7"/>
<pin name="PGED3/AN4/C1INB/USBOEN/RP28/CN6/RB4"/>
<pin name="RP12/GD7/CN56/RD11"/>
<pin name="RP16/USBID/CN71/RF3"/>
<pin name="RP20/GPWR/CN14/RD5"/>
<pin name="RP22/GEN/CN52/RD3"/>
<pin name="RP25/GCLK/CN13/RD4"/>
<pin name="RTCC/DMLN/RP2/CN53/RD8"/>
<pin name="SCL1/RP3/GD6/CN55/RD10"/>
<pin name="SCL2/RP17/GD5/CN18/RF5"/>
<pin name="SDA2/RP10/GD4/CN17/RF4"/>
<pin name="SOSCI/C3IND/CN1/RC13"/>
<pin name="SOSCO/SCLKI/T1CK/C3INC/RPI37/CN0/RC14"/>
<pin name="TCK/AN12/CTEDG2/CN30/RB12"/>
<pin name="TDI/AN13/CTEDG1/CN31/RB13"/>
<pin name="TDO/AN11/CN29/RB11"/>
<pin name="TMS/CVREF/AN10/CN28/RB10"/>
<pin name="VBUS/RF7" direction="in"/>
<pin name="VCAP" direction="pwr"/>
<pin name="VCPCON/RP24/GD9/VBUSCHG/CN50/RD1"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSYNC/CN63/RE5"/>
<pin name="VUSB" direction="pwr"/>
</symbol>
<symbol name="LED-1">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="SIMPLE_HOLE">
<description>&lt;h3&gt;Simple Hole&lt;/h3&gt;
&lt;p&gt;Basic conductive hole with single IO connection available.&lt;/p&gt;</description>
<pin name="P$1"/>
</symbol>
<symbol name="SIMPLE_HOLE_SM">
<description>&lt;h3&gt;Simple Hole- Small&lt;/h3&gt;
&lt;p&gt;Basic small conductive hole with single IO connection available.&lt;/p&gt;</description>
<pin name="P$1"/>
</symbol>
<symbol name="BLE112-A">
<description>BlueGiga BLE112-A module&lt;BR&gt;
Bluetooth 4.0 module with chip antenna.</description>
<pin name="GND1"/>
<pin name="AVDD1"/>
<pin name="AVDD2"/>
<pin name="P2_2"/>
<pin name="P2_1"/>
<pin name="P2_0"/>
<pin name="P1_7"/>
<pin name="P1_6"/>
<pin name="VDD_USB"/>
<pin name="GND2"/>
<pin name="USB+"/>
<pin name="USB-"/>
<pin name="P1_5"/>
<pin name="P1_4"/>
<pin name="P1_3"/>
<pin name="P1_2"/>
<pin name="P1_1"/>
<pin name="P1_0"/>
<pin name="P0_7"/>
<pin name="DVDD"/>
<pin name="GND3"/>
<pin name="P0_6"/>
<pin name="P0_5"/>
<pin name="P0_4"/>
<pin name="P0_3"/>
<pin name="P0_2"/>
<pin name="P0_1"/>
<pin name="P0_0"/>
<pin name="RESET"/>
<pin name="GND4"/>
</symbol>
<symbol name="RN-131G">
<pin name="SEN6"/>
<pin name="SEN4"/>
<pin name="SEN5"/>
<pin name="SEN7"/>
<pin name="RESET"/>
<pin name="EPC-A"/>
<pin name="EPC-B"/>
<pin name="S_CAP"/>
<pin name="F_AWAKE"/>
<pin name="GPIO-13"/>
<pin name="GPIO-12"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="MOSI"/>
<pin name="CLK"/>
<pin name="MISO"/>
<pin name="3.3V-ROUT"/>
<pin name="3.3V-RIN"/>
<pin name="GND@19"/>
<pin name="VDD-BATT"/>
<pin name="VDD-IN"/>
<pin name="DMA-TX"/>
<pin name="DMA-RX"/>
<pin name="GPIO-9"/>
<pin name="GPIO-8"/>
<pin name="GPIO-7"/>
<pin name="GPIO-6"/>
<pin name="GPIO-5"/>
<pin name="GPIO-4"/>
<pin name="SEN1"/>
<pin name="SEN2"/>
<pin name="SEN3"/>
<pin name="SENSE-PWR"/>
<pin name="SEN0"/>
<pin name="GND@36"/>
<pin name="GND@37"/>
<pin name="GND@38"/>
<pin name="GND@39"/>
<pin name="GND@40"/>
<pin name="GND@41"/>
<pin name="GND@42"/>
<pin name="GND@43"/>
<pin name="GND@44"/>
</symbol>
<symbol name="RS9110-N-11-22">
<pin name="VIN@46"/>
<pin name="VIN@47"/>
<pin name="JPD0"/>
<pin name="JPD1"/>
<pin name="JPD2"/>
<pin name="INTR"/>
<pin name="RST"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="SD3"/>
<pin name="CLK"/>
<pin name="CS"/>
<pin name="MOSI"/>
<pin name="MISO"/>
<pin name="MODE"/>
<pin name="GND@10"/>
<pin name="GND@16"/>
<pin name="GND@20"/>
<pin name="GND@21"/>
<pin name="GND@48"/>
<pin name="GND@PAD"/>
</symbol>
<symbol name="BADGER_HACK_LOGO">
</symbol>
<symbol name="FKIT-LOGO">
</symbol>
<symbol name="FKIT-LOGOTYPE">
</symbol>
<symbol name="OVERTONE_LOGO">
</symbol>
<symbol name="LOGO-LP">
</symbol>
<symbol name="96BOARDS-HI-SPEED">
<description>96-BOARDS High Speed Connector

Includes :
-1x DSI Interface
-2x CSI interfaces
-SD card/SPI1
-2x I2C interfaces</description>
<pin name="SD_DAT0/SPI1_DOUT"/>
<pin name="SD_DAT1"/>
<pin name="SD_DAT2"/>
<pin name="SD_DAT3/SPI1_CS"/>
<pin name="SD_SCLK/SPI1_SCLK"/>
<pin name="SD_CMD/SPI1_DIN"/>
<pin name="GND"/>
<pin name="CLK0/CSI0_MCLK"/>
<pin name="CLK1/CSI1_MCLK"/>
<pin name="DSI_CLK+"/>
<pin name="DSI_CLK-"/>
<pin name="DSI_D0+"/>
<pin name="DSI_D0-"/>
<pin name="DSI_D1+"/>
<pin name="DSI_D1-"/>
<pin name="DSI_D2+"/>
<pin name="DSI_D3+"/>
<pin name="DSI_D2-"/>
<pin name="CSI1_C-"/>
<pin name="CSI1_C+"/>
<pin name="CSI1_D1-"/>
<pin name="CSI1_D1+"/>
<pin name="CSI1_D0-"/>
<pin name="CSI1_D0+"/>
<pin name="I2C3_SDA"/>
<pin name="I2C3_SCL"/>
<pin name="I2C2_SCL"/>
<pin name="I2C2_SDA"/>
<pin name="CSI0_D3-"/>
<pin name="CSI0_D3+"/>
<pin name="CSI0_D2-"/>
<pin name="CSI0_D2+"/>
<pin name="CSI0_D1-"/>
<pin name="CSI0_D1+"/>
<pin name="CSI0_D0-"/>
<pin name="CSI0_D0+"/>
<pin name="CSI0_C+"/>
<pin name="CSI0_C-"/>
<pin name="DSI_D3-"/>
<pin name="USB_D+"/>
<pin name="USB_D-"/>
<pin name="HSIC_STR"/>
<pin name="HSIC_DATA"/>
</symbol>
<symbol name="96BOARDS-LO-SPEED">
<description>96 BOARDS Low Speed Connector
&lt;br&gt;&lt;br&gt;
UARTs, I2C, SPI, GPIO.</description>
<pin name="SYS_DCIN" direction="pwr"/>
<pin name="I2C0_SDA"/>
<pin name="I2C0_SCL"/>
<pin name="I2S_DI"/>
<pin name="SPI0_CS" direction="out"/>
<pin name="SPI0_DIN" direction="in"/>
<pin name="SPI0_SCLK" direction="out"/>
<pin name="SPI0_DOUT" direction="out"/>
<pin name="I2S_DO"/>
<pin name="I2S_CLK"/>
<pin name="I2S_FS"/>
<pin name="UART0_TXD" direction="out"/>
<pin name="UART0_CTS" direction="out"/>
<pin name="5V" direction="pwr"/>
<pin name="1.8V" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="!PWR_BTN"/>
<pin name="!RST_BTN"/>
<pin name="GPIO-A"/>
<pin name="UART0_RXD" direction="in"/>
<pin name="UART0_RTS" direction="in"/>
<pin name="UART1_TXD" direction="out"/>
<pin name="UART1_RXD" direction="in"/>
<pin name="I2C1_SDA"/>
<pin name="I2C1_SCL"/>
<pin name="GPIO-B"/>
<pin name="GPIO-C"/>
<pin name="GPIO-D"/>
<pin name="GPIO-E"/>
<pin name="GPIO-F"/>
<pin name="GPIO-G"/>
<pin name="GPIO-H"/>
<pin name="GPIO-I"/>
<pin name="GPIO-J"/>
<pin name="GPIO-K"/>
<pin name="GPIO-L"/>
</symbol>
<symbol name="ARDUINO_SHIELD">
<pin name="RX"/>
<pin name="TX"/>
<pin name="D2"/>
<pin name="*D3"/>
<pin name="D4"/>
<pin name="*D5"/>
<pin name="*D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="*D9"/>
<pin name="*D10"/>
<pin name="*D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="VIN"/>
<pin name="RES"/>
<pin name="5V"/>
<pin name="AREF"/>
<pin name="GND@2"/>
<pin name="GND@1"/>
<pin name="GND@0"/>
<pin name="3.3V"/>
</symbol>
<symbol name="ARDUINO_MINI">
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="13"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="GND"/>
<pin name="GND@2"/>
<pin name="RAW"/>
<pin name="RST"/>
<pin name="RST@2"/>
<pin name="RXI"/>
<pin name="TXO"/>
<pin name="VCC"/>
</symbol>
<symbol name="PCB_STANDARD">
</symbol>
<symbol name="XPORT">
<pin name="GND"/>
<pin name="3.3V"/>
<pin name="RST" function="dot"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="RTS"/>
<pin name="DTR"/>
<pin name="CTS"/>
</symbol>
<symbol name="XPORT_DIRECT">
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="3.3V"/>
<pin name="RST"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="RTS"/>
<pin name="DTR"/>
<pin name="CTS"/>
<pin name="CP1"/>
<pin name="CP2"/>
<pin name="GND@24"/>
</symbol>
<symbol name="LIGHTPIPE-7511">
</symbol>
<symbol name="APA3010SF4C">
<pin name="1"/>
<pin name="2"/>
</symbol>
<symbol name="LUXEON">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="S"/>
</symbol>
<symbol name="LED-2">
<description>&lt;h3&gt;LED&lt;/h3&gt;
&lt;p&gt;&lt;/p&gt;</description>
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="ATARI_CONNECTOR">
<pin name="UP"/>
<pin name="DOWN"/>
<pin name="LEFT"/>
<pin name="RIGHT"/>
<pin name="NC1"/>
<pin name="BUTTON"/>
<pin name="NC2"/>
<pin name="GND"/>
<pin name="NC3"/>
</symbol>
<symbol name="DB15">
<pin name="1" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
<symbol name="F25">
<pin name="1" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="13" direction="pas"/>
</symbol>
<symbol name="DB25">
<pin name="1" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="13" direction="pas"/>
</symbol>
<symbol name="IPOD_CONNECTOR_FEMALE">
<pin name="LEFT_IN"/>
<pin name="VIDEO_OUT"/>
<pin name="RIGHT_IN"/>
<pin name="SCHROME_OUT"/>
<pin name="GND@1"/>
<pin name="SLUM_OUT"/>
<pin name="GND@2"/>
<pin name="GND@11"/>
<pin name="LEFT_OUT"/>
<pin name="GND@16"/>
<pin name="RIGHT_OUT"/>
<pin name="FW_12V@20"/>
<pin name="ACC_INDICATOR"/>
<pin name="FW_TPA-"/>
<pin name="USB_5V"/>
<pin name="17"/>
<pin name="3.3V"/>
<pin name="FW_12V@19"/>
<pin name="GND@15"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="FW_TPA+"/>
<pin name="USB_D-"/>
<pin name="FW_TPB-"/>
<pin name="USB_D+"/>
<pin name="FW_TPB+"/>
<pin name="GND@29"/>
<pin name="GND@30"/>
<pin name="14"/>
<pin name="7"/>
</symbol>
<symbol name="KENT_LCD_CONN">
<pin name="VSS1"/>
<pin name="VSS2"/>
<pin name="VSS3"/>
<pin name="VSS4"/>
<pin name="VCC"/>
<pin name="VPWR1"/>
<pin name="VPWR2"/>
<pin name="VPWR3"/>
<pin name="/RESET"/>
<pin name="BUSY"/>
<pin name="SCK"/>
<pin name="SO"/>
<pin name="SI"/>
<pin name="CS"/>
<pin name="NC1"/>
<pin name="NC2"/>
</symbol>
<symbol name="LITTLEBITS_FEMALE">
<pin name="VCC"/>
<pin name="SIG"/>
<pin name="GND"/>
</symbol>
<symbol name="LITTLEBITS_MALE">
<pin name="GND"/>
<pin name="SIG"/>
<pin name="VCC"/>
</symbol>
<symbol name="LITTLEBITS">
<pin name="GND"/>
<pin name="SIG"/>
<pin name="VCC"/>
</symbol>
<symbol name="LCD_CFAX">
<description>&lt;h3&gt;CrystalFontz LCD connection&lt;/h3&gt;</description>
<pin name="VCC"/>
<pin name="RESET"/>
<pin name="GND"/>
<pin name="CS1B"/>
<pin name="CS2"/>
<pin name="RS"/>
<pin name="RW"/>
<pin name="ERD"/>
<pin name="MI"/>
<pin name="P/S"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
</symbol>
<symbol name="STW5093">
<pin name="VCC"/>
<pin name="REMOUT"/>
<pin name="REMIN"/>
<pin name="MIC3+"/>
<pin name="MIC3-"/>
<pin name="MBIAS"/>
<pin name="VCCA"/>
<pin name="MIC1+"/>
<pin name="MIC1-"/>
<pin name="GNDA"/>
<pin name="MIC2+"/>
<pin name="MIC2-"/>
<pin name="VCCP"/>
<pin name="VLR-"/>
<pin name="VLR+"/>
<pin name="GNDP"/>
<pin name="VFR"/>
<pin name="LO"/>
<pin name="BZ"/>
<pin name="CCLK"/>
<pin name="CS-"/>
<pin name="CI"/>
<pin name="AUXCLK"/>
<pin name="VCCIO"/>
<pin name="CO"/>
<pin name="GND"/>
<pin name="DX"/>
<pin name="DR"/>
<pin name="FS"/>
<pin name="MCLK"/>
</symbol>
<symbol name="DOSONCHIP-IC">
<pin name="UART_TX" direction="out"/>
<pin name="CARD_SCLK" direction="out"/>
<pin name="SPI_CS" direction="in" function="dot"/>
<pin name="CARD_DIN"/>
<pin name="CARD_WP" direction="in"/>
<pin name="CARD_CD" direction="in" function="dot"/>
<pin name="XTAL_OUT" direction="out"/>
<pin name="XTAL_IN" direction="in"/>
<pin name="SPI_MOSI" direction="in"/>
<pin name="UART_RX" direction="in"/>
<pin name="SPI_MISO" direction="out"/>
<pin name="SPI_SCLK" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="VDD" direction="in"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="MODE0" direction="in"/>
<pin name="CARD_DOUT" direction="out"/>
<pin name="CARD_CS" direction="in" function="dot"/>
<pin name="MODE1" direction="in"/>
<pin name="DIR" direction="in"/>
<pin name="UART_CTS" direction="in"/>
<pin name="UART_RTS/BUSY" direction="out"/>
<pin name="I2C_SCL"/>
<pin name="I2C_SDA"/>
</symbol>
<symbol name="MAX7219">
<pin name="DIN"/>
<pin name="DIG0"/>
<pin name="DIG4"/>
<pin name="GND"/>
<pin name="DIG6"/>
<pin name="DIG2"/>
<pin name="DIG3"/>
<pin name="DIG7"/>
<pin name="GND2"/>
<pin name="DIG5"/>
<pin name="DIG1"/>
<pin name="LOAD"/>
<pin name="CLK"/>
<pin name="SEGA"/>
<pin name="SEGF"/>
<pin name="SEGB"/>
<pin name="SEGG"/>
<pin name="ISET"/>
<pin name="VCC"/>
<pin name="SEGC"/>
<pin name="SEGE"/>
<pin name="SEGDP"/>
<pin name="SEGD"/>
<pin name="DOUT"/>
</symbol>
<symbol name="MAX7456">
<pin name="DVDD"/>
<pin name="DGND"/>
<pin name="CLKIN"/>
<pin name="XFB"/>
<pin name="CLKOUT"/>
<pin name="~CS"/>
<pin name="DIN"/>
<pin name="SCK"/>
<pin name="DOUT"/>
<pin name="LOS"/>
<pin name="~VSYNC"/>
<pin name="~HSYNC"/>
<pin name="~RESET"/>
<pin name="AGND"/>
<pin name="AVDD"/>
<pin name="VIN"/>
<pin name="PGND"/>
<pin name="PVDD"/>
<pin name="SAG"/>
<pin name="VOUT"/>
</symbol>
<symbol name="MCP130">
<pin name="RESET"/>
<pin name="GND"/>
<pin name="VCC"/>
</symbol>
<symbol name="NCP303LSN09">
<pin name="RST"/>
<pin name="IN"/>
<pin name="GND"/>
<pin name="CD"/>
<pin name="NC"/>
</symbol>
<symbol name="STM811">
<pin name="VCC"/>
<pin name="VSS"/>
<pin name="~RST"/>
<pin name="~MR"/>
</symbol>
<symbol name="TLC5940">
<pin name="GND"/>
<pin name="BLANK"/>
<pin name="SCLK"/>
<pin name="SIN"/>
<pin name="VPRG"/>
<pin name="OUT0"/>
<pin name="OUT1"/>
<pin name="OUT2"/>
<pin name="OUT3"/>
<pin name="OUT4"/>
<pin name="OUT5"/>
<pin name="OUT6"/>
<pin name="OUT7"/>
<pin name="OUT8"/>
<pin name="XLAT"/>
<pin name="OUT9"/>
<pin name="OUT10"/>
<pin name="OUT11"/>
<pin name="OUT12"/>
<pin name="OUT13"/>
<pin name="OUT14"/>
<pin name="OUT15"/>
<pin name="XERR"/>
<pin name="SOUT"/>
<pin name="GSCLK"/>
<pin name="DCPRG"/>
<pin name="IREF"/>
<pin name="VCC"/>
</symbol>
<symbol name="XR2206">
<pin name="AMSI" direction="in"/>
<pin name="STO" direction="out"/>
<pin name="MO" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="TC1" direction="in"/>
<pin name="TC2" direction="in"/>
<pin name="TR1" direction="out"/>
<pin name="TR2" direction="out"/>
<pin name="FSKI" direction="in"/>
<pin name="BIAS" direction="out"/>
<pin name="SYNCO" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="WAVEA1" direction="in"/>
<pin name="WAVEA2" direction="in"/>
<pin name="SYMA1" direction="in"/>
<pin name="SYMA2" direction="in"/>
</symbol>
<symbol name="AT42QT1010">
<pin name="OUT"/>
<pin name="VDD"/>
<pin name="VSS"/>
<pin name="SNSK"/>
<pin name="SNS"/>
<pin name="SYNC/MODE"/>
</symbol>
<symbol name="SLB9645">
<pin name="SDA"/>
<pin name="PP"/>
<pin name="!DAVINT#"/>
<pin name="!RESET#"/>
<pin name="SCL"/>
<pin name="GND@4"/>
<pin name="GND@11"/>
<pin name="GND@18"/>
<pin name="GND@25"/>
<pin name="VDD@5"/>
<pin name="VDD@10"/>
</symbol>
<symbol name="FT245R">
<pin name="3V3OUT" direction="out"/>
<pin name="USBDM"/>
<pin name="USBDP"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="OSCI" direction="in"/>
<pin name="OSCO" direction="out"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="D0" direction="out"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="RXF" function="dot"/>
<pin name="TXE" function="dot"/>
<pin name="RD" function="dot"/>
<pin name="WR"/>
<pin name="PWEN"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="TEST" direction="in"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="FT2232D">
<pin name="3V3OUT" direction="out"/>
<pin name="USBDM"/>
<pin name="USBDP"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="BDBUS0" direction="out"/>
<pin name="BDBUS1" direction="in"/>
<pin name="BDBUS2" direction="out"/>
<pin name="BDBUS3" direction="in"/>
<pin name="BDBUS4" direction="out"/>
<pin name="BDBUS5" direction="in"/>
<pin name="BDBUS6" direction="in"/>
<pin name="BDBUS7" direction="in"/>
<pin name="PWEN#"/>
<pin name="VCCIOA" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="TEST" direction="in"/>
<pin name="VCC2" direction="pwr"/>
<pin name="RSTOUT#"/>
<pin name="RESET#"/>
<pin name="XTIN"/>
<pin name="XTOUT"/>
<pin name="EECS"/>
<pin name="EESK"/>
<pin name="EEDATA"/>
<pin name="GND4"/>
<pin name="SI/WUB"/>
<pin name="BCBUS3"/>
<pin name="BCBUS2"/>
<pin name="BCBUS1"/>
<pin name="BCBUS0"/>
<pin name="ACBUS2"/>
<pin name="ACBUS1"/>
<pin name="ACBUS0"/>
<pin name="ADBUS7"/>
<pin name="ADBUS6"/>
<pin name="ADBUS5"/>
<pin name="SI/WUA"/>
<pin name="ACBUS3"/>
<pin name="ADBUS4"/>
<pin name="ADBUS3"/>
<pin name="ADBUS2"/>
<pin name="ADBUS1"/>
<pin name="ADBUS0"/>
<pin name="VCC1" direction="pwr"/>
<pin name="AVCC"/>
<pin name="VCCIOB"/>
</symbol>
<symbol name="MAX485">
<pin name="RO"/>
<pin name="RE" function="dot"/>
<pin name="DE"/>
<pin name="DI"/>
<pin name="GND"/>
<pin name="A"/>
<pin name="B"/>
<pin name="VCC"/>
</symbol>
<symbol name="PL-2303XA">
<pin name="TXD"/>
<pin name="DTR_N"/>
<pin name="RTS_N"/>
<pin name="VDD_325"/>
<pin name="RXD"/>
<pin name="RI_N"/>
<pin name="GND@7"/>
<pin name="VDD_33"/>
<pin name="DSR_N"/>
<pin name="DCD_N"/>
<pin name="CTS_N"/>
<pin name="SHTD_N"/>
<pin name="EE_CLK"/>
<pin name="EE_DATA"/>
<pin name="DP"/>
<pin name="DM"/>
<pin name="VO_33"/>
<pin name="GND@18"/>
<pin name="RESET_N"/>
<pin name="VDD_5"/>
<pin name="GND@21"/>
<pin name="GP0"/>
<pin name="GP1"/>
<pin name="VDD_33A"/>
<pin name="GND_A"/>
<pin name="PLL_TEST"/>
<pin name="OSC1"/>
<pin name="OSC2"/>
</symbol>
<symbol name="SC16IS750">
<pin name="RESET"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VDD"/>
<pin name="I2C-/SPI"/>
<pin name="A0-/CS"/>
<pin name="A1-SI"/>
<pin name="NC-SO"/>
<pin name="SCL-SCLK"/>
<pin name="SDA-VSS"/>
<pin name="/IRQ"/>
<pin name="GPIO0"/>
<pin name="GPIO1"/>
<pin name="GPIO2"/>
<pin name="GPIO3"/>
<pin name="VSS"/>
<pin name="GPIO4-/DSR"/>
<pin name="GPIO5-/DTR"/>
<pin name="GPIO6-/CD"/>
<pin name="GPIO7-/RI"/>
<pin name="/RTS"/>
<pin name="/CTS"/>
<pin name="TX"/>
<pin name="RX"/>
</symbol>
<symbol name="TJA1040TD-T">
<pin name="TXD"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="RXD"/>
<pin name="SPLIT"/>
<pin name="CANL"/>
<pin name="CANH"/>
<pin name="STB"/>
</symbol>
<symbol name="USB3318">
<pin name="DATA7"/>
<pin name="DATA6"/>
<pin name="DATA5"/>
<pin name="DATA4"/>
<pin name="DATA3"/>
<pin name="DATA2"/>
<pin name="DATA1"/>
<pin name="DATA0"/>
<pin name="STP"/>
<pin name="NXT"/>
<pin name="DIR"/>
<pin name="CLKOUT"/>
<pin name="RESETB"/>
<pin name="REFCLK"/>
<pin name="RBIAS"/>
<pin name="VBUS"/>
<pin name="VBAT"/>
<pin name="VDD33"/>
<pin name="VDDIO"/>
<pin name="VDD18"/>
<pin name="DM"/>
<pin name="DP"/>
<pin name="ID"/>
<pin name="CPEN"/>
<pin name="GND1"/>
<pin name="GND2"/>
</symbol>
<symbol name="ISD1932">
<pin name="_REC"/>
<pin name="_PLAYE/FMC2"/>
<pin name="_PLAYL/FMC1"/>
<pin name="S3/_M4"/>
<pin name="S2/_M3"/>
<pin name="S1/_M2"/>
<pin name="S0/_M1"/>
<pin name="E3/_M8"/>
<pin name="E2/_M7"/>
<pin name="E1/_M6"/>
<pin name="E0/_M5"/>
<pin name="_FT"/>
<pin name="MIC+"/>
<pin name="MIC-"/>
<pin name="AGC"/>
<pin name="ROSC"/>
<pin name="SP-"/>
<pin name="SP+"/>
<pin name="VSSP2"/>
<pin name="VSSP1"/>
<pin name="VCCP"/>
<pin name="VSSA"/>
<pin name="VCCA"/>
<pin name="VSSD"/>
<pin name="VCCD"/>
<pin name="XCLK/FMC3"/>
<pin name="_LED"/>
<pin name="ADDR/_DRCT"/>
</symbol>
<symbol name="VS1103">
<pin name="MICP"/>
<pin name="MICN"/>
<pin name="XRESET"/>
<pin name="D_REQ"/>
<pin name="GPIO2/DCLK"/>
<pin name="GPIO3/SDATA"/>
<pin name="XDCS/BSYNC"/>
<pin name="XTAL0"/>
<pin name="XTAL1"/>
<pin name="XCS"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="SCLK"/>
<pin name="SI"/>
<pin name="SO"/>
<pin name="TEST"/>
<pin name="SPIBOOT/GPIO0"/>
<pin name="GPIO1"/>
<pin name="RIGHT"/>
<pin name="GBUF"/>
<pin name="RCAP"/>
<pin name="LEFT"/>
<pin name="AVDD1" direction="pwr"/>
<pin name="AVDD2" direction="pwr"/>
<pin name="AVDD3" direction="pwr"/>
<pin name="AGND1"/>
<pin name="AGND2"/>
<pin name="AGND3"/>
<pin name="AGND4"/>
<pin name="DVDD1" direction="pwr"/>
<pin name="DVDD2" direction="pwr"/>
<pin name="DVDD3" direction="pwr"/>
<pin name="DGND2"/>
<pin name="DGND3"/>
<pin name="DGND4"/>
<pin name="DGND5"/>
<pin name="DGND1" direction="pwr"/>
<pin name="CVDD1"/>
<pin name="CVDD2"/>
<pin name="CVDD3"/>
<pin name="CVDD4"/>
</symbol>
<symbol name="VS1002">
<pin name="MICP"/>
<pin name="MICN"/>
<pin name="XRESET"/>
<pin name="D_REQ"/>
<pin name="GPIO2/DCLK"/>
<pin name="GPIO3/SDATA"/>
<pin name="XDCS/BSYNC"/>
<pin name="XTAL0"/>
<pin name="XTAL1"/>
<pin name="XCS"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="SCLK"/>
<pin name="SI"/>
<pin name="SO"/>
<pin name="TEST"/>
<pin name="SPIBOOT/GPIO0"/>
<pin name="GPIO1"/>
<pin name="RIGHT"/>
<pin name="GBUF"/>
<pin name="RCAP"/>
<pin name="LEFT"/>
<pin name="AVDD1" direction="pwr"/>
<pin name="AVDD2" direction="pwr"/>
<pin name="AVDD3" direction="pwr"/>
<pin name="AGND1"/>
<pin name="AGND2"/>
<pin name="AGND3"/>
<pin name="AGND4"/>
<pin name="DVDD1" direction="pwr"/>
<pin name="DVDD2" direction="pwr"/>
<pin name="DVDD3" direction="pwr"/>
<pin name="DGND2"/>
<pin name="DGND3"/>
<pin name="DGND4"/>
<pin name="DGND5"/>
<pin name="DGND1" direction="pwr"/>
</symbol>
<symbol name="BUFFER-DUAL">
<pin name="A2"/>
<pin name="A1"/>
<pin name="GND"/>
<pin name="Y1"/>
<pin name="VCC"/>
<pin name="Y2"/>
</symbol>
<symbol name="AT25FS010">
<pin name="SI"/>
<pin name="SCK"/>
<pin name="HOLD" function="dot"/>
<pin name="CS" function="dot"/>
<pin name="WP" function="dot"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="SO"/>
</symbol>
<symbol name="AT45DB041B">
<pin name="SI"/>
<pin name="SCK"/>
<pin name="RST" function="dot"/>
<pin name="CS" function="dot"/>
<pin name="WP" function="dot"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="SO"/>
</symbol>
<symbol name="AT45DB161D">
<pin name="CS" function="dot"/>
<pin name="RST" function="dot"/>
<pin name="SCK"/>
<pin name="SI"/>
<pin name="SO"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="WP" function="dot"/>
</symbol>
<symbol name="NAND256">
<pin name="RXB"/>
<pin name="XR"/>
<pin name="XE"/>
<pin name="CL"/>
<pin name="AL"/>
<pin name="XW"/>
<pin name="XWP"/>
<pin name="VDD1"/>
<pin name="VDD2"/>
<pin name="VSS1"/>
<pin name="IO7"/>
<pin name="IO6"/>
<pin name="IO5"/>
<pin name="IO4"/>
<pin name="IO3"/>
<pin name="IO2"/>
<pin name="IO1"/>
<pin name="IO0"/>
<pin name="VSS2"/>
</symbol>
<symbol name="CP2101">
<pin name="REGIN" direction="pas"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="VBUS" direction="in"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="!RST"/>
<pin name="SUSPEND" direction="out"/>
<pin name="!SUSPEND" direction="out"/>
<pin name="RI" direction="in"/>
<pin name="DCD" direction="in"/>
<pin name="DTR" direction="out"/>
<pin name="DSR" direction="in"/>
<pin name="TXD" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="RTS" direction="out"/>
<pin name="CTS" direction="in"/>
<pin name="GND@EXP" direction="pwr"/>
<pin name="GND@M" direction="pwr"/>
</symbol>
<symbol name="CP2103">
<pin name="REGIN" direction="pas"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="VBUS" direction="in"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="!RST"/>
<pin name="SUSPEND" direction="out"/>
<pin name="!SUSPEND" direction="out"/>
<pin name="RI" direction="in"/>
<pin name="DCD" direction="in"/>
<pin name="DTR" direction="out"/>
<pin name="DSR" direction="in"/>
<pin name="TXD" direction="out"/>
<pin name="RXD" direction="in"/>
<pin name="RTS" direction="out"/>
<pin name="CTS" direction="in"/>
<pin name="GND@EXP" direction="pwr"/>
<pin name="GND@M" direction="pwr"/>
<pin name="GPIO_0"/>
<pin name="GPIO_1"/>
<pin name="GPIO_2"/>
<pin name="GPIO_3"/>
<pin name="VIO" direction="pwr"/>
</symbol>
<symbol name="ENC28J60">
<pin name="VCAP"/>
<pin name="VSS"/>
<pin name="CLKOUT"/>
<pin name="/INT"/>
<pin name="NC"/>
<pin name="SO"/>
<pin name="SI"/>
<pin name="SCK"/>
<pin name="CS"/>
<pin name="RESET"/>
<pin name="VSSRX"/>
<pin name="TPIN-"/>
<pin name="TPIN+"/>
<pin name="RBIAS"/>
<pin name="VDDTX"/>
<pin name="TPOUT-"/>
<pin name="TPOUT+"/>
<pin name="VSSTX"/>
<pin name="VDDRX"/>
<pin name="VDDPLL"/>
<pin name="VSSPLL"/>
<pin name="VSSOSC"/>
<pin name="OSC1"/>
<pin name="OSC2"/>
<pin name="VDDOSC"/>
<pin name="LEDB"/>
<pin name="LEDA"/>
<pin name="VDD"/>
</symbol>
<symbol name="M93C46">
<pin name="CS"/>
<pin name="SK"/>
<pin name="DIN"/>
<pin name="DOUT"/>
<pin name="VCC"/>
<pin name="GND"/>
</symbol>
<symbol name="MAX323">
<pin name="NO1"/>
<pin name="COM1"/>
<pin name="IN2"/>
<pin name="V-"/>
<pin name="NO2"/>
<pin name="COM2"/>
<pin name="IN1"/>
<pin name="V+"/>
</symbol>
<symbol name="AD725">
<pin name="STND"/>
<pin name="AGND"/>
<pin name="4FSC"/>
<pin name="APOS"/>
<pin name="CE"/>
<pin name="RIN"/>
<pin name="GIN"/>
<pin name="BIN"/>
<pin name="HSYNC"/>
<pin name="VSYNC"/>
<pin name="DPOS"/>
<pin name="DGND"/>
<pin name="YTRAP"/>
<pin name="LUMA"/>
<pin name="COMP"/>
<pin name="CRMA"/>
</symbol>
<symbol name="AD5330">
<pin name="VDD"/>
<pin name="VREF"/>
<pin name="CS"/>
<pin name="DB0"/>
<pin name="DB1"/>
<pin name="DB2"/>
<pin name="DB3"/>
<pin name="DB4"/>
<pin name="DB5"/>
<pin name="DB6"/>
<pin name="DB7"/>
<pin name="WR"/>
<pin name="CLR"/>
<pin name="PD"/>
<pin name="GND"/>
<pin name="VOUT"/>
<pin name="LDAC"/>
<pin name="GAIN"/>
<pin name="BUF"/>
</symbol>
<symbol name="AD7302">
<pin name="DB7"/>
<pin name="DB6"/>
<pin name="DB5"/>
<pin name="DB4"/>
<pin name="DB3"/>
<pin name="DB2"/>
<pin name="DB1"/>
<pin name="DB0"/>
<pin name="CS"/>
<pin name="WR"/>
<pin name="DGND"/>
<pin name="VOUTA"/>
<pin name="VOUTB"/>
<pin name="AGND"/>
<pin name="REFIN"/>
<pin name="VDD"/>
<pin name="CLR"/>
<pin name="LDAC"/>
<pin name="PD"/>
<pin name="AB"/>
</symbol>
<symbol name="AD7745">
<pin name="/RDY"/>
<pin name="CIN1+"/>
<pin name="CIN1-"/>
<pin name="CIN2+"/>
<pin name="CIN2-"/>
<pin name="EXCA"/>
<pin name="EXCB"/>
<pin name="GND"/>
<pin name="NC"/>
<pin name="REFIN+"/>
<pin name="REFIN-"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="VDD"/>
<pin name="VIN+"/>
<pin name="VIN-"/>
</symbol>
<symbol name="AD7781">
<pin name="SCLK"/>
<pin name="DOUT"/>
<pin name="GAIN"/>
<pin name="AIN+"/>
<pin name="AIN-"/>
<pin name="REFIN+"/>
<pin name="REFIN-"/>
<pin name="BPDSW"/>
<pin name="GND"/>
<pin name="AVDD"/>
<pin name="DVDD"/>
<pin name="*PDRST"/>
<pin name="FILTER"/>
</symbol>
<symbol name="OP-AMP+--1">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="EPAD"/>
</symbol>
<symbol name="OP-AMP-1">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="AD9835">
<pin name="FS_ADJ"/>
<pin name="REFIN"/>
<pin name="REFOUT"/>
<pin name="DVDD"/>
<pin name="DGND"/>
<pin name="MCLK"/>
<pin name="SCLK"/>
<pin name="SDATA"/>
<pin name="FSYNC"/>
<pin name="FSEL"/>
<pin name="PSEL1"/>
<pin name="PSEL0"/>
<pin name="AGND"/>
<pin name="IOUT"/>
<pin name="AVDD"/>
<pin name="COMP"/>
</symbol>
<symbol name="AS3400">
<pin name="AGND"/>
<pin name="LINL"/>
<pin name="LINR"/>
<pin name="VOL_CSDA"/>
<pin name="MODE_CSCL"/>
<pin name="MICL"/>
<pin name="MICS"/>
<pin name="MICR"/>
<pin name="QMICR"/>
<pin name="QLINR"/>
<pin name="IOP1R"/>
<pin name="QOP1R"/>
<pin name="IOP2R"/>
<pin name="QOP2R"/>
<pin name="VSS"/>
<pin name="HPL"/>
<pin name="HPR"/>
<pin name="HPVDD"/>
<pin name="VBAT"/>
<pin name="CPP"/>
<pin name="GND"/>
<pin name="CPN"/>
<pin name="VNEG"/>
<pin name="QMICL"/>
<pin name="PAD"/>
</symbol>
<symbol name="HT8950">
<pin name="SW0"/>
<pin name="SW1"/>
<pin name="SW2"/>
<pin name="VSS"/>
<pin name="AO"/>
<pin name="AIN"/>
<pin name="VDD"/>
<pin name="LAMP"/>
<pin name="AUDIO"/>
<pin name="VREF"/>
<pin name="TS"/>
<pin name="FVIB"/>
<pin name="OSC2"/>
<pin name="OSC1"/>
<pin name="VIB"/>
<pin name="TGU"/>
<pin name="TGD"/>
<pin name="ROB"/>
</symbol>
<symbol name="OP-AMP+-">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="OP-AMP">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LT1014">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="-V" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="+V" direction="pwr"/>
</symbol>
<symbol name="LT1014_2">
<pin name="-IN" direction="pwr"/>
<pin name="+IN" direction="pwr"/>
<pin name="OUT" direction="pwr"/>
</symbol>
<symbol name="LTC6244">
<pin name="-IN"/>
<pin name="+IN"/>
<pin name="-V"/>
<pin name="+V"/>
<pin name="OUT"/>
</symbol>
<symbol name="LTC6244_2">
<pin name="-IN"/>
<pin name="+IN"/>
<pin name="OUT"/>
</symbol>
<symbol name="MCP42XXX">
<pin name="A0"/>
<pin name="W0"/>
<pin name="B0"/>
<pin name="A1"/>
<pin name="W1"/>
<pin name="B1"/>
<pin name="SCK"/>
<pin name="DI"/>
<pin name="DO"/>
<pin name="SHTDWN"/>
<pin name="RST"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="CS"/>
</symbol>
<symbol name="TS3A5017">
<pin name="IN2"/>
<pin name="1S4"/>
<pin name="1S3"/>
<pin name="1S2"/>
<pin name="1S1"/>
<pin name="1D"/>
<pin name="GND"/>
<pin name="2D"/>
<pin name="2S1"/>
<pin name="2S2"/>
<pin name="2S3"/>
<pin name="2S4"/>
<pin name="IN1"/>
<pin name="VCC"/>
<pin name="1EN" function="dot"/>
<pin name="2EN" function="dot"/>
</symbol>
<symbol name="TVP5150-NTSC_DECODER-1">
<pin name="AGND"/>
<pin name="AIP1A"/>
<pin name="AIP1B"/>
<pin name="AVID"/>
<pin name="CH_AGND"/>
<pin name="CH_AVDD"/>
<pin name="DGND"/>
<pin name="DVDD"/>
<pin name="FID/GLCO"/>
<pin name="HSYNC"/>
<pin name="INT_REQ"/>
<pin name="IO_DVDD"/>
<pin name="PCLK/SCLK"/>
<pin name="PDN"/>
<pin name="PLL_AGND"/>
<pin name="PLL_AVDD"/>
<pin name="REFM"/>
<pin name="REFP"/>
<pin name="RESET/"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="VSYNC"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="YOUT_0"/>
<pin name="YOUT_1"/>
<pin name="YOUT_2"/>
<pin name="YOUT_3"/>
<pin name="YOUT_4"/>
<pin name="YOUT_5"/>
<pin name="YOUT_6"/>
<pin name="YOUT_7"/>
</symbol>
<symbol name="X9015_DIGI_POT">
<pin name="VSS" direction="pwr"/>
<pin name="RW/VW"/>
<pin name="VCC" direction="pwr"/>
<pin name="CS'"/>
<pin name="INC'"/>
<pin name="U/D'"/>
<pin name="RH/VH"/>
<pin name="RL/VL"/>
</symbol>
<symbol name="INA139">
<pin name="VIN+"/>
<pin name="VIN-"/>
<pin name="V+"/>
<pin name="GND"/>
<pin name="OUT"/>
</symbol>
<symbol name="HIH6131">
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="AL_L"/>
<pin name="AL_H"/>
<pin name="VDD"/>
<pin name="VCORE"/>
<pin name="GND"/>
<pin name="NC"/>
</symbol>
<symbol name="MAX6675">
<pin name="GND"/>
<pin name="T-"/>
<pin name="T+"/>
<pin name="VCC"/>
<pin name="(MI)SO"/>
<pin name="!CS"/>
<pin name="SCK"/>
</symbol>
<symbol name="GENERIC-8PIN">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
</symbol>
<symbol name="EP2C20_PQ208_PLL">
<pin name="GND_PLL1" direction="pwr"/>
<pin name="GND_PLL1@1" direction="pwr"/>
<pin name="GND_PLL2" direction="pwr"/>
<pin name="GND_PLL2@1" direction="pwr"/>
<pin name="GNDA_PLL1" direction="pwr"/>
<pin name="GNDA_PLL2" direction="pwr"/>
<pin name="VCCD_PLL1" direction="pwr"/>
<pin name="VCCD_PLL2" direction="pwr"/>
<pin name="VCCA_PLL1" direction="pwr"/>
<pin name="VCCA_PLL2" direction="pwr"/>
</symbol>
<symbol name="EP2C20_PQ208_B3">
<pin name="IO_LVDS56N"/>
<pin name="IO_LVDS56P"/>
<pin name="VCCIO3@1"/>
<pin name="IO_LVDS53N"/>
<pin name="IO_LVDS53P"/>
<pin name="IO_LVDS52N"/>
<pin name="IO_LVDS52P"/>
<pin name="IO_LVDS51N"/>
<pin name="IO_LVDS51P"/>
<pin name="IO_VREFB3N1"/>
<pin name="VCCIO3@2"/>
<pin name="IO_LVDS48N"/>
<pin name="IO_LVDS48P"/>
<pin name="CLK7_LVDSCLK3N"/>
<pin name="CLK6_LVDSCLK3P"/>
<pin name="CLK5_LVDSCLK2N"/>
<pin name="CLK4_LVDSCLK2P"/>
<pin name="IO_LVDS47N"/>
<pin name="IO_LVDS47P"/>
<pin name="IO_LVDS46N"/>
<pin name="VCCIO3@3"/>
<pin name="IO_LVDS46P"/>
<pin name="IO_LVDS45N"/>
<pin name="IO_LVDS45P"/>
<pin name="IO_LVDS44N"/>
<pin name="IO_LVDS44P"/>
<pin name="IO_LVDS42N"/>
<pin name="IO_LVDS42P"/>
<pin name="IO_VREFB3N0"/>
<pin name="IO_LVDS39N"/>
<pin name="IO_LVDS39P"/>
<pin name="VCCIO3@4"/>
<pin name="IO_LVDS38N"/>
<pin name="IO_LVDS38P"/>
<pin name="IO_PLL2_OUTP"/>
<pin name="IO_PLL2_OUTN"/>
<pin name="IO@1"/>
</symbol>
<symbol name="EP2C20_PQ208_B1">
<pin name="IO_LVDS14P"/>
<pin name="IO_LVDS14N"/>
<pin name="VCCIO1@1"/>
<pin name="IO_LVDS13P"/>
<pin name="IO_LVDS13N"/>
<pin name="IO_LVDS12P"/>
<pin name="IO_LVDS12N"/>
<pin name="IO_VREFB1N0"/>
<pin name="IO_LVDS8P"/>
<pin name="IO_LVDS8N"/>
<pin name="CLK0_LVDSCLK0P"/>
<pin name="CLK1_LVDSCLK0N"/>
<pin name="CLK2_LVDSCLK1P"/>
<pin name="CLK3_LVDSCLK1N"/>
<pin name="VCCIO1@4"/>
<pin name="IO_LVDS7P"/>
<pin name="IO_LVDS7N"/>
<pin name="IO_LVDS6N"/>
<pin name="IO@2"/>
<pin name="IO_LVDS5P"/>
<pin name="IO_VREFB1N1"/>
<pin name="IO_LVDS3N"/>
<pin name="IO_LVDS2P"/>
<pin name="IO_LVDS2N"/>
<pin name="VCCIO1@6"/>
<pin name="IO@3"/>
<pin name="IO_LVDS0P"/>
<pin name="IO_LVDS0N"/>
<pin name="IO@4"/>
<pin name="IO_PLL1_OUTP"/>
<pin name="IO_PLL1_OUTN"/>
</symbol>
<symbol name="EP2C20_PQ208_B4">
<pin name="IO_LVDS77P"/>
<pin name="IO_LVDS76P"/>
<pin name="IO_LVDS76N"/>
<pin name="IO_LVDS75P"/>
<pin name="IO_LVDS75N"/>
<pin name="VCCIO4@1"/>
<pin name="IO_LVDS74P"/>
<pin name="IO_LVDS74N"/>
<pin name="IO_VREFB4N1"/>
<pin name="IO_LVDS70P"/>
<pin name="IO_LVDS70N"/>
<pin name="IO_LVDS68P"/>
<pin name="IO_LVDS68N"/>
<pin name="VCCIO4@2"/>
<pin name="IO_LVDS67P"/>
<pin name="IO_LVDS67N"/>
<pin name="IO_LVDS66P"/>
<pin name="IO_LVDS66N"/>
<pin name="IO_LVDS64P"/>
<pin name="IO_LVDS64N"/>
<pin name="VCCIO4@3"/>
<pin name="IO_LVDS63P"/>
<pin name="IO_LVDS63N"/>
<pin name="IO_LVDS62P"/>
<pin name="IO_LVDS62N"/>
<pin name="IO_VREFB4N0"/>
<pin name="IO_LVDS61P"/>
<pin name="VCCIO4@4"/>
<pin name="IO_LVDS61N"/>
<pin name="IO_LVDS60P"/>
<pin name="IO_LVDS60N"/>
<pin name="IO@2"/>
<pin name="IO_LVDS59P"/>
<pin name="VCCIO4@5"/>
<pin name="IO_LVDS59N"/>
<pin name="IO_LVDS58P"/>
<pin name="IO_LVDS58N"/>
<pin name="IO_LVDS57P"/>
<pin name="IO_LVDS57N"/>
<pin name="IO@1"/>
</symbol>
<symbol name="EP2C20_PQ208_POWER">
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@12" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="VCCINT@1" direction="pwr"/>
<pin name="VCCINT@2" direction="pwr"/>
<pin name="VCCINT@3" direction="pwr"/>
<pin name="VCCINT@4" direction="pwr"/>
<pin name="VCCINT@5" direction="pwr"/>
<pin name="VCCINT@6" direction="pwr"/>
<pin name="GND@15"/>
<pin name="GND@16"/>
<pin name="GND@17"/>
<pin name="GND@18"/>
<pin name="GND@19"/>
<pin name="GND@20"/>
<pin name="GND@21"/>
<pin name="GND@22"/>
<pin name="GND@23"/>
<pin name="GND@24"/>
<pin name="GND@25"/>
</symbol>
<symbol name="EP2C20_PQ208_B2">
<pin name="IO_LVDS37N"/>
<pin name="IO_LVDS37P"/>
<pin name="IO_LVDS36N"/>
<pin name="IO_LVDS36P"/>
<pin name="IO_LVDS35N"/>
<pin name="IO_LVDS35P"/>
<pin name="VCCIO2@1"/>
<pin name="IO_LVDS34N"/>
<pin name="IO_LVDS34P"/>
<pin name="IO_VREFB2N0"/>
<pin name="IO_LVDS33N"/>
<pin name="VCCIO2@2"/>
<pin name="IO_LVDS33P"/>
<pin name="IO_LVDS31N"/>
<pin name="IO_LVDS31P"/>
<pin name="IO_LVDS29N"/>
<pin name="IO_LVDS29P"/>
<pin name="IO_LVDS28N"/>
<pin name="IO_LVDS28P"/>
<pin name="VCCIO2@3"/>
<pin name="IO_LVDS26P"/>
<pin name="IO_LVDS25N"/>
<pin name="IO_LVDS25P"/>
<pin name="IO_LVDS24N"/>
<pin name="IO_LVDS24P"/>
<pin name="IO_VREFB2N1"/>
<pin name="IO_LVDS23N"/>
<pin name="VCCIO2@4"/>
<pin name="IO_LVDS23P"/>
<pin name="IO_LVDS21N"/>
<pin name="IO_LVDS21P"/>
<pin name="IO_LVDS19N"/>
<pin name="IO_LVDS19P"/>
<pin name="IO_LVDS18N"/>
<pin name="VCCIO2@5"/>
<pin name="IO_LVDS18P"/>
<pin name="IO_LVDS17P"/>
<pin name="IO_LVDS16N"/>
<pin name="IO_LVDS16P"/>
<pin name="IO_LVDS17N"/>
</symbol>
<symbol name="EP2C20_PQ208_CONFIG">
<pin name="ASDO"/>
<pin name="CRC_ERROR"/>
<pin name="TDO"/>
<pin name="TCK"/>
<pin name="DATA0"/>
<pin name="NCSO"/>
<pin name="CLKUSR"/>
<pin name="TMS"/>
<pin name="TDI"/>
<pin name="NCE"/>
<pin name="NCONFIG"/>
<pin name="DEV_OE"/>
<pin name="INIT_DONE"/>
<pin name="NCEO"/>
<pin name="NSTATUS"/>
<pin name="CONF_DONE"/>
<pin name="MSEL1"/>
<pin name="MSEL0"/>
<pin name="DCLK"/>
</symbol>
<symbol name="HEF4543">
<pin name="A"/>
<pin name="B"/>
<pin name="BL"/>
<pin name="C"/>
<pin name="D"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="E"/>
<pin name="F"/>
<pin name="G"/>
<pin name="GND"/>
<pin name="LD"/>
<pin name="PH"/>
<pin name="VCC"/>
</symbol>
<symbol name="PCF8575C">
<pin name="INT"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="PO0"/>
<pin name="PO1"/>
<pin name="PO2"/>
<pin name="PO3"/>
<pin name="PO4"/>
<pin name="PO5"/>
<pin name="PO6"/>
<pin name="PO7"/>
<pin name="GND"/>
<pin name="P10"/>
<pin name="P11"/>
<pin name="P12"/>
<pin name="P13"/>
<pin name="P14"/>
<pin name="P15"/>
<pin name="P16"/>
<pin name="P17"/>
<pin name="A0"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="VCC"/>
</symbol>
<symbol name="STP16CP05/A6282">
<pin name="GND"/>
<pin name="SDI"/>
<pin name="CLK"/>
<pin name="LE"/>
<pin name="OUT0"/>
<pin name="OUT1"/>
<pin name="OUT2"/>
<pin name="OUT3"/>
<pin name="OUT4"/>
<pin name="OUT5"/>
<pin name="OUT6"/>
<pin name="OUT7"/>
<pin name="VDD"/>
<pin name="REXT"/>
<pin name="SDO"/>
<pin name="~OE"/>
<pin name="OUT15"/>
<pin name="OUT14"/>
<pin name="OUT13"/>
<pin name="OUT12"/>
<pin name="OUT11"/>
<pin name="OUT10"/>
<pin name="OUT8"/>
<pin name="OUT9"/>
</symbol>
<symbol name="WS2801">
<pin name="CKI"/>
<pin name="SDI"/>
<pin name="VCC"/>
<pin name="POL"/>
<pin name="CKO"/>
<pin name="SDO"/>
<pin name="BOUT"/>
<pin name="GOUT"/>
<pin name="ROUT"/>
<pin name="BFB"/>
<pin name="GFB"/>
<pin name="RFB"/>
<pin name="GND"/>
</symbol>
<symbol name="XC3S250/500E-PQ208">
<pin name="GND"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="GND@4"/>
<pin name="GND@5"/>
<pin name="GND@6"/>
<pin name="GND@7"/>
<pin name="GND@8"/>
<pin name="GND@9"/>
<pin name="GND@10"/>
<pin name="GND@11"/>
<pin name="GND@12"/>
<pin name="GND@13"/>
<pin name="GND@14"/>
<pin name="GND@15"/>
<pin name="GND@16"/>
<pin name="GND@17"/>
<pin name="GND@18"/>
<pin name="GND@19"/>
<pin name="GND@20"/>
<pin name="VCCAUX"/>
<pin name="VCCAUX@2"/>
<pin name="VCCAUX@3"/>
<pin name="VCCAUX@4"/>
<pin name="VCCAUX@5"/>
<pin name="VCCAUX@6"/>
<pin name="VCCAUX@7"/>
<pin name="VCCAUX@8"/>
<pin name="VCCINT"/>
<pin name="VCCINT@2"/>
<pin name="VCCINT@3"/>
<pin name="VCCINT@4"/>
<pin name="DONE"/>
<pin name="PROG_B"/>
<pin name="TCK"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TMS"/>
<pin name="IO"/>
<pin name="IO/VREF_0"/>
<pin name="IO_L01N_0"/>
<pin name="IO_L01P_0"/>
<pin name="IO_L02N_0/VREF_0"/>
<pin name="IO_L02P_0"/>
<pin name="IO_L03N_0"/>
<pin name="IO_L03P_0"/>
<pin name="IO_L04N_0/VREF_0"/>
<pin name="IO_L04P_0"/>
<pin name="IO_L05N_0"/>
<pin name="IO_L05P_0"/>
<pin name="IO_L07N_0/GCLK5"/>
<pin name="IO_LO7P_0/GCLK4"/>
<pin name="IO_L08N_0/GCLK7"/>
<pin name="IO_L08P_0/GCLK6"/>
<pin name="IO_L10N_0/GCLK11"/>
<pin name="IO_L10P_0/GCLK10"/>
<pin name="IO_L11N_0"/>
<pin name="IO_L11P_0"/>
<pin name="IO_L12N_0/VREF_0"/>
<pin name="IO_L12P_0"/>
<pin name="IO_L13N_0"/>
<pin name="IO_L13P_0"/>
<pin name="IO_L14N_0/VREF_0"/>
<pin name="IO_L15N_0"/>
<pin name="IO_L14P_0"/>
<pin name="IO_L15P_0"/>
<pin name="IO_L16N_0/HSWAP"/>
<pin name="IO_L16P_0"/>
<pin name="IP"/>
<pin name="IP@2"/>
<pin name="IP@3"/>
<pin name="IP@4"/>
<pin name="IP_L06N_0"/>
<pin name="IP_L06P_0"/>
<pin name="IP_LO9N_0/GCLK9"/>
<pin name="IP_L09P_0/GCLK8"/>
<pin name="VCCO_0"/>
<pin name="VCCO_0@2"/>
<pin name="VCCO_0@3"/>
<pin name="IO_L01N_1/A15"/>
<pin name="IO_L01P_1/A16"/>
<pin name="IO_L02N_1/A13"/>
<pin name="IO_L02P_1/A14"/>
<pin name="IO_L03N_1/VREF_1"/>
<pin name="IO_L03P_1"/>
<pin name="IO_L04N_1"/>
<pin name="IO_L04P_1"/>
<pin name="IO_L05N_1/A11"/>
<pin name="IO_L05P_1/A12"/>
<pin name="IO_L06N_1/VREF_1"/>
<pin name="IO_L06P_1"/>
<pin name="IO_L07N_1/A7/RHCLK1"/>
<pin name="IO_L07P_1/A10/RHCLK0"/>
<pin name="IO_L08N_1/A7/RHCLK3"/>
<pin name="IO_L08P_1/A8/RHCLK2"/>
<pin name="IO_L09N_1/A5/RHCLK5"/>
<pin name="IO_L09P_1/A6/RHCLK4"/>
<pin name="IO_L10N_1/A3/RHCLK7"/>
<pin name="IO_L10P_1/A4/RHCLK6"/>
<pin name="IO_L11N_1/A1"/>
<pin name="IO_L11P_1/A2"/>
<pin name="IO_L12N_1/A0"/>
<pin name="IO_L12P_1"/>
<pin name="IO_L13N_1"/>
<pin name="IO_L13P_1"/>
<pin name="IO_L14N_1"/>
<pin name="IO_L14P_1"/>
<pin name="IO_L15_1/LDC0"/>
<pin name="IO_L15P_1/HDC"/>
<pin name="IO_L16N_1/LDC2"/>
<pin name="IO_16P_1/LDC1"/>
<pin name="IP@5"/>
<pin name="IP@6"/>
<pin name="IP@7"/>
<pin name="IP@8"/>
<pin name="IP@9"/>
<pin name="IP@10"/>
<pin name="IP@11"/>
<pin name="IP/VREF_1"/>
<pin name="VCC0_1"/>
<pin name="VCC0_1@2"/>
<pin name="VCC0_1@3"/>
<pin name="IO/D5"/>
<pin name="IO/M1"/>
<pin name="IO/VREF_2"/>
<pin name="IO/L01N_2/INIT_B"/>
<pin name="IO_L01P_2/CSO_B"/>
<pin name="IO_L03N_2/MOSI/CSI_B"/>
<pin name="IO_L03P_2/DOUT/BUSY"/>
<pin name="IO_L04N_2"/>
<pin name="IO_L04P_2"/>
<pin name="IO_L05N_2"/>
<pin name="IO_L05P_2"/>
<pin name="IO_L06N_2"/>
<pin name="IO_L06P_2"/>
<pin name="IO_L08N_2/D6/GCLK13"/>
<pin name="10_L08P_2/D7/GCLK12"/>
<pin name="IO_L09N_2/D3/GCLK15"/>
<pin name="IO_L09P_2/D4/GCLK14"/>
<pin name="IO_L11N_2/D1/GCLK3"/>
<pin name="IO_L11P_2/D2/GCLK2"/>
<pin name="IO_L12N_2/DIN/D0"/>
<pin name="IO_L12P_2/M0"/>
<pin name="IO_L13N_2"/>
<pin name="IO_L13P_2"/>
<pin name="IO_L14N_2/A22"/>
<pin name="IO_L14P_2/A23"/>
<pin name="IO_L15N_2/A20"/>
<pin name="IO_L15P_2/A21"/>
<pin name="IO_L16N_2/VS1/A18"/>
<pin name="IO_L16P_2/VS2/A19"/>
<pin name="IO_L17N_2/CCLK"/>
<pin name="IO_L17P_2/VS0/A17"/>
<pin name="IP@12"/>
<pin name="IP@13"/>
<pin name="IP@14"/>
<pin name="IP_L02N_2"/>
<pin name="IP_L02P_2"/>
<pin name="IP_L07N_2/VREF_2"/>
<pin name="IP_L07P_2"/>
<pin name="IP_L10N_2/M2/GCLK1"/>
<pin name="IP_L10P_2/RDWR_B/GCLK0"/>
<pin name="VCCO_2"/>
<pin name="VCCO_2@2"/>
<pin name="VCCO_2@3"/>
<pin name="IO/VREF_3"/>
<pin name="IO_L01N_3"/>
<pin name="IO_L01P_3"/>
<pin name="IO_L02N_3/VREF_3"/>
<pin name="IO_L02P_3"/>
<pin name="IO_L03N_3"/>
<pin name="IO_L03P_3"/>
<pin name="IO_L04N_3"/>
<pin name="IO_L04P_3"/>
<pin name="IO_L05N_3"/>
<pin name="IO_L05P_3"/>
<pin name="IO_L06N_3"/>
<pin name="IO_L06P_3"/>
<pin name="IO_L07N_3/LHCLK1"/>
<pin name="IO_L07P_3/LHCLK0"/>
<pin name="IO_L08N_3/LHCLK3"/>
<pin name="IO_L08P_3/LHCLK2"/>
<pin name="IO_L09N_3/LHCLK5"/>
<pin name="IO_L09P_3/LHCLK4"/>
<pin name="IO_L10N_3/LHCLK7"/>
<pin name="IO_L10P_3/LHCLK6"/>
<pin name="IO_L11N_3"/>
<pin name="IO_L11P_3"/>
<pin name="IO_L12N_3"/>
<pin name="IO_L12P_3"/>
<pin name="IO_L13N_3"/>
<pin name="IO_L13P_3"/>
<pin name="IO_L14N_3"/>
<pin name="IO_L14P_3"/>
<pin name="IO_L15N_3"/>
<pin name="IO_L15P_3"/>
<pin name="IO_L16N_3"/>
<pin name="IO_L16P_3"/>
<pin name="IP@15"/>
<pin name="IP@16"/>
<pin name="IP@17"/>
<pin name="IP@18"/>
<pin name="IP@19"/>
<pin name="IP@20"/>
<pin name="IP/VREF_3"/>
<pin name="VCCO_3"/>
<pin name="VCCO_3@2"/>
<pin name="VCCO_3@3"/>
</symbol>
<symbol name="XS1-L1-64LQFP">
<pin name="VDDIO_6"/>
<pin name="VDDIO_18"/>
<pin name="VDDIO_32"/>
<pin name="VDDIO_40"/>
<pin name="VDDIO_53"/>
<pin name="VDDIO_60"/>
<pin name="VDD_4"/>
<pin name="VDD_13"/>
<pin name="VDD_21"/>
<pin name="VDD_28"/>
<pin name="VDD_37"/>
<pin name="VDD_43"/>
<pin name="VDD_52"/>
<pin name="VDD_61"/>
<pin name="PLL_AVDD"/>
<pin name="PLL_AGND"/>
<pin name="MODE0"/>
<pin name="MODE1"/>
<pin name="MODE2"/>
<pin name="MODE3"/>
<pin name="DEBUG"/>
<pin name="RST_N"/>
<pin name="CLK"/>
<pin name="TDO"/>
<pin name="TDI"/>
<pin name="TMS"/>
<pin name="TCK"/>
<pin name="TRST_N"/>
<pin name="GND"/>
<pin name="X0D0"/>
<pin name="X0D1"/>
<pin name="X0D2"/>
<pin name="X0D3"/>
<pin name="X0D4"/>
<pin name="X0D5"/>
<pin name="X0D6"/>
<pin name="X0D7"/>
<pin name="X0D8"/>
<pin name="X0D9"/>
<pin name="X0D10"/>
<pin name="X0D11"/>
<pin name="X0D12"/>
<pin name="X0D13"/>
<pin name="X0D14"/>
<pin name="X0D15"/>
<pin name="X0D16"/>
<pin name="X0D17"/>
<pin name="X0D18"/>
<pin name="X0D19"/>
<pin name="X0D20"/>
<pin name="X0D21"/>
<pin name="X0D22"/>
<pin name="X0D23"/>
<pin name="X0D24"/>
<pin name="X0D25"/>
<pin name="X0D26"/>
<pin name="X0D32"/>
<pin name="X0D33"/>
<pin name="X0D34"/>
<pin name="X0D35"/>
<pin name="X0D36"/>
<pin name="X0D37"/>
<pin name="X0D38"/>
<pin name="X0D27"/>
<pin name="X0D39"/>
</symbol>
<symbol name="A6282">
<pin name="GND@1"/>
<pin name="SDI"/>
<pin name="CLK"/>
<pin name="LE"/>
<pin name="OUT0"/>
<pin name="OUT1"/>
<pin name="OUT2"/>
<pin name="OUT3"/>
<pin name="OUT4"/>
<pin name="OUT5"/>
<pin name="OUT6"/>
<pin name="OUT7"/>
<pin name="VDD"/>
<pin name="REXT"/>
<pin name="SDO"/>
<pin name="~OE"/>
<pin name="OUT15"/>
<pin name="OUT14"/>
<pin name="OUT13"/>
<pin name="OUT12"/>
<pin name="OUT11"/>
<pin name="OUT10"/>
<pin name="OUT8"/>
<pin name="OUT9"/>
<pin name="GND@2"/>
</symbol>
<symbol name="74HC03">
<pin name="Y1"/>
<pin name="A1"/>
<pin name="B1"/>
<pin name="Y2"/>
<pin name="A2"/>
<pin name="B2"/>
<pin name="Y3"/>
<pin name="A3"/>
<pin name="B3"/>
<pin name="Y4"/>
<pin name="A4"/>
<pin name="B4"/>
<pin name="VCC"/>
<pin name="VSS"/>
</symbol>
<symbol name="M74HC238">
<pin name="VCC"/>
<pin name="A"/>
<pin name="B"/>
<pin name="C"/>
<pin name="G1"/>
<pin name="~G2B"/>
<pin name="~G2A"/>
<pin name="GND"/>
<pin name="Y7"/>
<pin name="Y6"/>
<pin name="Y5"/>
<pin name="Y4"/>
<pin name="Y3"/>
<pin name="Y2"/>
<pin name="Y1"/>
<pin name="Y0"/>
</symbol>
<symbol name="74157">
<pin name="!A!/B" direction="in"/>
<pin name="1A" direction="in"/>
<pin name="1B" direction="in"/>
<pin name="1Y" direction="out"/>
<pin name="2A" direction="in"/>
<pin name="2B" direction="in"/>
<pin name="2Y" direction="out"/>
<pin name="3A" direction="in"/>
<pin name="3B" direction="in"/>
<pin name="3Y" direction="out"/>
<pin name="4A" direction="in"/>
<pin name="4B" direction="in"/>
<pin name="4Y" direction="out"/>
<pin name="G" direction="in" function="dot"/>
</symbol>
<symbol name="POWER_CONSORT">
<pin name="P$V+"/>
<pin name="P$V-"/>
</symbol>
<symbol name="CAP-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="RESISTOR">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="ALPHANUMERIC">
<pin name="A1"/>
<pin name="A2"/>
<pin name="B"/>
<pin name="C"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="E"/>
<pin name="F"/>
<pin name="G1"/>
<pin name="G2"/>
<pin name="H"/>
<pin name="J"/>
<pin name="K"/>
<pin name="L"/>
<pin name="M"/>
<pin name="N"/>
<pin name="NC@1"/>
<pin name="NC@13"/>
<pin name="VCC@6"/>
<pin name="VCC@18"/>
</symbol>
<symbol name="7-SEGMENT-DISPLAY">
<pin name="A"/>
<pin name="B"/>
<pin name="C"/>
<pin name="D"/>
<pin name="DP"/>
<pin name="E"/>
<pin name="F"/>
<pin name="G"/>
<pin name="G1"/>
<pin name="G2"/>
</symbol>
<symbol name="7-SEGMENT-4DIGIT">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="11"/>
<pin name="13"/>
<pin name="14"/>
<pin name="15"/>
<pin name="16"/>
</symbol>
<symbol name="BATTERY">
<pin name="-" direction="pwr"/>
<pin name="+" direction="pwr"/>
</symbol>
<symbol name="BUTTON-CONDUCTIVE">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="SEWTAP">
<pin name="1"/>
</symbol>
<symbol name="CAPSENSE_PAD">
<pin name="RES"/>
<pin name="RECEIVE"/>
</symbol>
<symbol name="2-POS-DIP">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
</symbol>
<symbol name="SW_DIP-8">
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="FKIT-BATTERY">
<pin name="NEG"/>
<pin name="POS"/>
</symbol>
<symbol name="FKIT-CONNECTOR_COND_03">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
</symbol>
<symbol name="FKIT-SNAP_CONNECTOR">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
</symbol>
<symbol name="G3VM-61E1">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
</symbol>
<symbol name="HEATSINK-SMD-2">
<pin name="P$1"/>
<pin name="P$2"/>
</symbol>
<symbol name="N35P112">
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="RESETN"/>
<pin name="ADDR"/>
<pin name="VDDP"/>
<pin name="VDD"/>
<pin name="INTN"/>
<pin name="SWITCHN"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="GND3"/>
<pin name="GND4"/>
<pin name="GND5"/>
</symbol>
<symbol name="POT">
<pin name="A" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="SWITCH-MOMENTARY-2-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="RELAY-SOLIDSTATE">
<pin name="T1"/>
<pin name="T2"/>
<pin name="+"/>
<pin name="-"/>
</symbol>
<symbol name="RELAY-SPDT">
<pin name="COIL2"/>
<pin name="MAIN"/>
<pin name="NO"/>
<pin name="NC"/>
<pin name="COIL1"/>
</symbol>
<symbol name="RELAY-SPDT-2">
<pin name="9"/>
<pin name="6"/>
<pin name="10"/>
<pin name="1"/>
<pin name="2"/>
<pin name="5"/>
</symbol>
<symbol name="SWITCH-4PDT">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
</symbol>
<symbol name="AYZ0202">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
</symbol>
<symbol name="SWITCH-MOMENTARY-2-CLOSED">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="SWITCH-MOMENTARY-2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="TOGGLE">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
</symbol>
<symbol name="SPST">
<pin name="P" direction="pas"/>
<pin name="O" direction="pas"/>
</symbol>
<symbol name="SW_SPDT">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
</symbol>
<symbol name="TURRET">
<pin name="1"/>
</symbol>
<symbol name="TRIMPOT-1">
<pin name="CCW" direction="pas"/>
<pin name="CW" direction="pas"/>
<pin name="WIPER" direction="pas"/>
</symbol>
<symbol name="SMARTCARD">
<pin name="VCC"/>
<pin name="RST"/>
<pin name="CLK"/>
<pin name="SW1"/>
<pin name="SW2"/>
<pin name="I/O"/>
<pin name="VPP"/>
<pin name="GND"/>
<pin name="C4"/>
<pin name="C8"/>
</symbol>
<symbol name="SMA_EDGE">
<pin name="GND@0"/>
<pin name="SIGNAL"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
</symbol>
<symbol name="TOUCH-SCREEN">
<pin name="TS4"/>
<pin name="TS3"/>
<pin name="TS2"/>
<pin name="TS1"/>
</symbol>
<symbol name="DIL-40-6">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
<pin name="P$9"/>
<pin name="P$10"/>
<pin name="P$11"/>
<pin name="P$12"/>
<pin name="P$13"/>
<pin name="P$14"/>
<pin name="P$15"/>
<pin name="P$16"/>
<pin name="P$17"/>
<pin name="P$18"/>
<pin name="P$19"/>
<pin name="P$20"/>
<pin name="P$21"/>
<pin name="P$22"/>
<pin name="P$23"/>
<pin name="P$24"/>
<pin name="P$25"/>
<pin name="P$26"/>
<pin name="P$27"/>
<pin name="P$28"/>
<pin name="P$29"/>
<pin name="P$30"/>
<pin name="P$31"/>
<pin name="P$32"/>
<pin name="P$33"/>
<pin name="P$34"/>
<pin name="P$35"/>
<pin name="P$36"/>
<pin name="P$37"/>
<pin name="P$38"/>
<pin name="P$39"/>
<pin name="P$40"/>
</symbol>
<symbol name="ZUNE_CONNECTOR_MALE">
<pin name="USB_5V@1"/>
<pin name="USB_5V@2"/>
<pin name="USB_5V@3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="VIDEO+"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
<pin name="AUDIO_L"/>
<pin name="AUDIO_R"/>
<pin name="15"/>
<pin name="16"/>
<pin name="17"/>
<pin name="18"/>
<pin name="GND@19"/>
<pin name="USB_DATA-"/>
<pin name="USB_DATA+"/>
<pin name="GND@22"/>
<pin name="GND@23"/>
<pin name="GND@24"/>
</symbol>
<symbol name="ATMEGA8U2">
<pin name="AVCC"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="GND"/>
<pin name="PB0"/>
<pin name="PB1(SCK)"/>
<pin name="PB2(MOSI)"/>
<pin name="PB3(MISO)"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PC2"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2(RX)"/>
<pin name="PD3(TX)"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6(RTS)"/>
<pin name="PD7(CTS)"/>
<pin name="RESET/PC1"/>
<pin name="UCAP"/>
<pin name="UGND"/>
<pin name="UVCC"/>
<pin name="VCC"/>
<pin name="XTAL1"/>
<pin name="XTAL2/PC0"/>
</symbol>
<symbol name="ATTINY13">
<pin name="VCC"/>
<pin name="PB1(MISO)"/>
<pin name="PB5(NRES)"/>
<pin name="GND"/>
<pin name="PB0(MOSI)"/>
<pin name="PB2(SCK/ADC1)"/>
<pin name="PB3(ADC3)"/>
<pin name="PB4(ADC2)"/>
</symbol>
<symbol name="ATTINY24">
<pin name="VCC"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3/RESET"/>
<pin name="PA7/ADC7"/>
<pin name="PA6/MOSI"/>
<pin name="PA5/MISO"/>
<pin name="PA4/SCL"/>
<pin name="PA3/ADC3"/>
<pin name="PA2/ADC2"/>
<pin name="PA1/ADC1"/>
<pin name="PA0/ADC0"/>
<pin name="GND"/>
<pin name="GND@0"/>
</symbol>
<symbol name="23-I/O">
<pin name="PB5(SCK)"/>
<pin name="PB7(XTAL2/TOSC2)"/>
<pin name="PB6(XTAL1/TOSC1)"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="VCC@1"/>
<pin name="VCC@2"/>
<pin name="AGND"/>
<pin name="AREF"/>
<pin name="AVCC"/>
<pin name="PB4(MISO)"/>
<pin name="PB3(MOSI/OC2)"/>
<pin name="PB2(SS/OC1B)"/>
<pin name="PB1(OC1A)"/>
<pin name="PB0(ICP)"/>
<pin name="PD7(AIN1)"/>
<pin name="PD6(AIN0)"/>
<pin name="PD5(T1)"/>
<pin name="PD4(XCK/T0)"/>
<pin name="PD3(INT1)"/>
<pin name="PD2(INT0)"/>
<pin name="PD1(TXD)"/>
<pin name="PD0(RXD)"/>
<pin name="ADC7"/>
<pin name="ADC6"/>
<pin name="PC5(ADC5/SCL)"/>
<pin name="PC4(ADC4/SDA)"/>
<pin name="PC3(ADC3)"/>
<pin name="PC2(ADC2)"/>
<pin name="PC1(ADC1)"/>
<pin name="PC0(ADC0)"/>
<pin name="PC6(/RESET)" function="dot"/>
</symbol>
<symbol name="23-I/O-2">
<pin name="PB5(SCK)"/>
<pin name="PB7(XTAL2/TOSC2)"/>
<pin name="PB6(XTAL1/TOSC1)"/>
<pin name="GND@1"/>
<pin name="VCC@1"/>
<pin name="AGND"/>
<pin name="AREF"/>
<pin name="AVCC"/>
<pin name="PB4(MISO)"/>
<pin name="PB3(MOSI/OC2)"/>
<pin name="PB2(SS/OC1B)"/>
<pin name="PB1(OC1A)"/>
<pin name="PB0(ICP)"/>
<pin name="PD7(AIN1)"/>
<pin name="PD6(AIN0)"/>
<pin name="PD5(T1)"/>
<pin name="PD4(XCK/T0)"/>
<pin name="PD3(INT1)"/>
<pin name="PD2(INT0)"/>
<pin name="PD1(TXD)"/>
<pin name="PD0(RXD)"/>
<pin name="PC5(ADC5/SCL)"/>
<pin name="PC4(ADC4/SDA)"/>
<pin name="PC3(ADC3)"/>
<pin name="PC2(ADC2)"/>
<pin name="PC1(ADC1)"/>
<pin name="PC0(ADC0)"/>
<pin name="PC6(/RESET)" function="dot"/>
</symbol>
<symbol name="CY7C64215">
<pin name="VSS@1"/>
<pin name="P07"/>
<pin name="P05"/>
<pin name="P03"/>
<pin name="P01"/>
<pin name="P25"/>
<pin name="P23"/>
<pin name="P21"/>
<pin name="P17"/>
<pin name="P15"/>
<pin name="P13"/>
<pin name="P11"/>
<pin name="VSS@13"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="VDD@16"/>
<pin name="P10"/>
<pin name="P12"/>
<pin name="P14"/>
<pin name="P16"/>
<pin name="P20"/>
<pin name="P22"/>
<pin name="P24"/>
<pin name="P00"/>
<pin name="P02"/>
<pin name="P04"/>
<pin name="P06"/>
<pin name="VDD@28"/>
</symbol>
<symbol name="DSPIC30F4011">
<pin name="MCLR"/>
<pin name="RB0/AREF+"/>
<pin name="RB1/AREF-"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="RB4/IC7"/>
<pin name="RB5/IC8"/>
<pin name="RB6"/>
<pin name="RB7"/>
<pin name="RB8"/>
<pin name="VDD0"/>
<pin name="VSS0"/>
<pin name="OSC1"/>
<pin name="OSC2"/>
<pin name="RC13/TX1"/>
<pin name="RC14/RX1"/>
<pin name="INT0/RE8"/>
<pin name="OC2/RD1"/>
<pin name="RD3"/>
<pin name="VSS1"/>
<pin name="VDD1"/>
<pin name="RD2"/>
<pin name="OC1/RD0"/>
<pin name="RF6/SCK1"/>
<pin name="PGD/SCL"/>
<pin name="PGC/SDA"/>
<pin name="RF5/TX2"/>
<pin name="RF4/RX2"/>
<pin name="RF1"/>
<pin name="RF0"/>
<pin name="VSS2"/>
<pin name="VDD2"/>
<pin name="RE5"/>
<pin name="RE4"/>
<pin name="RE3"/>
<pin name="RE2"/>
<pin name="RE1"/>
<pin name="RE0"/>
<pin name="AVSS"/>
<pin name="AVDD"/>
</symbol>
<symbol name="DSPIC30F6015">
<pin name="VDD@10"/>
<pin name="VDD@26"/>
<pin name="VDD@38"/>
<pin name="VDD@57"/>
<pin name="AVDD@19"/>
<pin name="MCLR@7"/>
<pin name="PGC@17"/>
<pin name="PGD@18"/>
<pin name="OSC1@39"/>
<pin name="OSC2@40"/>
<pin name="RX1@34"/>
<pin name="TX1@33"/>
<pin name="VREF+/RB0@16"/>
<pin name="VREF-/RB1@15"/>
<pin name="RB2@14"/>
<pin name="RB3@13"/>
<pin name="RB4@12"/>
<pin name="RB5@11"/>
<pin name="RB8@21"/>
<pin name="RB9@22"/>
<pin name="RB10@23"/>
<pin name="RB11@24"/>
<pin name="RB12@27"/>
<pin name="RB13@28"/>
<pin name="RB14@29"/>
<pin name="RB15@30"/>
<pin name="GND@56"/>
<pin name="GND@41"/>
<pin name="GND@25"/>
<pin name="GND@9"/>
<pin name="AGND@20"/>
<pin name="RC13@47"/>
<pin name="RC14@48"/>
<pin name="RD0@46"/>
<pin name="RD1@49"/>
<pin name="RD2@50"/>
<pin name="RD3@51"/>
<pin name="RD4@52"/>
<pin name="RD5@53"/>
<pin name="RD6@54"/>
<pin name="RD7@55"/>
<pin name="RG8@6"/>
<pin name="RG9@8"/>
<pin name="RG2@37"/>
<pin name="RD8@42"/>
<pin name="RF6@35"/>
<pin name="RG3@36"/>
<pin name="RD9@43"/>
<pin name="RD10@44"/>
<pin name="RD11@45"/>
<pin name="RF0@58"/>
<pin name="RF1@59"/>
<pin name="RE0@60"/>
<pin name="RE1@61"/>
<pin name="RE2@62"/>
<pin name="RE3@63"/>
<pin name="RG7@5"/>
<pin name="RG6@4"/>
<pin name="RE7@3"/>
<pin name="RE6@2"/>
<pin name="RE5@1"/>
<pin name="RE4@64"/>
<pin name="TX2@31"/>
<pin name="RX2@32"/>
</symbol>
<symbol name="DSPIC33FJ256GP710_POWER">
<pin name="VSS@75"/>
<pin name="VDD@2"/>
<pin name="VDD@86"/>
<pin name="VCAP"/>
<pin name="VDD@46"/>
<pin name="VSS@45"/>
<pin name="VDD@37"/>
<pin name="VSS@36"/>
<pin name="RA9/VREF-"/>
<pin name="RA10/VREF+"/>
<pin name="VDD@16"/>
<pin name="VSS@15"/>
<pin name="VSS@65"/>
<pin name="VDD@62"/>
<pin name="AVDD"/>
<pin name="AVSS"/>
</symbol>
<symbol name="DSPIC33FJ256GP710_CONTROL">
<pin name="RB0/AN0"/>
<pin name="RB1/AN1"/>
<pin name="RB3/AN3"/>
<pin name="RB4/AN4"/>
<pin name="RB5/AN5"/>
<pin name="RB6/AN6"/>
<pin name="RB7/AN7"/>
<pin name="RB8/AN8"/>
<pin name="RB9/AN9"/>
<pin name="RB10/AN10"/>
<pin name="RB11/AN11"/>
<pin name="RB12/AN12"/>
<pin name="RB13/AN13"/>
<pin name="RG2/SCL1"/>
<pin name="RG3/SDA1"/>
<pin name="RD8/IC1"/>
<pin name="RD9/IC2"/>
<pin name="RD14/U1CTS/IC7"/>
<pin name="RD15/U1RTS/IC8"/>
<pin name="RD10/IC3"/>
<pin name="RD11/IC4"/>
<pin name="RD0/OC1"/>
<pin name="RD3/OC4"/>
<pin name="RD4/OC5"/>
<pin name="RD12/IC5"/>
<pin name="RD13/IC6"/>
<pin name="RD5/OC6"/>
<pin name="RD6/OC7"/>
<pin name="RD7/OC8"/>
<pin name="RD1/OC2"/>
<pin name="RD2/OC3"/>
<pin name="RF2/U1RX"/>
<pin name="RF3/U1TX"/>
<pin name="RB14/AN14"/>
<pin name="RC4/AN19"/>
<pin name="RA6/AN22"/>
<pin name="RE4"/>
<pin name="RE3"/>
<pin name="RE2"/>
<pin name="RE1/AN25"/>
</symbol>
<symbol name="DSPIC33FJ256GP710_EXTERNAL">
<pin name="RB15/AN15"/>
<pin name="RC1/AN16"/>
<pin name="RC2/AN17"/>
<pin name="RC3/AN18"/>
<pin name="RA12/INT1"/>
<pin name="RA13/INT2"/>
<pin name="RA7/AN23"/>
<pin name="RG6/SCK2"/>
<pin name="RG7/SDI2"/>
<pin name="RG8/SDO2"/>
<pin name="RG9/SS2"/>
<pin name="RF4/U2RX"/>
<pin name="RF5/U2TX"/>
<pin name="RF13/U2RTS"/>
<pin name="RF12/U2CTS"/>
<pin name="RC14/PGEC2"/>
<pin name="RC13/PGED2"/>
<pin name="MCLR"/>
<pin name="RF1/C1TX1"/>
<pin name="RF0/C1RX1"/>
<pin name="RF6/SCK1"/>
<pin name="RF7/SDI1"/>
<pin name="RF8/SDO1"/>
<pin name="RA2/SCL2"/>
<pin name="RA3/SDA2"/>
<pin name="RB2/SS1"/>
<pin name="RE0/AN24"/>
<pin name="RA1"/>
<pin name="RA5/TDO"/>
<pin name="RA4/TDI"/>
<pin name="RA14"/>
</symbol>
<symbol name="DSPIC33FJ256GP710_EXTRA">
<pin name="RE5/AN29"/>
<pin name="RE6/AN30"/>
<pin name="RE7/AN31"/>
<pin name="RG0/C2RX"/>
<pin name="RG1/C2TX"/>
<pin name="RG13/CSDO"/>
<pin name="RG12/CSDI"/>
<pin name="RG14/CSCK"/>
<pin name="RA0/TMS"/>
<pin name="RA15"/>
<pin name="RC15/OSC2"/>
<pin name="RC12/OSC1"/>
<pin name="RG15/COFS"/>
</symbol>
<symbol name="LPC213X">
<pin name="P1.16(TRACEPKT0)"/>
<pin name="P1.17(TRACEPKT1)"/>
<pin name="P1.18(TRACEPKT2)"/>
<pin name="P1.19(TRACEPKT3)"/>
<pin name="P1.20(TRACESYNC)"/>
<pin name="P1.21(PIPESTAT0)"/>
<pin name="P1.22(PIPESTAT1)"/>
<pin name="P1.23(PIPESTAT2)"/>
<pin name="(MISO0/MAT0.1/A0.7)P0.5"/>
<pin name="(SSEL0/PWM2/EINT2)P0.7"/>
<pin name="(TXD1/PWM4/A1.1)P0.8"/>
<pin name="(RXD1/PWM6/EINT3)P0.9"/>
<pin name="(RTS1/CAP1.0/AD1.2)P0.10"/>
<pin name="(CTS1/CAP1.1/SCL1)P0.11"/>
<pin name="P1.24(TRACECLK)"/>
<pin name="P1.25(EXTIN0)"/>
<pin name="P1.26(RTCK)"/>
<pin name="P1.27(TDO)"/>
<pin name="P1.28(TDI)"/>
<pin name="P1.29(TCK)"/>
<pin name="P1.30(TMS)"/>
<pin name="P1.31(/TRST)"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="(DSR1/MAT1.0/AD1.3)P0.12"/>
<pin name="(DTR1/MAT1.1/AD1.4)P0.13"/>
<pin name="(DCD1/EINT1/SDA1)P0.14"/>
<pin name="(RI1/EINT2/AD1.5)P0.15"/>
<pin name="(EINT0/MAT0.2/CAP0.2)P0.16"/>
<pin name="(CAP1.2/SCK1/MAT1.2)P0.17"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VREF" direction="in"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VDDA3" direction="pwr"/>
<pin name="VDD3-1" direction="pwr"/>
<pin name="VDD3-2" direction="pwr"/>
<pin name="VDD3-3" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="(TXD0/PWM1)P0.0"/>
<pin name="(RXD0/PWM3/EINT0)P0.1"/>
<pin name="(SCL0/CAP0.0)P0.2"/>
<pin name="(SDA0/MAT0.0/EINT1)P0.3"/>
<pin name="(SCK0/CAP0.1/AD0.6)P0.4"/>
<pin name="(MOSI0/CAP0.2/AD1.0)P0.6"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="RTXC1" direction="in"/>
<pin name="RTXC2" direction="out"/>
<pin name="(CAP1.3/MISO1/MAT1.3)P0.18"/>
<pin name="(MAT1.2/MOSI1/CAP1.2)P0.19"/>
<pin name="(MAT1.3/SSEL1/EINT3)P0.20"/>
<pin name="(PWM5/AD1.6/CAP1.3)P0.21"/>
<pin name="(AD1.7/CAP0.0/MAT0.0)P0.22"/>
<pin name="P0.23"/>
<pin name="(AD0.4/AOUT)P0.25"/>
<pin name="(AD0.5)P0.26"/>
<pin name="(AD0.0/CAP0.1/MAT0.1)P0.27"/>
<pin name="(AD0.1/CAP0.2/MAT0.2)P0.28"/>
<pin name="(AD0.2/CAP0.3/MAT0.3)P0.29"/>
<pin name="(AD0.3/EINT3/CAP0.0)P0.30"/>
<pin name="P0.31" direction="out"/>
</symbol>
<symbol name="LPC2103">
<pin name="P0.19/MAT1.2/MISO1"/>
<pin name="P0.20/MAT1.3/MOSI1"/>
<pin name="P0.21/SSEL1/MAT3.0"/>
<pin name="VBAT"/>
<pin name="VDD(1V8)"/>
<pin name="RST"/>
<pin name="VSS@7"/>
<pin name="P0.27/TRST/CAP2.0"/>
<pin name="P0.28/TMS/CAP2.1"/>
<pin name="P0.29/TCK/CAP2.2"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="P0.0/TXD0/MAT3.1"/>
<pin name="P0.1/RXD0/MAT3.2"/>
<pin name="P0.30/TDI/MAT3.3"/>
<pin name="P0.31/TDO"/>
<pin name="VDD(3V3)@17"/>
<pin name="P0.2/SCL0/CAP0.0"/>
<pin name="VSS@19"/>
<pin name="RTCX1"/>
<pin name="P0.3/SDA0/MAT0.0"/>
<pin name="P0.4/SCK0/CAP0.1"/>
<pin name="P0.5/MISO0/MAT0.1"/>
<pin name="P0.6/MOSI0/CAP0.2"/>
<pin name="RTCX2"/>
<pin name="RTCK"/>
<pin name="DBGSEL"/>
<pin name="P0.7/SSEL0/MAT2.0"/>
<pin name="P0.8/TXD1/MAT2.1"/>
<pin name="P0.9/RXD1/MAT2.2"/>
<pin name="VSSA"/>
<pin name="P0.22/AD0.0"/>
<pin name="P0.23/AD0.1"/>
<pin name="P0.24/AD0.2"/>
<pin name="P0.10/RTS1/CAP1.0/AD0.3"/>
<pin name="P0.11/CTS1/CAP1.1/AD0.4"/>
<pin name="P0.12/DSR1/MAT1.0/AD0.5"/>
<pin name="P0.25/AD0.6"/>
<pin name="P0.26/AD0.7"/>
<pin name="VDD(3V3)@40"/>
<pin name="P0.13/DTR1/MAT1.1"/>
<pin name="VDDA"/>
<pin name="VSS@43"/>
<pin name="P0.14/DCD1/SCK1/EINT1"/>
<pin name="P0.15/RI1/EINT2"/>
<pin name="P0.16/EINT0/MAT0.2"/>
<pin name="P0.17/CAP1.2/SCL1"/>
<pin name="P0.18/CAP1.3/SDA1"/>
</symbol>
<symbol name="MC9S12XS64">
<pin name="PWM3/KWP3/PP3"/>
<pin name="TXD1/IOC2/PWM2/KWP2/PP2"/>
<pin name="IOC1/PWM1/KWP1/PP1"/>
<pin name="RXD1/IOC0/PWM0/KWP0/PP0"/>
<pin name="IOC0/PT0"/>
<pin name="IOC1/PT1"/>
<pin name="IOC2/PT2"/>
<pin name="IOC3/PT3"/>
<pin name="VDDF"/>
<pin name="VSS1"/>
<pin name="PWM4/IOC4/PT4"/>
<pin name="VREG_API/PWM5/IOC5/PT"/>
<pin name="PWM6/IOC6/PT6"/>
<pin name="PWM7/IOC7/PT7"/>
<pin name="MODC/BKGD"/>
<pin name="PB0"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="XCLKS/ECLKX2/PE7"/>
<pin name="ECLK/PE4"/>
<pin name="VSSX2"/>
<pin name="VDDX2"/>
<pin name="RESET"/>
<pin name="VDDR"/>
<pin name="VSS3"/>
<pin name="VSSPLL"/>
<pin name="EXTAL"/>
<pin name="XTAL"/>
<pin name="VDDPLL"/>
<pin name="IRQ/PE1"/>
<pin name="XIRQ/PE0"/>
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="VDD"/>
<pin name="VSS2"/>
<pin name="PAD00/AN00"/>
<pin name="PAD01/AN01"/>
<pin name="PAD02/AN02"/>
<pin name="PAD03/AN03"/>
<pin name="PAD04/AN04"/>
<pin name="PAD05/AN05"/>
<pin name="PAD06/AN06"/>
<pin name="PAD07/AN07"/>
<pin name="VDDA"/>
<pin name="VRH"/>
<pin name="VSSA/VRL"/>
<pin name="PS0/RXD0"/>
<pin name="PS1/TXD0"/>
<pin name="PS2/RXD1"/>
<pin name="PS3/TXD1"/>
<pin name="TEST"/>
<pin name="PM5/SCK0"/>
<pin name="PM4/MOSI0"/>
<pin name="PM3/SS0"/>
<pin name="PM2/MISO0"/>
<pin name="PM1/TXCAN0/TXD1"/>
<pin name="PM0/RXCAN0/RXD1"/>
<pin name="VSSX1"/>
<pin name="VDDX1"/>
<pin name="PP7/KWP7/PWM7"/>
<pin name="PP5/KPW5/PWM5"/>
</symbol>
<symbol name="4VDD4VSS">
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
</symbol>
<symbol name="P8X32A">
<pin name="BOE/" direction="in"/>
<pin name="P0"/>
<pin name="P1"/>
<pin name="P2"/>
<pin name="P3"/>
<pin name="P4"/>
<pin name="P5"/>
<pin name="P6"/>
<pin name="P7"/>
<pin name="P8"/>
<pin name="P9"/>
<pin name="P10"/>
<pin name="P11"/>
<pin name="P12"/>
<pin name="P13"/>
<pin name="P14"/>
<pin name="P15"/>
<pin name="P16"/>
<pin name="P17"/>
<pin name="P18"/>
<pin name="P19"/>
<pin name="P20"/>
<pin name="P21"/>
<pin name="P22"/>
<pin name="P23"/>
<pin name="P24"/>
<pin name="P25"/>
<pin name="P26"/>
<pin name="P27"/>
<pin name="P28"/>
<pin name="P29"/>
<pin name="P30"/>
<pin name="P31"/>
<pin name="RES/"/>
<pin name="XI" direction="in"/>
<pin name="XO" direction="out"/>
</symbol>
<symbol name="PIC16F688">
<pin name="RA3/MCLR"/>
<pin name="RA5/OSC1"/>
<pin name="RA0/PGD"/>
<pin name="RC2/AN6"/>
<pin name="RC1/AN5"/>
<pin name="RC0/AN4"/>
<pin name="RA2/AN2"/>
<pin name="RA1/PGC"/>
<pin name="RC3/AN7"/>
<pin name="RC4/TX"/>
<pin name="RC5/RX"/>
<pin name="RA4/OSC2"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="PIC16F883">
<pin name="RX/RC7" direction="in"/>
<pin name="RA2/AN2"/>
<pin name="RA3/AN3"/>
<pin name="RA4"/>
<pin name="TX/RC6"/>
<pin name="RC5/SDO"/>
<pin name="RB0/INT0"/>
<pin name="RC4/SDI"/>
<pin name="RB4/AN11"/>
<pin name="RB5/PGM"/>
<pin name="RB6/PGC"/>
<pin name="RB7/PGD"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@19" direction="pwr"/>
<pin name="RB2/INT2/AN8"/>
<pin name="RB1/INT1/AN10"/>
<pin name="OSC2"/>
<pin name="OSC1"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA5/AN4"/>
<pin name="MCLR/VPP"/>
<pin name="RB3/AN9"/>
<pin name="VDD" direction="pwr"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="RC3/SCK"/>
<pin name="RC0"/>
</symbol>
<symbol name="PIC16F913">
<pin name="RX/RC7/SDA" direction="in"/>
<pin name="RA2/AN2"/>
<pin name="RA3/AN3"/>
<pin name="RA4"/>
<pin name="TX/RC6/SCL"/>
<pin name="RC5"/>
<pin name="RB0/INT0"/>
<pin name="RC4/SD0"/>
<pin name="RB4"/>
<pin name="RB5"/>
<pin name="RB6/PGC"/>
<pin name="RB7/PGD"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@19" direction="pwr"/>
<pin name="RB2"/>
<pin name="RB1"/>
<pin name="RA6/OSC2"/>
<pin name="RA7/OSC1"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA5/AN4"/>
<pin name="MCLR/VPP"/>
<pin name="RB3"/>
<pin name="VDD" direction="pwr"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="RC3"/>
<pin name="RC0"/>
</symbol>
<symbol name="PIC18F2550">
<pin name="RX/RC7" direction="in"/>
<pin name="RA2/AN2"/>
<pin name="RA3/AN3"/>
<pin name="RA4/AN4"/>
<pin name="TX/RC6"/>
<pin name="RC5/D+"/>
<pin name="RB0/INT0"/>
<pin name="RC4/D-"/>
<pin name="RB4/AN11"/>
<pin name="RB5/PGM"/>
<pin name="RB6/PGC"/>
<pin name="RB7/PGD"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@19" direction="pwr"/>
<pin name="RB2/INT2/AN8"/>
<pin name="RB1/INT1/AN10"/>
<pin name="OSC2"/>
<pin name="OSC1"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA5/AN4"/>
<pin name="MCLR/VPP"/>
<pin name="RB3/AN9"/>
<pin name="VDD" direction="pwr"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="V-USB"/>
<pin name="RC0"/>
</symbol>
<symbol name="PIC24HJ32GP202">
<pin name="AN0/VREF+/CN2/RA0"/>
<pin name="AN1/VREF-/CN2/RA1"/>
<pin name="AN4/RP2/CN6/RB2"/>
<pin name="AN5/RP3/CN7/RB3"/>
<pin name="AN9/RP15/CN11/RB15"/>
<pin name="AN10/RP14/CN12/RB14"/>
<pin name="AN11/RP13/CN13/RB13"/>
<pin name="AN12/RP12/CN14/RB12"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="INT0/RP7/CN23/RB7"/>
<pin name="MCLR" direction="in"/>
<pin name="OSCO/CLKO/CN29/RA3" direction="out"/>
<pin name="OSCI/CLKI/CN30/RA2" direction="in"/>
<pin name="PGEC1/AN3/C2IN+/RP1/CN5/RB1"/>
<pin name="PGEC2/TMS/RP11/CN15/RB11"/>
<pin name="PGEC3/ASCL1/RP6/CN24/RB6"/>
<pin name="PGED1/AN2/C2IN-/RP0/CN4/RB0"/>
<pin name="PGED2/TDI/RP10/CN16/RB10"/>
<pin name="PGED3/ASDA1/RP5/CN27/RB5"/>
<pin name="SOSCI/RP4/CN1/RB4"/>
<pin name="SOSCO/T1CK/CN0/RA4"/>
<pin name="TCK/SCL/RP8/CN22/RB8"/>
<pin name="TDO/SDA1/RP9/CN12/RB9"/>
<pin name="VCAP/VDDCORE" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
</symbol>
<symbol name="PIC32MX440F512H">
<pin name="RE5/PMD5"/>
<pin name="RE6/PMD6"/>
<pin name="RE7/PMD7"/>
<pin name="RG6/PMA5/SCK2/CN8"/>
<pin name="RG7/PMA4/SDI2/CN9"/>
<pin name="RG8/PMA3/SDO2/CN10"/>
<pin name="~MCLR"/>
<pin name="RG9/PMA2/~SS2/CN11"/>
<pin name="VSS@9"/>
<pin name="VDD@10"/>
<pin name="RB5/AN5/VBUSON/C1IN+/CN7"/>
<pin name="RB4/AN4/C1IN-/CN6"/>
<pin name="RB3/AN3/C2IN+/CN5"/>
<pin name="RB2/AN2/C2IN-/CN4"/>
<pin name="RB1/AN1/PGEC1/VREF-/CVREF-/CN3"/>
<pin name="RB0/AN0/PGED1/EMUD1/PMA6/VREF+/CVREF+/CN2"/>
<pin name="RB6/AN6/PGEC2/OCFA"/>
<pin name="RB7/AN7/PGED2"/>
<pin name="AVDD"/>
<pin name="AVSS"/>
<pin name="RB8/AN8/~U2CTS/C1OUT"/>
<pin name="RB9/AN9/PMA7/C2OUT"/>
<pin name="RB10/AN10/TMS/CVREFOUT/PMA13"/>
<pin name="RB11/AN11/TDO/PMA12"/>
<pin name="VSS@25"/>
<pin name="VDD@26"/>
<pin name="RB12/AN12/TCK/PMA11"/>
<pin name="RB13/AN13/TDI/PMA10"/>
<pin name="RB14/AN14/PMALH/PMA1/~U2RTS/BCLK2"/>
<pin name="RB15/AN15/PMALL/PMA0/OCFB/CN12"/>
<pin name="RF4/PMA9/U2RX/SDA2/CN17"/>
<pin name="RF5/PMA8/U2TX/SCL2/CN18"/>
<pin name="RF3/USBID"/>
<pin name="VBUS"/>
<pin name="VUSB"/>
<pin name="D-/RG3"/>
<pin name="D+/RG2"/>
<pin name="VDD@38"/>
<pin name="RC12/OSC1/CLKI"/>
<pin name="RC15/OSC2/CLKO"/>
<pin name="VSS@41"/>
<pin name="RD8/IC1/RTCC/INT1"/>
<pin name="RD9/IC2/~U1CTS//INT2/SDA1"/>
<pin name="RD10/IC3/PMCS2/PMA15/INT3/SCL1"/>
<pin name="RD11/IC4/PMCS1/PMA14/INT4"/>
<pin name="RD0/OC1/INT0"/>
<pin name="RC13/SOSCI/CN1"/>
<pin name="RC14/SOSCO/T1CK/CN0"/>
<pin name="RD1/OC2/~U1RTS/BCLK1"/>
<pin name="RD2/OC3/U1RX"/>
<pin name="RD3/OC4/U1TX"/>
<pin name="RD4/PMWR/OC5/IC5/CN13"/>
<pin name="RD5/PMRD/CN14"/>
<pin name="RD6/CN15"/>
<pin name="RD7/CN16"/>
<pin name="VCAP/VDDCORE"/>
<pin name="ENVREG"/>
<pin name="RF0"/>
<pin name="RF1"/>
<pin name="RE0/PMD0"/>
<pin name="RE1/PMD1"/>
<pin name="RE2/PMD2"/>
<pin name="RE3/PMD3"/>
<pin name="RE4/PMD4"/>
</symbol>
<symbol name="UBW32_PIC32MX4XXL">
<pin name="AVDD"/>
<pin name="AVSS"/>
<pin name="C1IN-/AN4/CN6/RB4"/>
<pin name="C1OUT/AN8/RB8"/>
<pin name="C2IN+/AN3/CN5/RB3"/>
<pin name="C2IN-/AN2/CN4/RB2"/>
<pin name="C2OUT/AN9/RB9"/>
<pin name="CN20/U1CTS/RD14"/>
<pin name="CVREFOUT/PMA13/AN10/RB10"/>
<pin name="D+/RG2"/>
<pin name="D-/RG3"/>
<pin name="ENVREG"/>
<pin name="IC1/RTCC/RD8"/>
<pin name="IC2/SS1/RD9"/>
<pin name="IC3/SCKI/PMCS2/PMA15/RD10"/>
<pin name="IC4/PMCS1/PMA14/RD11"/>
<pin name="INT1/RE8"/>
<pin name="INT2/RE9"/>
<pin name="MCLR"/>
<pin name="OC2/RD1"/>
<pin name="OC3/RD2"/>
<pin name="OC4/RD3"/>
<pin name="OSC1/CLKI/RC12"/>
<pin name="OSC2/CLKO/RC15"/>
<pin name="PGC1/EMUC1/AN1/CN3/RB1"/>
<pin name="PGC2/EMUC2/AN6/OCFA/RB6"/>
<pin name="PGD1/EMUD1/AN0/CN2/RB0"/>
<pin name="PGD2/EMUD2/AN7/RB7"/>
<pin name="PMA2/SS2/CN11/RG9"/>
<pin name="PMA3/SDO2/CN10/RG8"/>
<pin name="PMA4/SDI2/CN9/RG7"/>
<pin name="PMA5/SCK2/CN8/RG6"/>
<pin name="PMA6/VREF+/CVREF+/RA10"/>
<pin name="PMA7/VREF-/CVREF-/RA9"/>
<pin name="PMA8/U2TX/CN18/RF5"/>
<pin name="PMA9/U2RX/CN17/RF4"/>
<pin name="PMA10/AN13/RB13"/>
<pin name="PMA11/AN12/RB12"/>
<pin name="PMA12/AN11/RB11"/>
<pin name="PMALH/PMA1/AN14/RB14"/>
<pin name="PMALL/PMA0/AN15/OCFB/CN12/RB15"/>
<pin name="PMD0/RE0"/>
<pin name="PMD1/RE1"/>
<pin name="PMD2/RE2"/>
<pin name="PMD3/RE3"/>
<pin name="PMD4/RE4"/>
<pin name="PMD5/RE5"/>
<pin name="PMD6/RE6"/>
<pin name="PMD7/RE7"/>
<pin name="PMD8/RG0"/>
<pin name="PMD9/RG1"/>
<pin name="PMD10/RF1"/>
<pin name="PMD11/RF0"/>
<pin name="PMD12/IC5/RD12"/>
<pin name="PMD13/CN19/RD13"/>
<pin name="PMD14/CN15/RD6"/>
<pin name="PMD15/CN16/RD7"/>
<pin name="PMRD/CN14/RD5"/>
<pin name="PMWR/OC5/CN13/RD4"/>
<pin name="RG15"/>
<pin name="SCL1/INT3/RA14"/>
<pin name="SCL2/RA2"/>
<pin name="SDA1/INT4/RA15"/>
<pin name="SDA2/RA3"/>
<pin name="SDI1/T5CK/RC4"/>
<pin name="SDO1/OC1/INT0/RD0"/>
<pin name="SOSCI/CN1/RC13"/>
<pin name="SOSCO/T1CK/CN0/RC14"/>
<pin name="T2CK/RC1"/>
<pin name="T3CK/RC2"/>
<pin name="T4CK/RC3"/>
<pin name="TCK/RA1"/>
<pin name="TDI/RA4"/>
<pin name="TDO/RA5"/>
<pin name="TMS/RA0"/>
<pin name="TRCLK/RA6"/>
<pin name="TRD0/RG13"/>
<pin name="TRD1/RG12"/>
<pin name="TRD2/RG14"/>
<pin name="TRD3/RA7"/>
<pin name="U1RTS/BCLK1/CN21/RD15"/>
<pin name="U1RX/RF2"/>
<pin name="U1TX/RF8"/>
<pin name="U2CTS/RF12"/>
<pin name="U2RTS/BCLK2/RF13"/>
<pin name="USBID/RF3"/>
<pin name="VBUS"/>
<pin name="VBUSON/C1IN+/AN5/CN7/RB5"/>
<pin name="VCAP/VDDCORE"/>
<pin name="VDD1"/>
<pin name="VDD2"/>
<pin name="VDD3"/>
<pin name="VDD4"/>
<pin name="VDD5"/>
<pin name="VSS1"/>
<pin name="VSS2"/>
<pin name="VSS3"/>
<pin name="VSS4"/>
<pin name="VSS6"/>
<pin name="VUSB"/>
</symbol>
<symbol name="XMEGA">
<pin name="GND@84"/>
<pin name="GND@93"/>
<pin name="AVCC@4"/>
<pin name="AVCC@94"/>
<pin name="GND@3"/>
<pin name="GND@13"/>
<pin name="GND@23"/>
<pin name="GND@33"/>
<pin name="GND@43"/>
<pin name="GND@53"/>
<pin name="GND@63"/>
<pin name="GND@73"/>
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PDI/PDI_DATA"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="PE7"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PH0"/>
<pin name="PH1"/>
<pin name="PH2"/>
<pin name="PH3"/>
<pin name="PH4"/>
<pin name="PH5"/>
<pin name="PH6"/>
<pin name="PH7"/>
<pin name="PJ0"/>
<pin name="PJ1"/>
<pin name="PJ2"/>
<pin name="PJ3"/>
<pin name="PJ4"/>
<pin name="PJ5"/>
<pin name="PJ6"/>
<pin name="PJ7"/>
<pin name="PK0"/>
<pin name="PK1"/>
<pin name="PK2"/>
<pin name="PK3"/>
<pin name="PK4"/>
<pin name="PK5"/>
<pin name="PK6"/>
<pin name="PK7"/>
<pin name="PQ0"/>
<pin name="PQ1"/>
<pin name="PQ2"/>
<pin name="PQ3"/>
<pin name="PR0"/>
<pin name="PR1"/>
<pin name="RESET/PDI_CLOCK"/>
<pin name="VCC@14"/>
<pin name="VCC@24"/>
<pin name="VCC@34"/>
<pin name="VCC@44"/>
<pin name="VCC@54"/>
<pin name="VCC@64"/>
<pin name="VCC@74"/>
<pin name="VCC@83"/>
</symbol>
<symbol name="XMEGA-A3B">
<pin name="/RESET_PDI_CLK"/>
<pin name="PDI_DATA"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="GND3"/>
<pin name="GND4"/>
<pin name="GND5"/>
<pin name="AVCC"/>
<pin name="AGND"/>
<pin name="VCC1"/>
<pin name="VCC2"/>
<pin name="VCC3"/>
<pin name="VCC4"/>
<pin name="VCC5"/>
<pin name="PF5"/>
<pin name="PR0(XTAL2)"/>
<pin name="PR1(XTAL1)"/>
<pin name="PA0(ADC0/AC0/AREF)"/>
<pin name="PA1(ADC1/AC1)"/>
<pin name="PA2(ADC2/AC2)"/>
<pin name="PA3(ADC3/AC3)"/>
<pin name="PA4(ADC4/AC4)"/>
<pin name="PA5(ADC5/AC5)"/>
<pin name="PA6(ADC6/AC6)"/>
<pin name="PA7(ADC7/AC7/AC0OUT)"/>
<pin name="PB0(ADC0/AC0/AREF)"/>
<pin name="PB1(ADC1/AC1)"/>
<pin name="PB2(ADC2/AC2/DAC0)"/>
<pin name="PB3(ADC3/AC3/DAC1)"/>
<pin name="PB4(ADC4/AC4/TMS)"/>
<pin name="PB5(ADC5/AC5/TDI)"/>
<pin name="PB6(ADC6/AC6/TCK)"/>
<pin name="PB7(ADC7/AC7/AC0OUT/TDO)"/>
<pin name="PC1(OC0B/AC0AH/XCK0/SCL)"/>
<pin name="PC0(OC0A/OC0AL/SDA)"/>
<pin name="PC2(OC0C/OC0BL/RXD0)"/>
<pin name="PC3(OC0D/OX0BH/TXD0)"/>
<pin name="PC4(AC1A/OC0CL/SS)"/>
<pin name="PC5(OC1B/OC0CH/XCK1/MOSI)"/>
<pin name="PC6(OC0DL/RXD1/MISO)"/>
<pin name="PC7(OC0DH/CKOUT/EVO/TXD1/SCK)"/>
<pin name="PD0(OC0A)"/>
<pin name="PD1(OC0B/XCK0)"/>
<pin name="PD2(OC0C/RXD0)"/>
<pin name="PD3(OX0D/TXD0)"/>
<pin name="PD4(OC1A/SS)"/>
<pin name="PD5(OC1B/XCK1/MOSI)"/>
<pin name="PD6(RXD1/MISO)"/>
<pin name="PD7(CKOUT/EVO/TXD1/SCK)"/>
<pin name="PE0(OC0A/SDA)"/>
<pin name="PE1(OC0B/XCK0/SCL)"/>
<pin name="PE2(OC0C/RXD0)"/>
<pin name="PE3(OC0D/TXD0)"/>
<pin name="PE4(OC1A/SS)"/>
<pin name="PE5(OC1B/XCK1/MOSI)"/>
<pin name="PE6(TOSC2/RXD1/MISO)"/>
<pin name="PE7(TOSC1/CKOUT/EVO/TXD1/SCK)"/>
<pin name="PF0(OC0A)"/>
<pin name="PF1(OC0B/XCK0)"/>
<pin name="PF2(OC0C/RXD0)"/>
<pin name="PF3(OC0D/TXD0)"/>
<pin name="PF4"/>
<pin name="PF6"/>
<pin name="PF7"/>
</symbol>
<symbol name="LPC213X-1">
<description>LPC2144/2146/2148</description>
<pin name="D-"/>
<pin name="(AD0.1/CAP0.2/MAT0.2)P0.28"/>
<pin name="(AD0.2/CAP0.3/MAT0.3)P0.29"/>
<pin name="(AD0.3/EINT3/CAP0.0)P0.30"/>
<pin name="(AD0.4/AOUT)P0.25"/>
<pin name="D+"/>
<pin name="(AD1.7/CAP0.0/MAT0.0)P0.22"/>
<pin name="(CAP1.2/SCK1/MAT1.2)P0.17"/>
<pin name="(CAP1.3/MISO1/MAT1.3)P0.18"/>
<pin name="(CTS1/CAP1.1/SCL1)P0.11"/>
<pin name="(DCD1/EINT1/SDA1)P0.14"/>
<pin name="(DSR1/MAT1.0/AD1.3)P0.12"/>
<pin name="(DTR1/MAT1.1/AD1.4)P0.13"/>
<pin name="(EINT0/MAT0.2/CAP0.2)P0.16"/>
<pin name="(MAT1.2/MOSI1/CAP1.2)P0.19"/>
<pin name="(MAT1.3/SSEL1/EINT3)P0.20"/>
<pin name="(MISO0/MAT0.1/A0.7)P0.5"/>
<pin name="(MOSI0/CAP0.2/AD1.0)P0.6"/>
<pin name="(PWM5/AD1.6/CAP1.3)P0.21"/>
<pin name="(RI1/EINT2/AD1.5)P0.15"/>
<pin name="(RTS1/CAP1.0/AD1.2)P0.10"/>
<pin name="(RXD0/PWM3/EINT0)P0.1"/>
<pin name="(RXD1/PWM6/EINT3)P0.9"/>
<pin name="(SCK0/CAP0.1/AD0.6)P0.4"/>
<pin name="(SCL0/CAP0.0)P0.2"/>
<pin name="(SDA0/MAT0.0/EINT1)P0.3"/>
<pin name="(SSEL0/PWM2/EINT2)P0.7"/>
<pin name="(TXD0/PWM1)P0.0"/>
<pin name="(TXD1/PWM4/A1.1)P0.8"/>
<pin name="(VBUS)P0.23"/>
<pin name="(UP_LED/CONNECT)P0.31"/>
<pin name="P1.16(TRACEPKT0)"/>
<pin name="P1.17(TRACEPKT1)"/>
<pin name="P1.18(TRACEPKT2)"/>
<pin name="P1.19(TRACEPKT3)"/>
<pin name="P1.20(TRACESYNC)"/>
<pin name="P1.21(PIPESTAT0)"/>
<pin name="P1.22(PIPESTAT1)"/>
<pin name="P1.23(PIPESTAT2)"/>
<pin name="P1.24(TRACECLK)"/>
<pin name="P1.25(EXTIN0)"/>
<pin name="P1.26(RTCK)"/>
<pin name="P1.27(TDO)"/>
<pin name="P1.28(TDI)"/>
<pin name="P1.29(TCK)"/>
<pin name="P1.30(TMS)"/>
<pin name="P1.31(/TRST)"/>
<pin name="!RESET" direction="in" function="dot"/>
<pin name="RTXC1" direction="in"/>
<pin name="RTXC2" direction="out"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VREF" direction="in"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
</symbol>
<symbol name="USB+SHIELD">
<description>&lt;h3&gt;USB A/B - with Shield Pins&lt;/h3&gt;
&lt;p&gt;USB connector for type-A and type-B connectors. Includes 2 shield pins broken out. &lt;/p&gt;</description>
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="S1"/>
<pin name="S2"/>
</symbol>
<symbol name="USB">
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS"/>
<pin name="GND"/>
</symbol>
<symbol name="CONN_06">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="CONN_04">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="COMPUTER-PERIPHERAL-POWER">
<pin name="12V" direction="pas"/>
<pin name="NC" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="5V" direction="pas"/>
</symbol>
<symbol name="PINH2X12">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
<pin name="21" direction="pas" function="dot"/>
<pin name="22" direction="pas" function="dot"/>
<pin name="23" direction="pas" function="dot"/>
<pin name="24" direction="pas" function="dot"/>
</symbol>
<symbol name="PINH2X3">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="PINH2X10">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
</symbol>
<symbol name="PINH2X26">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
<pin name="21" direction="pas" function="dot"/>
<pin name="22" direction="pas" function="dot"/>
<pin name="23" direction="pas" function="dot"/>
<pin name="25" direction="pas" function="dot"/>
<pin name="27" direction="pas" function="dot"/>
<pin name="29" direction="pas" function="dot"/>
<pin name="31" direction="pas" function="dot"/>
<pin name="33" direction="pas" function="dot"/>
<pin name="35" direction="pas" function="dot"/>
<pin name="37" direction="pas" function="dot"/>
<pin name="39" direction="pas" function="dot"/>
<pin name="41" direction="pas" function="dot"/>
<pin name="43" direction="pas" function="dot"/>
<pin name="45" direction="pas" function="dot"/>
<pin name="47" direction="pas" function="dot"/>
<pin name="49" direction="pas" function="dot"/>
<pin name="51" direction="pas" function="dot"/>
<pin name="24" direction="pas" function="dot"/>
<pin name="26" direction="pas" function="dot"/>
<pin name="28" direction="pas" function="dot"/>
<pin name="30" direction="pas" function="dot"/>
<pin name="32" direction="pas" function="dot"/>
<pin name="34" direction="pas" function="dot"/>
<pin name="36" direction="pas" function="dot"/>
<pin name="38" direction="pas" function="dot"/>
<pin name="40" direction="pas" function="dot"/>
<pin name="42" direction="pas" function="dot"/>
<pin name="44" direction="pas" function="dot"/>
<pin name="46" direction="pas" function="dot"/>
<pin name="48" direction="pas" function="dot"/>
<pin name="50" direction="pas" function="dot"/>
<pin name="52" direction="pas" function="dot"/>
</symbol>
<symbol name="RASPBERRYPI-GPIO">
<pin name="3.3V@1" direction="pwr"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="GP4"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GP17"/>
<pin name="GP27"/>
<pin name="GP22"/>
<pin name="3.3V@17" direction="pwr"/>
<pin name="MOSI" direction="out"/>
<pin name="MISO" direction="in"/>
<pin name="SCLK" direction="out"/>
<pin name="GND@25" direction="pwr"/>
<pin name="CE1" direction="out"/>
<pin name="CE0" direction="out"/>
<pin name="GP25"/>
<pin name="GND@20" direction="pwr"/>
<pin name="GP24"/>
<pin name="GP23"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GP18#"/>
<pin name="RXI" direction="in"/>
<pin name="TXO" direction="out"/>
<pin name="GND@6" direction="pwr"/>
<pin name="5V@4" direction="pwr"/>
<pin name="5V@2" direction="pwr"/>
</symbol>
<symbol name="AUDIO-JACK5-TRS-NORMALED">
<pin name="RING"/>
<pin name="EARTH"/>
<pin name="TIP"/>
<pin name="TIP-NORM"/>
<pin name="RING-NORM"/>
</symbol>
<symbol name="USDCARD">
<pin name="CS"/>
<pin name="DI"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="SCK"/>
<pin name="RSV"/>
<pin name="DO"/>
<pin name="NC"/>
<pin name="SHIELD@3"/>
<pin name="SHIELD@1"/>
<pin name="CD1"/>
<pin name="CD2"/>
</symbol>
<symbol name="USDCARD_SDIO">
<pin name="CD/DAT3"/>
<pin name="CMD"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="CLK"/>
<pin name="DAT1"/>
<pin name="DAT0"/>
<pin name="DAT2"/>
<pin name="SHIELD@3"/>
<pin name="SHIELD@1"/>
<pin name="CD1"/>
<pin name="CD2"/>
</symbol>
<symbol name="DRV8830">
<pin name="VCC" direction="pwr"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="!FAULT" direction="out"/>
<pin name="ISENSE"/>
<pin name="OUT2" direction="pwr"/>
<pin name="OUT1" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="PPAD" direction="pwr"/>
</symbol>
<symbol name="ADM1087">
<pin name="ENIN"/>
<pin name="GND"/>
<pin name="VIN"/>
<pin name="ENOUT"/>
<pin name="CEXT"/>
<pin name="VCC"/>
</symbol>
<symbol name="BD10KA5WF-E2">
<pin name="OUT"/>
<pin name="VCC"/>
<pin name="GND1"/>
<pin name="GND2"/>
<pin name="CTL"/>
</symbol>
<symbol name="HV826MG_BACKLIGHT">
<pin name="RSW"/>
<pin name="VA"/>
<pin name="VCC"/>
<pin name="VB"/>
<pin name="CS"/>
<pin name="LX"/>
<pin name="REL" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="LM4128-2.5VREF">
<pin name="VIN"/>
<pin name="EN"/>
<pin name="GND"/>
<pin name="VOUT"/>
</symbol>
<symbol name="LMZ14203">
<pin name="VIN"/>
<pin name="RON"/>
<pin name="EN"/>
<pin name="GND"/>
<pin name="SS"/>
<pin name="FB"/>
<pin name="VOUT"/>
<pin name="EP"/>
</symbol>
<symbol name="LT1528">
<pin name="OUT"/>
<pin name="SENSE"/>
<pin name="GND"/>
<pin name="SHDN"/>
<pin name="IN"/>
</symbol>
<symbol name="MAX1555">
<pin name="USB"/>
<pin name="GND"/>
<pin name="CHG"/>
<pin name="BATT"/>
<pin name="DC"/>
</symbol>
<symbol name="TPS6211*">
<pin name="AGND" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="LBI" direction="in"/>
<pin name="LBO" direction="out"/>
<pin name="PG" direction="out"/>
<pin name="PGND@1" direction="pwr"/>
<pin name="PGND@2" direction="pwr"/>
<pin name="PWPD" direction="pwr"/>
<pin name="SW@1" direction="out"/>
<pin name="SW@2" direction="out"/>
<pin name="SYNC" direction="in"/>
<pin name="VIN@1" direction="pwr"/>
<pin name="VIN@2" direction="pwr"/>
<pin name="VINA" direction="pwr"/>
</symbol>
<symbol name="TPS6213X">
<description>TPS62130, TPS62130A, TPS62131, TPS62132, TPS62133&lt;br/&gt;
(Will also work for TPS62140, TPS62140A, TPS62141, TPS62142, TPS62143)</description>
<pin name="PVIN@11"/>
<pin name="PVIN@12"/>
<pin name="AVIN"/>
<pin name="EN"/>
<pin name="FSW"/>
<pin name="PGND@15"/>
<pin name="PGND@16"/>
<pin name="EXT"/>
<pin name="SW@1"/>
<pin name="SW@2"/>
<pin name="SW@3"/>
<pin name="PG"/>
<pin name="VOS"/>
<pin name="SS/TR"/>
<pin name="AGND"/>
<pin name="DEF"/>
<pin name="FB"/>
</symbol>
<symbol name="NCP1400">
<pin name="LX" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="OUT" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="NC" direction="in"/>
</symbol>
<symbol name="TPS61040">
<pin name="EN"/>
<pin name="GND"/>
<pin name="VIN"/>
<pin name="SW"/>
<pin name="FB"/>
</symbol>
<symbol name="A4983">
<pin name="CP1"/>
<pin name="CP2"/>
<pin name="DIR" direction="in"/>
<pin name="ENABLE" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND_PAD" direction="pwr"/>
<pin name="MS1" direction="in"/>
<pin name="MS2" direction="in"/>
<pin name="MS3" direction="in"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="OUT1A"/>
<pin name="OUT1B"/>
<pin name="OUT2A"/>
<pin name="OUT2B"/>
<pin name="REF"/>
<pin name="RESET" direction="in"/>
<pin name="ROSC"/>
<pin name="SENSE1"/>
<pin name="SENSE2"/>
<pin name="SLEEP" direction="in"/>
<pin name="STEP" direction="in"/>
<pin name="VBB1"/>
<pin name="VBB2"/>
<pin name="VCP"/>
<pin name="VDD" direction="pwr"/>
<pin name="VREG"/>
</symbol>
<symbol name="LMD1820X">
<pin name="BS1"/>
<pin name="OUT1"/>
<pin name="DIR"/>
<pin name="BRK"/>
<pin name="PWM"/>
<pin name="PWR"/>
<pin name="PGND"/>
<pin name="SGND"/>
<pin name="TF"/>
<pin name="OUT2"/>
<pin name="BS2"/>
</symbol>
<symbol name="NJM2670">
<pin name="NC@1" direction="in"/>
<pin name="SENSEA"/>
<pin name="INA1"/>
<pin name="ENABLEA"/>
<pin name="GND@2"/>
<pin name="INB1"/>
<pin name="ENABLEB"/>
<pin name="NC@2"/>
<pin name="NC@3"/>
<pin name="TSDARM"/>
<pin name="INB2"/>
<pin name="GND@3"/>
<pin name="GND@1" direction="pwr"/>
<pin name="OUTA1" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="OUTA2" direction="pwr"/>
<pin name="NC@4"/>
<pin name="INA2"/>
<pin name="VCC"/>
<pin name="VSA"/>
<pin name="OUTB1"/>
<pin name="SENSEB"/>
<pin name="OUTB2"/>
<pin name="VSB"/>
</symbol>
<symbol name="ZXLD1360">
<pin name="LX"/>
<pin name="GND"/>
<pin name="ADJ"/>
<pin name="SENSE"/>
<pin name="VIN"/>
</symbol>
<symbol name="MIC">
<description>&lt;h3&gt;Microphone&lt;/h3&gt;
&lt;p&gt;Omni-directional electret microphones - one through-hole, the other SMD.&lt;/p&gt;</description>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="CONN_02">
<description>&lt;h3&gt;2 Pin Connection&lt;/h3&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="INDUCTOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ANDROID-ELECTRIC_SHEEP_LOGO" prefix="LOGO">
<description>Logos used for the Electric  Sheep</description>
<gates>
<gate name="G$1" symbol="ANDROID-ELECTRIC_SHEEP_LOGO"/>
</gates>
<devices>
<device name="_" package="ANDROID-ELECTRIC_SHEEP_LOGO">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="ANDROID-ELECTRIC_SHEEP_LOGO_SMALL">
<technologies>
<technology name="">
<attribute name="SF_ID" value="DEV-10745"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CREATIVE_COMMONS" prefix="CC_TEXT">
<description>Creative Commons License summary- RETIRED.

Please use parts FRAME-LETTER/FRAME-LEDGER to add this to both schematic and board file.</description>
<gates>
<gate name="G$1" symbol="CREATIVE_COMMONS"/>
</gates>
<devices>
<device name="" package="CREATIVE_COMMONS">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FRAME-A3" prefix="FRAME">
<description>&lt;b&gt;Schematic Frame&lt;/b&gt;&lt;p&gt;
A3 Larger Frame-RETIRED

Please use FRAME-LEDGER/FRAME-LETTER for schematics now.</description>
<gates>
<gate name="G$1" symbol="A3L-LOC"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LOGO-SFE" prefix="LOGO">
<description>&lt;b&gt;Spark Fun Electronics PCB Logo&lt;/b&gt;
This is the standard Spark Fun Electronics PCB logo.</description>
<gates>
<gate name="G$1" symbol="LOGO1"/>
</gates>
<devices>
<device name="M" package="SFE-LOGO">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NEW" package="SFE-NEW-WEBLOGO">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CP" package="SFE-LOGO-FLAME-COPPER">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SK" package="SFE-LOGO-FLAME">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NW2" package="SFE-NEW-WEB">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SM" package="SFE-NEW-WEB-SOLDERMASK">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STARBOARD_LOGO" prefix="LOGO">
<description>Starboard - RETIRED
PRT-10961
PRT-10640
PRT-10639
PRT-10638
PRT-10637
PRT-10572</description>
<gates>
<gate name="G$1" symbol="STARBOARD_LOGO"/>
</gates>
<devices>
<device name="" package="STARBOARD_LOGO">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-TEXT" package="STARBOARD_LOGO_TEXT">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FIDUCIAL" prefix="FID">
<description>&lt;b&gt;Fiducial Alignment Points&lt;/b&gt;
Various fiducial points for machine vision alignment.</description>
<gates>
<gate name="G$1" symbol="FIDUCIAL"/>
</gates>
<devices>
<device name="1.5X3" package="FIDUCIAL-1.5X3">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X2.5" package="FIDUCIAL-1X2.5">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARKFUN-EAGLE-RULES" prefix="RULES">
<description>&lt;b&gt;Description:&lt;/b&gt; These are the default rules that SparkFun engineers must follow. We highly recommend following these rules as well.</description>
<gates>
<gate name="G$1" symbol="SPARKFUN-EAGLE-RULES"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LOGO-FIRST" prefix="LOGO">
<gates>
<gate name="G$1" symbol="FIRST"/>
</gates>
<devices>
<device name="" package="FRIST_LOGO">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750KOHM1/10W1%(0603)" prefix="R" uservalue="yes">
<description>RES-07852</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="71.5OHM-1/4W-1%(PTH)" prefix="R" uservalue="yes">
<description>RES-10463</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="0.33OHM1/10W1%(0603)" prefix="R" uservalue="yes">
<description>RES-08412</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="1.0OHM1/4W5%PTH" prefix="R" uservalue="yes">
<description>RES-09453</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="1.4KOHM-1/10W-1%(0603)" prefix="R" uservalue="yes">
<description>RES-11114</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="3.6KOHM1/10W1%(0603)" prefix="R" uservalue="yes">
<description>RES-08417</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="1.2KOHM1/4W5%(PTH)" prefix="R" uservalue="yes">
<description>RES-09452</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="0.15OHM1/5W1%(0603)" prefix="R" uservalue="yes">
<description>RES-09738</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="3.0MOHM-1/10W-1%(0603)" prefix="R" uservalue="yes">
<description>RES-10937</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name=".47UF-16V(-20/+80%)(0805)" prefix="C" uservalue="yes">
<description>CAP-08139 - Retired</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name=".68UF-16V-20%,+80%(0603)" prefix="C" uservalue="yes">
<description>CAP-08708 - Retired</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="0.2F-3.3V--20%,+80%(COIN)" prefix="C" uservalue="yes">
<description>CAP-10408 - Retired</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="0.018UF-50V-10%(0603)" prefix="C" uservalue="yes">
<description>CAP-08494 - Retired</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="0.22UF-50V-?20%(ELECT)(PTH)" prefix="C" uservalue="yes">
<description>CAP-09998 - Retired</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="0.68UF-16V--20%,+80%(0603)" prefix="C" uservalue="yes">
<description>CAP-08723 - Retired</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="2.2UF-25V-10%(TANT)" prefix="C" uservalue="yes">
<description>CAP-08706 - Retired</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="3.3UF-80V-20%(ELECT)" prefix="C" uservalue="yes">
<description>CAP-08365 - Retired</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="6.7PF" prefix="C" uservalue="yes">
<description>CAP-08429 - Retired</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="6.8PF-50V-+/-.25PF(0603)" prefix="C" uservalue="yes">
<description>CAP-08620 - Retired</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="10UF-16V-20%(ELECT)" prefix="C" uservalue="yes">
<description>CAP-09575 - Retired</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name="12NF-200V-10%(0805)" prefix="C" uservalue="yes">
<description>CAP-11056 - Retired</description>
<gates>
</gates>
<devices>
</devices>
</deviceset>
<deviceset name=".1UF-CER" prefix="C">
<description>.1uF ceramic SMT&lt;br&gt;
CAP-00810- 25V +80%/-20% (0603)&lt;br&gt;
CAP-08390- 100V 10% (0603)&lt;br&gt;
CAP-08604- 25V 5% (0603)&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="" package="0402-CAP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="VALUE" value="0.1uF"/>
</technology>
</technologies>
</device>
<device name="CAP-08604" package="0402-CAP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="VALUE" value="0.1uF"/>
</technology>
</technologies>
</device>
<device name="CAP-08390" package="0402-CAP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-08390"/>
<attribute name="VALUE" value="0.1uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name=".22UF-CER" prefix="C" uservalue="yes">
<description>.22uF ceramic SMT&lt;br&gt;
CAP-09885- 50V +80%/-20% (0603)</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="" package="0402-CAP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-09885"/>
<attribute name="VALUE" value=".22uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2.2UF-CER" prefix="C">
<description>2.2uF Ceramic SMT&lt;BR&gt;
CAP-07888- 10V, 20% (0603)&lt;br&gt;
CAP-10009- 50V, 10% (1206)</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="CAP-07888" package="0402-CAP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-07888"/>
<attribute name="VALUE" value="2.2uF"/>
</technology>
</technologies>
</device>
<device name="CAP-10009" package="1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-10009"/>
<attribute name="VALUE" value="2.2uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="10NF-CER" prefix="C" uservalue="yes">
<description>10nF/.01uF/10000pF ceramic SMT&lt;br&gt;
CAP-00867- 50V 10% (0603)</description>
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="" package="0402-CAP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-00867"/>
<attribute name="VALUE" value="10nF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="10UF-TANT" prefix="C" uservalue="yes">
<description>10uF Tantalum SMT&lt;br&gt;
CAP-00811- 16V 10% (EIA-3216)</description>
<gates>
<gate name="G$1" symbol="CAP_POL"/>
</gates>
<devices>
<device name="" package="EIA3216">
<connects>
<connect gate="G$1" pin="+" pad="A"/>
<connect gate="G$1" pin="-" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-00811"/>
<attribute name="VALUE" value="10uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HSMC-C265">
<description>RETIRED &lt;BR&gt;
&lt;BR&gt;

Avago HSMC-C265 reverse-mounted red LED

This is a SMD LED that is mounted to one side of a PCB and shines through a hole to the other side of the PCB. Useful for making boards with no components on one side for mounting and having LED indicator lights shine through the board, panel, etc.</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="HSMC-C265">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74ACT125D">
<description>Quad Buffer with 3-State Outputs-
ON Semi Conductor:

Digikey P/N 74ACT125SC-ND</description>
<gates>
<gate name="G$1" symbol="74ACT125D"/>
</gates>
<devices>
<device name="" package="SO014">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="4"/>
<connect gate="G$1" pin="A2" pad="13"/>
<connect gate="G$1" pin="A3" pad="10"/>
<connect gate="G$1" pin="B0" pad="2"/>
<connect gate="G$1" pin="B1" pad="5"/>
<connect gate="G$1" pin="B2" pad="12"/>
<connect gate="G$1" pin="B3" pad="9"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="O0" pad="3"/>
<connect gate="G$1" pin="O1" pad="6"/>
<connect gate="G$1" pin="O2" pad="11"/>
<connect gate="G$1" pin="O3" pad="8"/>
<connect gate="G$1" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA32U4">
<description>Atmel 44-pin 8-bit Microcontroller with 32KBytes of ISP Flash and USB Controller ----- 

Please use the QFN-44-NOPAD_1:1 package for the footprint of all boards using a 32U4. Route traces directly away from the pads as much as possible.</description>
<gates>
<gate name="G$1" symbol="SPARKFUN-DIGITALIC_ATMEGA32U4"/>
</gates>
<devices>
<device name="QFN" package="SPARKFUN-DIGITALIC_QFN-44">
<connects>
<connect gate="G$1" pin="!RESET" pad="13"/>
<connect gate="G$1" pin="AREF" pad="42"/>
<connect gate="G$1" pin="AVCC@24" pad="24"/>
<connect gate="G$1" pin="AVCC@44" pad="44"/>
<connect gate="G$1" pin="D+" pad="4"/>
<connect gate="G$1" pin="D-" pad="3"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@23" pad="23"/>
<connect gate="G$1" pin="GND@35" pad="35"/>
<connect gate="G$1" pin="GND@43" pad="43"/>
<connect gate="G$1" pin="PB0(SS)" pad="8"/>
<connect gate="G$1" pin="PB1(SCK)" pad="9"/>
<connect gate="G$1" pin="PB2(MOSI)" pad="10"/>
<connect gate="G$1" pin="PB3(MISO)" pad="11"/>
<connect gate="G$1" pin="PB4(ADC11)" pad="28"/>
<connect gate="G$1" pin="PB5(ADC12)" pad="29"/>
<connect gate="G$1" pin="PB6(ADC13)" pad="30"/>
<connect gate="G$1" pin="PB7" pad="12"/>
<connect gate="G$1" pin="PC6" pad="31"/>
<connect gate="G$1" pin="PC7" pad="32"/>
<connect gate="G$1" pin="PD0(SCL)" pad="18"/>
<connect gate="G$1" pin="PD1(SDA)" pad="19"/>
<connect gate="G$1" pin="PD2(RX)" pad="20"/>
<connect gate="G$1" pin="PD3(TX)" pad="21"/>
<connect gate="G$1" pin="PD4(ADC8)" pad="25"/>
<connect gate="G$1" pin="PD5" pad="22"/>
<connect gate="G$1" pin="PD6(ADC9)" pad="26"/>
<connect gate="G$1" pin="PD7(ADC10)" pad="27"/>
<connect gate="G$1" pin="PE2/!HWB" pad="33"/>
<connect gate="G$1" pin="PE6" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="41"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="40"/>
<connect gate="G$1" pin="PF4(ADC4)" pad="39"/>
<connect gate="G$1" pin="PF5(ADC5)" pad="38"/>
<connect gate="G$1" pin="PF6(ADC6)" pad="37"/>
<connect gate="G$1" pin="PF7(ADC7)" pad="36"/>
<connect gate="G$1" pin="UCAP" pad="6"/>
<connect gate="G$1" pin="UGND" pad="5"/>
<connect gate="G$1" pin="UVCC" pad="2"/>
<connect gate="G$1" pin="VBUS" pad="7"/>
<connect gate="G$1" pin="VCC@14" pad="14"/>
<connect gate="G$1" pin="VCC@34" pad="34"/>
<connect gate="G$1" pin="XTAL1" pad="17"/>
<connect gate="G$1" pin="XTAL2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="QFN2" package="SPARKFUN-DIGITALIC_QFN-44-NOPAD">
<connects>
<connect gate="G$1" pin="!RESET" pad="13"/>
<connect gate="G$1" pin="AREF" pad="42"/>
<connect gate="G$1" pin="AVCC@24" pad="24"/>
<connect gate="G$1" pin="AVCC@44" pad="44"/>
<connect gate="G$1" pin="D+" pad="4"/>
<connect gate="G$1" pin="D-" pad="3"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@23" pad="23"/>
<connect gate="G$1" pin="GND@35" pad="35"/>
<connect gate="G$1" pin="GND@43" pad="43"/>
<connect gate="G$1" pin="PB0(SS)" pad="8"/>
<connect gate="G$1" pin="PB1(SCK)" pad="9"/>
<connect gate="G$1" pin="PB2(MOSI)" pad="10"/>
<connect gate="G$1" pin="PB3(MISO)" pad="11"/>
<connect gate="G$1" pin="PB4(ADC11)" pad="28"/>
<connect gate="G$1" pin="PB5(ADC12)" pad="29"/>
<connect gate="G$1" pin="PB6(ADC13)" pad="30"/>
<connect gate="G$1" pin="PB7" pad="12"/>
<connect gate="G$1" pin="PC6" pad="31"/>
<connect gate="G$1" pin="PC7" pad="32"/>
<connect gate="G$1" pin="PD0(SCL)" pad="18"/>
<connect gate="G$1" pin="PD1(SDA)" pad="19"/>
<connect gate="G$1" pin="PD2(RX)" pad="20"/>
<connect gate="G$1" pin="PD3(TX)" pad="21"/>
<connect gate="G$1" pin="PD4(ADC8)" pad="25"/>
<connect gate="G$1" pin="PD5" pad="22"/>
<connect gate="G$1" pin="PD6(ADC9)" pad="26"/>
<connect gate="G$1" pin="PD7(ADC10)" pad="27"/>
<connect gate="G$1" pin="PE2/!HWB" pad="33"/>
<connect gate="G$1" pin="PE6" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="41"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="40"/>
<connect gate="G$1" pin="PF4(ADC4)" pad="39"/>
<connect gate="G$1" pin="PF5(ADC5)" pad="38"/>
<connect gate="G$1" pin="PF6(ADC6)" pad="37"/>
<connect gate="G$1" pin="PF7(ADC7)" pad="36"/>
<connect gate="G$1" pin="UCAP" pad="6"/>
<connect gate="G$1" pin="UGND" pad="5"/>
<connect gate="G$1" pin="UVCC" pad="2"/>
<connect gate="G$1" pin="VBUS" pad="7"/>
<connect gate="G$1" pin="VCC@14" pad="14"/>
<connect gate="G$1" pin="VCC@34" pad="34"/>
<connect gate="G$1" pin="XTAL1" pad="17"/>
<connect gate="G$1" pin="XTAL2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TQFP" package="SPARKFUN-DIGITALIC_TQFP44">
<connects>
<connect gate="G$1" pin="!RESET" pad="13"/>
<connect gate="G$1" pin="AREF" pad="42"/>
<connect gate="G$1" pin="AVCC@24" pad="24"/>
<connect gate="G$1" pin="AVCC@44" pad="44"/>
<connect gate="G$1" pin="D+" pad="4"/>
<connect gate="G$1" pin="D-" pad="3"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@23" pad="23"/>
<connect gate="G$1" pin="GND@35" pad="35"/>
<connect gate="G$1" pin="GND@43" pad="43"/>
<connect gate="G$1" pin="PB0(SS)" pad="8"/>
<connect gate="G$1" pin="PB1(SCK)" pad="9"/>
<connect gate="G$1" pin="PB2(MOSI)" pad="10"/>
<connect gate="G$1" pin="PB3(MISO)" pad="11"/>
<connect gate="G$1" pin="PB4(ADC11)" pad="28"/>
<connect gate="G$1" pin="PB5(ADC12)" pad="29"/>
<connect gate="G$1" pin="PB6(ADC13)" pad="30"/>
<connect gate="G$1" pin="PB7" pad="12"/>
<connect gate="G$1" pin="PC6" pad="31"/>
<connect gate="G$1" pin="PC7" pad="32"/>
<connect gate="G$1" pin="PD0(SCL)" pad="18"/>
<connect gate="G$1" pin="PD1(SDA)" pad="19"/>
<connect gate="G$1" pin="PD2(RX)" pad="20"/>
<connect gate="G$1" pin="PD3(TX)" pad="21"/>
<connect gate="G$1" pin="PD4(ADC8)" pad="25"/>
<connect gate="G$1" pin="PD5" pad="22"/>
<connect gate="G$1" pin="PD6(ADC9)" pad="26"/>
<connect gate="G$1" pin="PD7(ADC10)" pad="27"/>
<connect gate="G$1" pin="PE2/!HWB" pad="33"/>
<connect gate="G$1" pin="PE6" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="41"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="40"/>
<connect gate="G$1" pin="PF4(ADC4)" pad="39"/>
<connect gate="G$1" pin="PF5(ADC5)" pad="38"/>
<connect gate="G$1" pin="PF6(ADC6)" pad="37"/>
<connect gate="G$1" pin="PF7(ADC7)" pad="36"/>
<connect gate="G$1" pin="UCAP" pad="6"/>
<connect gate="G$1" pin="UGND" pad="5"/>
<connect gate="G$1" pin="UVCC" pad="2"/>
<connect gate="G$1" pin="VBUS" pad="7"/>
<connect gate="G$1" pin="VCC@14" pad="14"/>
<connect gate="G$1" pin="VCC@34" pad="34"/>
<connect gate="G$1" pin="XTAL1" pad="17"/>
<connect gate="G$1" pin="XTAL2" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11161"/>
</technology>
</technologies>
</device>
<device name="QFN_1:1" package="QFN-44-NOPAD_1:1">
<connects>
<connect gate="G$1" pin="!RESET" pad="13"/>
<connect gate="G$1" pin="AREF" pad="42"/>
<connect gate="G$1" pin="AVCC@24" pad="24"/>
<connect gate="G$1" pin="AVCC@44" pad="44"/>
<connect gate="G$1" pin="D+" pad="4"/>
<connect gate="G$1" pin="D-" pad="3"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@23" pad="23"/>
<connect gate="G$1" pin="GND@35" pad="35"/>
<connect gate="G$1" pin="GND@43" pad="43"/>
<connect gate="G$1" pin="PB0(SS)" pad="8"/>
<connect gate="G$1" pin="PB1(SCK)" pad="9"/>
<connect gate="G$1" pin="PB2(MOSI)" pad="10"/>
<connect gate="G$1" pin="PB3(MISO)" pad="11"/>
<connect gate="G$1" pin="PB4(ADC11)" pad="28"/>
<connect gate="G$1" pin="PB5(ADC12)" pad="29"/>
<connect gate="G$1" pin="PB6(ADC13)" pad="30"/>
<connect gate="G$1" pin="PB7" pad="12"/>
<connect gate="G$1" pin="PC6" pad="31"/>
<connect gate="G$1" pin="PC7" pad="32"/>
<connect gate="G$1" pin="PD0(SCL)" pad="18"/>
<connect gate="G$1" pin="PD1(SDA)" pad="19"/>
<connect gate="G$1" pin="PD2(RX)" pad="20"/>
<connect gate="G$1" pin="PD3(TX)" pad="21"/>
<connect gate="G$1" pin="PD4(ADC8)" pad="25"/>
<connect gate="G$1" pin="PD5" pad="22"/>
<connect gate="G$1" pin="PD6(ADC9)" pad="26"/>
<connect gate="G$1" pin="PD7(ADC10)" pad="27"/>
<connect gate="G$1" pin="PE2/!HWB" pad="33"/>
<connect gate="G$1" pin="PE6" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="41"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="40"/>
<connect gate="G$1" pin="PF4(ADC4)" pad="39"/>
<connect gate="G$1" pin="PF5(ADC5)" pad="38"/>
<connect gate="G$1" pin="PF6(ADC6)" pad="37"/>
<connect gate="G$1" pin="PF7(ADC7)" pad="36"/>
<connect gate="G$1" pin="UCAP" pad="6"/>
<connect gate="G$1" pin="UGND" pad="5"/>
<connect gate="G$1" pin="UVCC" pad="2"/>
<connect gate="G$1" pin="VBUS" pad="7"/>
<connect gate="G$1" pin="VCC@14" pad="14"/>
<connect gate="G$1" pin="VCC@34" pad="34"/>
<connect gate="G$1" pin="XTAL1" pad="17"/>
<connect gate="G$1" pin="XTAL2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JUMPER-2" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Jumper&lt;/b&gt;
Basic 0.1" spaced jumper. Use with breakaway headers.</description>
<gates>
<gate name="A" symbol="JUMPER-2"/>
</gates>
<devices>
<device name="PTH" package="1X02">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-NC" package="SJ_2S">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_LOCK" package="1X02_LOCK">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-NO" package="SJ_2S-NO">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-NO-NS" package="SJ_2S-NO-NS">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JUMPER-2-OLD" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Jumper&lt;/b&gt;
Basic 0.1" spaced jumper. Use with breakaway headers.</description>
<gates>
<gate name="A" symbol="JUMPER-2"/>
</gates>
<devices>
<device name="PTH" package="1X02">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-NC" package="SJ_2S">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_LOCK" package="1X02_LOCK">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-NO" package="SJ_2S-NO">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JUMPER-3" prefix="JP">
<gates>
<gate name="G$1" symbol="JUMPER-3"/>
</gates>
<devices>
<device name="SMD" package="SJ_3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="1X03">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1-2" package="SJ_3_PASTE1&amp;2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2-3" package="SJ_3_PASTE2&amp;3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JUMPER-3-OLD" prefix="JP">
<gates>
<gate name="G$1" symbol="JUMPER-3"/>
</gates>
<devices>
<device name="SMD" package="SJ_3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="1X03">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1-2" package="SJ_3_PASTE1&amp;2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2-3" package="SJ_3_PASTE2&amp;3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOLDERJUMPER" prefix="SJ">
<description>&lt;b&gt;Solder Jumper&lt;/b&gt;
Standard SMD solder jumper. Used to automate production. Two varients : Normally Open and Normally Closed are the same, but have different paste layers. NC will have a large amount of paste and should jumper during reflow.</description>
<gates>
<gate name="1" symbol="SJ"/>
</gates>
<devices>
<device name="NC" package="SJ_2S">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TRACE" package="SJ_2S-TRACE">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NC2" package="SJ_2S-NOTRACE">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NO" package="SJ_2S-NO">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TRACE-PTH" package="SJ_2S-TRACE-PTH">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="SJ_2S-PTH">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROUND" package="SJ_ROUND">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOLDERJUMPER-OLD" prefix="SJ">
<description>&lt;b&gt;Solder Jumper&lt;/b&gt;
Standard SMD solder jumper. Used to automate production. Two varients : Normally Open and Normally Closed are the same, but have different paste layers. NC will have a large amount of paste and should jumper during reflow.</description>
<gates>
<gate name="1" symbol="SJ"/>
</gates>
<devices>
<device name="NC" package="SJ_2S">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TRACE" package="SJ_2S-TRACE">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NC2" package="SJ_2S-NOTRACE">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NO" package="SJ_2S-NO">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOLDERJUMPER_2WAY" prefix="SJ" uservalue="yes">
<description>&lt;b&gt;Solder Jumper&lt;/b&gt;
2 way solder jumper</description>
<gates>
<gate name="G$1" symbol="SJ_2"/>
</gates>
<devices>
<device name="W" package="SJ_2W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T" package="SJ_2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="SJ_3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PASTE1&amp;2" package="SJ_3_PASTE1&amp;2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PASTE2&amp;3" package="SJ_3_PASTE2&amp;3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PASTE1&amp;2&amp;3" package="SJ_3_PASTE1&amp;2&amp;3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOLDERJUMPER_2WAY-OLD" prefix="SJ" uservalue="yes">
<description>&lt;b&gt;Solder Jumper&lt;/b&gt;
2 way solder jumper</description>
<gates>
<gate name="G$1" symbol="SJ_2"/>
</gates>
<devices>
<device name="W" package="SJ_2W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T" package="SJ_2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="SJ_3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PASTE1&amp;2" package="SJ_3_PASTE1&amp;2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PASTE2&amp;3" package="SJ_3_PASTE2&amp;3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FRAME-LETTER" prefix="FRAME">
<description>&lt;b&gt;Schematic Frame&lt;/b&gt;&lt;p&gt;
Standard 8.5x11 US Letter frame</description>
<gates>
<gate name="G$1" symbol="LETTER_L"/>
<gate name="G$2" symbol="DOCFIELD"/>
</gates>
<devices>
<device name="" package="CREATIVE_COMMONS">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TAC_SWITCH" prefix="S" uservalue="yes">
<description>&lt;b&gt;Momentary Switch&lt;/b&gt;&lt;br&gt;
Button commonly used for reset or general input.&lt;br&gt;
Spark Fun Electronics SKU : COM-00097&lt;br&gt;
SMT- SWCH-08247</description>
<gates>
<gate name="S" symbol="SWITCH-MOMENTARY"/>
</gates>
<devices>
<device name="PTH" package="TACTILE-PTH">
<connects>
<connect gate="S" pin="1" pad="1"/>
<connect gate="S" pin="2" pad="2"/>
<connect gate="S" pin="3" pad="3"/>
<connect gate="S" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="KSA_SEALED" package="KSA_SEALED_TAC_SWITCH">
<connects>
<connect gate="S" pin="1" pad="P$1"/>
<connect gate="S" pin="2" pad="P$2"/>
<connect gate="S" pin="3" pad="P$3"/>
<connect gate="S" pin="4" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="TACTILE-SWITCH-SMD">
<connects>
<connect gate="S" pin="1" pad="1"/>
<connect gate="S" pin="2" pad="2"/>
<connect gate="S" pin="3" pad="3"/>
<connect gate="S" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-08247"/>
<attribute name="VALUE" value="TAC_SWITCHSMD"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FXXXDAX06" prefix="U">
<description>&lt;b&gt;PIC24FXXXDAX06&lt;/b&gt;&lt;br&gt;
PIC24FXXXDA106 / PIC24FXXXDA206&lt;br&gt;
PIC24FJ256DA206-I/PT for IOIO&lt;br&gt;
IC-10386</description>
<gates>
<gate name="G$1" symbol="PIC24FJXXXDAX06"/>
</gates>
<devices>
<device name="" package="PIC24FXXX_TQFP64">
<connects>
<connect gate="G$1" pin="!MCLR" pad="7"/>
<connect gate="G$1" pin="AN14/CTPLS/RP14/CN32/RB14" pad="29"/>
<connect gate="G$1" pin="AN15/RP29/REFO/CN12/RB15" pad="30"/>
<connect gate="G$1" pin="AN2/C2INB/VMIO/RP13/CN4/RB2" pad="14"/>
<connect gate="G$1" pin="AN3/C2INA/VPIO/CN5/RB3" pad="13"/>
<connect gate="G$1" pin="AN8/RP8/CN26/RB8" pad="21"/>
<connect gate="G$1" pin="AN9/RP9/CN27/RB9" pad="22"/>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="AVSS" pad="20"/>
<connect gate="G$1" pin="C1INC/RP26/CN9/RG7" pad="5"/>
<connect gate="G$1" pin="C1IND/RP21/CN8/RG6" pad="4"/>
<connect gate="G$1" pin="C2INC/RP27/GD15/CN11/RG9" pad="8"/>
<connect gate="G$1" pin="C2IND/RP19/GD14/CN10/RG8" pad="6"/>
<connect gate="G$1" pin="C3INA/SESSEND/CN16/RD7" pad="55"/>
<connect gate="G$1" pin="C3INB/CN15/RD6" pad="54"/>
<connect gate="G$1" pin="D+/CN83/RG2" pad="37"/>
<connect gate="G$1" pin="D-/CN84/RG3" pad="36"/>
<connect gate="G$1" pin="DMH/RP11/INT0/CN49/RD0" pad="46"/>
<connect gate="G$1" pin="DPH/RP23/CN51/RD2" pad="50"/>
<connect gate="G$1" pin="DPLN/SDA1/RP4/GD8/CN54/RD9" pad="43"/>
<connect gate="G$1" pin="ENVREG" pad="57"/>
<connect gate="G$1" pin="GD0/CN58/RE0" pad="60"/>
<connect gate="G$1" pin="GD1/CN59/RE1" pad="61"/>
<connect gate="G$1" pin="GD10/VBUSST/VCMPST1/VBUSVLD/CN68/RF0" pad="58"/>
<connect gate="G$1" pin="GD11/VCMPST2/SESSVLD/CN69/RF1" pad="59"/>
<connect gate="G$1" pin="GD12/SCL3/CN64/RE6" pad="2"/>
<connect gate="G$1" pin="GD13/SDA3/CN65/RE7" pad="3"/>
<connect gate="G$1" pin="GD2/CN60/RE2" pad="62"/>
<connect gate="G$1" pin="GD3/CN61/RE3" pad="63"/>
<connect gate="G$1" pin="HSYNC/CN62/RE4" pad="64"/>
<connect gate="G$1" pin="OSCI/CLKI/CN23/RC12" pad="39"/>
<connect gate="G$1" pin="OSCO/CLKO/CN22/RC15" pad="40"/>
<connect gate="G$1" pin="PGEC1/AN1/VREF-/RP1/CN3/RB1" pad="15"/>
<connect gate="G$1" pin="PGEC2/AN6/RP6/CN24/RB6" pad="17"/>
<connect gate="G$1" pin="PGEC3/AN5/C1INA/VBUSON/RP18/CN7/RB5" pad="11"/>
<connect gate="G$1" pin="PGED1/AN0/VREF+/RP0/CN2/RB0" pad="16"/>
<connect gate="G$1" pin="PGED2/AN7/RP7/RCV/CN25/RB7" pad="18"/>
<connect gate="G$1" pin="PGED3/AN4/C1INB/USBOEN/RP28/CN6/RB4" pad="12"/>
<connect gate="G$1" pin="RP12/GD7/CN56/RD11" pad="45"/>
<connect gate="G$1" pin="RP16/USBID/CN71/RF3" pad="33"/>
<connect gate="G$1" pin="RP20/GPWR/CN14/RD5" pad="53"/>
<connect gate="G$1" pin="RP22/GEN/CN52/RD3" pad="51"/>
<connect gate="G$1" pin="RP25/GCLK/CN13/RD4" pad="52"/>
<connect gate="G$1" pin="RTCC/DMLN/RP2/CN53/RD8" pad="42"/>
<connect gate="G$1" pin="SCL1/RP3/GD6/CN55/RD10" pad="44"/>
<connect gate="G$1" pin="SCL2/RP17/GD5/CN18/RF5" pad="32"/>
<connect gate="G$1" pin="SDA2/RP10/GD4/CN17/RF4" pad="31"/>
<connect gate="G$1" pin="SOSCI/C3IND/CN1/RC13" pad="47"/>
<connect gate="G$1" pin="SOSCO/SCLKI/T1CK/C3INC/RPI37/CN0/RC14" pad="48"/>
<connect gate="G$1" pin="TCK/AN12/CTEDG2/CN30/RB12" pad="27"/>
<connect gate="G$1" pin="TDI/AN13/CTEDG1/CN31/RB13" pad="28"/>
<connect gate="G$1" pin="TDO/AN11/CN29/RB11" pad="24"/>
<connect gate="G$1" pin="TMS/CVREF/AN10/CN28/RB10" pad="23"/>
<connect gate="G$1" pin="VBUS/RF7" pad="34"/>
<connect gate="G$1" pin="VCAP" pad="56"/>
<connect gate="G$1" pin="VCPCON/RP24/GD9/VBUSCHG/CN50/RD1" pad="49"/>
<connect gate="G$1" pin="VDD@1" pad="10"/>
<connect gate="G$1" pin="VDD@2" pad="26"/>
<connect gate="G$1" pin="VDD@3" pad="38"/>
<connect gate="G$1" pin="VSS@1" pad="9"/>
<connect gate="G$1" pin="VSS@2" pad="25"/>
<connect gate="G$1" pin="VSS@3" pad="41"/>
<connect gate="G$1" pin="VSYNC/CN63/RE5" pad="1"/>
<connect gate="G$1" pin="VUSB" pad="35"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-10386"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED" prefix="LED" uservalue="yes">
<description>&lt;b&gt;LEDs&lt;/b&gt;
Standard schematic elements and footprints for 5mm, 3mm, 1206, and 0603 sized LEDs. 5mm - Spark Fun Electronics SKU : Comp-SBL</description>
<gates>
<gate name="G$1" symbol="LED-1"/>
</gates>
<devices>
<device name="1206" package="LED-1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEW_HOLE" prefix="H">
<description>&lt;h3&gt;SparkFun LilyPad Sew Hole&lt;/h3&gt;
&lt;p&gt;Simple sew-tap with .1" diameter hole with 20mil annular ring&lt;/p&gt;
&lt;p&gt;SparkFun Products:
&lt;ul&gt;
&lt;li&gt;&lt;a href=”[PRODUCT1LINK]”&gt;[PRODUCT 1]&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”PRODUCT2LINK”&gt;[PRODUCT 2]&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”PRODUCT3LINK”&gt;[PRODUCT 3]&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SIMPLE_HOLE"/>
</gates>
<devices>
<device name="" package="SIMPLE_HOLE">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEW_HOLE-SMALL" prefix="CONN">
<description>&lt;h3&gt;SparkFun LilyPad Sew Hole&lt;/h3&gt;
&lt;p&gt;Simple sew-tap with .070" hole with 20mil annular ring&lt;/p&gt;
&lt;p&gt;SparkFun Products:
&lt;ul&gt;
&lt;li&gt;&lt;a href=”[PRODUCT1LINK]”&gt;[PRODUCT 1]&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”PRODUCT2LINK”&gt;[PRODUCT 2]&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”PRODUCT3LINK”&gt;[PRODUCT 3]&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SIMPLE_HOLE_SM"/>
</gates>
<devices>
<device name="" package="SIMPLE_HOLE_SM">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BLE112-A" prefix="U">
<description>&lt;H3&gt;BlueGiga Bluetooth 4.0 module&lt;/H3&gt;
&lt;p&gt;Bluetooth 4.0 module with integrated chip antenna and onboard 8051 processor and peripherals.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BLE112-A"/>
</gates>
<devices>
<device name="" package="BLE112-A">
<connects>
<connect gate="G$1" pin="AVDD1" pad="2"/>
<connect gate="G$1" pin="AVDD2" pad="3"/>
<connect gate="G$1" pin="DVDD" pad="20"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="10"/>
<connect gate="G$1" pin="GND3" pad="21"/>
<connect gate="G$1" pin="GND4" pad="30"/>
<connect gate="G$1" pin="P0_0" pad="28"/>
<connect gate="G$1" pin="P0_1" pad="27"/>
<connect gate="G$1" pin="P0_2" pad="26"/>
<connect gate="G$1" pin="P0_3" pad="25"/>
<connect gate="G$1" pin="P0_4" pad="24"/>
<connect gate="G$1" pin="P0_5" pad="23"/>
<connect gate="G$1" pin="P0_6" pad="22"/>
<connect gate="G$1" pin="P0_7" pad="19"/>
<connect gate="G$1" pin="P1_0" pad="18"/>
<connect gate="G$1" pin="P1_1" pad="17"/>
<connect gate="G$1" pin="P1_2" pad="16"/>
<connect gate="G$1" pin="P1_3" pad="15"/>
<connect gate="G$1" pin="P1_4" pad="14"/>
<connect gate="G$1" pin="P1_5" pad="13"/>
<connect gate="G$1" pin="P1_6" pad="8"/>
<connect gate="G$1" pin="P1_7" pad="7"/>
<connect gate="G$1" pin="P2_0" pad="6"/>
<connect gate="G$1" pin="P2_1" pad="5"/>
<connect gate="G$1" pin="P2_2" pad="4"/>
<connect gate="G$1" pin="RESET" pad="29"/>
<connect gate="G$1" pin="USB+" pad="11"/>
<connect gate="G$1" pin="USB-" pad="12"/>
<connect gate="G$1" pin="VDD_USB" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RN-131G">
<description>Roving Netowrks WiFLy GSX Module</description>
<gates>
<gate name="G$1" symbol="RN-131G"/>
</gates>
<devices>
<device name="" package="RN-131G">
<connects>
<connect gate="G$1" pin="3.3V-RIN" pad="P$18"/>
<connect gate="G$1" pin="3.3V-ROUT" pad="P$17"/>
<connect gate="G$1" pin="CLK" pad="P$15"/>
<connect gate="G$1" pin="DMA-RX" pad="P$23"/>
<connect gate="G$1" pin="DMA-TX" pad="P$22"/>
<connect gate="G$1" pin="EPC-A" pad="P$6"/>
<connect gate="G$1" pin="EPC-B" pad="P$7"/>
<connect gate="G$1" pin="F_AWAKE" pad="P$9"/>
<connect gate="G$1" pin="GND@19" pad="P$19"/>
<connect gate="G$1" pin="GND@36" pad="P$36"/>
<connect gate="G$1" pin="GND@37" pad="P$37"/>
<connect gate="G$1" pin="GND@38" pad="P$38"/>
<connect gate="G$1" pin="GND@39" pad="P$39"/>
<connect gate="G$1" pin="GND@40" pad="P$40"/>
<connect gate="G$1" pin="GND@41" pad="P$41"/>
<connect gate="G$1" pin="GND@42" pad="P$42"/>
<connect gate="G$1" pin="GND@43" pad="P$43"/>
<connect gate="G$1" pin="GND@44" pad="P$44"/>
<connect gate="G$1" pin="GPIO-12" pad="P$11"/>
<connect gate="G$1" pin="GPIO-13" pad="P$10"/>
<connect gate="G$1" pin="GPIO-4" pad="P$29"/>
<connect gate="G$1" pin="GPIO-5" pad="P$28"/>
<connect gate="G$1" pin="GPIO-6" pad="P$27"/>
<connect gate="G$1" pin="GPIO-7" pad="P$26"/>
<connect gate="G$1" pin="GPIO-8" pad="P$25"/>
<connect gate="G$1" pin="GPIO-9" pad="P$24"/>
<connect gate="G$1" pin="MISO" pad="P$16"/>
<connect gate="G$1" pin="MOSI" pad="P$14"/>
<connect gate="G$1" pin="RESET" pad="P$5"/>
<connect gate="G$1" pin="RX" pad="P$12"/>
<connect gate="G$1" pin="SEN0" pad="P$34"/>
<connect gate="G$1" pin="SEN1" pad="P$30"/>
<connect gate="G$1" pin="SEN2" pad="P$31"/>
<connect gate="G$1" pin="SEN3" pad="P$32"/>
<connect gate="G$1" pin="SEN4" pad="P$2"/>
<connect gate="G$1" pin="SEN5" pad="P$3"/>
<connect gate="G$1" pin="SEN6" pad="P$1"/>
<connect gate="G$1" pin="SEN7" pad="P$4"/>
<connect gate="G$1" pin="SENSE-PWR" pad="P$33"/>
<connect gate="G$1" pin="S_CAP" pad="P$8"/>
<connect gate="G$1" pin="TX" pad="P$13"/>
<connect gate="G$1" pin="VDD-BATT" pad="P$20"/>
<connect gate="G$1" pin="VDD-IN" pad="P$21"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-12671"/>
<attribute name="SF_ID" value="WRL-10004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RS9110" prefix="U">
<description>Redpine WiFi module</description>
<gates>
<gate name="G$1" symbol="RS9110-N-11-22"/>
</gates>
<devices>
<device name="" package="RS9110-N-11-22-SHORT">
<connects>
<connect gate="G$1" pin="CLK" pad="51"/>
<connect gate="G$1" pin="CS" pad="52"/>
<connect gate="G$1" pin="GND@10" pad="10"/>
<connect gate="G$1" pin="GND@16" pad="16"/>
<connect gate="G$1" pin="GND@20" pad="20"/>
<connect gate="G$1" pin="GND@21" pad="21"/>
<connect gate="G$1" pin="GND@48" pad="48"/>
<connect gate="G$1" pin="GND@PAD" pad="GND"/>
<connect gate="G$1" pin="INTR" pad="3"/>
<connect gate="G$1" pin="JPD0" pad="42"/>
<connect gate="G$1" pin="JPD1" pad="43"/>
<connect gate="G$1" pin="JPD2" pad="44"/>
<connect gate="G$1" pin="MISO" pad="2"/>
<connect gate="G$1" pin="MODE" pad="22"/>
<connect gate="G$1" pin="MOSI" pad="1"/>
<connect gate="G$1" pin="RST" pad="4"/>
<connect gate="G$1" pin="RX" pad="7"/>
<connect gate="G$1" pin="SD3" pad="6"/>
<connect gate="G$1" pin="TX" pad="5"/>
<connect gate="G$1" pin="VIN@46" pad="46"/>
<connect gate="G$1" pin="VIN@47" pad="47"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-10622"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BADGERHACK_LOGO">
<gates>
<gate name="G$1" symbol="BADGER_HACK_LOGO"/>
</gates>
<devices>
<device name="" package="BADGER_HACK">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DUMMY" package="DUMMY">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FKIT-LOGO" prefix="LOGO">
<description>&lt;h3&gt;Fabrick.it Logos&lt;/h3&gt;</description>
<gates>
<gate name="G$1" symbol="FKIT-LOGO"/>
</gates>
<devices>
<device name="-MEDIUM" package="FKIT-LOGO_MEDIUM">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMALL" package="FKIT-LOGO_SMALL">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-VERY_SMALL" package="FKIT-LOGO_VERY_SMALL">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-VERY_SMALL_VECTOR" package="FKIT-LOGO_VERY_SMALL">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FKIT-LOGOTYPE" prefix="LOGO">
<description>&lt;h3&gt;Fabrick.it Logotype&lt;/h3&gt;</description>
<gates>
<gate name="G$1" symbol="FKIT-LOGOTYPE"/>
</gates>
<devices>
<device name="-SMALL" package="FKIT-LOGOTYPE_SMALL">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-VERY_SMALL" package="FKIT-LOGOTYPE_VERY_SMALL">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MEDIUM" package="FKIT-LOGOTYPE_MEDIUM">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LOGO-OTL" prefix="LOGO">
<gates>
<gate name="G$1" symbol="OVERTONE_LOGO"/>
</gates>
<devices>
<device name="" package="OVERTONE_LOGO">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LOGO-LP">
<gates>
<gate name="G$1" symbol="LOGO-LP"/>
</gates>
<devices>
<device name="LP" package="LOGO-LILYPAD">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LPA" package="LOGO-LPA">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L" package="LOGO-L">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L-TINY" package="LOGO-L-TINY">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ARDUINO_ONLY" package="LOGO-A">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="96BOARDS_HIGH_SPEED" prefix="J" uservalue="yes">
<description>96 BOARDS high speed connectors.
&lt;br&gt;&lt;br&gt;
2 variants:
&lt;br&gt;&lt;br&gt;
1. "TOP" goes on the top of the board, called a "Receptacale" in the parlance.  Candidate parts would be FCI/Bergquist 61082-061409LF
&lt;br&gt;&lt;br&gt;
2. "BOTTOM" goes on the bottom of a board.  Candidate parts would be FCI 61083-063409LF for 7mm board-to-board clearance, or  61083-064409LF for 8mm clearance.
&lt;br&gt;&lt;br&gt;
If you're placing one on the bottom of a board, take care to mind the pin-1 orientation.</description>
<gates>
<gate name="G$1" symbol="96BOARDS-HI-SPEED"/>
</gates>
<devices>
<device name="BOTTOM" package="2X30-BERGSTAK-0.8MM-F">
<connects>
<connect gate="G$1" pin="CLK0/CSI0_MCLK" pad="15"/>
<connect gate="G$1" pin="CLK1/CSI1_MCLK" pad="17"/>
<connect gate="G$1" pin="CSI0_C+" pad="2"/>
<connect gate="G$1" pin="CSI0_C-" pad="4"/>
<connect gate="G$1" pin="CSI0_D0+" pad="8"/>
<connect gate="G$1" pin="CSI0_D0-" pad="10"/>
<connect gate="G$1" pin="CSI0_D1+" pad="14"/>
<connect gate="G$1" pin="CSI0_D1-" pad="16"/>
<connect gate="G$1" pin="CSI0_D2+" pad="20"/>
<connect gate="G$1" pin="CSI0_D2-" pad="22"/>
<connect gate="G$1" pin="CSI0_D3+" pad="26"/>
<connect gate="G$1" pin="CSI0_D3-" pad="28"/>
<connect gate="G$1" pin="CSI1_C+" pad="54"/>
<connect gate="G$1" pin="CSI1_C-" pad="56"/>
<connect gate="G$1" pin="CSI1_D0+" pad="42"/>
<connect gate="G$1" pin="CSI1_D0-" pad="44"/>
<connect gate="G$1" pin="CSI1_D1+" pad="48"/>
<connect gate="G$1" pin="CSI1_D1-" pad="50"/>
<connect gate="G$1" pin="DSI_CLK+" pad="21"/>
<connect gate="G$1" pin="DSI_CLK-" pad="23"/>
<connect gate="G$1" pin="DSI_D0+" pad="27"/>
<connect gate="G$1" pin="DSI_D0-" pad="29"/>
<connect gate="G$1" pin="DSI_D1+" pad="33"/>
<connect gate="G$1" pin="DSI_D1-" pad="35"/>
<connect gate="G$1" pin="DSI_D2+" pad="39"/>
<connect gate="G$1" pin="DSI_D2-" pad="41"/>
<connect gate="G$1" pin="DSI_D3+" pad="45"/>
<connect gate="G$1" pin="DSI_D3-" pad="47"/>
<connect gate="G$1" pin="GND" pad="6 12 13 18 19 24 25 30 31 37 40 43 46 49 52 55 58"/>
<connect gate="G$1" pin="HSIC_DATA" pad="59"/>
<connect gate="G$1" pin="HSIC_STR" pad="57"/>
<connect gate="G$1" pin="I2C2_SCL" pad="32"/>
<connect gate="G$1" pin="I2C2_SDA" pad="34"/>
<connect gate="G$1" pin="I2C3_SCL" pad="36"/>
<connect gate="G$1" pin="I2C3_SDA" pad="38"/>
<connect gate="G$1" pin="SD_CMD/SPI1_DIN" pad="11"/>
<connect gate="G$1" pin="SD_DAT0/SPI1_DOUT" pad="1"/>
<connect gate="G$1" pin="SD_DAT1" pad="3"/>
<connect gate="G$1" pin="SD_DAT2" pad="5"/>
<connect gate="G$1" pin="SD_DAT3/SPI1_CS" pad="7"/>
<connect gate="G$1" pin="SD_SCLK/SPI1_SCLK" pad="9"/>
<connect gate="G$1" pin="USB_D+" pad="51"/>
<connect gate="G$1" pin="USB_D-" pad="53"/>
</connects>
<technologies>
<technology name="">
<attribute name="VALUE" value="96BOARDS HIGH SPEED"/>
</technology>
</technologies>
</device>
<device name="TOP" package="2X30-BERGSTAK-0.8MM-M">
<connects>
<connect gate="G$1" pin="CLK0/CSI0_MCLK" pad="15"/>
<connect gate="G$1" pin="CLK1/CSI1_MCLK" pad="17"/>
<connect gate="G$1" pin="CSI0_C+" pad="2"/>
<connect gate="G$1" pin="CSI0_C-" pad="4"/>
<connect gate="G$1" pin="CSI0_D0+" pad="8"/>
<connect gate="G$1" pin="CSI0_D0-" pad="10"/>
<connect gate="G$1" pin="CSI0_D1+" pad="14"/>
<connect gate="G$1" pin="CSI0_D1-" pad="16"/>
<connect gate="G$1" pin="CSI0_D2+" pad="20"/>
<connect gate="G$1" pin="CSI0_D2-" pad="22"/>
<connect gate="G$1" pin="CSI0_D3+" pad="26"/>
<connect gate="G$1" pin="CSI0_D3-" pad="28"/>
<connect gate="G$1" pin="CSI1_C+" pad="54"/>
<connect gate="G$1" pin="CSI1_C-" pad="56"/>
<connect gate="G$1" pin="CSI1_D0+" pad="42"/>
<connect gate="G$1" pin="CSI1_D0-" pad="44"/>
<connect gate="G$1" pin="CSI1_D1+" pad="48"/>
<connect gate="G$1" pin="CSI1_D1-" pad="50"/>
<connect gate="G$1" pin="DSI_CLK+" pad="21"/>
<connect gate="G$1" pin="DSI_CLK-" pad="23"/>
<connect gate="G$1" pin="DSI_D0+" pad="27"/>
<connect gate="G$1" pin="DSI_D0-" pad="29"/>
<connect gate="G$1" pin="DSI_D1+" pad="33"/>
<connect gate="G$1" pin="DSI_D1-" pad="35"/>
<connect gate="G$1" pin="DSI_D2+" pad="39"/>
<connect gate="G$1" pin="DSI_D2-" pad="41"/>
<connect gate="G$1" pin="DSI_D3+" pad="45"/>
<connect gate="G$1" pin="DSI_D3-" pad="47"/>
<connect gate="G$1" pin="GND" pad="6 12 13 18 19 24 25 30 31 37 40 43 46 49 52 55 58"/>
<connect gate="G$1" pin="HSIC_DATA" pad="59"/>
<connect gate="G$1" pin="HSIC_STR" pad="57"/>
<connect gate="G$1" pin="I2C2_SCL" pad="32"/>
<connect gate="G$1" pin="I2C2_SDA" pad="34"/>
<connect gate="G$1" pin="I2C3_SCL" pad="36"/>
<connect gate="G$1" pin="I2C3_SDA" pad="38"/>
<connect gate="G$1" pin="SD_CMD/SPI1_DIN" pad="11"/>
<connect gate="G$1" pin="SD_DAT0/SPI1_DOUT" pad="1"/>
<connect gate="G$1" pin="SD_DAT1" pad="3"/>
<connect gate="G$1" pin="SD_DAT2" pad="5"/>
<connect gate="G$1" pin="SD_DAT3/SPI1_CS" pad="7"/>
<connect gate="G$1" pin="SD_SCLK/SPI1_SCLK" pad="9"/>
<connect gate="G$1" pin="USB_D+" pad="51"/>
<connect gate="G$1" pin="USB_D-" pad="53"/>
</connects>
<technologies>
<technology name="">
<attribute name="VALUE" value="96 BOARDS HIGH SPEED"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="96BOARDS_LOW_SPEED" prefix="J">
<description>96 BOARDS SPEC LOW SPEED CONNECTOR &lt;br&gt;&lt;br&gt;


2x20, 40-pin, header for low speed expansion. &lt;br&gt;
Has UARTS, I2C, I2S, SPI and GPIO.&lt;br&gt;&lt;br&gt;

* 2mm-pitch variant interfaces directly with the header on a 96-boards-compliant board.&lt;br&gt;
* 0.1-pitch version is for applications where the header has been translated to the larger, more available 0.1" 2x20 connector.&lt;br&gt;&lt;br&gt;

For more details, see the spec at https://www.96boards.org</description>
<gates>
<gate name="G$1" symbol="96BOARDS-LO-SPEED"/>
</gates>
<devices>
<device name="PTH" package="2X20-2MM-SHROUDED-PTH">
<connects>
<connect gate="G$1" pin="!PWR_BTN" pad="4"/>
<connect gate="G$1" pin="!RST_BTN" pad="6"/>
<connect gate="G$1" pin="1.8V" pad="35"/>
<connect gate="G$1" pin="5V" pad="37"/>
<connect gate="G$1" pin="GND" pad="1 2 39 40"/>
<connect gate="G$1" pin="GPIO-A" pad="23"/>
<connect gate="G$1" pin="GPIO-B" pad="24"/>
<connect gate="G$1" pin="GPIO-C" pad="25"/>
<connect gate="G$1" pin="GPIO-D" pad="26"/>
<connect gate="G$1" pin="GPIO-E" pad="27"/>
<connect gate="G$1" pin="GPIO-F" pad="28"/>
<connect gate="G$1" pin="GPIO-G" pad="29"/>
<connect gate="G$1" pin="GPIO-H" pad="30"/>
<connect gate="G$1" pin="GPIO-I" pad="31"/>
<connect gate="G$1" pin="GPIO-J" pad="32"/>
<connect gate="G$1" pin="GPIO-K" pad="33"/>
<connect gate="G$1" pin="GPIO-L" pad="34"/>
<connect gate="G$1" pin="I2C0_SCL" pad="15"/>
<connect gate="G$1" pin="I2C0_SDA" pad="17"/>
<connect gate="G$1" pin="I2C1_SCL" pad="19"/>
<connect gate="G$1" pin="I2C1_SDA" pad="21"/>
<connect gate="G$1" pin="I2S_CLK" pad="18"/>
<connect gate="G$1" pin="I2S_DI" pad="22"/>
<connect gate="G$1" pin="I2S_DO" pad="20"/>
<connect gate="G$1" pin="I2S_FS" pad="16"/>
<connect gate="G$1" pin="SPI0_CS" pad="12"/>
<connect gate="G$1" pin="SPI0_DIN" pad="10"/>
<connect gate="G$1" pin="SPI0_DOUT" pad="14"/>
<connect gate="G$1" pin="SPI0_SCLK" pad="8"/>
<connect gate="G$1" pin="SYS_DCIN" pad="36 38"/>
<connect gate="G$1" pin="UART0_CTS" pad="3"/>
<connect gate="G$1" pin="UART0_RTS" pad="9"/>
<connect gate="G$1" pin="UART0_RXD" pad="7"/>
<connect gate="G$1" pin="UART0_TXD" pad="5"/>
<connect gate="G$1" pin="UART1_RXD" pad="13"/>
<connect gate="G$1" pin="UART1_TXD" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0.1&quot;-PTH" package="2X20-SHROUDED">
<connects>
<connect gate="G$1" pin="!PWR_BTN" pad="4"/>
<connect gate="G$1" pin="!RST_BTN" pad="6"/>
<connect gate="G$1" pin="1.8V" pad="35"/>
<connect gate="G$1" pin="5V" pad="37"/>
<connect gate="G$1" pin="GND" pad="1 2 39 40"/>
<connect gate="G$1" pin="GPIO-A" pad="23"/>
<connect gate="G$1" pin="GPIO-B" pad="24"/>
<connect gate="G$1" pin="GPIO-C" pad="25"/>
<connect gate="G$1" pin="GPIO-D" pad="26"/>
<connect gate="G$1" pin="GPIO-E" pad="27"/>
<connect gate="G$1" pin="GPIO-F" pad="28"/>
<connect gate="G$1" pin="GPIO-G" pad="29"/>
<connect gate="G$1" pin="GPIO-H" pad="30"/>
<connect gate="G$1" pin="GPIO-I" pad="31"/>
<connect gate="G$1" pin="GPIO-J" pad="32"/>
<connect gate="G$1" pin="GPIO-K" pad="33"/>
<connect gate="G$1" pin="GPIO-L" pad="34"/>
<connect gate="G$1" pin="I2C0_SCL" pad="15"/>
<connect gate="G$1" pin="I2C0_SDA" pad="17"/>
<connect gate="G$1" pin="I2C1_SCL" pad="19"/>
<connect gate="G$1" pin="I2C1_SDA" pad="21"/>
<connect gate="G$1" pin="I2S_CLK" pad="18"/>
<connect gate="G$1" pin="I2S_DI" pad="22"/>
<connect gate="G$1" pin="I2S_DO" pad="20"/>
<connect gate="G$1" pin="I2S_FS" pad="16"/>
<connect gate="G$1" pin="SPI0_CS" pad="12"/>
<connect gate="G$1" pin="SPI0_DIN" pad="10"/>
<connect gate="G$1" pin="SPI0_DOUT" pad="14"/>
<connect gate="G$1" pin="SPI0_SCLK" pad="8"/>
<connect gate="G$1" pin="SYS_DCIN" pad="36 38"/>
<connect gate="G$1" pin="UART0_CTS" pad="3"/>
<connect gate="G$1" pin="UART0_RTS" pad="9"/>
<connect gate="G$1" pin="UART0_RXD" pad="7"/>
<connect gate="G$1" pin="UART0_TXD" pad="5"/>
<connect gate="G$1" pin="UART1_RXD" pad="13"/>
<connect gate="G$1" pin="UART1_TXD" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMT-F" package="2X20-2MM-SMT-F">
<connects>
<connect gate="G$1" pin="!PWR_BTN" pad="4"/>
<connect gate="G$1" pin="!RST_BTN" pad="6"/>
<connect gate="G$1" pin="1.8V" pad="35"/>
<connect gate="G$1" pin="5V" pad="37"/>
<connect gate="G$1" pin="GND" pad="1 2 39 40"/>
<connect gate="G$1" pin="GPIO-A" pad="23"/>
<connect gate="G$1" pin="GPIO-B" pad="24"/>
<connect gate="G$1" pin="GPIO-C" pad="25"/>
<connect gate="G$1" pin="GPIO-D" pad="26"/>
<connect gate="G$1" pin="GPIO-E" pad="27"/>
<connect gate="G$1" pin="GPIO-F" pad="28"/>
<connect gate="G$1" pin="GPIO-G" pad="29"/>
<connect gate="G$1" pin="GPIO-H" pad="30"/>
<connect gate="G$1" pin="GPIO-I" pad="31"/>
<connect gate="G$1" pin="GPIO-J" pad="32"/>
<connect gate="G$1" pin="GPIO-K" pad="33"/>
<connect gate="G$1" pin="GPIO-L" pad="34"/>
<connect gate="G$1" pin="I2C0_SCL" pad="15"/>
<connect gate="G$1" pin="I2C0_SDA" pad="17"/>
<connect gate="G$1" pin="I2C1_SCL" pad="19"/>
<connect gate="G$1" pin="I2C1_SDA" pad="21"/>
<connect gate="G$1" pin="I2S_CLK" pad="18"/>
<connect gate="G$1" pin="I2S_DI" pad="22"/>
<connect gate="G$1" pin="I2S_DO" pad="20"/>
<connect gate="G$1" pin="I2S_FS" pad="16"/>
<connect gate="G$1" pin="SPI0_CS" pad="12"/>
<connect gate="G$1" pin="SPI0_DIN" pad="10"/>
<connect gate="G$1" pin="SPI0_DOUT" pad="14"/>
<connect gate="G$1" pin="SPI0_SCLK" pad="8"/>
<connect gate="G$1" pin="SYS_DCIN" pad="36 38"/>
<connect gate="G$1" pin="UART0_CTS" pad="3"/>
<connect gate="G$1" pin="UART0_RTS" pad="9"/>
<connect gate="G$1" pin="UART0_RXD" pad="7"/>
<connect gate="G$1" pin="UART0_TXD" pad="5"/>
<connect gate="G$1" pin="UART1_RXD" pad="13"/>
<connect gate="G$1" pin="UART1_TXD" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-12977"/>
</technology>
</technologies>
</device>
<device name="SMT-M-BOTTOM" package="2X20-2MM-SHROUDED-SMT-BOTTOM-M">
<connects>
<connect gate="G$1" pin="!PWR_BTN" pad="4"/>
<connect gate="G$1" pin="!RST_BTN" pad="6"/>
<connect gate="G$1" pin="1.8V" pad="35"/>
<connect gate="G$1" pin="5V" pad="37"/>
<connect gate="G$1" pin="GND" pad="1 2 39 40"/>
<connect gate="G$1" pin="GPIO-A" pad="23"/>
<connect gate="G$1" pin="GPIO-B" pad="24"/>
<connect gate="G$1" pin="GPIO-C" pad="25"/>
<connect gate="G$1" pin="GPIO-D" pad="26"/>
<connect gate="G$1" pin="GPIO-E" pad="27"/>
<connect gate="G$1" pin="GPIO-F" pad="28"/>
<connect gate="G$1" pin="GPIO-G" pad="29"/>
<connect gate="G$1" pin="GPIO-H" pad="30"/>
<connect gate="G$1" pin="GPIO-I" pad="31"/>
<connect gate="G$1" pin="GPIO-J" pad="32"/>
<connect gate="G$1" pin="GPIO-K" pad="33"/>
<connect gate="G$1" pin="GPIO-L" pad="34"/>
<connect gate="G$1" pin="I2C0_SCL" pad="15"/>
<connect gate="G$1" pin="I2C0_SDA" pad="17"/>
<connect gate="G$1" pin="I2C1_SCL" pad="19"/>
<connect gate="G$1" pin="I2C1_SDA" pad="21"/>
<connect gate="G$1" pin="I2S_CLK" pad="18"/>
<connect gate="G$1" pin="I2S_DI" pad="22"/>
<connect gate="G$1" pin="I2S_DO" pad="20"/>
<connect gate="G$1" pin="I2S_FS" pad="16"/>
<connect gate="G$1" pin="SPI0_CS" pad="12"/>
<connect gate="G$1" pin="SPI0_DIN" pad="10"/>
<connect gate="G$1" pin="SPI0_DOUT" pad="14"/>
<connect gate="G$1" pin="SPI0_SCLK" pad="8"/>
<connect gate="G$1" pin="SYS_DCIN" pad="36 38"/>
<connect gate="G$1" pin="UART0_CTS" pad="3"/>
<connect gate="G$1" pin="UART0_RTS" pad="9"/>
<connect gate="G$1" pin="UART0_RXD" pad="7"/>
<connect gate="G$1" pin="UART0_TXD" pad="5"/>
<connect gate="G$1" pin="UART1_RXD" pad="13"/>
<connect gate="G$1" pin="UART1_TXD" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-12975"/>
</technology>
</technologies>
</device>
<device name="" package="2X20-2MM-SHROUDED-RA-PTH">
<connects>
<connect gate="G$1" pin="!PWR_BTN" pad="4"/>
<connect gate="G$1" pin="!RST_BTN" pad="6"/>
<connect gate="G$1" pin="1.8V" pad="35"/>
<connect gate="G$1" pin="5V" pad="37"/>
<connect gate="G$1" pin="GND" pad="1 2 39 40"/>
<connect gate="G$1" pin="GPIO-A" pad="23"/>
<connect gate="G$1" pin="GPIO-B" pad="24"/>
<connect gate="G$1" pin="GPIO-C" pad="25"/>
<connect gate="G$1" pin="GPIO-D" pad="26"/>
<connect gate="G$1" pin="GPIO-E" pad="27"/>
<connect gate="G$1" pin="GPIO-F" pad="28"/>
<connect gate="G$1" pin="GPIO-G" pad="29"/>
<connect gate="G$1" pin="GPIO-H" pad="30"/>
<connect gate="G$1" pin="GPIO-I" pad="31"/>
<connect gate="G$1" pin="GPIO-J" pad="32"/>
<connect gate="G$1" pin="GPIO-K" pad="33"/>
<connect gate="G$1" pin="GPIO-L" pad="34"/>
<connect gate="G$1" pin="I2C0_SCL" pad="15"/>
<connect gate="G$1" pin="I2C0_SDA" pad="17"/>
<connect gate="G$1" pin="I2C1_SCL" pad="19"/>
<connect gate="G$1" pin="I2C1_SDA" pad="21"/>
<connect gate="G$1" pin="I2S_CLK" pad="18"/>
<connect gate="G$1" pin="I2S_DI" pad="22"/>
<connect gate="G$1" pin="I2S_DO" pad="20"/>
<connect gate="G$1" pin="I2S_FS" pad="16"/>
<connect gate="G$1" pin="SPI0_CS" pad="12"/>
<connect gate="G$1" pin="SPI0_DIN" pad="10"/>
<connect gate="G$1" pin="SPI0_DOUT" pad="14"/>
<connect gate="G$1" pin="SPI0_SCLK" pad="8"/>
<connect gate="G$1" pin="SYS_DCIN" pad="36 38"/>
<connect gate="G$1" pin="UART0_CTS" pad="3"/>
<connect gate="G$1" pin="UART0_RTS" pad="9"/>
<connect gate="G$1" pin="UART0_RXD" pad="7"/>
<connect gate="G$1" pin="UART0_TXD" pad="5"/>
<connect gate="G$1" pin="UART1_RXD" pad="13"/>
<connect gate="G$1" pin="UART1_TXD" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMT-M-TOP" package="2X20-2MM-SHROUDED-SMT-TOP-M">
<connects>
<connect gate="G$1" pin="!PWR_BTN" pad="4"/>
<connect gate="G$1" pin="!RST_BTN" pad="6"/>
<connect gate="G$1" pin="1.8V" pad="35"/>
<connect gate="G$1" pin="5V" pad="37"/>
<connect gate="G$1" pin="GND" pad="1 2 39 40"/>
<connect gate="G$1" pin="GPIO-A" pad="23"/>
<connect gate="G$1" pin="GPIO-B" pad="24"/>
<connect gate="G$1" pin="GPIO-C" pad="25"/>
<connect gate="G$1" pin="GPIO-D" pad="26"/>
<connect gate="G$1" pin="GPIO-E" pad="27"/>
<connect gate="G$1" pin="GPIO-F" pad="28"/>
<connect gate="G$1" pin="GPIO-G" pad="29"/>
<connect gate="G$1" pin="GPIO-H" pad="30"/>
<connect gate="G$1" pin="GPIO-I" pad="31"/>
<connect gate="G$1" pin="GPIO-J" pad="32"/>
<connect gate="G$1" pin="GPIO-K" pad="33"/>
<connect gate="G$1" pin="GPIO-L" pad="34"/>
<connect gate="G$1" pin="I2C0_SCL" pad="15"/>
<connect gate="G$1" pin="I2C0_SDA" pad="17"/>
<connect gate="G$1" pin="I2C1_SCL" pad="19"/>
<connect gate="G$1" pin="I2C1_SDA" pad="21"/>
<connect gate="G$1" pin="I2S_CLK" pad="18"/>
<connect gate="G$1" pin="I2S_DI" pad="22"/>
<connect gate="G$1" pin="I2S_DO" pad="20"/>
<connect gate="G$1" pin="I2S_FS" pad="16"/>
<connect gate="G$1" pin="SPI0_CS" pad="12"/>
<connect gate="G$1" pin="SPI0_DIN" pad="10"/>
<connect gate="G$1" pin="SPI0_DOUT" pad="14"/>
<connect gate="G$1" pin="SPI0_SCLK" pad="8"/>
<connect gate="G$1" pin="SYS_DCIN" pad="36 38"/>
<connect gate="G$1" pin="UART0_CTS" pad="3"/>
<connect gate="G$1" pin="UART0_RTS" pad="9"/>
<connect gate="G$1" pin="UART0_RXD" pad="7"/>
<connect gate="G$1" pin="UART0_TXD" pad="5"/>
<connect gate="G$1" pin="UART1_RXD" pad="13"/>
<connect gate="G$1" pin="UART1_TXD" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-12975"/>
</technology>
</technologies>
</device>
<device name="RIBBON-COMPATIBLE" package="2X20-2MM-SHROUDED-SMT-RIBBON-M">
<connects>
<connect gate="G$1" pin="!PWR_BTN" pad="4"/>
<connect gate="G$1" pin="!RST_BTN" pad="6"/>
<connect gate="G$1" pin="1.8V" pad="35"/>
<connect gate="G$1" pin="5V" pad="37"/>
<connect gate="G$1" pin="GND" pad="1 2 39 40"/>
<connect gate="G$1" pin="GPIO-A" pad="23"/>
<connect gate="G$1" pin="GPIO-B" pad="24"/>
<connect gate="G$1" pin="GPIO-C" pad="25"/>
<connect gate="G$1" pin="GPIO-D" pad="26"/>
<connect gate="G$1" pin="GPIO-E" pad="27"/>
<connect gate="G$1" pin="GPIO-F" pad="28"/>
<connect gate="G$1" pin="GPIO-G" pad="29"/>
<connect gate="G$1" pin="GPIO-H" pad="30"/>
<connect gate="G$1" pin="GPIO-I" pad="31"/>
<connect gate="G$1" pin="GPIO-J" pad="32"/>
<connect gate="G$1" pin="GPIO-K" pad="33"/>
<connect gate="G$1" pin="GPIO-L" pad="34"/>
<connect gate="G$1" pin="I2C0_SCL" pad="15"/>
<connect gate="G$1" pin="I2C0_SDA" pad="17"/>
<connect gate="G$1" pin="I2C1_SCL" pad="19"/>
<connect gate="G$1" pin="I2C1_SDA" pad="21"/>
<connect gate="G$1" pin="I2S_CLK" pad="18"/>
<connect gate="G$1" pin="I2S_DI" pad="22"/>
<connect gate="G$1" pin="I2S_DO" pad="20"/>
<connect gate="G$1" pin="I2S_FS" pad="16"/>
<connect gate="G$1" pin="SPI0_CS" pad="12"/>
<connect gate="G$1" pin="SPI0_DIN" pad="10"/>
<connect gate="G$1" pin="SPI0_DOUT" pad="14"/>
<connect gate="G$1" pin="SPI0_SCLK" pad="8"/>
<connect gate="G$1" pin="SYS_DCIN" pad="36 38"/>
<connect gate="G$1" pin="UART0_CTS" pad="3"/>
<connect gate="G$1" pin="UART0_RTS" pad="9"/>
<connect gate="G$1" pin="UART0_RXD" pad="7"/>
<connect gate="G$1" pin="UART0_TXD" pad="5"/>
<connect gate="G$1" pin="UART1_RXD" pad="13"/>
<connect gate="G$1" pin="UART1_TXD" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO_DUEMILANOVE" prefix="U">
<description>&lt;h3&gt;Arduino Duemilanove Shield Footprint&lt;/h3&gt;

Shield form compatible with the Arduino Duemilanove.</description>
<gates>
<gate name="G$1" symbol="ARDUINO_SHIELD"/>
</gates>
<devices>
<device name="LABEL" package="DUEMILANOVE_SHIELD">
<connects>
<connect gate="G$1" pin="*D10" pad="D10"/>
<connect gate="G$1" pin="*D11" pad="D11"/>
<connect gate="G$1" pin="*D3" pad="D3"/>
<connect gate="G$1" pin="*D5" pad="D5"/>
<connect gate="G$1" pin="*D6" pad="D6"/>
<connect gate="G$1" pin="*D9" pad="D9"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="GND@0" pad="GND@0"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="RES" pad="RES"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NO_SILK" package="DUEMILANOVE_VIAS">
<connects>
<connect gate="G$1" pin="*D10" pad="D10"/>
<connect gate="G$1" pin="*D11" pad="D11"/>
<connect gate="G$1" pin="*D3" pad="D3"/>
<connect gate="G$1" pin="*D5" pad="D5"/>
<connect gate="G$1" pin="*D6" pad="D6"/>
<connect gate="G$1" pin="*D9" pad="D9"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="GND@0" pad="GND@0"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="RES" pad="RES"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NOHOLES" package="DUEMILANOVE_SHIELD_NOHOLES">
<connects>
<connect gate="G$1" pin="*D10" pad="D10"/>
<connect gate="G$1" pin="*D11" pad="D11"/>
<connect gate="G$1" pin="*D3" pad="D3"/>
<connect gate="G$1" pin="*D5" pad="D5"/>
<connect gate="G$1" pin="*D6" pad="D6"/>
<connect gate="G$1" pin="*D9" pad="D9"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="GND@0" pad="GND@0"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="RES" pad="RES"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LONGPADS" package="DUEMILANOVE_SHIELD_LONGPADS">
<connects>
<connect gate="G$1" pin="*D10" pad="D10"/>
<connect gate="G$1" pin="*D11" pad="D11"/>
<connect gate="G$1" pin="*D3" pad="D3"/>
<connect gate="G$1" pin="*D5" pad="D5"/>
<connect gate="G$1" pin="*D6" pad="D6"/>
<connect gate="G$1" pin="*D9" pad="D9"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="GND@0" pad="GND@0"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="RES" pad="RES"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NOLABELS" package="DUEMILANOVE_SHIELD_NOLABELS">
<connects>
<connect gate="G$1" pin="*D10" pad="D10"/>
<connect gate="G$1" pin="*D11" pad="D11"/>
<connect gate="G$1" pin="*D3" pad="D3"/>
<connect gate="G$1" pin="*D5" pad="D5"/>
<connect gate="G$1" pin="*D6" pad="D6"/>
<connect gate="G$1" pin="*D9" pad="D9"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="GND@0" pad="GND@0"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="RES" pad="RES"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NOHOLESORLABELS" package="DUEMILANOVE_SHIELD_NOHOLES_NOLABELS">
<connects>
<connect gate="G$1" pin="*D10" pad="D10"/>
<connect gate="G$1" pin="*D11" pad="D11"/>
<connect gate="G$1" pin="*D3" pad="D3"/>
<connect gate="G$1" pin="*D5" pad="D5"/>
<connect gate="G$1" pin="*D6" pad="D6"/>
<connect gate="G$1" pin="*D9" pad="D9"/>
<connect gate="G$1" pin="3.3V" pad="3.3V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="A0" pad="A0"/>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="AREF" pad="AREF"/>
<connect gate="G$1" pin="D12" pad="D12"/>
<connect gate="G$1" pin="D13" pad="D13"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="D7" pad="D7"/>
<connect gate="G$1" pin="D8" pad="D8"/>
<connect gate="G$1" pin="GND@0" pad="GND@0"/>
<connect gate="G$1" pin="GND@1" pad="GND@1"/>
<connect gate="G$1" pin="GND@2" pad="GND@2"/>
<connect gate="G$1" pin="RES" pad="RES"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO_MINI">
<description>Arduino Pro Mini footprint</description>
<gates>
<gate name="G$1" symbol="ARDUINO_MINI"/>
</gates>
<devices>
<device name="" package="ARDUINO_MINI">
<connects>
<connect gate="G$1" pin="10" pad="13"/>
<connect gate="G$1" pin="11" pad="14"/>
<connect gate="G$1" pin="12" pad="15"/>
<connect gate="G$1" pin="13" pad="16"/>
<connect gate="G$1" pin="2" pad="5"/>
<connect gate="G$1" pin="3" pad="6"/>
<connect gate="G$1" pin="4" pad="7"/>
<connect gate="G$1" pin="5" pad="8"/>
<connect gate="G$1" pin="6" pad="9"/>
<connect gate="G$1" pin="7" pad="10"/>
<connect gate="G$1" pin="8" pad="11"/>
<connect gate="G$1" pin="9" pad="12"/>
<connect gate="G$1" pin="A0" pad="17"/>
<connect gate="G$1" pin="A1" pad="18"/>
<connect gate="G$1" pin="A2" pad="19"/>
<connect gate="G$1" pin="A3" pad="20"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="23"/>
<connect gate="G$1" pin="RAW" pad="24"/>
<connect gate="G$1" pin="RST" pad="3"/>
<connect gate="G$1" pin="RST@2" pad="22"/>
<connect gate="G$1" pin="RXI" pad="2"/>
<connect gate="G$1" pin="TXO" pad="1"/>
<connect gate="G$1" pin="VCC" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCB_DP_RECTANGLE" prefix="PCB">
<description>Dangerous Prototypes Standard Rectangular PCB sizes</description>
<gates>
<gate name="G$1" symbol="PCB_STANDARD"/>
</gates>
<devices>
<device name="-37X60" package="DP6037_V1">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XPORT">
<description>TCP/IP stack and phy in RJ-45 jack footprint</description>
<gates>
<gate name="G$1" symbol="XPORT"/>
</gates>
<devices>
<device name="" package="XPORT">
<connects>
<connect gate="G$1" pin="3.3V" pad="P2"/>
<connect gate="G$1" pin="CTS" pad="P8"/>
<connect gate="G$1" pin="DTR" pad="P7"/>
<connect gate="G$1" pin="GND" pad="P1"/>
<connect gate="G$1" pin="RST" pad="P3"/>
<connect gate="G$1" pin="RTS" pad="P6"/>
<connect gate="G$1" pin="RX" pad="P5"/>
<connect gate="G$1" pin="TX" pad="P4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XPORT-DIRECT">
<description>TCP/IP phy and stack module</description>
<gates>
<gate name="G$1" symbol="XPORT_DIRECT"/>
</gates>
<devices>
<device name="" package="XPORT_DIRECT_MODULE">
<connects>
<connect gate="G$1" pin="3.3V" pad="P3"/>
<connect gate="G$1" pin="CP1" pad="P23"/>
<connect gate="G$1" pin="CP2" pad="P21"/>
<connect gate="G$1" pin="CTS" pad="P15"/>
<connect gate="G$1" pin="DTR" pad="P13"/>
<connect gate="G$1" pin="GND@1" pad="P1"/>
<connect gate="G$1" pin="GND@2" pad="P2"/>
<connect gate="G$1" pin="GND@24" pad="P24"/>
<connect gate="G$1" pin="RST" pad="P5"/>
<connect gate="G$1" pin="RTS" pad="P11"/>
<connect gate="G$1" pin="RX" pad="P9"/>
<connect gate="G$1" pin="TX" pad="P7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="XPORT_DIRECT_MODULE-SMD">
<connects>
<connect gate="G$1" pin="3.3V" pad="P3"/>
<connect gate="G$1" pin="CP1" pad="P23"/>
<connect gate="G$1" pin="CP2" pad="P21"/>
<connect gate="G$1" pin="CTS" pad="P15"/>
<connect gate="G$1" pin="DTR" pad="P13"/>
<connect gate="G$1" pin="GND@1" pad="P1"/>
<connect gate="G$1" pin="GND@2" pad="P2"/>
<connect gate="G$1" pin="GND@24" pad="P24"/>
<connect gate="G$1" pin="RST" pad="P5"/>
<connect gate="G$1" pin="RTS" pad="P11"/>
<connect gate="G$1" pin="RX" pad="P9"/>
<connect gate="G$1" pin="TX" pad="P7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LIGHTPIPE-7511">
<gates>
<gate name="G$1" symbol="LIGHTPIPE-7511"/>
</gates>
<devices>
<device name="" package="LIGHTPIPE-7511">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="APA3010SF4C" prefix="D">
<description>DIO-10854 &lt;BR&gt;&lt;br&gt;
Right-angle 880nm SMT infrared LED</description>
<gates>
<gate name="G$1" symbol="APA3010SF4C"/>
</gates>
<devices>
<device name="" package="APA3010SF4C">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-10854"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LUXEON">
<description>&lt;b&gt;Luxeon LED&lt;/b&gt;
This footprint works with the current 1 Watt, 3 Watt, and 5 Watt LEDs. These blindingly bright LEDs generate a lot of heat so the footprint has a large pad under the LED for thermal transfer. Schematic and footprint are proven. Spark Fun Electronics SKU : COM-00603</description>
<gates>
<gate name="G$1" symbol="LUXEON"/>
</gates>
<devices>
<device name="SMD" package="LUXEON">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LUXEON-REBEL">
<description>Luxeon Rebel single-color high output LED</description>
<gates>
<gate name="G$1" symbol="LUXEON"/>
</gates>
<devices>
<device name="" package="LUXEON-REBEL">
<connects>
<connect gate="G$1" pin="A" pad="ANODE"/>
<connect gate="G$1" pin="C" pad="CATHODE"/>
<connect gate="G$1" pin="S" pad="P$3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-PURPLE" prefix="D" uservalue="yes">
<description>Various green LEDs&lt;br&gt;
0603- DIO-00821&lt;br&gt;
LARGE- DIO-00862&lt;br&gt;
LILYPAD- DIO-09910&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="LED-2"/>
</gates>
<devices>
<device name="1206" package="LED-1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-11140"/>
<attribute name="VALUE" value="PURPLE"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATARI_CONNECTOR">
<description>DB9 labeled for Atari joystick</description>
<gates>
<gate name="G$1" symbol="ATARI_CONNECTOR"/>
</gates>
<devices>
<device name="" package="ATARI_CONNECTOR">
<connects>
<connect gate="G$1" pin="BUTTON" pad="P$1"/>
<connect gate="G$1" pin="DOWN" pad="P$6"/>
<connect gate="G$1" pin="GND" pad="P$3"/>
<connect gate="G$1" pin="LEFT" pad="P$7"/>
<connect gate="G$1" pin="NC1" pad="P$9"/>
<connect gate="G$1" pin="NC2" pad="P$2"/>
<connect gate="G$1" pin="NC3" pad="P$4"/>
<connect gate="G$1" pin="RIGHT" pad="P$8"/>
<connect gate="G$1" pin="UP" pad="P$5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DB15">
<description>DB15 / VGA right angle through-hole female connector.</description>
<gates>
<gate name="G$1" symbol="DB15"/>
</gates>
<devices>
<device name="" package="DB15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DB25_FEMALE" prefix="X" uservalue="yes">
<description>25 Pin male connector. PCB edge mount for regular PCB thicknesses. This connector will connect directly to the back of a PC parallel port or through a normal DB25 extension cable (M/F). SKU: PRT-08287</description>
<gates>
<gate name="-1" symbol="F25"/>
</gates>
<devices>
<device name="D" package="F25D">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="H" package="F25H">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HP" package="F25HP">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V" package="F25V">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VP" package="F25VP">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VB" package="F25VB">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DB25_MALE" prefix="X" uservalue="yes">
<description>Various DB25 connectors</description>
<gates>
<gate name="-1" symbol="DB25"/>
</gates>
<devices>
<device name="D" package="M25D">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="H" package="M25H">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HP" package="M25HP">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V" package="M25V">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VP" package="M25VP">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VB" package="M25VB">
<connects>
<connect gate="-1" pin="1" pad="1"/>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="17" pad="17"/>
<connect gate="-1" pin="18" pad="18"/>
<connect gate="-1" pin="19" pad="19"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="20" pad="20"/>
<connect gate="-1" pin="21" pad="21"/>
<connect gate="-1" pin="22" pad="22"/>
<connect gate="-1" pin="23" pad="23"/>
<connect gate="-1" pin="24" pad="24"/>
<connect gate="-1" pin="25" pad="25"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="4" pad="4"/>
<connect gate="-1" pin="5" pad="5"/>
<connect gate="-1" pin="6" pad="6"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IPOD_CONNECTOR_FEMALE">
<description>&lt;b&gt;iPod Female Connector&lt;/b&gt;
This is the connector found inside current iPods. Use this connector to attach to iPod accessories like Nike+iPods, etc. Schematic and footprint are not yet production proven. Spark Fun Electronics SKU : DEV-08035</description>
<gates>
<gate name="G$1" symbol="IPOD_CONNECTOR_FEMALE"/>
</gates>
<devices>
<device name="" package="IPOD_FEMALE_CONNECTOR">
<connects>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="3.3V" pad="18"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="ACC_INDICATOR" pad="21"/>
<connect gate="G$1" pin="FW_12V@19" pad="19"/>
<connect gate="G$1" pin="FW_12V@20" pad="20"/>
<connect gate="G$1" pin="FW_TPA+" pad="24"/>
<connect gate="G$1" pin="FW_TPA-" pad="22"/>
<connect gate="G$1" pin="FW_TPB+" pad="28"/>
<connect gate="G$1" pin="FW_TPB-" pad="26"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@11" pad="11"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@16" pad="16"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@29" pad="29"/>
<connect gate="G$1" pin="GND@30" pad="30"/>
<connect gate="G$1" pin="LEFT_IN" pad="6"/>
<connect gate="G$1" pin="LEFT_OUT" pad="4"/>
<connect gate="G$1" pin="RIGHT_IN" pad="5"/>
<connect gate="G$1" pin="RIGHT_OUT" pad="3"/>
<connect gate="G$1" pin="RX" pad="13"/>
<connect gate="G$1" pin="SCHROME_OUT" pad="9"/>
<connect gate="G$1" pin="SLUM_OUT" pad="10"/>
<connect gate="G$1" pin="TX" pad="12"/>
<connect gate="G$1" pin="USB_5V" pad="23"/>
<connect gate="G$1" pin="USB_D+" pad="27"/>
<connect gate="G$1" pin="USB_D-" pad="25"/>
<connect gate="G$1" pin="VIDEO_OUT" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IPOD_CONNECTOR_MALE">
<description>&lt;b&gt;iPod Male Connector&lt;/b&gt;
This is the connector that will insert into an iPods. Use this connector to gain access to the various iPod pins. Schematic and footprint are not yet production proven. The PCB thickness must be more thin than the standard 0.062" FR4. Spark Fun Electronics SKU : DEV-00633</description>
<gates>
<gate name="G$1" symbol="IPOD_CONNECTOR_FEMALE"/>
</gates>
<devices>
<device name="" package="IPOD_MALE_CONNECTOR">
<connects>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="3.3V" pad="18"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="ACC_INDICATOR" pad="21"/>
<connect gate="G$1" pin="FW_12V@19" pad="19"/>
<connect gate="G$1" pin="FW_12V@20" pad="20"/>
<connect gate="G$1" pin="FW_TPA+" pad="24"/>
<connect gate="G$1" pin="FW_TPA-" pad="22"/>
<connect gate="G$1" pin="FW_TPB+" pad="28"/>
<connect gate="G$1" pin="FW_TPB-" pad="26"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@11" pad="11"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@16" pad="16"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@29" pad="29"/>
<connect gate="G$1" pin="GND@30" pad="30"/>
<connect gate="G$1" pin="LEFT_IN" pad="6"/>
<connect gate="G$1" pin="LEFT_OUT" pad="4"/>
<connect gate="G$1" pin="RIGHT_IN" pad="5"/>
<connect gate="G$1" pin="RIGHT_OUT" pad="3"/>
<connect gate="G$1" pin="RX" pad="13"/>
<connect gate="G$1" pin="SCHROME_OUT" pad="9"/>
<connect gate="G$1" pin="SLUM_OUT" pad="10"/>
<connect gate="G$1" pin="TX" pad="12"/>
<connect gate="G$1" pin="USB_5V" pad="23"/>
<connect gate="G$1" pin="USB_D+" pad="27"/>
<connect gate="G$1" pin="USB_D-" pad="25"/>
<connect gate="G$1" pin="VIDEO_OUT" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="KENT_LCD_CONN">
<description>Connector for Kent display (LCD-09560)
&lt;br&gt;
SparkFun no longer uses this connector on any active designs, however 4Ucon still makes this connector as of 7/19/2016.
&lt;br&gt;

http://www.4uconnector.com/online/object/4udrawing/07612.pdf</description>
<gates>
<gate name="G$1" symbol="KENT_LCD_CONN"/>
</gates>
<devices>
<device name="" package="FFC_16">
<connects>
<connect gate="G$1" pin="/RESET" pad="1"/>
<connect gate="G$1" pin="BUSY" pad="2"/>
<connect gate="G$1" pin="CS" pad="7"/>
<connect gate="G$1" pin="NC1" pad="15"/>
<connect gate="G$1" pin="NC2" pad="16"/>
<connect gate="G$1" pin="SCK" pad="4"/>
<connect gate="G$1" pin="SI" pad="6"/>
<connect gate="G$1" pin="SO" pad="5"/>
<connect gate="G$1" pin="VCC" pad="9"/>
<connect gate="G$1" pin="VPWR1" pad="10"/>
<connect gate="G$1" pin="VPWR2" pad="11"/>
<connect gate="G$1" pin="VPWR3" pad="13"/>
<connect gate="G$1" pin="VSS1" pad="3"/>
<connect gate="G$1" pin="VSS2" pad="8"/>
<connect gate="G$1" pin="VSS3" pad="12"/>
<connect gate="G$1" pin="VSS4" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LITTLEBITS_FEMALE" prefix="J">
<description>Female end for LittleBits boards</description>
<gates>
<gate name="G$1" symbol="LITTLEBITS_FEMALE"/>
</gates>
<devices>
<device name="" package="LITTLE_BITS_FEMALE">
<connects>
<connect gate="G$1" pin="GND" pad="V-"/>
<connect gate="G$1" pin="SIG" pad="SIG"/>
<connect gate="G$1" pin="VCC" pad="V+"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LITTLEBITS_MALE">
<description>Male end for LittleBits boards</description>
<gates>
<gate name="G$1" symbol="LITTLEBITS_MALE"/>
</gates>
<devices>
<device name="" package="LITTLE_BITS_MALE">
<connects>
<connect gate="G$1" pin="GND" pad="V-"/>
<connect gate="G$1" pin="SIG" pad="SIG"/>
<connect gate="G$1" pin="VCC" pad="V+"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LITTLE_BITS_CONN">
<description>Connector used in LittleBits</description>
<gates>
<gate name="G$1" symbol="LITTLEBITS"/>
</gates>
<devices>
<device name="" package="LITTLEBITS">
<connects>
<connect gate="G$1" pin="GND" pad="P$3"/>
<connect gate="G$1" pin="SIG" pad="P$4"/>
<connect gate="G$1" pin="VCC" pad="P$5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LCD_CFAX">
<description>Graphic LCD module (LCD-00463) DISCONTINUED</description>
<gates>
<gate name="LCD" symbol="LCD_CFAX"/>
</gates>
<devices>
<device name="" package="LCD_CFAX">
<connects>
<connect gate="LCD" pin="CS1B" pad="P$3"/>
<connect gate="LCD" pin="CS2" pad="P$4"/>
<connect gate="LCD" pin="D0" pad="P$9"/>
<connect gate="LCD" pin="D1" pad="P$10"/>
<connect gate="LCD" pin="D2" pad="P$11"/>
<connect gate="LCD" pin="D3" pad="P$12"/>
<connect gate="LCD" pin="D4" pad="P$13"/>
<connect gate="LCD" pin="D5" pad="P$14"/>
<connect gate="LCD" pin="D6" pad="P$15"/>
<connect gate="LCD" pin="D7" pad="P$16"/>
<connect gate="LCD" pin="ERD" pad="P$8"/>
<connect gate="LCD" pin="GND" pad="P$2"/>
<connect gate="LCD" pin="MI" pad="P$17"/>
<connect gate="LCD" pin="P/S" pad="P$18"/>
<connect gate="LCD" pin="RESET" pad="P$5"/>
<connect gate="LCD" pin="RS" pad="P$6"/>
<connect gate="LCD" pin="RW" pad="P$7"/>
<connect gate="LCD" pin="VCC" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT25FS010">
<description>1-Mbit SPI flash memory
&lt;br&gt;
&lt;br&gt;
Retired: IC-09350</description>
<gates>
<gate name="G$1" symbol="AT25FS010"/>
</gates>
<devices>
<device name="" package="SO08WIDE">
<connects>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="HOLD" pad="7"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="SI" pad="5"/>
<connect gate="G$1" pin="SO" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT45DB041B">
<description>4-Mbit SPI flash memory
&lt;br&gt;&lt;br&gt;
Not in catalog</description>
<gates>
<gate name="G$1" symbol="AT45DB041B"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="CS" pad="4"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="RST" pad="3"/>
<connect gate="G$1" pin="SCK" pad="2"/>
<connect gate="G$1" pin="SI" pad="1"/>
<connect gate="G$1" pin="SO" pad="8"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="WP" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WIDE" package="SO08WIDE">
<connects>
<connect gate="G$1" pin="CS" pad="4"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="RST" pad="3"/>
<connect gate="G$1" pin="SCK" pad="2"/>
<connect gate="G$1" pin="SI" pad="1"/>
<connect gate="G$1" pin="SO" pad="8"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="WP" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT45DB161D">
<description>16-Mbit SPI flash memory
&lt;br&gt;
&lt;br&gt;
Retired IC-08556</description>
<gates>
<gate name="G$1" symbol="AT45DB161D"/>
</gates>
<devices>
<device name="" package="SO08-EIAJ">
<connects>
<connect gate="G$1" pin="CS" pad="4"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="RST" pad="3"/>
<connect gate="G$1" pin="SCK" pad="2"/>
<connect gate="G$1" pin="SI" pad="1"/>
<connect gate="G$1" pin="SO" pad="8"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="WP" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT42QT1010">
<gates>
<gate name="G$1" symbol="AT42QT1010"/>
</gates>
<devices>
<device name="SOT23" package="SOT23-6">
<connects>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="SNS" pad="4"/>
<connect gate="G$1" pin="SNSK" pad="3"/>
<connect gate="G$1" pin="SYNC/MODE" pad="6"/>
<connect gate="G$1" pin="VDD" pad="5"/>
<connect gate="G$1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CP210X_USB_UART" prefix="IC">
<description>&lt;b&gt;Single-Chip USB to UART Bridge&lt;/b&gt;&lt;p&gt;
Source: www.silabs.com .. CP2101.pdf / cp2102.pdf. Spark Fun Electronics SKU : COM-00310
&lt;br&gt;&lt;br&gt;
RETIRED: IC-00865</description>
<gates>
<gate name="G$1" symbol="CP2101"/>
</gates>
<devices>
<device name="" package="MLP28">
<connects>
<connect gate="G$1" pin="!RST" pad="9"/>
<connect gate="G$1" pin="!SUSPEND" pad="11"/>
<connect gate="G$1" pin="CTS" pad="23"/>
<connect gate="G$1" pin="D+" pad="4"/>
<connect gate="G$1" pin="D-" pad="5"/>
<connect gate="G$1" pin="DCD" pad="1"/>
<connect gate="G$1" pin="DSR" pad="27"/>
<connect gate="G$1" pin="DTR" pad="28"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="GND@EXP" pad="EXP"/>
<connect gate="G$1" pin="GND@M" pad="M"/>
<connect gate="G$1" pin="REGIN" pad="7"/>
<connect gate="G$1" pin="RI" pad="2"/>
<connect gate="G$1" pin="RTS" pad="24"/>
<connect gate="G$1" pin="RXD" pad="25"/>
<connect gate="G$1" pin="SUSPEND" pad="12"/>
<connect gate="G$1" pin="TXD" pad="26"/>
<connect gate="G$1" pin="VBUS" pad="8"/>
<connect gate="G$1" pin="VDD" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COM-00310"/>
<attribute name="VALUE" value="CP2101"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CP2103_USB_UART" prefix="IC">
<description>&lt;b&gt;Single-Chip USB to UART Bridge&lt;/b&gt;
Source: www.silabs.com .. CP2103.pdf. Spark Fun Electronics SKU : COM-00309
&lt;br&gt;&lt;br&gt;
Retired: IC-00866</description>
<gates>
<gate name="G$1" symbol="CP2103"/>
</gates>
<devices>
<device name="" package="MLP28">
<connects>
<connect gate="G$1" pin="!RST" pad="9"/>
<connect gate="G$1" pin="!SUSPEND" pad="11"/>
<connect gate="G$1" pin="CTS" pad="22"/>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="4"/>
<connect gate="G$1" pin="DCD" pad="28"/>
<connect gate="G$1" pin="DSR" pad="26"/>
<connect gate="G$1" pin="DTR" pad="27"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND@EXP" pad="EXP"/>
<connect gate="G$1" pin="GND@M" pad="M"/>
<connect gate="G$1" pin="GPIO_0" pad="19"/>
<connect gate="G$1" pin="GPIO_1" pad="18"/>
<connect gate="G$1" pin="GPIO_2" pad="17"/>
<connect gate="G$1" pin="GPIO_3" pad="16"/>
<connect gate="G$1" pin="REGIN" pad="7"/>
<connect gate="G$1" pin="RI" pad="1"/>
<connect gate="G$1" pin="RTS" pad="23"/>
<connect gate="G$1" pin="RXD" pad="24"/>
<connect gate="G$1" pin="SUSPEND" pad="12"/>
<connect gate="G$1" pin="TXD" pad="25"/>
<connect gate="G$1" pin="VBUS" pad="8"/>
<connect gate="G$1" pin="VDD" pad="6"/>
<connect gate="G$1" pin="VIO" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COM-00309"/>
<attribute name="VALUE" value="CP2103"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DOSONCHIP-IC">
<description>&lt;b&gt;DOSonCHIP IC&lt;/b&gt;
This is the tested schematic and footprint for the DOSonCHIP FAT16 FAT32 IC. Spark Fun Electronics SKU : COM-07956. QFN package also tested/proven.</description>
<gates>
<gate name="G$1" symbol="DOSONCHIP-IC"/>
</gates>
<devices>
<device name="LQFP" package="LQFP-32">
<connects>
<connect gate="G$1" pin="CARD_CD" pad="13"/>
<connect gate="G$1" pin="CARD_CS" pad="18"/>
<connect gate="G$1" pin="CARD_DIN" pad="15"/>
<connect gate="G$1" pin="CARD_DOUT" pad="17"/>
<connect gate="G$1" pin="CARD_SCLK" pad="16"/>
<connect gate="G$1" pin="CARD_WP" pad="14"/>
<connect gate="G$1" pin="DIR" pad="22"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="I2C_SCL" pad="25"/>
<connect gate="G$1" pin="I2C_SDA" pad="26"/>
<connect gate="G$1" pin="MODE0" pad="6"/>
<connect gate="G$1" pin="MODE1" pad="21"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="SPI_CS" pad="27"/>
<connect gate="G$1" pin="SPI_MISO" pad="1"/>
<connect gate="G$1" pin="SPI_MOSI" pad="28"/>
<connect gate="G$1" pin="SPI_SCLK" pad="2"/>
<connect gate="G$1" pin="UART_CTS" pad="23"/>
<connect gate="G$1" pin="UART_RTS/BUSY" pad="24"/>
<connect gate="G$1" pin="UART_RX" pad="29"/>
<connect gate="G$1" pin="UART_TX" pad="30"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="XTAL_IN" pad="32"/>
<connect gate="G$1" pin="XTAL_OUT" pad="31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="QFN" package="QFN-24">
<connects>
<connect gate="G$1" pin="CARD_CD" pad="7"/>
<connect gate="G$1" pin="CARD_CS" pad="12"/>
<connect gate="G$1" pin="CARD_DIN" pad="9"/>
<connect gate="G$1" pin="CARD_DOUT" pad="11"/>
<connect gate="G$1" pin="CARD_SCLK" pad="10"/>
<connect gate="G$1" pin="CARD_WP" pad="8"/>
<connect gate="G$1" pin="DIR" pad="14"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="I2C_SCL" pad="17"/>
<connect gate="G$1" pin="I2C_SDA" pad="18"/>
<connect gate="G$1" pin="MODE0" pad="6"/>
<connect gate="G$1" pin="MODE1" pad="13"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="SPI_CS" pad="19"/>
<connect gate="G$1" pin="SPI_MISO" pad="1"/>
<connect gate="G$1" pin="SPI_MOSI" pad="20"/>
<connect gate="G$1" pin="SPI_SCLK" pad="2"/>
<connect gate="G$1" pin="UART_CTS" pad="15"/>
<connect gate="G$1" pin="UART_RTS/BUSY" pad="16"/>
<connect gate="G$1" pin="UART_RX" pad="21"/>
<connect gate="G$1" pin="UART_TX" pad="22"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="XTAL_IN" pad="24"/>
<connect gate="G$1" pin="XTAL_OUT" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="QFN_ALT1" package="QFN-24_ALT1.PAC">
<connects>
<connect gate="G$1" pin="CARD_CD" pad="7"/>
<connect gate="G$1" pin="CARD_CS" pad="12"/>
<connect gate="G$1" pin="CARD_DIN" pad="9"/>
<connect gate="G$1" pin="CARD_DOUT" pad="11"/>
<connect gate="G$1" pin="CARD_SCLK" pad="10"/>
<connect gate="G$1" pin="CARD_WP" pad="8"/>
<connect gate="G$1" pin="DIR" pad="14"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="I2C_SCL" pad="17"/>
<connect gate="G$1" pin="I2C_SDA" pad="18"/>
<connect gate="G$1" pin="MODE0" pad="6"/>
<connect gate="G$1" pin="MODE1" pad="13"/>
<connect gate="G$1" pin="RESET" pad="5"/>
<connect gate="G$1" pin="SPI_CS" pad="19"/>
<connect gate="G$1" pin="SPI_MISO" pad="1"/>
<connect gate="G$1" pin="SPI_MOSI" pad="20"/>
<connect gate="G$1" pin="SPI_SCLK" pad="2"/>
<connect gate="G$1" pin="UART_CTS" pad="15"/>
<connect gate="G$1" pin="UART_RTS/BUSY" pad="16"/>
<connect gate="G$1" pin="UART_RX" pad="21"/>
<connect gate="G$1" pin="UART_TX" pad="22"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="XTAL_IN" pad="24"/>
<connect gate="G$1" pin="XTAL_OUT" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ENC28J60" prefix="U" uservalue="yes">
<description>Microchip SPI 10Base ethernet IC
&lt;br&gt;&lt;br&gt;
Prototype by abe, 2010.  Dead?</description>
<gates>
<gate name="G$1" symbol="ENC28J60"/>
</gates>
<devices>
<device name="" package="SSOP28DB">
<connects>
<connect gate="G$1" pin="/INT" pad="4"/>
<connect gate="G$1" pin="CLKOUT" pad="3"/>
<connect gate="G$1" pin="CS" pad="9"/>
<connect gate="G$1" pin="LEDA" pad="27"/>
<connect gate="G$1" pin="LEDB" pad="26"/>
<connect gate="G$1" pin="NC" pad="5"/>
<connect gate="G$1" pin="OSC1" pad="23"/>
<connect gate="G$1" pin="OSC2" pad="24"/>
<connect gate="G$1" pin="RBIAS" pad="14"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="SCK" pad="8"/>
<connect gate="G$1" pin="SI" pad="7"/>
<connect gate="G$1" pin="SO" pad="6"/>
<connect gate="G$1" pin="TPIN+" pad="13"/>
<connect gate="G$1" pin="TPIN-" pad="12"/>
<connect gate="G$1" pin="TPOUT+" pad="17"/>
<connect gate="G$1" pin="TPOUT-" pad="16"/>
<connect gate="G$1" pin="VCAP" pad="1"/>
<connect gate="G$1" pin="VDD" pad="28"/>
<connect gate="G$1" pin="VDDOSC" pad="25"/>
<connect gate="G$1" pin="VDDPLL" pad="20"/>
<connect gate="G$1" pin="VDDRX" pad="19"/>
<connect gate="G$1" pin="VDDTX" pad="15"/>
<connect gate="G$1" pin="VSS" pad="2"/>
<connect gate="G$1" pin="VSSOSC" pad="22"/>
<connect gate="G$1" pin="VSSPLL" pad="21"/>
<connect gate="G$1" pin="VSSRX" pad="11"/>
<connect gate="G$1" pin="VSSTX" pad="18"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09541"/>
<attribute name="VALUE" value="ENC28J60"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT245RL">
<description>&lt;b&gt;USB FIFO Controller&lt;/b&gt;
4&lt;sup&gt;th&lt;/sup&gt; Generation USB Controller (USB &amp;lt;-&amp;gt; Parallel) - FIFO. Spark Fun Electronics SKU : COM-00787


&lt;br&gt;&lt;br&gt;&lt;b&gt;TODO:&lt;/b&gt; Move this to retired</description>
<gates>
<gate name="G$1" symbol="FT245R"/>
</gates>
<devices>
<device name="" package="SSOP28DB">
<connects>
<connect gate="G$1" pin="3V3OUT" pad="17"/>
<connect gate="G$1" pin="AGND" pad="25"/>
<connect gate="G$1" pin="D0" pad="1"/>
<connect gate="G$1" pin="D1" pad="5"/>
<connect gate="G$1" pin="D2" pad="3"/>
<connect gate="G$1" pin="D3" pad="11"/>
<connect gate="G$1" pin="D4" pad="2"/>
<connect gate="G$1" pin="D5" pad="9"/>
<connect gate="G$1" pin="D6" pad="10"/>
<connect gate="G$1" pin="D7" pad="6"/>
<connect gate="G$1" pin="GND1" pad="7"/>
<connect gate="G$1" pin="GND2" pad="18"/>
<connect gate="G$1" pin="GND3" pad="21"/>
<connect gate="G$1" pin="OSCI" pad="27"/>
<connect gate="G$1" pin="OSCO" pad="28"/>
<connect gate="G$1" pin="PWEN" pad="12"/>
<connect gate="G$1" pin="RD" pad="13"/>
<connect gate="G$1" pin="RESET" pad="19"/>
<connect gate="G$1" pin="RXF" pad="23"/>
<connect gate="G$1" pin="TEST" pad="26"/>
<connect gate="G$1" pin="TXE" pad="22"/>
<connect gate="G$1" pin="USBDM" pad="16"/>
<connect gate="G$1" pin="USBDP" pad="15"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="VCCIO" pad="4"/>
<connect gate="G$1" pin="WR" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COM-00787"/>
<attribute name="VALUE" value="FT245RL"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT2232D">
<description>USB to USART/FIFO/JTAG/SPI/I2C</description>
<gates>
<gate name="G$1" symbol="FT2232D"/>
</gates>
<devices>
<device name="" package="LQFP-48">
<connects>
<connect gate="G$1" pin="3V3OUT" pad="6"/>
<connect gate="G$1" pin="ACBUS0" pad="15"/>
<connect gate="G$1" pin="ACBUS1" pad="13"/>
<connect gate="G$1" pin="ACBUS2" pad="12"/>
<connect gate="G$1" pin="ACBUS3" pad="11"/>
<connect gate="G$1" pin="ADBUS0" pad="24"/>
<connect gate="G$1" pin="ADBUS1" pad="23"/>
<connect gate="G$1" pin="ADBUS2" pad="22"/>
<connect gate="G$1" pin="ADBUS3" pad="21"/>
<connect gate="G$1" pin="ADBUS4" pad="20"/>
<connect gate="G$1" pin="ADBUS5" pad="19"/>
<connect gate="G$1" pin="ADBUS6" pad="17"/>
<connect gate="G$1" pin="ADBUS7" pad="16"/>
<connect gate="G$1" pin="AGND" pad="45"/>
<connect gate="G$1" pin="AVCC" pad="46"/>
<connect gate="G$1" pin="BCBUS0" pad="30"/>
<connect gate="G$1" pin="BCBUS1" pad="29"/>
<connect gate="G$1" pin="BCBUS2" pad="28"/>
<connect gate="G$1" pin="BCBUS3" pad="27"/>
<connect gate="G$1" pin="BDBUS0" pad="40"/>
<connect gate="G$1" pin="BDBUS1" pad="39"/>
<connect gate="G$1" pin="BDBUS2" pad="38"/>
<connect gate="G$1" pin="BDBUS3" pad="37"/>
<connect gate="G$1" pin="BDBUS4" pad="36"/>
<connect gate="G$1" pin="BDBUS5" pad="35"/>
<connect gate="G$1" pin="BDBUS6" pad="33"/>
<connect gate="G$1" pin="BDBUS7" pad="32"/>
<connect gate="G$1" pin="EECS" pad="48"/>
<connect gate="G$1" pin="EEDATA" pad="2"/>
<connect gate="G$1" pin="EESK" pad="1"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="25"/>
<connect gate="G$1" pin="GND3" pad="34"/>
<connect gate="G$1" pin="GND4" pad="9"/>
<connect gate="G$1" pin="PWEN#" pad="41"/>
<connect gate="G$1" pin="RESET#" pad="4"/>
<connect gate="G$1" pin="RSTOUT#" pad="5"/>
<connect gate="G$1" pin="SI/WUA" pad="10"/>
<connect gate="G$1" pin="SI/WUB" pad="26"/>
<connect gate="G$1" pin="TEST" pad="47"/>
<connect gate="G$1" pin="USBDM" pad="8"/>
<connect gate="G$1" pin="USBDP" pad="7"/>
<connect gate="G$1" pin="VCC1" pad="3"/>
<connect gate="G$1" pin="VCC2" pad="42"/>
<connect gate="G$1" pin="VCCIOA" pad="14"/>
<connect gate="G$1" pin="VCCIOB" pad="31"/>
<connect gate="G$1" pin="XTIN" pad="43"/>
<connect gate="G$1" pin="XTOUT" pad="44"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ISD1900" prefix="U">
<description>Voice recorder IC
&lt;br&gt;
&lt;br&gt;
Retired IC -- Limited supply available</description>
<gates>
<gate name="G$1" symbol="ISD1932"/>
</gates>
<devices>
<device name="ISD1932" package="SO-28W">
<connects>
<connect gate="G$1" pin="ADDR/_DRCT" pad="27"/>
<connect gate="G$1" pin="AGC" pad="17"/>
<connect gate="G$1" pin="E0/_M5" pad="7"/>
<connect gate="G$1" pin="E1/_M6" pad="9"/>
<connect gate="G$1" pin="E2/_M7" pad="10"/>
<connect gate="G$1" pin="E3/_M8" pad="11"/>
<connect gate="G$1" pin="MIC+" pad="18"/>
<connect gate="G$1" pin="MIC-" pad="19"/>
<connect gate="G$1" pin="ROSC" pad="20"/>
<connect gate="G$1" pin="S0/_M1" pad="2"/>
<connect gate="G$1" pin="S1/_M2" pad="3"/>
<connect gate="G$1" pin="S2/_M3" pad="4"/>
<connect gate="G$1" pin="S3/_M4" pad="5"/>
<connect gate="G$1" pin="SP+" pad="15"/>
<connect gate="G$1" pin="SP-" pad="13"/>
<connect gate="G$1" pin="VCCA" pad="21"/>
<connect gate="G$1" pin="VCCD" pad="28"/>
<connect gate="G$1" pin="VCCP" pad="14"/>
<connect gate="G$1" pin="VSSA" pad="8"/>
<connect gate="G$1" pin="VSSD" pad="1"/>
<connect gate="G$1" pin="VSSP1" pad="16"/>
<connect gate="G$1" pin="VSSP2" pad="12"/>
<connect gate="G$1" pin="XCLK/FMC3" pad="25"/>
<connect gate="G$1" pin="_FT" pad="26"/>
<connect gate="G$1" pin="_LED" pad="22"/>
<connect gate="G$1" pin="_PLAYE/FMC2" pad="23"/>
<connect gate="G$1" pin="_PLAYL/FMC1" pad="6"/>
<connect gate="G$1" pin="_REC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M93C46">
<description>&lt;h3&gt;&lt;/h3&gt;
&lt;p&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=""&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href=""&gt;&lt;/a&gt; ()&lt;/li&gt;
&lt;li&gt;&lt;a href=""&gt;&lt;/a&gt; ()&lt;/li&gt;
&lt;/ul&gt;


1kbit SPI EEPROM
&lt;br&gt;&lt;br&gt;
IC-09397 -- Dead prototype</description>
<gates>
<gate name="G$1" symbol="M93C46"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DIN" pad="3"/>
<connect gate="G$1" pin="DOUT" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="SK" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX323" prefix="U">
<description>RETIRED

Dual low-voltage SPST analog switch&lt;br&gt;
&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="MAX323"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="COM1" pad="2"/>
<connect gate="G$1" pin="COM2" pad="6"/>
<connect gate="G$1" pin="IN1" pad="7"/>
<connect gate="G$1" pin="IN2" pad="3"/>
<connect gate="G$1" pin="NO1" pad="1"/>
<connect gate="G$1" pin="NO2" pad="5"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-08171"/>
<attribute name="VALUE" value="MAX323"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX485">
<description>RS-485 transceiver</description>
<gates>
<gate name="G$1" symbol="MAX485"/>
</gates>
<devices>
<device name="DIL" package="DIL08">
<connects>
<connect gate="G$1" pin="A" pad="6"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="DE" pad="3"/>
<connect gate="G$1" pin="DI" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="RE" pad="2"/>
<connect gate="G$1" pin="RO" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX7219">
<description>8-digit, 8-segment LED display driver, serial input</description>
<gates>
<gate name="G$1" symbol="MAX7219"/>
</gates>
<devices>
<device name="DIP" package="DIL24">
<connects>
<connect gate="G$1" pin="CLK" pad="13"/>
<connect gate="G$1" pin="DIG0" pad="2"/>
<connect gate="G$1" pin="DIG1" pad="11"/>
<connect gate="G$1" pin="DIG2" pad="6"/>
<connect gate="G$1" pin="DIG3" pad="7"/>
<connect gate="G$1" pin="DIG4" pad="3"/>
<connect gate="G$1" pin="DIG5" pad="10"/>
<connect gate="G$1" pin="DIG6" pad="5"/>
<connect gate="G$1" pin="DIG7" pad="8"/>
<connect gate="G$1" pin="DIN" pad="1"/>
<connect gate="G$1" pin="DOUT" pad="24"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND2" pad="9"/>
<connect gate="G$1" pin="ISET" pad="18"/>
<connect gate="G$1" pin="LOAD" pad="12"/>
<connect gate="G$1" pin="SEGA" pad="14"/>
<connect gate="G$1" pin="SEGB" pad="16"/>
<connect gate="G$1" pin="SEGC" pad="20"/>
<connect gate="G$1" pin="SEGD" pad="23"/>
<connect gate="G$1" pin="SEGDP" pad="22"/>
<connect gate="G$1" pin="SEGE" pad="21"/>
<connect gate="G$1" pin="SEGF" pad="15"/>
<connect gate="G$1" pin="SEGG" pad="17"/>
<connect gate="G$1" pin="VCC" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX7456">
<description>Monochrome NTSC/PAL on-screen display generator (SPI)</description>
<gates>
<gate name="G$1" symbol="MAX7456"/>
</gates>
<devices>
<device name="" package="TSSOP28">
<connects>
<connect gate="G$1" pin="AGND" pad="20"/>
<connect gate="G$1" pin="AVDD" pad="21"/>
<connect gate="G$1" pin="CLKIN" pad="5"/>
<connect gate="G$1" pin="CLKOUT" pad="7"/>
<connect gate="G$1" pin="DGND" pad="4"/>
<connect gate="G$1" pin="DIN" pad="9"/>
<connect gate="G$1" pin="DOUT" pad="11"/>
<connect gate="G$1" pin="DVDD" pad="3"/>
<connect gate="G$1" pin="LOS" pad="12"/>
<connect gate="G$1" pin="PGND" pad="23"/>
<connect gate="G$1" pin="PVDD" pad="24"/>
<connect gate="G$1" pin="SAG" pad="25"/>
<connect gate="G$1" pin="SCK" pad="10"/>
<connect gate="G$1" pin="VIN" pad="22"/>
<connect gate="G$1" pin="VOUT" pad="26"/>
<connect gate="G$1" pin="XFB" pad="6"/>
<connect gate="G$1" pin="~CS" pad="8"/>
<connect gate="G$1" pin="~HSYNC" pad="18"/>
<connect gate="G$1" pin="~RESET" pad="19"/>
<connect gate="G$1" pin="~VSYNC" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GROUNDPAD" package="TSSOP28-GROUNDPAD">
<connects>
<connect gate="G$1" pin="AGND" pad="20"/>
<connect gate="G$1" pin="AVDD" pad="21"/>
<connect gate="G$1" pin="CLKIN" pad="5"/>
<connect gate="G$1" pin="CLKOUT" pad="7"/>
<connect gate="G$1" pin="DGND" pad="4"/>
<connect gate="G$1" pin="DIN" pad="9"/>
<connect gate="G$1" pin="DOUT" pad="11"/>
<connect gate="G$1" pin="DVDD" pad="3"/>
<connect gate="G$1" pin="LOS" pad="12"/>
<connect gate="G$1" pin="PGND" pad="23"/>
<connect gate="G$1" pin="PVDD" pad="24"/>
<connect gate="G$1" pin="SAG" pad="25"/>
<connect gate="G$1" pin="SCK" pad="10"/>
<connect gate="G$1" pin="VIN" pad="22"/>
<connect gate="G$1" pin="VOUT" pad="26"/>
<connect gate="G$1" pin="XFB" pad="6"/>
<connect gate="G$1" pin="~CS" pad="8"/>
<connect gate="G$1" pin="~HSYNC" pad="18"/>
<connect gate="G$1" pin="~RESET" pad="19"/>
<connect gate="G$1" pin="~VSYNC" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP130" prefix="U">
<description>Open-drain microcontroller supervisor chip</description>
<gates>
<gate name="G$1" symbol="MCP130"/>
</gates>
<devices>
<device name="SOT" package="SOT23-3">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NAND256">
<description>NAND flash
&lt;br&gt;&lt;br&gt;
Not in catalog</description>
<gates>
<gate name="G$1" symbol="NAND256"/>
</gates>
<devices>
<device name="" package="TSOP48">
<connects>
<connect gate="G$1" pin="AL" pad="17"/>
<connect gate="G$1" pin="CL" pad="16"/>
<connect gate="G$1" pin="IO0" pad="29"/>
<connect gate="G$1" pin="IO1" pad="30"/>
<connect gate="G$1" pin="IO2" pad="31"/>
<connect gate="G$1" pin="IO3" pad="32"/>
<connect gate="G$1" pin="IO4" pad="41"/>
<connect gate="G$1" pin="IO5" pad="42"/>
<connect gate="G$1" pin="IO6" pad="43"/>
<connect gate="G$1" pin="IO7" pad="44"/>
<connect gate="G$1" pin="RXB" pad="7"/>
<connect gate="G$1" pin="VDD1" pad="12"/>
<connect gate="G$1" pin="VDD2" pad="37"/>
<connect gate="G$1" pin="VSS1" pad="13"/>
<connect gate="G$1" pin="VSS2" pad="36"/>
<connect gate="G$1" pin="XE" pad="9"/>
<connect gate="G$1" pin="XR" pad="8"/>
<connect gate="G$1" pin="XW" pad="18"/>
<connect gate="G$1" pin="XWP" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NC7WZ07">
<description>Ultra-high speed dual open-drain output buffer (non-inverting)
&lt;br&gt;&lt;br&gt;
Retired: IC-09351</description>
<gates>
<gate name="G$1" symbol="BUFFER-DUAL"/>
</gates>
<devices>
<device name="" package="SC70-6">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="Y1" pad="6"/>
<connect gate="G$1" pin="Y2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP303LSN09">
<description>Power-on uC reset controller</description>
<gates>
<gate name="G$1" symbol="NCP303LSN09"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="CD" pad="5"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="NC" pad="4"/>
<connect gate="G$1" pin="RST" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PL-2303XA">
<description>Prolific USB chip, requires 12MHz xtal

Never stocked</description>
<gates>
<gate name="G$1" symbol="PL-2303XA"/>
</gates>
<devices>
<device name="" package="SSOP28DB">
<connects>
<connect gate="G$1" pin="CTS_N" pad="11"/>
<connect gate="G$1" pin="DCD_N" pad="10"/>
<connect gate="G$1" pin="DM" pad="16"/>
<connect gate="G$1" pin="DP" pad="15"/>
<connect gate="G$1" pin="DSR_N" pad="9"/>
<connect gate="G$1" pin="DTR_N" pad="2"/>
<connect gate="G$1" pin="EE_CLK" pad="13"/>
<connect gate="G$1" pin="EE_DATA" pad="14"/>
<connect gate="G$1" pin="GND@18" pad="18"/>
<connect gate="G$1" pin="GND@21" pad="21"/>
<connect gate="G$1" pin="GND@7" pad="7"/>
<connect gate="G$1" pin="GND_A" pad="25"/>
<connect gate="G$1" pin="GP0" pad="22"/>
<connect gate="G$1" pin="GP1" pad="23"/>
<connect gate="G$1" pin="OSC1" pad="27"/>
<connect gate="G$1" pin="OSC2" pad="28"/>
<connect gate="G$1" pin="PLL_TEST" pad="26"/>
<connect gate="G$1" pin="RESET_N" pad="19"/>
<connect gate="G$1" pin="RI_N" pad="6"/>
<connect gate="G$1" pin="RTS_N" pad="3"/>
<connect gate="G$1" pin="RXD" pad="5"/>
<connect gate="G$1" pin="SHTD_N" pad="12"/>
<connect gate="G$1" pin="TXD" pad="1"/>
<connect gate="G$1" pin="VDD_325" pad="4"/>
<connect gate="G$1" pin="VDD_33" pad="8"/>
<connect gate="G$1" pin="VDD_33A" pad="24"/>
<connect gate="G$1" pin="VDD_5" pad="20"/>
<connect gate="G$1" pin="VO_33" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SC16IS750" prefix="IC">
<description>SPI/I2C/IrDA to UART</description>
<gates>
<gate name="G$1" symbol="SC16IS750"/>
</gates>
<devices>
<device name="" package="QFN-24">
<connects>
<connect gate="G$1" pin="/CTS" pad="22"/>
<connect gate="G$1" pin="/IRQ" pad="11"/>
<connect gate="G$1" pin="/RTS" pad="21"/>
<connect gate="G$1" pin="A0-/CS" pad="6"/>
<connect gate="G$1" pin="A1-SI" pad="7"/>
<connect gate="G$1" pin="GPIO0" pad="12"/>
<connect gate="G$1" pin="GPIO1" pad="13"/>
<connect gate="G$1" pin="GPIO2" pad="14"/>
<connect gate="G$1" pin="GPIO3" pad="15"/>
<connect gate="G$1" pin="GPIO4-/DSR" pad="17"/>
<connect gate="G$1" pin="GPIO5-/DTR" pad="18"/>
<connect gate="G$1" pin="GPIO6-/CD" pad="19"/>
<connect gate="G$1" pin="GPIO7-/RI" pad="20"/>
<connect gate="G$1" pin="I2C-/SPI" pad="5"/>
<connect gate="G$1" pin="NC-SO" pad="8"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="RX" pad="24"/>
<connect gate="G$1" pin="SCL-SCLK" pad="9"/>
<connect gate="G$1" pin="SDA-VSS" pad="10"/>
<connect gate="G$1" pin="TX" pad="23"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS" pad="16"/>
<connect gate="G$1" pin="XTAL1" pad="2"/>
<connect gate="G$1" pin="XTAL2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SLB9645">
<gates>
<gate name="G$1" symbol="SLB9645"/>
</gates>
<devices>
<device name="" package="TSSOP28">
<connects>
<connect gate="G$1" pin="!DAVINT#" pad="6"/>
<connect gate="G$1" pin="!RESET#" pad="9"/>
<connect gate="G$1" pin="GND@11" pad="11"/>
<connect gate="G$1" pin="GND@18" pad="18"/>
<connect gate="G$1" pin="GND@25" pad="25"/>
<connect gate="G$1" pin="GND@4" pad="4"/>
<connect gate="G$1" pin="PP" pad="7"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SDA" pad="1"/>
<connect gate="G$1" pin="VDD@10" pad="10"/>
<connect gate="G$1" pin="VDD@5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-XXXX"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STM811" prefix="U">
<description>&lt;h3&gt;STM811 Reset Circuit&lt;/h3&gt;
Used in the Ethernet Shield</description>
<gates>
<gate name="G$1" symbol="STM811"/>
</gates>
<devices>
<device name="" package="SOT143">
<connects>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="VSS" pad="1"/>
<connect gate="G$1" pin="~MR" pad="3"/>
<connect gate="G$1" pin="~RST" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STW5093">
<description>STW5093 - PCM Audio Codec
&lt;br&gt;
&lt;br&gt;
Never was a sparkfun component -- Stock available</description>
<gates>
<gate name="G$1" symbol="STW5093"/>
</gates>
<devices>
<device name="" package="TSSOP30">
<connects>
<connect gate="G$1" pin="AUXCLK" pad="P$23"/>
<connect gate="G$1" pin="BZ" pad="P$19"/>
<connect gate="G$1" pin="CCLK" pad="P$20"/>
<connect gate="G$1" pin="CI" pad="P$22"/>
<connect gate="G$1" pin="CO" pad="P$25"/>
<connect gate="G$1" pin="CS-" pad="P$21"/>
<connect gate="G$1" pin="DR" pad="P$28"/>
<connect gate="G$1" pin="DX" pad="P$27"/>
<connect gate="G$1" pin="FS" pad="P$29"/>
<connect gate="G$1" pin="GND" pad="P$26"/>
<connect gate="G$1" pin="GNDA" pad="P$10"/>
<connect gate="G$1" pin="GNDP" pad="P$16"/>
<connect gate="G$1" pin="LO" pad="P$18"/>
<connect gate="G$1" pin="MBIAS" pad="P$6"/>
<connect gate="G$1" pin="MCLK" pad="P$30"/>
<connect gate="G$1" pin="MIC1+" pad="P$8"/>
<connect gate="G$1" pin="MIC1-" pad="P$9"/>
<connect gate="G$1" pin="MIC2+" pad="P$11"/>
<connect gate="G$1" pin="MIC2-" pad="P$12"/>
<connect gate="G$1" pin="MIC3+" pad="P$4"/>
<connect gate="G$1" pin="MIC3-" pad="P$5"/>
<connect gate="G$1" pin="REMIN" pad="P$3"/>
<connect gate="G$1" pin="REMOUT" pad="P$2"/>
<connect gate="G$1" pin="VCC" pad="P$1"/>
<connect gate="G$1" pin="VCCA" pad="P$7"/>
<connect gate="G$1" pin="VCCIO" pad="P$24"/>
<connect gate="G$1" pin="VCCP" pad="P$13"/>
<connect gate="G$1" pin="VFR" pad="P$17"/>
<connect gate="G$1" pin="VLR+" pad="P$15"/>
<connect gate="G$1" pin="VLR-" pad="P$14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TJA1040">
<description>CAN Tranceiver

Retired</description>
<gates>
<gate name="G$1" symbol="TJA1040TD-T"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="CANH" pad="7"/>
<connect gate="G$1" pin="CANL" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="RXD" pad="4"/>
<connect gate="G$1" pin="SPLIT" pad="5"/>
<connect gate="G$1" pin="STB" pad="8"/>
<connect gate="G$1" pin="TXD" pad="1"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLC5940" prefix="U">
<description>16-channel LED Driver with Dot Correction and Grayscale PWM Control
&lt;hr&gt;
&lt;p&gt;The TLC5940 is a 16-channel, constant-current sink LED driver. Each channel has an individually adjustable 4096-step grayscale PWM brightness control and a 64-step, constant-current sink (dot correction). The dot correction adjusts the brightness variations between LED channels and other LED drivers. The dot correction data is stored in an integrated EEPROM. Both grayscale control and dot correction are accessible via a serial interface. A single external resistor sets the maximum current value of all 16 channels.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Packages:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;28-pin HTSSOP
&lt;li&gt;32-pin 5x5mm QFN
&lt;li&gt;28-pin DIP&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TLC5940"/>
</gates>
<devices>
<device name="-NT" package="DIL28-3">
<connects>
<connect gate="G$1" pin="BLANK" pad="23"/>
<connect gate="G$1" pin="DCPRG" pad="19"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GSCLK" pad="18"/>
<connect gate="G$1" pin="IREF" pad="20"/>
<connect gate="G$1" pin="OUT0" pad="28"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT10" pad="10"/>
<connect gate="G$1" pin="OUT11" pad="11"/>
<connect gate="G$1" pin="OUT12" pad="12"/>
<connect gate="G$1" pin="OUT13" pad="13"/>
<connect gate="G$1" pin="OUT14" pad="14"/>
<connect gate="G$1" pin="OUT15" pad="15"/>
<connect gate="G$1" pin="OUT2" pad="2"/>
<connect gate="G$1" pin="OUT3" pad="3"/>
<connect gate="G$1" pin="OUT4" pad="4"/>
<connect gate="G$1" pin="OUT5" pad="5"/>
<connect gate="G$1" pin="OUT6" pad="6"/>
<connect gate="G$1" pin="OUT7" pad="7"/>
<connect gate="G$1" pin="OUT8" pad="8"/>
<connect gate="G$1" pin="OUT9" pad="9"/>
<connect gate="G$1" pin="SCLK" pad="25"/>
<connect gate="G$1" pin="SIN" pad="26"/>
<connect gate="G$1" pin="SOUT" pad="17"/>
<connect gate="G$1" pin="VCC" pad="21"/>
<connect gate="G$1" pin="VPRG" pad="27"/>
<connect gate="G$1" pin="XERR" pad="16"/>
<connect gate="G$1" pin="XLAT" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-RHB" package="QFN-32">
<connects>
<connect gate="G$1" pin="BLANK" pad="31"/>
<connect gate="G$1" pin="DCPRG" pad="25"/>
<connect gate="G$1" pin="GND" pad="30"/>
<connect gate="G$1" pin="GSCLK" pad="24"/>
<connect gate="G$1" pin="IREF" pad="26"/>
<connect gate="G$1" pin="OUT0" pad="4"/>
<connect gate="G$1" pin="OUT1" pad="5"/>
<connect gate="G$1" pin="OUT10" pad="16"/>
<connect gate="G$1" pin="OUT11" pad="17"/>
<connect gate="G$1" pin="OUT12" pad="18"/>
<connect gate="G$1" pin="OUT13" pad="19"/>
<connect gate="G$1" pin="OUT14" pad="20"/>
<connect gate="G$1" pin="OUT15" pad="21"/>
<connect gate="G$1" pin="OUT2" pad="6"/>
<connect gate="G$1" pin="OUT3" pad="7"/>
<connect gate="G$1" pin="OUT4" pad="8"/>
<connect gate="G$1" pin="OUT5" pad="9"/>
<connect gate="G$1" pin="OUT6" pad="10"/>
<connect gate="G$1" pin="OUT7" pad="11"/>
<connect gate="G$1" pin="OUT8" pad="14"/>
<connect gate="G$1" pin="OUT9" pad="15"/>
<connect gate="G$1" pin="SCLK" pad="1"/>
<connect gate="G$1" pin="SIN" pad="2"/>
<connect gate="G$1" pin="SOUT" pad="23"/>
<connect gate="G$1" pin="VCC" pad="27"/>
<connect gate="G$1" pin="VPRG" pad="3"/>
<connect gate="G$1" pin="XERR" pad="22"/>
<connect gate="G$1" pin="XLAT" pad="32"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-10398"/>
</technology>
</technologies>
</device>
<device name="PWP" package="TSSOP28-GROUNDPAD">
<connects>
<connect gate="G$1" pin="BLANK" pad="2"/>
<connect gate="G$1" pin="DCPRG" pad="26"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GSCLK" pad="25"/>
<connect gate="G$1" pin="IREF" pad="27"/>
<connect gate="G$1" pin="OUT0" pad="7"/>
<connect gate="G$1" pin="OUT1" pad="8"/>
<connect gate="G$1" pin="OUT10" pad="17"/>
<connect gate="G$1" pin="OUT11" pad="18"/>
<connect gate="G$1" pin="OUT12" pad="19"/>
<connect gate="G$1" pin="OUT13" pad="20"/>
<connect gate="G$1" pin="OUT14" pad="21"/>
<connect gate="G$1" pin="OUT15" pad="22"/>
<connect gate="G$1" pin="OUT2" pad="9"/>
<connect gate="G$1" pin="OUT3" pad="10"/>
<connect gate="G$1" pin="OUT4" pad="11"/>
<connect gate="G$1" pin="OUT5" pad="12"/>
<connect gate="G$1" pin="OUT6" pad="13"/>
<connect gate="G$1" pin="OUT7" pad="14"/>
<connect gate="G$1" pin="OUT8" pad="15"/>
<connect gate="G$1" pin="OUT9" pad="16"/>
<connect gate="G$1" pin="SCLK" pad="4"/>
<connect gate="G$1" pin="SIN" pad="5"/>
<connect gate="G$1" pin="SOUT" pad="24"/>
<connect gate="G$1" pin="VCC" pad="28"/>
<connect gate="G$1" pin="VPRG" pad="6"/>
<connect gate="G$1" pin="XERR" pad="23"/>
<connect gate="G$1" pin="XLAT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB3318">
<description>Hi-speed USB transceiver
&lt;br&gt;&lt;br&gt;
Retired</description>
<gates>
<gate name="G$1" symbol="USB3318"/>
</gates>
<devices>
<device name="" package="QFN-24-USB">
<connects>
<connect gate="G$1" pin="CLKOUT" pad="12"/>
<connect gate="G$1" pin="CPEN" pad="7"/>
<connect gate="G$1" pin="DATA0" pad="16"/>
<connect gate="G$1" pin="DATA1" pad="15"/>
<connect gate="G$1" pin="DATA2" pad="14"/>
<connect gate="G$1" pin="DATA3" pad="13"/>
<connect gate="G$1" pin="DATA4" pad="11"/>
<connect gate="G$1" pin="DATA5" pad="10"/>
<connect gate="G$1" pin="DATA6" pad="9"/>
<connect gate="G$1" pin="DATA7" pad="8"/>
<connect gate="G$1" pin="DIR" pad="19"/>
<connect gate="G$1" pin="DM" pad="5"/>
<connect gate="G$1" pin="DP" pad="6"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="ID" pad="1"/>
<connect gate="G$1" pin="NXT" pad="18"/>
<connect gate="G$1" pin="RBIAS" pad="24"/>
<connect gate="G$1" pin="REFCLK" pad="23"/>
<connect gate="G$1" pin="RESETB" pad="22"/>
<connect gate="G$1" pin="STP" pad="20"/>
<connect gate="G$1" pin="VBAT" pad="3"/>
<connect gate="G$1" pin="VBUS" pad="2"/>
<connect gate="G$1" pin="VDD18" pad="21"/>
<connect gate="G$1" pin="VDD33" pad="4"/>
<connect gate="G$1" pin="VDDIO" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VS1002">
<description>MP3 deecoder
&lt;br&gt;
&lt;br&gt;
Retired IC-08217</description>
<gates>
<gate name="G$1" symbol="VS1002"/>
</gates>
<devices>
<device name="" package="LQFP-48">
<connects>
<connect gate="G$1" pin="AGND1" pad="37"/>
<connect gate="G$1" pin="AGND2" pad="40"/>
<connect gate="G$1" pin="AGND3" pad="41"/>
<connect gate="G$1" pin="AGND4" pad="47"/>
<connect gate="G$1" pin="AVDD1" pad="38"/>
<connect gate="G$1" pin="AVDD2" pad="43"/>
<connect gate="G$1" pin="AVDD3" pad="45"/>
<connect gate="G$1" pin="DGND1" pad="4"/>
<connect gate="G$1" pin="DGND2" pad="16"/>
<connect gate="G$1" pin="DGND3" pad="20"/>
<connect gate="G$1" pin="DGND4" pad="21"/>
<connect gate="G$1" pin="DGND5" pad="22"/>
<connect gate="G$1" pin="DVDD1" pad="6"/>
<connect gate="G$1" pin="DVDD2" pad="14"/>
<connect gate="G$1" pin="DVDD3" pad="19"/>
<connect gate="G$1" pin="D_REQ" pad="8"/>
<connect gate="G$1" pin="GBUF" pad="42"/>
<connect gate="G$1" pin="GPIO1" pad="34"/>
<connect gate="G$1" pin="GPIO2/DCLK" pad="9"/>
<connect gate="G$1" pin="GPIO3/SDATA" pad="10"/>
<connect gate="G$1" pin="LEFT" pad="46"/>
<connect gate="G$1" pin="MICN" pad="2"/>
<connect gate="G$1" pin="MICP" pad="1"/>
<connect gate="G$1" pin="RCAP" pad="44"/>
<connect gate="G$1" pin="RIGHT" pad="39"/>
<connect gate="G$1" pin="RX" pad="26"/>
<connect gate="G$1" pin="SCLK" pad="28"/>
<connect gate="G$1" pin="SI" pad="29"/>
<connect gate="G$1" pin="SO" pad="30"/>
<connect gate="G$1" pin="SPIBOOT/GPIO0" pad="33"/>
<connect gate="G$1" pin="TEST" pad="32"/>
<connect gate="G$1" pin="TX" pad="27"/>
<connect gate="G$1" pin="XCS" pad="23"/>
<connect gate="G$1" pin="XDCS/BSYNC" pad="13"/>
<connect gate="G$1" pin="XRESET" pad="3"/>
<connect gate="G$1" pin="XTAL0" pad="17"/>
<connect gate="G$1" pin="XTAL1" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VS1103">
<description>MIDI/ADPCM/WAV codec, MIDI synth
&lt;br&gt;
&lt;br&gt;
Retired -- Stock still available but looks EOL</description>
<gates>
<gate name="G$1" symbol="VS1103"/>
</gates>
<devices>
<device name="" package="LQFP-48">
<connects>
<connect gate="G$1" pin="AGND1" pad="37"/>
<connect gate="G$1" pin="AGND2" pad="40"/>
<connect gate="G$1" pin="AGND3" pad="41"/>
<connect gate="G$1" pin="AGND4" pad="47"/>
<connect gate="G$1" pin="AVDD1" pad="38"/>
<connect gate="G$1" pin="AVDD2" pad="43"/>
<connect gate="G$1" pin="AVDD3" pad="45"/>
<connect gate="G$1" pin="CVDD1" pad="5"/>
<connect gate="G$1" pin="CVDD2" pad="7"/>
<connect gate="G$1" pin="CVDD3" pad="24"/>
<connect gate="G$1" pin="CVDD4" pad="31"/>
<connect gate="G$1" pin="DGND1" pad="4"/>
<connect gate="G$1" pin="DGND2" pad="16"/>
<connect gate="G$1" pin="DGND3" pad="20"/>
<connect gate="G$1" pin="DGND4" pad="21"/>
<connect gate="G$1" pin="DGND5" pad="22"/>
<connect gate="G$1" pin="DVDD1" pad="6"/>
<connect gate="G$1" pin="DVDD2" pad="14"/>
<connect gate="G$1" pin="DVDD3" pad="19"/>
<connect gate="G$1" pin="D_REQ" pad="8"/>
<connect gate="G$1" pin="GBUF" pad="42"/>
<connect gate="G$1" pin="GPIO1" pad="34"/>
<connect gate="G$1" pin="GPIO2/DCLK" pad="9"/>
<connect gate="G$1" pin="GPIO3/SDATA" pad="10"/>
<connect gate="G$1" pin="LEFT" pad="46"/>
<connect gate="G$1" pin="MICN" pad="2"/>
<connect gate="G$1" pin="MICP" pad="1"/>
<connect gate="G$1" pin="RCAP" pad="44"/>
<connect gate="G$1" pin="RIGHT" pad="39"/>
<connect gate="G$1" pin="RX" pad="26"/>
<connect gate="G$1" pin="SCLK" pad="28"/>
<connect gate="G$1" pin="SI" pad="29"/>
<connect gate="G$1" pin="SO" pad="30"/>
<connect gate="G$1" pin="SPIBOOT/GPIO0" pad="33"/>
<connect gate="G$1" pin="TEST" pad="32"/>
<connect gate="G$1" pin="TX" pad="27"/>
<connect gate="G$1" pin="XCS" pad="23"/>
<connect gate="G$1" pin="XDCS/BSYNC" pad="13"/>
<connect gate="G$1" pin="XRESET" pad="3"/>
<connect gate="G$1" pin="XTAL0" pad="18"/>
<connect gate="G$1" pin="XTAL1" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XR2206" prefix="U">
<description>XR2206 Monolithic Function Generator</description>
<gates>
<gate name="G$1" symbol="XR2206"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="AMSI" pad="1"/>
<connect gate="G$1" pin="BIAS" pad="10"/>
<connect gate="G$1" pin="FSKI" pad="9"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="MO" pad="3"/>
<connect gate="G$1" pin="STO" pad="2"/>
<connect gate="G$1" pin="SYMA1" pad="15"/>
<connect gate="G$1" pin="SYMA2" pad="16"/>
<connect gate="G$1" pin="SYNCO" pad="11"/>
<connect gate="G$1" pin="TC1" pad="5"/>
<connect gate="G$1" pin="TC2" pad="6"/>
<connect gate="G$1" pin="TR1" pad="7"/>
<connect gate="G$1" pin="TR2" pad="8"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="WAVEA1" pad="13"/>
<connect gate="G$1" pin="WAVEA2" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD725">
<description>RGB component to NTSC/PAL Encoder&lt;br&gt;
&lt;br&gt;
Not in catalog&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="AD725"/>
</gates>
<devices>
<device name="" package="SO16L">
<connects>
<connect gate="G$1" pin="4FSC" pad="3"/>
<connect gate="G$1" pin="AGND" pad="2"/>
<connect gate="G$1" pin="APOS" pad="4"/>
<connect gate="G$1" pin="BIN" pad="8"/>
<connect gate="G$1" pin="CE" pad="5"/>
<connect gate="G$1" pin="COMP" pad="10"/>
<connect gate="G$1" pin="CRMA" pad="9"/>
<connect gate="G$1" pin="DGND" pad="13"/>
<connect gate="G$1" pin="DPOS" pad="14"/>
<connect gate="G$1" pin="GIN" pad="7"/>
<connect gate="G$1" pin="HSYNC" pad="16"/>
<connect gate="G$1" pin="LUMA" pad="11"/>
<connect gate="G$1" pin="RIN" pad="6"/>
<connect gate="G$1" pin="STND" pad="1"/>
<connect gate="G$1" pin="VSYNC" pad="15"/>
<connect gate="G$1" pin="YTRAP" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD5330" prefix="U">
<description>8-bit parallel input DAC&lt;br&gt;
&lt;br&gt;
Retired: IC-09612</description>
<gates>
<gate name="G$1" symbol="AD5330"/>
</gates>
<devices>
<device name="" package="TSSOP20">
<connects>
<connect gate="G$1" pin="BUF" pad="1"/>
<connect gate="G$1" pin="CLR" pad="9"/>
<connect gate="G$1" pin="CS" pad="6"/>
<connect gate="G$1" pin="DB0" pad="13"/>
<connect gate="G$1" pin="DB1" pad="14"/>
<connect gate="G$1" pin="DB2" pad="15"/>
<connect gate="G$1" pin="DB3" pad="16"/>
<connect gate="G$1" pin="DB4" pad="17"/>
<connect gate="G$1" pin="DB5" pad="18"/>
<connect gate="G$1" pin="DB6" pad="19"/>
<connect gate="G$1" pin="DB7" pad="20"/>
<connect gate="G$1" pin="GAIN" pad="8"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="LDAC" pad="10"/>
<connect gate="G$1" pin="PD" pad="11"/>
<connect gate="G$1" pin="VDD" pad="12"/>
<connect gate="G$1" pin="VOUT" pad="4"/>
<connect gate="G$1" pin="VREF" pad="3"/>
<connect gate="G$1" pin="WR" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD7302">
<description>8-bit parallel input 2-output DAC&lt;br&gt;
&lt;br&gt;
Retired: IC-09157&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="AD7302"/>
</gates>
<devices>
<device name="SMD" package="TSSOP20">
<connects>
<connect gate="G$1" pin="AB" pad="11"/>
<connect gate="G$1" pin="AGND" pad="17"/>
<connect gate="G$1" pin="CLR" pad="14"/>
<connect gate="G$1" pin="CS" pad="9"/>
<connect gate="G$1" pin="DB0" pad="8"/>
<connect gate="G$1" pin="DB1" pad="7"/>
<connect gate="G$1" pin="DB2" pad="6"/>
<connect gate="G$1" pin="DB3" pad="5"/>
<connect gate="G$1" pin="DB4" pad="4"/>
<connect gate="G$1" pin="DB5" pad="3"/>
<connect gate="G$1" pin="DB6" pad="2"/>
<connect gate="G$1" pin="DB7" pad="1"/>
<connect gate="G$1" pin="DGND" pad="20"/>
<connect gate="G$1" pin="LDAC" pad="13"/>
<connect gate="G$1" pin="PD" pad="12"/>
<connect gate="G$1" pin="REFIN" pad="16"/>
<connect gate="G$1" pin="VDD" pad="15"/>
<connect gate="G$1" pin="VOUTA" pad="19"/>
<connect gate="G$1" pin="VOUTB" pad="18"/>
<connect gate="G$1" pin="WR" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD7745">
<description>24-bit capacitance to digital converter&lt;br&gt;
&lt;br&gt;
Not in catalog&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="AD7745"/>
</gates>
<devices>
<device name="" package="TSSOP16">
<connects>
<connect gate="G$1" pin="/RDY" pad="2"/>
<connect gate="G$1" pin="CIN1+" pad="8"/>
<connect gate="G$1" pin="CIN1-" pad="7"/>
<connect gate="G$1" pin="CIN2+" pad="9"/>
<connect gate="G$1" pin="CIN2-" pad="10"/>
<connect gate="G$1" pin="EXCA" pad="3"/>
<connect gate="G$1" pin="EXCB" pad="4"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="NC" pad="15"/>
<connect gate="G$1" pin="REFIN+" pad="5"/>
<connect gate="G$1" pin="REFIN-" pad="6"/>
<connect gate="G$1" pin="SCL" pad="1"/>
<connect gate="G$1" pin="SDA" pad="16"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VIN+" pad="11"/>
<connect gate="G$1" pin="VIN-" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD7781" prefix="U">
<description>20-Bit, Pin-Programmable, Ultralow Power Sigma-Delta ADC&lt;br&gt;
&lt;br&gt;
Dead Prototype: IC-10476</description>
<gates>
<gate name="G$1" symbol="AD7781"/>
</gates>
<devices>
<device name="CRZ" package="SOIC-14">
<connects>
<connect gate="G$1" pin="*PDRST" pad="13"/>
<connect gate="G$1" pin="AIN+" pad="5"/>
<connect gate="G$1" pin="AIN-" pad="6"/>
<connect gate="G$1" pin="AVDD" pad="11"/>
<connect gate="G$1" pin="BPDSW" pad="9"/>
<connect gate="G$1" pin="DOUT" pad="2"/>
<connect gate="G$1" pin="DVDD" pad="12"/>
<connect gate="G$1" pin="FILTER" pad="14"/>
<connect gate="G$1" pin="GAIN" pad="4"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="REFIN+" pad="7"/>
<connect gate="G$1" pin="REFIN-" pad="8"/>
<connect gate="G$1" pin="SCLK" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CRUZ" package="TSSOP-16">
<connects>
<connect gate="G$1" pin="*PDRST" pad="14"/>
<connect gate="G$1" pin="AIN+" pad="6"/>
<connect gate="G$1" pin="AIN-" pad="7"/>
<connect gate="G$1" pin="AVDD" pad="12"/>
<connect gate="G$1" pin="BPDSW" pad="10"/>
<connect gate="G$1" pin="DOUT" pad="3"/>
<connect gate="G$1" pin="DVDD" pad="13"/>
<connect gate="G$1" pin="FILTER" pad="15"/>
<connect gate="G$1" pin="GAIN" pad="5"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="REFIN+" pad="8"/>
<connect gate="G$1" pin="REFIN-" pad="9"/>
<connect gate="G$1" pin="SCLK" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8397-EPAD" prefix="IC">
<description>Rail-to-rail high current output op-amp&lt;br&gt;
&lt;br&gt;
Retired: IC-10041&lt;br&gt;
Retired: IC-09592&lt;br&gt;</description>
<gates>
<gate name="A" symbol="OP-AMP+--1"/>
<gate name="B" symbol="OP-AMP-1"/>
</gates>
<devices>
<device name="EPAD" package="SO08-EPAD">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="EPAD" pad="EPAD"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD9835">
<description>50MHz DDS waveform generator&lt;br&gt;
&lt;br&gt;
Retired: IC-09105&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="AD9835"/>
</gates>
<devices>
<device name="" package="TSSOP16">
<connects>
<connect gate="G$1" pin="AGND" pad="13"/>
<connect gate="G$1" pin="AVDD" pad="15"/>
<connect gate="G$1" pin="COMP" pad="16"/>
<connect gate="G$1" pin="DGND" pad="5"/>
<connect gate="G$1" pin="DVDD" pad="4"/>
<connect gate="G$1" pin="FSEL" pad="10"/>
<connect gate="G$1" pin="FSYNC" pad="9"/>
<connect gate="G$1" pin="FS_ADJ" pad="1"/>
<connect gate="G$1" pin="IOUT" pad="14"/>
<connect gate="G$1" pin="MCLK" pad="6"/>
<connect gate="G$1" pin="PSEL0" pad="12"/>
<connect gate="G$1" pin="PSEL1" pad="11"/>
<connect gate="G$1" pin="REFIN" pad="2"/>
<connect gate="G$1" pin="REFOUT" pad="3"/>
<connect gate="G$1" pin="SCLK" pad="7"/>
<connect gate="G$1" pin="SDATA" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AS3400" prefix="U">
<description>Active noise cancellation chip.&lt;br&gt;
Stereo in, stereo out, two microphones.&lt;br&gt;
Single alkaline cell power.&lt;br&gt;
QFN-24 w/exposed pad.&lt;br&gt;
&lt;br&gt;
Dead Prototype: IC-10703&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="AS3400"/>
</gates>
<devices>
<device name="" package="QFN-24_ALT2">
<connects>
<connect gate="G$1" pin="AGND" pad="1"/>
<connect gate="G$1" pin="CPN" pad="22"/>
<connect gate="G$1" pin="CPP" pad="20"/>
<connect gate="G$1" pin="GND" pad="21"/>
<connect gate="G$1" pin="HPL" pad="16"/>
<connect gate="G$1" pin="HPR" pad="17"/>
<connect gate="G$1" pin="HPVDD" pad="18"/>
<connect gate="G$1" pin="IOP1R" pad="11"/>
<connect gate="G$1" pin="IOP2R" pad="13"/>
<connect gate="G$1" pin="LINL" pad="2"/>
<connect gate="G$1" pin="LINR" pad="3"/>
<connect gate="G$1" pin="MICL" pad="6"/>
<connect gate="G$1" pin="MICR" pad="8"/>
<connect gate="G$1" pin="MICS" pad="7"/>
<connect gate="G$1" pin="MODE_CSCL" pad="5"/>
<connect gate="G$1" pin="PAD" pad="EP"/>
<connect gate="G$1" pin="QLINR" pad="10"/>
<connect gate="G$1" pin="QMICL" pad="24"/>
<connect gate="G$1" pin="QMICR" pad="9"/>
<connect gate="G$1" pin="QOP1R" pad="12"/>
<connect gate="G$1" pin="QOP2R" pad="14"/>
<connect gate="G$1" pin="VBAT" pad="19"/>
<connect gate="G$1" pin="VNEG" pad="23"/>
<connect gate="G$1" pin="VOL_CSDA" pad="4"/>
<connect gate="G$1" pin="VSS" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GENERIC-SOIC8" prefix="U">
<description>A placeholder for generic narrow &amp; wide SOIC8 foorptints - used on the DIP adapter board.&lt;br&gt;
&lt;br&gt;
Has strange reference to IC-10141, a Seven Band Graphic Equalizer Display Filter SOIC-8&lt;br&gt;
VFP: IC-10141&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="GENERIC-8PIN"/>
</gates>
<devices>
<device name="" package="SO08-UNIVERSAL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MSGEQ7N-FILTER" package="SO08">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-10141"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HIH6131">
<description>Humidity sensor&lt;br&gt;
&lt;br&gt;
Not in catalog&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="HIH6131"/>
</gates>
<devices>
<device name="" package="SOIC8">
<connects>
<connect gate="G$1" pin="AL_H" pad="5"/>
<connect gate="G$1" pin="AL_L" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="SCL" pad="3"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="VCORE" pad="1"/>
<connect gate="G$1" pin="VDD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HT8950">
<description>Holtek voice modulator IC, COM-10574&lt;br&gt;
&lt;br&gt;
Retired: No prod ID (PN 5207)</description>
<gates>
<gate name="G$1" symbol="HT8950"/>
</gates>
<devices>
<device name="" package="DIL18">
<connects>
<connect gate="G$1" pin="AIN" pad="6"/>
<connect gate="G$1" pin="AO" pad="5"/>
<connect gate="G$1" pin="AUDIO" pad="9"/>
<connect gate="G$1" pin="FVIB" pad="12"/>
<connect gate="G$1" pin="LAMP" pad="8"/>
<connect gate="G$1" pin="OSC1" pad="14"/>
<connect gate="G$1" pin="OSC2" pad="13"/>
<connect gate="G$1" pin="ROB" pad="18"/>
<connect gate="G$1" pin="SW0" pad="1"/>
<connect gate="G$1" pin="SW1" pad="2"/>
<connect gate="G$1" pin="SW2" pad="3"/>
<connect gate="G$1" pin="TGD" pad="17"/>
<connect gate="G$1" pin="TGU" pad="16"/>
<connect gate="G$1" pin="TS" pad="11"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VIB" pad="15"/>
<connect gate="G$1" pin="VREF" pad="10"/>
<connect gate="G$1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA139" prefix="U" uservalue="yes">
<description>High-side shunt current sense&lt;BR&gt;
2.7V-40V, 1%&lt;br&gt;
&lt;br&gt;
Prototype: IC-11211&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="INA139"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="VIN+" pad="3"/>
<connect gate="G$1" pin="VIN-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM393">
<description>Low-voltage comparator&lt;br&gt;
&lt;br&gt;
Prototype: IC-09375</description>
<gates>
<gate name="G1" symbol="OP-AMP+-"/>
<gate name="G2" symbol="OP-AMP"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G1" pin="+IN" pad="3"/>
<connect gate="G1" pin="-IN" pad="2"/>
<connect gate="G1" pin="OUT" pad="1"/>
<connect gate="G1" pin="V+" pad="8"/>
<connect gate="G1" pin="V-" pad="4"/>
<connect gate="G2" pin="+IN" pad="5"/>
<connect gate="G2" pin="-IN" pad="6"/>
<connect gate="G2" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1014">
<description>Precision quad op-amp. I/O range includes negative rail.&lt;br&gt;
&lt;br&gt;
Dead Prototype: IC-08606&lt;br&gt;
TODO: fix symbol&lt;br&gt;</description>
<gates>
<gate name="G1" symbol="LT1014"/>
<gate name="G2" symbol="LT1014_2"/>
<gate name="G3" symbol="LT1014_2"/>
<gate name="G4" symbol="LT1014_2"/>
</gates>
<devices>
<device name="" package="SO16L">
<connects>
<connect gate="G1" pin="+IN" pad="3"/>
<connect gate="G1" pin="+V" pad="4"/>
<connect gate="G1" pin="-IN" pad="2"/>
<connect gate="G1" pin="-V" pad="13"/>
<connect gate="G1" pin="OUT" pad="1"/>
<connect gate="G2" pin="+IN" pad="5"/>
<connect gate="G2" pin="-IN" pad="6"/>
<connect gate="G2" pin="OUT" pad="7"/>
<connect gate="G3" pin="+IN" pad="12"/>
<connect gate="G3" pin="-IN" pad="11"/>
<connect gate="G3" pin="OUT" pad="10"/>
<connect gate="G4" pin="+IN" pad="14"/>
<connect gate="G4" pin="-IN" pad="15"/>
<connect gate="G4" pin="OUT" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC6244">
<description>Low-noise, high-speed rail-to-rail CMOS op-amp&lt;br&gt;
&lt;br&gt;
Not in catalog&lt;br&gt;</description>
<gates>
<gate name="G1" symbol="LTC6244"/>
<gate name="G2" symbol="LTC6244_2"/>
</gates>
<devices>
<device name="" package="MSOP8">
<connects>
<connect gate="G1" pin="+IN" pad="3"/>
<connect gate="G1" pin="+V" pad="8"/>
<connect gate="G1" pin="-IN" pad="2"/>
<connect gate="G1" pin="-V" pad="4"/>
<connect gate="G1" pin="OUT" pad="1"/>
<connect gate="G2" pin="+IN" pad="5"/>
<connect gate="G2" pin="-IN" pad="6"/>
<connect gate="G2" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX6675" prefix="U">
<description>&lt;b&gt;Cold-Junction-Compensated K-Thermocoupleto-Digital
Converter (0°C to +1024°C)&lt;br/&gt;&lt;/b&gt;
The MAX6675 performs cold-junction compensation
and digitizes the signal from a type-K thermocouple.&lt;br/&gt;
The data is output in a 12-bit resolution, SPI™-compatible,
read-only format.&lt;br/&gt;
This converter resolves temperatures to 0.25°C, allows readings as high as +1024°C, and exhibits thermocouple accuracy of 8LSBs for temperatures ranging from 0°C to +700°C.&lt;br&gt;
&lt;br&gt;
Dead Prototype: IC-12512&lt;br.</description>
<gates>
<gate name="G$1" symbol="MAX6675"/>
</gates>
<devices>
<device name="" package="SOIC8">
<connects>
<connect gate="G$1" pin="!CS" pad="6"/>
<connect gate="G$1" pin="(MI)SO" pad="7"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="SCK" pad="5"/>
<connect gate="G$1" pin="T+" pad="3"/>
<connect gate="G$1" pin="T-" pad="2"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-12512"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP42XXX" prefix="U">
<description>SPI controlled dual digital potentiometer by Microchip&lt;br&gt;
&lt;br&gt;
Not in catalog?&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="MCP42XXX"/>
</gates>
<devices>
<device name="" package="SO014">
<connects>
<connect gate="G$1" pin="A0" pad="8"/>
<connect gate="G$1" pin="A1" pad="7"/>
<connect gate="G$1" pin="B0" pad="10"/>
<connect gate="G$1" pin="B1" pad="5"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="13"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="RST" pad="11"/>
<connect gate="G$1" pin="SCK" pad="2"/>
<connect gate="G$1" pin="SHTDWN" pad="12"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="W0" pad="9"/>
<connect gate="G$1" pin="W1" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MUX-TS3A5017">
<description>Dual-channel 4:1 analog mux&lt;br&gt;
&lt;br&gt;
Retired: IC-08862</description>
<gates>
<gate name="G$1" symbol="TS3A5017"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G$1" pin="1D" pad="7"/>
<connect gate="G$1" pin="1EN" pad="1"/>
<connect gate="G$1" pin="1S1" pad="6"/>
<connect gate="G$1" pin="1S2" pad="5"/>
<connect gate="G$1" pin="1S3" pad="4"/>
<connect gate="G$1" pin="1S4" pad="3"/>
<connect gate="G$1" pin="2D" pad="9"/>
<connect gate="G$1" pin="2EN" pad="15"/>
<connect gate="G$1" pin="2S1" pad="10"/>
<connect gate="G$1" pin="2S2" pad="11"/>
<connect gate="G$1" pin="2S3" pad="12"/>
<connect gate="G$1" pin="2S4" pad="13"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="IN1" pad="14"/>
<connect gate="G$1" pin="IN2" pad="2"/>
<connect gate="G$1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TVP5150-NTSC_DECODER">
<description>Texas Instrument NTSC/PAL Decoder
TI Part #TVP5150AM1
*** UNPROVEN FOOTPRINT ***

Decodes NTSC video signal to YCbCr 4:2:2 signal&lt;br&gt;
&lt;br&gt;
Retired: IC-09311&lt;br&gt;
Retired: IC-09080</description>
<gates>
<gate name="G$1" symbol="TVP5150-NTSC_DECODER-1"/>
</gates>
<devices>
<device name="" package="TQFP32-5MM">
<connects>
<connect gate="G$1" pin="AGND" pad="7"/>
<connect gate="G$1" pin="AIP1A" pad="1"/>
<connect gate="G$1" pin="AIP1B" pad="2"/>
<connect gate="G$1" pin="AVID" pad="26"/>
<connect gate="G$1" pin="CH_AGND" pad="31"/>
<connect gate="G$1" pin="CH_AVDD" pad="32"/>
<connect gate="G$1" pin="DGND" pad="19"/>
<connect gate="G$1" pin="DVDD" pad="20"/>
<connect gate="G$1" pin="FID/GLCO" pad="23"/>
<connect gate="G$1" pin="HSYNC" pad="25"/>
<connect gate="G$1" pin="INT_REQ" pad="27"/>
<connect gate="G$1" pin="IO_DVDD" pad="10"/>
<connect gate="G$1" pin="PCLK/SCLK" pad="9"/>
<connect gate="G$1" pin="PDN" pad="28"/>
<connect gate="G$1" pin="PLL_AGND" pad="3"/>
<connect gate="G$1" pin="PLL_AVDD" pad="4"/>
<connect gate="G$1" pin="REFM" pad="30"/>
<connect gate="G$1" pin="REFP" pad="29"/>
<connect gate="G$1" pin="RESET/" pad="8"/>
<connect gate="G$1" pin="SCL" pad="21"/>
<connect gate="G$1" pin="SDA" pad="22"/>
<connect gate="G$1" pin="VSYNC" pad="24"/>
<connect gate="G$1" pin="XTAL1" pad="5"/>
<connect gate="G$1" pin="XTAL2" pad="6"/>
<connect gate="G$1" pin="YOUT_0" pad="18"/>
<connect gate="G$1" pin="YOUT_1" pad="17"/>
<connect gate="G$1" pin="YOUT_2" pad="16"/>
<connect gate="G$1" pin="YOUT_3" pad="15"/>
<connect gate="G$1" pin="YOUT_4" pad="14"/>
<connect gate="G$1" pin="YOUT_5" pad="13"/>
<connect gate="G$1" pin="YOUT_6" pad="12"/>
<connect gate="G$1" pin="YOUT_7" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="X9015_DIGI_POT">
<description>Digital pot- up/down/increment control only&lt;br&gt;
&lt;br&gt;
Prototype: IC-08072 no stock, old part (2008-2010)</description>
<gates>
<gate name="G$1" symbol="X9015_DIGI_POT"/>
</gates>
<devices>
<device name="S" package="SO08">
<connects>
<connect gate="G$1" pin="CS'" pad="7"/>
<connect gate="G$1" pin="INC'" pad="1"/>
<connect gate="G$1" pin="RH/VH" pad="3"/>
<connect gate="G$1" pin="RL/VL" pad="6"/>
<connect gate="G$1" pin="RW/VW" pad="5"/>
<connect gate="G$1" pin="U/D'" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*157" prefix="IC">
<description>Quadruple 2-line to 1-line data &lt;b&gt;SELECTOR/MULTIPLEXER&lt;/b&gt;
&lt;br&gt;
RETIRED: IC-09602</description>
<gates>
<gate name="A" symbol="74157"/>
<gate name="G$1" symbol="POWER_CONSORT"/>
</gates>
<devices>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="!A!/B" pad="2"/>
<connect gate="A" pin="1A" pad="3"/>
<connect gate="A" pin="1B" pad="4"/>
<connect gate="A" pin="1Y" pad="5"/>
<connect gate="A" pin="2A" pad="7"/>
<connect gate="A" pin="2B" pad="8"/>
<connect gate="A" pin="2Y" pad="9"/>
<connect gate="A" pin="3A" pad="14"/>
<connect gate="A" pin="3B" pad="13"/>
<connect gate="A" pin="3Y" pad="12"/>
<connect gate="A" pin="4A" pad="18"/>
<connect gate="A" pin="4B" pad="17"/>
<connect gate="A" pin="4Y" pad="15"/>
<connect gate="A" pin="G" pad="19"/>
<connect gate="G$1" pin="P$V+" pad="20"/>
<connect gate="G$1" pin="P$V-" pad="10"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="N" package="DIP16">
<connects>
<connect gate="A" pin="!A!/B" pad="1"/>
<connect gate="A" pin="1A" pad="2"/>
<connect gate="A" pin="1B" pad="3"/>
<connect gate="A" pin="1Y" pad="4"/>
<connect gate="A" pin="2A" pad="5"/>
<connect gate="A" pin="2B" pad="6"/>
<connect gate="A" pin="2Y" pad="7"/>
<connect gate="A" pin="3A" pad="11"/>
<connect gate="A" pin="3B" pad="10"/>
<connect gate="A" pin="3Y" pad="9"/>
<connect gate="A" pin="4A" pad="14"/>
<connect gate="A" pin="4B" pad="13"/>
<connect gate="A" pin="4Y" pad="12"/>
<connect gate="A" pin="G" pad="15"/>
<connect gate="G$1" pin="P$V+" pad="16"/>
<connect gate="G$1" pin="P$V-" pad="8"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="SO" package="SO16">
<connects>
<connect gate="A" pin="!A!/B" pad="1"/>
<connect gate="A" pin="1A" pad="2"/>
<connect gate="A" pin="1B" pad="3"/>
<connect gate="A" pin="1Y" pad="4"/>
<connect gate="A" pin="2A" pad="5"/>
<connect gate="A" pin="2B" pad="6"/>
<connect gate="A" pin="2Y" pad="7"/>
<connect gate="A" pin="3A" pad="11"/>
<connect gate="A" pin="3B" pad="10"/>
<connect gate="A" pin="3Y" pad="9"/>
<connect gate="A" pin="4A" pad="14"/>
<connect gate="A" pin="4B" pad="13"/>
<connect gate="A" pin="4Y" pad="12"/>
<connect gate="A" pin="G" pad="15"/>
<connect gate="G$1" pin="P$V+" pad="16"/>
<connect gate="G$1" pin="P$V-" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XS1_L1_64LQFP">
<description>XMos processor (multicore)
&lt;br&gt;
&lt;br&gt;
Not in catalog</description>
<gates>
<gate name="G$1" symbol="XS1-L1-64LQFP"/>
</gates>
<devices>
<device name="" package="SQFP-S-10X10-64-XS1">
<connects>
<connect gate="G$1" pin="CLK" pad="9"/>
<connect gate="G$1" pin="DEBUG" pad="17"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="MODE0" pad="22"/>
<connect gate="G$1" pin="MODE1" pad="23"/>
<connect gate="G$1" pin="MODE2" pad="24"/>
<connect gate="G$1" pin="MODE3" pad="25"/>
<connect gate="G$1" pin="PLL_AGND" pad="19"/>
<connect gate="G$1" pin="PLL_AVDD" pad="20"/>
<connect gate="G$1" pin="RST_N" pad="8"/>
<connect gate="G$1" pin="TCK" pad="29"/>
<connect gate="G$1" pin="TDI" pad="30"/>
<connect gate="G$1" pin="TDO" pad="31"/>
<connect gate="G$1" pin="TMS" pad="27"/>
<connect gate="G$1" pin="TRST_N" pad="26"/>
<connect gate="G$1" pin="VDDIO_18" pad="18"/>
<connect gate="G$1" pin="VDDIO_32" pad="32"/>
<connect gate="G$1" pin="VDDIO_40" pad="40"/>
<connect gate="G$1" pin="VDDIO_53" pad="53"/>
<connect gate="G$1" pin="VDDIO_6" pad="6"/>
<connect gate="G$1" pin="VDDIO_60" pad="60"/>
<connect gate="G$1" pin="VDD_13" pad="13"/>
<connect gate="G$1" pin="VDD_21" pad="21"/>
<connect gate="G$1" pin="VDD_28" pad="28"/>
<connect gate="G$1" pin="VDD_37" pad="37"/>
<connect gate="G$1" pin="VDD_4" pad="4"/>
<connect gate="G$1" pin="VDD_43" pad="43"/>
<connect gate="G$1" pin="VDD_52" pad="52"/>
<connect gate="G$1" pin="VDD_61" pad="61"/>
<connect gate="G$1" pin="X0D0" pad="16"/>
<connect gate="G$1" pin="X0D1" pad="15"/>
<connect gate="G$1" pin="X0D10" pad="1"/>
<connect gate="G$1" pin="X0D11" pad="64"/>
<connect gate="G$1" pin="X0D12" pad="63"/>
<connect gate="G$1" pin="X0D13" pad="62"/>
<connect gate="G$1" pin="X0D14" pad="59"/>
<connect gate="G$1" pin="X0D15" pad="58"/>
<connect gate="G$1" pin="X0D16" pad="57"/>
<connect gate="G$1" pin="X0D17" pad="56"/>
<connect gate="G$1" pin="X0D18" pad="55"/>
<connect gate="G$1" pin="X0D19" pad="54"/>
<connect gate="G$1" pin="X0D2" pad="14"/>
<connect gate="G$1" pin="X0D20" pad="51"/>
<connect gate="G$1" pin="X0D21" pad="50"/>
<connect gate="G$1" pin="X0D22" pad="49"/>
<connect gate="G$1" pin="X0D23" pad="48"/>
<connect gate="G$1" pin="X0D24" pad="47"/>
<connect gate="G$1" pin="X0D25" pad="46"/>
<connect gate="G$1" pin="X0D26" pad="45"/>
<connect gate="G$1" pin="X0D27" pad="44"/>
<connect gate="G$1" pin="X0D3" pad="12"/>
<connect gate="G$1" pin="X0D32" pad="36"/>
<connect gate="G$1" pin="X0D33" pad="35"/>
<connect gate="G$1" pin="X0D34" pad="34"/>
<connect gate="G$1" pin="X0D35" pad="33"/>
<connect gate="G$1" pin="X0D36" pad="42"/>
<connect gate="G$1" pin="X0D37" pad="41"/>
<connect gate="G$1" pin="X0D38" pad="39"/>
<connect gate="G$1" pin="X0D39" pad="38"/>
<connect gate="G$1" pin="X0D4" pad="11"/>
<connect gate="G$1" pin="X0D5" pad="10"/>
<connect gate="G$1" pin="X0D6" pad="7"/>
<connect gate="G$1" pin="X0D7" pad="5"/>
<connect gate="G$1" pin="X0D8" pad="3"/>
<connect gate="G$1" pin="X0D9" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XC3S250/500E-PQ208">
<description>Xilinx Spartan3E FPGA
&lt;br&gt;
&lt;br&gt;
Not in catalog</description>
<gates>
<gate name="G$1" symbol="XC3S250/500E-PQ208"/>
</gates>
<devices>
<device name="" package="PQ208">
<connects>
<connect gate="G$1" pin="10_L08P_2/D7/GCLK12" pad="74"/>
<connect gate="G$1" pin="DONE" pad="104"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="GND@10" pad="95"/>
<connect gate="G$1" pin="GND@11" pad="105"/>
<connect gate="G$1" pin="GND@12" pad="121"/>
<connect gate="G$1" pin="GND@13" pad="131"/>
<connect gate="G$1" pin="GND@14" pad="141"/>
<connect gate="G$1" pin="GND@15" pad="156"/>
<connect gate="G$1" pin="GND@16" pad="173"/>
<connect gate="G$1" pin="GND@17" pad="182"/>
<connect gate="G$1" pin="GND@18" pad="188"/>
<connect gate="G$1" pin="GND@19" pad="198"/>
<connect gate="G$1" pin="GND@2" pad="17"/>
<connect gate="G$1" pin="GND@20" pad="208"/>
<connect gate="G$1" pin="GND@3" pad="27"/>
<connect gate="G$1" pin="GND@4" pad="37"/>
<connect gate="G$1" pin="GND@5" pad="52"/>
<connect gate="G$1" pin="GND@6" pad="53"/>
<connect gate="G$1" pin="GND@7" pad="70"/>
<connect gate="G$1" pin="GND@8" pad="79"/>
<connect gate="G$1" pin="GND@9" pad="85"/>
<connect gate="G$1" pin="IO" pad="187"/>
<connect gate="G$1" pin="IO/D5" pad="76"/>
<connect gate="G$1" pin="IO/L01N_2/INIT_B" pad="56"/>
<connect gate="G$1" pin="IO/M1" pad="84"/>
<connect gate="G$1" pin="IO/VREF_0" pad="179"/>
<connect gate="G$1" pin="IO/VREF_2" pad="98"/>
<connect gate="G$1" pin="IO/VREF_3" pad="45"/>
<connect gate="G$1" pin="IO_16P_1/LDC1" pad="152"/>
<connect gate="G$1" pin="IO_L01N_0" pad="161"/>
<connect gate="G$1" pin="IO_L01N_1/A15" pad="107"/>
<connect gate="G$1" pin="IO_L01N_3" pad="3"/>
<connect gate="G$1" pin="IO_L01P_0" pad="160"/>
<connect gate="G$1" pin="IO_L01P_1/A16" pad="106"/>
<connect gate="G$1" pin="IO_L01P_2/CSO_B" pad="55"/>
<connect gate="G$1" pin="IO_L01P_3" pad="2"/>
<connect gate="G$1" pin="IO_L02N_0/VREF_0" pad="163"/>
<connect gate="G$1" pin="IO_L02N_1/A13" pad="109"/>
<connect gate="G$1" pin="IO_L02N_3/VREF_3" pad="5"/>
<connect gate="G$1" pin="IO_L02P_0" pad="162"/>
<connect gate="G$1" pin="IO_L02P_1/A14" pad="108"/>
<connect gate="G$1" pin="IO_L02P_3" pad="4"/>
<connect gate="G$1" pin="IO_L03N_0" pad="165"/>
<connect gate="G$1" pin="IO_L03N_1/VREF_1" pad="113"/>
<connect gate="G$1" pin="IO_L03N_2/MOSI/CSI_B" pad="61"/>
<connect gate="G$1" pin="IO_L03N_3" pad="9"/>
<connect gate="G$1" pin="IO_L03P_0" pad="164"/>
<connect gate="G$1" pin="IO_L03P_1" pad="112"/>
<connect gate="G$1" pin="IO_L03P_2/DOUT/BUSY" pad="60"/>
<connect gate="G$1" pin="IO_L03P_3" pad="8"/>
<connect gate="G$1" pin="IO_L04N_0/VREF_0" pad="168"/>
<connect gate="G$1" pin="IO_L04N_1" pad="116"/>
<connect gate="G$1" pin="IO_L04N_2" pad="63"/>
<connect gate="G$1" pin="IO_L04N_3" pad="12"/>
<connect gate="G$1" pin="IO_L04P_0" pad="167"/>
<connect gate="G$1" pin="IO_L04P_1" pad="115"/>
<connect gate="G$1" pin="IO_L04P_2" pad="62"/>
<connect gate="G$1" pin="IO_L04P_3" pad="11"/>
<connect gate="G$1" pin="IO_L05N_0" pad="172"/>
<connect gate="G$1" pin="IO_L05N_1/A11" pad="120"/>
<connect gate="G$1" pin="IO_L05N_2" pad="65"/>
<connect gate="G$1" pin="IO_L05N_3" pad="16"/>
<connect gate="G$1" pin="IO_L05P_0" pad="171"/>
<connect gate="G$1" pin="IO_L05P_1/A12" pad="119"/>
<connect gate="G$1" pin="IO_L05P_2" pad="64"/>
<connect gate="G$1" pin="IO_L05P_3" pad="15"/>
<connect gate="G$1" pin="IO_L06N_1/VREF_1" pad="123"/>
<connect gate="G$1" pin="IO_L06N_2" pad="69"/>
<connect gate="G$1" pin="IO_L06N_3" pad="19"/>
<connect gate="G$1" pin="IO_L06P_1" pad="122"/>
<connect gate="G$1" pin="IO_L06P_2" pad="68"/>
<connect gate="G$1" pin="IO_L06P_3" pad="18"/>
<connect gate="G$1" pin="IO_L07N_0/GCLK5" pad="178"/>
<connect gate="G$1" pin="IO_L07N_1/A7/RHCLK1" pad="127"/>
<connect gate="G$1" pin="IO_L07N_3/LHCLK1" pad="23"/>
<connect gate="G$1" pin="IO_L07P_1/A10/RHCLK0" pad="126"/>
<connect gate="G$1" pin="IO_L07P_3/LHCLK0" pad="22"/>
<connect gate="G$1" pin="IO_L08N_0/GCLK7" pad="181"/>
<connect gate="G$1" pin="IO_L08N_1/A7/RHCLK3" pad="129"/>
<connect gate="G$1" pin="IO_L08N_2/D6/GCLK13" pad="75"/>
<connect gate="G$1" pin="IO_L08N_3/LHCLK3" pad="25"/>
<connect gate="G$1" pin="IO_L08P_0/GCLK6" pad="180"/>
<connect gate="G$1" pin="IO_L08P_1/A8/RHCLK2" pad="128"/>
<connect gate="G$1" pin="IO_L08P_3/LHCLK2" pad="24"/>
<connect gate="G$1" pin="IO_L09N_1/A5/RHCLK5" pad="133"/>
<connect gate="G$1" pin="IO_L09N_2/D3/GCLK15" pad="78"/>
<connect gate="G$1" pin="IO_L09N_3/LHCLK5" pad="29"/>
<connect gate="G$1" pin="IO_L09P_1/A6/RHCLK4" pad="132"/>
<connect gate="G$1" pin="IO_L09P_2/D4/GCLK14" pad="77"/>
<connect gate="G$1" pin="IO_L09P_3/LHCLK4" pad="28"/>
<connect gate="G$1" pin="IO_L10N_0/GCLK11" pad="186"/>
<connect gate="G$1" pin="IO_L10N_1/A3/RHCLK7" pad="135"/>
<connect gate="G$1" pin="IO_L10N_3/LHCLK7" pad="31"/>
<connect gate="G$1" pin="IO_L10P_0/GCLK10" pad="185"/>
<connect gate="G$1" pin="IO_L10P_1/A4/RHCLK6" pad="134"/>
<connect gate="G$1" pin="IO_L10P_3/LHCLK6" pad="30"/>
<connect gate="G$1" pin="IO_L11N_0" pad="190"/>
<connect gate="G$1" pin="IO_L11N_1/A1" pad="138"/>
<connect gate="G$1" pin="IO_L11N_2/D1/GCLK3" pad="83"/>
<connect gate="G$1" pin="IO_L11N_3" pad="34"/>
<connect gate="G$1" pin="IO_L11P_0" pad="189"/>
<connect gate="G$1" pin="IO_L11P_1/A2" pad="137"/>
<connect gate="G$1" pin="IO_L11P_2/D2/GCLK2" pad="82"/>
<connect gate="G$1" pin="IO_L11P_3" pad="33"/>
<connect gate="G$1" pin="IO_L12N_0/VREF_0" pad="193"/>
<connect gate="G$1" pin="IO_L12N_1/A0" pad="140"/>
<connect gate="G$1" pin="IO_L12N_2/DIN/D0" pad="87"/>
<connect gate="G$1" pin="IO_L12N_3" pad="36"/>
<connect gate="G$1" pin="IO_L12P_0" pad="192"/>
<connect gate="G$1" pin="IO_L12P_1" pad="139"/>
<connect gate="G$1" pin="IO_L12P_2/M0" pad="86"/>
<connect gate="G$1" pin="IO_L12P_3" pad="35"/>
<connect gate="G$1" pin="IO_L13N_0" pad="197"/>
<connect gate="G$1" pin="IO_L13N_1" pad="145"/>
<connect gate="G$1" pin="IO_L13N_2" pad="90"/>
<connect gate="G$1" pin="IO_L13N_3" pad="40"/>
<connect gate="G$1" pin="IO_L13P_0" pad="196"/>
<connect gate="G$1" pin="IO_L13P_1" pad="144"/>
<connect gate="G$1" pin="IO_L13P_2" pad="89"/>
<connect gate="G$1" pin="IO_L13P_3" pad="39"/>
<connect gate="G$1" pin="IO_L14N_0/VREF_0" pad="200"/>
<connect gate="G$1" pin="IO_L14N_1" pad="147"/>
<connect gate="G$1" pin="IO_L14N_2/A22" pad="94"/>
<connect gate="G$1" pin="IO_L14N_3" pad="42"/>
<connect gate="G$1" pin="IO_L14P_0" pad="199"/>
<connect gate="G$1" pin="IO_L14P_1" pad="146"/>
<connect gate="G$1" pin="IO_L14P_2/A23" pad="93"/>
<connect gate="G$1" pin="IO_L14P_3" pad="41"/>
<connect gate="G$1" pin="IO_L15N_0" pad="203"/>
<connect gate="G$1" pin="IO_L15N_2/A20" pad="97"/>
<connect gate="G$1" pin="IO_L15N_3" pad="48"/>
<connect gate="G$1" pin="IO_L15P_0" pad="202"/>
<connect gate="G$1" pin="IO_L15P_1/HDC" pad="150"/>
<connect gate="G$1" pin="IO_L15P_2/A21" pad="96"/>
<connect gate="G$1" pin="IO_L15P_3" pad="47"/>
<connect gate="G$1" pin="IO_L15_1/LDC0" pad="151"/>
<connect gate="G$1" pin="IO_L16N_0/HSWAP" pad="206"/>
<connect gate="G$1" pin="IO_L16N_1/LDC2" pad="153"/>
<connect gate="G$1" pin="IO_L16N_2/VS1/A18" pad="100"/>
<connect gate="G$1" pin="IO_L16N_3" pad="50"/>
<connect gate="G$1" pin="IO_L16P_0" pad="205"/>
<connect gate="G$1" pin="IO_L16P_2/VS2/A19" pad="99"/>
<connect gate="G$1" pin="IO_L16P_3" pad="49"/>
<connect gate="G$1" pin="IO_L17N_2/CCLK" pad="103"/>
<connect gate="G$1" pin="IO_L17P_2/VS0/A17" pad="102"/>
<connect gate="G$1" pin="IO_LO7P_0/GCLK4" pad="177"/>
<connect gate="G$1" pin="IP" pad="159"/>
<connect gate="G$1" pin="IP/VREF_1" pad="136"/>
<connect gate="G$1" pin="IP/VREF_3" pad="20"/>
<connect gate="G$1" pin="IP@10" pad="148"/>
<connect gate="G$1" pin="IP@11" pad="154"/>
<connect gate="G$1" pin="IP@12" pad="54"/>
<connect gate="G$1" pin="IP@13" pad="91"/>
<connect gate="G$1" pin="IP@14" pad="101"/>
<connect gate="G$1" pin="IP@15" pad="6"/>
<connect gate="G$1" pin="IP@16" pad="14"/>
<connect gate="G$1" pin="IP@17" pad="26"/>
<connect gate="G$1" pin="IP@18" pad="32"/>
<connect gate="G$1" pin="IP@19" pad="43"/>
<connect gate="G$1" pin="IP@2" pad="169"/>
<connect gate="G$1" pin="IP@20" pad="51"/>
<connect gate="G$1" pin="IP@3" pad="194"/>
<connect gate="G$1" pin="IP@4" pad="204"/>
<connect gate="G$1" pin="IP@5" pad="110"/>
<connect gate="G$1" pin="IP@6" pad="118"/>
<connect gate="G$1" pin="IP@7" pad="124"/>
<connect gate="G$1" pin="IP@8" pad="130"/>
<connect gate="G$1" pin="IP@9" pad="142"/>
<connect gate="G$1" pin="IP_L02N_2" pad="58"/>
<connect gate="G$1" pin="IP_L02P_2" pad="57"/>
<connect gate="G$1" pin="IP_L06N_0" pad="175"/>
<connect gate="G$1" pin="IP_L06P_0" pad="174"/>
<connect gate="G$1" pin="IP_L07N_2/VREF_2" pad="72"/>
<connect gate="G$1" pin="IP_L07P_2" pad="71"/>
<connect gate="G$1" pin="IP_L09P_0/GCLK8" pad="183"/>
<connect gate="G$1" pin="IP_L10N_2/M2/GCLK1" pad="81"/>
<connect gate="G$1" pin="IP_L10P_2/RDWR_B/GCLK0" pad="80"/>
<connect gate="G$1" pin="IP_LO9N_0/GCLK9" pad="184"/>
<connect gate="G$1" pin="PROG_B" pad="1"/>
<connect gate="G$1" pin="TCK" pad="158"/>
<connect gate="G$1" pin="TDI" pad="207"/>
<connect gate="G$1" pin="TDO" pad="157"/>
<connect gate="G$1" pin="TMS" pad="155"/>
<connect gate="G$1" pin="VCC0_1" pad="114"/>
<connect gate="G$1" pin="VCC0_1@2" pad="125"/>
<connect gate="G$1" pin="VCC0_1@3" pad="143"/>
<connect gate="G$1" pin="VCCAUX" pad="7"/>
<connect gate="G$1" pin="VCCAUX@2" pad="44"/>
<connect gate="G$1" pin="VCCAUX@3" pad="66"/>
<connect gate="G$1" pin="VCCAUX@4" pad="92"/>
<connect gate="G$1" pin="VCCAUX@5" pad="111"/>
<connect gate="G$1" pin="VCCAUX@6" pad="149"/>
<connect gate="G$1" pin="VCCAUX@7" pad="166"/>
<connect gate="G$1" pin="VCCAUX@8" pad="195"/>
<connect gate="G$1" pin="VCCINT" pad="13"/>
<connect gate="G$1" pin="VCCINT@2" pad="67"/>
<connect gate="G$1" pin="VCCINT@3" pad="117"/>
<connect gate="G$1" pin="VCCINT@4" pad="170"/>
<connect gate="G$1" pin="VCCO_0" pad="176"/>
<connect gate="G$1" pin="VCCO_0@2" pad="191"/>
<connect gate="G$1" pin="VCCO_0@3" pad="201"/>
<connect gate="G$1" pin="VCCO_2" pad="59"/>
<connect gate="G$1" pin="VCCO_2@2" pad="73"/>
<connect gate="G$1" pin="VCCO_2@3" pad="88"/>
<connect gate="G$1" pin="VCCO_3" pad="21"/>
<connect gate="G$1" pin="VCCO_3@2" pad="38"/>
<connect gate="G$1" pin="VCCO_3@3" pad="46"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WS2801" prefix="U">
<description>&lt;h3&gt;WS2801&lt;/h3&gt;
3 Channel Constant Current LED Driver with programmable PWM outputs.
&lt;br&gt;
&lt;br&gt;
Datasheet:  http://www.sparkfun.com/datasheets/Components/LED/WS2801.pdf
&lt;br&gt;
&lt;br&gt;
RETIRED: IC-10297 (also, wrong cat)</description>
<gates>
<gate name="G$1" symbol="WS2801"/>
</gates>
<devices>
<device name="" package="SOP-14">
<connects>
<connect gate="G$1" pin="BFB" pad="6"/>
<connect gate="G$1" pin="BOUT" pad="8"/>
<connect gate="G$1" pin="CKI" pad="1"/>
<connect gate="G$1" pin="CKO" pad="13"/>
<connect gate="G$1" pin="GFB" pad="5"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="GOUT" pad="9"/>
<connect gate="G$1" pin="POL" pad="3"/>
<connect gate="G$1" pin="RFB" pad="4"/>
<connect gate="G$1" pin="ROUT" pad="10"/>
<connect gate="G$1" pin="SDI" pad="2"/>
<connect gate="G$1" pin="SDO" pad="12"/>
<connect gate="G$1" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STP16CP05">
<description>16-pin constant current sink shift register LED driver
&lt;br&gt;&lt;br&gt;
Not in catalog</description>
<gates>
<gate name="G$1" symbol="STP16CP05/A6282"/>
</gates>
<devices>
<device name="" package="SO-24DW">
<connects>
<connect gate="G$1" pin="CLK" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="LE" pad="4"/>
<connect gate="G$1" pin="OUT0" pad="5"/>
<connect gate="G$1" pin="OUT1" pad="6"/>
<connect gate="G$1" pin="OUT10" pad="15"/>
<connect gate="G$1" pin="OUT11" pad="16"/>
<connect gate="G$1" pin="OUT12" pad="17"/>
<connect gate="G$1" pin="OUT13" pad="18"/>
<connect gate="G$1" pin="OUT14" pad="19"/>
<connect gate="G$1" pin="OUT15" pad="20"/>
<connect gate="G$1" pin="OUT2" pad="7"/>
<connect gate="G$1" pin="OUT3" pad="8"/>
<connect gate="G$1" pin="OUT4" pad="9"/>
<connect gate="G$1" pin="OUT5" pad="10"/>
<connect gate="G$1" pin="OUT6" pad="11"/>
<connect gate="G$1" pin="OUT7" pad="12"/>
<connect gate="G$1" pin="OUT8" pad="13"/>
<connect gate="G$1" pin="OUT9" pad="14"/>
<connect gate="G$1" pin="REXT" pad="23"/>
<connect gate="G$1" pin="SDI" pad="2"/>
<connect gate="G$1" pin="SDO" pad="22"/>
<connect gate="G$1" pin="VDD" pad="24"/>
<connect gate="G$1" pin="~OE" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF8575C">
<description>PCF8575C I/O Expander.
&lt;br&gt;
RETIRED IC-08153 (Also move to special)</description>
<gates>
<gate name="G$1" symbol="PCF8575C"/>
</gates>
<devices>
<device name="" package="SO-24DW">
<connects>
<connect gate="G$1" pin="A0" pad="21"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="INT" pad="1"/>
<connect gate="G$1" pin="P10" pad="13"/>
<connect gate="G$1" pin="P11" pad="14"/>
<connect gate="G$1" pin="P12" pad="15"/>
<connect gate="G$1" pin="P13" pad="16"/>
<connect gate="G$1" pin="P14" pad="17"/>
<connect gate="G$1" pin="P15" pad="18"/>
<connect gate="G$1" pin="P16" pad="19"/>
<connect gate="G$1" pin="P17" pad="20"/>
<connect gate="G$1" pin="PO0" pad="4"/>
<connect gate="G$1" pin="PO1" pad="5"/>
<connect gate="G$1" pin="PO2" pad="6"/>
<connect gate="G$1" pin="PO3" pad="7"/>
<connect gate="G$1" pin="PO4" pad="8"/>
<connect gate="G$1" pin="PO5" pad="9"/>
<connect gate="G$1" pin="PO6" pad="10"/>
<connect gate="G$1" pin="PO7" pad="11"/>
<connect gate="G$1" pin="SCL" pad="22"/>
<connect gate="G$1" pin="SDA" pad="23"/>
<connect gate="G$1" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEF4543">
<description>BCD to 7-seg decoder/driver
&lt;br&gt;
&lt;br&gt;
Not in catalog</description>
<gates>
<gate name="G$1" symbol="HEF4543"/>
</gates>
<devices>
<device name="PTH" package="DIP16">
<connects>
<connect gate="G$1" pin="A" pad="9"/>
<connect gate="G$1" pin="B" pad="10"/>
<connect gate="G$1" pin="BL" pad="7"/>
<connect gate="G$1" pin="C" pad="11"/>
<connect gate="G$1" pin="D" pad="12"/>
<connect gate="G$1" pin="D0" pad="5"/>
<connect gate="G$1" pin="D1" pad="3"/>
<connect gate="G$1" pin="D2" pad="2"/>
<connect gate="G$1" pin="D3" pad="4"/>
<connect gate="G$1" pin="E" pad="13"/>
<connect gate="G$1" pin="F" pad="15"/>
<connect gate="G$1" pin="G" pad="14"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="LD" pad="1"/>
<connect gate="G$1" pin="PH" pad="6"/>
<connect gate="G$1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EP2C8_PQ208">
<description>Altera Cyclone2 FPGA, PQFP-208
&lt;br&gt;
Not in catalog</description>
<gates>
<gate name="G$2" symbol="EP2C20_PQ208_PLL"/>
<gate name="G$6" symbol="EP2C20_PQ208_B3"/>
<gate name="G$4" symbol="EP2C20_PQ208_B1"/>
<gate name="G$3" symbol="EP2C20_PQ208_B4"/>
<gate name="G$7" symbol="EP2C20_PQ208_POWER"/>
<gate name="G$5" symbol="EP2C20_PQ208_B2"/>
<gate name="G$1" symbol="EP2C20_PQ208_CONFIG"/>
</gates>
<devices>
<device name="" package="PQFP208">
<connects>
<connect gate="G$1" pin="ASDO" pad="1"/>
<connect gate="G$1" pin="CLKUSR" pad="4"/>
<connect gate="G$1" pin="CONF_DONE" pad="123"/>
<connect gate="G$1" pin="CRC_ERROR" pad="3"/>
<connect gate="G$1" pin="DATA0" pad="20"/>
<connect gate="G$1" pin="DCLK" pad="21"/>
<connect gate="G$1" pin="DEV_OE" pad="56"/>
<connect gate="G$1" pin="INIT_DONE" pad="107"/>
<connect gate="G$1" pin="MSEL0" pad="126"/>
<connect gate="G$1" pin="MSEL1" pad="125"/>
<connect gate="G$1" pin="NCE" pad="22"/>
<connect gate="G$1" pin="NCEO" pad="108"/>
<connect gate="G$1" pin="NCONFIG" pad="26"/>
<connect gate="G$1" pin="NCSO" pad="2"/>
<connect gate="G$1" pin="NSTATUS" pad="121"/>
<connect gate="G$1" pin="TCK" pad="18"/>
<connect gate="G$1" pin="TDI" pad="19"/>
<connect gate="G$1" pin="TDO" pad="16"/>
<connect gate="G$1" pin="TMS" pad="17"/>
<connect gate="G$2" pin="GNDA_PLL1" pad="54"/>
<connect gate="G$2" pin="GNDA_PLL2" pad="158"/>
<connect gate="G$2" pin="GND_PLL1" pad="50"/>
<connect gate="G$2" pin="GND_PLL1@1" pad="52"/>
<connect gate="G$2" pin="GND_PLL2" pad="154"/>
<connect gate="G$2" pin="GND_PLL2@1" pad="156"/>
<connect gate="G$2" pin="VCCA_PLL1" pad="53"/>
<connect gate="G$2" pin="VCCA_PLL2" pad="157"/>
<connect gate="G$2" pin="VCCD_PLL1" pad="51"/>
<connect gate="G$2" pin="VCCD_PLL2" pad="155"/>
<connect gate="G$3" pin="IO@1" pad="80"/>
<connect gate="G$3" pin="IO@2" pad="96"/>
<connect gate="G$3" pin="IO_LVDS57N" pad="104"/>
<connect gate="G$3" pin="IO_LVDS57P" pad="103"/>
<connect gate="G$3" pin="IO_LVDS58N" pad="102"/>
<connect gate="G$3" pin="IO_LVDS58P" pad="101"/>
<connect gate="G$3" pin="IO_LVDS59N" pad="99"/>
<connect gate="G$3" pin="IO_LVDS59P" pad="97"/>
<connect gate="G$3" pin="IO_LVDS60N" pad="95"/>
<connect gate="G$3" pin="IO_LVDS60P" pad="94"/>
<connect gate="G$3" pin="IO_LVDS61N" pad="92"/>
<connect gate="G$3" pin="IO_LVDS61P" pad="90"/>
<connect gate="G$3" pin="IO_LVDS62N" pad="88"/>
<connect gate="G$3" pin="IO_LVDS62P" pad="87"/>
<connect gate="G$3" pin="IO_LVDS63N" pad="86"/>
<connect gate="G$3" pin="IO_LVDS63P" pad="84"/>
<connect gate="G$3" pin="IO_LVDS64N" pad="82"/>
<connect gate="G$3" pin="IO_LVDS64P" pad="81"/>
<connect gate="G$3" pin="IO_LVDS66N" pad="77"/>
<connect gate="G$3" pin="IO_LVDS66P" pad="76"/>
<connect gate="G$3" pin="IO_LVDS67N" pad="75"/>
<connect gate="G$3" pin="IO_LVDS67P" pad="74"/>
<connect gate="G$3" pin="IO_LVDS68N" pad="72"/>
<connect gate="G$3" pin="IO_LVDS68P" pad="70"/>
<connect gate="G$3" pin="IO_LVDS70N" pad="69"/>
<connect gate="G$3" pin="IO_LVDS70P" pad="68"/>
<connect gate="G$3" pin="IO_LVDS74N" pad="64"/>
<connect gate="G$3" pin="IO_LVDS74P" pad="63"/>
<connect gate="G$3" pin="IO_LVDS75N" pad="61"/>
<connect gate="G$3" pin="IO_LVDS75P" pad="60"/>
<connect gate="G$3" pin="IO_LVDS76N" pad="59"/>
<connect gate="G$3" pin="IO_LVDS76P" pad="58"/>
<connect gate="G$3" pin="IO_LVDS77P" pad="57"/>
<connect gate="G$3" pin="IO_VREFB4N0" pad="89"/>
<connect gate="G$3" pin="IO_VREFB4N1" pad="67"/>
<connect gate="G$3" pin="VCCIO4@1" pad="62"/>
<connect gate="G$3" pin="VCCIO4@2" pad="71"/>
<connect gate="G$3" pin="VCCIO4@3" pad="83"/>
<connect gate="G$3" pin="VCCIO4@4" pad="91"/>
<connect gate="G$3" pin="VCCIO4@5" pad="98"/>
<connect gate="G$4" pin="CLK0_LVDSCLK0P" pad="23"/>
<connect gate="G$4" pin="CLK1_LVDSCLK0N" pad="24"/>
<connect gate="G$4" pin="CLK2_LVDSCLK1P" pad="27"/>
<connect gate="G$4" pin="CLK3_LVDSCLK1N" pad="28"/>
<connect gate="G$4" pin="IO@2" pad="34"/>
<connect gate="G$4" pin="IO@3" pad="43"/>
<connect gate="G$4" pin="IO@4" pad="46"/>
<connect gate="G$4" pin="IO_LVDS0N" pad="45"/>
<connect gate="G$4" pin="IO_LVDS0P" pad="44"/>
<connect gate="G$4" pin="IO_LVDS12N" pad="12"/>
<connect gate="G$4" pin="IO_LVDS12P" pad="11"/>
<connect gate="G$4" pin="IO_LVDS13N" pad="10"/>
<connect gate="G$4" pin="IO_LVDS13P" pad="8"/>
<connect gate="G$4" pin="IO_LVDS14N" pad="6"/>
<connect gate="G$4" pin="IO_LVDS14P" pad="5"/>
<connect gate="G$4" pin="IO_LVDS2N" pad="41"/>
<connect gate="G$4" pin="IO_LVDS2P" pad="40"/>
<connect gate="G$4" pin="IO_LVDS3N" pad="39"/>
<connect gate="G$4" pin="IO_LVDS5P" pad="35"/>
<connect gate="G$4" pin="IO_LVDS6N" pad="33"/>
<connect gate="G$4" pin="IO_LVDS7N" pad="31"/>
<connect gate="G$4" pin="IO_LVDS7P" pad="30"/>
<connect gate="G$4" pin="IO_LVDS8N" pad="15"/>
<connect gate="G$4" pin="IO_LVDS8P" pad="14"/>
<connect gate="G$4" pin="IO_PLL1_OUTN" pad="48"/>
<connect gate="G$4" pin="IO_PLL1_OUTP" pad="47"/>
<connect gate="G$4" pin="IO_VREFB1N0" pad="13"/>
<connect gate="G$4" pin="IO_VREFB1N1" pad="37"/>
<connect gate="G$4" pin="VCCIO1@1" pad="7"/>
<connect gate="G$4" pin="VCCIO1@4" pad="29"/>
<connect gate="G$4" pin="VCCIO1@6" pad="42"/>
<connect gate="G$5" pin="IO_LVDS16N" pad="208"/>
<connect gate="G$5" pin="IO_LVDS16P" pad="207"/>
<connect gate="G$5" pin="IO_LVDS17N" pad="206"/>
<connect gate="G$5" pin="IO_LVDS17P" pad="205"/>
<connect gate="G$5" pin="IO_LVDS18N" pad="201"/>
<connect gate="G$5" pin="IO_LVDS18P" pad="203"/>
<connect gate="G$5" pin="IO_LVDS19N" pad="199"/>
<connect gate="G$5" pin="IO_LVDS19P" pad="200"/>
<connect gate="G$5" pin="IO_LVDS21N" pad="197"/>
<connect gate="G$5" pin="IO_LVDS21P" pad="198"/>
<connect gate="G$5" pin="IO_LVDS23N" pad="193"/>
<connect gate="G$5" pin="IO_LVDS23P" pad="195"/>
<connect gate="G$5" pin="IO_LVDS24N" pad="189"/>
<connect gate="G$5" pin="IO_LVDS24P" pad="191"/>
<connect gate="G$5" pin="IO_LVDS25N" pad="187"/>
<connect gate="G$5" pin="IO_LVDS25P" pad="188"/>
<connect gate="G$5" pin="IO_LVDS26P" pad="185"/>
<connect gate="G$5" pin="IO_LVDS28N" pad="181"/>
<connect gate="G$5" pin="IO_LVDS28P" pad="182"/>
<connect gate="G$5" pin="IO_LVDS29N" pad="179"/>
<connect gate="G$5" pin="IO_LVDS29P" pad="180"/>
<connect gate="G$5" pin="IO_LVDS31N" pad="175"/>
<connect gate="G$5" pin="IO_LVDS31P" pad="176"/>
<connect gate="G$5" pin="IO_LVDS33N" pad="171"/>
<connect gate="G$5" pin="IO_LVDS33P" pad="173"/>
<connect gate="G$5" pin="IO_LVDS34N" pad="168"/>
<connect gate="G$5" pin="IO_LVDS34P" pad="169"/>
<connect gate="G$5" pin="IO_LVDS35N" pad="164"/>
<connect gate="G$5" pin="IO_LVDS35P" pad="165"/>
<connect gate="G$5" pin="IO_LVDS36N" pad="162"/>
<connect gate="G$5" pin="IO_LVDS36P" pad="163"/>
<connect gate="G$5" pin="IO_LVDS37N" pad="160"/>
<connect gate="G$5" pin="IO_LVDS37P" pad="161"/>
<connect gate="G$5" pin="IO_VREFB2N0" pad="170"/>
<connect gate="G$5" pin="IO_VREFB2N1" pad="192"/>
<connect gate="G$5" pin="VCCIO2@1" pad="166"/>
<connect gate="G$5" pin="VCCIO2@2" pad="172"/>
<connect gate="G$5" pin="VCCIO2@3" pad="183"/>
<connect gate="G$5" pin="VCCIO2@4" pad="194"/>
<connect gate="G$5" pin="VCCIO2@5" pad="202"/>
<connect gate="G$6" pin="CLK4_LVDSCLK2P" pad="132"/>
<connect gate="G$6" pin="CLK5_LVDSCLK2N" pad="131"/>
<connect gate="G$6" pin="CLK6_LVDSCLK3P" pad="130"/>
<connect gate="G$6" pin="CLK7_LVDSCLK3N" pad="129"/>
<connect gate="G$6" pin="IO@1" pad="118"/>
<connect gate="G$6" pin="IO_LVDS38N" pad="149"/>
<connect gate="G$6" pin="IO_LVDS38P" pad="150"/>
<connect gate="G$6" pin="IO_LVDS39N" pad="146"/>
<connect gate="G$6" pin="IO_LVDS39P" pad="147"/>
<connect gate="G$6" pin="IO_LVDS42N" pad="143"/>
<connect gate="G$6" pin="IO_LVDS42P" pad="144"/>
<connect gate="G$6" pin="IO_LVDS44N" pad="141"/>
<connect gate="G$6" pin="IO_LVDS44P" pad="142"/>
<connect gate="G$6" pin="IO_LVDS45N" pad="138"/>
<connect gate="G$6" pin="IO_LVDS45P" pad="139"/>
<connect gate="G$6" pin="IO_LVDS46N" pad="135"/>
<connect gate="G$6" pin="IO_LVDS46P" pad="137"/>
<connect gate="G$6" pin="IO_LVDS47N" pad="133"/>
<connect gate="G$6" pin="IO_LVDS47P" pad="134"/>
<connect gate="G$6" pin="IO_LVDS48N" pad="127"/>
<connect gate="G$6" pin="IO_LVDS48P" pad="128"/>
<connect gate="G$6" pin="IO_LVDS51N" pad="115"/>
<connect gate="G$6" pin="IO_LVDS51P" pad="116"/>
<connect gate="G$6" pin="IO_LVDS52N" pad="113"/>
<connect gate="G$6" pin="IO_LVDS52P" pad="114"/>
<connect gate="G$6" pin="IO_LVDS53N" pad="110"/>
<connect gate="G$6" pin="IO_LVDS53P" pad="112"/>
<connect gate="G$6" pin="IO_LVDS56N" pad="105"/>
<connect gate="G$6" pin="IO_LVDS56P" pad="106"/>
<connect gate="G$6" pin="IO_PLL2_OUTN" pad="152"/>
<connect gate="G$6" pin="IO_PLL2_OUTP" pad="151"/>
<connect gate="G$6" pin="IO_VREFB3N0" pad="145"/>
<connect gate="G$6" pin="IO_VREFB3N1" pad="117"/>
<connect gate="G$6" pin="VCCIO3@1" pad="109"/>
<connect gate="G$6" pin="VCCIO3@2" pad="122"/>
<connect gate="G$6" pin="VCCIO3@3" pad="136"/>
<connect gate="G$6" pin="VCCIO3@4" pad="148"/>
<connect gate="G$7" pin="GND@1" pad="9"/>
<connect gate="G$7" pin="GND@10" pad="85"/>
<connect gate="G$7" pin="GND@11" pad="93"/>
<connect gate="G$7" pin="GND@12" pad="100"/>
<connect gate="G$7" pin="GND@13" pad="111"/>
<connect gate="G$7" pin="GND@14" pad="119"/>
<connect gate="G$7" pin="GND@15" pad="124"/>
<connect gate="G$7" pin="GND@16" pad="140"/>
<connect gate="G$7" pin="GND@17" pad="153"/>
<connect gate="G$7" pin="GND@18" pad="159"/>
<connect gate="G$7" pin="GND@19" pad="167"/>
<connect gate="G$7" pin="GND@2" pad="25"/>
<connect gate="G$7" pin="GND@20" pad="174"/>
<connect gate="G$7" pin="GND@21" pad="177"/>
<connect gate="G$7" pin="GND@22" pad="184"/>
<connect gate="G$7" pin="GND@23" pad="186"/>
<connect gate="G$7" pin="GND@24" pad="196"/>
<connect gate="G$7" pin="GND@25" pad="204"/>
<connect gate="G$7" pin="GND@3" pad="36"/>
<connect gate="G$7" pin="GND@4" pad="38"/>
<connect gate="G$7" pin="GND@5" pad="49"/>
<connect gate="G$7" pin="GND@6" pad="55"/>
<connect gate="G$7" pin="GND@7" pad="65"/>
<connect gate="G$7" pin="GND@8" pad="73"/>
<connect gate="G$7" pin="GND@9" pad="78"/>
<connect gate="G$7" pin="VCCINT@1" pad="32"/>
<connect gate="G$7" pin="VCCINT@2" pad="66"/>
<connect gate="G$7" pin="VCCINT@3" pad="79"/>
<connect gate="G$7" pin="VCCINT@4" pad="120"/>
<connect gate="G$7" pin="VCCINT@5" pad="178"/>
<connect gate="G$7" pin="VCCINT@6" pad="190"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="A6282" prefix="U">
<description>16-Channel Constant-Current LED Driver&lt;br&gt;
Packages: TSSOP-24, 24-pin QFN&lt;br&gt;
&lt;br&gt;
Last modified: 8/20/10&lt;br&gt;
&lt;B&gt;Unproven!&lt;/b&gt;&lt;br&gt;

RETIRED! (and wrong category)</description>
<gates>
<gate name="G$1" symbol="A6282"/>
</gates>
<devices>
<device name="-LP" package="TSSOP-24">
<connects>
<connect gate="G$1" pin="CLK" pad="3"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@2" pad="EP"/>
<connect gate="G$1" pin="LE" pad="4"/>
<connect gate="G$1" pin="OUT0" pad="5"/>
<connect gate="G$1" pin="OUT1" pad="6"/>
<connect gate="G$1" pin="OUT10" pad="15"/>
<connect gate="G$1" pin="OUT11" pad="16"/>
<connect gate="G$1" pin="OUT12" pad="17"/>
<connect gate="G$1" pin="OUT13" pad="18"/>
<connect gate="G$1" pin="OUT14" pad="19"/>
<connect gate="G$1" pin="OUT15" pad="20"/>
<connect gate="G$1" pin="OUT2" pad="7"/>
<connect gate="G$1" pin="OUT3" pad="8"/>
<connect gate="G$1" pin="OUT4" pad="9"/>
<connect gate="G$1" pin="OUT5" pad="10"/>
<connect gate="G$1" pin="OUT6" pad="11"/>
<connect gate="G$1" pin="OUT7" pad="12"/>
<connect gate="G$1" pin="OUT8" pad="13"/>
<connect gate="G$1" pin="OUT9" pad="14"/>
<connect gate="G$1" pin="REXT" pad="23"/>
<connect gate="G$1" pin="SDI" pad="2"/>
<connect gate="G$1" pin="SDO" pad="22"/>
<connect gate="G$1" pin="VDD" pad="24"/>
<connect gate="G$1" pin="~OE" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-ES" package="QFN-24_ALT2">
<connects>
<connect gate="G$1" pin="CLK" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="4"/>
<connect gate="G$1" pin="GND@2" pad="EP"/>
<connect gate="G$1" pin="LE" pad="7"/>
<connect gate="G$1" pin="OUT0" pad="8"/>
<connect gate="G$1" pin="OUT1" pad="9"/>
<connect gate="G$1" pin="OUT10" pad="18"/>
<connect gate="G$1" pin="OUT11" pad="19"/>
<connect gate="G$1" pin="OUT12" pad="20"/>
<connect gate="G$1" pin="OUT13" pad="21"/>
<connect gate="G$1" pin="OUT14" pad="22"/>
<connect gate="G$1" pin="OUT15" pad="23"/>
<connect gate="G$1" pin="OUT2" pad="10"/>
<connect gate="G$1" pin="OUT3" pad="11"/>
<connect gate="G$1" pin="OUT4" pad="12"/>
<connect gate="G$1" pin="OUT5" pad="13"/>
<connect gate="G$1" pin="OUT6" pad="14"/>
<connect gate="G$1" pin="OUT7" pad="15"/>
<connect gate="G$1" pin="OUT8" pad="16"/>
<connect gate="G$1" pin="OUT9" pad="17"/>
<connect gate="G$1" pin="REXT" pad="2"/>
<connect gate="G$1" pin="SDI" pad="5"/>
<connect gate="G$1" pin="SDO" pad="1"/>
<connect gate="G$1" pin="VDD" pad="3"/>
<connect gate="G$1" pin="~OE" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74HC03">
<description>&lt;B&gt;Quad 2-input open-drain NAND&lt;/B&gt;&lt;br&gt;
2-5V operating voltage&lt;br&gt;
Some part numbers may include a clamping diode from OD output to VCC; check datasheet for specific part.&lt;br&gt;
We use an NXP part which does NOT have a clamping diode.
&lt;br&gt;&lt;br&gt;
Doesn't seem to be in inventory anywhere.  We have nands but not open-drain</description>
<gates>
<gate name="G$1" symbol="74HC03"/>
</gates>
<devices>
<device name="" package="TSSOP14">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="4"/>
<connect gate="G$1" pin="A3" pad="9"/>
<connect gate="G$1" pin="A4" pad="12"/>
<connect gate="G$1" pin="B1" pad="2"/>
<connect gate="G$1" pin="B2" pad="5"/>
<connect gate="G$1" pin="B3" pad="10"/>
<connect gate="G$1" pin="B4" pad="13"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="VSS" pad="7"/>
<connect gate="G$1" pin="Y1" pad="3"/>
<connect gate="G$1" pin="Y2" pad="6"/>
<connect gate="G$1" pin="Y3" pad="8"/>
<connect gate="G$1" pin="Y4" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M74HC238">
<description>M74HC238 - CMOS 3 TO 8 LINE DECODER
&lt;br&gt;
&lt;br&gt;
RETIRED: IC-09771</description>
<gates>
<gate name="G$1" symbol="M74HC238"/>
</gates>
<devices>
<device name="" package="DIP16">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="G1" pad="6"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="VCC" pad="16"/>
<connect gate="G$1" pin="Y0" pad="15"/>
<connect gate="G$1" pin="Y1" pad="14"/>
<connect gate="G$1" pin="Y2" pad="13"/>
<connect gate="G$1" pin="Y3" pad="12"/>
<connect gate="G$1" pin="Y4" pad="11"/>
<connect gate="G$1" pin="Y5" pad="10"/>
<connect gate="G$1" pin="Y6" pad="9"/>
<connect gate="G$1" pin="Y7" pad="7"/>
<connect gate="G$1" pin="~G2A" pad="4"/>
<connect gate="G$1" pin="~G2B" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="0.75PF-50V(-/+.25PF)(0603)" prefix="C">
<description>CAP-07878</description>
<gates>
<gate name="G$1" symbol="CAP-1"/>
</gates>
<devices>
<device name="" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-07878"/>
<attribute name="VALUE" value="0.75pF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1.2PF-50V-20%(0603)" prefix="C">
<description>CAP-09201</description>
<gates>
<gate name="G$1" symbol="CAP-1"/>
</gates>
<devices>
<device name="" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-09201"/>
<attribute name="VALUE" value="1.2pF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="4.7NF-50V-10%(0603)" prefix="C">
<description>CAP-11378</description>
<gates>
<gate name="G$1" symbol="CAP-1"/>
</gates>
<devices>
<device name="" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-11378"/>
<attribute name="VALUE" value="4.7nF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="100UF6.3V20%(1210)" prefix="C" uservalue="yes">
<description>CAP-09827</description>
<gates>
<gate name="G$1" symbol="CAP-1"/>
</gates>
<devices>
<device name="" package="1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-09827"/>
<attribute name="VALUE" value="100uF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="330PF-25V-10%-(0603)" prefix="C" uservalue="yes">
<description>CAP-10108</description>
<gates>
<gate name="G$1" symbol="CAP-1"/>
</gates>
<devices>
<device name="" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CAP-10108"/>
<attribute name="VALUE" value="330pF"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2.2MOHM-1/10W-5%(0603)" prefix="R">
<description>RES-09288</description>
<gates>
<gate name="G$1" symbol="RESISTOR"/>
</gates>
<devices>
<device name="" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-09288"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="4.7OHM-1/10W-5%(0603)" prefix="R">
<description>RES-08295</description>
<gates>
<gate name="G$1" symbol="RESISTOR"/>
</gates>
<devices>
<device name="" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-08295"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="10.5KOHM1/10W1%(0603)" prefix="R">
<description>RES-09570</description>
<gates>
<gate name="G$1" symbol="RESISTOR"/>
</gates>
<devices>
<device name="" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-09570"/>
<attribute name="VALUE" value="10.5k"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ALPHANUMERIC" prefix="U">
<description>&lt;b&gt;Alphanumeric LED Display&lt;/b&gt; Common anode. Multiple LEDs on some segments. Multiple LED colors available. Works great with A6282 driver IC. Decimal points are unfornately not connected. SKU: COM-09933.</description>
<gates>
<gate name="G$1" symbol="ALPHANUMERIC"/>
</gates>
<devices>
<device name="PTH" package="ALPHANUMERIC">
<connects>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="22"/>
<connect gate="G$1" pin="B" pad="21"/>
<connect gate="G$1" pin="C" pad="16"/>
<connect gate="G$1" pin="D1" pad="10"/>
<connect gate="G$1" pin="D2" pad="14"/>
<connect gate="G$1" pin="E" pad="9"/>
<connect gate="G$1" pin="F" pad="4"/>
<connect gate="G$1" pin="G1" pad="7"/>
<connect gate="G$1" pin="G2" pad="19"/>
<connect gate="G$1" pin="H" pad="3"/>
<connect gate="G$1" pin="J" pad="24"/>
<connect gate="G$1" pin="K" pad="23"/>
<connect gate="G$1" pin="L" pad="15"/>
<connect gate="G$1" pin="M" pad="12"/>
<connect gate="G$1" pin="N" pad="11"/>
<connect gate="G$1" pin="NC@1" pad="1"/>
<connect gate="G$1" pin="NC@13" pad="13"/>
<connect gate="G$1" pin="VCC@18" pad="18"/>
<connect gate="G$1" pin="VCC@6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7-SEGMENT-DISPLAY">
<gates>
<gate name="G$1" symbol="7-SEGMENT-DISPLAY"/>
</gates>
<devices>
<device name="PTH" package="7-SEGMENT-DISPLAY">
<connects>
<connect gate="G$1" pin="A" pad="7"/>
<connect gate="G$1" pin="B" pad="6"/>
<connect gate="G$1" pin="C" pad="4"/>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="DP" pad="5"/>
<connect gate="G$1" pin="E" pad="1"/>
<connect gate="G$1" pin="F" pad="9"/>
<connect gate="G$1" pin="G" pad="10"/>
<connect gate="G$1" pin="G1" pad="3"/>
<connect gate="G$1" pin="G2" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7-SEGMENT-4DIGIT">
<gates>
<gate name="G$1" symbol="7-SEGMENT-4DIGIT"/>
</gates>
<devices>
<device name="PTH" package="7-SEGMENT-4DIGIT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="7-SEGMENT-4DIGIT-YOUNGSUN">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FOR_POGOBED_ONLY" package="7-SEGMENT-4DIGIT_LONGPADS_FOR_POGOBED">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP6291" prefix="U">
<description>Rail to rail OpAmp with 10MHz GBP&lt;br&gt;
&lt;br&gt;
Prototype: IC-11991&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="OP-AMP+-"/>
</gates>
<devices>
<device name="T-E/OT" package="SOT23-5">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11991"/>
<attribute name="VALUE" value="MCP6291T"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BATTERY" prefix="BT" uservalue="yes">
<description>&lt;h3&gt;Battery - Single Cell&lt;/h3&gt;
&lt;p&gt;A variety of battery chemistries, sizes, and footprints.&lt;/p&gt;
&lt;p&gt;Including AA, AAA, 18650 (PRT-12895), 20mm coin cell and 12mm coin cell.&lt;/p&gt;
20MM_4LEGS, BATT-10373</description>
<gates>
<gate name="G$1" symbol="BATTERY"/>
</gates>
<devices>
<device name="20PTH2" package="BATTERY">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="24.5MM" package="BATTCON_24.5MM">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1100" package="LIPO-1100MAH">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="AA-PANEL" package="BATTERY-AA-PANEL">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FOB" package="BATTERY_20MM_PTH_COMPACT">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LIPO-TABS" package="LIPO-110-TABS">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BUTTON-CONDUCTIVE">
<description>Used with rubber key pads. This one was designed and proven to work with the PolyCase Key FOB enclosures.</description>
<gates>
<gate name="G$1" symbol="BUTTON-CONDUCTIVE"/>
</gates>
<devices>
<device name="SMD-0.1&quot;" package="BUTTON-CONDUCTIVE-0.1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="BUTTON-CONDUCTIVE-MINI">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BUTTON-MAGNETIC">
<description>Magnetic metal snaps. 18mm is DEV-08682.</description>
<gates>
<gate name="G$1" symbol="SEWTAP"/>
</gates>
<devices>
<device name="10MM" package="BUTTON-10MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_SKU" value="DEV-08697"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAPSENSE_PAD" prefix="S">
<description>Generic copper pad for a capacitive touch sensor.</description>
<gates>
<gate name="G$1" symbol="CAPSENSE_PAD"/>
</gates>
<devices>
<device name="" package="CAPSENSE_PAD">
<connects>
<connect gate="G$1" pin="RECEIVE" pad="P$1"/>
<connect gate="G$1" pin="RES" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIP-02" prefix="S">
<description>SMD dip switch 2 positions</description>
<gates>
<gate name="G$1" symbol="2-POS-DIP"/>
</gates>
<devices>
<device name="02" package="DIPSWITCH-02">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$3" pad="3"/>
<connect gate="G$1" pin="P$4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIP-08" prefix="SW" uservalue="yes">
<description>&lt;b&gt;DIP Switch 8 Position&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="SW_DIP-8"/>
</gates>
<devices>
<device name="-SMT-HALFSIZE" package="DIPSWITCH-08-50MIL">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FKIT-COIN_CELL" prefix="BATT">
<description>&lt;h3&gt;Fabrick.it Coin Cell Holder&lt;/h3&gt;
Coin cell holder for 24.5mm rechargable coin cell</description>
<gates>
<gate name="G$1" symbol="FKIT-BATTERY"/>
</gates>
<devices>
<device name="LIR2450-H" package="FKIT-LIR2450-H">
<connects>
<connect gate="G$1" pin="NEG" pad="NEG"/>
<connect gate="G$1" pin="POS" pad="POS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FKIT-RIBBON_CONNECTOR" prefix="J">
<description>&lt;h3&gt;fabrick.it Conductive Ribbon Connector&lt;/h3&gt;</description>
<gates>
<gate name="G$1" symbol="FKIT-CONNECTOR_COND_03"/>
</gates>
<devices>
<device name="-2MM_L_REV2" package="FKIT-RIBBON_CONNECTOR_03_2MM_L">
<connects>
<connect gate="G$1" pin="P$1" pad="P1A"/>
<connect gate="G$1" pin="P$2" pad="P2A"/>
<connect gate="G$1" pin="P$3" pad="P3A"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-2MM_R_REV2" package="FKIT-RIBBON_CONNECTOR_03_2MM_R">
<connects>
<connect gate="G$1" pin="P$1" pad="P1A"/>
<connect gate="G$1" pin="P$2" pad="P2A"/>
<connect gate="G$1" pin="P$3" pad="P3A"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FKIT-SNAP_CONNECTOR">
<description>Snap connector for Fabrick.it products</description>
<gates>
<gate name="G$1" symbol="FKIT-SNAP_CONNECTOR"/>
</gates>
<devices>
<device name="-FEMALE" package="FKIT-SNAP_FEMALE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MALE" package="FKIT-SNAP_MALE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G3VM-61E1">
<description>Omron NO solid state relay</description>
<gates>
<gate name="G$1" symbol="G3VM-61E1"/>
</gates>
<devices>
<device name="" package="G3VM-61E1">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
<connect gate="G$1" pin="P$3" pad="P$3"/>
<connect gate="G$1" pin="P$4" pad="P$4"/>
<connect gate="G$1" pin="P$5" pad="P$5"/>
<connect gate="G$1" pin="P$6" pad="P$6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-08720"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HEATSINK-SMD-2" prefix="HS">
<description>Aavid/Thermaloy Surface-Mount Heat Sinks&lt;p&gt;
&lt;a href="http://media.digikey.com/pdf/Data%20Sheets/Aavid%20Thermal%20Technologies%20PDFs/Surface%20Mount%20Heat%20Sinks.pdf"&gt;Datasheet&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="HEATSINK-SMD-2"/>
</gates>
<devices>
<device name="-AAVID_573400" package="AAVID_573400">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-12096"/>
<attribute name="VALUE" value="HEATSINK"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="N35P112" prefix="U" uservalue="yes">
<description>Hall-effect based I2C analog mini-joystick with button</description>
<gates>
<gate name="G$1" symbol="N35P112"/>
</gates>
<devices>
<device name="" package="N35P112">
<connects>
<connect gate="G$1" pin="ADDR" pad="9"/>
<connect gate="G$1" pin="GND1" pad="3"/>
<connect gate="G$1" pin="GND2" pad="10"/>
<connect gate="G$1" pin="GND3" pad="11"/>
<connect gate="G$1" pin="GND4" pad="12"/>
<connect gate="G$1" pin="GND5" pad="13"/>
<connect gate="G$1" pin="INTN" pad="7"/>
<connect gate="G$1" pin="RESETN" pad="6"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="SWITCHN" pad="8"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VDDP" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-10635"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="POT" prefix="RV" uservalue="yes">
<gates>
<gate name="G$1" symbol="POT"/>
</gates>
<devices>
<device name="TRIM" package="TRIM_POT">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
<connect gate="G$1" pin="S" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COM-00104"/>
</technology>
</technologies>
</device>
<device name="100K_3362U" package="3362U">
<connects>
<connect gate="G$1" pin="A" pad="P$3"/>
<connect gate="G$1" pin="E" pad="P$1"/>
<connect gate="G$1" pin="S" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-08876"/>
<attribute name="SF_SKU" value="COM-08647"/>
</technology>
</technologies>
</device>
<device name="-RV16AF-20" package="POT_ALPHA_RV16AF-20">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-10002"/>
</technology>
</technologies>
</device>
<device name="MAM" package="POT_MAMMOTH">
<connects>
<connect gate="G$1" pin="A" pad="P$2"/>
<connect gate="G$1" pin="E" pad="P$3"/>
<connect gate="G$1" pin="S" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="POT_SWITCH" prefix="U" uservalue="yes">
<description>Potentiometer w/ switch.</description>
<gates>
<gate name="G$1" symbol="POT"/>
<gate name="G$2" symbol="SWITCH-MOMENTARY-2-1"/>
</gates>
<devices>
<device name="POT_PTH" package="POT_PTH">
<connects>
<connect gate="G$1" pin="A" pad="E@1"/>
<connect gate="G$1" pin="E" pad="E@2"/>
<connect gate="G$1" pin="S" pad="WAND"/>
<connect gate="G$2" pin="1" pad="S1"/>
<connect gate="G$2" pin="2" pad="S2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RELAY-SOLIDSTATE" prefix="U">
<description>SPST SS relay</description>
<gates>
<gate name="G$1" symbol="RELAY-SOLIDSTATE"/>
</gates>
<devices>
<device name="PTH" package="RELAY-S108T02">
<connects>
<connect gate="G$1" pin="+" pad="3"/>
<connect gate="G$1" pin="-" pad="4"/>
<connect gate="G$1" pin="T1" pad="1"/>
<connect gate="G$1" pin="T2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-10481"/>
<attribute name="SF_SKU" value="COM-10636"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RELAY-SPDT" prefix="K">
<description>SPDT relay (COM-00101)</description>
<gates>
<gate name="K$1" symbol="RELAY-SPDT"/>
</gates>
<devices>
<device name="-G5Q-1A" package="RELAY-G5Q">
<connects>
<connect gate="K$1" pin="COIL1" pad="5"/>
<connect gate="K$1" pin="COIL2" pad="1"/>
<connect gate="K$1" pin="MAIN" pad="2"/>
<connect gate="K$1" pin="NC" pad="4"/>
<connect gate="K$1" pin="NO" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH2" package="RELAY-T9A">
<connects>
<connect gate="K$1" pin="COIL1" pad="COIL1"/>
<connect gate="K$1" pin="COIL2" pad="COIL2"/>
<connect gate="K$1" pin="MAIN" pad="MAIN"/>
<connect gate="K$1" pin="NC" pad="NC"/>
<connect gate="K$1" pin="NO" pad="NO"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH3" package="RELAY-T9A-2">
<connects>
<connect gate="K$1" pin="COIL1" pad="COIL1"/>
<connect gate="K$1" pin="COIL2" pad="COIL2"/>
<connect gate="K$1" pin="MAIN" pad="MAIN"/>
<connect gate="K$1" pin="NC" pad="NC"/>
<connect gate="K$1" pin="NO" pad="NO"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-10736"/>
<attribute name="SF_SKU" value="COM-10924"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RELAY-SPDT-2">
<description>&lt;h3&gt;SPDT Relay w/ Two Common Terminals&lt;/h3&gt;
SPDT relay (COM-00100)</description>
<gates>
<gate name="G$1" symbol="RELAY-SPDT-2"/>
</gates>
<devices>
<device name="-G5V" package="RELAY-G5V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_SKU" value="COM-00524"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH-4PDT">
<description>For use with a push-button switch made by CnK components.</description>
<gates>
<gate name="G$1" symbol="SWITCH-4PDT"/>
</gates>
<devices>
<device name="CNK_LOCK" package="SWITCH-4PDT-CNK">
<connects>
<connect gate="G$1" pin="1" pad="PP$1"/>
<connect gate="G$1" pin="10" pad="PP$10"/>
<connect gate="G$1" pin="11" pad="PP$11"/>
<connect gate="G$1" pin="12" pad="PP$12"/>
<connect gate="G$1" pin="2" pad="PP$2"/>
<connect gate="G$1" pin="3" pad="PP$3"/>
<connect gate="G$1" pin="4" pad="PP$4"/>
<connect gate="G$1" pin="5" pad="PP$5"/>
<connect gate="G$1" pin="6" pad="PP$6"/>
<connect gate="G$1" pin="7" pad="PP$7"/>
<connect gate="G$1" pin="8" pad="PP$8"/>
<connect gate="G$1" pin="9" pad="PP$9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-09564"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH-DPDT" prefix="S" uservalue="yes">
<description>DPDT Version of the COM-00597</description>
<gates>
<gate name="G$1" symbol="AYZ0202"/>
</gates>
<devices>
<device name="PTH" package="MSS22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-09244"/>
</technology>
</technologies>
</device>
<device name="PTH1" package="MS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_SKU" value="COM-11139"/>
</technology>
</technologies>
</device>
<device name="ES" package="ES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="OS" package="OS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EG2211" package="EG2211">
<connects>
<connect gate="G$1" pin="1" pad="P1-TA"/>
<connect gate="G$1" pin="2" pad="P1"/>
<connect gate="G$1" pin="3" pad="P1-TB"/>
<connect gate="G$1" pin="4" pad="P2-TA"/>
<connect gate="G$1" pin="5" pad="P2"/>
<connect gate="G$1" pin="6" pad="P2-TB"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="STOMP-PTH" package="STOMP-SWITCH-DPDT">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
<connect gate="G$1" pin="3" pad="P$3"/>
<connect gate="G$1" pin="4" pad="P$4"/>
<connect gate="G$1" pin="5" pad="P$5"/>
<connect gate="G$1" pin="6" pad="P$6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-12340"/>
<attribute name="SF_SKU" value="COM-11151"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH-MOMENTARY-2-CLOSED" prefix="S">
<description>Closed Switch for tutorial schematics.  Not intended for PCB design.

Maps to 12mm tact switch, only because eagle won't place a part with no package defined.

The ordinary SWITCH-MOMENTARY-2 is likely to be more useful for regular schematics.</description>
<gates>
<gate name="G$1" symbol="SWITCH-MOMENTARY-2-CLOSED"/>
</gates>
<devices>
<device name="" package="TACTILE-PTH-12MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH-MOMENTARY-SPST" prefix="S">
<description>Various NO switches- pushbuttons, reed, etc</description>
<gates>
<gate name="G$1" symbol="SWITCH-MOMENTARY-2"/>
</gates>
<devices>
<device name="SMD-3" package="TACTILE_SWITCH_SMD-3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH-SPDT" prefix="S" uservalue="yes">
<description>&lt;b&gt;SPDT Switch&lt;/b&gt;&lt;br&gt;
Simple slide switch, Spark Fun Electronics SKU : COM-00102&lt;br&gt;
DPDT SMT slide switch, AYZ0202, SWCH-08179</description>
<gates>
<gate name="1" symbol="TOGGLE"/>
</gates>
<devices>
<device name="PTH2" package="SWITCH-DPDT">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH3" package="R_SW_TH">
<connects>
<connect gate="1" pin="O" pad="P$1"/>
<connect gate="1" pin="P" pad="P$2"/>
<connect gate="1" pin="S" pad="P$3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="SWITCH_SPDT_SMD">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH-SPST-2">
<gates>
<gate name="G$1" symbol="SPST"/>
</gates>
<devices>
<device name="RA" package="R_SW_TH">
<connects>
<connect gate="G$1" pin="O" pad="P$3"/>
<connect gate="G$1" pin="P" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TV" package="SWITCH-SPST-VERTICAL">
<connects>
<connect gate="G$1" pin="O" pad="1"/>
<connect gate="G$1" pin="P" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH_SPDT">
<description>SWCH-10651

Side-actuated SPDT slide switch, as used on the Arduino Pro</description>
<gates>
<gate name="G$1" symbol="SW_SPDT"/>
</gates>
<devices>
<device name="" package="KPS-1290">
<connects>
<connect gate="G$1" pin="O" pad="O"/>
<connect gate="G$1" pin="P" pad="P"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-10651"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TURRET-1520" uservalue="yes">
<description>Turret FP for Keystone Electronics Part#1520</description>
<gates>
<gate name="G$1" symbol="TURRET"/>
</gates>
<devices>
<device name="PTH" package="1X01_TURRET">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09156"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRIMPOT" prefix="R" uservalue="yes">
<description>Various small potentiometers for "set-and-forget" applications</description>
<gates>
<gate name="R?" symbol="TRIMPOT-1"/>
</gates>
<devices>
<device name="-2" package="TRIMPOT_TC33">
<connects>
<connect gate="R?" pin="CCW" pad="1"/>
<connect gate="R?" pin="CW" pad="3"/>
<connect gate="R?" pin="WIPER" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3362U-2" package="3362U-2">
<connects>
<connect gate="R?" pin="CCW" pad="1"/>
<connect gate="R?" pin="CW" pad="3"/>
<connect gate="R?" pin="WIPER" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-08876"/>
</technology>
</technologies>
</device>
<device name="PTH" package="TRIM_POT_PTH">
<connects>
<connect gate="R?" pin="CCW" pad="1"/>
<connect gate="R?" pin="CW" pad="3"/>
<connect gate="R?" pin="WIPER" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-08445"/>
</technology>
</technologies>
</device>
<device name="-SMD" package="TRIMPOT-3MM">
<connects>
<connect gate="R?" pin="CCW" pad="1"/>
<connect gate="R?" pin="CW" pad="3"/>
<connect gate="R?" pin="WIPER" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-08048"/>
<attribute name="VALUE" value="10k"/>
</technology>
</technologies>
</device>
<device name="TRIMPOT-5MM" package="TRIMPOT-5MM">
<connects>
<connect gate="R?" pin="CCW" pad="A"/>
<connect gate="R?" pin="CW" pad="C"/>
<connect gate="R?" pin="WIPER" pad="B"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-11156"/>
<attribute name="VALUE" value="5k"/>
</technology>
</technologies>
</device>
<device name="TRIMPOT_PTH_S3_LOCK" package="TRIMPOT_PTH_S3_LOCK">
<connects>
<connect gate="R?" pin="CCW" pad="1"/>
<connect gate="R?" pin="CW" pad="3"/>
<connect gate="R?" pin="WIPER" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="TRIMPOT-5MM-V2">
<connects>
<connect gate="R?" pin="CCW" pad="A"/>
<connect gate="R?" pin="CW" pad="C"/>
<connect gate="R?" pin="WIPER" pad="B"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SMARTCARD" prefix="J">
<description>Smart card socket- PRT-09368</description>
<gates>
<gate name="G$1" symbol="SMARTCARD"/>
</gates>
<devices>
<device name="SMD" package="SMARTCARD">
<connects>
<connect gate="G$1" pin="C4" pad="C4"/>
<connect gate="G$1" pin="C8" pad="C8"/>
<connect gate="G$1" pin="CLK" pad="C3"/>
<connect gate="G$1" pin="GND" pad="C5"/>
<connect gate="G$1" pin="I/O" pad="C7"/>
<connect gate="G$1" pin="RST" pad="C2"/>
<connect gate="G$1" pin="SW1" pad="P1"/>
<connect gate="G$1" pin="SW2" pad="P2"/>
<connect gate="G$1" pin="VCC" pad="C1"/>
<connect gate="G$1" pin="VPP" pad="C6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SMA_EDGE" prefix="J$">
<description>&lt;b&gt;SMA Antenna Connector&lt;/b&gt;
End launch SMA connector. The paste layer has been removed so that the connector can be hand soldered onto the board after reflow.</description>
<gates>
<gate name="1" symbol="SMA_EDGE"/>
</gates>
<devices>
<device name="" package="SMA-EDGE">
<connects>
<connect gate="1" pin="GND@0" pad="GND@0"/>
<connect gate="1" pin="GND@1" pad="GND@1"/>
<connect gate="1" pin="GND@2" pad="GND@2"/>
<connect gate="1" pin="GND@3" pad="GND@3"/>
<connect gate="1" pin="SIGNAL" pad="SIG"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TOUCH-SCREEN">
<description>Nintendo DS touch screen connector LCD-09105</description>
<gates>
<gate name="G$1" symbol="TOUCH-SCREEN"/>
</gates>
<devices>
<device name="" package="TOUCH-SCREEN">
<connects>
<connect gate="G$1" pin="TS1" pad="P$4"/>
<connect gate="G$1" pin="TS2" pad="P$3"/>
<connect gate="G$1" pin="TS3" pad="P$2"/>
<connect gate="G$1" pin="TS4" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ZIFSOCKET-40-6">
<description>Lever-action ZIF socket for 40-pin ICs</description>
<gates>
<gate name="G$1" symbol="DIL-40-6"/>
</gates>
<devices>
<device name="DIL40-6-ZIF_SOCKET" package="DIL40-6-ZIF_SOCKET">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$10" pad="10"/>
<connect gate="G$1" pin="P$11" pad="11"/>
<connect gate="G$1" pin="P$12" pad="12"/>
<connect gate="G$1" pin="P$13" pad="13"/>
<connect gate="G$1" pin="P$14" pad="14"/>
<connect gate="G$1" pin="P$15" pad="15"/>
<connect gate="G$1" pin="P$16" pad="16"/>
<connect gate="G$1" pin="P$17" pad="17"/>
<connect gate="G$1" pin="P$18" pad="18"/>
<connect gate="G$1" pin="P$19" pad="19"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$20" pad="20"/>
<connect gate="G$1" pin="P$21" pad="21"/>
<connect gate="G$1" pin="P$22" pad="22"/>
<connect gate="G$1" pin="P$23" pad="23"/>
<connect gate="G$1" pin="P$24" pad="24"/>
<connect gate="G$1" pin="P$25" pad="25"/>
<connect gate="G$1" pin="P$26" pad="26"/>
<connect gate="G$1" pin="P$27" pad="27"/>
<connect gate="G$1" pin="P$28" pad="28"/>
<connect gate="G$1" pin="P$29" pad="29"/>
<connect gate="G$1" pin="P$3" pad="3"/>
<connect gate="G$1" pin="P$30" pad="30"/>
<connect gate="G$1" pin="P$31" pad="31"/>
<connect gate="G$1" pin="P$32" pad="32"/>
<connect gate="G$1" pin="P$33" pad="33"/>
<connect gate="G$1" pin="P$34" pad="34"/>
<connect gate="G$1" pin="P$35" pad="35"/>
<connect gate="G$1" pin="P$36" pad="36"/>
<connect gate="G$1" pin="P$37" pad="37"/>
<connect gate="G$1" pin="P$38" pad="38"/>
<connect gate="G$1" pin="P$39" pad="39"/>
<connect gate="G$1" pin="P$4" pad="4"/>
<connect gate="G$1" pin="P$40" pad="40"/>
<connect gate="G$1" pin="P$5" pad="5"/>
<connect gate="G$1" pin="P$6" pad="6"/>
<connect gate="G$1" pin="P$7" pad="7"/>
<connect gate="G$1" pin="P$8" pad="8"/>
<connect gate="G$1" pin="P$9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ZUNE_CONNECTOR_MALE">
<description>Male connector for the Zune media player.  UNPROVEN FOOTPRINT!  This connector must be used only with a 1.2mm PCB thickness.</description>
<gates>
<gate name="G$1" symbol="ZUNE_CONNECTOR_MALE"/>
</gates>
<devices>
<device name="" package="ZUNE_CONNECTOR_MALE">
<connects>
<connect gate="G$1" pin="10" pad="P$10"/>
<connect gate="G$1" pin="11" pad="P$11"/>
<connect gate="G$1" pin="12" pad="P$12"/>
<connect gate="G$1" pin="15" pad="P$15"/>
<connect gate="G$1" pin="16" pad="P$16"/>
<connect gate="G$1" pin="17" pad="P$17"/>
<connect gate="G$1" pin="18" pad="P$18"/>
<connect gate="G$1" pin="4" pad="P$4"/>
<connect gate="G$1" pin="5" pad="P$5"/>
<connect gate="G$1" pin="6" pad="P$6"/>
<connect gate="G$1" pin="7" pad="P$7"/>
<connect gate="G$1" pin="8" pad="P$8"/>
<connect gate="G$1" pin="AUDIO_L" pad="P$13"/>
<connect gate="G$1" pin="AUDIO_R" pad="P$14"/>
<connect gate="G$1" pin="GND@19" pad="P$19"/>
<connect gate="G$1" pin="GND@22" pad="P$22"/>
<connect gate="G$1" pin="GND@23" pad="P$23"/>
<connect gate="G$1" pin="GND@24" pad="P$24"/>
<connect gate="G$1" pin="USB_5V@1" pad="P$1"/>
<connect gate="G$1" pin="USB_5V@2" pad="P$2"/>
<connect gate="G$1" pin="USB_5V@3" pad="P$3"/>
<connect gate="G$1" pin="USB_DATA+" pad="P$21"/>
<connect gate="G$1" pin="USB_DATA-" pad="P$20"/>
<connect gate="G$1" pin="VIDEO+" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA8U2" prefix="U">
<description>&lt;h3&gt;Atmel 32-pin 8-bit Microcontroller with 8/16/32K Bystes of ISP Flash and USB Controller. ATmega8U2, ATmega16U2, and ATmega32U2&lt;/h3&gt;
&lt;p&gt;&lt;a href=""&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13703"&gt;Storefront component: ATMEGA8U2-AU&lt;/a&gt; (COM-13703)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="ATMEGA8U2"/>
</gates>
<devices>
<device name="AU" package="TQFP32-08_MCU">
<connects>
<connect gate="G$1" pin="AVCC" pad="32"/>
<connect gate="G$1" pin="D+" pad="29"/>
<connect gate="G$1" pin="D-" pad="30"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="PB0" pad="14"/>
<connect gate="G$1" pin="PB1(SCK)" pad="15"/>
<connect gate="G$1" pin="PB2(MOSI)" pad="16"/>
<connect gate="G$1" pin="PB3(MISO)" pad="17"/>
<connect gate="G$1" pin="PB4" pad="18"/>
<connect gate="G$1" pin="PB5" pad="19"/>
<connect gate="G$1" pin="PB6" pad="20"/>
<connect gate="G$1" pin="PB7" pad="21"/>
<connect gate="G$1" pin="PC2" pad="5"/>
<connect gate="G$1" pin="PC4" pad="26"/>
<connect gate="G$1" pin="PC5" pad="25"/>
<connect gate="G$1" pin="PC6" pad="23"/>
<connect gate="G$1" pin="PC7" pad="22"/>
<connect gate="G$1" pin="PD0" pad="6"/>
<connect gate="G$1" pin="PD1" pad="7"/>
<connect gate="G$1" pin="PD2(RX)" pad="8"/>
<connect gate="G$1" pin="PD3(TX)" pad="9"/>
<connect gate="G$1" pin="PD4" pad="10"/>
<connect gate="G$1" pin="PD5" pad="11"/>
<connect gate="G$1" pin="PD6(RTS)" pad="12"/>
<connect gate="G$1" pin="PD7(CTS)" pad="13"/>
<connect gate="G$1" pin="RESET/PC1" pad="24"/>
<connect gate="G$1" pin="UCAP" pad="27"/>
<connect gate="G$1" pin="UGND" pad="28"/>
<connect gate="G$1" pin="UVCC" pad="31"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="XTAL1" pad="1"/>
<connect gate="G$1" pin="XTAL2/PC0" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-10104"/>
<attribute name="VALUE" value="8U2-AU"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY13">
<description>&lt;h3&gt;ATTINY13&lt;/h3&gt;
&lt;p&gt;Retired&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ATTINY13"/>
</gates>
<devices>
<device name="SOIC" package="SO08_MCU">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB0(MOSI)" pad="5"/>
<connect gate="G$1" pin="PB1(MISO)" pad="6"/>
<connect gate="G$1" pin="PB2(SCK/ADC1)" pad="7"/>
<connect gate="G$1" pin="PB3(ADC3)" pad="2"/>
<connect gate="G$1" pin="PB4(ADC2)" pad="3"/>
<connect gate="G$1" pin="PB5(NRES)" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DIP" package="DIP08_MCU">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB0(MOSI)" pad="5"/>
<connect gate="G$1" pin="PB1(MISO)" pad="6"/>
<connect gate="G$1" pin="PB2(SCK/ADC1)" pad="7"/>
<connect gate="G$1" pin="PB3(ADC3)" pad="2"/>
<connect gate="G$1" pin="PB4(ADC2)" pad="3"/>
<connect gate="G$1" pin="PB5(NRES)" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY24">
<description>&lt;h3&gt;Atmel 20-pin 2kB flash uC&lt;/h3&gt;
&lt;p&gt;Retired&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ATTINY24"/>
</gates>
<devices>
<device name="QFN" package="QFN20_MCU">
<connects>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="GND@0" pad="0"/>
<connect gate="G$1" pin="PA0/ADC0" pad="5"/>
<connect gate="G$1" pin="PA1/ADC1" pad="4"/>
<connect gate="G$1" pin="PA2/ADC2" pad="3"/>
<connect gate="G$1" pin="PA3/ADC3" pad="2"/>
<connect gate="G$1" pin="PA4/SCL" pad="1"/>
<connect gate="G$1" pin="PA5/MISO" pad="20"/>
<connect gate="G$1" pin="PA6/MOSI" pad="16"/>
<connect gate="G$1" pin="PA7/ADC7" pad="15"/>
<connect gate="G$1" pin="PB0" pad="11"/>
<connect gate="G$1" pin="PB1" pad="12"/>
<connect gate="G$1" pin="PB2" pad="14"/>
<connect gate="G$1" pin="PB3/RESET" pad="13"/>
<connect gate="G$1" pin="VCC" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY45" prefix="U" uservalue="yes">
<description>&lt;h3&gt;Atmel 8-pin 2/4/8kB flash uC&lt;/h3&gt;
&lt;p&gt;Retired&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ATTINY13"/>
</gates>
<devices>
<device name="TINY45-20-SMT" package="SO08-EIAJ_MCU">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB0(MOSI)" pad="5"/>
<connect gate="G$1" pin="PB1(MISO)" pad="6"/>
<connect gate="G$1" pin="PB2(SCK/ADC1)" pad="7"/>
<connect gate="G$1" pin="PB3(ADC3)" pad="2"/>
<connect gate="G$1" pin="PB4(ADC2)" pad="3"/>
<connect gate="G$1" pin="PB5(NRES)" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-08922"/>
<attribute name="VALUE" value="Tiny45-20-SMT"/>
</technology>
</technologies>
</device>
<device name="TINY45-20-DIP" package="DIP08_MCU">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB0(MOSI)" pad="5"/>
<connect gate="G$1" pin="PB1(MISO)" pad="6"/>
<connect gate="G$1" pin="PB2(SCK/ADC1)" pad="7"/>
<connect gate="G$1" pin="PB3(ADC3)" pad="2"/>
<connect gate="G$1" pin="PB4(ADC2)" pad="3"/>
<connect gate="G$1" pin="PB5(NRES)" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09439"/>
<attribute name="VALUE" value="TINY45-20-DIP"/>
</technology>
</technologies>
</device>
<device name="TINY85-20-DIP" package="DIP08_MCU">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB0(MOSI)" pad="5"/>
<connect gate="G$1" pin="PB1(MISO)" pad="6"/>
<connect gate="G$1" pin="PB2(SCK/ADC1)" pad="7"/>
<connect gate="G$1" pin="PB3(ADC3)" pad="2"/>
<connect gate="G$1" pin="PB4(ADC2)" pad="3"/>
<connect gate="G$1" pin="PB5(NRES)" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09445"/>
<attribute name="VALUE" value="TINY85-20-DIP"/>
</technology>
</technologies>
</device>
<device name="TINY85-20-SMT" package="SO08-EIAJ_MCU">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB0(MOSI)" pad="5"/>
<connect gate="G$1" pin="PB1(MISO)" pad="6"/>
<connect gate="G$1" pin="PB2(SCK/ADC1)" pad="7"/>
<connect gate="G$1" pin="PB3(ADC3)" pad="2"/>
<connect gate="G$1" pin="PB4(ADC2)" pad="3"/>
<connect gate="G$1" pin="PB5(NRES)" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09092"/>
<attribute name="VALUE" value="Tiny85-20-SMT"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AVR-MEGA8" prefix="U$">
<description>&lt;h3&gt;MCU&lt;/h3&gt;
&lt;p&gt;8 Kbytes FLASH&lt;br&gt;
1 kbytes SRAM&lt;br&gt;
512 bytes EEPROM&lt;br&gt;
USART&lt;br&gt;
6-channel 10 bit ADC&lt;br&gt;
2-channel 8 bit ADC
&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;None.&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="23-I/O"/>
</gates>
<devices>
<device name="-MI" package="MLF32_MCU">
<connects>
<connect gate="G$1" pin="ADC6" pad="19"/>
<connect gate="G$1" pin="ADC7" pad="22"/>
<connect gate="G$1" pin="AGND" pad="21"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="PB0(ICP)" pad="12"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="13"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="14"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="15"/>
<connect gate="G$1" pin="PB4(MISO)" pad="16"/>
<connect gate="G$1" pin="PB5(SCK)" pad="17"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="7"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="8"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="29"/>
<connect gate="G$1" pin="PD0(RXD)" pad="30"/>
<connect gate="G$1" pin="PD1(TXD)" pad="31"/>
<connect gate="G$1" pin="PD2(INT0)" pad="32"/>
<connect gate="G$1" pin="PD3(INT1)" pad="1"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="2"/>
<connect gate="G$1" pin="PD5(T1)" pad="9"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="10"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="11"/>
<connect gate="G$1" pin="VCC@1" pad="4"/>
<connect gate="G$1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-AI" package="TQFP32-08_MCU">
<connects>
<connect gate="G$1" pin="ADC6" pad="19"/>
<connect gate="G$1" pin="ADC7" pad="22"/>
<connect gate="G$1" pin="AGND" pad="21"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="PB0(ICP)" pad="12"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="13"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="14"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="15"/>
<connect gate="G$1" pin="PB4(MISO)" pad="16"/>
<connect gate="G$1" pin="PB5(SCK)" pad="17"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="7"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="8"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="29"/>
<connect gate="G$1" pin="PD0(RXD)" pad="30"/>
<connect gate="G$1" pin="PD1(TXD)" pad="31"/>
<connect gate="G$1" pin="PD2(INT0)" pad="32"/>
<connect gate="G$1" pin="PD3(INT1)" pad="1"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="2"/>
<connect gate="G$1" pin="PD5(T1)" pad="9"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="10"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="11"/>
<connect gate="G$1" pin="VCC@1" pad="4"/>
<connect gate="G$1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AVR-MEGA8-P" prefix="IC">
<description>&lt;h3&gt;MCU&lt;/h3&gt;
&lt;p&gt;8 Kbytes FLASH&lt;br&gt;
1 kbytes SRAM&lt;br&gt;
512 bytes EEPROM&lt;br&gt;
USART&lt;br&gt;
6-channel 10 bit ADC&lt;br&gt;
2-channel 8 bit ADC
&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;None.&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="23-I/O-2"/>
</gates>
<devices>
<device name="PTH" package="DIP28_MCU">
<connects>
<connect gate="G$1" pin="AGND" pad="22"/>
<connect gate="G$1" pin="AREF" pad="21"/>
<connect gate="G$1" pin="AVCC" pad="20"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="PB0(ICP)" pad="14"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="15"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="16"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="17"/>
<connect gate="G$1" pin="PB4(MISO)" pad="18"/>
<connect gate="G$1" pin="PB5(SCK)" pad="19"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="9"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="10"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="1"/>
<connect gate="G$1" pin="PD0(RXD)" pad="2"/>
<connect gate="G$1" pin="PD1(TXD)" pad="3"/>
<connect gate="G$1" pin="PD2(INT0)" pad="4"/>
<connect gate="G$1" pin="PD3(INT1)" pad="5"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="6"/>
<connect gate="G$1" pin="PD5(T1)" pad="11"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="12"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="13"/>
<connect gate="G$1" pin="VCC@1" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SIM" package="DIP28-KIT_MCU">
<connects>
<connect gate="G$1" pin="AGND" pad="22"/>
<connect gate="G$1" pin="AREF" pad="21"/>
<connect gate="G$1" pin="AVCC" pad="20"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="PB0(ICP)" pad="14"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="15"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="16"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="17"/>
<connect gate="G$1" pin="PB4(MISO)" pad="18"/>
<connect gate="G$1" pin="PB5(SCK)" pad="19"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="9"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="10"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="1"/>
<connect gate="G$1" pin="PD0(RXD)" pad="2"/>
<connect gate="G$1" pin="PD1(TXD)" pad="3"/>
<connect gate="G$1" pin="PD2(INT0)" pad="4"/>
<connect gate="G$1" pin="PD3(INT1)" pad="5"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="6"/>
<connect gate="G$1" pin="PD5(T1)" pad="11"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="12"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="13"/>
<connect gate="G$1" pin="VCC@1" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ZIF_SOCKET" package="DIL28-ZIF_SOCKET_MCU">
<connects>
<connect gate="G$1" pin="AGND" pad="22"/>
<connect gate="G$1" pin="AREF" pad="21"/>
<connect gate="G$1" pin="AVCC" pad="20"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="PB0(ICP)" pad="14"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="15"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="16"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="17"/>
<connect gate="G$1" pin="PB4(MISO)" pad="18"/>
<connect gate="G$1" pin="PB5(SCK)" pad="19"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="9"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="10"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="1"/>
<connect gate="G$1" pin="PD0(RXD)" pad="2"/>
<connect gate="G$1" pin="PD1(TXD)" pad="3"/>
<connect gate="G$1" pin="PD2(INT0)" pad="4"/>
<connect gate="G$1" pin="PD3(INT1)" pad="5"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="6"/>
<connect gate="G$1" pin="PD5(T1)" pad="11"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="12"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="13"/>
<connect gate="G$1" pin="VCC@1" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CY7C64215">
<description>&lt;h3&gt;Cypress PSOC uC with USB&lt;/h3&gt;
&lt;p&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;None&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="CY7C64215"/>
</gates>
<devices>
<device name="" package="SSOP28DB_MCU">
<connects>
<connect gate="G$1" pin="D+" pad="14"/>
<connect gate="G$1" pin="D-" pad="15"/>
<connect gate="G$1" pin="P00" pad="24"/>
<connect gate="G$1" pin="P01" pad="5"/>
<connect gate="G$1" pin="P02" pad="25"/>
<connect gate="G$1" pin="P03" pad="4"/>
<connect gate="G$1" pin="P04" pad="26"/>
<connect gate="G$1" pin="P05" pad="3"/>
<connect gate="G$1" pin="P06" pad="27"/>
<connect gate="G$1" pin="P07" pad="2"/>
<connect gate="G$1" pin="P10" pad="17"/>
<connect gate="G$1" pin="P11" pad="12"/>
<connect gate="G$1" pin="P12" pad="18"/>
<connect gate="G$1" pin="P13" pad="11"/>
<connect gate="G$1" pin="P14" pad="19"/>
<connect gate="G$1" pin="P15" pad="10"/>
<connect gate="G$1" pin="P16" pad="20"/>
<connect gate="G$1" pin="P17" pad="9"/>
<connect gate="G$1" pin="P20" pad="21"/>
<connect gate="G$1" pin="P21" pad="8"/>
<connect gate="G$1" pin="P22" pad="22"/>
<connect gate="G$1" pin="P23" pad="7"/>
<connect gate="G$1" pin="P24" pad="23"/>
<connect gate="G$1" pin="P25" pad="6"/>
<connect gate="G$1" pin="VDD@16" pad="16"/>
<connect gate="G$1" pin="VDD@28" pad="28"/>
<connect gate="G$1" pin="VSS@1" pad="1"/>
<connect gate="G$1" pin="VSS@13" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC30F4011">
<description>&lt;h3&gt;Microchip 16-bit DSP for UAVv2x&lt;/h3&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;None&lt;/li&gt;
&lt;/ul&gt;

Not tested</description>
<gates>
<gate name="G$1" symbol="DSPIC30F4011"/>
</gates>
<devices>
<device name="DIL" package="DIP40_MCU">
<connects>
<connect gate="G$1" pin="AVDD" pad="40"/>
<connect gate="G$1" pin="AVSS" pad="39"/>
<connect gate="G$1" pin="INT0/RE8" pad="17"/>
<connect gate="G$1" pin="MCLR" pad="1"/>
<connect gate="G$1" pin="OC1/RD0" pad="23"/>
<connect gate="G$1" pin="OC2/RD1" pad="18"/>
<connect gate="G$1" pin="OSC1" pad="13"/>
<connect gate="G$1" pin="OSC2" pad="14"/>
<connect gate="G$1" pin="PGC/SDA" pad="26"/>
<connect gate="G$1" pin="PGD/SCL" pad="25"/>
<connect gate="G$1" pin="RB0/AREF+" pad="2"/>
<connect gate="G$1" pin="RB1/AREF-" pad="3"/>
<connect gate="G$1" pin="RB2" pad="4"/>
<connect gate="G$1" pin="RB3" pad="5"/>
<connect gate="G$1" pin="RB4/IC7" pad="6"/>
<connect gate="G$1" pin="RB5/IC8" pad="7"/>
<connect gate="G$1" pin="RB6" pad="8"/>
<connect gate="G$1" pin="RB7" pad="9"/>
<connect gate="G$1" pin="RB8" pad="10"/>
<connect gate="G$1" pin="RC13/TX1" pad="15"/>
<connect gate="G$1" pin="RC14/RX1" pad="16"/>
<connect gate="G$1" pin="RD2" pad="22"/>
<connect gate="G$1" pin="RD3" pad="19"/>
<connect gate="G$1" pin="RE0" pad="38"/>
<connect gate="G$1" pin="RE1" pad="37"/>
<connect gate="G$1" pin="RE2" pad="36"/>
<connect gate="G$1" pin="RE3" pad="35"/>
<connect gate="G$1" pin="RE4" pad="34"/>
<connect gate="G$1" pin="RE5" pad="33"/>
<connect gate="G$1" pin="RF0" pad="30"/>
<connect gate="G$1" pin="RF1" pad="29"/>
<connect gate="G$1" pin="RF4/RX2" pad="28"/>
<connect gate="G$1" pin="RF5/TX2" pad="27"/>
<connect gate="G$1" pin="RF6/SCK1" pad="24"/>
<connect gate="G$1" pin="VDD0" pad="11"/>
<connect gate="G$1" pin="VDD1" pad="21"/>
<connect gate="G$1" pin="VDD2" pad="32"/>
<connect gate="G$1" pin="VSS0" pad="12"/>
<connect gate="G$1" pin="VSS1" pad="20"/>
<connect gate="G$1" pin="VSS2" pad="31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="TQFP44_MCU">
<connects>
<connect gate="G$1" pin="AVDD" pad="17"/>
<connect gate="G$1" pin="AVSS" pad="16"/>
<connect gate="G$1" pin="INT0/RE8" pad="36"/>
<connect gate="G$1" pin="MCLR" pad="18"/>
<connect gate="G$1" pin="OC1/RD0" pad="42"/>
<connect gate="G$1" pin="OC2/RD1" pad="37"/>
<connect gate="G$1" pin="OSC1" pad="30"/>
<connect gate="G$1" pin="OSC2" pad="31"/>
<connect gate="G$1" pin="PGC/SDA" pad="1"/>
<connect gate="G$1" pin="PGD/SCL" pad="44"/>
<connect gate="G$1" pin="RB0/AREF+" pad="19"/>
<connect gate="G$1" pin="RB1/AREF-" pad="20"/>
<connect gate="G$1" pin="RB2" pad="21"/>
<connect gate="G$1" pin="RB3" pad="22"/>
<connect gate="G$1" pin="RB4/IC7" pad="23"/>
<connect gate="G$1" pin="RB5/IC8" pad="24"/>
<connect gate="G$1" pin="RB6" pad="25"/>
<connect gate="G$1" pin="RB7" pad="26"/>
<connect gate="G$1" pin="RB8" pad="27"/>
<connect gate="G$1" pin="RC13/TX1" pad="32"/>
<connect gate="G$1" pin="RC14/RX1" pad="35"/>
<connect gate="G$1" pin="RD2" pad="41"/>
<connect gate="G$1" pin="RD3" pad="38"/>
<connect gate="G$1" pin="RE0" pad="15"/>
<connect gate="G$1" pin="RE1" pad="14"/>
<connect gate="G$1" pin="RE2" pad="11"/>
<connect gate="G$1" pin="RE3" pad="10"/>
<connect gate="G$1" pin="RE4" pad="9"/>
<connect gate="G$1" pin="RE5" pad="8"/>
<connect gate="G$1" pin="RF0" pad="5"/>
<connect gate="G$1" pin="RF1" pad="4"/>
<connect gate="G$1" pin="RF4/RX2" pad="3"/>
<connect gate="G$1" pin="RF5/TX2" pad="2"/>
<connect gate="G$1" pin="RF6/SCK1" pad="43"/>
<connect gate="G$1" pin="VDD0" pad="7"/>
<connect gate="G$1" pin="VDD1" pad="28"/>
<connect gate="G$1" pin="VDD2" pad="40"/>
<connect gate="G$1" pin="VSS0" pad="6"/>
<connect gate="G$1" pin="VSS1" pad="29"/>
<connect gate="G$1" pin="VSS2" pad="39"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC30F6015" prefix="U">
<description>&lt;h3&gt;Microchip 16-bit DSP&lt;/h3&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;None&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="DSPIC30F6015"/>
</gates>
<devices>
<device name="SMD" package="TQFP64_MCU">
<connects>
<connect gate="G$1" pin="AGND@20" pad="20"/>
<connect gate="G$1" pin="AVDD@19" pad="19"/>
<connect gate="G$1" pin="GND@25" pad="25"/>
<connect gate="G$1" pin="GND@41" pad="41"/>
<connect gate="G$1" pin="GND@56" pad="56"/>
<connect gate="G$1" pin="GND@9" pad="9"/>
<connect gate="G$1" pin="MCLR@7" pad="7"/>
<connect gate="G$1" pin="OSC1@39" pad="39"/>
<connect gate="G$1" pin="OSC2@40" pad="40"/>
<connect gate="G$1" pin="PGC@17" pad="17"/>
<connect gate="G$1" pin="PGD@18" pad="18"/>
<connect gate="G$1" pin="RB10@23" pad="23"/>
<connect gate="G$1" pin="RB11@24" pad="24"/>
<connect gate="G$1" pin="RB12@27" pad="27"/>
<connect gate="G$1" pin="RB13@28" pad="28"/>
<connect gate="G$1" pin="RB14@29" pad="29"/>
<connect gate="G$1" pin="RB15@30" pad="30"/>
<connect gate="G$1" pin="RB2@14" pad="14"/>
<connect gate="G$1" pin="RB3@13" pad="13"/>
<connect gate="G$1" pin="RB4@12" pad="12"/>
<connect gate="G$1" pin="RB5@11" pad="11"/>
<connect gate="G$1" pin="RB8@21" pad="21"/>
<connect gate="G$1" pin="RB9@22" pad="22"/>
<connect gate="G$1" pin="RC13@47" pad="47"/>
<connect gate="G$1" pin="RC14@48" pad="48"/>
<connect gate="G$1" pin="RD0@46" pad="46"/>
<connect gate="G$1" pin="RD10@44" pad="44"/>
<connect gate="G$1" pin="RD11@45" pad="45"/>
<connect gate="G$1" pin="RD1@49" pad="49"/>
<connect gate="G$1" pin="RD2@50" pad="50"/>
<connect gate="G$1" pin="RD3@51" pad="51"/>
<connect gate="G$1" pin="RD4@52" pad="52"/>
<connect gate="G$1" pin="RD5@53" pad="53"/>
<connect gate="G$1" pin="RD6@54" pad="54"/>
<connect gate="G$1" pin="RD7@55" pad="55"/>
<connect gate="G$1" pin="RD8@42" pad="42"/>
<connect gate="G$1" pin="RD9@43" pad="43"/>
<connect gate="G$1" pin="RE0@60" pad="60"/>
<connect gate="G$1" pin="RE1@61" pad="61"/>
<connect gate="G$1" pin="RE2@62" pad="62"/>
<connect gate="G$1" pin="RE3@63" pad="63"/>
<connect gate="G$1" pin="RE4@64" pad="64"/>
<connect gate="G$1" pin="RE5@1" pad="1"/>
<connect gate="G$1" pin="RE6@2" pad="2"/>
<connect gate="G$1" pin="RE7@3" pad="3"/>
<connect gate="G$1" pin="RF0@58" pad="58"/>
<connect gate="G$1" pin="RF1@59" pad="59"/>
<connect gate="G$1" pin="RF6@35" pad="35"/>
<connect gate="G$1" pin="RG2@37" pad="37"/>
<connect gate="G$1" pin="RG3@36" pad="36"/>
<connect gate="G$1" pin="RG6@4" pad="4"/>
<connect gate="G$1" pin="RG7@5" pad="5"/>
<connect gate="G$1" pin="RG8@6" pad="6"/>
<connect gate="G$1" pin="RG9@8" pad="8"/>
<connect gate="G$1" pin="RX1@34" pad="34"/>
<connect gate="G$1" pin="RX2@32" pad="32"/>
<connect gate="G$1" pin="TX1@33" pad="33"/>
<connect gate="G$1" pin="TX2@31" pad="31"/>
<connect gate="G$1" pin="VDD@10" pad="10"/>
<connect gate="G$1" pin="VDD@26" pad="26"/>
<connect gate="G$1" pin="VDD@38" pad="38"/>
<connect gate="G$1" pin="VDD@57" pad="57"/>
<connect gate="G$1" pin="VREF+/RB0@16" pad="16"/>
<connect gate="G$1" pin="VREF-/RB1@15" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSPIC33FJ256GP710" prefix="U">
<description>&lt;h3&gt;Microchip 16-bit DSP&lt;/h3&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;None&lt;/li&gt;
&lt;/ul&gt;

Not tested</description>
<gates>
<gate name="G1" symbol="DSPIC33FJ256GP710_POWER"/>
<gate name="G2" symbol="DSPIC33FJ256GP710_CONTROL"/>
<gate name="G3" symbol="DSPIC33FJ256GP710_EXTERNAL"/>
<gate name="G4" symbol="DSPIC33FJ256GP710_EXTRA"/>
</gates>
<devices>
<device name="_" package="TQFP-100-12X12MM_MCU">
<connects>
<connect gate="G1" pin="AVDD" pad="30"/>
<connect gate="G1" pin="AVSS" pad="31"/>
<connect gate="G1" pin="RA10/VREF+" pad="29"/>
<connect gate="G1" pin="RA9/VREF-" pad="28"/>
<connect gate="G1" pin="VCAP" pad="85"/>
<connect gate="G1" pin="VDD@16" pad="16"/>
<connect gate="G1" pin="VDD@2" pad="2"/>
<connect gate="G1" pin="VDD@37" pad="37"/>
<connect gate="G1" pin="VDD@46" pad="46"/>
<connect gate="G1" pin="VDD@62" pad="62"/>
<connect gate="G1" pin="VDD@86" pad="86"/>
<connect gate="G1" pin="VSS@15" pad="15"/>
<connect gate="G1" pin="VSS@36" pad="36"/>
<connect gate="G1" pin="VSS@45" pad="45"/>
<connect gate="G1" pin="VSS@65" pad="65"/>
<connect gate="G1" pin="VSS@75" pad="75"/>
<connect gate="G2" pin="RA6/AN22" pad="91"/>
<connect gate="G2" pin="RB0/AN0" pad="25"/>
<connect gate="G2" pin="RB1/AN1" pad="24"/>
<connect gate="G2" pin="RB10/AN10" pad="34"/>
<connect gate="G2" pin="RB11/AN11" pad="35"/>
<connect gate="G2" pin="RB12/AN12" pad="41"/>
<connect gate="G2" pin="RB13/AN13" pad="42"/>
<connect gate="G2" pin="RB14/AN14" pad="43"/>
<connect gate="G2" pin="RB3/AN3" pad="22"/>
<connect gate="G2" pin="RB4/AN4" pad="21"/>
<connect gate="G2" pin="RB5/AN5" pad="20"/>
<connect gate="G2" pin="RB6/AN6" pad="26"/>
<connect gate="G2" pin="RB7/AN7" pad="27"/>
<connect gate="G2" pin="RB8/AN8" pad="32"/>
<connect gate="G2" pin="RB9/AN9" pad="33"/>
<connect gate="G2" pin="RC4/AN19" pad="9"/>
<connect gate="G2" pin="RD0/OC1" pad="72"/>
<connect gate="G2" pin="RD1/OC2" pad="76"/>
<connect gate="G2" pin="RD10/IC3" pad="70"/>
<connect gate="G2" pin="RD11/IC4" pad="71"/>
<connect gate="G2" pin="RD12/IC5" pad="79"/>
<connect gate="G2" pin="RD13/IC6" pad="80"/>
<connect gate="G2" pin="RD14/U1CTS/IC7" pad="47"/>
<connect gate="G2" pin="RD15/U1RTS/IC8" pad="48"/>
<connect gate="G2" pin="RD2/OC3" pad="77"/>
<connect gate="G2" pin="RD3/OC4" pad="78"/>
<connect gate="G2" pin="RD4/OC5" pad="81"/>
<connect gate="G2" pin="RD5/OC6" pad="82"/>
<connect gate="G2" pin="RD6/OC7" pad="83"/>
<connect gate="G2" pin="RD7/OC8" pad="84"/>
<connect gate="G2" pin="RD8/IC1" pad="68"/>
<connect gate="G2" pin="RD9/IC2" pad="69"/>
<connect gate="G2" pin="RE1/AN25" pad="94"/>
<connect gate="G2" pin="RE2" pad="98"/>
<connect gate="G2" pin="RE3" pad="99"/>
<connect gate="G2" pin="RE4" pad="100"/>
<connect gate="G2" pin="RF2/U1RX" pad="52"/>
<connect gate="G2" pin="RF3/U1TX" pad="51"/>
<connect gate="G2" pin="RG2/SCL1" pad="57"/>
<connect gate="G2" pin="RG3/SDA1" pad="56"/>
<connect gate="G3" pin="MCLR" pad="13"/>
<connect gate="G3" pin="RA1" pad="38"/>
<connect gate="G3" pin="RA12/INT1" pad="18"/>
<connect gate="G3" pin="RA13/INT2" pad="19"/>
<connect gate="G3" pin="RA14" pad="66"/>
<connect gate="G3" pin="RA2/SCL2" pad="58"/>
<connect gate="G3" pin="RA3/SDA2" pad="59"/>
<connect gate="G3" pin="RA4/TDI" pad="60"/>
<connect gate="G3" pin="RA5/TDO" pad="61"/>
<connect gate="G3" pin="RA7/AN23" pad="92"/>
<connect gate="G3" pin="RB15/AN15" pad="44"/>
<connect gate="G3" pin="RB2/SS1" pad="23"/>
<connect gate="G3" pin="RC1/AN16" pad="6"/>
<connect gate="G3" pin="RC13/PGED2" pad="73"/>
<connect gate="G3" pin="RC14/PGEC2" pad="74"/>
<connect gate="G3" pin="RC2/AN17" pad="7"/>
<connect gate="G3" pin="RC3/AN18" pad="8"/>
<connect gate="G3" pin="RE0/AN24" pad="93"/>
<connect gate="G3" pin="RF0/C1RX1" pad="87"/>
<connect gate="G3" pin="RF1/C1TX1" pad="88"/>
<connect gate="G3" pin="RF12/U2CTS" pad="40"/>
<connect gate="G3" pin="RF13/U2RTS" pad="39"/>
<connect gate="G3" pin="RF4/U2RX" pad="49"/>
<connect gate="G3" pin="RF5/U2TX" pad="50"/>
<connect gate="G3" pin="RF6/SCK1" pad="55"/>
<connect gate="G3" pin="RF7/SDI1" pad="54"/>
<connect gate="G3" pin="RF8/SDO1" pad="53"/>
<connect gate="G3" pin="RG6/SCK2" pad="10"/>
<connect gate="G3" pin="RG7/SDI2" pad="11"/>
<connect gate="G3" pin="RG8/SDO2" pad="12"/>
<connect gate="G3" pin="RG9/SS2" pad="14"/>
<connect gate="G4" pin="RA0/TMS" pad="17"/>
<connect gate="G4" pin="RA15" pad="67"/>
<connect gate="G4" pin="RC12/OSC1" pad="63"/>
<connect gate="G4" pin="RC15/OSC2" pad="64"/>
<connect gate="G4" pin="RE5/AN29" pad="3"/>
<connect gate="G4" pin="RE6/AN30" pad="4"/>
<connect gate="G4" pin="RE7/AN31" pad="5"/>
<connect gate="G4" pin="RG0/C2RX" pad="90"/>
<connect gate="G4" pin="RG1/C2TX" pad="89"/>
<connect gate="G4" pin="RG12/CSDI" pad="96"/>
<connect gate="G4" pin="RG13/CSDO" pad="97"/>
<connect gate="G4" pin="RG14/CSCK" pad="95"/>
<connect gate="G4" pin="RG15/COFS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC213X" prefix="IC">
<description>NXP LPC213x uC. Spark Fun Electronics SKU : COM-00520
&lt;br&gt;&lt;br&gt;
RETIRED</description>
<gates>
<gate name="G$1" symbol="LPC213X"/>
</gates>
<devices>
<device name="" package="SQFP-S-10X10-64_MCU">
<connects>
<connect gate="G$1" pin="(AD0.0/CAP0.1/MAT0.1)P0.27" pad="11"/>
<connect gate="G$1" pin="(AD0.1/CAP0.2/MAT0.2)P0.28" pad="13"/>
<connect gate="G$1" pin="(AD0.2/CAP0.3/MAT0.3)P0.29" pad="14"/>
<connect gate="G$1" pin="(AD0.3/EINT3/CAP0.0)P0.30" pad="15"/>
<connect gate="G$1" pin="(AD0.4/AOUT)P0.25" pad="9"/>
<connect gate="G$1" pin="(AD0.5)P0.26" pad="10"/>
<connect gate="G$1" pin="(AD1.7/CAP0.0/MAT0.0)P0.22" pad="2"/>
<connect gate="G$1" pin="(CAP1.2/SCK1/MAT1.2)P0.17" pad="47"/>
<connect gate="G$1" pin="(CAP1.3/MISO1/MAT1.3)P0.18" pad="53"/>
<connect gate="G$1" pin="(CTS1/CAP1.1/SCL1)P0.11" pad="37"/>
<connect gate="G$1" pin="(DCD1/EINT1/SDA1)P0.14" pad="41"/>
<connect gate="G$1" pin="(DSR1/MAT1.0/AD1.3)P0.12" pad="38"/>
<connect gate="G$1" pin="(DTR1/MAT1.1/AD1.4)P0.13" pad="39"/>
<connect gate="G$1" pin="(EINT0/MAT0.2/CAP0.2)P0.16" pad="46"/>
<connect gate="G$1" pin="(MAT1.2/MOSI1/CAP1.2)P0.19" pad="54"/>
<connect gate="G$1" pin="(MAT1.3/SSEL1/EINT3)P0.20" pad="55"/>
<connect gate="G$1" pin="(MISO0/MAT0.1/A0.7)P0.5" pad="29"/>
<connect gate="G$1" pin="(MOSI0/CAP0.2/AD1.0)P0.6" pad="30"/>
<connect gate="G$1" pin="(PWM5/AD1.6/CAP1.3)P0.21" pad="1"/>
<connect gate="G$1" pin="(RI1/EINT2/AD1.5)P0.15" pad="45"/>
<connect gate="G$1" pin="(RTS1/CAP1.0/AD1.2)P0.10" pad="35"/>
<connect gate="G$1" pin="(RXD0/PWM3/EINT0)P0.1" pad="21"/>
<connect gate="G$1" pin="(RXD1/PWM6/EINT3)P0.9" pad="34"/>
<connect gate="G$1" pin="(SCK0/CAP0.1/AD0.6)P0.4" pad="27"/>
<connect gate="G$1" pin="(SCL0/CAP0.0)P0.2" pad="22"/>
<connect gate="G$1" pin="(SDA0/MAT0.0/EINT1)P0.3" pad="26"/>
<connect gate="G$1" pin="(SSEL0/PWM2/EINT2)P0.7" pad="31"/>
<connect gate="G$1" pin="(TXD0/PWM1)P0.0" pad="19"/>
<connect gate="G$1" pin="(TXD1/PWM4/A1.1)P0.8" pad="33"/>
<connect gate="G$1" pin="P0.23" pad="58"/>
<connect gate="G$1" pin="P0.31" pad="17"/>
<connect gate="G$1" pin="P1.16(TRACEPKT0)" pad="16"/>
<connect gate="G$1" pin="P1.17(TRACEPKT1)" pad="12"/>
<connect gate="G$1" pin="P1.18(TRACEPKT2)" pad="8"/>
<connect gate="G$1" pin="P1.19(TRACEPKT3)" pad="4"/>
<connect gate="G$1" pin="P1.20(TRACESYNC)" pad="48"/>
<connect gate="G$1" pin="P1.21(PIPESTAT0)" pad="44"/>
<connect gate="G$1" pin="P1.22(PIPESTAT1)" pad="40"/>
<connect gate="G$1" pin="P1.23(PIPESTAT2)" pad="36"/>
<connect gate="G$1" pin="P1.24(TRACECLK)" pad="32"/>
<connect gate="G$1" pin="P1.25(EXTIN0)" pad="28"/>
<connect gate="G$1" pin="P1.26(RTCK)" pad="24"/>
<connect gate="G$1" pin="P1.27(TDO)" pad="64"/>
<connect gate="G$1" pin="P1.28(TDI)" pad="60"/>
<connect gate="G$1" pin="P1.29(TCK)" pad="56"/>
<connect gate="G$1" pin="P1.30(TMS)" pad="52"/>
<connect gate="G$1" pin="P1.31(/TRST)" pad="20"/>
<connect gate="G$1" pin="RESET" pad="57"/>
<connect gate="G$1" pin="RTXC1" pad="3"/>
<connect gate="G$1" pin="RTXC2" pad="5"/>
<connect gate="G$1" pin="VBAT" pad="49"/>
<connect gate="G$1" pin="VDD3-1" pad="23"/>
<connect gate="G$1" pin="VDD3-2" pad="43"/>
<connect gate="G$1" pin="VDD3-3" pad="51"/>
<connect gate="G$1" pin="VDDA3" pad="7"/>
<connect gate="G$1" pin="VREF" pad="63"/>
<connect gate="G$1" pin="VSS" pad="6"/>
<connect gate="G$1" pin="VSS@1" pad="18"/>
<connect gate="G$1" pin="VSS@2" pad="25"/>
<connect gate="G$1" pin="VSS@3" pad="42"/>
<connect gate="G$1" pin="VSS@4" pad="50"/>
<connect gate="G$1" pin="VSSA" pad="59"/>
<connect gate="G$1" pin="XTAL1" pad="62"/>
<connect gate="G$1" pin="XTAL2" pad="61"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC2103">
<description>&lt;h3&gt;NXP LPC2103 ARM7 based MCU&lt;/h3&gt;
Dead prototype</description>
<gates>
<gate name="G$1" symbol="LPC2103"/>
</gates>
<devices>
<device name="" package="LQFP-48_MCU">
<connects>
<connect gate="G$1" pin="DBGSEL" pad="27"/>
<connect gate="G$1" pin="P0.0/TXD0/MAT3.1" pad="13"/>
<connect gate="G$1" pin="P0.1/RXD0/MAT3.2" pad="14"/>
<connect gate="G$1" pin="P0.10/RTS1/CAP1.0/AD0.3" pad="35"/>
<connect gate="G$1" pin="P0.11/CTS1/CAP1.1/AD0.4" pad="36"/>
<connect gate="G$1" pin="P0.12/DSR1/MAT1.0/AD0.5" pad="37"/>
<connect gate="G$1" pin="P0.13/DTR1/MAT1.1" pad="41"/>
<connect gate="G$1" pin="P0.14/DCD1/SCK1/EINT1" pad="44"/>
<connect gate="G$1" pin="P0.15/RI1/EINT2" pad="45"/>
<connect gate="G$1" pin="P0.16/EINT0/MAT0.2" pad="46"/>
<connect gate="G$1" pin="P0.17/CAP1.2/SCL1" pad="47"/>
<connect gate="G$1" pin="P0.18/CAP1.3/SDA1" pad="48"/>
<connect gate="G$1" pin="P0.19/MAT1.2/MISO1" pad="1"/>
<connect gate="G$1" pin="P0.2/SCL0/CAP0.0" pad="18"/>
<connect gate="G$1" pin="P0.20/MAT1.3/MOSI1" pad="2"/>
<connect gate="G$1" pin="P0.21/SSEL1/MAT3.0" pad="3"/>
<connect gate="G$1" pin="P0.22/AD0.0" pad="32"/>
<connect gate="G$1" pin="P0.23/AD0.1" pad="33"/>
<connect gate="G$1" pin="P0.24/AD0.2" pad="34"/>
<connect gate="G$1" pin="P0.25/AD0.6" pad="38"/>
<connect gate="G$1" pin="P0.26/AD0.7" pad="39"/>
<connect gate="G$1" pin="P0.27/TRST/CAP2.0" pad="8"/>
<connect gate="G$1" pin="P0.28/TMS/CAP2.1" pad="9"/>
<connect gate="G$1" pin="P0.29/TCK/CAP2.2" pad="10"/>
<connect gate="G$1" pin="P0.3/SDA0/MAT0.0" pad="21"/>
<connect gate="G$1" pin="P0.30/TDI/MAT3.3" pad="15"/>
<connect gate="G$1" pin="P0.31/TDO" pad="16"/>
<connect gate="G$1" pin="P0.4/SCK0/CAP0.1" pad="22"/>
<connect gate="G$1" pin="P0.5/MISO0/MAT0.1" pad="23"/>
<connect gate="G$1" pin="P0.6/MOSI0/CAP0.2" pad="24"/>
<connect gate="G$1" pin="P0.7/SSEL0/MAT2.0" pad="28"/>
<connect gate="G$1" pin="P0.8/TXD1/MAT2.1" pad="29"/>
<connect gate="G$1" pin="P0.9/RXD1/MAT2.2" pad="30"/>
<connect gate="G$1" pin="RST" pad="6"/>
<connect gate="G$1" pin="RTCK" pad="26"/>
<connect gate="G$1" pin="RTCX1" pad="20"/>
<connect gate="G$1" pin="RTCX2" pad="25"/>
<connect gate="G$1" pin="VBAT" pad="4"/>
<connect gate="G$1" pin="VDD(1V8)" pad="5"/>
<connect gate="G$1" pin="VDD(3V3)@17" pad="17"/>
<connect gate="G$1" pin="VDD(3V3)@40" pad="40"/>
<connect gate="G$1" pin="VDDA" pad="42"/>
<connect gate="G$1" pin="VSS@19" pad="19"/>
<connect gate="G$1" pin="VSS@43" pad="43"/>
<connect gate="G$1" pin="VSS@7" pad="7"/>
<connect gate="G$1" pin="VSSA" pad="31"/>
<connect gate="G$1" pin="XTAL1" pad="11"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09387"/>
<attribute name="VALUE" value="LPC2103"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC9S12XS64">
<description>&lt;h3&gt;Freescale 16-bit uC&lt;/h3&gt;
Dead prototype</description>
<gates>
<gate name="G$1" symbol="MC9S12XS64"/>
</gates>
<devices>
<device name="" package="SQFP-S-10X10-64_MCU">
<connects>
<connect gate="G$1" pin="ECLK/PE4" pad="21"/>
<connect gate="G$1" pin="EXTAL" pad="28"/>
<connect gate="G$1" pin="IOC0/PT0" pad="5"/>
<connect gate="G$1" pin="IOC1/PT1" pad="6"/>
<connect gate="G$1" pin="IOC1/PWM1/KWP1/PP1" pad="3"/>
<connect gate="G$1" pin="IOC2/PT2" pad="7"/>
<connect gate="G$1" pin="IOC3/PT3" pad="8"/>
<connect gate="G$1" pin="IRQ/PE1" pad="31"/>
<connect gate="G$1" pin="MODC/BKGD" pad="15"/>
<connect gate="G$1" pin="PA0" pad="33"/>
<connect gate="G$1" pin="PA1" pad="34"/>
<connect gate="G$1" pin="PA2" pad="35"/>
<connect gate="G$1" pin="PA3" pad="36"/>
<connect gate="G$1" pin="PAD00/AN00" pad="39"/>
<connect gate="G$1" pin="PAD01/AN01" pad="40"/>
<connect gate="G$1" pin="PAD02/AN02" pad="41"/>
<connect gate="G$1" pin="PAD03/AN03" pad="42"/>
<connect gate="G$1" pin="PAD04/AN04" pad="43"/>
<connect gate="G$1" pin="PAD05/AN05" pad="44"/>
<connect gate="G$1" pin="PAD06/AN06" pad="45"/>
<connect gate="G$1" pin="PAD07/AN07" pad="46"/>
<connect gate="G$1" pin="PB0" pad="16"/>
<connect gate="G$1" pin="PB5" pad="17"/>
<connect gate="G$1" pin="PB6" pad="18"/>
<connect gate="G$1" pin="PB7" pad="19"/>
<connect gate="G$1" pin="PM0/RXCAN0/RXD1" pad="60"/>
<connect gate="G$1" pin="PM1/TXCAN0/TXD1" pad="59"/>
<connect gate="G$1" pin="PM2/MISO0" pad="58"/>
<connect gate="G$1" pin="PM3/SS0" pad="57"/>
<connect gate="G$1" pin="PM4/MOSI0" pad="56"/>
<connect gate="G$1" pin="PM5/SCK0" pad="55"/>
<connect gate="G$1" pin="PP5/KPW5/PWM5" pad="64"/>
<connect gate="G$1" pin="PP7/KWP7/PWM7" pad="63"/>
<connect gate="G$1" pin="PS0/RXD0" pad="50"/>
<connect gate="G$1" pin="PS1/TXD0" pad="51"/>
<connect gate="G$1" pin="PS2/RXD1" pad="52"/>
<connect gate="G$1" pin="PS3/TXD1" pad="53"/>
<connect gate="G$1" pin="PWM3/KWP3/PP3" pad="1"/>
<connect gate="G$1" pin="PWM4/IOC4/PT4" pad="11"/>
<connect gate="G$1" pin="PWM6/IOC6/PT6" pad="13"/>
<connect gate="G$1" pin="PWM7/IOC7/PT7" pad="14"/>
<connect gate="G$1" pin="RESET" pad="24"/>
<connect gate="G$1" pin="RXD1/IOC0/PWM0/KWP0/PP0" pad="4"/>
<connect gate="G$1" pin="TEST" pad="54"/>
<connect gate="G$1" pin="TXD1/IOC2/PWM2/KWP2/PP2" pad="2"/>
<connect gate="G$1" pin="VDD" pad="37"/>
<connect gate="G$1" pin="VDDA" pad="47"/>
<connect gate="G$1" pin="VDDF" pad="9"/>
<connect gate="G$1" pin="VDDPLL" pad="30"/>
<connect gate="G$1" pin="VDDR" pad="25"/>
<connect gate="G$1" pin="VDDX1" pad="62"/>
<connect gate="G$1" pin="VDDX2" pad="23"/>
<connect gate="G$1" pin="VREG_API/PWM5/IOC5/PT" pad="12"/>
<connect gate="G$1" pin="VRH" pad="48"/>
<connect gate="G$1" pin="VSS1" pad="10"/>
<connect gate="G$1" pin="VSS2" pad="38"/>
<connect gate="G$1" pin="VSS3" pad="26"/>
<connect gate="G$1" pin="VSSA/VRL" pad="49"/>
<connect gate="G$1" pin="VSSPLL" pad="27"/>
<connect gate="G$1" pin="VSSX1" pad="61"/>
<connect gate="G$1" pin="VSSX2" pad="22"/>
<connect gate="G$1" pin="XCLKS/ECLKX2/PE7" pad="20"/>
<connect gate="G$1" pin="XIRQ/PE0" pad="32"/>
<connect gate="G$1" pin="XTAL" pad="29"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09432"/>
<attribute name="VALUE" value="MC9S12XS64"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16F688">
<description>&lt;h3&gt;PIC 16F68&lt;/h3&gt;
&lt;p&gt;8-Bit PIC16F88&lt;/p&gt;
RETIRED: IC-07818</description>
<gates>
<gate name="G$1" symbol="PIC16F688"/>
</gates>
<devices>
<device name="SMD" package="SO14_MCU">
<connects>
<connect gate="G$1" pin="RA0/PGD" pad="13"/>
<connect gate="G$1" pin="RA1/PGC" pad="12"/>
<connect gate="G$1" pin="RA2/AN2" pad="11"/>
<connect gate="G$1" pin="RA3/MCLR" pad="4"/>
<connect gate="G$1" pin="RA4/OSC2" pad="3"/>
<connect gate="G$1" pin="RA5/OSC1" pad="2"/>
<connect gate="G$1" pin="RC0/AN4" pad="10"/>
<connect gate="G$1" pin="RC1/AN5" pad="9"/>
<connect gate="G$1" pin="RC2/AN6" pad="8"/>
<connect gate="G$1" pin="RC3/AN7" pad="7"/>
<connect gate="G$1" pin="RC4/TX" pad="6"/>
<connect gate="G$1" pin="RC5/RX" pad="5"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16F883">
<description>&lt;h3&gt;PIC16F833&lt;/h3&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;None&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="PIC16F883"/>
</gates>
<devices>
<device name="" package="SO-28W_MCU">
<connects>
<connect gate="G$1" pin="MCLR/VPP" pad="1"/>
<connect gate="G$1" pin="OSC1" pad="9"/>
<connect gate="G$1" pin="OSC2" pad="10"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2" pad="4"/>
<connect gate="G$1" pin="RA3/AN3" pad="5"/>
<connect gate="G$1" pin="RA4" pad="6"/>
<connect gate="G$1" pin="RA5/AN4" pad="7"/>
<connect gate="G$1" pin="RB0/INT0" pad="21"/>
<connect gate="G$1" pin="RB1/INT1/AN10" pad="22"/>
<connect gate="G$1" pin="RB2/INT2/AN8" pad="23"/>
<connect gate="G$1" pin="RB3/AN9" pad="24"/>
<connect gate="G$1" pin="RB4/AN11" pad="25"/>
<connect gate="G$1" pin="RB5/PGM" pad="26"/>
<connect gate="G$1" pin="RB6/PGC" pad="27"/>
<connect gate="G$1" pin="RB7/PGD" pad="28"/>
<connect gate="G$1" pin="RC0" pad="11"/>
<connect gate="G$1" pin="RC1" pad="12"/>
<connect gate="G$1" pin="RC2" pad="13"/>
<connect gate="G$1" pin="RC3/SCK" pad="14"/>
<connect gate="G$1" pin="RC4/SDI" pad="15"/>
<connect gate="G$1" pin="RC5/SDO" pad="16"/>
<connect gate="G$1" pin="RX/RC7" pad="18"/>
<connect gate="G$1" pin="TX/RC6" pad="17"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@19" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16F913">
<description>&lt;h3&gt;PIC16F913&lt;/h3&gt;
&lt;p&gt;IC PIC MCU FLASH 4KX14 28SOIC&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8661"&gt;Polar Heart Rate Monitor Interface&lt;/a&gt; (SEN-08661)&lt;/li&gt;
&lt;/ul&gt;

Short timer</description>
<gates>
<gate name="G$1" symbol="PIC16F913"/>
</gates>
<devices>
<device name="SOIC28" package="SO-28W_MCU">
<connects>
<connect gate="G$1" pin="MCLR/VPP" pad="1"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2" pad="4"/>
<connect gate="G$1" pin="RA3/AN3" pad="5"/>
<connect gate="G$1" pin="RA4" pad="6"/>
<connect gate="G$1" pin="RA5/AN4" pad="7"/>
<connect gate="G$1" pin="RA6/OSC2" pad="10"/>
<connect gate="G$1" pin="RA7/OSC1" pad="9"/>
<connect gate="G$1" pin="RB0/INT0" pad="21"/>
<connect gate="G$1" pin="RB1" pad="22"/>
<connect gate="G$1" pin="RB2" pad="23"/>
<connect gate="G$1" pin="RB3" pad="24"/>
<connect gate="G$1" pin="RB4" pad="25"/>
<connect gate="G$1" pin="RB5" pad="26"/>
<connect gate="G$1" pin="RB6/PGC" pad="27"/>
<connect gate="G$1" pin="RB7/PGD" pad="28"/>
<connect gate="G$1" pin="RC0" pad="11"/>
<connect gate="G$1" pin="RC1" pad="12"/>
<connect gate="G$1" pin="RC2" pad="13"/>
<connect gate="G$1" pin="RC3" pad="14"/>
<connect gate="G$1" pin="RC4/SD0" pad="15"/>
<connect gate="G$1" pin="RC5" pad="16"/>
<connect gate="G$1" pin="RX/RC7/SDA" pad="18"/>
<connect gate="G$1" pin="TX/RC6/SCL" pad="17"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@19" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F2455">
<description>&lt;h3&gt;PIC18F2455-I/SO&lt;/h3&gt;

Retired: IC-08246</description>
<gates>
<gate name="G$1" symbol="PIC18F2550"/>
</gates>
<devices>
<device name="SMD" package="SO-28W_MCU">
<connects>
<connect gate="G$1" pin="MCLR/VPP" pad="1"/>
<connect gate="G$1" pin="OSC1" pad="9"/>
<connect gate="G$1" pin="OSC2" pad="10"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2" pad="4"/>
<connect gate="G$1" pin="RA3/AN3" pad="5"/>
<connect gate="G$1" pin="RA4/AN4" pad="6"/>
<connect gate="G$1" pin="RA5/AN4" pad="7"/>
<connect gate="G$1" pin="RB0/INT0" pad="21"/>
<connect gate="G$1" pin="RB1/INT1/AN10" pad="22"/>
<connect gate="G$1" pin="RB2/INT2/AN8" pad="23"/>
<connect gate="G$1" pin="RB3/AN9" pad="24"/>
<connect gate="G$1" pin="RB4/AN11" pad="25"/>
<connect gate="G$1" pin="RB5/PGM" pad="26"/>
<connect gate="G$1" pin="RB6/PGC" pad="27"/>
<connect gate="G$1" pin="RB7/PGD" pad="28"/>
<connect gate="G$1" pin="RC0" pad="11"/>
<connect gate="G$1" pin="RC1" pad="12"/>
<connect gate="G$1" pin="RC2" pad="13"/>
<connect gate="G$1" pin="RC4/D-" pad="15"/>
<connect gate="G$1" pin="RC5/D+" pad="16"/>
<connect gate="G$1" pin="RX/RC7" pad="18"/>
<connect gate="G$1" pin="TX/RC6" pad="17"/>
<connect gate="G$1" pin="V-USB" pad="14"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@19" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F2550">
<description>&lt;h3&gt;PIC18F2550&lt;/h3&gt;
Retired: IC-08240</description>
<gates>
<gate name="G$1" symbol="PIC18F2550"/>
</gates>
<devices>
<device name="" package="DIP28_MCU">
<connects>
<connect gate="G$1" pin="MCLR/VPP" pad="1"/>
<connect gate="G$1" pin="OSC1" pad="9"/>
<connect gate="G$1" pin="OSC2" pad="10"/>
<connect gate="G$1" pin="RA0/AN0" pad="2"/>
<connect gate="G$1" pin="RA1/AN1" pad="3"/>
<connect gate="G$1" pin="RA2/AN2" pad="4"/>
<connect gate="G$1" pin="RA3/AN3" pad="5"/>
<connect gate="G$1" pin="RA4/AN4" pad="6"/>
<connect gate="G$1" pin="RA5/AN4" pad="7"/>
<connect gate="G$1" pin="RB0/INT0" pad="21"/>
<connect gate="G$1" pin="RB1/INT1/AN10" pad="22"/>
<connect gate="G$1" pin="RB2/INT2/AN8" pad="23"/>
<connect gate="G$1" pin="RB3/AN9" pad="24"/>
<connect gate="G$1" pin="RB4/AN11" pad="25"/>
<connect gate="G$1" pin="RB5/PGM" pad="26"/>
<connect gate="G$1" pin="RB6/PGC" pad="27"/>
<connect gate="G$1" pin="RB7/PGD" pad="28"/>
<connect gate="G$1" pin="RC0" pad="11"/>
<connect gate="G$1" pin="RC1" pad="12"/>
<connect gate="G$1" pin="RC2" pad="13"/>
<connect gate="G$1" pin="RC4/D-" pad="15"/>
<connect gate="G$1" pin="RC5/D+" pad="16"/>
<connect gate="G$1" pin="RX/RC7" pad="18"/>
<connect gate="G$1" pin="TX/RC6" pad="17"/>
<connect gate="G$1" pin="V-USB" pad="14"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="8"/>
<connect gate="G$1" pin="VSS@19" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24FXXXGPX06" prefix="U">
<description>&lt;h3&gt;PIC24FXXXGPX06&lt;/h3&gt;
&lt;p&gt;PIC24FXXXGP106 / PIC24FXXXDA206&lt;br&gt;
PIC24FJ256GP206-I/PT for IOIO&lt;br&gt;
&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Dev/Android/39975a.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13613"&gt;IOIO-OTG - V2.2&lt;/a&gt; (DEV-13613)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="PIC24FJXXXDAX06"/>
</gates>
<devices>
<device name="" package="PIC24FXXX_TQFP64_MCU">
<connects>
<connect gate="G$1" pin="!MCLR" pad="7"/>
<connect gate="G$1" pin="AN14/CTPLS/RP14/CN32/RB14" pad="29"/>
<connect gate="G$1" pin="AN15/RP29/REFO/CN12/RB15" pad="30"/>
<connect gate="G$1" pin="AN2/C2INB/VMIO/RP13/CN4/RB2" pad="14"/>
<connect gate="G$1" pin="AN3/C2INA/VPIO/CN5/RB3" pad="13"/>
<connect gate="G$1" pin="AN8/RP8/CN26/RB8" pad="21"/>
<connect gate="G$1" pin="AN9/RP9/CN27/RB9" pad="22"/>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="AVSS" pad="20"/>
<connect gate="G$1" pin="C1INC/RP26/CN9/RG7" pad="5"/>
<connect gate="G$1" pin="C1IND/RP21/CN8/RG6" pad="4"/>
<connect gate="G$1" pin="C2INC/RP27/GD15/CN11/RG9" pad="8"/>
<connect gate="G$1" pin="C2IND/RP19/GD14/CN10/RG8" pad="6"/>
<connect gate="G$1" pin="C3INA/SESSEND/CN16/RD7" pad="55"/>
<connect gate="G$1" pin="C3INB/CN15/RD6" pad="54"/>
<connect gate="G$1" pin="D+/CN83/RG2" pad="37"/>
<connect gate="G$1" pin="D-/CN84/RG3" pad="36"/>
<connect gate="G$1" pin="DMH/RP11/INT0/CN49/RD0" pad="46"/>
<connect gate="G$1" pin="DPH/RP23/CN51/RD2" pad="50"/>
<connect gate="G$1" pin="DPLN/SDA1/RP4/GD8/CN54/RD9" pad="43"/>
<connect gate="G$1" pin="ENVREG" pad="57"/>
<connect gate="G$1" pin="GD0/CN58/RE0" pad="60"/>
<connect gate="G$1" pin="GD1/CN59/RE1" pad="61"/>
<connect gate="G$1" pin="GD10/VBUSST/VCMPST1/VBUSVLD/CN68/RF0" pad="58"/>
<connect gate="G$1" pin="GD11/VCMPST2/SESSVLD/CN69/RF1" pad="59"/>
<connect gate="G$1" pin="GD12/SCL3/CN64/RE6" pad="2"/>
<connect gate="G$1" pin="GD13/SDA3/CN65/RE7" pad="3"/>
<connect gate="G$1" pin="GD2/CN60/RE2" pad="62"/>
<connect gate="G$1" pin="GD3/CN61/RE3" pad="63"/>
<connect gate="G$1" pin="HSYNC/CN62/RE4" pad="64"/>
<connect gate="G$1" pin="OSCI/CLKI/CN23/RC12" pad="39"/>
<connect gate="G$1" pin="OSCO/CLKO/CN22/RC15" pad="40"/>
<connect gate="G$1" pin="PGEC1/AN1/VREF-/RP1/CN3/RB1" pad="15"/>
<connect gate="G$1" pin="PGEC2/AN6/RP6/CN24/RB6" pad="17"/>
<connect gate="G$1" pin="PGEC3/AN5/C1INA/VBUSON/RP18/CN7/RB5" pad="11"/>
<connect gate="G$1" pin="PGED1/AN0/VREF+/RP0/CN2/RB0" pad="16"/>
<connect gate="G$1" pin="PGED2/AN7/RP7/RCV/CN25/RB7" pad="18"/>
<connect gate="G$1" pin="PGED3/AN4/C1INB/USBOEN/RP28/CN6/RB4" pad="12"/>
<connect gate="G$1" pin="RP12/GD7/CN56/RD11" pad="45"/>
<connect gate="G$1" pin="RP16/USBID/CN71/RF3" pad="33"/>
<connect gate="G$1" pin="RP20/GPWR/CN14/RD5" pad="53"/>
<connect gate="G$1" pin="RP22/GEN/CN52/RD3" pad="51"/>
<connect gate="G$1" pin="RP25/GCLK/CN13/RD4" pad="52"/>
<connect gate="G$1" pin="RTCC/DMLN/RP2/CN53/RD8" pad="42"/>
<connect gate="G$1" pin="SCL1/RP3/GD6/CN55/RD10" pad="44"/>
<connect gate="G$1" pin="SCL2/RP17/GD5/CN18/RF5" pad="32"/>
<connect gate="G$1" pin="SDA2/RP10/GD4/CN17/RF4" pad="31"/>
<connect gate="G$1" pin="SOSCI/C3IND/CN1/RC13" pad="47"/>
<connect gate="G$1" pin="SOSCO/SCLKI/T1CK/C3INC/RPI37/CN0/RC14" pad="48"/>
<connect gate="G$1" pin="TCK/AN12/CTEDG2/CN30/RB12" pad="27"/>
<connect gate="G$1" pin="TDI/AN13/CTEDG1/CN31/RB13" pad="28"/>
<connect gate="G$1" pin="TDO/AN11/CN29/RB11" pad="24"/>
<connect gate="G$1" pin="TMS/CVREF/AN10/CN28/RB10" pad="23"/>
<connect gate="G$1" pin="VBUS/RF7" pad="34"/>
<connect gate="G$1" pin="VCAP" pad="56"/>
<connect gate="G$1" pin="VCPCON/RP24/GD9/VBUSCHG/CN50/RD1" pad="49"/>
<connect gate="G$1" pin="VDD@1" pad="10"/>
<connect gate="G$1" pin="VDD@2" pad="26"/>
<connect gate="G$1" pin="VDD@3" pad="38"/>
<connect gate="G$1" pin="VSS@1" pad="9"/>
<connect gate="G$1" pin="VSS@2" pad="25"/>
<connect gate="G$1" pin="VSS@3" pad="41"/>
<connect gate="G$1" pin="VSYNC/CN63/RE5" pad="1"/>
<connect gate="G$1" pin="VUSB" pad="35"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11312"/>
<attribute name="VALUE" value="PIC24FJ256GB206"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC24HJ32GP202">
<description>&lt;h3&gt;PIC24HJ32GP202&lt;/h3&gt;
Retired: IC-08923</description>
<gates>
<gate name="G$1" symbol="PIC24HJ32GP202"/>
</gates>
<devices>
<device name="DIP" package="DIP28_MCU">
<connects>
<connect gate="G$1" pin="AN0/VREF+/CN2/RA0" pad="2"/>
<connect gate="G$1" pin="AN1/VREF-/CN2/RA1" pad="3"/>
<connect gate="G$1" pin="AN10/RP14/CN12/RB14" pad="25"/>
<connect gate="G$1" pin="AN11/RP13/CN13/RB13" pad="24"/>
<connect gate="G$1" pin="AN12/RP12/CN14/RB12" pad="23"/>
<connect gate="G$1" pin="AN4/RP2/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="AN5/RP3/CN7/RB3" pad="7"/>
<connect gate="G$1" pin="AN9/RP15/CN11/RB15" pad="26"/>
<connect gate="G$1" pin="AVDD" pad="28"/>
<connect gate="G$1" pin="AVSS" pad="27"/>
<connect gate="G$1" pin="INT0/RP7/CN23/RB7" pad="16"/>
<connect gate="G$1" pin="MCLR" pad="1"/>
<connect gate="G$1" pin="OSCI/CLKI/CN30/RA2" pad="9"/>
<connect gate="G$1" pin="OSCO/CLKO/CN29/RA3" pad="10"/>
<connect gate="G$1" pin="PGEC1/AN3/C2IN+/RP1/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="PGEC2/TMS/RP11/CN15/RB11" pad="22"/>
<connect gate="G$1" pin="PGEC3/ASCL1/RP6/CN24/RB6" pad="15"/>
<connect gate="G$1" pin="PGED1/AN2/C2IN-/RP0/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="PGED2/TDI/RP10/CN16/RB10" pad="21"/>
<connect gate="G$1" pin="PGED3/ASDA1/RP5/CN27/RB5" pad="14"/>
<connect gate="G$1" pin="SOSCI/RP4/CN1/RB4" pad="11"/>
<connect gate="G$1" pin="SOSCO/T1CK/CN0/RA4" pad="12"/>
<connect gate="G$1" pin="TCK/SCL/RP8/CN22/RB8" pad="17"/>
<connect gate="G$1" pin="TDO/SDA1/RP9/CN12/RB9" pad="18"/>
<connect gate="G$1" pin="VCAP/VDDCORE" pad="20"/>
<connect gate="G$1" pin="VDD" pad="13"/>
<connect gate="G$1" pin="VSS@1" pad="8"/>
<connect gate="G$1" pin="VSS@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="SO-28W_MCU">
<connects>
<connect gate="G$1" pin="AN0/VREF+/CN2/RA0" pad="2"/>
<connect gate="G$1" pin="AN1/VREF-/CN2/RA1" pad="3"/>
<connect gate="G$1" pin="AN10/RP14/CN12/RB14" pad="25"/>
<connect gate="G$1" pin="AN11/RP13/CN13/RB13" pad="24"/>
<connect gate="G$1" pin="AN12/RP12/CN14/RB12" pad="23"/>
<connect gate="G$1" pin="AN4/RP2/CN6/RB2" pad="6"/>
<connect gate="G$1" pin="AN5/RP3/CN7/RB3" pad="7"/>
<connect gate="G$1" pin="AN9/RP15/CN11/RB15" pad="26"/>
<connect gate="G$1" pin="AVDD" pad="28"/>
<connect gate="G$1" pin="AVSS" pad="27"/>
<connect gate="G$1" pin="INT0/RP7/CN23/RB7" pad="16"/>
<connect gate="G$1" pin="MCLR" pad="1"/>
<connect gate="G$1" pin="OSCI/CLKI/CN30/RA2" pad="9"/>
<connect gate="G$1" pin="OSCO/CLKO/CN29/RA3" pad="10"/>
<connect gate="G$1" pin="PGEC1/AN3/C2IN+/RP1/CN5/RB1" pad="5"/>
<connect gate="G$1" pin="PGEC2/TMS/RP11/CN15/RB11" pad="22"/>
<connect gate="G$1" pin="PGEC3/ASCL1/RP6/CN24/RB6" pad="15"/>
<connect gate="G$1" pin="PGED1/AN2/C2IN-/RP0/CN4/RB0" pad="4"/>
<connect gate="G$1" pin="PGED2/TDI/RP10/CN16/RB10" pad="21"/>
<connect gate="G$1" pin="PGED3/ASDA1/RP5/CN27/RB5" pad="14"/>
<connect gate="G$1" pin="SOSCI/RP4/CN1/RB4" pad="11"/>
<connect gate="G$1" pin="SOSCO/T1CK/CN0/RA4" pad="12"/>
<connect gate="G$1" pin="TCK/SCL/RP8/CN22/RB8" pad="17"/>
<connect gate="G$1" pin="TDO/SDA1/RP9/CN12/RB9" pad="18"/>
<connect gate="G$1" pin="VCAP/VDDCORE" pad="20"/>
<connect gate="G$1" pin="VDD" pad="13"/>
<connect gate="G$1" pin="VSS@1" pad="8"/>
<connect gate="G$1" pin="VSS@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC32MX440F512H">
<description>&lt;h3&gt;PIC32MX440F512H&lt;/h3&gt;
Retired: IC-09313</description>
<gates>
<gate name="G$1" symbol="PIC32MX440F512H"/>
</gates>
<devices>
<device name="" package="SQFP-S-10X10-64_MCU">
<connects>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="AVSS" pad="20"/>
<connect gate="G$1" pin="D+/RG2" pad="37"/>
<connect gate="G$1" pin="D-/RG3" pad="36"/>
<connect gate="G$1" pin="ENVREG" pad="57"/>
<connect gate="G$1" pin="RB0/AN0/PGED1/EMUD1/PMA6/VREF+/CVREF+/CN2" pad="16"/>
<connect gate="G$1" pin="RB1/AN1/PGEC1/VREF-/CVREF-/CN3" pad="15"/>
<connect gate="G$1" pin="RB10/AN10/TMS/CVREFOUT/PMA13" pad="23"/>
<connect gate="G$1" pin="RB11/AN11/TDO/PMA12" pad="24"/>
<connect gate="G$1" pin="RB12/AN12/TCK/PMA11" pad="27"/>
<connect gate="G$1" pin="RB13/AN13/TDI/PMA10" pad="28"/>
<connect gate="G$1" pin="RB14/AN14/PMALH/PMA1/~U2RTS/BCLK2" pad="29"/>
<connect gate="G$1" pin="RB15/AN15/PMALL/PMA0/OCFB/CN12" pad="30"/>
<connect gate="G$1" pin="RB2/AN2/C2IN-/CN4" pad="14"/>
<connect gate="G$1" pin="RB3/AN3/C2IN+/CN5" pad="13"/>
<connect gate="G$1" pin="RB4/AN4/C1IN-/CN6" pad="12"/>
<connect gate="G$1" pin="RB5/AN5/VBUSON/C1IN+/CN7" pad="11"/>
<connect gate="G$1" pin="RB6/AN6/PGEC2/OCFA" pad="17"/>
<connect gate="G$1" pin="RB7/AN7/PGED2" pad="18"/>
<connect gate="G$1" pin="RB8/AN8/~U2CTS/C1OUT" pad="21"/>
<connect gate="G$1" pin="RB9/AN9/PMA7/C2OUT" pad="22"/>
<connect gate="G$1" pin="RC12/OSC1/CLKI" pad="39"/>
<connect gate="G$1" pin="RC13/SOSCI/CN1" pad="47"/>
<connect gate="G$1" pin="RC14/SOSCO/T1CK/CN0" pad="48"/>
<connect gate="G$1" pin="RC15/OSC2/CLKO" pad="40"/>
<connect gate="G$1" pin="RD0/OC1/INT0" pad="46"/>
<connect gate="G$1" pin="RD1/OC2/~U1RTS/BCLK1" pad="49"/>
<connect gate="G$1" pin="RD10/IC3/PMCS2/PMA15/INT3/SCL1" pad="44"/>
<connect gate="G$1" pin="RD11/IC4/PMCS1/PMA14/INT4" pad="45"/>
<connect gate="G$1" pin="RD2/OC3/U1RX" pad="50"/>
<connect gate="G$1" pin="RD3/OC4/U1TX" pad="51"/>
<connect gate="G$1" pin="RD4/PMWR/OC5/IC5/CN13" pad="52"/>
<connect gate="G$1" pin="RD5/PMRD/CN14" pad="53"/>
<connect gate="G$1" pin="RD6/CN15" pad="54"/>
<connect gate="G$1" pin="RD7/CN16" pad="55"/>
<connect gate="G$1" pin="RD8/IC1/RTCC/INT1" pad="42"/>
<connect gate="G$1" pin="RD9/IC2/~U1CTS//INT2/SDA1" pad="43"/>
<connect gate="G$1" pin="RE0/PMD0" pad="60"/>
<connect gate="G$1" pin="RE1/PMD1" pad="61"/>
<connect gate="G$1" pin="RE2/PMD2" pad="62"/>
<connect gate="G$1" pin="RE3/PMD3" pad="63"/>
<connect gate="G$1" pin="RE4/PMD4" pad="64"/>
<connect gate="G$1" pin="RE5/PMD5" pad="1"/>
<connect gate="G$1" pin="RE6/PMD6" pad="2"/>
<connect gate="G$1" pin="RE7/PMD7" pad="3"/>
<connect gate="G$1" pin="RF0" pad="58"/>
<connect gate="G$1" pin="RF1" pad="59"/>
<connect gate="G$1" pin="RF3/USBID" pad="33"/>
<connect gate="G$1" pin="RF4/PMA9/U2RX/SDA2/CN17" pad="31"/>
<connect gate="G$1" pin="RF5/PMA8/U2TX/SCL2/CN18" pad="32"/>
<connect gate="G$1" pin="RG6/PMA5/SCK2/CN8" pad="4"/>
<connect gate="G$1" pin="RG7/PMA4/SDI2/CN9" pad="5"/>
<connect gate="G$1" pin="RG8/PMA3/SDO2/CN10" pad="6"/>
<connect gate="G$1" pin="RG9/PMA2/~SS2/CN11" pad="8"/>
<connect gate="G$1" pin="VBUS" pad="34"/>
<connect gate="G$1" pin="VCAP/VDDCORE" pad="56"/>
<connect gate="G$1" pin="VDD@10" pad="10"/>
<connect gate="G$1" pin="VDD@26" pad="26"/>
<connect gate="G$1" pin="VDD@38" pad="38"/>
<connect gate="G$1" pin="VSS@25" pad="25"/>
<connect gate="G$1" pin="VSS@41" pad="41"/>
<connect gate="G$1" pin="VSS@9" pad="9"/>
<connect gate="G$1" pin="VUSB" pad="35"/>
<connect gate="G$1" pin="~MCLR" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UBW32_PIC32MX4XXL">
<description>&lt;h3&gt;Generic PIC32MX4XXL&lt;/h3&gt;
&lt;p&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;None&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="UBW32_PIC32MX4XXL"/>
</gates>
<devices>
<device name="TQFP100" package="UBW32_TQFP100_MCU">
<connects>
<connect gate="G$1" pin="AVDD" pad="30"/>
<connect gate="G$1" pin="AVSS" pad="31"/>
<connect gate="G$1" pin="C1IN-/AN4/CN6/RB4" pad="21"/>
<connect gate="G$1" pin="C1OUT/AN8/RB8" pad="32"/>
<connect gate="G$1" pin="C2IN+/AN3/CN5/RB3" pad="22"/>
<connect gate="G$1" pin="C2IN-/AN2/CN4/RB2" pad="23"/>
<connect gate="G$1" pin="C2OUT/AN9/RB9" pad="33"/>
<connect gate="G$1" pin="CN20/U1CTS/RD14" pad="47"/>
<connect gate="G$1" pin="CVREFOUT/PMA13/AN10/RB10" pad="34"/>
<connect gate="G$1" pin="D+/RG2" pad="57"/>
<connect gate="G$1" pin="D-/RG3" pad="56"/>
<connect gate="G$1" pin="ENVREG" pad="86"/>
<connect gate="G$1" pin="IC1/RTCC/RD8" pad="68"/>
<connect gate="G$1" pin="IC2/SS1/RD9" pad="69"/>
<connect gate="G$1" pin="IC3/SCKI/PMCS2/PMA15/RD10" pad="70"/>
<connect gate="G$1" pin="IC4/PMCS1/PMA14/RD11" pad="71"/>
<connect gate="G$1" pin="INT1/RE8" pad="18"/>
<connect gate="G$1" pin="INT2/RE9" pad="19"/>
<connect gate="G$1" pin="MCLR" pad="13"/>
<connect gate="G$1" pin="OC2/RD1" pad="76"/>
<connect gate="G$1" pin="OC3/RD2" pad="77"/>
<connect gate="G$1" pin="OC4/RD3" pad="78"/>
<connect gate="G$1" pin="OSC1/CLKI/RC12" pad="63"/>
<connect gate="G$1" pin="OSC2/CLKO/RC15" pad="64"/>
<connect gate="G$1" pin="PGC1/EMUC1/AN1/CN3/RB1" pad="24"/>
<connect gate="G$1" pin="PGC2/EMUC2/AN6/OCFA/RB6" pad="26"/>
<connect gate="G$1" pin="PGD1/EMUD1/AN0/CN2/RB0" pad="25"/>
<connect gate="G$1" pin="PGD2/EMUD2/AN7/RB7" pad="27"/>
<connect gate="G$1" pin="PMA10/AN13/RB13" pad="42"/>
<connect gate="G$1" pin="PMA11/AN12/RB12" pad="41"/>
<connect gate="G$1" pin="PMA12/AN11/RB11" pad="35"/>
<connect gate="G$1" pin="PMA2/SS2/CN11/RG9" pad="14"/>
<connect gate="G$1" pin="PMA3/SDO2/CN10/RG8" pad="12"/>
<connect gate="G$1" pin="PMA4/SDI2/CN9/RG7" pad="11"/>
<connect gate="G$1" pin="PMA5/SCK2/CN8/RG6" pad="10"/>
<connect gate="G$1" pin="PMA6/VREF+/CVREF+/RA10" pad="29"/>
<connect gate="G$1" pin="PMA7/VREF-/CVREF-/RA9" pad="28"/>
<connect gate="G$1" pin="PMA8/U2TX/CN18/RF5" pad="50"/>
<connect gate="G$1" pin="PMA9/U2RX/CN17/RF4" pad="49"/>
<connect gate="G$1" pin="PMALH/PMA1/AN14/RB14" pad="43"/>
<connect gate="G$1" pin="PMALL/PMA0/AN15/OCFB/CN12/RB15" pad="44"/>
<connect gate="G$1" pin="PMD0/RE0" pad="93"/>
<connect gate="G$1" pin="PMD1/RE1" pad="94"/>
<connect gate="G$1" pin="PMD10/RF1" pad="88"/>
<connect gate="G$1" pin="PMD11/RF0" pad="87"/>
<connect gate="G$1" pin="PMD12/IC5/RD12" pad="79"/>
<connect gate="G$1" pin="PMD13/CN19/RD13" pad="80"/>
<connect gate="G$1" pin="PMD14/CN15/RD6" pad="83"/>
<connect gate="G$1" pin="PMD15/CN16/RD7" pad="84"/>
<connect gate="G$1" pin="PMD2/RE2" pad="98"/>
<connect gate="G$1" pin="PMD3/RE3" pad="99"/>
<connect gate="G$1" pin="PMD4/RE4" pad="100"/>
<connect gate="G$1" pin="PMD5/RE5" pad="3"/>
<connect gate="G$1" pin="PMD6/RE6" pad="4"/>
<connect gate="G$1" pin="PMD7/RE7" pad="5"/>
<connect gate="G$1" pin="PMD8/RG0" pad="90"/>
<connect gate="G$1" pin="PMD9/RG1" pad="89"/>
<connect gate="G$1" pin="PMRD/CN14/RD5" pad="82"/>
<connect gate="G$1" pin="PMWR/OC5/CN13/RD4" pad="81"/>
<connect gate="G$1" pin="RG15" pad="1"/>
<connect gate="G$1" pin="SCL1/INT3/RA14" pad="66"/>
<connect gate="G$1" pin="SCL2/RA2" pad="58"/>
<connect gate="G$1" pin="SDA1/INT4/RA15" pad="67"/>
<connect gate="G$1" pin="SDA2/RA3" pad="59"/>
<connect gate="G$1" pin="SDI1/T5CK/RC4" pad="9"/>
<connect gate="G$1" pin="SDO1/OC1/INT0/RD0" pad="72"/>
<connect gate="G$1" pin="SOSCI/CN1/RC13" pad="73"/>
<connect gate="G$1" pin="SOSCO/T1CK/CN0/RC14" pad="74"/>
<connect gate="G$1" pin="T2CK/RC1" pad="6"/>
<connect gate="G$1" pin="T3CK/RC2" pad="7"/>
<connect gate="G$1" pin="T4CK/RC3" pad="8"/>
<connect gate="G$1" pin="TCK/RA1" pad="38"/>
<connect gate="G$1" pin="TDI/RA4" pad="60"/>
<connect gate="G$1" pin="TDO/RA5" pad="61"/>
<connect gate="G$1" pin="TMS/RA0" pad="17"/>
<connect gate="G$1" pin="TRCLK/RA6" pad="91"/>
<connect gate="G$1" pin="TRD0/RG13" pad="97"/>
<connect gate="G$1" pin="TRD1/RG12" pad="96"/>
<connect gate="G$1" pin="TRD2/RG14" pad="95"/>
<connect gate="G$1" pin="TRD3/RA7" pad="92"/>
<connect gate="G$1" pin="U1RTS/BCLK1/CN21/RD15" pad="48"/>
<connect gate="G$1" pin="U1RX/RF2" pad="52"/>
<connect gate="G$1" pin="U1TX/RF8" pad="53"/>
<connect gate="G$1" pin="U2CTS/RF12" pad="40"/>
<connect gate="G$1" pin="U2RTS/BCLK2/RF13" pad="39"/>
<connect gate="G$1" pin="USBID/RF3" pad="51"/>
<connect gate="G$1" pin="VBUS" pad="54"/>
<connect gate="G$1" pin="VBUSON/C1IN+/AN5/CN7/RB5" pad="20"/>
<connect gate="G$1" pin="VCAP/VDDCORE" pad="85"/>
<connect gate="G$1" pin="VDD1" pad="2"/>
<connect gate="G$1" pin="VDD2" pad="16"/>
<connect gate="G$1" pin="VDD3" pad="37"/>
<connect gate="G$1" pin="VDD4" pad="46"/>
<connect gate="G$1" pin="VDD5" pad="62"/>
<connect gate="G$1" pin="VSS1" pad="15"/>
<connect gate="G$1" pin="VSS2" pad="36"/>
<connect gate="G$1" pin="VSS3" pad="45"/>
<connect gate="G$1" pin="VSS4" pad="65"/>
<connect gate="G$1" pin="VSS6" pad="75"/>
<connect gate="G$1" pin="VUSB" pad="55"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XMEGA-100">
<description>&lt;h3&gt;Atmel XMega uC&lt;/h3&gt;
Not in catalog</description>
<gates>
<gate name="G$1" symbol="XMEGA"/>
</gates>
<devices>
<device name="SMD" package="TQFP-100-14X14MM_MCU">
<connects>
<connect gate="G$1" pin="AVCC@4" pad="4"/>
<connect gate="G$1" pin="AVCC@94" pad="94"/>
<connect gate="G$1" pin="GND@13" pad="13"/>
<connect gate="G$1" pin="GND@23" pad="23"/>
<connect gate="G$1" pin="GND@3" pad="3"/>
<connect gate="G$1" pin="GND@33" pad="33"/>
<connect gate="G$1" pin="GND@43" pad="43"/>
<connect gate="G$1" pin="GND@53" pad="53"/>
<connect gate="G$1" pin="GND@63" pad="63"/>
<connect gate="G$1" pin="GND@73" pad="73"/>
<connect gate="G$1" pin="GND@84" pad="84"/>
<connect gate="G$1" pin="GND@93" pad="93"/>
<connect gate="G$1" pin="PA0" pad="95"/>
<connect gate="G$1" pin="PA1" pad="96"/>
<connect gate="G$1" pin="PA2" pad="97"/>
<connect gate="G$1" pin="PA3" pad="98"/>
<connect gate="G$1" pin="PA4" pad="99"/>
<connect gate="G$1" pin="PA5" pad="100"/>
<connect gate="G$1" pin="PA6" pad="1"/>
<connect gate="G$1" pin="PA7" pad="2"/>
<connect gate="G$1" pin="PB0" pad="5"/>
<connect gate="G$1" pin="PB1" pad="6"/>
<connect gate="G$1" pin="PB2" pad="7"/>
<connect gate="G$1" pin="PB3" pad="8"/>
<connect gate="G$1" pin="PB4" pad="9"/>
<connect gate="G$1" pin="PB5" pad="10"/>
<connect gate="G$1" pin="PB6" pad="11"/>
<connect gate="G$1" pin="PB7" pad="12"/>
<connect gate="G$1" pin="PC0" pad="15"/>
<connect gate="G$1" pin="PC1" pad="16"/>
<connect gate="G$1" pin="PC2" pad="17"/>
<connect gate="G$1" pin="PC3" pad="18"/>
<connect gate="G$1" pin="PC4" pad="19"/>
<connect gate="G$1" pin="PC5" pad="20"/>
<connect gate="G$1" pin="PC6" pad="21"/>
<connect gate="G$1" pin="PC7" pad="22"/>
<connect gate="G$1" pin="PD0" pad="25"/>
<connect gate="G$1" pin="PD1" pad="26"/>
<connect gate="G$1" pin="PD2" pad="27"/>
<connect gate="G$1" pin="PD3" pad="28"/>
<connect gate="G$1" pin="PD4" pad="29"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PD6" pad="31"/>
<connect gate="G$1" pin="PD7" pad="32"/>
<connect gate="G$1" pin="PDI/PDI_DATA" pad="89"/>
<connect gate="G$1" pin="PE0" pad="35"/>
<connect gate="G$1" pin="PE1" pad="36"/>
<connect gate="G$1" pin="PE2" pad="37"/>
<connect gate="G$1" pin="PE3" pad="38"/>
<connect gate="G$1" pin="PE4" pad="39"/>
<connect gate="G$1" pin="PE5" pad="40"/>
<connect gate="G$1" pin="PE6" pad="41"/>
<connect gate="G$1" pin="PE7" pad="42"/>
<connect gate="G$1" pin="PF0" pad="45"/>
<connect gate="G$1" pin="PF1" pad="46"/>
<connect gate="G$1" pin="PF2" pad="47"/>
<connect gate="G$1" pin="PF3" pad="48"/>
<connect gate="G$1" pin="PF4" pad="49"/>
<connect gate="G$1" pin="PF5" pad="50"/>
<connect gate="G$1" pin="PF6" pad="51"/>
<connect gate="G$1" pin="PF7" pad="52"/>
<connect gate="G$1" pin="PH0" pad="55"/>
<connect gate="G$1" pin="PH1" pad="56"/>
<connect gate="G$1" pin="PH2" pad="57"/>
<connect gate="G$1" pin="PH3" pad="58"/>
<connect gate="G$1" pin="PH4" pad="59"/>
<connect gate="G$1" pin="PH5" pad="60"/>
<connect gate="G$1" pin="PH6" pad="61"/>
<connect gate="G$1" pin="PH7" pad="62"/>
<connect gate="G$1" pin="PJ0" pad="65"/>
<connect gate="G$1" pin="PJ1" pad="66"/>
<connect gate="G$1" pin="PJ2" pad="67"/>
<connect gate="G$1" pin="PJ3" pad="68"/>
<connect gate="G$1" pin="PJ4" pad="69"/>
<connect gate="G$1" pin="PJ5" pad="70"/>
<connect gate="G$1" pin="PJ6" pad="71"/>
<connect gate="G$1" pin="PJ7" pad="72"/>
<connect gate="G$1" pin="PK0" pad="75"/>
<connect gate="G$1" pin="PK1" pad="76"/>
<connect gate="G$1" pin="PK2" pad="77"/>
<connect gate="G$1" pin="PK3" pad="78"/>
<connect gate="G$1" pin="PK4" pad="79"/>
<connect gate="G$1" pin="PK5" pad="80"/>
<connect gate="G$1" pin="PK6" pad="81"/>
<connect gate="G$1" pin="PK7" pad="82"/>
<connect gate="G$1" pin="PQ0" pad="85"/>
<connect gate="G$1" pin="PQ1" pad="86"/>
<connect gate="G$1" pin="PQ2" pad="87"/>
<connect gate="G$1" pin="PQ3" pad="88"/>
<connect gate="G$1" pin="PR0" pad="91"/>
<connect gate="G$1" pin="PR1" pad="92"/>
<connect gate="G$1" pin="RESET/PDI_CLOCK" pad="90"/>
<connect gate="G$1" pin="VCC@14" pad="14"/>
<connect gate="G$1" pin="VCC@24" pad="24"/>
<connect gate="G$1" pin="VCC@34" pad="34"/>
<connect gate="G$1" pin="VCC@44" pad="44"/>
<connect gate="G$1" pin="VCC@54" pad="54"/>
<connect gate="G$1" pin="VCC@64" pad="64"/>
<connect gate="G$1" pin="VCC@74" pad="74"/>
<connect gate="G$1" pin="VCC@83" pad="83"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XMEGA-A3">
<description>&lt;h3&gt;Atmel's 8/16-bit AVR XMEGA A3 Microcontroller - ATxmega256A3, etc.&lt;/h3&gt;
Retired: IC-09806 - ATXMEGA256A3&lt;br&gt;
Retired: IC-09429 - ATXMEGA128A1&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="XMEGA-A3B"/>
</gates>
<devices>
<device name="-AU" package="TQFP64_14X14MM_MCU">
<connects>
<connect gate="G$1" pin="/RESET_PDI_CLK" pad="57"/>
<connect gate="G$1" pin="AGND" pad="60"/>
<connect gate="G$1" pin="AVCC" pad="61"/>
<connect gate="G$1" pin="GND1" pad="14"/>
<connect gate="G$1" pin="GND2" pad="24"/>
<connect gate="G$1" pin="GND3" pad="34"/>
<connect gate="G$1" pin="GND4" pad="44"/>
<connect gate="G$1" pin="GND5" pad="52"/>
<connect gate="G$1" pin="PA0(ADC0/AC0/AREF)" pad="62"/>
<connect gate="G$1" pin="PA1(ADC1/AC1)" pad="63"/>
<connect gate="G$1" pin="PA2(ADC2/AC2)" pad="64"/>
<connect gate="G$1" pin="PA3(ADC3/AC3)" pad="1"/>
<connect gate="G$1" pin="PA4(ADC4/AC4)" pad="2"/>
<connect gate="G$1" pin="PA5(ADC5/AC5)" pad="3"/>
<connect gate="G$1" pin="PA6(ADC6/AC6)" pad="4"/>
<connect gate="G$1" pin="PA7(ADC7/AC7/AC0OUT)" pad="5"/>
<connect gate="G$1" pin="PB0(ADC0/AC0/AREF)" pad="6"/>
<connect gate="G$1" pin="PB1(ADC1/AC1)" pad="7"/>
<connect gate="G$1" pin="PB2(ADC2/AC2/DAC0)" pad="8"/>
<connect gate="G$1" pin="PB3(ADC3/AC3/DAC1)" pad="9"/>
<connect gate="G$1" pin="PB4(ADC4/AC4/TMS)" pad="10"/>
<connect gate="G$1" pin="PB5(ADC5/AC5/TDI)" pad="11"/>
<connect gate="G$1" pin="PB6(ADC6/AC6/TCK)" pad="12"/>
<connect gate="G$1" pin="PB7(ADC7/AC7/AC0OUT/TDO)" pad="13"/>
<connect gate="G$1" pin="PC0(OC0A/OC0AL/SDA)" pad="16"/>
<connect gate="G$1" pin="PC1(OC0B/AC0AH/XCK0/SCL)" pad="17"/>
<connect gate="G$1" pin="PC2(OC0C/OC0BL/RXD0)" pad="18"/>
<connect gate="G$1" pin="PC3(OC0D/OX0BH/TXD0)" pad="19"/>
<connect gate="G$1" pin="PC4(AC1A/OC0CL/SS)" pad="20"/>
<connect gate="G$1" pin="PC5(OC1B/OC0CH/XCK1/MOSI)" pad="21"/>
<connect gate="G$1" pin="PC6(OC0DL/RXD1/MISO)" pad="22"/>
<connect gate="G$1" pin="PC7(OC0DH/CKOUT/EVO/TXD1/SCK)" pad="23"/>
<connect gate="G$1" pin="PD0(OC0A)" pad="26"/>
<connect gate="G$1" pin="PD1(OC0B/XCK0)" pad="27"/>
<connect gate="G$1" pin="PD2(OC0C/RXD0)" pad="28"/>
<connect gate="G$1" pin="PD3(OX0D/TXD0)" pad="29"/>
<connect gate="G$1" pin="PD4(OC1A/SS)" pad="30"/>
<connect gate="G$1" pin="PD5(OC1B/XCK1/MOSI)" pad="31"/>
<connect gate="G$1" pin="PD6(RXD1/MISO)" pad="32"/>
<connect gate="G$1" pin="PD7(CKOUT/EVO/TXD1/SCK)" pad="33"/>
<connect gate="G$1" pin="PDI_DATA" pad="56"/>
<connect gate="G$1" pin="PE0(OC0A/SDA)" pad="36"/>
<connect gate="G$1" pin="PE1(OC0B/XCK0/SCL)" pad="37"/>
<connect gate="G$1" pin="PE2(OC0C/RXD0)" pad="38"/>
<connect gate="G$1" pin="PE3(OC0D/TXD0)" pad="39"/>
<connect gate="G$1" pin="PE4(OC1A/SS)" pad="40"/>
<connect gate="G$1" pin="PE5(OC1B/XCK1/MOSI)" pad="41"/>
<connect gate="G$1" pin="PE6(TOSC2/RXD1/MISO)" pad="42"/>
<connect gate="G$1" pin="PE7(TOSC1/CKOUT/EVO/TXD1/SCK)" pad="43"/>
<connect gate="G$1" pin="PF0(OC0A)" pad="46"/>
<connect gate="G$1" pin="PF1(OC0B/XCK0)" pad="47"/>
<connect gate="G$1" pin="PF2(OC0C/RXD0)" pad="48"/>
<connect gate="G$1" pin="PF3(OC0D/TXD0)" pad="49"/>
<connect gate="G$1" pin="PF4" pad="50"/>
<connect gate="G$1" pin="PF5" pad="51"/>
<connect gate="G$1" pin="PF6" pad="54"/>
<connect gate="G$1" pin="PF7" pad="55"/>
<connect gate="G$1" pin="PR0(XTAL2)" pad="58"/>
<connect gate="G$1" pin="PR1(XTAL1)" pad="59"/>
<connect gate="G$1" pin="VCC1" pad="15"/>
<connect gate="G$1" pin="VCC2" pad="25"/>
<connect gate="G$1" pin="VCC3" pad="35"/>
<connect gate="G$1" pin="VCC4" pad="45"/>
<connect gate="G$1" pin="VCC5" pad="53"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P8X32A-Q44" prefix="U" uservalue="yes">
<description>&lt;h3&gt;Propellor uC&lt;/h3&gt;
RETIRED</description>
<gates>
<gate name="P" symbol="4VDD4VSS"/>
<gate name="P8X32A-Q44" symbol="P8X32A"/>
</gates>
<devices>
<device name="" package="P8X32A-Q44_MCU">
<connects>
<connect gate="P" pin="VDD@1" pad="8"/>
<connect gate="P" pin="VDD@2" pad="18"/>
<connect gate="P" pin="VDD@3" pad="30"/>
<connect gate="P" pin="VDD@4" pad="40"/>
<connect gate="P" pin="VSS@1" pad="5"/>
<connect gate="P" pin="VSS@2" pad="17"/>
<connect gate="P" pin="VSS@3" pad="27"/>
<connect gate="P" pin="VSS@4" pad="39"/>
<connect gate="P8X32A-Q44" pin="BOE/" pad="6"/>
<connect gate="P8X32A-Q44" pin="P0" pad="41"/>
<connect gate="P8X32A-Q44" pin="P1" pad="42"/>
<connect gate="P8X32A-Q44" pin="P10" pad="11"/>
<connect gate="P8X32A-Q44" pin="P11" pad="12"/>
<connect gate="P8X32A-Q44" pin="P12" pad="13"/>
<connect gate="P8X32A-Q44" pin="P13" pad="14"/>
<connect gate="P8X32A-Q44" pin="P14" pad="15"/>
<connect gate="P8X32A-Q44" pin="P15" pad="16"/>
<connect gate="P8X32A-Q44" pin="P16" pad="19"/>
<connect gate="P8X32A-Q44" pin="P17" pad="20"/>
<connect gate="P8X32A-Q44" pin="P18" pad="21"/>
<connect gate="P8X32A-Q44" pin="P19" pad="22"/>
<connect gate="P8X32A-Q44" pin="P2" pad="43"/>
<connect gate="P8X32A-Q44" pin="P20" pad="23"/>
<connect gate="P8X32A-Q44" pin="P21" pad="24"/>
<connect gate="P8X32A-Q44" pin="P22" pad="25"/>
<connect gate="P8X32A-Q44" pin="P23" pad="26"/>
<connect gate="P8X32A-Q44" pin="P24" pad="31"/>
<connect gate="P8X32A-Q44" pin="P25" pad="32"/>
<connect gate="P8X32A-Q44" pin="P26" pad="33"/>
<connect gate="P8X32A-Q44" pin="P27" pad="34"/>
<connect gate="P8X32A-Q44" pin="P28" pad="35"/>
<connect gate="P8X32A-Q44" pin="P29" pad="36"/>
<connect gate="P8X32A-Q44" pin="P3" pad="44"/>
<connect gate="P8X32A-Q44" pin="P30" pad="37"/>
<connect gate="P8X32A-Q44" pin="P31" pad="38"/>
<connect gate="P8X32A-Q44" pin="P4" pad="1"/>
<connect gate="P8X32A-Q44" pin="P5" pad="2"/>
<connect gate="P8X32A-Q44" pin="P6" pad="3"/>
<connect gate="P8X32A-Q44" pin="P7" pad="4"/>
<connect gate="P8X32A-Q44" pin="P8" pad="9"/>
<connect gate="P8X32A-Q44" pin="P9" pad="10"/>
<connect gate="P8X32A-Q44" pin="RES/" pad="7"/>
<connect gate="P8X32A-Q44" pin="XI" pad="28"/>
<connect gate="P8X32A-Q44" pin="XO" pad="29"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-10929"/>
<attribute name="VALUE" value="P8X32A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC214X" prefix="U">
<description>&lt;h3&gt;NXP LPC2144/2146/2148&lt;/h3&gt;
&lt;p&gt;ARM7 MCU FLASH 512K 64LQFP&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Widgets/LPC2141_42_44_46_48.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12772"&gt;SparkFun Logomatic v2 - Serial SD Datalogger (FAT32)&lt;/a&gt; (WIG-12772)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="LPC213X-1"/>
</gates>
<devices>
<device name="" package="LQFP-10X10-64_MCU">
<connects>
<connect gate="G$1" pin="!RESET" pad="57"/>
<connect gate="G$1" pin="(AD0.1/CAP0.2/MAT0.2)P0.28" pad="13"/>
<connect gate="G$1" pin="(AD0.2/CAP0.3/MAT0.3)P0.29" pad="14"/>
<connect gate="G$1" pin="(AD0.3/EINT3/CAP0.0)P0.30" pad="15"/>
<connect gate="G$1" pin="(AD0.4/AOUT)P0.25" pad="9"/>
<connect gate="G$1" pin="(AD1.7/CAP0.0/MAT0.0)P0.22" pad="2"/>
<connect gate="G$1" pin="(CAP1.2/SCK1/MAT1.2)P0.17" pad="47"/>
<connect gate="G$1" pin="(CAP1.3/MISO1/MAT1.3)P0.18" pad="53"/>
<connect gate="G$1" pin="(CTS1/CAP1.1/SCL1)P0.11" pad="37"/>
<connect gate="G$1" pin="(DCD1/EINT1/SDA1)P0.14" pad="41"/>
<connect gate="G$1" pin="(DSR1/MAT1.0/AD1.3)P0.12" pad="38"/>
<connect gate="G$1" pin="(DTR1/MAT1.1/AD1.4)P0.13" pad="39"/>
<connect gate="G$1" pin="(EINT0/MAT0.2/CAP0.2)P0.16" pad="46"/>
<connect gate="G$1" pin="(MAT1.2/MOSI1/CAP1.2)P0.19" pad="54"/>
<connect gate="G$1" pin="(MAT1.3/SSEL1/EINT3)P0.20" pad="55"/>
<connect gate="G$1" pin="(MISO0/MAT0.1/A0.7)P0.5" pad="29"/>
<connect gate="G$1" pin="(MOSI0/CAP0.2/AD1.0)P0.6" pad="30"/>
<connect gate="G$1" pin="(PWM5/AD1.6/CAP1.3)P0.21" pad="1"/>
<connect gate="G$1" pin="(RI1/EINT2/AD1.5)P0.15" pad="45"/>
<connect gate="G$1" pin="(RTS1/CAP1.0/AD1.2)P0.10" pad="35"/>
<connect gate="G$1" pin="(RXD0/PWM3/EINT0)P0.1" pad="21"/>
<connect gate="G$1" pin="(RXD1/PWM6/EINT3)P0.9" pad="34"/>
<connect gate="G$1" pin="(SCK0/CAP0.1/AD0.6)P0.4" pad="27"/>
<connect gate="G$1" pin="(SCL0/CAP0.0)P0.2" pad="22"/>
<connect gate="G$1" pin="(SDA0/MAT0.0/EINT1)P0.3" pad="26"/>
<connect gate="G$1" pin="(SSEL0/PWM2/EINT2)P0.7" pad="31"/>
<connect gate="G$1" pin="(TXD0/PWM1)P0.0" pad="19"/>
<connect gate="G$1" pin="(TXD1/PWM4/A1.1)P0.8" pad="33"/>
<connect gate="G$1" pin="(UP_LED/CONNECT)P0.31" pad="17"/>
<connect gate="G$1" pin="(VBUS)P0.23" pad="58"/>
<connect gate="G$1" pin="D+" pad="10"/>
<connect gate="G$1" pin="D-" pad="11"/>
<connect gate="G$1" pin="P1.16(TRACEPKT0)" pad="16"/>
<connect gate="G$1" pin="P1.17(TRACEPKT1)" pad="12"/>
<connect gate="G$1" pin="P1.18(TRACEPKT2)" pad="8"/>
<connect gate="G$1" pin="P1.19(TRACEPKT3)" pad="4"/>
<connect gate="G$1" pin="P1.20(TRACESYNC)" pad="48"/>
<connect gate="G$1" pin="P1.21(PIPESTAT0)" pad="44"/>
<connect gate="G$1" pin="P1.22(PIPESTAT1)" pad="40"/>
<connect gate="G$1" pin="P1.23(PIPESTAT2)" pad="36"/>
<connect gate="G$1" pin="P1.24(TRACECLK)" pad="32"/>
<connect gate="G$1" pin="P1.25(EXTIN0)" pad="28"/>
<connect gate="G$1" pin="P1.26(RTCK)" pad="24"/>
<connect gate="G$1" pin="P1.27(TDO)" pad="64"/>
<connect gate="G$1" pin="P1.28(TDI)" pad="60"/>
<connect gate="G$1" pin="P1.29(TCK)" pad="56"/>
<connect gate="G$1" pin="P1.30(TMS)" pad="52"/>
<connect gate="G$1" pin="P1.31(/TRST)" pad="20"/>
<connect gate="G$1" pin="RTXC1" pad="3"/>
<connect gate="G$1" pin="RTXC2" pad="5"/>
<connect gate="G$1" pin="VBAT" pad="49"/>
<connect gate="G$1" pin="VDD@1" pad="23"/>
<connect gate="G$1" pin="VDD@2" pad="43"/>
<connect gate="G$1" pin="VDD@3" pad="51"/>
<connect gate="G$1" pin="VDDA" pad="7"/>
<connect gate="G$1" pin="VREF" pad="63"/>
<connect gate="G$1" pin="VSS@1" pad="6"/>
<connect gate="G$1" pin="VSS@2" pad="18"/>
<connect gate="G$1" pin="VSS@3" pad="25"/>
<connect gate="G$1" pin="VSS@4" pad="42"/>
<connect gate="G$1" pin="VSS@5" pad="50"/>
<connect gate="G$1" pin="VSSA" pad="59"/>
<connect gate="G$1" pin="XTAL1" pad="62"/>
<connect gate="G$1" pin="XTAL2" pad="61"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-07934"/>
<attribute name="VALUE" value="LPC2148"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB+SHIELD">
<description>&lt;h3&gt;USB+Shield&lt;/h3&gt;
USB connector with shield pins connectable</description>
<gates>
<gate name="G$1" symbol="USB+SHIELD"/>
</gates>
<devices>
<device name="" package="USB-B-PTH">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="S1" pad="S1"/>
<connect gate="G$1" pin="S2" pad="S2"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB" prefix="J">
<description>&lt;b&gt;USB Connectors&lt;/b&gt;
&lt;p&gt;USB-B-PTH is fully proven SKU : PRT-00139/CONN-08278
&lt;p&gt;USB-miniB is fully proven SKU : PRT-00587
&lt;p&gt;USB-A-PCB is untested.
&lt;p&gt;USB-A-H is throughly reviewed, but untested. Spark Fun Electronics SKU : PRT-00437
&lt;p&gt;USB-B-SMT is throughly reviewed, but untested. Needs silkscreen touching up.
&lt;p&gt;USB-A-S has not been used/tested
&lt;p&gt;USB-MB-H has not been used/tested
&lt;P&gt;USB-MICROB has been used. CONN-09505</description>
<gates>
<gate name="G$1" symbol="USB"/>
</gates>
<devices>
<device name="-MB-H" package="USB-MB-H">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="OLD" package="USB-MINIB-OLD">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-JST-2MM-SMT" package="S4B-PH">
<connects>
<connect gate="G$1" pin="D+" pad="2"/>
<connect gate="G$1" pin="D-" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VBUS" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08193"/>
</technology>
</technologies>
</device>
<device name="SMD" package="USB-MINIB">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08193"/>
</technology>
</technologies>
</device>
<device name="-SMD-NS" package="USB-MINIB-NOSTOP">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MICROB" package="USB-MICROB">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND MT1 MT2"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09505"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MINI-DIN6">
<description>&lt;h3&gt;Mini DIN 6 Connector&lt;/h3&gt;

SparkFun used to sell this connector and has used it on a couple designs, however the connector and the designs are now retired. &lt;br&gt;&lt;/br&gt;
&lt;br&gt;&lt;/br&gt;
&lt;a href="https://www.sparkfun.com/products/retired/8509"&gt;Mini DIN 6 Connector [RETIRED]&lt;/a&gt;
&lt;br&gt;&lt;/br&gt;
&lt;br&gt;&lt;/br&gt;
&lt;a href="https://www.sparkfun.com/products/retired/8652"&gt;SparkFun Key Counter - PS2 [RETIRED]&lt;/a&gt;
&lt;br&gt;&lt;/br&gt;
&lt;br&gt;&lt;/br&gt;
Commonly found on the back of a computer for PS2 keyboard and mice. Schematic and footprint are proven.</description>
<gates>
<gate name="G$1" symbol="CONN_06"/>
</gates>
<devices>
<device name="PTH" package="MINI-DIN6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RJ9">
<description>This is a 4-pin connector commonly found on phone handsets. Great for simple TX/RX/PWR/GND connections. Sometime referred to as RJ9 or 4P4C.
&lt;br&gt;&lt;/br&gt;
&lt;br&gt;&lt;/br&gt;
SparkFun does not currently use this on any active designs, and the connector alone has been retired. However, for more info visit here:
&lt;br&gt;&lt;/br&gt;
&lt;br&gt;&lt;/br&gt;
&lt;a href="https://www.sparkfun.com/products/retired/8694"&gt;https://www.sparkfun.com/products/retired/8694&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="CONN_04"/>
</gates>
<devices>
<device name="PTH" package="RJ9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="COMPUTER_PERIPHERAL_POWER" prefix="J">
<gates>
<gate name="G$1" symbol="COMPUTER-PERIPHERAL-POWER"/>
</gates>
<devices>
<device name="RA" package="COMPUTER-PERIPHERAL-POWER-RA">
<connects>
<connect gate="G$1" pin="12V" pad="12V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="NC" pad="NC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VERTICAL" package="COMPUTER-PERIPHERAL-POWER">
<connects>
<connect gate="G$1" pin="12V" pad="12V"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="NC" pad="NC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINH2X12">
<gates>
<gate name="G$1" symbol="PINH2X12"/>
</gates>
<devices>
<device name="" package="2X12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X3" prefix="J" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X3"/>
</gates>
<devices>
<device name="" package="2X03">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X10" prefix="J" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X10"/>
</gates>
<devices>
<device name="" package="2X10">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X26">
<gates>
<gate name="G$1" symbol="PINH2X26"/>
</gates>
<devices>
<device name="" package="2X26">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="41" pad="41"/>
<connect gate="G$1" pin="42" pad="42"/>
<connect gate="G$1" pin="43" pad="43"/>
<connect gate="G$1" pin="44" pad="44"/>
<connect gate="G$1" pin="45" pad="45"/>
<connect gate="G$1" pin="46" pad="46"/>
<connect gate="G$1" pin="47" pad="47"/>
<connect gate="G$1" pin="48" pad="48"/>
<connect gate="G$1" pin="49" pad="49"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="50" pad="50"/>
<connect gate="G$1" pin="51" pad="51"/>
<connect gate="G$1" pin="52" pad="52"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RASPBERRYPI-GPIO" prefix="J">
<description>RASPBERRY PI I/O HEADER

As defined for the Revistion 2 Pi.</description>
<gates>
<gate name="JP1" symbol="RASPBERRYPI-GPIO"/>
</gates>
<devices>
<device name="PTH" package="2X13-SHROUDED">
<connects>
<connect gate="JP1" pin="3.3V@1" pad="1"/>
<connect gate="JP1" pin="3.3V@17" pad="17"/>
<connect gate="JP1" pin="5V@2" pad="2"/>
<connect gate="JP1" pin="5V@4" pad="4"/>
<connect gate="JP1" pin="CE0" pad="24"/>
<connect gate="JP1" pin="CE1" pad="26"/>
<connect gate="JP1" pin="GND@14" pad="14"/>
<connect gate="JP1" pin="GND@20" pad="20"/>
<connect gate="JP1" pin="GND@25" pad="25"/>
<connect gate="JP1" pin="GND@6" pad="6"/>
<connect gate="JP1" pin="GND@9" pad="9"/>
<connect gate="JP1" pin="GP17" pad="11"/>
<connect gate="JP1" pin="GP18#" pad="12"/>
<connect gate="JP1" pin="GP22" pad="15"/>
<connect gate="JP1" pin="GP23" pad="16"/>
<connect gate="JP1" pin="GP24" pad="18"/>
<connect gate="JP1" pin="GP25" pad="22"/>
<connect gate="JP1" pin="GP27" pad="13"/>
<connect gate="JP1" pin="GP4" pad="7"/>
<connect gate="JP1" pin="MISO" pad="21"/>
<connect gate="JP1" pin="MOSI" pad="19"/>
<connect gate="JP1" pin="RXI" pad="10"/>
<connect gate="JP1" pin="SCL" pad="5"/>
<connect gate="JP1" pin="SCLK" pad="23"/>
<connect gate="JP1" pin="SDA" pad="3"/>
<connect gate="JP1" pin="TXO" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIST" value="sparkfun"/>
<attribute name="DIST_ID" value="PRT-11490"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AUDIO_JACK_TRS_0.25&quot;_PTH_VERTICAL" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Audio Jack, 1/4" TRS jack, VERTICLEl, PTH, aka "Phono jack"&lt;/h3&gt;
&lt;p&gt;&lt;/p&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Note, this footprint is UN-proven. It has not yet been used by SparkFun on a design.&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="AUDIO-JACK5-TRS-NORMALED"/>
</gates>
<devices>
<device name="" package="AUDIO_JACK_0.25&quot;_TRS_PTH_VERTICAL">
<connects>
<connect gate="G$1" pin="EARTH" pad="SLEEVE"/>
<connect gate="G$1" pin="RING" pad="RING"/>
<connect gate="G$1" pin="RING-NORM" pad="RING-NORM"/>
<connect gate="G$1" pin="TIP" pad="TIP"/>
<connect gate="G$1" pin="TIP-NORM" pad="TIP-NORM"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COM-11152"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USD-SOCKET" prefix="JP">
<description>&lt;b&gt;microSD Socket&lt;/b&gt;
Push-push type uSD socket. Schematic element and footprint production proven. Spark Fun Electronics SKU : PRT-00127. tDoc lines correctly indicate media card edge positions when inserting (unlocked, locked, depressed).

NOTE: CD1 and CD2 are connected internally</description>
<gates>
<gate name="G$1" symbol="USDCARD"/>
</gates>
<devices>
<device name="USD" package="USD-SOCKET-PP">
<connects>
<connect gate="G$1" pin="CD1" pad="CD2"/>
<connect gate="G$1" pin="CD2" pad="GND2"/>
<connect gate="G$1" pin="CS" pad="2"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="7"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="RSV" pad="8"/>
<connect gate="G$1" pin="SCK" pad="5"/>
<connect gate="G$1" pin="SHIELD@1" pad="CD1"/>
<connect gate="G$1" pin="SHIELD@3" pad="GND1"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NEW" package="MICRO-SD-SOCKET-PP">
<connects>
<connect gate="G$1" pin="CD1" pad="CD1"/>
<connect gate="G$1" pin="CD2" pad="CD2"/>
<connect gate="G$1" pin="CS" pad="CS"/>
<connect gate="G$1" pin="DI" pad="DI"/>
<connect gate="G$1" pin="DO" pad="DO"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="NC" pad="RSV1"/>
<connect gate="G$1" pin="RSV" pad="RSV2"/>
<connect gate="G$1" pin="SCK" pad="SCLK"/>
<connect gate="G$1" pin="SHIELD@1" pad="GND3"/>
<connect gate="G$1" pin="SHIELD@3" pad="GND1"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-07820"/>
</technology>
</technologies>
</device>
<device name="" package="MICROSD_1:1">
<connects>
<connect gate="G$1" pin="CD1" pad="CD1"/>
<connect gate="G$1" pin="CD2" pad="CD2"/>
<connect gate="G$1" pin="CS" pad="2"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="7"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="RSV" pad="8"/>
<connect gate="G$1" pin="SCK" pad="5"/>
<connect gate="G$1" pin="SHIELD@1" pad="GND3"/>
<connect gate="G$1" pin="SHIELD@3" pad="GND1"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-07820"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USD-SDIO-SOCKET" prefix="JP">
<description>microSD Socket
&lt;br&gt;&lt;br&gt;
Push-push type uSD socket with full SDIO signal mapping. Spark Fun Electronics SKU : PRT-00127. tDoc lines correctly indicate media card edge positions when inserting (unlocked, locked, depressed). NOTE: CD1 and CD2 are connected internally, and short to ground when card is removed.</description>
<gates>
<gate name="G$1" symbol="USDCARD_SDIO"/>
</gates>
<devices>
<device name="" package="MICRO-SD-SOCKET-SDIO">
<connects>
<connect gate="G$1" pin="CD/DAT3" pad="CD/DAT3"/>
<connect gate="G$1" pin="CD1" pad="CD1"/>
<connect gate="G$1" pin="CD2" pad="CD2"/>
<connect gate="G$1" pin="CLK" pad="CLK"/>
<connect gate="G$1" pin="CMD" pad="CMD"/>
<connect gate="G$1" pin="DAT0" pad="DAT0"/>
<connect gate="G$1" pin="DAT1" pad="DAT1"/>
<connect gate="G$1" pin="DAT2" pad="DAT2"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="SHIELD@1" pad="GND1"/>
<connect gate="G$1" pin="SHIELD@3" pad="GND3"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-07820"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DRV8830" prefix="U">
<description>&lt;h2&gt;DRV8830 I&lt;sup&gt;2&lt;/sup&gt;C DC Motor Driver&lt;/h2&gt;
TSSOP-10 with exposed power pad&lt;br&gt;
1A current limit, 2.75V to 6.8V</description>
<gates>
<gate name="G$1" symbol="DRV8830"/>
</gates>
<devices>
<device name="" package="MSOP-10-GNDPAD">
<connects>
<connect gate="G$1" pin="!FAULT" pad="6"/>
<connect gate="G$1" pin="A0" pad="7"/>
<connect gate="G$1" pin="A1" pad="8"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ISENSE" pad="2"/>
<connect gate="G$1" pin="OUT1" pad="3"/>
<connect gate="G$1" pin="OUT2" pad="1"/>
<connect gate="G$1" pin="PPAD" pad="GND"/>
<connect gate="G$1" pin="SCL" pad="10"/>
<connect gate="G$1" pin="SDA" pad="9"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11646"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADM1087">
<description>Power supply sequencer</description>
<gates>
<gate name="G$1" symbol="ADM1087"/>
</gates>
<devices>
<device name="SC-70" package="SC-70">
<connects>
<connect gate="G$1" pin="CEXT" pad="5"/>
<connect gate="G$1" pin="ENIN" pad="1"/>
<connect gate="G$1" pin="ENOUT" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="VIN" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BD10KA5WF-E2">
<description>500mA LDO, 1.0V SO-8 (COM-10827)</description>
<gates>
<gate name="G$1" symbol="BD10KA5WF-E2"/>
</gates>
<devices>
<device name="" package="SO08WIDE">
<connects>
<connect gate="G$1" pin="CTL" pad="5"/>
<connect gate="G$1" pin="GND1" pad="6"/>
<connect gate="G$1" pin="GND2" pad="7"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HV826MG_BACKLIGHT">
<description>Small EL backlight driver for the CFAX 128x64 graphical display.</description>
<gates>
<gate name="G$1" symbol="HV826MG_BACKLIGHT"/>
</gates>
<devices>
<device name="" package="MSOP8">
<connects>
<connect gate="G$1" pin="CS" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="LX" pad="5"/>
<connect gate="G$1" pin="REL" pad="3"/>
<connect gate="G$1" pin="RSW" pad="2"/>
<connect gate="G$1" pin="VA" pad="8"/>
<connect gate="G$1" pin="VB" pad="7"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4128-2.5VREF">
<description>.1% accurate low-current voltage reference</description>
<gates>
<gate name="G$1" symbol="LM4128-2.5VREF"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VIN" pad="4"/>
<connect gate="G$1" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMZ14203" prefix="U">
<description>3A, Simple Switcher Power Module with 42V Maximum Input</description>
<gates>
<gate name="G$1" symbol="LMZ14203"/>
</gates>
<devices>
<device name="" package="TO-PMOD-7">
<connects>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="EP" pad="EP"/>
<connect gate="G$1" pin="FB" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="RON" pad="2"/>
<connect gate="G$1" pin="SS" pad="5"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1528">
<description>High current voltage regulator commonly used with GM862 cellular module. Spark Fun Electronics SKU : COM-00311. Footprint may need to have the large paste aperature reduced.</description>
<gates>
<gate name="G$1" symbol="LT1528"/>
</gates>
<devices>
<device name="" package="Q5-DD">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="5"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="2"/>
<connect gate="G$1" pin="SHDN" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX1555" prefix="U">
<description>&lt;b&gt;MAX1555 Lithium Charger IC&lt;/b&gt;
SOT-23 Lithium Polymer charging IC. Schematic element and footprint proven. Spark Fun Electronics SKU : COM-00674</description>
<gates>
<gate name="G$1" symbol="MAX1555"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="BATT" pad="5"/>
<connect gate="G$1" pin="CHG" pad="3"/>
<connect gate="G$1" pin="DC" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="USB" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS6211*" prefix="U">
<description>TPS62112: 1.5A Step-Down Converter</description>
<gates>
<gate name="G$1" symbol="TPS6211*"/>
</gates>
<devices>
<device name="" package="QFN16-4X4">
<connects>
<connect gate="G$1" pin="AGND" pad="9"/>
<connect gate="G$1" pin="EN" pad="4"/>
<connect gate="G$1" pin="FB" pad="10"/>
<connect gate="G$1" pin="GND@1" pad="11"/>
<connect gate="G$1" pin="GND@2" pad="12"/>
<connect gate="G$1" pin="LBI" pad="7"/>
<connect gate="G$1" pin="LBO" pad="6"/>
<connect gate="G$1" pin="PG" pad="13"/>
<connect gate="G$1" pin="PGND@1" pad="1"/>
<connect gate="G$1" pin="PGND@2" pad="16"/>
<connect gate="G$1" pin="PWPD" pad="EXP"/>
<connect gate="G$1" pin="SW@1" pad="14"/>
<connect gate="G$1" pin="SW@2" pad="15"/>
<connect gate="G$1" pin="SYNC" pad="5"/>
<connect gate="G$1" pin="VIN@1" pad="2"/>
<connect gate="G$1" pin="VIN@2" pad="3"/>
<connect gate="G$1" pin="VINA" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS6213X">
<description>3-17V, 3A Step Down Converter(new? IC-11155)</description>
<gates>
<gate name="G$1" symbol="TPS6213X"/>
</gates>
<devices>
<device name="V1" package="QFN16-3X3MM">
<connects>
<connect gate="G$1" pin="AGND" pad="6"/>
<connect gate="G$1" pin="AVIN" pad="10"/>
<connect gate="G$1" pin="DEF" pad="8"/>
<connect gate="G$1" pin="EN" pad="13"/>
<connect gate="G$1" pin="EXT" pad="EXT"/>
<connect gate="G$1" pin="FB" pad="5"/>
<connect gate="G$1" pin="FSW" pad="7"/>
<connect gate="G$1" pin="PG" pad="4"/>
<connect gate="G$1" pin="PGND@15" pad="15"/>
<connect gate="G$1" pin="PGND@16" pad="16"/>
<connect gate="G$1" pin="PVIN@11" pad="11"/>
<connect gate="G$1" pin="PVIN@12" pad="12"/>
<connect gate="G$1" pin="SS/TR" pad="9"/>
<connect gate="G$1" pin="SW@1" pad="1"/>
<connect gate="G$1" pin="SW@2" pad="2"/>
<connect gate="G$1" pin="SW@3" pad="3"/>
<connect gate="G$1" pin="VOS" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-11630"/>
</technology>
</technologies>
</device>
<device name="TI" package="QFN16-3X3MM_TI">
<connects>
<connect gate="G$1" pin="AGND" pad="6"/>
<connect gate="G$1" pin="AVIN" pad="10"/>
<connect gate="G$1" pin="DEF" pad="8"/>
<connect gate="G$1" pin="EN" pad="13"/>
<connect gate="G$1" pin="EXT" pad="EXT@1 EXT@2 EXT@3 EXT@4 EXT@5 EXT@6"/>
<connect gate="G$1" pin="FB" pad="5"/>
<connect gate="G$1" pin="FSW" pad="7"/>
<connect gate="G$1" pin="PG" pad="4"/>
<connect gate="G$1" pin="PGND@15" pad="15"/>
<connect gate="G$1" pin="PGND@16" pad="16"/>
<connect gate="G$1" pin="PVIN@11" pad="11"/>
<connect gate="G$1" pin="PVIN@12" pad="12"/>
<connect gate="G$1" pin="SS/TR" pad="9"/>
<connect gate="G$1" pin="SW@1" pad="1"/>
<connect gate="G$1" pin="SW@2" pad="2"/>
<connect gate="G$1" pin="SW@3" pad="3"/>
<connect gate="G$1" pin="VOS" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_NCP1400" prefix="IC" uservalue="yes">
<description>&lt;b&gt;Switching step-up voltage regulator&lt;/b&gt;
NCP1400 switiching regulator takes single cell AA and outputs 100mA at 3.3V or 5V with minimal number of external components.</description>
<gates>
<gate name="G$1" symbol="NCP1400"/>
</gates>
<devices>
<device name="_3.3V" package="SOT23-5">
<connects>
<connect gate="G$1" pin="EN" pad="1"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="LX" pad="5"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-10788"/>
<attribute name="VALUE" value="3.3v"/>
</technology>
</technologies>
</device>
<device name="_5V" package="SOT23-5">
<connects>
<connect gate="G$1" pin="EN" pad="1"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="LX" pad="5"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-10787"/>
<attribute name="VALUE" value="5.0v"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_TPS61040">
<gates>
<gate name="G$1" symbol="TPS61040"/>
</gates>
<devices>
<device name="SMD" package="SOT23-5">
<connects>
<connect gate="G$1" pin="EN" pad="4"/>
<connect gate="G$1" pin="FB" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SW" pad="1"/>
<connect gate="G$1" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="A4983" prefix="U">
<description>DMOS Microstepping Driver with Translator</description>
<gates>
<gate name="G$1" symbol="A4983"/>
</gates>
<devices>
<device name="5MM" package="QFN-28-5MM">
<connects>
<connect gate="G$1" pin="CP1" pad="P$4"/>
<connect gate="G$1" pin="CP2" pad="P$5"/>
<connect gate="G$1" pin="DIR" pad="P$19"/>
<connect gate="G$1" pin="ENABLE" pad="P$2"/>
<connect gate="G$1" pin="GND@1" pad="P$3"/>
<connect gate="G$1" pin="GND@2" pad="P$18"/>
<connect gate="G$1" pin="GND_PAD" pad="P$29"/>
<connect gate="G$1" pin="MS1" pad="P$9"/>
<connect gate="G$1" pin="MS2" pad="P$10"/>
<connect gate="G$1" pin="MS3" pad="P$11"/>
<connect gate="G$1" pin="NC@1" pad="P$7"/>
<connect gate="G$1" pin="NC@2" pad="P$20"/>
<connect gate="G$1" pin="NC@3" pad="P$25"/>
<connect gate="G$1" pin="OUT1A" pad="P$24"/>
<connect gate="G$1" pin="OUT1B" pad="P$21"/>
<connect gate="G$1" pin="OUT2A" pad="P$26"/>
<connect gate="G$1" pin="OUT2B" pad="P$1"/>
<connect gate="G$1" pin="REF" pad="P$17"/>
<connect gate="G$1" pin="RESET" pad="P$12"/>
<connect gate="G$1" pin="ROSC" pad="P$13"/>
<connect gate="G$1" pin="SENSE1" pad="P$23"/>
<connect gate="G$1" pin="SENSE2" pad="P$27"/>
<connect gate="G$1" pin="SLEEP" pad="P$14"/>
<connect gate="G$1" pin="STEP" pad="P$16"/>
<connect gate="G$1" pin="VBB1" pad="P$22"/>
<connect gate="G$1" pin="VBB2" pad="P$28"/>
<connect gate="G$1" pin="VCP" pad="P$6"/>
<connect gate="G$1" pin="VDD" pad="P$15"/>
<connect gate="G$1" pin="VREG" pad="P$8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ALT1" package="QFN-28-5MM_ALT1">
<connects>
<connect gate="G$1" pin="CP1" pad="P$4"/>
<connect gate="G$1" pin="CP2" pad="P$5"/>
<connect gate="G$1" pin="DIR" pad="P$19"/>
<connect gate="G$1" pin="ENABLE" pad="P$2"/>
<connect gate="G$1" pin="GND@1" pad="P$3"/>
<connect gate="G$1" pin="GND@2" pad="P$18"/>
<connect gate="G$1" pin="GND_PAD" pad="P$29"/>
<connect gate="G$1" pin="MS1" pad="P$9"/>
<connect gate="G$1" pin="MS2" pad="P$10"/>
<connect gate="G$1" pin="MS3" pad="P$11"/>
<connect gate="G$1" pin="NC@1" pad="P$7"/>
<connect gate="G$1" pin="NC@2" pad="P$20"/>
<connect gate="G$1" pin="NC@3" pad="P$25"/>
<connect gate="G$1" pin="OUT1A" pad="P$24"/>
<connect gate="G$1" pin="OUT1B" pad="P$21"/>
<connect gate="G$1" pin="OUT2A" pad="P$26"/>
<connect gate="G$1" pin="OUT2B" pad="P$1"/>
<connect gate="G$1" pin="REF" pad="P$17"/>
<connect gate="G$1" pin="RESET" pad="P$12"/>
<connect gate="G$1" pin="ROSC" pad="P$13"/>
<connect gate="G$1" pin="SENSE1" pad="P$23"/>
<connect gate="G$1" pin="SENSE2" pad="P$27"/>
<connect gate="G$1" pin="SLEEP" pad="P$14"/>
<connect gate="G$1" pin="STEP" pad="P$16"/>
<connect gate="G$1" pin="VBB1" pad="P$22"/>
<connect gate="G$1" pin="VBB2" pad="P$28"/>
<connect gate="G$1" pin="VCP" pad="P$6"/>
<connect gate="G$1" pin="VDD" pad="P$15"/>
<connect gate="G$1" pin="VREG" pad="P$8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09890"/>
</technology>
</technologies>
</device>
<device name="ALT2" package="QFN-28-5MM_ALT2">
<connects>
<connect gate="G$1" pin="CP1" pad="P$4"/>
<connect gate="G$1" pin="CP2" pad="P$5"/>
<connect gate="G$1" pin="DIR" pad="P$19"/>
<connect gate="G$1" pin="ENABLE" pad="P$2"/>
<connect gate="G$1" pin="GND@1" pad="P$3"/>
<connect gate="G$1" pin="GND@2" pad="P$18"/>
<connect gate="G$1" pin="GND_PAD" pad="P$29"/>
<connect gate="G$1" pin="MS1" pad="P$9"/>
<connect gate="G$1" pin="MS2" pad="P$10"/>
<connect gate="G$1" pin="MS3" pad="P$11"/>
<connect gate="G$1" pin="NC@1" pad="P$7"/>
<connect gate="G$1" pin="NC@2" pad="P$20"/>
<connect gate="G$1" pin="NC@3" pad="P$25"/>
<connect gate="G$1" pin="OUT1A" pad="P$24"/>
<connect gate="G$1" pin="OUT1B" pad="P$21"/>
<connect gate="G$1" pin="OUT2A" pad="P$26"/>
<connect gate="G$1" pin="OUT2B" pad="P$1"/>
<connect gate="G$1" pin="REF" pad="P$17"/>
<connect gate="G$1" pin="RESET" pad="P$12"/>
<connect gate="G$1" pin="ROSC" pad="P$13"/>
<connect gate="G$1" pin="SENSE1" pad="P$23"/>
<connect gate="G$1" pin="SENSE2" pad="P$27"/>
<connect gate="G$1" pin="SLEEP" pad="P$14"/>
<connect gate="G$1" pin="STEP" pad="P$16"/>
<connect gate="G$1" pin="VBB1" pad="P$22"/>
<connect gate="G$1" pin="VBB2" pad="P$28"/>
<connect gate="G$1" pin="VCP" pad="P$6"/>
<connect gate="G$1" pin="VDD" pad="P$15"/>
<connect gate="G$1" pin="VREG" pad="P$8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1:1" package="QFN-28-5MM-1:1">
<connects>
<connect gate="G$1" pin="CP1" pad="P$4"/>
<connect gate="G$1" pin="CP2" pad="P$5"/>
<connect gate="G$1" pin="DIR" pad="P$19"/>
<connect gate="G$1" pin="ENABLE" pad="P$2"/>
<connect gate="G$1" pin="GND@1" pad="P$3"/>
<connect gate="G$1" pin="GND@2" pad="P$18"/>
<connect gate="G$1" pin="GND_PAD" pad="P$29"/>
<connect gate="G$1" pin="MS1" pad="P$9"/>
<connect gate="G$1" pin="MS2" pad="P$10"/>
<connect gate="G$1" pin="MS3" pad="P$11"/>
<connect gate="G$1" pin="NC@1" pad="P$7"/>
<connect gate="G$1" pin="NC@2" pad="P$20"/>
<connect gate="G$1" pin="NC@3" pad="P$25"/>
<connect gate="G$1" pin="OUT1A" pad="P$24"/>
<connect gate="G$1" pin="OUT1B" pad="P$21"/>
<connect gate="G$1" pin="OUT2A" pad="P$26"/>
<connect gate="G$1" pin="OUT2B" pad="P$1"/>
<connect gate="G$1" pin="REF" pad="P$17"/>
<connect gate="G$1" pin="RESET" pad="P$12"/>
<connect gate="G$1" pin="ROSC" pad="P$13"/>
<connect gate="G$1" pin="SENSE1" pad="P$23"/>
<connect gate="G$1" pin="SENSE2" pad="P$27"/>
<connect gate="G$1" pin="SLEEP" pad="P$14"/>
<connect gate="G$1" pin="STEP" pad="P$16"/>
<connect gate="G$1" pin="VBB1" pad="P$22"/>
<connect gate="G$1" pin="VBB2" pad="P$28"/>
<connect gate="G$1" pin="VCP" pad="P$6"/>
<connect gate="G$1" pin="VDD" pad="P$15"/>
<connect gate="G$1" pin="VREG" pad="P$8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ALT1_REDUCED_PASTE" package="QFN-28-5MM_ALT1_REDUCED_PASTE">
<connects>
<connect gate="G$1" pin="CP1" pad="P$4"/>
<connect gate="G$1" pin="CP2" pad="P$5"/>
<connect gate="G$1" pin="DIR" pad="P$19"/>
<connect gate="G$1" pin="ENABLE" pad="P$2"/>
<connect gate="G$1" pin="GND@1" pad="P$3"/>
<connect gate="G$1" pin="GND@2" pad="P$18"/>
<connect gate="G$1" pin="GND_PAD" pad="P$29"/>
<connect gate="G$1" pin="MS1" pad="P$9"/>
<connect gate="G$1" pin="MS2" pad="P$10"/>
<connect gate="G$1" pin="MS3" pad="P$11"/>
<connect gate="G$1" pin="NC@1" pad="P$7"/>
<connect gate="G$1" pin="NC@2" pad="P$20"/>
<connect gate="G$1" pin="NC@3" pad="P$25"/>
<connect gate="G$1" pin="OUT1A" pad="P$24"/>
<connect gate="G$1" pin="OUT1B" pad="P$21"/>
<connect gate="G$1" pin="OUT2A" pad="P$26"/>
<connect gate="G$1" pin="OUT2B" pad="P$1"/>
<connect gate="G$1" pin="REF" pad="P$17"/>
<connect gate="G$1" pin="RESET" pad="P$12"/>
<connect gate="G$1" pin="ROSC" pad="P$13"/>
<connect gate="G$1" pin="SENSE1" pad="P$23"/>
<connect gate="G$1" pin="SENSE2" pad="P$27"/>
<connect gate="G$1" pin="SLEEP" pad="P$14"/>
<connect gate="G$1" pin="STEP" pad="P$16"/>
<connect gate="G$1" pin="VBB1" pad="P$22"/>
<connect gate="G$1" pin="VBB2" pad="P$28"/>
<connect gate="G$1" pin="VCP" pad="P$6"/>
<connect gate="G$1" pin="VDD" pad="P$15"/>
<connect gate="G$1" pin="VREG" pad="P$8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09890"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMD1820X">
<description>LMD1820X H-Bridge - BOB-00747</description>
<gates>
<gate name="G$1" symbol="LMD1820X"/>
</gates>
<devices>
<device name="" package="TO-220-11LEAD">
<connects>
<connect gate="G$1" pin="BRK" pad="4"/>
<connect gate="G$1" pin="BS1" pad="1"/>
<connect gate="G$1" pin="BS2" pad="11"/>
<connect gate="G$1" pin="DIR" pad="3"/>
<connect gate="G$1" pin="OUT1" pad="2"/>
<connect gate="G$1" pin="OUT2" pad="10"/>
<connect gate="G$1" pin="PGND" pad="7"/>
<connect gate="G$1" pin="PWM" pad="5"/>
<connect gate="G$1" pin="PWR" pad="6"/>
<connect gate="G$1" pin="SGND" pad="8"/>
<connect gate="G$1" pin="TF" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NJM2670">
<description>Dual H-bridge driver</description>
<gates>
<gate name="G$1" symbol="NJM2670"/>
</gates>
<devices>
<device name="SMD" package="SO-24W">
<connects>
<connect gate="G$1" pin="ENABLEA" pad="3"/>
<connect gate="G$1" pin="ENABLEB" pad="9"/>
<connect gate="G$1" pin="GND@1" pad="6"/>
<connect gate="G$1" pin="GND@2" pad="7"/>
<connect gate="G$1" pin="GND@3" pad="18"/>
<connect gate="G$1" pin="GND@4" pad="19"/>
<connect gate="G$1" pin="INA1" pad="2"/>
<connect gate="G$1" pin="INA2" pad="22"/>
<connect gate="G$1" pin="INB1" pad="8"/>
<connect gate="G$1" pin="INB2" pad="17"/>
<connect gate="G$1" pin="NC@1" pad="4"/>
<connect gate="G$1" pin="NC@2" pad="10"/>
<connect gate="G$1" pin="NC@3" pad="15"/>
<connect gate="G$1" pin="NC@4" pad="21"/>
<connect gate="G$1" pin="OUTA1" pad="5"/>
<connect gate="G$1" pin="OUTA2" pad="20"/>
<connect gate="G$1" pin="OUTB1" pad="11"/>
<connect gate="G$1" pin="OUTB2" pad="14"/>
<connect gate="G$1" pin="SENSEA" pad="1"/>
<connect gate="G$1" pin="SENSEB" pad="12"/>
<connect gate="G$1" pin="TSDARM" pad="16"/>
<connect gate="G$1" pin="VCC" pad="23"/>
<connect gate="G$1" pin="VSA" pad="24"/>
<connect gate="G$1" pin="VSB" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ZXLD1360">
<description>Adjustable constant current switching driver for high-power LEDs</description>
<gates>
<gate name="G$1" symbol="ZXLD1360"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="ADJ" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="LX" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="4"/>
<connect gate="G$1" pin="VIN" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MIC" prefix="MK">
<description>&lt;h3&gt;Microphone&lt;/h3&gt;
&lt;p&gt;Omni-directional electret microphones - one through-hole, the other SMD.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Sensors/Sound/CEM-C9745JAD462P2.54R.pdf"&gt;Datasheet&lt;/a&gt; (through-hole mic)&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.challengeelectronics.com/downloads/microphones/omni_directional/CEM-OB6018-3EAD443C43MR.pdf"&gt;Datasheet&lt;/a&gt; (SMD mic)&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8635"&gt;PTH Electret Microphone&lt;/a&gt; (COM-08635)&lt;/li&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9964"&gt;SparkFun Electret Microphone Breakout &lt;/a&gt; (BOB-09964)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12651"&gt;Digital Sandbox&lt;/a&gt; (DEV-12651)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12642"&gt;SparkFun Sound Detector&lt;/a&gt; (SEN-12642)&lt;/li&gt;
&lt;/ul&gt;
&lt;li&gt;SMD Microphone&lt;/li&gt;
&lt;ul&gt;&lt;a href="https://www.sparkfun.com/products/retired/10653"&gt;SparkFun Voice Recorder Breakout - ISD1932&lt;/a&gt; (BOB-10653)&lt;/li&gt;</description>
<gates>
<gate name="&gt;NAME" symbol="MIC"/>
</gates>
<devices>
<device name="-PTH" package="MICROPHONE-PTH-9.7MM">
<connects>
<connect gate="&gt;NAME" pin="1" pad="1"/>
<connect gate="&gt;NAME" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-08856"/>
<attribute name="SF_ID" value="COM-08635"/>
</technology>
</technologies>
</device>
<device name="-SMD" package="MICROPHONE-SMD-6MM">
<connects>
<connect gate="&gt;NAME" pin="1" pad="1"/>
<connect gate="&gt;NAME" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-10458"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONN_02" prefix="J" uservalue="yes">
<description>&lt;h3&gt;Multi connection point. Often used as Generic Header-pin footprint for 0.1 inch spaced/style header connections&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;On any of the 0.1 inch spaced packages, you can populate with these:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/116"&gt; Break Away Headers - Straight&lt;/a&gt; (PRT-00116)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/553"&gt; Break Away Male Headers - Right Angle&lt;/a&gt; (PRT-00553)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/115"&gt; Female Headers&lt;/a&gt; (PRT-00115)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/117"&gt; Break Away Headers - Machine Pin&lt;/a&gt; (PRT-00117)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/743"&gt; Break Away Female Headers - Swiss Machine Pin&lt;/a&gt; (PRT-00743)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt; For SCREWTERMINALS and SPRING TERMINALS visit here:&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/search/results?term=Screw+Terminals"&gt; Screw Terimnals on SparkFun.com&lt;/a&gt; (5mm/3.5mm/2.54mm spacing)&lt;/li&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;This device is also useful as a general connection point to wire up your design to another part of your project. Our various solder wires solder well into these plated through hole pads.&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11375"&gt; Hook-Up Wire - Assortment (Stranded, 22 AWG)&lt;/a&gt; (PRT-11375)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11367"&gt; Hook-Up Wire - Assortment (Solid Core, 22 AWG)&lt;/a&gt; (PRT-11367)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/categories/141"&gt; View the entire wire category on our website here&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;/p&gt;
&lt;/ul&gt;

&lt;p&gt;&lt;/p&gt;
&lt;b&gt;Special notes:&lt;/b&gt;

 Molex polarized connector foot print use with: PRT-08233 with associated crimp pins and housings.&lt;br&gt;&lt;br&gt;

2.54_SCREWTERM for use with  PRT-10571.&lt;br&gt;&lt;br&gt;

3.5mm Screw Terminal footprints for  PRT-08084&lt;br&gt;&lt;br&gt;

5mm Screw Terminal footprints for use with PRT-08432</description>
<gates>
<gate name="G$1" symbol="CONN_02"/>
</gates>
<devices>
<device name="" package="1X02">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR" package="MOLEX-1X2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="PRT-09918"/>
</technology>
</technologies>
</device>
<device name="3.5MM" package="SCREWTERMINAL-3.5MM-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08399"/>
</technology>
</technologies>
</device>
<device name="-JST-2MM-SMT" package="JST-2-SMD">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-11443"/>
</technology>
</technologies>
</device>
<device name="PTH2" package="1X02_BIG">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="4UCON-15767" package="JST-2-SMD-VERT">
<connects>
<connect gate="G$1" pin="1" pad="GND"/>
<connect gate="G$1" pin="2" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="SCREWTERMINAL-5MM-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_SKU" value="PRT-08432"/>
</technology>
</technologies>
</device>
<device name="LOCK" package="1X02_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR_LOCK" package="MOLEX-1X2_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="PRT-09918"/>
</technology>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X02_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM_LOCK" package="SCREWTERMINAL-3.5MM-2_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08399"/>
</technology>
</technologies>
</device>
<device name="PTH3" package="1X02_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1X02_NO_SILK" package="1X02_NO_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PTH-2" package="JST-2-PTH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09863"/>
<attribute name="SKU" value="PRT-09914"/>
</technology>
</technologies>
</device>
<device name="PTH4" package="1X02_XTRA_BIG">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POGO_PIN_HOLES_ONLY" package="1X02_PP_HOLES_ONLY">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM-NO_SILK" package="SCREWTERMINAL-3.5MM-2-NS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08399"/>
</technology>
</technologies>
</device>
<device name="-JST-2-PTH-NO_SILK" package="JST-2-PTH-NS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PTH-2-KIT" package="JST-2-PTH-KIT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SPRING-2.54-RA" package="SPRINGTERMINAL-2.54MM-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2.54MM_SCREWTERM" package="1X02_2.54_SCREWTERM">
<connects>
<connect gate="G$1" pin="1" pad="P1"/>
<connect gate="G$1" pin="2" pad="P2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JST-PTH-VERT" package="JST-2-PTH-VERT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-12097"/>
</technology>
</technologies>
</device>
<device name="SMALL_POKEHOME" package="1X02_POKEHOME">
<connects>
<connect gate="G$1" pin="1" pad="P1 P3"/>
<connect gate="G$1" pin="2" pad="P2 P4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-13512"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INDUCTOR" prefix="L" uservalue="yes">
<gates>
<gate name="G$1" symbol="INDUCTOR"/>
</gates>
<devices>
<device name="-VLF4012AT-2.2UH" package="INDUCTOR_2.2UH">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NDUC-09513"/>
<attribute name="VALUE" value="2.2µH/±20%/1.5A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
