<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.2">
<drawing>
<library>
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIPSWITCH-02-CHS-02A">
<description>&lt;h3&gt;2-Position DIP Switch - SMD, J-Hook Pads, 0.05"-Pitch&lt;/h3&gt;
&lt;p&gt;2-circuit DIP (dual inline package) switch. Commonly used to physcially set a circuit's behavior.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.nidec-copal-electronics.com/e/catalog/switch/chs.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="DIPSWITCH-02-209-2LPST">
<description>&lt;h3&gt;2-Position DIP Switch - PTH 0.1"-Pitch&lt;/h3&gt;
&lt;p&gt;2-circuit DIP (dual inline package) switch. Commonly used to physcially set a circuit's behavior.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.ctscorp.com/wp-content/uploads/209-210.pdf"&gt;Datasheet&lt;/a&gt; (209-2LPST )&lt;/p&gt;</description>
</package>
<package name="DIPSWITCH-04-SMD">
<description>&lt;h3&gt;4-Position DIP Switch - SMD, 0.1"-Pitch&lt;/h3&gt;
&lt;p&gt;&lt;a href="http://www.ctscorp.com/wp-content/uploads/2015/11/219.pdf"&gt;Datasheet&lt;/a&gt; (219-4MST)&lt;/p&gt;</description>
</package>
<package name="SWITCH_DPDT_SMD_AYZ0202">
<description>&lt;h3&gt;ITT Industries AYZ0202 DPDT Switch - SMD&lt;/h3&gt;
&lt;p&gt;Double-pole, double-throw switches.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/SW_slide_ayz.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="BUTTON-CONDUCTIVE">
<description>&lt;h3&gt;Conductive Button&lt;/h3&gt;
&lt;p&gt;Used with rubber key pads on the &lt;a href="https://www.sparkfun.com/products/retired/8602"&gt;Nordic Key FOB&lt;/a&gt;. This one was designed and proven to work with the &lt;a href="https://www.sparkfun.com/products/retired/9377"&gt;PolyCase Key FOB enclosures&lt;/a&gt;.&lt;/p&gt;</description>
</package>
<package name="BUTTON-18MM">
<description>&lt;h3&gt;Magnetic Metal Snaps&lt;/h3&gt;
&lt;p&gt;18mm diameter snaps that couple together very strongly (must be pried apart), rotate freely on the axis, and are electrically conductive. Overall connection resistance is less than 200 miliOhm. Snaps will couple when closer than 10mm.&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8682"&gt;Magnetic Snap 18mm&lt;/a&gt; (WRL-08682)&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="BUTTONPAD-2X2">
<description>&lt;h3&gt;2x2 Button Pad w/ RGB LEDs&lt;/h3&gt;
&lt;p&gt;Layout and schematic for 2x2 button pad with single-color LEDs under each button. For use with the &lt;a href="https://www.sparkfun.com/products/7836"&gt;Button Pad 2x2 - LED Compatible&lt;/a&gt; and &lt;a href="https://www.sparkfun.com/products/8746"&gt;Button Pad 2x2 Top Bezel&lt;/a&gt;.&lt;/p&gt;
&lt;p&gt;Any &lt;a href="https://www.sparkfun.com/categories/172"&gt;RGB-color 5mm LED&lt;/a&gt; should be compatible.&lt;/p&gt;</description>
</package>
<package name="BUTTONPAD-2X2-STAGGERED">
<description>&lt;h3&gt;2x2 Button Pad w/ RGB LEDs - Staggered LED Footprint&lt;/h3&gt;
&lt;p&gt;Layout and schematic for 2x2 button pad with single-color LEDs under each button. For use with the &lt;a href="https://www.sparkfun.com/products/7836"&gt;Button Pad 2x2 - LED Compatible&lt;/a&gt; and &lt;a href="https://www.sparkfun.com/products/8746"&gt;Button Pad 2x2 Top Bezel&lt;/a&gt;.&lt;/p&gt;
&lt;p&gt;Any &lt;a href="https://www.sparkfun.com/categories/172"&gt;RGB-color 5mm LED&lt;/a&gt; should be compatible.&lt;/p&gt;</description>
</package>
<package name="BUTTONPAD-2X2-SINGLE-LED">
<description>&lt;h3&gt;2x2 Button Pad w/ Single LEDs&lt;/h3&gt;
&lt;p&gt;Layout and schematic for 2x2 button pad with single-color LEDs under each button. For use with the &lt;a href="https://www.sparkfun.com/products/7836"&gt;Button Pad 2x2 - LED Compatible&lt;/a&gt; and &lt;a href="https://www.sparkfun.com/products/8746"&gt;Button Pad 2x2 Top Bezel&lt;/a&gt;.&lt;/p&gt;
&lt;p&gt;Any &lt;a href="https://www.sparkfun.com/categories/172"&gt;single-color 5mm LED&lt;/a&gt; should be compatible.&lt;/p&gt;</description>
</package>
<package name="BUTTONPAD-2X2-SINGLE-LED-KIT">
<description>&lt;h3&gt;2x2 Button Pad w/ Single LEDs&lt;/h3&gt;
&lt;p&gt;Layout and schematic for 2x2 button pad with single-color LEDs under each button. For use with the &lt;a href="https://www.sparkfun.com/products/7836"&gt;Button Pad 2x2 - LED Compatible&lt;/a&gt; and &lt;a href="https://www.sparkfun.com/products/8746"&gt;Button Pad 2x2 Top Bezel&lt;/a&gt;.&lt;/p&gt;
&lt;p&gt;Any &lt;a href="https://www.sparkfun.com/categories/172"&gt;single-color 5mm LED&lt;/a&gt; should be compatible.&lt;/p&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.</description>
</package>
<package name="BUTTONPAD-4X4">
<description>&lt;h3&gt;4x4 Button Pad w/ RGB LEDs&lt;/h3&gt;
&lt;p&gt;Layout and schematic for 4x4 button pad with tri-color LEDs under each button. For use with the 4x &lt;a href="https://www.sparkfun.com/products/7836"&gt;Button Pad 2x2 - LED Compatible&lt;/a&gt; and 4x &lt;a href="https://www.sparkfun.com/products/8746"&gt;Button Pad 2x2 Top Bezel&lt;/a&gt;.&lt;/p&gt;
&lt;p&gt;Any &lt;a href="https://www.sparkfun.com/categories/172"&gt;RGB 5mm LED&lt;/a&gt; should be compatible.&lt;/p&gt;</description>
</package>
<package name="BUTTONPAD-4X4-STAGGERED">
<description>&lt;h3&gt;4x4 Button Pad w/ RGB LEDs - Staggered LED Footprint&lt;/h3&gt;
&lt;p&gt;Layout and schematic for 4x4 button pad with tri-color LEDs under each button. For use with the 4x &lt;a href="https://www.sparkfun.com/products/7836"&gt;Button Pad 2x2 - LED Compatible&lt;/a&gt; and 4x &lt;a href="https://www.sparkfun.com/products/8746"&gt;Button Pad 2x2 Top Bezel&lt;/a&gt;.&lt;/p&gt;
&lt;p&gt;Any &lt;a href="https://www.sparkfun.com/categories/172"&gt;RGB 5mm LED&lt;/a&gt; should be compatible.&lt;/p&gt;</description>
</package>
<package name="CHERRY-MX-LED">
<description>&lt;h3&gt;Cherry MX Switch - Electromechanical Swith w/ LED&lt;/h3&gt;

&lt;p&gt;Cherry MX Keyswitches are top-of-the-line mechanical keyboard switches. They’re satisfyingly “clicky”, reliable up to tens-of-millions of key presses, and a standard in gaming and programming keyboards across the globe. This ‘blue’ version Cherry MX Switch is favored by most due to its secondary internal actuator making it less likely to “double-tap.” If you are looking for a noticeably audible and high-quality key switch, this is the perfect option for you!&lt;/p&gt;

&lt;p&gt;&lt;a href="https://www.sparkfun.com/products/13834"&gt;SparkFun Product Link&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Components/Switches/MX%20Series.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="ENCODER-16MM-QUAD">
<description>&lt;h3&gt;Rotary Encoder - 16mm Top Width&lt;/h3&gt;
&lt;p&gt;Encoders rotate similarly to potentiometers, but they’re different from potentiometers in that an encoder has full rotation without limits. They output gray code so that you can tell how much and in which direction the encoder has been turned.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.top-up.com.tw/front/bin/ptdetail.phtml?Part=EC16PXHFB-B"&gt;Datasheet&lt;/a&gt; (EC16PHBF-B-20F-24-24C-16Y)&lt;/p&gt;</description>
</package>
<package name="ENCODER_LED_2">
<description>&lt;h3&gt;Illuminated Rotary Encoder w/ 2 LEDs&lt;/h3&gt;
&lt;p&gt;Rotary encoders rotate similarly to potentiometers, but they’re different from potentiometers in that an encoder has full rotation without limits. They output gray code so that you can tell how much and in which direction the encoder has been turned.&lt;/p&gt;
&lt;p&gt;This encoder has a red/green LED built-in, which shines through the encoder shaft.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/LED/EC12PLRVF-D-24K-24-24C-0206-6H%28SPEC%29.pdf"&gt;Datasheet&lt;/a&gt; (EC12PLGRSDVF-D-25K-24-32/07-6H)&lt;/p&gt;</description>
</package>
<package name="ENCODER_LED_2_KIT">
<description>&lt;h3&gt;Illuminated Rotary Encoder w/ 2 LEDs - KIT Package&lt;/h3&gt;
&lt;p&gt;Rotary encoders rotate similarly to potentiometers, but they’re different from potentiometers in that an encoder has full rotation without limits. They output gray code so that you can tell how much and in which direction the encoder has been turned.&lt;/p&gt;
&lt;p&gt;This encoder has a red/green LED built-in, which shines through the encoder shaft.&lt;/p&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/LED/EC12PLRVF-D-24K-24-24C-0206-6H%28SPEC%29.pdf"&gt;Datasheet&lt;/a&gt; (EC12PLGRSDVF-D-25K-24-32/07-6H)&lt;/p&gt;</description>
</package>
<package name="ENCODER_LED_3">
<description>&lt;h3&gt;Illuminated Rotary Encoder w/ RGB LED and select switch&lt;/h3&gt;
&lt;p&gt;Encoders rotate similarly to potentiometers, but they’re different from potentiometers in that an encoder has full rotation without limits. They output gray code so that you can tell how much and in which direction the encoder has been turned.&lt;/p&gt;
&lt;p&gt;This encoder includes an RGB LED and a push-down select switch.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/Switches/EC12PLRGBSDVBF-D-25K-24-24C-6108-6H.pdf"&gt;Dimensional Drawing&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="ENCODER_LED_3_KIT">
<description>&lt;h3&gt;Illuminated Rotary Encoder w/ RGB LED and select switch&lt;/h3&gt;
&lt;p&gt;Encoders rotate similarly to potentiometers, but they’re different from potentiometers in that an encoder has full rotation without limits. They output gray code so that you can tell how much and in which direction the encoder has been turned.&lt;/p&gt;
&lt;p&gt;This encoder includes an RGB LED and a push-down select switch.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/Switches/EC12PLRGBSDVBF-D-25K-24-24C-6108-6H.pdf"&gt;Dimensional Drawing&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="JOYSTICK">
<description>&lt;h3&gt;Thumb Joystick&lt;/h3&gt;
&lt;p&gt;This is a joystick very similar to the ‘analog’ joysticks on PS2 (PlayStation 2) controllers. Directional movements are simply two potentiometers - one for each axis. Pots are ~10k each. This joystick also has a select button that is actuated when the joystick is pressed down.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.p3america.com/pp/802.htm"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="JOYSTICK-PSP1000">
<description>&lt;h3&gt;PSP-1000 Thumb Slide Joystick&lt;/h3&gt;
&lt;p&gt;This is a resistive analog joystick, very similar to those found on the PSP1000. These compact joysticks are different in that they have a very interesting ‘slide’ feeling.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/products/9426"&gt;Product Page&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="JOYSTICK_MINI">
<description>&lt;h3&gt;Small Tactile Joystick w/ Select Switch&lt;/h3&gt;
&lt;p&gt;A 5-way tactile switch allows for a joystick-like interface in a very small package.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.sparkfun.com/datasheets/Components/Buttons/SF303GJ26-3.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="NAV_SWITCH">
<description>&lt;h3&gt;Navigation Switch&lt;/h3&gt;
&lt;p&gt;Three way navigation switch. Commonly used as up/down/select on MP3 players. Schematic element and footprint production proven.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/Switches/LEVER8184.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="ROTARY_ENC_PLAIN">
<description>&lt;h3&gt;Rotary Encoder w/ Select Switch&lt;/h3&gt;
&lt;p&gt;Encoders rotate similarly to potentiometers, but they’re different from potentiometers in that an encoder has full rotation without limits. They output gray code so that you can tell how much and in which direction the encoder has been turned.&lt;/p&gt;
&lt;p&gt;This encoder includes a push-down select switch built into the shaft.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.sparkfun.com/datasheets/Components/TW-700198.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="STOMP_SWITCH_3PDT">
<description>&lt;h3&gt;3-Pole, Double-Throw (3PDT) Stomp Switch&lt;/h3&gt;
&lt;p&gt;Three-pole, double-throw stomp switch. Drawn as three separate gates for schematic clarity.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.mouser.com/ds/2/13/SF17_SF12030F-492761.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="SWITCH_DPDT_PTH_GPI-152-3013">
<description>&lt;h3&gt;CW Industries  GPI-152-3013  DPDT Switch - PTH&lt;/h3&gt;
&lt;p&gt;Double-pole, double-throw switches.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://switches-connectors-custom.cwind.com/Asset/GPI-152-Dimension-DRAWING.pdf"&gt;Dimensional Drawing&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="TACTILE_SWITCH_PTH_6.0MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, 6.0mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.omron.com/ecb/products/pdf/en-b3f.pdf"&gt;Datasheet&lt;/a&gt; (B3F-1000)&lt;/p&gt;</description>
</package>
<package name="TACTILE_SWITCH_SMD_4.5MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, 4.5mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="http://spec_sheets.e-switch.com/specs/P010338.pdf"&gt;Dimensional Drawing&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="TACTILE_SWITCH_PTH_12MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, 12mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.omron.com/ecb/products/pdf/en-b3f.pdf"&gt;Datasheet&lt;/a&gt; (B3F-5050)&lt;/p&gt;</description>
</package>
<package name="TACTILE_SWITCH_SMD_6.0X3.5MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, 6.0 x 3.5 mm&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/1101.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="REED_SWITCH_GLASS">
<description>&lt;h3&gt;Reed Switch - Glass case - PTH&lt;/h3&gt;
&lt;p&gt;A reed switch is a magnetically-actuated switch. When the device is exposed to a magnetic field, the two ferrous materials inside the switch pull together and the switch closes.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/Buttons/MDSR-4.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="TACTILE_SWITCH_SMD_6.2MM_TALL">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, 6.2mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.apem.com/files/apem/brochures/ADTS6-ADTSM-KTSC6.pdf"&gt;Datasheet&lt;/a&gt; (ADTSM63NVTR)&lt;/p&gt;</description>
</package>
<package name="REED_SWITCH_PLASTIC">
<description>&lt;h3&gt;Reed Switch - Insulated Case - PTH&lt;/h3&gt;
&lt;p&gt;A reed switch is a magnetically-actuated switch. When the device is exposed to a magnetic field, the two ferrous materials inside the switch pull together and the switch closes.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Dev/LilyPad/RS-01C.jpg"&gt;Datasheet&lt;/a&gt; (RS-01C)&lt;/p&gt;</description>
</package>
<package name="TACTILE_SWITCH_PTH_RIGHT_ANGLE_KIT">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, Right-angle&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/Switches/SW016.JPG"&gt;Dimensional Drawing&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="TACTILE_SWITCH_SMD_12MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, 12mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Components/Switches/N301102.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="TACTILE_SWITCH_PTH_6.0MM_KIT">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, 6.0mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.omron.com/ecb/products/pdf/en-b3f.pdf"&gt;Datasheet&lt;/a&gt; (B3F-1000)&lt;/p&gt;</description>
</package>
<package name="TACTILE_SWITCH_SMD_5.2MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, 5.2mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/Buttons/SMD-Button.pdf"&gt;Dimensional Drawing&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="TACTILE_SWITCH_SMD_RIGHT_ANGLE">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, Right-angle&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;</description>
</package>
<package name="TACTILE_SWITCH_SMD_4.6X2.8MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, 4.6 x 2.8mm&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.ck-components.com/media/1479/kmr2.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="TACTILE_SWITCH_LED_PTH_12MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - w/ LED - PTH&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons), with a built-in LED.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/General/TSD1265.png"&gt;Dimensional Drawing&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="TACTILE_SWITCH_LED_PTH_12MM_KIT">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - w/ LED - PTH, KIT Variant&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons), with a built-in LED.&lt;/p&gt;
&lt;p&gt;KIT variant is for soldering kits. There is no tStop (covering up the top side of the pads with mask). This helps the beginner see which side they should be soldering too.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/General/TSD1265.png"&gt;Dimensional Drawing&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="SWITCH_SP3T_SMD">
<description>&lt;h3&gt;CUS Low-Profile SP3T Slide Switch - SMD&lt;/h3&gt;
&lt;p&gt;&lt;a href="http://www.nidec-copal-electronics.com/e/catalog/switch/cus.pdf"&gt;Datasheet&lt;/a&gt; (CUS-13TB)&lt;/p&gt;</description>
</package>
<package name="SWITCH_SPDT_PTH_11.6X4.0MM">
<description>&lt;h3&gt;SPDT PTH Slide Switch&lt;/h3&gt;
&lt;p&gt;Single-pole, double-throw (SPDT) switch.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/Buttons/P040040c.pdf"&gt;Dimensional Drawing&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="SWITCH_SPDT_PTH_11.6X4.0MM_LOCK">
<description>&lt;h3&gt;SPDT PTH Slide Switch - Locking Footprint&lt;/h3&gt;
&lt;p&gt;Single-pole, double-throw (SPDT) switch.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Warning:&lt;/b&gt; This is the LOCK version of this package. This package has offset PTH pins, which help to hold the part in place while soldering.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/Buttons/P040040c.pdf"&gt;Dimensional Drawing&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="SWITCH_SPDT_PTH_11.6X4.0MM_KIT">
<description>&lt;h3&gt;SPDT PTH Slide Switch - KIT Footprint&lt;/h3&gt;
&lt;p&gt;Single-pole, double-throw (SPDT) switch.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/Buttons/P040040c.pdf"&gt;Dimensional Drawing&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="SWITCH_SPST_SMD_A">
<description>&lt;h3&gt;SPDT Slide Switch - SMD&lt;/h3&gt;
&lt;p&gt;Single-pole, double-throw (SPDT) switch.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/Switches/SLIDE.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="ROTARY_SWITCH_1X10">
<description>&lt;h3&gt;10-Position Rotary Switch&lt;/h3&gt;
&lt;p&gt;Taiwan Alpha 1 pole, 10 pos rotary switch.&lt;/p&gt;
&lt;p&gt;Arrows in tDocu denote pointer positions for 45-degree shaft, assuming a knob with a pointer that's opposite the set screw.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Components/Switches/SP14040026%20SPEC.pdf"&gt;Datasheet&lt;/a&gt; (Alpha PN SR2512F-0110-16f2b-c9-s-k)&lt;/p&gt;</description>
</package>
<package name="ROTARY_SWITCH_1X10_KIT">
<description>&lt;h3&gt;10-Position Rotary Switch - KIT Version&lt;/h3&gt;
&lt;p&gt;Taiwan Alpha 1 pole, 10 pos rotary switch.&lt;/p&gt;
&lt;p&gt;Arrows in tDocu denote pointer positions for 45-degree shaft, assuming a knob with a pointer that's opposite the set screw.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Components/Switches/SP14040026%20SPEC.pdf"&gt;Datasheet&lt;/a&gt; (Alpha PN SR2512F-0110-16f2b-c9-s-k)&lt;/p&gt;</description>
</package>
<package name="DIPSWITCH-02-50MIL">
<description>&lt;b&gt;2-Pin DIP Switch - SMD, 0.05"-Pitch&lt;/b&gt;
&lt;p&gt;Half-size SMT DIP switch, 1.27 mm / 0.05" pitch. For example the following:&lt;/p&gt;
&lt;ul&gt;
  &lt;li&gt;A6H-2101 or A6H-2102 in Omron A6H series; &lt;a href="http://www.omron.com/ecb/products/pdf/en-a6h.pdf"&gt;Datasheet&lt;/a&gt;&lt;/li&gt;
  &lt;li&gt;Digikey &lt;a href="http://www.digikey.com/product-detail/en/A6H-2101/A6H-2101-ND/1811590"&gt;A6H-2101-ND&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;</description>
</package>
<package name="DIPSWITCH-08">
<description>&lt;h3&gt;8-Position DIP Switch - PTH, 0.1"-Pitch&lt;/h3&gt;
&lt;p&gt;Standard size through-hole DIP switch, 2.54 mm / 0.1" pitch&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.sparkfun.com/datasheets/Components/Switch-DIP8.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="TRACKBALL">
<description>&lt;h3&gt;Trackball - Mechanical&lt;/h3&gt;
&lt;p&gt;This is a tiny trackball akin to those found on a number of Blackberry models (8100, 8300, 8320, 8800, 8830, etc). Each of the four spindles have a tiny circular magnet on each end. Great when paired with very small SMD Hall effect sensors.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/products/9308"&gt;Product Page&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="DIPSWITCH-06-SMD">
</package>
<package name="TACTILE_SWITCH_PTH_RIGHT_ANGLE">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, Right-angle&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/Switches/SW016.JPG"&gt;Dimensional Drawing&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="SWITCH_DPDT_SMD_JS202011JCQN">
</package>
</packages>
<symbols>
<symbol name="DIPSWITCH-02">
<description>&lt;h3&gt;2-Position DIP Switch&lt;/h3&gt;
&lt;p&gt;2-circuit DIP (dual inline package) switch. Commonly used to physcially set a circuit's behavior.&lt;/p&gt;</description>
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$11"/>
<pin name="P$12"/>
<pin name="P$10"/>
<pin name="P$9"/>
<pin name="P$8"/>
<pin name="P$7"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
</symbol>
<symbol name="DIPSWITCH-04">
<description>&lt;h3&gt;4-Position DIP Switch&lt;/h3&gt;
&lt;p&gt;4-circuit DIP (dual inline package) switch. Commonly used to physcially set a circuit's behavior.&lt;/p&gt;</description>
<pin name="1B"/>
<pin name="2B"/>
<pin name="3B"/>
<pin name="4B"/>
<pin name="1A"/>
<pin name="2A"/>
<pin name="3A"/>
<pin name="4A"/>
</symbol>
<symbol name="SWITCH-DPDT">
<description>&lt;h3&gt;Double-Pole, Double-Throw (DPDT) Switch&lt;/h3&gt;
&lt;p&gt;Double-pole, double-throw switches.&lt;/p&gt;</description>
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
</symbol>
<symbol name="BUTTON-CONDUCTIVE">
<description>&lt;h3&gt;Conductive Button&lt;/h3&gt;
&lt;p&gt;Used with rubber key pads on the &lt;a href="https://www.sparkfun.com/products/retired/8602"&gt;Nordic Key FOB&lt;/a&gt;. This one was designed and proven to work with the &lt;a href="https://www.sparkfun.com/products/retired/9377"&gt;PolyCase Key FOB enclosures&lt;/a&gt;.&lt;/p&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="BUTTON-MAGNETIC-SNAP">
<description>&lt;h3&gt;Magnetic Metal Snaps&lt;/h3&gt;
&lt;p&gt;18mm diameter snaps that couple together very strongly (must be pried apart), rotate freely on the axis, and are electrically conductive. Overall connection resistance is less than 200 miliOhm. Snaps will couple when closer than 10mm.&lt;/p&gt;</description>
<pin name="1"/>
</symbol>
<symbol name="BUTTONPAD-RGB">
<description>&lt;h3&gt;Button Pad w/ RGB LED&lt;/h3&gt;
&lt;p&gt;Used by 2x2 and 4x4 button pads&lt;/p&gt;</description>
<pin name="GRN"/>
<pin name="BLU"/>
<pin name="GND"/>
<pin name="RED"/>
<pin name="SIG2"/>
<pin name="SIG1"/>
</symbol>
<symbol name="BUTTONPAD-LED">
<description>&lt;h3&gt;Button Pad w/ Single LEDs&lt;/h3&gt;
&lt;p&gt;Used by 2x2 and 4x4 button pads.&lt;/p&gt;</description>
<pin name="A"/>
<pin name="K"/>
<pin name="SIG2"/>
<pin name="SIG1"/>
</symbol>
<symbol name="ENCODER-QUADRATURE">
<description>&lt;h3&gt;Rotary Encoder&lt;/h3&gt;
&lt;p&gt;Encoders rotate similarly to potentiometers, but they’re different from potentiometers in that an encoder has full rotation without limits. They output gray code so that you can tell how much and in which direction the encoder has been turned.&lt;/p&gt;</description>
<pin name="C"/>
<pin name="A"/>
<pin name="B"/>
</symbol>
<symbol name="ENCODER_LED_2-1">
<description>&lt;h3&gt;Illuminated Rotary Encoder w/ 2 LEDs&lt;/h3&gt;
&lt;p&gt;Rotary encoders rotate similarly to potentiometers, but they’re different from potentiometers in that an encoder has full rotation without limits. They output gray code so that you can tell how much and in which direction the encoder has been turned.&lt;/p&gt;</description>
<pin name="-" direction="pas"/>
<pin name="+R" direction="pas"/>
<pin name="A"/>
<pin name="C"/>
<pin name="B"/>
<pin name="+G" direction="pas"/>
<pin name="SW" direction="pas"/>
</symbol>
<symbol name="ENCODER_LED_3_CA">
<description>&lt;h3&gt;Illuminated Rotary Encoder w/ RGB LED and select switch&lt;/h3&gt;
&lt;p&gt;Encoders rotate similarly to potentiometers, but they’re different from potentiometers in that an encoder has full rotation without limits. They output gray code so that you can tell how much and in which direction the encoder has been turned.&lt;/p&gt;</description>
<pin name="+" direction="pas"/>
<pin name="-G" direction="pas"/>
<pin name="A"/>
<pin name="C"/>
<pin name="B"/>
<pin name="-R" direction="pas"/>
<pin name="SW" direction="pas"/>
<pin name="-B" direction="pas"/>
</symbol>
<symbol name="JOYSTICK">
<description>&lt;h3&gt;Analog Thumb Joystick&lt;/h3&gt;
&lt;p&gt;This is a joystick very similar to the ‘analog’ joysticks on PS2 (PlayStation 2) controllers. Directional movements are simply two potentiometers - one for each axis. Pots are ~10k each. This joystick also has a select button that is actuated when the joystick is pressed down.&lt;/p&gt;</description>
<pin name="V+"/>
<pin name="V"/>
<pin name="V-"/>
<pin name="H+"/>
<pin name="H"/>
<pin name="H-"/>
<pin name="SEL+"/>
<pin name="SEL-"/>
</symbol>
<symbol name="JOYSTICK-PSP1000">
<description>&lt;h3&gt;Resistive Thumb Slide Joystick&lt;/h3&gt;
&lt;p&gt;This is a resistive analog joystick, very similar to those found on the PSP1000. These compact joysticks are different in that they have a very interesting ‘slide’ feeling.&lt;/p&gt;</description>
<pin name="X"/>
<pin name="Y"/>
<pin name="VCC"/>
<pin name="GND"/>
</symbol>
<symbol name="JOYSTICK_MINI">
<description>&lt;h3&gt;Small Tactile Joystick w/ Select Switch&lt;/h3&gt;
&lt;p&gt;A 5-way tactile switch allows for a joystick-like interface in a very small package.&lt;/p&gt;</description>
<pin name="CENT"/>
<pin name="DOWN"/>
<pin name="GND"/>
<pin name="LEFT"/>
<pin name="RIGHT"/>
<pin name="UP"/>
</symbol>
<symbol name="NAV_SWITCH">
<description>&lt;h3&gt;Navigation Switch&lt;/h3&gt;
&lt;p&gt;Three way navigation switch. Commonly used as up/down/select on MP3 players. Schematic element and footprint production proven.&lt;/p&gt;</description>
<pin name="1" direction="in"/>
<pin name="T" direction="in"/>
<pin name="2" direction="in"/>
<pin name="C" direction="pwr"/>
</symbol>
<symbol name="ROT_ENCODER">
<description>&lt;h3&gt;Rotary Encoder w/ Select Switch&lt;/h3&gt;
&lt;p&gt;Encoders rotate similarly to potentiometers, but they’re different from potentiometers in that an encoder has full rotation without limits. They output gray code so that you can tell how much and in which direction the encoder has been turned.&lt;/p&gt;</description>
<pin name="SW+"/>
<pin name="SW-"/>
<pin name="B"/>
<pin name="C"/>
<pin name="A"/>
</symbol>
<symbol name="SW_SPDT_POL">
<description>&lt;h3&gt;SPST Switch w/ Polarity Mark&lt;/h3&gt;
&lt;p&gt;Used by 3PDT switch. Drawn as three separate gates for schematic clarity.&lt;/p&gt;</description>
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
</symbol>
<symbol name="SWITCH-MOMENTARY-2">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="SWITCH-MOMENTARY-LED">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - w/ LED&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons), with a built-in LED.&lt;/p&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="SWITCH-SP3T">
<description>&lt;h3&gt;Single-Pole, Triple-Throw (SP3T) Switch&lt;/h3&gt;
&lt;p&gt;Single-Pole, Triple-Throw switches&lt;/p&gt;</description>
<pin name="1"/>
<pin name="3"/>
<pin name="2"/>
<pin name="4"/>
</symbol>
<symbol name="TOGGLE">
<description>&lt;h3&gt;Single Pole, Double Throw (SPDT) Switch&lt;/h3&gt;
&lt;p&gt;Single-pole, double-throw (SPDT) switch.&lt;/p&gt;</description>
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="O" direction="pas"/>
</symbol>
<symbol name="ROTARY-SWITCH-1X10">
<description>&lt;h3&gt;10-Position Rotary Switch&lt;/h3&gt;
&lt;p&gt;Single pole, 10 position rotary switch able to select up to 10 different states.&lt;/p&gt;</description>
<pin name="COMMON"/>
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
</symbol>
<symbol name="SWITCH-MOMENTARY">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - Two Circuits&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons). Schematic symbol includes two switch circuits.&lt;/p&gt;</description>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="SW_DIP-8">
<description>&lt;h3&gt;8-Position DIP Switch&lt;/h3&gt;
&lt;p&gt;8-circuit DIP (dual inline package) switch. Commonly used to physcially set a circuit's behavior.&lt;/p&gt;</description>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="TRACKBALL">
<description>&lt;h3&gt;Trackball - Mechanical&lt;/h3&gt;
&lt;p&gt;This is a tiny trackball akin to those found on a number of Blackberry models (8100, 8300, 8320, 8800, 8830, etc). Each of the four spindles have a tiny circular magnet on each end. Great when paired with very small SMD Hall effect sensors.&lt;/p&gt;</description>
</symbol>
<symbol name="REED_SWITCH">
<description>&lt;h3&gt;Reed Switch&lt;/h3&gt;
&lt;p&gt;A reed switch is a magnetically-actuated switch. When the device is exposed to a magnetic field, the two ferrous materials inside the switch pull together and the switch closes.&lt;/p&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="DIPSWITCH-06">
<pin name="1"/>
<pin name="2"/>
<pin name="11"/>
<pin name="12"/>
<pin name="10"/>
<pin name="9"/>
<pin name="8"/>
<pin name="7"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="DIP-02" prefix="S">
<description>&lt;h3&gt;2-Position DIP Switch&lt;/h3&gt;
&lt;p&gt;2-circuit DIP (dual inline package) switch. Commonly used to physcially set a circuit's behavior.&lt;/p&gt;
&lt;h4&gt;Variants&lt;/h4&gt;
&lt;h5&gt;PTH-100MIL - Through-hole, 0.1"-Pitch&lt;/h5&gt;
&lt;ul&gt;
&lt;li&gt;Used on &lt;a href="https://www.sparkfun.com/products/13899"&gt;SparkFun Stepoko&lt;/a&gt; (ROB-13899)&lt;/li&gt;
&lt;/ul&gt;
&lt;h5&gt;SMD-50MIL-JWING - SMD (J-Wing Pads), 0.05"-Pitch&lt;/h5&gt;
&lt;ul&gt;
&lt;li&gt;&lt;em&gt;Prototype Part&lt;/em&gt;&lt;/li&gt;
&lt;/ul&gt;
&lt;h5&gt;SMD-50MIL - SMD, 0.05"-Pitch&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;Used on &lt;a href="https://www.sparkfun.com/products/13777"&gt;SparkFun Battery Babysitter&lt;/a&gt; (PRT-13777)&lt;/li&gt;&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="DIPSWITCH-02"/>
</gates>
<devices>
<device name="-SMD-50MIL-JWING" package="DIPSWITCH-02-CHS-02A">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$11" pad="3"/>
<connect gate="G$1" pin="P$12" pad="4"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-12372"/>
</technology>
</technologies>
</device>
<device name="-PTH-100MIL" package="DIPSWITCH-02-209-2LPST">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$11" pad="3"/>
<connect gate="G$1" pin="P$12" pad="4"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-12532"/>
</technology>
</technologies>
</device>
<device name="-SMD-50MIL" package="DIPSWITCH-02-50MIL">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$11" pad="3"/>
<connect gate="G$1" pin="P$12" pad="4"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-13215"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIP-04" prefix="S">
<description>&lt;h3&gt;4-Position DIP Switch&lt;/h3&gt;
&lt;p&gt;4-circuit DIP (dual inline package) switch. Commonly used to physcially set a circuit's behavior.&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;&lt;em&gt;Prototype Part&lt;/em&gt;&lt;/li&gt;&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="DIPSWITCH-04"/>
</gates>
<devices>
<device name="SMD" package="DIPSWITCH-04-SMD">
<connects>
<connect gate="G$1" pin="1A" pad="1"/>
<connect gate="G$1" pin="1B" pad="8"/>
<connect gate="G$1" pin="2A" pad="2"/>
<connect gate="G$1" pin="2B" pad="7"/>
<connect gate="G$1" pin="3A" pad="3"/>
<connect gate="G$1" pin="3B" pad="6"/>
<connect gate="G$1" pin="4A" pad="4"/>
<connect gate="G$1" pin="4B" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-12418"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BUTTON-CONDUCTIVE" prefix="S">
<description>&lt;h3&gt;Conductive Button&lt;/h3&gt;
&lt;p&gt;Used with rubber key pads on the &lt;a href="https://www.sparkfun.com/products/retired/8602"&gt;Nordic Key FOB&lt;/a&gt;. This one was designed and proven to work with the &lt;a href="https://www.sparkfun.com/products/retired/9377"&gt;PolyCase Key FOB enclosures&lt;/a&gt;.&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/retired/8602"&gt;Nordic Fob&lt;/a&gt; (WRL-08602)&lt;/li&gt;&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="BUTTON-CONDUCTIVE"/>
</gates>
<devices>
<device name="SMD" package="BUTTON-CONDUCTIVE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BUTTON-MAGNETIC-SNAP" prefix="S">
<description>&lt;h3&gt;Magnetic Metal Snaps&lt;/h3&gt;
&lt;p&gt;18mm diameter snaps that couple together very strongly (must be pried apart), rotate freely on the axis, and are electrically conductive. Overall connection resistance is less than 200 miliOhm. Snaps will couple when closer than 10mm.&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8682"&gt;Magnetic Snap 18mm&lt;/a&gt; (WRL-08682)&lt;/li&gt;&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="BUTTON-MAGNETIC-SNAP"/>
</gates>
<devices>
<device name="18MM" package="BUTTON-18MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_SKU" value="DEV-08682"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BUTTONPAD-2X2-RGB" prefix="S">
<description>&lt;h3&gt;2x2 Button Pad w/ RGB LEDs&lt;/h3&gt;
&lt;p&gt;Layout and schematic for 2x2 button pad with tri-color LEDs under each button. For use with the &lt;a href="https://www.sparkfun.com/products/7836"&gt;Button Pad 2x2 - LED Compatible&lt;/a&gt; and &lt;a href="https://www.sparkfun.com/products/8746"&gt;Button Pad 2x2 Top Bezel&lt;/a&gt;.&lt;/p&gt;
&lt;p&gt;Any &lt;a href="https://www.sparkfun.com/categories/172"&gt;RGB 5mm LED&lt;/a&gt; should be compatible.&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10547"&gt;SparkFun Simon Says - Through-Hole Soldering Kit&lt;/a&gt; (KIT-10547)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9277"&gt;Button Pad 2x2 - Breakout PCB&lt;/a&gt; (COM-09277)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="-C1" symbol="BUTTONPAD-RGB"/>
<gate name="-C2" symbol="BUTTONPAD-RGB"/>
<gate name="-C3" symbol="BUTTONPAD-RGB"/>
<gate name="-C4" symbol="BUTTONPAD-RGB"/>
</gates>
<devices>
<device name="" package="BUTTONPAD-2X2">
<connects>
<connect gate="-C1" pin="BLU" pad="BLU1"/>
<connect gate="-C1" pin="GND" pad="GND1"/>
<connect gate="-C1" pin="GRN" pad="GRN1"/>
<connect gate="-C1" pin="RED" pad="RED1"/>
<connect gate="-C1" pin="SIG1" pad="SIG1"/>
<connect gate="-C1" pin="SIG2" pad="SIG2"/>
<connect gate="-C2" pin="BLU" pad="BLU2"/>
<connect gate="-C2" pin="GND" pad="GND2"/>
<connect gate="-C2" pin="GRN" pad="GRN2"/>
<connect gate="-C2" pin="RED" pad="RED2"/>
<connect gate="-C2" pin="SIG1" pad="SIG3"/>
<connect gate="-C2" pin="SIG2" pad="SIG4"/>
<connect gate="-C3" pin="BLU" pad="BLU3"/>
<connect gate="-C3" pin="GND" pad="GND3"/>
<connect gate="-C3" pin="GRN" pad="GRN3"/>
<connect gate="-C3" pin="RED" pad="RED3"/>
<connect gate="-C3" pin="SIG1" pad="SIG5"/>
<connect gate="-C3" pin="SIG2" pad="SIG6"/>
<connect gate="-C4" pin="BLU" pad="BLU4"/>
<connect gate="-C4" pin="GND" pad="GND4"/>
<connect gate="-C4" pin="GRN" pad="GRN4"/>
<connect gate="-C4" pin="RED" pad="RED4"/>
<connect gate="-C4" pin="SIG1" pad="SIG7"/>
<connect gate="-C4" pin="SIG2" pad="SIG8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-08481"/>
<attribute name="SF_SKU" value="COM-07836"/>
</technology>
</technologies>
</device>
<device name="-STAGGERED" package="BUTTONPAD-2X2-STAGGERED">
<connects>
<connect gate="-C1" pin="BLU" pad="BLU1"/>
<connect gate="-C1" pin="GND" pad="GND1"/>
<connect gate="-C1" pin="GRN" pad="GRN1"/>
<connect gate="-C1" pin="RED" pad="RED1"/>
<connect gate="-C1" pin="SIG1" pad="SIG1"/>
<connect gate="-C1" pin="SIG2" pad="SIG2"/>
<connect gate="-C2" pin="BLU" pad="BLU2"/>
<connect gate="-C2" pin="GND" pad="GND2"/>
<connect gate="-C2" pin="GRN" pad="GRN2"/>
<connect gate="-C2" pin="RED" pad="RED2"/>
<connect gate="-C2" pin="SIG1" pad="SIG3"/>
<connect gate="-C2" pin="SIG2" pad="SIG4"/>
<connect gate="-C3" pin="BLU" pad="BLU3"/>
<connect gate="-C3" pin="GND" pad="GND3"/>
<connect gate="-C3" pin="GRN" pad="GRN3"/>
<connect gate="-C3" pin="RED" pad="RED3"/>
<connect gate="-C3" pin="SIG1" pad="SIG5"/>
<connect gate="-C3" pin="SIG2" pad="SIG6"/>
<connect gate="-C4" pin="BLU" pad="BLU4"/>
<connect gate="-C4" pin="GND" pad="GND4"/>
<connect gate="-C4" pin="GRN" pad="GRN4"/>
<connect gate="-C4" pin="RED" pad="RED4"/>
<connect gate="-C4" pin="SIG1" pad="SIG7"/>
<connect gate="-C4" pin="SIG2" pad="SIG8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-08481"/>
<attribute name="SF_SKU" value="COM-07836"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BUTTONPAD-2X2-LED" prefix="S">
<description>&lt;h3&gt;2x2 Button Pad w/ Single LEDs&lt;/h3&gt;
&lt;p&gt;Layout and schematic for 2x2 button pad with single-color LEDs under each button. For use with the &lt;a href="https://www.sparkfun.com/products/7836"&gt;Button Pad 2x2 - LED Compatible&lt;/a&gt; and &lt;a href="https://www.sparkfun.com/products/8746"&gt;Button Pad 2x2 Top Bezel&lt;/a&gt;.&lt;/p&gt;
&lt;p&gt;Any &lt;a href="https://www.sparkfun.com/categories/172"&gt;single-color 5mm LED&lt;/a&gt; should be compatible.&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10547"&gt;SparkFun Simon Says - Through-Hole Soldering Kit&lt;/a&gt; (KIT-10547)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9277"&gt;Button Pad 2x2 - Breakout PCB&lt;/a&gt; (COM-09277)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="C1" symbol="BUTTONPAD-LED"/>
<gate name="C2" symbol="BUTTONPAD-LED"/>
<gate name="C3" symbol="BUTTONPAD-LED"/>
<gate name="C4" symbol="BUTTONPAD-LED"/>
</gates>
<devices>
<device name="" package="BUTTONPAD-2X2-SINGLE-LED">
<connects>
<connect gate="C1" pin="A" pad="A1"/>
<connect gate="C1" pin="K" pad="K1"/>
<connect gate="C1" pin="SIG1" pad="SIG1"/>
<connect gate="C1" pin="SIG2" pad="SIG2"/>
<connect gate="C2" pin="A" pad="A2"/>
<connect gate="C2" pin="K" pad="K2"/>
<connect gate="C2" pin="SIG1" pad="SIG3"/>
<connect gate="C2" pin="SIG2" pad="SIG4"/>
<connect gate="C3" pin="A" pad="A3"/>
<connect gate="C3" pin="K" pad="K3"/>
<connect gate="C3" pin="SIG1" pad="SIG5"/>
<connect gate="C3" pin="SIG2" pad="SIG6"/>
<connect gate="C4" pin="A" pad="A4"/>
<connect gate="C4" pin="K" pad="K4"/>
<connect gate="C4" pin="SIG1" pad="SIG7"/>
<connect gate="C4" pin="SIG2" pad="SIG8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-08481"/>
<attribute name="SF_SKU" value="COM-07836"/>
</technology>
</technologies>
</device>
<device name="KIT" package="BUTTONPAD-2X2-SINGLE-LED-KIT">
<connects>
<connect gate="C1" pin="A" pad="A1"/>
<connect gate="C1" pin="K" pad="K1"/>
<connect gate="C1" pin="SIG1" pad="SIG1"/>
<connect gate="C1" pin="SIG2" pad="SIG2"/>
<connect gate="C2" pin="A" pad="A2"/>
<connect gate="C2" pin="K" pad="K2"/>
<connect gate="C2" pin="SIG1" pad="SIG3"/>
<connect gate="C2" pin="SIG2" pad="SIG4"/>
<connect gate="C3" pin="A" pad="A3"/>
<connect gate="C3" pin="K" pad="K3"/>
<connect gate="C3" pin="SIG1" pad="SIG5"/>
<connect gate="C3" pin="SIG2" pad="SIG6"/>
<connect gate="C4" pin="A" pad="A4"/>
<connect gate="C4" pin="K" pad="K4"/>
<connect gate="C4" pin="SIG1" pad="SIG7"/>
<connect gate="C4" pin="SIG2" pad="SIG8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-08481"/>
<attribute name="SF_SKU" value="COM-07836"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BUTTONPAD-4X4-RGB" prefix="S">
<description>&lt;h3&gt;4x4 Button Pad w/ RGB LEDs&lt;/h3&gt;
&lt;p&gt;Layout and schematic for 4x4 button pad with tri-color LEDs under each button. For use with the 4x &lt;a href="https://www.sparkfun.com/products/7836"&gt;Button Pad 2x2 - LED Compatible&lt;/a&gt; and 4x &lt;a href="https://www.sparkfun.com/products/8746"&gt;Button Pad 2x2 Top Bezel&lt;/a&gt;.&lt;/p&gt;
&lt;p&gt;Any &lt;a href="https://www.sparkfun.com/categories/172"&gt;RGB 5mm LED&lt;/a&gt; should be compatible.&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10547"&gt;SparkFun Simon Says - Through-Hole Soldering Kit&lt;/a&gt; (KIT-10547)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9277"&gt;Button Pad 2x2 - Breakout PCB&lt;/a&gt; (COM-09277)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$0" symbol="BUTTONPAD-RGB"/>
<gate name="G$1" symbol="BUTTONPAD-RGB"/>
<gate name="G$2" symbol="BUTTONPAD-RGB"/>
<gate name="G$3" symbol="BUTTONPAD-RGB"/>
<gate name="G$4" symbol="BUTTONPAD-RGB"/>
<gate name="G$5" symbol="BUTTONPAD-RGB"/>
<gate name="G$6" symbol="BUTTONPAD-RGB"/>
<gate name="G$7" symbol="BUTTONPAD-RGB"/>
<gate name="G$8" symbol="BUTTONPAD-RGB"/>
<gate name="G$9" symbol="BUTTONPAD-RGB"/>
<gate name="G$10" symbol="BUTTONPAD-RGB"/>
<gate name="G$11" symbol="BUTTONPAD-RGB"/>
<gate name="G$12" symbol="BUTTONPAD-RGB"/>
<gate name="G$13" symbol="BUTTONPAD-RGB"/>
<gate name="G$14" symbol="BUTTONPAD-RGB"/>
<gate name="G$15" symbol="BUTTONPAD-RGB"/>
</gates>
<devices>
<device name="" package="BUTTONPAD-4X4">
<connects>
<connect gate="G$0" pin="BLU" pad="BLU0"/>
<connect gate="G$0" pin="GND" pad="GND0"/>
<connect gate="G$0" pin="GRN" pad="GRN0"/>
<connect gate="G$0" pin="RED" pad="RED0"/>
<connect gate="G$0" pin="SIG1" pad="SIG0"/>
<connect gate="G$0" pin="SIG2" pad="SIG1"/>
<connect gate="G$1" pin="BLU" pad="BLU1"/>
<connect gate="G$1" pin="GND" pad="GND1"/>
<connect gate="G$1" pin="GRN" pad="GRN1"/>
<connect gate="G$1" pin="RED" pad="RED1"/>
<connect gate="G$1" pin="SIG1" pad="SIG2"/>
<connect gate="G$1" pin="SIG2" pad="SIG3"/>
<connect gate="G$10" pin="BLU" pad="BLU10"/>
<connect gate="G$10" pin="GND" pad="GND10"/>
<connect gate="G$10" pin="GRN" pad="GRN10"/>
<connect gate="G$10" pin="RED" pad="RED10"/>
<connect gate="G$10" pin="SIG1" pad="SIG20"/>
<connect gate="G$10" pin="SIG2" pad="SIG21"/>
<connect gate="G$11" pin="BLU" pad="BLU11"/>
<connect gate="G$11" pin="GND" pad="GND11"/>
<connect gate="G$11" pin="GRN" pad="GRN11"/>
<connect gate="G$11" pin="RED" pad="RED11"/>
<connect gate="G$11" pin="SIG1" pad="SIG22"/>
<connect gate="G$11" pin="SIG2" pad="SIG23"/>
<connect gate="G$12" pin="BLU" pad="BLU12"/>
<connect gate="G$12" pin="GND" pad="GND12"/>
<connect gate="G$12" pin="GRN" pad="GRN12"/>
<connect gate="G$12" pin="RED" pad="RED12"/>
<connect gate="G$12" pin="SIG1" pad="SIG24"/>
<connect gate="G$12" pin="SIG2" pad="SIG25"/>
<connect gate="G$13" pin="BLU" pad="BLU13"/>
<connect gate="G$13" pin="GND" pad="GND13"/>
<connect gate="G$13" pin="GRN" pad="GRN13"/>
<connect gate="G$13" pin="RED" pad="RED13"/>
<connect gate="G$13" pin="SIG1" pad="SIG26"/>
<connect gate="G$13" pin="SIG2" pad="SIG27"/>
<connect gate="G$14" pin="BLU" pad="BLU14"/>
<connect gate="G$14" pin="GND" pad="GND14"/>
<connect gate="G$14" pin="GRN" pad="GRN14"/>
<connect gate="G$14" pin="RED" pad="RED14"/>
<connect gate="G$14" pin="SIG1" pad="SIG28"/>
<connect gate="G$14" pin="SIG2" pad="SIG29"/>
<connect gate="G$15" pin="BLU" pad="BLU15"/>
<connect gate="G$15" pin="GND" pad="GND15"/>
<connect gate="G$15" pin="GRN" pad="GRN15"/>
<connect gate="G$15" pin="RED" pad="RED15"/>
<connect gate="G$15" pin="SIG1" pad="SIG30"/>
<connect gate="G$15" pin="SIG2" pad="SIG31"/>
<connect gate="G$2" pin="BLU" pad="BLU2"/>
<connect gate="G$2" pin="GND" pad="GND2"/>
<connect gate="G$2" pin="GRN" pad="GRN2"/>
<connect gate="G$2" pin="RED" pad="RED2"/>
<connect gate="G$2" pin="SIG1" pad="SIG4"/>
<connect gate="G$2" pin="SIG2" pad="SIG5"/>
<connect gate="G$3" pin="BLU" pad="BLU3"/>
<connect gate="G$3" pin="GND" pad="GND3"/>
<connect gate="G$3" pin="GRN" pad="GRN3"/>
<connect gate="G$3" pin="RED" pad="RED3"/>
<connect gate="G$3" pin="SIG1" pad="SIG6"/>
<connect gate="G$3" pin="SIG2" pad="SIG7"/>
<connect gate="G$4" pin="BLU" pad="BLU4"/>
<connect gate="G$4" pin="GND" pad="GND4"/>
<connect gate="G$4" pin="GRN" pad="GRN4"/>
<connect gate="G$4" pin="RED" pad="RED4"/>
<connect gate="G$4" pin="SIG1" pad="SIG8"/>
<connect gate="G$4" pin="SIG2" pad="SIG9"/>
<connect gate="G$5" pin="BLU" pad="BLU5"/>
<connect gate="G$5" pin="GND" pad="GND5"/>
<connect gate="G$5" pin="GRN" pad="GRN6"/>
<connect gate="G$5" pin="RED" pad="RED5"/>
<connect gate="G$5" pin="SIG1" pad="SIG10"/>
<connect gate="G$5" pin="SIG2" pad="SIG11"/>
<connect gate="G$6" pin="BLU" pad="BLU6"/>
<connect gate="G$6" pin="GND" pad="GND6"/>
<connect gate="G$6" pin="GRN" pad="GRN5"/>
<connect gate="G$6" pin="RED" pad="RED6"/>
<connect gate="G$6" pin="SIG1" pad="SIG12"/>
<connect gate="G$6" pin="SIG2" pad="SIG13"/>
<connect gate="G$7" pin="BLU" pad="BLU7"/>
<connect gate="G$7" pin="GND" pad="GND7"/>
<connect gate="G$7" pin="GRN" pad="GRN7"/>
<connect gate="G$7" pin="RED" pad="RED7"/>
<connect gate="G$7" pin="SIG1" pad="SIG14"/>
<connect gate="G$7" pin="SIG2" pad="SIG15"/>
<connect gate="G$8" pin="BLU" pad="BLU8"/>
<connect gate="G$8" pin="GND" pad="GND8"/>
<connect gate="G$8" pin="GRN" pad="GRN8"/>
<connect gate="G$8" pin="RED" pad="RED8"/>
<connect gate="G$8" pin="SIG1" pad="SIG16"/>
<connect gate="G$8" pin="SIG2" pad="SIG17"/>
<connect gate="G$9" pin="BLU" pad="BLU9"/>
<connect gate="G$9" pin="GND" pad="GND9"/>
<connect gate="G$9" pin="GRN" pad="GRN9"/>
<connect gate="G$9" pin="RED" pad="RED9"/>
<connect gate="G$9" pin="SIG1" pad="SIG18"/>
<connect gate="G$9" pin="SIG2" pad="SIG19"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-08481"/>
<attribute name="SF_SKU" value="COM-07836"/>
</technology>
</technologies>
</device>
<device name="-STAGGERED" package="BUTTONPAD-4X4-STAGGERED">
<connects>
<connect gate="G$0" pin="BLU" pad="BLU0"/>
<connect gate="G$0" pin="GND" pad="GND0"/>
<connect gate="G$0" pin="GRN" pad="GRN0"/>
<connect gate="G$0" pin="RED" pad="RED0"/>
<connect gate="G$0" pin="SIG1" pad="SIG0"/>
<connect gate="G$0" pin="SIG2" pad="SIG1"/>
<connect gate="G$1" pin="BLU" pad="BLU1"/>
<connect gate="G$1" pin="GND" pad="GND1"/>
<connect gate="G$1" pin="GRN" pad="GRN1"/>
<connect gate="G$1" pin="RED" pad="RED1"/>
<connect gate="G$1" pin="SIG1" pad="SIG2"/>
<connect gate="G$1" pin="SIG2" pad="SIG3"/>
<connect gate="G$10" pin="BLU" pad="BLU10"/>
<connect gate="G$10" pin="GND" pad="GND10"/>
<connect gate="G$10" pin="GRN" pad="GRN10"/>
<connect gate="G$10" pin="RED" pad="RED10"/>
<connect gate="G$10" pin="SIG1" pad="SIG20"/>
<connect gate="G$10" pin="SIG2" pad="SIG21"/>
<connect gate="G$11" pin="BLU" pad="BLU11"/>
<connect gate="G$11" pin="GND" pad="GND11"/>
<connect gate="G$11" pin="GRN" pad="GRN11"/>
<connect gate="G$11" pin="RED" pad="RED11"/>
<connect gate="G$11" pin="SIG1" pad="SIG22"/>
<connect gate="G$11" pin="SIG2" pad="SIG23"/>
<connect gate="G$12" pin="BLU" pad="BLU12"/>
<connect gate="G$12" pin="GND" pad="GND12"/>
<connect gate="G$12" pin="GRN" pad="GRN12"/>
<connect gate="G$12" pin="RED" pad="RED12"/>
<connect gate="G$12" pin="SIG1" pad="SIG24"/>
<connect gate="G$12" pin="SIG2" pad="SIG25"/>
<connect gate="G$13" pin="BLU" pad="BLU13"/>
<connect gate="G$13" pin="GND" pad="GND13"/>
<connect gate="G$13" pin="GRN" pad="GRN13"/>
<connect gate="G$13" pin="RED" pad="RED13"/>
<connect gate="G$13" pin="SIG1" pad="SIG26"/>
<connect gate="G$13" pin="SIG2" pad="SIG27"/>
<connect gate="G$14" pin="BLU" pad="BLU14"/>
<connect gate="G$14" pin="GND" pad="GND14"/>
<connect gate="G$14" pin="GRN" pad="GRN14"/>
<connect gate="G$14" pin="RED" pad="RED14"/>
<connect gate="G$14" pin="SIG1" pad="SIG28"/>
<connect gate="G$14" pin="SIG2" pad="SIG29"/>
<connect gate="G$15" pin="BLU" pad="BLU15"/>
<connect gate="G$15" pin="GND" pad="GND15"/>
<connect gate="G$15" pin="GRN" pad="GRN15"/>
<connect gate="G$15" pin="RED" pad="RED15"/>
<connect gate="G$15" pin="SIG1" pad="SIG30"/>
<connect gate="G$15" pin="SIG2" pad="SIG31"/>
<connect gate="G$2" pin="BLU" pad="BLU2"/>
<connect gate="G$2" pin="GND" pad="GND2"/>
<connect gate="G$2" pin="GRN" pad="GRN2"/>
<connect gate="G$2" pin="RED" pad="RED2"/>
<connect gate="G$2" pin="SIG1" pad="SIG4"/>
<connect gate="G$2" pin="SIG2" pad="SIG5"/>
<connect gate="G$3" pin="BLU" pad="BLU3"/>
<connect gate="G$3" pin="GND" pad="GND3"/>
<connect gate="G$3" pin="GRN" pad="GRN3"/>
<connect gate="G$3" pin="RED" pad="RED3"/>
<connect gate="G$3" pin="SIG1" pad="SIG6"/>
<connect gate="G$3" pin="SIG2" pad="SIG7"/>
<connect gate="G$4" pin="BLU" pad="BLU4"/>
<connect gate="G$4" pin="GND" pad="GND4"/>
<connect gate="G$4" pin="GRN" pad="GRN4"/>
<connect gate="G$4" pin="RED" pad="RED4"/>
<connect gate="G$4" pin="SIG1" pad="SIG8"/>
<connect gate="G$4" pin="SIG2" pad="SIG9"/>
<connect gate="G$5" pin="BLU" pad="BLU5"/>
<connect gate="G$5" pin="GND" pad="GND5"/>
<connect gate="G$5" pin="GRN" pad="GRN6"/>
<connect gate="G$5" pin="RED" pad="RED5"/>
<connect gate="G$5" pin="SIG1" pad="SIG10"/>
<connect gate="G$5" pin="SIG2" pad="SIG11"/>
<connect gate="G$6" pin="BLU" pad="BLU6"/>
<connect gate="G$6" pin="GND" pad="GND6"/>
<connect gate="G$6" pin="GRN" pad="GRN5"/>
<connect gate="G$6" pin="RED" pad="RED6"/>
<connect gate="G$6" pin="SIG1" pad="SIG12"/>
<connect gate="G$6" pin="SIG2" pad="SIG13"/>
<connect gate="G$7" pin="BLU" pad="BLU7"/>
<connect gate="G$7" pin="GND" pad="GND7"/>
<connect gate="G$7" pin="GRN" pad="GRN7"/>
<connect gate="G$7" pin="RED" pad="RED7"/>
<connect gate="G$7" pin="SIG1" pad="SIG14"/>
<connect gate="G$7" pin="SIG2" pad="SIG15"/>
<connect gate="G$8" pin="BLU" pad="BLU8"/>
<connect gate="G$8" pin="GND" pad="GND8"/>
<connect gate="G$8" pin="GRN" pad="GRN8"/>
<connect gate="G$8" pin="RED" pad="RED8"/>
<connect gate="G$8" pin="SIG1" pad="SIG16"/>
<connect gate="G$8" pin="SIG2" pad="SIG17"/>
<connect gate="G$9" pin="BLU" pad="BLU9"/>
<connect gate="G$9" pin="GND" pad="GND9"/>
<connect gate="G$9" pin="GRN" pad="GRN9"/>
<connect gate="G$9" pin="RED" pad="RED9"/>
<connect gate="G$9" pin="SIG1" pad="SIG18"/>
<connect gate="G$9" pin="SIG2" pad="SIG19"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-08481"/>
<attribute name="SF_SKU" value="COM-07836"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ENCODER" prefix="S" uservalue="yes">
<description>&lt;h3&gt;Rotary Encoder&lt;/h3&gt;
&lt;p&gt;Encoders rotate similarly to potentiometers, but they’re different from potentiometers in that an encoder has full rotation without limits. They output gray code so that you can tell how much and in which direction the encoder has been turned.&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;Used on the &lt;a href="https://www.sparkfun.com/products/11043"&gt;https://www.sparkfun.com/products/11043&lt;/a&gt; (COM-11043)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="ENCODER-QUADRATURE"/>
</gates>
<devices>
<device name="" package="ENCODER-16MM-QUAD">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-11299"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ENCODER-2LED" prefix="S">
<description>&lt;h3&gt;Illuminated Rotary Encoder w/ 2 LEDs&lt;/h3&gt;
&lt;p&gt;Rotary encoders rotate similarly to potentiometers, but they’re different from potentiometers in that an encoder has full rotation without limits. They output gray code so that you can tell how much and in which direction the encoder has been turned.&lt;/p&gt;
&lt;p&gt;This encoder has a red/green LED built-in, which shines through the encoder shaft.&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10596"&gt;Rotary Encoder - Illuminated (Red/Green)&lt;/a&gt; (COM-10596)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11722"&gt;SparkFun Rotary Encoder Breakout - Illuminated (RG/RGB)&lt;/a&gt; (BOB-11722)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="ENCODER_LED_2-1"/>
</gates>
<devices>
<device name="" package="ENCODER_LED_2">
<connects>
<connect gate="G$1" pin="+G" pad="+G"/>
<connect gate="G$1" pin="+R" pad="+R"/>
<connect gate="G$1" pin="-" pad="GND"/>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="SW" pad="SW"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-11113"/>
<attribute name="SF_SKU" value="COM-10596"/>
</technology>
</technologies>
</device>
<device name="KIT" package="ENCODER_LED_2_KIT">
<connects>
<connect gate="G$1" pin="+G" pad="+G"/>
<connect gate="G$1" pin="+R" pad="+R"/>
<connect gate="G$1" pin="-" pad="GND"/>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="SW" pad="SW"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-11113"/>
<attribute name="SF_SKU" value="COM-10596"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ENCODER-RGB-SWITCH" prefix="S" uservalue="yes">
<description>&lt;h3&gt;Illuminated Rotary Encoder w/ RGB LED and select switch&lt;/h3&gt;
&lt;p&gt;Encoders rotate similarly to potentiometers, but they’re different from potentiometers in that an encoder has full rotation without limits. They output gray code so that you can tell how much and in which direction the encoder has been turned.&lt;/p&gt;
&lt;p&gt;This encoder includes an RGB LED and a push-down select switch.&lt;/p&gt;
&lt;p&gt;Part #: Top Up &lt;a href="http://top-up.so-buy.com/front/bin/ptdetail.phtml?Part=EC12PLRGBSDVBF-D"&gt;EC12PLRGBSDVBF-D&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10982"&gt;Rotary Encoder - Illuminated (RGB)&lt;/a&gt; (COM-10982)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="ENCODER_LED_3_CA"/>
</gates>
<devices>
<device name="" package="ENCODER_LED_3">
<connects>
<connect gate="G$1" pin="+" pad="5"/>
<connect gate="G$1" pin="-B" pad="4"/>
<connect gate="G$1" pin="-G" pad="2"/>
<connect gate="G$1" pin="-R" pad="1"/>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="SW" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-10859"/>
<attribute name="SF_SKU" value="COM-10982"/>
</technology>
</technologies>
</device>
<device name="KIT" package="ENCODER_LED_3_KIT">
<connects>
<connect gate="G$1" pin="+" pad="5"/>
<connect gate="G$1" pin="-B" pad="4"/>
<connect gate="G$1" pin="-G" pad="2"/>
<connect gate="G$1" pin="-R" pad="1"/>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="SW" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="RES-10859"/>
<attribute name="SF_SKU" value="COM-10982"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JOYSTICK_THUMB" prefix="S">
<description>&lt;h3&gt;Analog Thumb Joystick&lt;/h3&gt;
&lt;p&gt;This is a joystick very similar to the ‘analog’ joysticks on PS2 (PlayStation 2) controllers. Directional movements are simply two potentiometers - one for each axis. Pots are ~10k each. This joystick also has a select button that is actuated when the joystick is pressed down.&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9032"&gt;Thumb Joystick&lt;/a&gt; (COM-09032)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9110"&gt;SparkFun Thumb Joystick Breakout&lt;/a&gt; (BOB-09110)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9760"&gt;SparkFun Joystick Shield Kit&lt;/a&gt; (DEV-09760)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="JOYSTICK"/>
</gates>
<devices>
<device name="" package="JOYSTICK">
<connects>
<connect gate="G$1" pin="H" pad="H2"/>
<connect gate="G$1" pin="H+" pad="H1"/>
<connect gate="G$1" pin="H-" pad="H3"/>
<connect gate="G$1" pin="SEL+" pad="B1A"/>
<connect gate="G$1" pin="SEL-" pad="B2A"/>
<connect gate="G$1" pin="V" pad="V2"/>
<connect gate="G$1" pin="V+" pad="V1"/>
<connect gate="G$1" pin="V-" pad="V3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-09744"/>
<attribute name="SF_SKU" value="COM-09032"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JOYSTICK_SLIDE" prefix="S">
<description>&lt;h3&gt;Resistive Thumb Slide Joystick&lt;/h3&gt;
&lt;p&gt;This is a resistive analog joystick, very similar to those found on the PSP1000. These compact joysticks are different in that they have a very interesting ‘slide’ feeling.&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9426"&gt;Thumb Slide Joystick&lt;/a&gt; (COM-09426)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="JOYSTICK-PSP1000"/>
</gates>
<devices>
<device name="" package="JOYSTICK-PSP1000">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
<connect gate="G$1" pin="X" pad="X"/>
<connect gate="G$1" pin="Y" pad="Y"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_SKU" value="COM-09426"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JOYSTICK_MINI" prefix="S" uservalue="yes">
<description>&lt;h3&gt;Small Tactile Joystick w/ Select Switch&lt;/h3&gt;
&lt;p&gt;A 5-way tactile switch allows for a joystick-like interface in a very small package.&lt;/p&gt;
&lt;p&gt;Part #: 4UCON SF303GJ26&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10063"&gt;5-way Tactile Switch&lt;/a&gt; (COM-10063)&lt;/li&gt;
&lt;li&gt;Used on &lt;a href="https://www.sparkfun.com/products/13035"&gt;SparkFun Block for Intel® Edison - OLED&lt;/a&gt; (DEV-13035)&lt;/li&gt;
&lt;li&gt;Used on &lt;a href="https://www.sparkfun.com/products/13262"&gt;CAN-BUS Shield&lt;/a&gt; (DEV-13262)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="JOYSTICK_MINI"/>
</gates>
<devices>
<device name="" package="JOYSTICK_MINI">
<connects>
<connect gate="G$1" pin="CENT" pad="CTR"/>
<connect gate="G$1" pin="DOWN" pad="D"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="LEFT" pad="C"/>
<connect gate="G$1" pin="RIGHT" pad="B"/>
<connect gate="G$1" pin="UP" pad="A"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-09905"/>
<attribute name="SF_SKU" value="COM-10063"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NAV_SWITCH" prefix="S">
<description>&lt;h3&gt;Navigation Switch&lt;/h3&gt;
&lt;p&gt;Three way navigation switch. Commonly used as up/down/select on MP3 players. Schematic element and footprint production proven.&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8184"&gt;Surface Mount Navigation Switch&lt;/a&gt; (COM-08184)&lt;/li&gt;
&lt;li&gt;Used on &lt;a href="https://www.sparkfun.com/products/13720"&gt;SparkFun MP3 Trigger&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="NAV_SWITCH"/>
</gates>
<devices>
<device name="" package="NAV_SWITCH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="T" pad="T"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-08301"/>
<attribute name="SF_SKU" value="COM-08184"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ENCODER-SWITCH" prefix="S">
<description>&lt;h3&gt;Rotary Encoder w/ Select Switch&lt;/h3&gt;
&lt;p&gt;Encoders rotate similarly to potentiometers, but they’re different from potentiometers in that an encoder has full rotation without limits. They output gray code so that you can tell how much and in which direction the encoder has been turned.&lt;/p&gt;
&lt;p&gt;This encoder includes a push-down select switch built into the shaft.&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9117"&gt;Rotary Encoder&lt;/a&gt; (COM-09117)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="ROT_ENCODER"/>
</gates>
<devices>
<device name="" package="ROTARY_ENC_PLAIN">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="SW+" pad="SW+"/>
<connect gate="G$1" pin="SW-" pad="SW-"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_SKU" value="COM-09117"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH-3PDT" prefix="S">
<description>&lt;h3&gt;3-Pole, Double-Throw (3PDT) Switch&lt;/h3&gt;
&lt;p&gt;Three-pole, double-throw stomp switch. Drawn as three separate gates for schematic clarity.&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;Used in &lt;a href="https://www.sparkfun.com/products/13124"&gt;SparkFun Proto Pedal&lt;/a&gt; (PRT-13124)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="A" symbol="SW_SPDT_POL"/>
<gate name="B" symbol="SW_SPDT_POL"/>
<gate name="C" symbol="SW_SPDT_POL"/>
</gates>
<devices>
<device name="-PTH-STOMP" package="STOMP_SWITCH_3PDT">
<connects>
<connect gate="A" pin="O" pad="P$1"/>
<connect gate="A" pin="P" pad="P$2"/>
<connect gate="A" pin="S" pad="P$3"/>
<connect gate="B" pin="O" pad="P$4"/>
<connect gate="B" pin="P" pad="P$5"/>
<connect gate="B" pin="S" pad="P$6"/>
<connect gate="C" pin="O" pad="P$7"/>
<connect gate="C" pin="P" pad="P$8"/>
<connect gate="C" pin="S" pad="P$9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-13197"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH-DPDT" prefix="S" uservalue="yes">
<description>&lt;h3&gt;Double-Pole, Double-Throw (DPDT) Switch&lt;/h3&gt;
&lt;p&gt;Double-pole, double-throw switches.&lt;/p&gt;
&lt;h4&gt;Variant Overview&lt;/h4&gt;
&lt;h5&gt;PTH-GPI-152-3013&lt;/h5&gt;
&lt;ul&gt;
&lt;li&gt;Used on &lt;a href="https://www.sparkfun.com/products/11345"&gt;SparkFun Geiger Counter&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;
&lt;h5&gt;SMD-AY0202&lt;/h5&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/597"&gt;Surface Mount DPDT Switch&lt;/a&gt; (COM-00597)&lt;/li&gt;
&lt;li&gt;Used on e.g. &lt;a href="https://www.sparkfun.com/products/12049"&gt;LilyPad Arduino USB - ATmega32U4 Board&lt;/a&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="SWITCH-DPDT"/>
</gates>
<devices>
<device name="-SMD-AYZ0202" package="SWITCH_DPDT_SMD_AYZ0202">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-08179"/>
<attribute name="SF_SKU" value="COM-00597"/>
</technology>
</technologies>
</device>
<device name="-PTH-GPI-152-3013" package="SWITCH_DPDT_PTH_GPI-152-3013">
<connects>
<connect gate="G$1" pin="1" pad="10"/>
<connect gate="G$1" pin="2" pad="C@1"/>
<connect gate="G$1" pin="3" pad="20"/>
<connect gate="G$1" pin="4" pad="11"/>
<connect gate="G$1" pin="5" pad="C@2"/>
<connect gate="G$1" pin="6" pad="21"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-10554"/>
</technology>
</technologies>
</device>
<device name="-SMD-JS202011JCQN" package="SWITCH_DPDT_SMD_JS202011JCQN">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="6"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-14133"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOMENTARY-SWITCH-SPST" prefix="S">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;h4&gt;Variants&lt;/h4&gt;
&lt;h5&gt;PTH-12MM - 12mm square, through-hole&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9190"&gt;Momentary Pushbutton Switch - 12mm Square&lt;/a&gt; (COM-09190)&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;PTH-6.0MM, PTH-6.0MM-KIT - 6.0mm square, through-hole&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/97"&gt;Mini Pushbutton Switch&lt;/a&gt; (COM-00097)&lt;/li&gt;
&lt;li&gt;KIT package intended for soldering kit's - only one side of pads' copper is exposed.&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;PTH-RIGHT-ANGLE-KIT - Right-angle, through-hole&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10791"&gt;Right Angle Tactile Button&lt;/a&gt; - Used on &lt;a href="https://www.sparkfun.com/products/11734"&gt;
SparkFun BigTime Watch Kit&lt;/a&gt;&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;SMD-12MM - 12mm square, surface-mount&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12993"&gt;Tactile Button - SMD (12mm)&lt;/a&gt; (COM-12993)&lt;/li&gt;
&lt;li&gt;Used on &lt;a href="https://www.sparkfun.com/products/11888"&gt;SparkFun PicoBoard&lt;/a&gt;&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;SMD-4.5MM - 4.5mm Square Trackball Switch&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;Used on &lt;a href="https://www.sparkfun.com/products/13169"&gt;SparkFun Blackberry Trackballer Breakout&lt;/a&gt;&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;SMD-4.6MMX2.8MM -  4.60mm x 2.80mm, surface mount&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;Used on &lt;a href="https://www.sparkfun.com/products/13664"&gt;SparkFun SAMD21 Mini Breakout&lt;/a&gt;&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;SMD-5.2MM, SMD-5.2-REDUNDANT - 5.2mm square, surface-mount&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8720"&gt;Mini Pushbutton Switch - SMD&lt;/a&gt; (COM-08720)&lt;/li&gt;
&lt;li&gt;Used on &lt;a href="https://www.sparkfun.com/products/11114"&gt;Arduino Pro Mini&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;REDUNDANT package connects both switch circuits together&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;SMD-6.0X3.5MM - 6.0 x 3.5mm, surface mount&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8229"&gt;Momentary Reset Switch SMD&lt;/a&gt; (COM-08229)&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;SMD-6.2MM-TALL - 6.2mm square, surface mount&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/12992"&gt;Tactile Button - SMD (6mm)&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;Used on &lt;a href="https://www.sparkfun.com/products/12651"&gt;SparkFun Digital Sandbox&lt;/a&gt;&lt;/li&gt;&lt;/ul&gt;
&lt;h5&gt;SMD-RIGHT-ANGLE - Right-angle, surface mount&lt;/h5&gt;
&lt;ul&gt;&lt;li&gt;Used on &lt;a href="https://www.sparkfun.com/products/13036"&gt;SparkFun Block for Intel® Edison - Arduino&lt;/a&gt;&lt;/li&gt;&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="SWITCH-MOMENTARY-2"/>
</gates>
<devices>
<device name="-PTH-6.0MM" package="TACTILE_SWITCH_PTH_6.0MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097"/>
</technology>
</technologies>
</device>
<device name="-SMD-4.5MM" package="TACTILE_SWITCH_SMD_4.5MM">
<connects>
<connect gate="G$1" pin="1" pad="2 3"/>
<connect gate="G$1" pin="2" pad="1 4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-09213"/>
</technology>
</technologies>
</device>
<device name="-PTH-12MM" package="TACTILE_SWITCH_PTH_12MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-09185"/>
<attribute name="SF_SKU" value="COM-09190"/>
</technology>
</technologies>
</device>
<device name="-SMD-6.0X3.5MM" package="TACTILE_SWITCH_SMD_6.0X3.5MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-14278"/>
<attribute name="SF_SKU" value="COM-08229"/>
</technology>
</technologies>
</device>
<device name="-SMD-6.2MM-TALL" package="TACTILE_SWITCH_SMD_6.2MM_TALL">
<connects>
<connect gate="G$1" pin="1" pad="A2"/>
<connect gate="G$1" pin="2" pad="B2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-11966"/>
<attribute name="SF_SKU" value="COM-12992"/>
</technology>
</technologies>
</device>
<device name="-PTH-RIGHT-ANGLE-KIT" package="TACTILE_SWITCH_PTH_RIGHT_ANGLE_KIT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10672"/>
<attribute name="SF_SKU" value="COM-10791"/>
</technology>
</technologies>
</device>
<device name="-SMD-12MM" package="TACTILE_SWITCH_SMD_12MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-11967"/>
<attribute name="SF_SKU" value="COM-12993"/>
</technology>
</technologies>
</device>
<device name="-PTH-6.0MM-KIT" package="TACTILE_SWITCH_PTH_6.0MM_KIT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097 "/>
</technology>
</technologies>
</device>
<device name="-SMD-5.2MM" package="TACTILE_SWITCH_SMD_5.2MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-08247"/>
<attribute name="SF_SKU" value="COM-08720"/>
</technology>
</technologies>
</device>
<device name="-SMD-5.2-REDUNDANT" package="TACTILE_SWITCH_SMD_5.2MM">
<connects>
<connect gate="G$1" pin="1" pad="1 2"/>
<connect gate="G$1" pin="2" pad="3 4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-08247"/>
<attribute name="SF_SKU" value="COM-08720"/>
</technology>
</technologies>
</device>
<device name="-SMD-RIGHT-ANGLE" package="TACTILE_SWITCH_SMD_RIGHT_ANGLE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-12265"/>
</technology>
</technologies>
</device>
<device name="-SMD-4.6X2.8MM" package="TACTILE_SWITCH_SMD_4.6X2.8MM">
<connects>
<connect gate="G$1" pin="1" pad="1 2"/>
<connect gate="G$1" pin="2" pad="3 4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-13065"/>
</technology>
</technologies>
</device>
<device name="-PTH-RIGHT-ANGLE" package="TACTILE_SWITCH_PTH_RIGHT_ANGLE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-10672"/>
<attribute name="SF_SKU" value="COM-10791"/>
</technology>
</technologies>
</device>
<device name="-SMD-5.2-TALL-REDUNDANT" package="TACTILE_SWITCH_SMD_5.2MM">
<connects>
<connect gate="G$1" pin="1" pad="1 2"/>
<connect gate="G$1" pin="2" pad="3 4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-14139"/>
</technology>
</technologies>
</device>
<device name="-SMD-5.2MM-TALL" package="TACTILE_SWITCH_SMD_5.2MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-14139"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOMENTARY-SWITCH-SPST-LED" prefix="S">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - w/ LED&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons), with a built-in LED.&lt;/p&gt;
&lt;h4&gt;Variants&lt;/h4&gt;
&lt;h5&gt;PTH-CHERRY - Cherry MX Switch&lt;/h5&gt;
&lt;p&gt;Cherry MX Keyswitches are top-of-the-line mechanical keyboard switches. They’re satisfyingly “clicky”, reliable up to tens-of-millions of key presses, and a standard in gaming and programming keyboards across the globe. This ‘blue’ version Cherry MX Switch is favored by most due to its secondary internal actuator making it less likely to “double-tap.” If you are looking for a noticeably audible and high-quality key switch, this is the perfect option for you!&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13834"&gt;Cherry MX Switch&lt;/a&gt; (COM-13834)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13773"&gt;Cherry MX Switch Breakout&lt;/a&gt; (BOB-13773)&lt;/li&gt;
&lt;/ul&gt;
&lt;h5&gt;PTH-12MM and PTH-12MM-KIT - 12mm Illuminated LED&lt;/h5&gt;
&lt;p&gt;KIT variant is for soldering kits. There is no tStop (covering up the top side of the pads with mask). This helps the beginner see which side they should be soldering too.&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10467"&gt;LED Tactile Button Breakout&lt;/a&gt; (BOB-10467)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10442"&gt;LED Tactile Button - Red&lt;/a&gt; (COM-10442)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10443"&gt;LED Tactile Button - Blue&lt;/a&gt; (COM-10443)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10440"&gt;LED Tactile Button - Green&lt;/a&gt; (COM-10440)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10441"&gt;LED Tactile Button - Orange&lt;/a&gt; (COM-10441)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10439"&gt;LED Tactile Button - White&lt;/a&gt; (COM-10439)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="SWITCH-MOMENTARY-LED"/>
</gates>
<devices>
<device name="-PTH-12MM" package="TACTILE_SWITCH_LED_PTH_12MM">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-11758"/>
<attribute name="SF_SKU" value="COM-10442"/>
</technology>
</technologies>
</device>
<device name="-PTH-12MM-KIT" package="TACTILE_SWITCH_LED_PTH_12MM_KIT">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-11758"/>
<attribute name="SF_SKU" value="COM-10442"/>
</technology>
</technologies>
</device>
<device name="-PTH-CHERRY" package="CHERRY-MX-LED">
<connects>
<connect gate="G$1" pin="1" pad="S1"/>
<connect gate="G$1" pin="2" pad="S2"/>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="COM-13834"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH-SP3T" prefix="S" uservalue="yes">
<description>&lt;h3&gt;Single-Pole, Triple-Throw (SP3T) Switch&lt;/h3&gt;
&lt;p&gt;Single-Pole, Triple-Throw switches&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;em&gt;Prototype Part&lt;/em&gt;&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="SWITCH-SP3T"/>
</gates>
<devices>
<device name="-SMD" package="SWITCH_SP3T_SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-10805"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH-SPDT" prefix="S" uservalue="yes">
<description>&lt;h3&gt;Single Pole, Double Throw (SPDT) Switch&lt;/h3&gt;
&lt;p&gt;Single-pole, double-throw (SPDT) switch.&lt;/p&gt;
&lt;h4&gt;Variant Overview&lt;/h4&gt;
&lt;h5&gt;SMD-AYZ0202&lt;/h5&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/597"&gt;Surface Mount DPDT Switch&lt;/a&gt; (COM-00597)&lt;/li&gt;
&lt;li&gt;Used on e.g. &lt;a href="https://www.sparkfun.com/products/12049"&gt;LilyPad Arduino USB - ATmega32U4 Board&lt;/a&gt;
&lt;/ul&gt;
&lt;h5&gt;PTH-11.6X4.0MM&lt;/h5&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/102"&gt;SPDT Mini Power Switch&lt;/a&gt; (COM-00102)&lt;/li&gt;
&lt;li&gt;Used on e.g. &lt;a href="https://www.sparkfun.com/products/10547"&gt;SparkFun Simon Says - Through-Hole Soldering Kit&lt;/a&gt; (KIT-10547)&lt;/li&gt;
&lt;/ul&gt;
&lt;h5&gt;PTH-11.6X4.0MM-KIT&lt;/h5&gt;
&lt;ul&gt;
&lt;li&gt;KIT version of SPDT Mini Power Switch - Simplifies soldering by removing tStop of switch pins - only one side can be soldered.&lt;/li&gt;
&lt;/ul&gt;
&lt;h5&gt;PTH-11.6X4.0MM-LOCK&lt;/h5&gt;
&lt;ul&gt;
&lt;li&gt;LOCK version of SPDT Mini Power Switch - Offset pins hold switch in place for easier soldering.&lt;/li&gt;
&lt;/ul&gt;
&lt;h5&gt;SMD-RIGHT-ANGLE&lt;/h5&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10860"&gt;Surface Mount Right Angle Switch&lt;/a&gt; (COM-10860)&lt;/li&gt;
&lt;li&gt;Used on e.g. &lt;a href="https://www.sparkfun.com/products/13231"&gt;SparkFun ESP8266 Thing&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="1" symbol="TOGGLE"/>
</gates>
<devices>
<device name="-PTH-11.6X4.0MM" package="SWITCH_SPDT_PTH_11.6X4.0MM">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-08261"/>
<attribute name="SF_SKU" value="COM-00102"/>
</technology>
</technologies>
</device>
<device name="-SMD-AYZ0202" package="SWITCH_DPDT_SMD_AYZ0202">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-08179"/>
<attribute name="SF_ID" value="COM-00597"/>
</technology>
</technologies>
</device>
<device name="-PTH-11.6X4.0MM-LOCK" package="SWITCH_SPDT_PTH_11.6X4.0MM_LOCK">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-08261"/>
<attribute name="SF_SKU" value="COM-00102 "/>
</technology>
</technologies>
</device>
<device name="-PTH-11.6X4.0MM-KIT" package="SWITCH_SPDT_PTH_11.6X4.0MM_KIT">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-08261"/>
<attribute name="SF_SKU" value="COM-00102"/>
</technology>
</technologies>
</device>
<device name="-SMD-RIGHT-ANGLE" package="SWITCH_SPST_SMD_A">
<connects>
<connect gate="1" pin="O" pad="1"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-10651"/>
<attribute name="SF_SKU" value="COM-10860"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH_ROTARY_1X10" prefix="S">
<description>&lt;h3&gt;10-Position Rotary Switch&lt;/h3&gt;
&lt;p&gt;Single pole, 10 position rotary switch able to select up to 10 different states.&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13253"&gt;Rotary Switch - 10 Position&lt;/a&gt; (COM-13253)&lt;/li&gt;
&lt;li&gt;Used on &lt;a href="https://www.sparkfun.com/products/13006"&gt;SparkFun Decade Resistance Box&lt;/a&gt;&lt;/li&gt;</description>
<gates>
<gate name="G$1" symbol="ROTARY-SWITCH-1X10"/>
</gates>
<devices>
<device name="-PTH" package="ROTARY_SWITCH_1X10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="COMMON" pad="COMMON"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-12120"/>
<attribute name="SF_SKU" value="COM-13253"/>
</technology>
</technologies>
</device>
<device name="-PTH-KIT" package="ROTARY_SWITCH_1X10_KIT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="COMMON" pad="COMMON"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-12120"/>
<attribute name="SF_SKU" value="COM-13253"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOMENTARY-SWITCH-SPST-2" prefix="S" uservalue="yes">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - Two Circuits&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons). Schematic symbol includes two switch circuits.&lt;/p&gt;
&lt;h4&gt;Variants&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;b&gt;SMD-4.6MMX2.8MM&lt;/b&gt; -  4.60mm x 2.80mm Tactile Momentary Button Switch  - Used on &lt;a href="https://www.sparkfun.com/products/13664"&gt;SparkFun SAMD21 Mini Breakout&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;b&gt;SMD-5.2MM&lt;/b&gt; - &lt;a href="https://www.sparkfun.com/products/8720"&gt;Mini Pushbutton Switch - SMD&lt;/a&gt; - Used on &lt;a href="https://www.sparkfun.com/products/11114"&gt;Arduino Pro Mini&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="SWITCH-MOMENTARY"/>
</gates>
<devices>
<device name="-SMD-5.2MM" package="TACTILE_SWITCH_SMD_5.2MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-08247"/>
<attribute name="SF_SKU" value="COM-08720"/>
</technology>
</technologies>
</device>
<device name="-SMD-4.6X2.8MM" package="TACTILE_SWITCH_SMD_4.6X2.8MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-13065"/>
</technology>
</technologies>
</device>
<device name="-SMD-5.2MM-TALL" package="TACTILE_SWITCH_SMD_5.2MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-14139"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIP-08" prefix="S" uservalue="yes">
<description>&lt;h3&gt;8-Position DIP Switch&lt;/h3&gt;
&lt;p&gt;8-circuit DIP (dual inline package) switch. Commonly used to physcially set a circuit's behavior.&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8034"&gt;DIP Switch - 8 Position&lt;/a&gt; (COM-08034)&lt;/li&gt;&lt;/ul&gt;</description>
<gates>
<gate name="A" symbol="SW_DIP-8"/>
</gates>
<devices>
<device name="-PTH" package="DIPSWITCH-08">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-12197"/>
<attribute name="SF_SKU" value="COM-08034"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRACKBALL" prefix="S">
<description>&lt;h3&gt;Trackball - Mechanical&lt;/h3&gt;
&lt;p&gt;This is a tiny trackball akin to those found on a number of Blackberry models (8100, 8300, 8320, 8800, 8830, etc). Each of the four spindles have a tiny circular magnet on each end. Great when paired with very small SMD Hall effect sensors.&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9308"&gt;Blackberry Trackball&lt;/a&gt; (COM-09308)&lt;/li&gt;
&lt;li&gt;Used on &lt;a href="https://www.sparkfun.com/products/13169"&gt;SparkFun Blackberry Trackballer Breakout&lt;/a&gt;&lt;/li&gt;</description>
<gates>
<gate name="G$1" symbol="TRACKBALL"/>
</gates>
<devices>
<device name="MECH" package="TRACKBALL">
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-09237"/>
<attribute name="SF_SKU" value="COM-09308"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="REED_SWITCH" prefix="S">
<description>&lt;h3&gt;Reed Switch&lt;/h3&gt;
&lt;p&gt;A reed switch is a magnetically-actuated switch. When the device is exposed to a magnetic field, the two ferrous materials inside the switch pull together and the switch closes.&lt;/p&gt;
&lt;h4&gt;Variant Overview&lt;/h4&gt;
&lt;h5&gt;PTH-GLASS&lt;/h5&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8642"&gt;Reed Switch&lt;/a&gt; (COM-08642) - PTH reed switch w/ glass body (6.0 x 0.9 mm)&lt;/li&gt;
&lt;/ul&gt;
&lt;h5&gt;PTH-INSULATED&lt;/h5&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10601"&gt;Reed Switch - Insulated&lt;/a&gt; (COM-10601) - PTH reed switch w/ insulated body (15.1 x 4.2 mm)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="REED_SWITCH"/>
</gates>
<devices>
<device name="-PTH-GLASS" package="REED_SWITCH_GLASS">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-09282"/>
<attribute name="SF_SKU" value="COM-08642"/>
</technology>
</technologies>
</device>
<device name="-PTH-INSULATED" package="REED_SWITCH_PLASTIC">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-10467"/>
<attribute name="SF_SKU" value="COM-10601"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIP-06" prefix="SW">
<gates>
<gate name="G$1" symbol="DIPSWITCH-06"/>
</gates>
<devices>
<device name="" package="DIPSWITCH-06-SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="SWCH-13756"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
