<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<library>
<description>&lt;b&gt;DIY Modules for Arduino, Raspberry Pi, CubieBoard etc.&lt;/b&gt;
&lt;br&gt;&lt;br&gt;
The library contains a list of symbols and footprints for popular, cheap and easy-to-use electronic modules.&lt;br&gt;
The modules are intend to work with microprocessor-based platforms such as &lt;a href="http://arduino.cc"&gt;Arduino&lt;/a&gt;, &lt;a href="http://raspberrypi.org/"&gt;Raspberry Pi&lt;/a&gt;, &lt;a href="http://cubieboard.org/"&gt;CubieBoard&lt;/a&gt;, &lt;a href="http://beagleboard.org/"&gt;BeagleBone&lt;/a&gt; and many others. There are many manufacturers of the modules in the world. Almost all of them can be bought on &lt;a href="ebay.com"&gt;ebay.com&lt;/a&gt;.&lt;br&gt;
&lt;br&gt;
By using this library, you can design a PCB for devices created with usage of modules. Even if you do not need to create PCB design, you can also use the library to quickly document your work by drawing schematics of devices built by you.&lt;br&gt;
&lt;br&gt;
The latest version, examples, photos and much more can be found at: &lt;b&gt;&lt;a href="http://diymodules.org/eagle"&gt;diymodules.org/eagle&lt;/a&gt;&lt;/b&gt;&lt;br&gt;&lt;br&gt;
Comments, suggestions and bug reports please send to: &lt;b&gt;&lt;a href="mailto:eagle@diymodules.org"&gt;eagle@diymodules.org&lt;/b&gt;&lt;/a&gt;&lt;br&gt;&lt;br&gt;
&lt;i&gt;Version: 1.8.0 (2017-Jul-02)&lt;/i&gt;&lt;br&gt;
&lt;i&gt;Created by: Miroslaw Brudnowski&lt;/i&gt;&lt;br&gt;&lt;br&gt;
&lt;i&gt;Released under the Creative Commons Attribution 4.0 International License: &lt;a href="http://creativecommons.org/licenses/by/4.0"&gt;http://creativecommons.org/licenses/by/4.0&lt;/a&gt;&lt;/i&gt;
&lt;br&gt;&lt;br&gt;
&lt;center&gt;
&lt;a href="http://diymodules.org/eagle"&gt;&lt;img src="http://www.diymodules.org/img/diymodules-lbr-image.php?v=1.8.0" alt="DIYmodules.org"&gt;&lt;/a&gt;
&lt;/center&gt;</description>
<packages>
<package name="ARDUINO-PRO-MINI">
<description>&lt;b&gt;Arduino Pro Mini&lt;/b&gt;</description>
</package>
<package name="ARDUINO-PRO-MINI#APC">
<description>&lt;b&gt;Arduino Pro Mini&lt;/b&gt;&lt;br&gt;
Footprint with angle programming connector</description>
</package>
<package name="WIRELESS-NRF24L01">
<description>&lt;b&gt;2.4 GHz Wireless Module&lt;/b&gt; based on &lt;b&gt;NRF24L01&lt;/b&gt; chip</description>
</package>
<package name="ARDUINO-PRO-MINI#NP">
<description>&lt;b&gt;Arduino Pro Mini&lt;/b&gt;&lt;br&gt;
Footprint without programming pads</description>
</package>
<package name="ARDUINO-PRO-MINI#SMP">
<description>&lt;b&gt;Arduino Pro Mini&lt;/b&gt;&lt;br&gt;
Footprint with 2 connectors only</description>
</package>
<package name="WIRELESS-XY-MK-5V">
<description>&lt;b&gt;RF Wireless XY-MK-5V Receiver&lt;/b&gt;</description>
</package>
<package name="WIRELESS-XY-FST">
<description>&lt;b&gt;RF Wireless XY-FST Transmitter&lt;/b&gt;</description>
</package>
<package name="WIRELESS-XY-MK-5V#V">
<description>&lt;b&gt;RF Wireless XY-MK-5V Receiver&lt;/b&gt; vertically mounted</description>
</package>
<package name="WIRELESS-XY-FST#V">
<description>&lt;b&gt;RF Wireless XY-FST Transmitter&lt;/b&gt; vertically mounted</description>
</package>
<package name="ARDUINO-NANO-3.0#ISP">
<description>&lt;b&gt;Arduino Nano 3.0&lt;/b&gt;&lt;br&gt;
Footprint with ISP pads</description>
</package>
<package name="ARDUINO-NANO-3.0">
<description>&lt;b&gt;Arduino Nano 3.0&lt;/b&gt;</description>
</package>
<package name="ETHERNET-ENC28J60">
<description>&lt;b&gt;Ethernet Module&lt;/b&gt; based on &lt;b&gt;ENC28J60&lt;/b&gt; chip</description>
</package>
<package name="BATTERY-HOLDER-2AA">
<description>&lt;b&gt;2 x AA Battery Holder&lt;/b&gt;</description>
</package>
<package name="BATTERY-HOLDER-2AAA">
<description>&lt;b&gt;2 x AAA Battery Holder&lt;/b&gt;</description>
</package>
<package name="DISPLAY-NOKIA-3310">
<description>&lt;b&gt;84x48 Dot Matrix LCD Module&lt;/b&gt; based on &lt;b&gt;Nokia 3310&lt;/b&gt; display</description>
</package>
<package name="DC-DC-STEP-UP-5V-USB">
<description>&lt;b&gt;DC/DC Step-Up Converter&lt;/b&gt; with &lt;b&gt;USB-A&lt;/b&gt; connector</description>
</package>
<package name="ULTRASONIC-HC-SR04">
<description>&lt;b&gt;Ultrasonic Ranging Module HC-SR04&lt;/b&gt;</description>
</package>
<package name="ULTRASONIC-HC-SR04#V">
<description>&lt;b&gt;Ultrasonic Ranging Module HC-SR04&lt;/b&gt; vertically mounted</description>
</package>
<package name="MOTION-PIR-DYP-ME003">
<description>&lt;b&gt;PIR Motion Sensor Module DYP-ME003&lt;/b&gt; based on &lt;b&gt;BISS0001&lt;/b&gt; pyroelectic detector</description>
</package>
<package name="REG-AMS1117">
<description>&lt;b&gt;Linear Regulator&lt;/b&gt; based on &lt;b&gt;AMS1117&lt;/b&gt; chip</description>
</package>
<package name="ADC-DAC-PCF8591">
<description>&lt;b&gt;4-Channel ADC and 1-Channel DAC Module&lt;/b&gt; based on &lt;b&gt;PCF8591&lt;/b&gt; chip</description>
</package>
<package name="DRIVER-ULN2003">
<description>&lt;b&gt;7-Channel Darlington NPN Transistor Module&lt;/b&gt; based on &lt;b&gt;ULN2003&lt;/b&gt; chip&lt;br&gt;</description>
</package>
<package name="DRIVER-ULN2003#MC">
<description>&lt;b&gt;7-Channel Darlington NPN Transistor Module&lt;/b&gt; based on &lt;b&gt;ULN2003&lt;/b&gt; chip&lt;br&gt;
Footprint with motor connector</description>
</package>
<package name="SOUND-DETECTOR">
<description>&lt;b&gt;Sound Detection Module&lt;/b&gt;</description>
</package>
<package name="SOUND-BUZZER">
<description>&lt;b&gt;Sound Buzzer Module&lt;/b&gt;</description>
</package>
<package name="CURRENT-SENSOR-ACS712#IC">
<description>&lt;b&gt;Isolated Bipolar Current Sensors&lt;/b&gt; based on &lt;b&gt;ACS712&lt;/b&gt; chip&lt;br&gt;
Footprint with input connector</description>
</package>
<package name="CURRENT-SENSOR-ACS712">
<description>&lt;b&gt;Isolated Bipolar Current Sensors&lt;/b&gt; based on &lt;b&gt;ACS712&lt;/b&gt; chip</description>
</package>
<package name="SOIL-MOISTURE-SENSOR">
<description>&lt;b&gt;Soil Moisture Sensor&lt;/b&gt;</description>
</package>
<package name="RELAY-2-SRD#RC">
<description>&lt;b&gt;2-Channel Relay Module&lt;/b&gt; based on &lt;b&gt;SRD-05VDC-SL-C&lt;/b&gt; relays&lt;br /&gt;
Footprint with relays connector</description>
</package>
<package name="COMPASS-HMC5883L">
<description>&lt;b&gt;3-Axis Digital Compass Module&lt;/b&gt; based on &lt;b&gt;HMC5883L&lt;/b&gt; chip</description>
</package>
<package name="WIRELESS-WIFI-ESP-01">
<description>&lt;b&gt;Wireless Wi-Fi ESP-01 Module&lt;/b&gt; based on &lt;b&gt;ESP8266&lt;/b&gt; chip</description>
</package>
<package name="DC-DC-STEP-DOWN-LM2596">
<description>&lt;b&gt;DC/DC Step-Down Regulator&lt;/b&gt; based on &lt;b&gt;LM2596-ADJ&lt;/b&gt; chip</description>
</package>
<package name="CARD-SD-ADAPTER">
<description>&lt;b&gt;Full Size SD Card Adapter Module&lt;/b&gt; with onboard 3.3V regulator</description>
</package>
<package name="LCD-I2C-CONVERTER">
<description>&lt;b&gt;I2C Bus to 4-Bit Parallel LCD Interface&lt;/b&gt; with LED backlight driver</description>
</package>
<package name="RTC-EEPROM-BATTERY">
<description>&lt;b&gt;RTC Module with Battery and EEPROM&lt;/b&gt; based on &lt;b&gt;DS1307&lt;/b&gt; and &lt;b&gt;AT24C32&lt;/b&gt; chips</description>
</package>
<package name="AMPLIFIER-PAM8403">
<description>&lt;b&gt;Stereo Class-D 3W Audio Amplifier&lt;/b&gt; based on &lt;b&gt;PAM8403&lt;/b&gt; chip</description>
</package>
<package name="BREADBOARD-POWER-V1">
<description>&lt;b&gt;Breadboard Power Adapter&lt;/b&gt; with onboard 3.3V and 5V regulators</description>
</package>
<package name="RELAY-2-SRD">
<description>&lt;b&gt;2-Channel Relay Module&lt;/b&gt; based on &lt;b&gt;SRD-05VDC-SL-C&lt;/b&gt; relays</description>
</package>
<package name="DC-DC-STEP-UP-5V">
<description>&lt;b&gt;DC/DC Step-Up Converter&lt;/b&gt;</description>
</package>
<package name="WIRELESS-NRF24L01-PA-EXT">
<description>&lt;b&gt;2.4 GHz Wireless Module&lt;/b&gt; based on &lt;b&gt;NRF24L01&lt;/b&gt; chip with preamplifier and external antenna</description>
</package>
<package name="AC-DC-3.5W">
<description>&lt;b&gt;AC/DC 3.5W Converter&lt;/b&gt;</description>
</package>
<package name="BATTERY-CHARGER-LI-5V">
<description>&lt;b&gt;Lithium Battery 5V Charger&lt;/b&gt;</description>
</package>
<package name="FLAME-DETECTOR">
<description>&lt;b&gt;Flame Detector&lt;/b&gt;</description>
</package>
<package name="IR-RECEIVER">
<description>&lt;b&gt;IR Receiver Module&lt;/b&gt;</description>
</package>
<package name="IR-RECEIVER#NC">
<description>&lt;b&gt;IR Receiver Module&lt;/b&gt;&lt;br&gt;
Symbol wihtout IR sensor connector</description>
</package>
<package name="STEPPER-MOTOR-EASY-DRIVER">
<description>&lt;b&gt;Stepper Motor Easy Driver&lt;/b&gt;</description>
</package>
<package name="RS485-TTL-CONVERTER">
<description>&lt;b&gt;RS485 to TTL converter&lt;/b&gt; based on &lt;b&gt;MAX485&lt;/b&gt; chip</description>
</package>
<package name="TOUCH-KEYPAD-4X4">
<description>&lt;b&gt;16 Channel Capacitive Touch Keypad&lt;/b&gt;</description>
</package>
<package name="LIGHT-DETECTOR">
<description>&lt;b&gt;Light Detection Module&lt;/b&gt;</description>
</package>
<package name="GSM-MODEM-SIM900A">
<description>&lt;b&gt;GSM Mini Module&lt;/b&gt; based on &lt;b&gt;SIM900A&lt;/b&gt;</description>
</package>
<package name="LED-24XRGB-RING">
<description>&lt;b&gt;24 LEDs RGB Ring&lt;/b&gt; based on &lt;b&gt;WS2812B&lt;/b&gt;</description>
</package>
<package name="N-MOSFET-SWITCH">
<description>&lt;b&gt;Low Side N-MOSFET Switch&lt;/b&gt; with &lt;b&gt;Optocoupler&lt;/b&gt;</description>
</package>
<package name="N-MOSFET-SWITCH#IC">
<description>&lt;b&gt;Low Side N-MOSFET Switch&lt;/b&gt; with &lt;b&gt;Optocoupler&lt;/b&gt;&lt;br /&gt;
Package with connector pins</description>
</package>
<package name="BREADBOARD-POWER-V2">
<description>&lt;b&gt;Breadboard Power Adapter&lt;/b&gt; with onboard 3.3V and 5V regulators</description>
</package>
<package name="SPARKFUN-AD-MUX-16X1">
<description>&lt;b&gt;SparkFun Analog/Digital MUX Breakout&lt;/b&gt; based on &lt;b&gt;CD74HC4067&lt;/b&gt; chip</description>
</package>
<package name="RELAY-1-SRD">
<description>&lt;b&gt;1-Channel Relay Module&lt;/b&gt; based on &lt;b&gt;SRD-05VDC-SL-C&lt;/b&gt; relay</description>
</package>
<package name="RELAY-4-SRD">
<description>&lt;b&gt;4-Channel Relay Module&lt;/b&gt; based on &lt;b&gt;SRD-05VDC-SL-C&lt;/b&gt; relays</description>
</package>
<package name="RELAY-8-SRD">
<description>&lt;b&gt;8-Channel Relay Module&lt;/b&gt; based on &lt;b&gt;SRD-05VDC-SL-C&lt;/b&gt; relays</description>
</package>
<package name="RELAY-1-SRD#RC">
<description>&lt;b&gt;1-Channel Relay Module&lt;/b&gt; based on &lt;b&gt;SRD-05VDC-SL-C&lt;/b&gt; relay&lt;br&gt;
Footprint with relays connector</description>
</package>
<package name="RELAY-4-SRD#RC">
<description>&lt;b&gt;4-Channel Relay Module&lt;/b&gt; based on &lt;b&gt;SRD-05VDC-SL-C&lt;/b&gt; relays&lt;br /&gt;
Footprint with relays connector</description>
</package>
<package name="RELAY-8-SRD#RC">
<description>&lt;b&gt;8-Channel Relay Module&lt;/b&gt; based on &lt;b&gt;SRD-05VDC-SL-C&lt;/b&gt; relays&lt;br /&gt;
Footprint with relays connector</description>
</package>
<package name="DC-DC-LM2596-DISP">
<description>&lt;b&gt;DC/DC Step-Down Regulator&lt;/b&gt; with &lt;b&gt;Voltage Display&lt;/b&gt; based on &lt;b&gt;LM2596-ADJ&lt;/b&gt; chip</description>
</package>
<package name="DC-DC-LM2596-DISP#RC">
<description>&lt;b&gt;DC/DC Step-Down Regulator&lt;/b&gt; with &lt;b&gt;Voltage Display&lt;/b&gt; based on &lt;b&gt;LM2596-ADJ&lt;/b&gt; chip&lt;br /&gt;
Footprint with connector pins.</description>
</package>
<package name="TOUCH-KEYPAD-4X2">
<description>&lt;b&gt;8 Channel Capacitive Touch Keypad&lt;/b&gt;</description>
</package>
<package name="TOUCH-KEYPAD-4X1">
<description>&lt;b&gt;4 Channel Capacitive Touch Keypad&lt;/b&gt;</description>
</package>
<package name="BATTERY-CHARGER-LI-PROT">
<description>&lt;b&gt;Protected Lithium Battery 5V Charger&lt;/b&gt; with micro-USB connector</description>
</package>
<package name="DFPLAYER-MINI-MODULE">
<description>&lt;b&gt;DFPlayer Mini&lt;/b&gt; - MP3 player module based on &lt;b&gt;YX5200&lt;/b&gt; chip</description>
</package>
<package name="DISPLAY-OLED-128X64">
<description>&lt;b&gt;128x64 Dot Matrix OLED Module&lt;/b&gt;&lt;br /&gt;
Variant with SPI interface</description>
</package>
<package name="LED-8XRGB-LINE">
<description>&lt;b&gt;8 LEDs RGB Line Display&lt;/b&gt; based on &lt;b&gt;WS2812B&lt;/b&gt;</description>
</package>
<package name="LED-15XRGB-QRING">
<description>&lt;b&gt;15 LEDs RGB Quarter-Ring&lt;/b&gt; based on &lt;b&gt;WS2812B&lt;/b&gt;</description>
</package>
<package name="WIRELESS-BLUETOOTH-XS3868">
<description>&lt;b&gt;Bluetooth Stereo Audio Module&lt;/b&gt; based on &lt;b&gt;OVC3860&lt;/b&gt; chip</description>
</package>
<package name="BATTERY-LI-MH12210">
<description>&lt;b&gt;Lithium-Ion MH12210 Rechargeable Battery&lt;/b&gt;</description>
</package>
<package name="TEMP-HUM-SENSOR-DHT11">
<description>&lt;b&gt;DHT11 - digital humidity &amp; temperature sensor&lt;/b&gt;</description>
</package>
<package name="TEMP-HUM-SENSOR-DHT22">
<description>&lt;b&gt;DHT22 - digital humidity &amp; temperature sensor&lt;/b&gt;</description>
</package>
<package name="DISPLAY-OLED-128X32">
<description>&lt;b&gt;128x32 Dot Matrix OLED Module&lt;/b&gt; with &lt;b&gt;I2C&lt;/b&gt; interface</description>
</package>
<package name="DC-DC-STEP-DOWN-MP2307">
<description>&lt;b&gt;DC/DC Step-Down Regulator&lt;/b&gt; based on &lt;b&gt;MP2307DN&lt;/b&gt; chip</description>
</package>
<package name="RADIO-RECEIVER-DCF77">
<description>&lt;b&gt;DCF-77 Longwave Radio Time Signal Receiver&lt;/b&gt; based on &lt;b&gt;MAS6180B1&lt;/b&gt; chip</description>
</package>
<package name="THERMOCOUPLE-MAX31855">
<description>&lt;b&gt;Thermocouple Analog-to-Digital Converter&lt;/b&gt; based on &lt;b&gt;MAX31855&lt;/b&gt; chip</description>
</package>
<package name="THERMOCOUPLE-MAX31855#IC">
<description>&lt;b&gt;Thermocouple Analog-to-Digital Converter&lt;/b&gt; based on &lt;b&gt;MAX31855&lt;/b&gt; chip&lt;br /&gt;
Footprint with thermocouple connector pins</description>
</package>
<package name="LEVEL-SHIFTER-4CH">
<description>&lt;b&gt;4-Channel Bi-Directional  Logic Level Converter&lt;/b&gt; based on &lt;b&gt;BSS128&lt;/b&gt; transistors</description>
</package>
<package name="RTC-DS3231-AT24C32">
<description>&lt;b&gt;RTC Module with Battery and EEPROM&lt;/b&gt; based on &lt;b&gt;DS3231&lt;/b&gt; and &lt;b&gt;AT24C32&lt;/b&gt; chips</description>
</package>
<package name="WIRELESS-LORA-RFM95W#THT">
<description>&lt;b&gt;868/915 MHz LoRa Radio Transceiver Module&lt;/b&gt;&lt;br /&gt;
Footprint for THT assembly.</description>
</package>
<package name="WIRELESS-LORA-RFM95W#SMD">
<description>&lt;b&gt;868/915 MHz LoRa Radio Transceiver Module&lt;/b&gt;&lt;br /&gt;
Footprint for SMD assembly.</description>
</package>
<package name="TEMP-HUM-PRES-BME280">
<description>&lt;b&gt;Digital Humidity-Temperature-Pressure Sensor&lt;/b&gt; based on &lt;b&gt;BME280&lt;/b&gt; device</description>
</package>
<package name="TEMP-HUM-SENSOR-HTU21D">
<description>&lt;b&gt;Digital Humidity &amp; Temperature Sensor&lt;/b&gt; based on &lt;b&gt;HTU21D&lt;/b&gt; device</description>
</package>
<package name="USB-SERIAL-FT232R">
<description>&lt;b&gt;USB to Serial UART Converter&lt;/b&gt; based on &lt;b&gt;FT232R&lt;/b&gt; chip</description>
</package>
<package name="DATA-LOGGER-MINI">
<description>&lt;b&gt;Mini Data Logger&lt;/b&gt; with &lt;b&gt;microSD card&lt;/b&gt; and  battery powered &lt;b&gt;RTC&lt;/b&gt; based on &lt;b&gt;DS1307&lt;/b&gt; chip</description>
</package>
<package name="GAS-SENSOR-MQ2">
<description>&lt;b&gt;Gas Sensor&lt;/b&gt; based on &lt;b&gt;MQ-2&lt;/b&gt; device</description>
</package>
<package name="UV-SENSOR-ML8511">
<description>&lt;b&gt;UV  Sensor&lt;/b&gt; based on &lt;b&gt;ML8511&lt;/b&gt; device</description>
</package>
<package name="ADC-4CH-ADS1115">
<description>&lt;b&gt;4 Channel 16-Bit Analog-to-Digital Converter&lt;/b&gt; based on &lt;b&gt;ADS1115&lt;/b&gt; chip</description>
</package>
<package name="WIRELESS-BLUETOOTH-BK8000">
<description>&lt;b&gt;Bluetooth Audio Module&lt;/b&gt; based on &lt;b&gt;BK8000L&lt;/b&gt; chip</description>
</package>
<package name="GPS-RECEIVER-NEO6M">
<description>&lt;b&gt;GPS Receiver Module&lt;/b&gt; based on &lt;b&gt;NEO-6&lt;/b&gt; device</description>
</package>
<package name="STEPPER-MOTOR-DRIVER-L6470">
<description>&lt;b&gt;Stepper Motor Driver&lt;/b&gt; based on &lt;b&gt;L6470&lt;/b&gt; chip</description>
</package>
<package name="LEVEL-SHIFTER-8CH">
<description>&lt;b&gt;8-Channel Bi-Directional  Logic Level Converter&lt;/b&gt; based on &lt;b&gt;BSS128&lt;/b&gt; transistors</description>
</package>
<package name="LIGHT-SENSOR-BH1750">
<description>&lt;b&gt;Digital Light Sensor&lt;/b&gt; based on &lt;b&gt;BH1750&lt;/b&gt;</description>
</package>
<package name="PWM-SERVO-DRIVER-16CH">
<description>&lt;b&gt;16-Channel 12-bit PWM/Servo Driver&lt;/b&gt; based on &lt;b&gt;PCA9685&lt;/b&gt; chip</description>
</package>
<package name="RANGING-SENSOR-VL53L0X">
<description>&lt;b&gt;Laser Ranging Sensor&lt;/b&gt; based on &lt;b&gt;VL53L0X&lt;/b&gt; device</description>
</package>
<package name="WEMOS-D1-MINI-PRO">
<description>&lt;b&gt;WEMOS D1 mini Pro&lt;/b&gt;: Mini Wi-Fi Board based on &lt;b&gt;ESP-8266EX&lt;/b&gt; chip</description>
</package>
<package name="WEMOS-D1-MINI-SHIELD">
<description>Template package for &lt;b&gt;WEMOS D1 mini&lt;/b&gt; shields</description>
</package>
<package name="WEMOS-D1-MINI">
<description>&lt;b&gt;WEMOS D1 mini&lt;/b&gt;: Mini Wi-Fi Board based on &lt;b&gt;ESP-8266&lt;/b&gt; device</description>
</package>
<package name="DC-DC-STEP-UP-MT3608">
<description>&lt;b&gt;DC/DC Step-Up Regulator&lt;/b&gt; based on &lt;b&gt;MT3608&lt;/b&gt; chip</description>
</package>
<package name="USB-SERIAL-CP2102">
<description>&lt;b&gt;USB to Serial UART Converter&lt;/b&gt; based on &lt;b&gt;CP2102&lt;/b&gt; chip</description>
</package>
<package name="TEMP-HUM-SENSOR-AM2322">
<description>&lt;b&gt;AM2322 - digital humidity &amp; temperature sensor&lt;/b&gt;</description>
</package>
<package name="DISPLAY-OLED-128X64-I2C">
<description>&lt;b&gt;128x64 Dot Matrix OLED Module&lt;/b&gt;&lt;br /&gt;
Variant with I2C interface</description>
</package>
<package name="REG-AMS1117-3P">
<description>&lt;b&gt;Linear Regulator&lt;/b&gt; based on &lt;b&gt;AMS1117&lt;/b&gt; chip&lt;br /&gt;
3-pin version</description>
</package>
<package name="REG-AMS1117-3P#V">
<description>&lt;b&gt;Linear Regulator&lt;/b&gt; based on &lt;b&gt;AMS1117&lt;/b&gt; chip&lt;br /&gt;
3-pin version, vertically mounted</description>
</package>
<package name="AC-VOLTAGE-SENSOR">
<description>&lt;b&gt;Isolated AC Voltage Sensor&lt;/b&gt; based on &lt;b&gt;ZMPT101B&lt;/b&gt; transformer</description>
</package>
<package name="AC-VOLTAGE-SENSOR#IC">
<description>&lt;b&gt;Isolated AC Voltage Sensor&lt;/b&gt; based on &lt;b&gt;ZMPT101B&lt;/b&gt; transformer&lt;br /&gt;
Footprint with input connector</description>
</package>
<package name="WIRELESS-BLUETOOTH-HC-05">
<description>&lt;b&gt;Bluetooth Transceiver Module&lt;/b&gt; based on &lt;b&gt;HC-05&lt;/b&gt; board</description>
</package>
<package name="JOYSTICK-2AXIS-BUTTON">
<description>&lt;b&gt;2-Axis Analog Joystick&lt;/b&gt; with Push Button</description>
</package>
<package name="DC-DC-STEP-DOWN-MP1584">
<description>&lt;b&gt;DC/DC Step-Down Regulator&lt;/b&gt; based on &lt;b&gt;MP1584&lt;/b&gt; chip</description>
</package>
</packages>
<symbols>
<symbol name="ARDUINO-NANO-3.0#ISP">
<description>&lt;b&gt;Arduino Nano 3.0&lt;/b&gt; with ISP pads</description>
<pin name="D1/TX"/>
<pin name="D0/RX"/>
<pin name="RST.1"/>
<pin name="GND.1" direction="pwr"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11/MOSI"/>
<pin name="D12/MISO"/>
<pin name="VIN" direction="pwr"/>
<pin name="GND.2" direction="pwr"/>
<pin name="RST.2"/>
<pin name="5V" direction="pwr"/>
<pin name="A7"/>
<pin name="A6"/>
<pin name="A5"/>
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="AREF"/>
<pin name="3V3" direction="pwr"/>
<pin name="D13/SCK"/>
<pin name="ISP_MISO"/>
<pin name="ISP_5V"/>
<pin name="ISP_SCK"/>
<pin name="ISP_MOSI"/>
<pin name="ISP_RST"/>
<pin name="ISP_GND"/>
</symbol>
<symbol name="ARDUINO-NANO-3.0">
<description>&lt;b&gt;Arduino Nano 3.0&lt;/b&gt;</description>
<pin name="D1/TX"/>
<pin name="D0/RX"/>
<pin name="RST.1"/>
<pin name="GND.1" direction="pwr"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11/MOSI"/>
<pin name="D12/MISO"/>
<pin name="VIN" direction="pwr"/>
<pin name="GND.2" direction="pwr"/>
<pin name="RST.2"/>
<pin name="5V" direction="pwr"/>
<pin name="A7"/>
<pin name="A6"/>
<pin name="A5"/>
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="AREF"/>
<pin name="3V3" direction="pwr"/>
<pin name="D13/SCK"/>
</symbol>
<symbol name="ARDUINO-PRO-MINI">
<description>&lt;b&gt;Arduino Pro Mini&lt;/b&gt;</description>
<pin name="D1/TX"/>
<pin name="D0/RX"/>
<pin name="RST.1"/>
<pin name="GND.1" direction="pwr"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="RAW" direction="pwr"/>
<pin name="GND.2" direction="pwr"/>
<pin name="RST.2"/>
<pin name="VCC" direction="pwr"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="D13"/>
<pin name="D12"/>
<pin name="D11"/>
<pin name="D10"/>
<pin name="P_GND"/>
<pin name="P_CTS"/>
<pin name="P_VCC"/>
<pin name="P_RXD"/>
<pin name="P_TXD"/>
<pin name="P_DTR"/>
<pin name="A7"/>
<pin name="A6"/>
<pin name="GND.3"/>
<pin name="A4"/>
<pin name="A5"/>
</symbol>
<symbol name="ARDUINO-PRO-MINI#NP">
<description>&lt;b&gt;Arduino Pro Mini&lt;/b&gt; without programming pins</description>
<pin name="D1/TX"/>
<pin name="D0/RX"/>
<pin name="RST.1"/>
<pin name="GND.1" direction="pwr"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="RAW" direction="pwr"/>
<pin name="GND.2" direction="pwr"/>
<pin name="RST.2"/>
<pin name="VCC" direction="pwr"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="D13"/>
<pin name="D12"/>
<pin name="D11"/>
<pin name="D10"/>
<pin name="A7"/>
<pin name="A6"/>
<pin name="GND.3"/>
<pin name="A4"/>
<pin name="A5"/>
</symbol>
<symbol name="ARDUINO-PRO-MINI#SMP">
<description>&lt;b&gt;Arduino Pro Mini&lt;/b&gt; with 2 connectors only</description>
<pin name="D1/TX"/>
<pin name="D0/RX"/>
<pin name="RST.1"/>
<pin name="GND.1" direction="pwr"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="RAW" direction="pwr"/>
<pin name="GND.2" direction="pwr"/>
<pin name="RST.2"/>
<pin name="VCC" direction="pwr"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="D13"/>
<pin name="D12"/>
<pin name="D11"/>
<pin name="D10"/>
</symbol>
<symbol name="BATTERY-HOLDER-2AA">
<description>&lt;b&gt;2 x AA Battery Holder&lt;/b&gt;</description>
<pin name="BAT+" direction="pwr"/>
<pin name="BAT-" direction="pwr"/>
</symbol>
<symbol name="DC-DC-STEP-UP-5V-USB">
<description>&lt;b&gt;DC/DC Step-Up Converter&lt;/b&gt; with &lt;b&gt;USB-A&lt;/b&gt; connector</description>
<pin name="IN+" direction="pwr"/>
<pin name="IN-" direction="pwr"/>
</symbol>
<symbol name="DISPLAY-NOKIA-3310">
<description>&lt;b&gt;84x48 Dot Matrix LCD Module&lt;/b&gt; based on &lt;b&gt;Nokia 3310&lt;/b&gt; display</description>
<pin name="VCC.2" direction="pwr"/>
<pin name="GND.2" direction="pwr"/>
<pin name="SCE.2"/>
<pin name="RST.2"/>
<pin name="D/C.2"/>
<pin name="DIN.2"/>
<pin name="SCK.2"/>
<pin name="LED.2" direction="in"/>
<pin name="VCC.1" direction="pwr"/>
<pin name="GND.1" direction="pwr"/>
<pin name="SCE.1"/>
<pin name="RST.1"/>
<pin name="D/C.1"/>
<pin name="DIN.1"/>
<pin name="SCK.1"/>
<pin name="LED.1" direction="in"/>
</symbol>
<symbol name="ETHERNET-ENC28J60">
<description>&lt;b&gt;Ethernet Module&lt;/b&gt; based on &lt;b&gt;ENC28J60&lt;/b&gt; chip</description>
<pin name="GND.1" direction="pwr"/>
<pin name="3V3" direction="pwr"/>
<pin name="CS"/>
<pin name="RST"/>
<pin name="SI"/>
<pin name="SCK"/>
<pin name="WOL"/>
<pin name="SO"/>
<pin name="CLK"/>
<pin name="INT"/>
<pin name="GND.2" direction="pwr"/>
<pin name="5V" direction="pwr"/>
</symbol>
<symbol name="WIRELESS-NRF24L01">
<description>&lt;b&gt;2.4 GHz Wireless Module&lt;/b&gt; based on &lt;b&gt;NRF24L01&lt;/b&gt; chip</description>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="CE"/>
<pin name="CSN"/>
<pin name="SCK"/>
<pin name="MOSI"/>
<pin name="MISO"/>
<pin name="IRQ"/>
</symbol>
<symbol name="WIRELESS-XY-FST">
<description>&lt;b&gt;RF Wireless XY-FST Transmitter&lt;/b&gt;</description>
<pin name="ANT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="ATAD" direction="in"/>
</symbol>
<symbol name="WIRELESS-XY-FST#V">
<description>&lt;b&gt;RF Wireless XY-FST Transmitter&lt;/b&gt; vertically mounted</description>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="ATAD" direction="in"/>
</symbol>
<symbol name="WIRELESS-XY-MK-5V">
<description>&lt;b&gt;RF Wireless XY-MK-5V Receiver&lt;/b&gt;</description>
<pin name="GND"/>
<pin name="DATA.1"/>
<pin name="DATA.2"/>
<pin name="VCC"/>
<pin name="ANT" direction="out"/>
</symbol>
<symbol name="ADC-DAC-PCF8591">
<description>&lt;b&gt;4-Channel ADC and 1-Channel DAC Module&lt;/b&gt; based on &lt;b&gt;PCF8591&lt;/b&gt; chip</description>
<pin name="AOUT"/>
<pin name="AIN0"/>
<pin name="AIN1"/>
<pin name="AIN2"/>
<pin name="AIN3"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="AMPLIFIER-PAM8403">
<description>&lt;b&gt;Stereo Class-D 3W Audio Amplifier&lt;/b&gt; based on &lt;b&gt;PAM8403&lt;/b&gt; chip</description>
<pin name="IN.L" direction="in"/>
<pin name="IN.COM" direction="in"/>
<pin name="IN.R"/>
<pin name="+5V" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT.L-" direction="out"/>
<pin name="OUT.L+" direction="out"/>
<pin name="OUT.R+" direction="out"/>
<pin name="OUT.R-" direction="out"/>
</symbol>
<symbol name="BREADBOARD-POWER-V1">
<description>&lt;b&gt;Breadboard Power Adapter&lt;/b&gt; with onboard 3.3V and 5V regulators</description>
<pin name="P.1"/>
<pin name="P.2"/>
<pin name="P.3"/>
<pin name="P.4"/>
<pin name="P.5"/>
<pin name="M.1"/>
<pin name="M.2"/>
<pin name="M.3"/>
<pin name="M.4"/>
<pin name="M.5"/>
</symbol>
<symbol name="CARD-SD-ADAPTER">
<description>&lt;b&gt;Full Size SD Card Adapter Module&lt;/b&gt; with onboard 3.3V regulator</description>
<pin name="GND.1" direction="pwr"/>
<pin name="3V3" direction="pwr"/>
<pin name="5V" direction="pwr"/>
<pin name="CS"/>
<pin name="MOSI"/>
<pin name="SCK"/>
<pin name="MISO"/>
<pin name="GND.2" direction="pwr"/>
</symbol>
<symbol name="COMPASS-HMC5883L">
<description>&lt;b&gt;3-Axis Digital Compass Module&lt;/b&gt; based on &lt;b&gt;HMC5883L&lt;/b&gt; chip</description>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="DRDY"/>
</symbol>
<symbol name="CURRENT-SENSOR-ACS712">
<description>&lt;b&gt;Isolated Bipolar Current Sensors&lt;/b&gt; based on &lt;b&gt;ACS712&lt;/b&gt; chip</description>
<pin name="VCC" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="CURRENT-SENSOR-ACS712#IC">
<description>&lt;b&gt;Isolated Bipolar Current Sensors&lt;/b&gt; based on &lt;b&gt;ACS712&lt;/b&gt; chip&lt;br&gt;
Symbol with input pads</description>
<pin name="VCC" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="IN+"/>
<pin name="IN-"/>
</symbol>
<symbol name="DC-DC-STEP-DOWN-LM2596">
<description>&lt;b&gt;DC/DC Step-Down Regulator&lt;/b&gt; based on &lt;b&gt;LM2596-ADJ&lt;/b&gt; chip</description>
<pin name="IN+"/>
<pin name="IN-"/>
<pin name="OUT+"/>
<pin name="OUT-"/>
</symbol>
<symbol name="DRIVER-ULN2003">
<description>&lt;b&gt;7-Channel Darlington NPN Transistor Module&lt;/b&gt; based on &lt;b&gt;ULN2003&lt;/b&gt; chip&lt;br&gt;</description>
<pin name="IN.1"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC.1" direction="pwr"/>
<pin name="VCC.2"/>
<pin name="MOT+"/>
<pin name="OUT.A"/>
<pin name="IN.2"/>
<pin name="IN.3"/>
<pin name="IN.4"/>
<pin name="IN.5"/>
<pin name="IN.6"/>
<pin name="IN.7"/>
<pin name="OUT.B"/>
<pin name="OUT.C"/>
<pin name="OUT.D"/>
<pin name="OUT.E"/>
<pin name="OUT.F"/>
<pin name="OUT.G"/>
</symbol>
<symbol name="DRIVER-ULN2003#MC">
<description>&lt;b&gt;7-Channel Darlington NPN Transistor Module&lt;/b&gt; based on &lt;b&gt;ULN2003&lt;/b&gt; chip&lt;br&gt;
Symbol with motor connector pins</description>
<pin name="IN.1"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC.1" direction="pwr"/>
<pin name="VCC.2"/>
<pin name="MOT+"/>
<pin name="OUT.A"/>
<pin name="IN.2"/>
<pin name="IN.3"/>
<pin name="IN.4"/>
<pin name="IN.5"/>
<pin name="IN.6"/>
<pin name="IN.7"/>
<pin name="OUT.B"/>
<pin name="OUT.C"/>
<pin name="OUT.D"/>
<pin name="OUT.E"/>
<pin name="OUT.F"/>
<pin name="OUT.G"/>
<pin name="MOT.+"/>
<pin name="MOT.A"/>
<pin name="MOT.B"/>
<pin name="MOT.C"/>
<pin name="MOT.D"/>
</symbol>
<symbol name="LCD-I2C-CONVERTER">
<description>&lt;b&gt;I2C Bus to 4-Bit Parallel LCD Interface&lt;/b&gt; with LED backlight driver</description>
<pin name="GND" direction="pwr"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="VCC" direction="pwr"/>
<pin name="VSS"/>
<pin name="VDD"/>
<pin name="VEE"/>
<pin name="RS"/>
<pin name="R/W"/>
<pin name="DB0"/>
<pin name="DB1"/>
<pin name="DB2"/>
<pin name="DB3"/>
<pin name="DB4"/>
<pin name="DB5"/>
<pin name="DB6"/>
<pin name="DB7"/>
<pin name="LED.A"/>
<pin name="LED.K"/>
<pin name="EN"/>
</symbol>
<symbol name="LIGHT-DETECTOR">
<description>&lt;b&gt;Light Detection Module&lt;/b&gt;</description>
<pin name="5V" direction="pwr"/>
<pin name="OUT"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="MOTION-PIR-DYP-ME003">
<description>&lt;b&gt;PIR Motion Sensor Module DYP-ME003&lt;/b&gt; based on &lt;b&gt;BISS0001&lt;/b&gt; pyroelectic detector</description>
<pin name="GND" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="REG-AMS1117">
<description>&lt;b&gt;Linear Regulator&lt;/b&gt; based on &lt;b&gt;AMS1117&lt;/b&gt; chip</description>
<pin name="VIN"/>
<pin name="GND.I"/>
<pin name="VOUT"/>
<pin name="GND.O"/>
</symbol>
<symbol name="RELAY-2-SRD#RC">
<description>&lt;b&gt;2-Channel Relay Module&lt;/b&gt; based on &lt;b&gt;SRD-05VDC-SL-C&lt;/b&gt; relays&lt;br&gt;
Symbol with relays pins</description>
<pin name="REL.1.NO"/>
<pin name="REL.1.COM"/>
<pin name="REL.1.NC"/>
<pin name="REL.2.NO"/>
<pin name="REL.2.COM"/>
<pin name="REL.2.NC"/>
<pin name="VCC.1" direction="pwr"/>
<pin name="IN2"/>
<pin name="IN1"/>
<pin name="GND.1" direction="pwr"/>
<pin name="GND.2" direction="pwr"/>
<pin name="VCC.2" direction="pwr"/>
<pin name="JD-VCC"/>
</symbol>
<symbol name="RELAY-2-SRD">
<description>&lt;b&gt;2-Channel Relay Module&lt;/b&gt; based on &lt;b&gt;SRD-05VDC-SL-C&lt;/b&gt; relays</description>
<pin name="VCC.1" direction="pwr"/>
<pin name="IN2"/>
<pin name="IN1"/>
<pin name="GND.1" direction="pwr"/>
<pin name="GND.2" direction="pwr"/>
<pin name="VCC.2" direction="pwr"/>
<pin name="JD-VCC"/>
</symbol>
<symbol name="RTC-EEPROM-BATTERY">
<description>&lt;b&gt;RTC Module with Battery and EEPROM&lt;/b&gt; based on &lt;b&gt;DS1307&lt;/b&gt; and &lt;b&gt;AT24C32&lt;/b&gt; chips</description>
<pin name="GND.1" direction="pwr"/>
<pin name="VCC.1" direction="pwr"/>
<pin name="SDA.1"/>
<pin name="SCL.1"/>
<pin name="DS.1"/>
<pin name="BAT"/>
<pin name="GND.2" direction="pwr"/>
<pin name="VCC.2" direction="pwr"/>
<pin name="SDA.2"/>
<pin name="SCL.2"/>
<pin name="DS.2"/>
<pin name="SQ"/>
</symbol>
<symbol name="SOIL-MOISTURE-SENSOR">
<description>&lt;b&gt;Soil Moisture Sensor&lt;/b&gt;</description>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="DO" direction="out"/>
<pin name="A0"/>
<pin name="SENS.2"/>
<pin name="SENS.1"/>
</symbol>
<symbol name="SOUND-DETECTOR">
<description>&lt;b&gt;Sound Detection Module&lt;/b&gt;</description>
<pin name="GND" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="+5V" direction="pwr"/>
</symbol>
<symbol name="ULTRASONIC-HC-SR04">
<description>&lt;b&gt;Ultrasonic Ranging Module HC-SR04&lt;/b&gt;</description>
<pin name="VCC" direction="pwr"/>
<pin name="TRIG" direction="in"/>
<pin name="ECHO" direction="out"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="WIRELESS-WIFI-ESP-01">
<description>&lt;b&gt;Wireless Wi-Fi ESP-01 Module&lt;/b&gt; based on &lt;b&gt;ESP8266&lt;/b&gt; chip</description>
<pin name="GND" direction="pwr"/>
<pin name="UTXD"/>
<pin name="GPIO2"/>
<pin name="CH_PD"/>
<pin name="GPIO0"/>
<pin name="RST"/>
<pin name="URXD"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="DC-DC-STEP-UP-5V">
<description>&lt;b&gt;DC/DC Step-Up Converter&lt;/b&gt;</description>
<pin name="IN+" direction="pwr"/>
<pin name="IN-" direction="pwr"/>
<pin name="GND"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="5V"/>
</symbol>
<symbol name="WIRELESS-NRF24L01-PA-EXT">
<description>&lt;b&gt;2.4 GHz Wireless Module&lt;/b&gt; based on &lt;b&gt;NRF24L01&lt;/b&gt; chip with preamplifier and external antenna</description>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="CE"/>
<pin name="CSN"/>
<pin name="SCK"/>
<pin name="MOSI"/>
<pin name="MISO"/>
<pin name="IRQ"/>
</symbol>
<symbol name="AC-DC-3.5W">
<description>&lt;b&gt;AC/DC 3.5W Converter&lt;/b&gt;</description>
<pin name="AC1"/>
<pin name="AC2"/>
<pin name="OUT-"/>
<pin name="OUT+"/>
<pin name="5V"/>
</symbol>
<symbol name="BATTERY-CHARGER-LI-5V">
<description>&lt;b&gt;Lithium Battery 5V Charger&lt;/b&gt;</description>
<pin name="IN+"/>
<pin name="IN-"/>
<pin name="BAT+"/>
<pin name="BAT-"/>
</symbol>
<symbol name="FLAME-DETECTOR">
<description>&lt;b&gt;Flame Detector&lt;/b&gt;</description>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="DO"/>
<pin name="AO"/>
</symbol>
<symbol name="IR-RECEIVER">
<description>&lt;b&gt;IR Receiver Module&lt;/b&gt;</description>
<pin name="VCC.1"/>
<pin name="VCC.2"/>
<pin name="GND.1"/>
<pin name="GND.2"/>
<pin name="IN.1"/>
<pin name="IN.2"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="IN"/>
</symbol>
<symbol name="IR-RECEIVER#NC">
<description>&lt;b&gt;IR Receiver Module&lt;/b&gt; without IR sensor connector</description>
<pin name="VCC.1"/>
<pin name="VCC.2"/>
<pin name="GND.1"/>
<pin name="GND.2"/>
<pin name="IN.1"/>
<pin name="IN.2"/>
</symbol>
<symbol name="STEPPER-MOTOR-EASY-DRIVER">
<description>&lt;b&gt;Stepper Motor Easy Driver&lt;/b&gt;</description>
<pin name="GND.1"/>
<pin name="+5V"/>
<pin name="SLP"/>
<pin name="MS1"/>
<pin name="GND.2"/>
<pin name="STER"/>
<pin name="DIR"/>
<pin name="A.1"/>
<pin name="A.2"/>
<pin name="B.1"/>
<pin name="B.2"/>
<pin name="PFD"/>
<pin name="RST"/>
<pin name="ENA"/>
<pin name="MS2"/>
<pin name="GND"/>
<pin name="M+"/>
</symbol>
<symbol name="RS485-TTL-CONVERTER">
<description>&lt;b&gt;RS485 to TTL converter&lt;/b&gt; based on &lt;b&gt;MAX485&lt;/b&gt; chip</description>
<pin name="B" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="RO" direction="pas"/>
<pin name="RE" direction="pas"/>
<pin name="DE" direction="pas"/>
<pin name="DI" direction="pas"/>
</symbol>
<symbol name="TOUCH-KEYPAD-4X4">
<description>&lt;b&gt;16 Channel Capacitive Touch Keypad&lt;/b&gt;</description>
<pin name="OUT8"/>
<pin name="OUT6"/>
<pin name="OUT5"/>
<pin name="OUT4"/>
<pin name="OUT3"/>
<pin name="OUT2"/>
<pin name="OUT1"/>
<pin name="SDO"/>
<pin name="SCL"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="OUT7"/>
</symbol>
<symbol name="N-MOSFET-SWITCH">
<description>&lt;b&gt;Low Side N-MOSFET Switch&lt;/b&gt; with &lt;b&gt;Optocoupler&lt;/b&gt;</description>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="CTRL"/>
</symbol>
<symbol name="N-MOSFET-SWITCH#IC">
<description>&lt;b&gt;Low Side N-MOSFET Switch&lt;/b&gt; with &lt;b&gt;Optocoupler&lt;/b&gt;&lt;br /&gt;
Symbol with connector pins</description>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="CTRL"/>
<pin name="IN.V+" direction="pwr"/>
<pin name="IN.COM" direction="pwr"/>
<pin name="OUT.V+" direction="pwr"/>
<pin name="OUT.SW" direction="pwr"/>
</symbol>
<symbol name="SOUND-BUZZER">
<description>&lt;b&gt;Sound Buzzer Module&lt;/b&gt;</description>
<pin name="VCC" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="BREADBOARD-POWER-V2">
<description>&lt;b&gt;Breadboard Power Adapter&lt;/b&gt; with onboard 3.3V and 5V regulators</description>
<pin name="P.1"/>
<pin name="P.2"/>
<pin name="M.1"/>
<pin name="M.2"/>
</symbol>
<symbol name="LED-24XRGB-RING">
<description>&lt;b&gt;24 LEDs RGB Ring&lt;/b&gt; based on &lt;b&gt;WS2812B&lt;/b&gt;</description>
<pin name="GND.1" direction="pwr"/>
<pin name="VCC.1" direction="pwr"/>
<pin name="DIN" direction="in"/>
<pin name="GND.2" direction="pwr"/>
<pin name="VCC.2" direction="pwr"/>
<pin name="DOUT" direction="in"/>
</symbol>
<symbol name="GSM-MODEM-SIM900A">
<description>&lt;b&gt;GSM Mini Moodule&lt;/b&gt; based on &lt;b&gt;SIM900A&lt;/b&gt;</description>
<pin name="VCC5" direction="pwr"/>
<pin name="GND.1" direction="pwr"/>
<pin name="VCC4" direction="pwr"/>
<pin name="VCCMCU" direction="pwr"/>
<pin name="SIMR"/>
<pin name="SIMT"/>
<pin name="GND.2" direction="pwr"/>
<pin name="RST"/>
</symbol>
<symbol name="SPARKFUN-AD-MUX-16X1">
<description>&lt;b&gt;SparkFun Analog/Digital MUX Breakout&lt;/b&gt; based on &lt;b&gt;CD74HC4067&lt;/b&gt; chip</description>
<pin name="C15"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="S0"/>
<pin name="S1"/>
<pin name="S2"/>
<pin name="S3"/>
<pin name="C14"/>
<pin name="C13"/>
<pin name="C12"/>
<pin name="C11"/>
<pin name="C10"/>
<pin name="C9"/>
<pin name="C8"/>
<pin name="C7"/>
<pin name="C6"/>
<pin name="C5"/>
<pin name="C4"/>
<pin name="C3"/>
<pin name="C2"/>
<pin name="C1"/>
<pin name="C0"/>
<pin name="SIG"/>
</symbol>
<symbol name="RELAY-1-SRD">
<description>&lt;b&gt;1-Channel Relay Module&lt;/b&gt; based on &lt;b&gt;SRD-05VDC-SL-C&lt;/b&gt; relay</description>
<pin name="VCC.1" direction="pwr"/>
<pin name="IN1"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC.2" direction="pwr"/>
<pin name="JD-VCC"/>
</symbol>
<symbol name="RELAY-4-SRD">
<description>&lt;b&gt;4-Channel Relay Module&lt;/b&gt; based on &lt;b&gt;SRD-05VDC-SL-C&lt;/b&gt; relays</description>
<pin name="VCC.1" direction="pwr"/>
<pin name="IN2"/>
<pin name="IN1"/>
<pin name="GND" direction="pwr"/>
<pin name="IN3"/>
<pin name="IN4"/>
<pin name="VCC.2" direction="pwr"/>
<pin name="JD-VCC"/>
</symbol>
<symbol name="RELAY-8-SRD">
<description>&lt;b&gt;8-Channel Relay Module&lt;/b&gt; based on &lt;b&gt;SRD-05VDC-SL-C&lt;/b&gt; relays</description>
<pin name="VCC.1" direction="pwr"/>
<pin name="IN2"/>
<pin name="IN1"/>
<pin name="GND.1" direction="pwr"/>
<pin name="IN3"/>
<pin name="IN4"/>
<pin name="IN5"/>
<pin name="IN6"/>
<pin name="IN7"/>
<pin name="IN8"/>
<pin name="VCC.2" direction="pwr"/>
<pin name="JD-VCC"/>
<pin name="GND.2" direction="pwr"/>
</symbol>
<symbol name="RELAY-4-SRD#RC">
<description>&lt;b&gt;4-Channel Relay Module&lt;/b&gt; based on &lt;b&gt;SRD-05VDC-SL-C&lt;/b&gt; relays&lt;br&gt;
Symbol with relays pins</description>
<pin name="VCC.1" direction="pwr"/>
<pin name="IN2"/>
<pin name="IN1"/>
<pin name="GND" direction="pwr"/>
<pin name="IN3"/>
<pin name="IN4"/>
<pin name="VCC.2" direction="pwr"/>
<pin name="JD-VCC"/>
<pin name="REL.1.NO"/>
<pin name="REL.1.COM"/>
<pin name="REL.1.NC"/>
<pin name="REL.2.NO"/>
<pin name="REL.2.COM"/>
<pin name="REL.2.NC"/>
<pin name="REL.3.NO"/>
<pin name="REL.3.COM"/>
<pin name="REL.3.NC"/>
<pin name="REL.4.NO"/>
<pin name="REL.4.COM"/>
<pin name="REL.4.NC"/>
</symbol>
<symbol name="RELAY-8-SRD#RC">
<description>&lt;b&gt;8-Channel Relay Module&lt;/b&gt; based on &lt;b&gt;SRD-05VDC-SL-C&lt;/b&gt; relays&lt;br&gt;
Symbol with relays pins</description>
<pin name="VCC.1" direction="pwr"/>
<pin name="IN2"/>
<pin name="IN1"/>
<pin name="GND.1" direction="pwr"/>
<pin name="IN3"/>
<pin name="IN4"/>
<pin name="IN5"/>
<pin name="IN6"/>
<pin name="IN7"/>
<pin name="IN8"/>
<pin name="VCC.2" direction="pwr"/>
<pin name="JD-VCC"/>
<pin name="GND.2" direction="pwr"/>
<pin name="REL.1.NO"/>
<pin name="REL.1.COM"/>
<pin name="REL.1.NC"/>
<pin name="REL.2.NO"/>
<pin name="REL.2.COM"/>
<pin name="REL.2.NC"/>
<pin name="REL.3.NO"/>
<pin name="REL.3.COM"/>
<pin name="REL.3.NC"/>
<pin name="REL.4.NO"/>
<pin name="REL.4.COM"/>
<pin name="REL.4.NC"/>
<pin name="REL.5.NO"/>
<pin name="REL.5.COM"/>
<pin name="REL.5.NC"/>
<pin name="REL.6.NO"/>
<pin name="REL.6.COM"/>
<pin name="REL.6.NC"/>
<pin name="REL.7.NO"/>
<pin name="REL.7.COM"/>
<pin name="REL.7.NC"/>
<pin name="REL.8.NO"/>
<pin name="REL.8.COM"/>
<pin name="REL.8.NC"/>
</symbol>
<symbol name="RELAY-1-SRD#RC">
<description>&lt;b&gt;1-Channel Relay Module&lt;/b&gt; based on &lt;b&gt;SRD-05VDC-SL-C&lt;/b&gt; relay&lt;br&gt;
Symbol with relays pins</description>
<pin name="VCC.1" direction="pwr"/>
<pin name="IN1"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC.2" direction="pwr"/>
<pin name="JD-VCC"/>
<pin name="REL.1.NO"/>
<pin name="REL.1.COM"/>
<pin name="REL.1.NC"/>
</symbol>
<symbol name="BATTERY-LI-MH12210">
<description>&lt;b&gt;MH12210 Li-ion Rechargeable Battery&lt;/b&gt;</description>
<pin name="BAT+" direction="pwr"/>
<pin name="BAT-" direction="pwr"/>
</symbol>
<symbol name="TOUCH-KEYPAD-4X2">
<description>&lt;b&gt;8 Channel Capacitive Touch Keypad&lt;/b&gt;</description>
<pin name="GND" direction="pwr"/>
<pin name="OUT1"/>
<pin name="OUT2"/>
<pin name="OUT3"/>
<pin name="OUT4"/>
<pin name="OUT5"/>
<pin name="OUT6"/>
<pin name="OUT7"/>
<pin name="OUT8"/>
<pin name="DV"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="TOUCH-KEYPAD-4X1">
<description>&lt;b&gt;4 Channel Capacitive Touch Keypad&lt;/b&gt;</description>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT4"/>
<pin name="OUT3"/>
<pin name="OUT2"/>
<pin name="OUT1"/>
</symbol>
<symbol name="BATTERY-CHARGER-LI-PROT">
<description>&lt;b&gt;Protected Lithium Battery 5V Charger&lt;/b&gt; with micro-USB connector</description>
<pin name="IN+"/>
<pin name="IN-"/>
<pin name="B+"/>
<pin name="B-"/>
<pin name="OUT+"/>
<pin name="OUT-"/>
</symbol>
<symbol name="DCF77-RECEIVER">
<description>&lt;b&gt;DCF77 Time Signal Receiver&lt;/b&gt; based on &lt;b&gt;MAS6180&lt;/b&gt; chip.</description>
<pin name="V" direction="pwr"/>
<pin name="G" direction="pwr"/>
<pin name="P2"/>
<pin name="T"/>
<pin name="P1"/>
<pin name="AON"/>
<pin name="ANT1" direction="pas"/>
<pin name="ANT2" direction="pas"/>
</symbol>
<symbol name="WIRELESS-BLUETOOTH-XS3868">
<description>&lt;b&gt;Bluetooth Stereo Audio Module&lt;/b&gt; based on &lt;b&gt;OVC3860&lt;/b&gt; chip</description>
<pin name="AGND" direction="pwr"/>
<pin name="ARIGHT" direction="out"/>
<pin name="ALEFT" direction="out"/>
<pin name="MIC+"/>
<pin name="MIC-"/>
<pin name="CH.STAT"/>
<pin name="CHRG"/>
<pin name="CH.POW"/>
<pin name="GND" direction="pwr"/>
<pin name="NC.1" direction="pas"/>
<pin name="VBAT" direction="pwr"/>
<pin name="1.8V_OUT" direction="pwr"/>
<pin name="RST" direction="pwr"/>
<pin name="NC.2" direction="pas"/>
<pin name="VOL+"/>
<pin name="VOL-"/>
<pin name="NC.3" direction="pas"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="NC.4" direction="pas"/>
<pin name="NEXT"/>
<pin name="BACK"/>
<pin name="PLAY"/>
</symbol>
<symbol name="DISPLAY-OLED-128X64">
<description>&lt;b&gt;128x64 Dot Matrix OLED Module&lt;/b&gt;</description>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="RES"/>
<pin name="DC"/>
<pin name="CS"/>
</symbol>
<symbol name="DFPLAYER-MINI-MODULE">
<description>&lt;b&gt;DFPlayer Mini&lt;/b&gt; - MP3 player module based on &lt;b&gt;YX5200&lt;/b&gt; chip</description>
<pin name="VCC" direction="pwr"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="DAC_R"/>
<pin name="DAC_I"/>
<pin name="SPK_1"/>
<pin name="GND.1" direction="pwr"/>
<pin name="SPK_2"/>
<pin name="IO_1"/>
<pin name="GND.2" direction="pwr"/>
<pin name="IO_2"/>
<pin name="ADKEY_1"/>
<pin name="ADKEY_2"/>
<pin name="USB+"/>
<pin name="USB-"/>
<pin name="BUSY"/>
</symbol>
<symbol name="DC-DC-LM2596-DISP">
<description>&lt;b&gt;DC/DC Step-Down Regulator&lt;/b&gt; with &lt;b&gt;Voltage Display&lt;/b&gt; based on &lt;b&gt;LM2596-ADJ&lt;/b&gt; chip</description>
<pin name="IN+"/>
<pin name="IN-"/>
<pin name="OUT+"/>
<pin name="OUT-"/>
</symbol>
<symbol name="DC-DC-LM2596-DISP#RC">
<description>&lt;b&gt;DC/DC Step-Down Regulator&lt;/b&gt; with &lt;b&gt;Voltage Display&lt;/b&gt; based on &lt;b&gt;LM2596-ADJ&lt;/b&gt; chip&lt;br /&gt;
Symbol with connector pins.</description>
<pin name="IN+"/>
<pin name="IN-"/>
<pin name="OUT+"/>
<pin name="OUT-"/>
<pin name="C.IN+"/>
<pin name="C.IN-"/>
<pin name="C.OUT+"/>
<pin name="C.OUT-"/>
</symbol>
<symbol name="LED-8XRGB-LINE">
<description>&lt;b&gt;8 LEDs RGB Line Display&lt;/b&gt; based on &lt;b&gt;WS2812B&lt;/b&gt;</description>
<pin name="GND.1" direction="pwr"/>
<pin name="VCC.1" direction="pwr"/>
<pin name="GND.2" direction="pwr"/>
<pin name="DOUT" direction="out"/>
<pin name="GND.3" direction="pwr"/>
<pin name="GND.4" direction="pwr"/>
<pin name="VCC.2" direction="pwr"/>
<pin name="DIN" direction="in"/>
</symbol>
<symbol name="LED-15XRGB-QRING">
<description>&lt;b&gt;15 LEDs RGB Quarter-Ring&lt;/b&gt; based on &lt;b&gt;WS2812B&lt;/b&gt;</description>
<pin name="GND.1" direction="pwr"/>
<pin name="VCC.1" direction="pwr"/>
<pin name="GND.2" direction="pwr"/>
<pin name="DOUT" direction="out"/>
<pin name="VCC.2" direction="pwr"/>
<pin name="DIN" direction="in"/>
</symbol>
<symbol name="TEMP-HUM-SENSOR-DHT11">
<description>&lt;b&gt;DHT11 - digital humidity &amp; temperature sensor&lt;/b&gt;</description>
<pin name="VDD" direction="pwr"/>
<pin name="DAT"/>
<pin name="N.C." direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="TEMP-HUM-SENSOR-DHT22">
<description>&lt;b&gt;DHT22 - digital humidity &amp; temperature sensor&lt;/b&gt;</description>
<pin name="VDD" direction="pwr"/>
<pin name="DAT"/>
<pin name="N.C." direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="DISPLAY-OLED-128X32">
<description>&lt;b&gt;128x32 Dot Matrix OLED Module&lt;/b&gt; with &lt;b&gt;I2C&lt;/b&gt; interface</description>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="SDA"/>
<pin name="SCL"/>
</symbol>
<symbol name="DC-DC-STEP-DOWN-MP2307">
<description>&lt;b&gt;DC/DC Step-Down Regulator&lt;/b&gt; based on &lt;b&gt;MP2307DN&lt;/b&gt; chip</description>
<pin name="IN+"/>
<pin name="IN-"/>
<pin name="OUT+"/>
<pin name="OUT-"/>
</symbol>
<symbol name="RADIO-RECEIVER-DCF77">
<description>&lt;b&gt;DCF-77 Longwave Radio Time Signal Receiver&lt;/b&gt; based on &lt;b&gt;MAS6180B1&lt;/b&gt; chip</description>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="P2"/>
<pin name="T" direction="out"/>
<pin name="ANT1" direction="pas"/>
<pin name="ANT2" direction="pas"/>
<pin name="P1"/>
<pin name="AON"/>
</symbol>
<symbol name="BATTERY-HOLDER-2AAA">
<description>&lt;b&gt;2 x AAA Battery Holder&lt;/b&gt;</description>
<pin name="BAT+" direction="pwr"/>
<pin name="BAT-" direction="pwr"/>
</symbol>
<symbol name="THERMOCOUPLE-MAX31855">
<description>&lt;b&gt;Thermocouple Analog-to-Digital Converter&lt;/b&gt; based on &lt;b&gt;MAX31855&lt;/b&gt; chip</description>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="out"/>
<pin name="SO"/>
<pin name="CS"/>
<pin name="SCK"/>
</symbol>
<symbol name="THERMOCOUPLE-MAX31855#IC">
<description>&lt;b&gt;Thermocouple Analog-to-Digital Converter&lt;/b&gt; based on &lt;b&gt;MAX31855&lt;/b&gt; chip&lt;br /&gt;
Symbol with thermocouple connector pins</description>
<pin name="T-"/>
<pin name="T+"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="out"/>
<pin name="SO"/>
<pin name="CS"/>
<pin name="SCK"/>
</symbol>
<symbol name="LEVEL-SHIFTER-4CH">
<description>&lt;b&gt;4-Channel Bi-Directional  Logic Level Converter&lt;/b&gt; based on &lt;b&gt;BSS128&lt;/b&gt; transistors</description>
<pin name="LV3"/>
<pin name="GND.1" direction="pwr"/>
<pin name="LV" direction="pwr"/>
<pin name="LV2"/>
<pin name="LV1"/>
<pin name="HV4"/>
<pin name="HV3"/>
<pin name="GND.2" direction="pwr"/>
<pin name="HV" direction="pwr"/>
<pin name="HV2"/>
<pin name="HV1"/>
<pin name="LV4"/>
</symbol>
<symbol name="RTC-DS3231-AT24C32">
<description>&lt;b&gt;RTC Module with Battery and EEPROM&lt;/b&gt; based on &lt;b&gt;DS3231&lt;/b&gt; and &lt;b&gt;AT24C32&lt;/b&gt; chips</description>
<pin name="VCC.1" direction="pwr"/>
<pin name="SDA.1"/>
<pin name="SCL.1"/>
<pin name="SQW"/>
<pin name="32K"/>
<pin name="GND.2" direction="pwr"/>
<pin name="VCC.2" direction="pwr"/>
<pin name="SDA.2"/>
<pin name="SCL.2"/>
<pin name="GND.1" direction="pwr"/>
</symbol>
<symbol name="WIRELESS-LORA-RFM95W">
<description>&lt;b&gt;868/915 MHz LoRa Radio Transceiver Module&lt;/b&gt;</description>
<pin name="GND.1" direction="pwr"/>
<pin name="MISO"/>
<pin name="MOSI"/>
<pin name="SCK"/>
<pin name="NSS"/>
<pin name="RST"/>
<pin name="DIO5"/>
<pin name="GND.2" direction="pwr"/>
<pin name="ANT" direction="pas"/>
<pin name="GND.3" direction="pwr"/>
<pin name="DIO3"/>
<pin name="DIO4"/>
<pin name="3.3V" direction="pwr"/>
<pin name="DIO0"/>
<pin name="DIO1"/>
<pin name="DIO2"/>
</symbol>
<symbol name="TEMP-HUM-PRES-BME280">
<description>&lt;b&gt;Digital Humidity-Temperature-Pressure Sensor&lt;/b&gt; based on &lt;b&gt;BME280&lt;/b&gt; device</description>
<pin name="VIN" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SCL"/>
<pin name="SDA"/>
</symbol>
<symbol name="TEMP-HUM-SENSOR-HTU21D">
<description>&lt;b&gt;Digital Humidity &amp; Temperature Sensor&lt;/b&gt; based on &lt;b&gt;HTU21D&lt;/b&gt; device</description>
<pin name="VIN" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SCL"/>
<pin name="SDA"/>
</symbol>
<symbol name="USB-SERIAL-FT232R">
<description>&lt;b&gt;USB to Serial UART Converter&lt;/b&gt; based on &lt;b&gt;FT232R&lt;/b&gt; chip</description>
<pin name="RX"/>
<pin name="TX"/>
<pin name="DTR"/>
<pin name="VCC" direction="pwr"/>
<pin name="CTS"/>
<pin name="GND"/>
</symbol>
<symbol name="DATA-LOGGER-MINI">
<description>&lt;b&gt;Mini Data Logger&lt;/b&gt; with &lt;b&gt;microSD card&lt;/b&gt; and  battery powered &lt;b&gt;RTC&lt;/b&gt; based on &lt;b&gt;DS1307&lt;/b&gt; chip</description>
<pin name="5V" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="SCK"/>
<pin name="MISO"/>
<pin name="MOSI"/>
<pin name="CS" direction="pwr"/>
</symbol>
<symbol name="GAS-SENSOR-MQ2">
<description>&lt;b&gt;Gas Sensor&lt;/b&gt; based on &lt;b&gt;MQ-2&lt;/b&gt; device</description>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="DO" direction="out"/>
<pin name="AO" direction="out"/>
</symbol>
<symbol name="UV-SENSOR-ML8511">
<description>&lt;b&gt;UV  Sensor&lt;/b&gt; based on &lt;b&gt;ML8511&lt;/b&gt; device</description>
<pin name="VIN" direction="pwr"/>
<pin name="3V3" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT"/>
<pin name="EN"/>
</symbol>
<symbol name="ADC-4CH-ADS1115">
<description>&lt;b&gt;4 Channel 16-Bit Analog-to-Digital Converter&lt;/b&gt; based on &lt;b&gt;ADS1115&lt;/b&gt; chip</description>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="ADDR"/>
<pin name="ALRT"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
</symbol>
<symbol name="WIRELESS-BLUETOOTH-BK8000">
<description>&lt;b&gt;Bluetooth Audio Module&lt;/b&gt; based on &lt;b&gt;BK8000L&lt;/b&gt; chip</description>
<pin name="GND.1" direction="pwr"/>
<pin name="ANT" direction="pas"/>
<pin name="GND.2" direction="pwr"/>
<pin name="TMS"/>
<pin name="TCK"/>
<pin name="TDO"/>
<pin name="TDI"/>
<pin name="RSTN"/>
<pin name="MBISTEN"/>
<pin name="RX/GPIO0"/>
<pin name="TX/GPIO1"/>
<pin name="GPIO2"/>
<pin name="MIC_P" direction="in"/>
<pin name="VMIC" direction="pas"/>
<pin name="AUD_LN" direction="out"/>
<pin name="AUD_LP" direction="out"/>
<pin name="AUD_RP" direction="out"/>
<pin name="AUD_RN" direction="out"/>
<pin name="VBUS" direction="pas"/>
<pin name="VBAT" direction="pas"/>
<pin name="3V_OUT" direction="pwr"/>
<pin name="VADC" direction="pwr"/>
<pin name="GND.5" direction="pwr"/>
<pin name="GPIO3"/>
<pin name="GPIO4"/>
<pin name="GPIO5"/>
<pin name="GND.3" direction="pwr"/>
<pin name="MIC_N" direction="in"/>
<pin name="IN_L" direction="in"/>
<pin name="IN_R" direction="in"/>
<pin name="GPIO11"/>
<pin name="GND.4" direction="pwr"/>
</symbol>
<symbol name="GPS-RECEIVER-NEO6M">
<description>&lt;b&gt;GPS Receiver Module&lt;/b&gt; based on &lt;b&gt;NEO-6&lt;/b&gt; device</description>
<pin name="PPS" direction="pwr"/>
<pin name="RXD" direction="pwr"/>
<pin name="TXD"/>
<pin name="GND"/>
<pin name="VCC"/>
</symbol>
<symbol name="STEPPER-MOTOR-DRIVER-L6470">
<description>&lt;b&gt;Stepper Motor Driver&lt;/b&gt; based on &lt;b&gt;L6470&lt;/b&gt; chip</description>
<pin name="5V" direction="pwr"/>
<pin name="O1B" direction="out"/>
<pin name="O1A" direction="out"/>
<pin name="O2B" direction="out"/>
<pin name="O2A" direction="out"/>
<pin name="R4.2" direction="pas"/>
<pin name="R4.1" direction="pas"/>
<pin name="GND.2"/>
<pin name="SW"/>
<pin name="GND.1" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="SDO"/>
<pin name="CK"/>
<pin name="SDI"/>
<pin name="BSYN"/>
<pin name="CSN"/>
<pin name="FLGN"/>
<pin name="STCK"/>
<pin name="STBY"/>
<pin name="GND.3" direction="pwr"/>
<pin name="R4.3" direction="pas"/>
</symbol>
<symbol name="PWM-SERVO-DRIVER-16CH">
<description>&lt;b&gt;16-Channel 12-bit PWM/Servo Driver&lt;/b&gt; based on &lt;b&gt;PCA9685&lt;/b&gt; chip</description>
<pin name="GND.1" direction="pwr"/>
<pin name="C0.PWM"/>
<pin name="C0.V+"/>
<pin name="OE.1"/>
<pin name="SCL.1"/>
<pin name="SDA.1"/>
<pin name="VCC.1" direction="pwr"/>
<pin name="V+.1" direction="pwr"/>
<pin name="C0.GND"/>
<pin name="C1.PWM"/>
<pin name="C1.V+"/>
<pin name="C1.GND"/>
<pin name="C2.PWM"/>
<pin name="C2.V+"/>
<pin name="C2.GND"/>
<pin name="C3.PWM"/>
<pin name="C3.V+"/>
<pin name="C3.GND"/>
<pin name="C4.PWM"/>
<pin name="C4.V+"/>
<pin name="C4.GND"/>
<pin name="C5.PWM"/>
<pin name="C5.V+"/>
<pin name="C5.GND"/>
<pin name="C6.PWM"/>
<pin name="C6.V+"/>
<pin name="C6.GND"/>
<pin name="C7.PWM"/>
<pin name="C7.V+"/>
<pin name="C7.GND"/>
<pin name="C8.PWM"/>
<pin name="C8.V+"/>
<pin name="C8.GND"/>
<pin name="C9.PWM"/>
<pin name="C9.V+"/>
<pin name="C9.GND"/>
<pin name="C10.PWM"/>
<pin name="C10.V+"/>
<pin name="C10.GND"/>
<pin name="C11.PWM"/>
<pin name="C11.V+"/>
<pin name="C11.GND"/>
<pin name="C12.PWM"/>
<pin name="C12.V+"/>
<pin name="C12.GND"/>
<pin name="C13.PWM"/>
<pin name="C13.V+"/>
<pin name="C13.GND"/>
<pin name="C14.PWM"/>
<pin name="C14.V+"/>
<pin name="C14.GND"/>
<pin name="C15.PWM"/>
<pin name="C15.V+"/>
<pin name="C15.GND"/>
<pin name="V+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND.2" direction="pwr"/>
<pin name="OE.2"/>
<pin name="SCL.2"/>
<pin name="SDA.2"/>
<pin name="VCC.2" direction="pwr"/>
<pin name="V+.2" direction="pwr"/>
</symbol>
<symbol name="LEVEL-SHIFTER-8CH">
<description>&lt;b&gt;8-Channel Bi-Directional  Logic Level Converter&lt;/b&gt; based on &lt;b&gt;BSS128&lt;/b&gt; transistors</description>
<pin name="LV3"/>
<pin name="GND.1" direction="pwr"/>
<pin name="LV" direction="pwr"/>
<pin name="LV2"/>
<pin name="LV1"/>
<pin name="HV4"/>
<pin name="HV3"/>
<pin name="GND.2" direction="pwr"/>
<pin name="HV" direction="pwr"/>
<pin name="HV2"/>
<pin name="HV1"/>
<pin name="LV4"/>
<pin name="LV5"/>
<pin name="LV6"/>
<pin name="LV7"/>
<pin name="LV8"/>
<pin name="HV5"/>
<pin name="HV6"/>
<pin name="HV7"/>
<pin name="HV8"/>
</symbol>
<symbol name="LIGHT-SENSOR-BH1750">
<description>&lt;b&gt;Digital Light Sensor&lt;/b&gt; based on &lt;b&gt;BH1750&lt;/b&gt;</description>
<pin name="ADDR"/>
<pin name="GND" direction="pwr"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="RANGING-SENSOR-VL53L0X">
<description>&lt;b&gt;Laser Ranging Sensor&lt;/b&gt; based on &lt;b&gt;VL53L0X&lt;/b&gt; device</description>
<pin name="VIN" direction="pwr"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="GND" direction="pwr"/>
<pin name="GPIO1"/>
<pin name="XSHUT"/>
</symbol>
<symbol name="WEMOS-D1-MINI-PRO">
<description>&lt;b&gt;WEMOS D1 mini Pro&lt;/b&gt;: Mini Wi-Fi Board based on &lt;b&gt;ESP-8266EX&lt;/b&gt; chip</description>
<pin name="RST"/>
<pin name="A0"/>
<pin name="D0"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="3V3" direction="pwr"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="GND" direction="pwr"/>
<pin name="5V" direction="pwr"/>
</symbol>
<symbol name="WEMOS-D1-MINI-SHIELD">
<description>Template symbol for &lt;b&gt;WEMOS D1 mini&lt;/b&gt; shields</description>
<pin name="RST"/>
<pin name="A0"/>
<pin name="D0"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="3V3" direction="pwr"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="GND" direction="pwr"/>
<pin name="5V" direction="pwr"/>
</symbol>
<symbol name="WEMOS-D1-MINI">
<description>&lt;b&gt;WEMOS D1 mini&lt;/b&gt;: Mini Wi-Fi Board based on &lt;b&gt;ESP-8266&lt;/b&gt; device</description>
<pin name="RST"/>
<pin name="A0"/>
<pin name="D0"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="3V3" direction="pwr"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="GND" direction="pwr"/>
<pin name="5V" direction="pwr"/>
</symbol>
<symbol name="DC-DC-STEP-UP-MT3608">
<description>&lt;b&gt;DC/DC Step-Up Regulator&lt;/b&gt; based on &lt;b&gt;MT3608&lt;/b&gt; chip</description>
<pin name="IN+"/>
<pin name="IN-"/>
<pin name="OUT+"/>
<pin name="OUT-"/>
</symbol>
<symbol name="USB-SERIAL-CP2102">
<description>&lt;b&gt;USB to Serial UART Converter&lt;/b&gt; based on &lt;b&gt;CP2102&lt;/b&gt; chip</description>
<pin name="DTR"/>
<pin name="RXI"/>
<pin name="3V3" direction="pwr"/>
<pin name="TDO"/>
<pin name="GND" direction="pwr"/>
<pin name="+5V" direction="pwr"/>
</symbol>
<symbol name="TEMP-HUM-SENSOR-AM2322">
<description>&lt;b&gt;AM2322 - digital humidity &amp; temperature sensor&lt;/b&gt;</description>
<pin name="VDD" direction="pwr"/>
<pin name="SDA"/>
<pin name="GND" direction="pwr"/>
<pin name="SCL"/>
</symbol>
<symbol name="DISPLAY-OLED-128X64-I2C">
<description>&lt;b&gt;128x64 Dot Matrix OLED Module&lt;/b&gt;&lt;br /&gt;
Variant with I2C interface</description>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="SCL"/>
<pin name="SDA"/>
</symbol>
<symbol name="REG-AMS1117-3P">
<description>&lt;b&gt;Linear Regulator&lt;/b&gt; based on &lt;b&gt;AMS1117&lt;/b&gt; chip&lt;br /&gt;
3-pin version</description>
<pin name="IN"/>
<pin name="GND"/>
<pin name="OUT"/>
</symbol>
<symbol name="AC-VOLTAGE-SENSOR">
<description>&lt;b&gt;Isolated AC Voltage Sensor&lt;/b&gt; based on &lt;b&gt;ZMPT101B&lt;/b&gt; transformer</description>
<pin name="VCC" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="GND.1" direction="pwr"/>
<pin name="GND.2" direction="pwr"/>
</symbol>
<symbol name="AC-VOLTAGE-SENSOR#IC">
<description>&lt;b&gt;Isolated AC Voltage Sensor&lt;/b&gt; based on &lt;b&gt;ZMPT101B&lt;/b&gt; transformer&lt;br /&gt;
Symbol with input connector</description>
<pin name="VCC" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="GND.1" direction="pwr"/>
<pin name="GND.2" direction="pwr"/>
<pin name="L" direction="pas"/>
<pin name="N" direction="pas"/>
</symbol>
<symbol name="WIRELESS-BLUETOOTH-HC-05">
<description>&lt;b&gt;Bluetooth Transceiver Module&lt;/b&gt; based on &lt;b&gt;HC-05&lt;/b&gt; board</description>
<pin name="STATE"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="GND" direction="pwr"/>
<pin name="+5V" direction="pwr"/>
<pin name="EN"/>
</symbol>
<symbol name="JOYSTICK-2AXIS-BUTTON">
<description>&lt;b&gt;2-Axis Analog Joystick&lt;/b&gt; with Push Button</description>
<pin name="GND" direction="pwr"/>
<pin name="+5V" direction="pwr"/>
<pin name="VRX" direction="pas"/>
<pin name="VRY" direction="pas"/>
<pin name="SW" direction="pas"/>
</symbol>
<symbol name="DC-DC-STEP-DOWN-MP1584">
<description>&lt;b&gt;DC/DC Step-Down Regulator&lt;/b&gt; based on &lt;b&gt;MP1584&lt;/b&gt; chip</description>
<pin name="IN+.2"/>
<pin name="IN-.1"/>
<pin name="OUT+.2"/>
<pin name="OUT-.1"/>
<pin name="IN-.2"/>
<pin name="IN+.1"/>
<pin name="OUT-.2"/>
<pin name="OUT+.1"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ARDUINO-NANO-3.0#ISP" prefix="M">
<description>&lt;b&gt;Arduino Nano 3.0&lt;/b&gt; (and compatible devices) with ISP pads
&lt;p&gt;More details available here:&lt;br&gt;
&lt;a href="https://www.arduino.cc/en/Main/ArduinoBoardNano"&gt;https://www.arduino.cc/en/Main/ArduinoBoardNano&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/arduino+nano"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=ARDUINO-NANO-3.0"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ARDUINO-NANO-3.0#ISP"/>
</gates>
<devices>
<device name="" package="ARDUINO-NANO-3.0#ISP">
<connects>
<connect gate="G$1" pin="3V3" pad="J2.14"/>
<connect gate="G$1" pin="5V" pad="J2.4"/>
<connect gate="G$1" pin="A0" pad="J2.12"/>
<connect gate="G$1" pin="A1" pad="J2.11"/>
<connect gate="G$1" pin="A2" pad="J2.10"/>
<connect gate="G$1" pin="A3" pad="J2.9"/>
<connect gate="G$1" pin="A4" pad="J2.8"/>
<connect gate="G$1" pin="A5" pad="J2.7"/>
<connect gate="G$1" pin="A6" pad="J2.6"/>
<connect gate="G$1" pin="A7" pad="J2.5"/>
<connect gate="G$1" pin="AREF" pad="J2.13"/>
<connect gate="G$1" pin="D0/RX" pad="J1.2"/>
<connect gate="G$1" pin="D1/TX" pad="J1.1"/>
<connect gate="G$1" pin="D10" pad="J1.13"/>
<connect gate="G$1" pin="D11/MOSI" pad="J1.14"/>
<connect gate="G$1" pin="D12/MISO" pad="J1.15"/>
<connect gate="G$1" pin="D13/SCK" pad="J2.15"/>
<connect gate="G$1" pin="D2" pad="J1.5"/>
<connect gate="G$1" pin="D3" pad="J1.6"/>
<connect gate="G$1" pin="D4" pad="J1.7"/>
<connect gate="G$1" pin="D5" pad="J1.8"/>
<connect gate="G$1" pin="D6" pad="J1.9"/>
<connect gate="G$1" pin="D7" pad="J1.10"/>
<connect gate="G$1" pin="D8" pad="J1.11"/>
<connect gate="G$1" pin="D9" pad="J1.12"/>
<connect gate="G$1" pin="GND.1" pad="J1.4"/>
<connect gate="G$1" pin="GND.2" pad="J2.2"/>
<connect gate="G$1" pin="ISP_5V" pad="J4.2"/>
<connect gate="G$1" pin="ISP_GND" pad="J4.6"/>
<connect gate="G$1" pin="ISP_MISO" pad="J4.1"/>
<connect gate="G$1" pin="ISP_MOSI" pad="J4.4"/>
<connect gate="G$1" pin="ISP_RST" pad="J4.5"/>
<connect gate="G$1" pin="ISP_SCK" pad="J4.3"/>
<connect gate="G$1" pin="RST.1" pad="J1.3"/>
<connect gate="G$1" pin="RST.2" pad="J2.3"/>
<connect gate="G$1" pin="VIN" pad="J2.1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO-NANO-3.0" prefix="M">
<description>&lt;b&gt;Arduino Nano 3.0&lt;/b&gt; and compatible devices
&lt;p&gt;More details available here:&lt;br&gt;
&lt;a href="https://www.arduino.cc/en/Main/ArduinoBoardNano"&gt;https://www.arduino.cc/en/Main/ArduinoBoardNano&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/arduino+nano"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=ARDUINO-NANO-3.0"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ARDUINO-NANO-3.0"/>
</gates>
<devices>
<device name="" package="ARDUINO-NANO-3.0">
<connects>
<connect gate="G$1" pin="3V3" pad="J2.14"/>
<connect gate="G$1" pin="5V" pad="J2.4"/>
<connect gate="G$1" pin="A0" pad="J2.12"/>
<connect gate="G$1" pin="A1" pad="J2.11"/>
<connect gate="G$1" pin="A2" pad="J2.10"/>
<connect gate="G$1" pin="A3" pad="J2.9"/>
<connect gate="G$1" pin="A4" pad="J2.8"/>
<connect gate="G$1" pin="A5" pad="J2.7"/>
<connect gate="G$1" pin="A6" pad="J2.6"/>
<connect gate="G$1" pin="A7" pad="J2.5"/>
<connect gate="G$1" pin="AREF" pad="J2.13"/>
<connect gate="G$1" pin="D0/RX" pad="J1.2"/>
<connect gate="G$1" pin="D1/TX" pad="J1.1"/>
<connect gate="G$1" pin="D10" pad="J1.13"/>
<connect gate="G$1" pin="D11/MOSI" pad="J1.14"/>
<connect gate="G$1" pin="D12/MISO" pad="J1.15"/>
<connect gate="G$1" pin="D13/SCK" pad="J2.15"/>
<connect gate="G$1" pin="D2" pad="J1.5"/>
<connect gate="G$1" pin="D3" pad="J1.6"/>
<connect gate="G$1" pin="D4" pad="J1.7"/>
<connect gate="G$1" pin="D5" pad="J1.8"/>
<connect gate="G$1" pin="D6" pad="J1.9"/>
<connect gate="G$1" pin="D7" pad="J1.10"/>
<connect gate="G$1" pin="D8" pad="J1.11"/>
<connect gate="G$1" pin="D9" pad="J1.12"/>
<connect gate="G$1" pin="GND.1" pad="J1.4"/>
<connect gate="G$1" pin="GND.2" pad="J2.2"/>
<connect gate="G$1" pin="RST.1" pad="J1.3"/>
<connect gate="G$1" pin="RST.2" pad="J2.3"/>
<connect gate="G$1" pin="VIN" pad="J2.1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO-PRO-MINI-*" prefix="M">
<description>&lt;b&gt;Arduino Pro Mini&lt;/b&gt; and compatible devices
&lt;p&gt;More details available here:&lt;br&gt;
&lt;a href="https://www.arduino.cc/en/Main/ArduinoBoardProMini"&gt;https://www.arduino.cc/en/Main/ArduinoBoardProMini&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/arduino+pro+mini"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=ARDUINO-PRO-MINI-"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ARDUINO-PRO-MINI"/>
</gates>
<devices>
<device name="" package="ARDUINO-PRO-MINI">
<connects>
<connect gate="G$1" pin="A0" pad="J6.8"/>
<connect gate="G$1" pin="A1" pad="J6.7"/>
<connect gate="G$1" pin="A2" pad="J6.6"/>
<connect gate="G$1" pin="A3" pad="J6.5"/>
<connect gate="G$1" pin="A4" pad="J2.1"/>
<connect gate="G$1" pin="A5" pad="J2.2"/>
<connect gate="G$1" pin="A6" pad="J3.2"/>
<connect gate="G$1" pin="A7" pad="J3.3"/>
<connect gate="G$1" pin="D0/RX" pad="J7.11"/>
<connect gate="G$1" pin="D1/TX" pad="J7.12"/>
<connect gate="G$1" pin="D10" pad="J6.12"/>
<connect gate="G$1" pin="D11" pad="J6.11"/>
<connect gate="G$1" pin="D12" pad="J6.10"/>
<connect gate="G$1" pin="D13" pad="J6.9"/>
<connect gate="G$1" pin="D2" pad="J7.8"/>
<connect gate="G$1" pin="D3" pad="J7.7"/>
<connect gate="G$1" pin="D4" pad="J7.6"/>
<connect gate="G$1" pin="D5" pad="J7.5"/>
<connect gate="G$1" pin="D6" pad="J7.4"/>
<connect gate="G$1" pin="D7" pad="J7.3"/>
<connect gate="G$1" pin="D8" pad="J7.2"/>
<connect gate="G$1" pin="D9" pad="J7.1"/>
<connect gate="G$1" pin="GND.1" pad="J7.9"/>
<connect gate="G$1" pin="GND.2" pad="J6.2"/>
<connect gate="G$1" pin="GND.3" pad="J3.1"/>
<connect gate="G$1" pin="P_CTS" pad="J1.2"/>
<connect gate="G$1" pin="P_DTR" pad="J1.6"/>
<connect gate="G$1" pin="P_GND" pad="J1.1"/>
<connect gate="G$1" pin="P_RXD" pad="J1.4"/>
<connect gate="G$1" pin="P_TXD" pad="J1.5"/>
<connect gate="G$1" pin="P_VCC" pad="J1.3"/>
<connect gate="G$1" pin="RAW" pad="J6.1"/>
<connect gate="G$1" pin="RST.1" pad="J7.10"/>
<connect gate="G$1" pin="RST.2" pad="J6.3"/>
<connect gate="G$1" pin="VCC" pad="J6.4"/>
</connects>
<technologies>
<technology name="3.3V"/>
<technology name="5.0V"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO-PRO-MINI-*#NP" prefix="M">
<description>&lt;b&gt;Arduino Pro Mini&lt;/b&gt; (and compatible devices) without programming pads
&lt;p&gt;More details available here:&lt;br&gt;
&lt;a href="https://www.arduino.cc/en/Main/ArduinoBoardProMini"&gt;https://www.arduino.cc/en/Main/ArduinoBoardProMini&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/arduino+pro+mini"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=ARDUINO-PRO-MINI-"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ARDUINO-PRO-MINI#NP"/>
</gates>
<devices>
<device name="" package="ARDUINO-PRO-MINI#NP">
<connects>
<connect gate="G$1" pin="A0" pad="J6.8"/>
<connect gate="G$1" pin="A1" pad="J6.7"/>
<connect gate="G$1" pin="A2" pad="J6.6"/>
<connect gate="G$1" pin="A3" pad="J6.5"/>
<connect gate="G$1" pin="A4" pad="J2.1"/>
<connect gate="G$1" pin="A5" pad="J2.2"/>
<connect gate="G$1" pin="A6" pad="J3.2"/>
<connect gate="G$1" pin="A7" pad="J3.3"/>
<connect gate="G$1" pin="D0/RX" pad="J7.11"/>
<connect gate="G$1" pin="D1/TX" pad="J7.12"/>
<connect gate="G$1" pin="D10" pad="J6.12"/>
<connect gate="G$1" pin="D11" pad="J6.11"/>
<connect gate="G$1" pin="D12" pad="J6.10"/>
<connect gate="G$1" pin="D13" pad="J6.9"/>
<connect gate="G$1" pin="D2" pad="J7.8"/>
<connect gate="G$1" pin="D3" pad="J7.7"/>
<connect gate="G$1" pin="D4" pad="J7.6"/>
<connect gate="G$1" pin="D5" pad="J7.5"/>
<connect gate="G$1" pin="D6" pad="J7.4"/>
<connect gate="G$1" pin="D7" pad="J7.3"/>
<connect gate="G$1" pin="D8" pad="J7.2"/>
<connect gate="G$1" pin="D9" pad="J7.1"/>
<connect gate="G$1" pin="GND.1" pad="J7.9"/>
<connect gate="G$1" pin="GND.2" pad="J6.2"/>
<connect gate="G$1" pin="GND.3" pad="J3.1"/>
<connect gate="G$1" pin="RAW" pad="J6.1"/>
<connect gate="G$1" pin="RST.1" pad="J6.3"/>
<connect gate="G$1" pin="RST.2" pad="J7.10"/>
<connect gate="G$1" pin="VCC" pad="J6.4"/>
</connects>
<technologies>
<technology name="3.3V"/>
<technology name="5.0V"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO-PRO-MINI-*#APC" prefix="M">
<description>&lt;b&gt;Arduino Pro Mini&lt;/b&gt; (and compatible devices) with angle programming connector
&lt;p&gt;More details available here:&lt;br&gt;
&lt;a href="https://www.arduino.cc/en/Main/ArduinoBoardProMini"&gt;https://www.arduino.cc/en/Main/ArduinoBoardProMini&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/arduino+pro+mini"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=ARDUINO-PRO-MINI-"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ARDUINO-PRO-MINI#NP"/>
</gates>
<devices>
<device name="" package="ARDUINO-PRO-MINI#APC">
<connects>
<connect gate="G$1" pin="A0" pad="J6.8"/>
<connect gate="G$1" pin="A1" pad="J6.7"/>
<connect gate="G$1" pin="A2" pad="J6.6"/>
<connect gate="G$1" pin="A3" pad="J6.5"/>
<connect gate="G$1" pin="A4" pad="J2.1"/>
<connect gate="G$1" pin="A5" pad="J2.2"/>
<connect gate="G$1" pin="A6" pad="J3.2"/>
<connect gate="G$1" pin="A7" pad="J3.3"/>
<connect gate="G$1" pin="D0/RX" pad="J7.11"/>
<connect gate="G$1" pin="D1/TX" pad="J7.12"/>
<connect gate="G$1" pin="D10" pad="J6.12"/>
<connect gate="G$1" pin="D11" pad="J6.11"/>
<connect gate="G$1" pin="D12" pad="J6.10"/>
<connect gate="G$1" pin="D13" pad="J6.9"/>
<connect gate="G$1" pin="D2" pad="J7.8"/>
<connect gate="G$1" pin="D3" pad="J7.7"/>
<connect gate="G$1" pin="D4" pad="J7.6"/>
<connect gate="G$1" pin="D5" pad="J7.5"/>
<connect gate="G$1" pin="D6" pad="J7.4"/>
<connect gate="G$1" pin="D7" pad="J7.3"/>
<connect gate="G$1" pin="D8" pad="J7.2"/>
<connect gate="G$1" pin="D9" pad="J7.1"/>
<connect gate="G$1" pin="GND.1" pad="J7.9"/>
<connect gate="G$1" pin="GND.2" pad="J6.2"/>
<connect gate="G$1" pin="GND.3" pad="J3.1"/>
<connect gate="G$1" pin="RAW" pad="J6.1"/>
<connect gate="G$1" pin="RST.1" pad="J7.10"/>
<connect gate="G$1" pin="RST.2" pad="J6.3"/>
<connect gate="G$1" pin="VCC" pad="J6.4"/>
</connects>
<technologies>
<technology name="3.3V"/>
<technology name="5.0V"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ARDUINO-PRO-MINI-*#SMP" prefix="M">
<description>&lt;b&gt;Arduino Pro Mini&lt;/b&gt; (and compatible devices) with 2 connectors only
&lt;p&gt;More details available here:&lt;br&gt;
&lt;a href="https://www.arduino.cc/en/Main/ArduinoBoardProMini"&gt;https://www.arduino.cc/en/Main/ArduinoBoardProMini&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/arduino+pro+mini"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=ARDUINO-PRO-MINI-"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ARDUINO-PRO-MINI#SMP"/>
</gates>
<devices>
<device name="" package="ARDUINO-PRO-MINI#SMP">
<connects>
<connect gate="G$1" pin="A0" pad="J6.8"/>
<connect gate="G$1" pin="A1" pad="J6.7"/>
<connect gate="G$1" pin="A2" pad="J6.6"/>
<connect gate="G$1" pin="A3" pad="J6.5"/>
<connect gate="G$1" pin="D0/RX" pad="J7.11"/>
<connect gate="G$1" pin="D1/TX" pad="J7.12"/>
<connect gate="G$1" pin="D10" pad="J6.12"/>
<connect gate="G$1" pin="D11" pad="J6.11"/>
<connect gate="G$1" pin="D12" pad="J6.10"/>
<connect gate="G$1" pin="D13" pad="J6.9"/>
<connect gate="G$1" pin="D2" pad="J7.8"/>
<connect gate="G$1" pin="D3" pad="J7.7"/>
<connect gate="G$1" pin="D4" pad="J7.6"/>
<connect gate="G$1" pin="D5" pad="J7.5"/>
<connect gate="G$1" pin="D6" pad="J7.4"/>
<connect gate="G$1" pin="D7" pad="J7.3"/>
<connect gate="G$1" pin="D8" pad="J7.2"/>
<connect gate="G$1" pin="D9" pad="J7.1"/>
<connect gate="G$1" pin="GND.1" pad="J7.9"/>
<connect gate="G$1" pin="GND.2" pad="J6.2"/>
<connect gate="G$1" pin="RAW" pad="J6.1"/>
<connect gate="G$1" pin="RST.1" pad="J7.10"/>
<connect gate="G$1" pin="RST.2" pad="J6.3"/>
<connect gate="G$1" pin="VCC" pad="J6.4"/>
</connects>
<technologies>
<technology name="3.3V"/>
<technology name="5.0V"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BATTERY-HOLDER-2AA">
<description>&lt;b&gt;Battery Holder 2 x AA&lt;/b&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/battery+plastic+holder+aa+2x1.5v"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=BATTERY-HOLDER-2AA"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BATTERY-HOLDER-2AA"/>
</gates>
<devices>
<device name="" package="BATTERY-HOLDER-2AA">
<connects>
<connect gate="G$1" pin="BAT+" pad="BAT+"/>
<connect gate="G$1" pin="BAT-" pad="BAT-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DC-DC-STEP-UP-5V-USB" prefix="M">
<description>&lt;b&gt;DC/DC Step-Up Converter&lt;/b&gt; with &lt;b&gt;USB-A&lt;/b&gt; connector based on &lt;b&gt;CE8301&lt;/b&gt; chip
&lt;p&gt;&lt;b&gt;CE8301&lt;/b&gt; datasheet available here:&lt;br /&gt;
&lt;a href="https://www.mpja.com/download/ce830.pdf"&gt;https://www.mpja.com/download/ce830.pdf&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/boost+5v+0.9+usb+pfm"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=DC-DC-STEP-UP-5V-USB"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DC-DC-STEP-UP-5V-USB"/>
</gates>
<devices>
<device name="" package="DC-DC-STEP-UP-5V-USB">
<connects>
<connect gate="G$1" pin="IN+" pad="IN+"/>
<connect gate="G$1" pin="IN-" pad="IN-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISPLAY-NOKIA-3310">
<description>&lt;b&gt;84x48 Dot Matrix LCD Module&lt;/b&gt; based on &lt;b&gt;Nokia 3310&lt;/b&gt; display
&lt;p&gt;More details available here:&lt;br /&gt;
&lt;a href="https://arduinoandsoftware.wordpress.com/2012/12/30/nokia-33105110-3-3v-display-with-5v-arduino/"&gt;https://arduinoandsoftware.wordpress.com/2012/12/30/nokia-33105110-3-3v-display-with-5v-arduino/&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=DISPLAY-NOKIA-3310"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DISPLAY-NOKIA-3310"/>
</gates>
<devices>
<device name="" package="DISPLAY-NOKIA-3310">
<connects>
<connect gate="G$1" pin="D/C.1" pad="J1.5"/>
<connect gate="G$1" pin="D/C.2" pad="J2.5"/>
<connect gate="G$1" pin="DIN.1" pad="J1.6"/>
<connect gate="G$1" pin="DIN.2" pad="J2.6"/>
<connect gate="G$1" pin="GND.1" pad="J1.2"/>
<connect gate="G$1" pin="GND.2" pad="J2.2"/>
<connect gate="G$1" pin="LED.1" pad="J1.8"/>
<connect gate="G$1" pin="LED.2" pad="J2.8"/>
<connect gate="G$1" pin="RST.1" pad="J1.4"/>
<connect gate="G$1" pin="RST.2" pad="J2.4"/>
<connect gate="G$1" pin="SCE.1" pad="J1.3"/>
<connect gate="G$1" pin="SCE.2" pad="J2.3"/>
<connect gate="G$1" pin="SCK.1" pad="J1.7"/>
<connect gate="G$1" pin="SCK.2" pad="J2.7"/>
<connect gate="G$1" pin="VCC.1" pad="J1.1"/>
<connect gate="G$1" pin="VCC.2" pad="J2.1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ETHERNET-ENC28J60" prefix="M">
<description>&lt;b&gt;Ethernet Module&lt;/b&gt; based on &lt;b&gt;ENC28J60&lt;/b&gt; chip
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/end28j60+ethernet+lan+module"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;br /&gt;
&lt;b&gt;Note:&lt;/b&gt; There are many variants. Search for the proper version.&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=ETHERNET-ENC28J60"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ETHERNET-ENC28J60"/>
</gates>
<devices>
<device name="" package="ETHERNET-ENC28J60">
<connects>
<connect gate="G$1" pin="3V3" pad="2"/>
<connect gate="G$1" pin="5V" pad="12"/>
<connect gate="G$1" pin="CLK" pad="9"/>
<connect gate="G$1" pin="CS" pad="3"/>
<connect gate="G$1" pin="GND.1" pad="1"/>
<connect gate="G$1" pin="GND.2" pad="11"/>
<connect gate="G$1" pin="INT" pad="10"/>
<connect gate="G$1" pin="RST" pad="4"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="SI" pad="5"/>
<connect gate="G$1" pin="SO" pad="8"/>
<connect gate="G$1" pin="WOL" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WIRELESS-NRF24L01" prefix="M">
<description>&lt;b&gt;2.4 GHz Wireless Module&lt;/b&gt; based on &lt;b&gt;NRF24L01&lt;/b&gt; chip
&lt;p&gt;More details available here:&lt;br&gt;
&lt;a href="http://www.electrodragon.com/w/NRF24L01"&gt;http://www.electrodragon.com/w/NRF24L01&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/nrf24l01+arduino"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=WIRELESS-NRF24L01"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="WIRELESS-NRF24L01"/>
</gates>
<devices>
<device name="" package="WIRELESS-NRF24L01">
<connects>
<connect gate="G$1" pin="CE" pad="3"/>
<connect gate="G$1" pin="CSN" pad="4"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IRQ" pad="8"/>
<connect gate="G$1" pin="MISO" pad="7"/>
<connect gate="G$1" pin="MOSI" pad="6"/>
<connect gate="G$1" pin="SCK" pad="5"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WIRELESS-XY-FST" prefix="M">
<description>&lt;b&gt;RF Wireless XY-FST Transmitter&lt;/b&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/xd+fst+transmitter"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;br /&gt;
&lt;b&gt;Note:&lt;/b&gt; Sold together with receiver.&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=WIRELESS-XY-FST"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="WIRELESS-XY-FST"/>
</gates>
<devices>
<device name="" package="WIRELESS-XY-FST">
<connects>
<connect gate="G$1" pin="ANT" pad="ANT"/>
<connect gate="G$1" pin="ATAD" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WIRELESS-XY-FST#V" prefix="M">
<description>&lt;b&gt;RF Wireless XY-FST Transmitter&lt;/b&gt; vertically mounted
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/xd+fst+transmitter"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;br /&gt;
&lt;b&gt;Note:&lt;/b&gt; Sold together with receiver.&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=WIRELESS-XY-FST"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="WIRELESS-XY-FST#V"/>
</gates>
<devices>
<device name="" package="WIRELESS-XY-FST#V">
<connects>
<connect gate="G$1" pin="ATAD" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WIRELESS-XY-MK-5V" prefix="M">
<description>&lt;b&gt;RF Wireless XY-MK-5V Receiver&lt;/b&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/xd+rf+5v-receiver"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;br /&gt;
&lt;b&gt;Note:&lt;/b&gt; Sold together with transmitter.&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=WIRELESS-XY-MK-5V"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="WIRELESS-XY-MK-5V"/>
</gates>
<devices>
<device name="" package="WIRELESS-XY-MK-5V">
<connects>
<connect gate="G$1" pin="ANT" pad="ANT"/>
<connect gate="G$1" pin="DATA.1" pad="2"/>
<connect gate="G$1" pin="DATA.2" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-V" package="WIRELESS-XY-MK-5V#V">
<connects>
<connect gate="G$1" pin="ANT" pad="ANT"/>
<connect gate="G$1" pin="DATA.1" pad="2"/>
<connect gate="G$1" pin="DATA.2" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC-DAC-PCF8591">
<description>&lt;b&gt;4-Channel ADC and 1-Channel DAC Module&lt;/b&gt; based on &lt;b&gt;PCF8591&lt;/b&gt; chip
&lt;p&gt;More details available here:&lt;br&gt;
&lt;a href="https://brainfyre.wordpress.com/2012/10/25/pcf8591-yl-40-ad-da-module-review/"&gt;
https://brainfyre.wordpress.com/2012/10/25/pcf8591-yl-40-ad-da-module-review/&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/pcf8591+arduino"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=ADC-DAC-PCF8591"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ADC-DAC-PCF8591"/>
</gates>
<devices>
<device name="" package="ADC-DAC-PCF8591">
<connects>
<connect gate="G$1" pin="AIN0" pad="J1.2"/>
<connect gate="G$1" pin="AIN1" pad="J1.3"/>
<connect gate="G$1" pin="AIN2" pad="J1.4"/>
<connect gate="G$1" pin="AIN3" pad="J1.5"/>
<connect gate="G$1" pin="AOUT" pad="J1.1"/>
<connect gate="G$1" pin="GND" pad="J2.3"/>
<connect gate="G$1" pin="SCL" pad="J2.1"/>
<connect gate="G$1" pin="SDA" pad="J2.2"/>
<connect gate="G$1" pin="VCC" pad="J2.4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AMPLIFIER-PAM8403">
<description>&lt;b&gt;Stereo Class-D 3W Audio Amplifier&lt;/b&gt; based on &lt;b&gt;PAM8403&lt;/b&gt; chip
&lt;p&gt;More details available here:&lt;br&gt;
&lt;a href="http://artofcircuits.com/product/pam8403-5v-two-channel-stereo-mini-class-d-3w3w-audio-amplifier"&gt;
http://artofcircuits.com/product/pam8403-5v-two-channel-stereo-mini-class-d-3w3w-audio-amplifier&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/pam8403+mini+class+d"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=AMPLIFIER-PAM8403"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="AMPLIFIER-PAM8403"/>
</gates>
<devices>
<device name="" package="AMPLIFIER-PAM8403">
<connects>
<connect gate="G$1" pin="+5V" pad="+5V"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="IN.COM" pad="IN.COM"/>
<connect gate="G$1" pin="IN.L" pad="IN.L"/>
<connect gate="G$1" pin="IN.R" pad="IN.R"/>
<connect gate="G$1" pin="OUT.L+" pad="OUT.L+"/>
<connect gate="G$1" pin="OUT.L-" pad="OUT.L-"/>
<connect gate="G$1" pin="OUT.R+" pad="OUT.R+"/>
<connect gate="G$1" pin="OUT.R-" pad="OUT.R-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BREADBOARD-POWER-V1" uservalue="yes">
<description>&lt;b&gt;Breadboard Power Adapter&lt;/b&gt; with onboard 3.3V and 5V regulators
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=BREADBOARD-POWER-V1"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BREADBOARD-POWER-V1"/>
<gate name="G$2" symbol="BREADBOARD-POWER-V1"/>
</gates>
<devices>
<device name="" package="BREADBOARD-POWER-V1">
<connects>
<connect gate="G$1" pin="M.1" pad="A.M.1"/>
<connect gate="G$1" pin="M.2" pad="A.M.2"/>
<connect gate="G$1" pin="M.3" pad="A.M.3"/>
<connect gate="G$1" pin="M.4" pad="A.M.4"/>
<connect gate="G$1" pin="M.5" pad="A.M.5"/>
<connect gate="G$1" pin="P.1" pad="A.P.1"/>
<connect gate="G$1" pin="P.2" pad="A.P.2"/>
<connect gate="G$1" pin="P.3" pad="A.P.3"/>
<connect gate="G$1" pin="P.4" pad="A.P.4"/>
<connect gate="G$1" pin="P.5" pad="A.P.5"/>
<connect gate="G$2" pin="M.1" pad="B.M.1"/>
<connect gate="G$2" pin="M.2" pad="B.M.2"/>
<connect gate="G$2" pin="M.3" pad="B.M.3"/>
<connect gate="G$2" pin="M.4" pad="B.M.4"/>
<connect gate="G$2" pin="M.5" pad="B.M.5"/>
<connect gate="G$2" pin="P.1" pad="B.P.1"/>
<connect gate="G$2" pin="P.2" pad="B.P.2"/>
<connect gate="G$2" pin="P.3" pad="B.P.3"/>
<connect gate="G$2" pin="P.4" pad="B.P.4"/>
<connect gate="G$2" pin="P.5" pad="B.P.5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CARD-SD-ADAPTER">
<description>&lt;b&gt;Full Size SD Card Adapter Module&lt;/b&gt; with onboard 3.3V regulator
&lt;p&gt;Guide describing how to use SD card with Arduino is available here:&lt;br /&gt;
&lt;a href="https://www.arduino.cc/en/Reference/SDCardNotes"&gt;https://www.arduino.cc/en/Reference/SDCardNotes&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/sd+card+socket+module"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=CARD-SD-ADAPTER"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CARD-SD-ADAPTER"/>
</gates>
<devices>
<device name="" package="CARD-SD-ADAPTER">
<connects>
<connect gate="G$1" pin="3V3" pad="3"/>
<connect gate="G$1" pin="5V" pad="5"/>
<connect gate="G$1" pin="CS" pad="7"/>
<connect gate="G$1" pin="GND.1" pad="1"/>
<connect gate="G$1" pin="GND.2" pad="15"/>
<connect gate="G$1" pin="MISO" pad="13"/>
<connect gate="G$1" pin="MOSI" pad="9"/>
<connect gate="G$1" pin="SCK" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="COMPASS-HMC5883L" uservalue="yes">
<description>&lt;b&gt;3-Axis Digital Compass Module&lt;/b&gt; based on &lt;b&gt;HMC5883L&lt;/b&gt; chip
&lt;p&gt;More details available here:&lt;br&gt;
&lt;a href="http://www.electrodragon.com/w/HMC"&gt;http://www.electrodragon.com/w/HMC&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/gy+271+hmc5883+ module"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=COMPASS-HMC5883L"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="COMPASS-HMC5883L"/>
</gates>
<devices>
<device name="" package="COMPASS-HMC5883L">
<connects>
<connect gate="G$1" pin="DRDY" pad="5"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SCL" pad="3"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CURRENT-SENSOR-ACS712">
<description>&lt;b&gt;Isolated Bipolar Current Sensors&lt;/b&gt; based on &lt;b&gt;ACS712&lt;/b&gt; chip
&lt;p&gt;More details available here:&lt;br&gt;
&lt;a href="http://embedded-lab.com/blog/a-brief-overview-of-allegro-acs712-current-sensor-part-1/"&gt;
http://embedded-lab.com/blog/a-brief-overview-of-allegro-acs712-current-sensor-part-1/&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/acs712+module "&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;br /&gt;
&lt;b&gt;Note:&lt;/b&gt; There are many available versions with different pinout. Please check before use&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=CURRENT-SENSOR-ACS712"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CURRENT-SENSOR-ACS712"/>
</gates>
<devices>
<device name="" package="CURRENT-SENSOR-ACS712">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CURRENT-SENSOR-ACS712#IC">
<description>&lt;b&gt;Isolated Bipolar Current Sensors&lt;/b&gt; based on &lt;b&gt;ACS712&lt;/b&gt; chip&lt;br&gt;
Symbol with input pins
&lt;p&gt;More details available here:&lt;br&gt;
&lt;a href="http://embedded-lab.com/blog/a-brief-overview-of-allegro-acs712-current-sensor-part-1/"&gt;
http://embedded-lab.com/blog/a-brief-overview-of-allegro-acs712-current-sensor-part-1/&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/acs712+module "&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;br /&gt;
&lt;b&gt;Note:&lt;/b&gt; There are many available versions with different pinout. Please check before use&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=CURRENT-SENSOR-ACS712"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CURRENT-SENSOR-ACS712#IC"/>
</gates>
<devices>
<device name="" package="CURRENT-SENSOR-ACS712#IC">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN+" pad="P1.1"/>
<connect gate="G$1" pin="IN-" pad="P1.2"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DC-DC-STEP-DOWN-LM2596">
<description>&lt;b&gt;DC/DC Step-Down Regulator&lt;/b&gt; based on &lt;b&gt;LM2596-ADJ&lt;/b&gt; chip
&lt;p&gt;&lt;b&gt;LM2596&lt;/b&gt; datasheet available here:&lt;br /&gt;&lt;a href="http://www.ti.com/lit/ds/symlink/lm2596.pdf"&gt;http://www.ti.com/lit/ds/symlink/lm2596.pdf&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/lm2596+power+regulator"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=DC-DC-STEP-DOWN-LM2596"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DC-DC-STEP-DOWN-LM2596"/>
</gates>
<devices>
<device name="" package="DC-DC-STEP-DOWN-LM2596">
<connects>
<connect gate="G$1" pin="IN+" pad="IN+"/>
<connect gate="G$1" pin="IN-" pad="IN-"/>
<connect gate="G$1" pin="OUT+" pad="OUT+"/>
<connect gate="G$1" pin="OUT-" pad="OUT-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DRIVER-ULN2003">
<description>&lt;b&gt;7-Channel Darlington NPN Transistor Module&lt;/b&gt; based on &lt;b&gt;ULN2003&lt;/b&gt; chip
&lt;p&gt;More details available here:&lt;br /&gt;&lt;a href="https://www.elecrow.com/wiki/index.php?title=ULN2003_Stepper_Motor_Driver"&gt;https://www.elecrow.com/wiki/index.php?title=ULN2003_Stepper_Motor_Driver&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;ULN2003&lt;/b&gt; datasheet available here:&lt;br /&gt;
&lt;a href="http://www.ti.com/lit/ds/slrs027o/slrs027o.pdf"&gt;http://www.ti.com/lit/ds/slrs027o/slrs027o.pdf&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/uln2003+stepper+driver+module"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;br /&gt;
&lt;b&gt;Note:&lt;/b&gt; There are many variants. Search for the proper version.&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=DRIVER-ULN2003"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DRIVER-ULN2003"/>
</gates>
<devices>
<device name="" package="DRIVER-ULN2003">
<connects>
<connect gate="G$1" pin="GND" pad="J3.1"/>
<connect gate="G$1" pin="IN.1" pad="J1.1"/>
<connect gate="G$1" pin="IN.2" pad="J1.2"/>
<connect gate="G$1" pin="IN.3" pad="J1.3"/>
<connect gate="G$1" pin="IN.4" pad="J1.4"/>
<connect gate="G$1" pin="IN.5" pad="J1.5"/>
<connect gate="G$1" pin="IN.6" pad="J1.6"/>
<connect gate="G$1" pin="IN.7" pad="J1.7"/>
<connect gate="G$1" pin="MOT+" pad="J3.4"/>
<connect gate="G$1" pin="OUT.A" pad="J2.1"/>
<connect gate="G$1" pin="OUT.B" pad="J2.2"/>
<connect gate="G$1" pin="OUT.C" pad="J2.3"/>
<connect gate="G$1" pin="OUT.D" pad="J2.4"/>
<connect gate="G$1" pin="OUT.E" pad="J2.5"/>
<connect gate="G$1" pin="OUT.F" pad="J2.6"/>
<connect gate="G$1" pin="OUT.G" pad="J2.7"/>
<connect gate="G$1" pin="VCC.1" pad="J3.2"/>
<connect gate="G$1" pin="VCC.2" pad="J3.3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DRIVER-ULN2003#MC">
<description>&lt;b&gt;7-Channel Darlington NPN Transistor Module&lt;/b&gt; based on &lt;b&gt;ULN2003&lt;/b&gt; chip&lt;br&gt;
Symbol with motor connector pins
&lt;p&gt;More details available here:&lt;br /&gt;&lt;a href="https://www.elecrow.com/wiki/index.php?title=ULN2003_Stepper_Motor_Driver"&gt;https://www.elecrow.com/wiki/index.php?title=ULN2003_Stepper_Motor_Driver&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;ULN2003&lt;/b&gt; datasheet available here:&lt;br /&gt;
&lt;a href="http://www.ti.com/lit/ds/slrs027o/slrs027o.pdf"&gt;http://www.ti.com/lit/ds/slrs027o/slrs027o.pdf&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/uln2003+stepper+driver+module"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;br /&gt;
&lt;b&gt;Note:&lt;/b&gt; There are many variants. Search for the proper version.&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=DRIVER-ULN2003"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DRIVER-ULN2003#MC"/>
</gates>
<devices>
<device name="" package="DRIVER-ULN2003#MC">
<connects>
<connect gate="G$1" pin="GND" pad="J3.1"/>
<connect gate="G$1" pin="IN.1" pad="J1.1"/>
<connect gate="G$1" pin="IN.2" pad="J1.2"/>
<connect gate="G$1" pin="IN.3" pad="J1.3"/>
<connect gate="G$1" pin="IN.4" pad="J1.4"/>
<connect gate="G$1" pin="IN.5" pad="J1.5"/>
<connect gate="G$1" pin="IN.6" pad="J1.6"/>
<connect gate="G$1" pin="IN.7" pad="J1.7"/>
<connect gate="G$1" pin="MOT+" pad="J3.4"/>
<connect gate="G$1" pin="MOT.+" pad="P3.5"/>
<connect gate="G$1" pin="MOT.A" pad="P3.4"/>
<connect gate="G$1" pin="MOT.B" pad="P3.3"/>
<connect gate="G$1" pin="MOT.C" pad="P3.2"/>
<connect gate="G$1" pin="MOT.D" pad="P3.1"/>
<connect gate="G$1" pin="OUT.A" pad="J2.1"/>
<connect gate="G$1" pin="OUT.B" pad="J2.2"/>
<connect gate="G$1" pin="OUT.C" pad="J2.3"/>
<connect gate="G$1" pin="OUT.D" pad="J2.4"/>
<connect gate="G$1" pin="OUT.E" pad="J2.5"/>
<connect gate="G$1" pin="OUT.F" pad="J2.6"/>
<connect gate="G$1" pin="OUT.G" pad="J2.7"/>
<connect gate="G$1" pin="VCC.1" pad="J3.2"/>
<connect gate="G$1" pin="VCC.2" pad="J3.3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LCD-I2C-CONVERTER">
<description>&lt;b&gt;I2C Bus to 4-Bit Parallel LCD Interface&lt;/b&gt; with LED backlight driver
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=LCD-I2C-CONVERTER"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LCD-I2C-CONVERTER"/>
</gates>
<devices>
<device name="" package="LCD-I2C-CONVERTER">
<connects>
<connect gate="G$1" pin="DB0" pad="J2.7"/>
<connect gate="G$1" pin="DB1" pad="J2.8"/>
<connect gate="G$1" pin="DB2" pad="J2.9"/>
<connect gate="G$1" pin="DB3" pad="J2.10"/>
<connect gate="G$1" pin="DB4" pad="J2.11"/>
<connect gate="G$1" pin="DB5" pad="J2.12"/>
<connect gate="G$1" pin="DB6" pad="J2.13"/>
<connect gate="G$1" pin="DB7" pad="J2.14"/>
<connect gate="G$1" pin="EN" pad="J2.6"/>
<connect gate="G$1" pin="GND" pad="J1.4"/>
<connect gate="G$1" pin="LED.A" pad="J2.15"/>
<connect gate="G$1" pin="LED.K" pad="J2.16"/>
<connect gate="G$1" pin="R/W" pad="J2.5"/>
<connect gate="G$1" pin="RS" pad="J2.4"/>
<connect gate="G$1" pin="SCL" pad="J1.3"/>
<connect gate="G$1" pin="SDA" pad="J1.2"/>
<connect gate="G$1" pin="VCC" pad="J1.1"/>
<connect gate="G$1" pin="VDD" pad="J2.2"/>
<connect gate="G$1" pin="VEE" pad="J2.3"/>
<connect gate="G$1" pin="VSS" pad="J2.1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LIGHT-DETECTOR">
<description>&lt;b&gt;Light Detection Module&lt;/b&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=LIGHT-DETECTOR"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LIGHT-DETECTOR"/>
</gates>
<devices>
<device name="" package="LIGHT-DETECTOR">
<connects>
<connect gate="G$1" pin="5V" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOTION-PIR-DYP-ME003">
<description>&lt;b&gt;PIR Motion Sensor Module DYP-ME003&lt;/b&gt; based on &lt;b&gt;BISS0001&lt;/b&gt; pyroelectic detector
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/dyp+me003"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=MOTION-PIR-DYP-ME003"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MOTION-PIR-DYP-ME003"/>
</gates>
<devices>
<device name="" package="MOTION-PIR-DYP-ME003">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="REG-AMS1117-*">
<description>&lt;b&gt;Linear Regulator&lt;/b&gt; based on &lt;b&gt;AMS1117&lt;/b&gt; chip
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=REG-AMS1117-"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="REG-AMS1117"/>
</gates>
<devices>
<device name="" package="REG-AMS1117">
<connects>
<connect gate="G$1" pin="GND.I" pad="J1.2"/>
<connect gate="G$1" pin="GND.O" pad="J2.2"/>
<connect gate="G$1" pin="VIN" pad="J1.1"/>
<connect gate="G$1" pin="VOUT" pad="J2.1"/>
</connects>
<technologies>
<technology name="3.3V"/>
<technology name="5.0V"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RELAY-2-SRD#RC">
<description>&lt;b&gt;2-Channel Relay Module&lt;/b&gt; based on &lt;b&gt;SRD-05VDC-SL-C&lt;/b&gt; relays&lt;br&gt;
Symbol with relays pins
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/two+channel+relay+module+optocoupler+5v"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=RELAY-2-SRD"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RELAY-2-SRD#RC"/>
</gates>
<devices>
<device name="" package="RELAY-2-SRD#RC">
<connects>
<connect gate="G$1" pin="GND.1" pad="J1.4"/>
<connect gate="G$1" pin="GND.2" pad="J2.3"/>
<connect gate="G$1" pin="IN1" pad="J1.3"/>
<connect gate="G$1" pin="IN2" pad="J1.2"/>
<connect gate="G$1" pin="JD-VCC" pad="J2.1"/>
<connect gate="G$1" pin="REL.1.COM" pad="P1.5"/>
<connect gate="G$1" pin="REL.1.NC" pad="P1.6"/>
<connect gate="G$1" pin="REL.1.NO" pad="P1.4"/>
<connect gate="G$1" pin="REL.2.COM" pad="P1.2"/>
<connect gate="G$1" pin="REL.2.NC" pad="P1.3"/>
<connect gate="G$1" pin="REL.2.NO" pad="P1.1"/>
<connect gate="G$1" pin="VCC.1" pad="J1.1"/>
<connect gate="G$1" pin="VCC.2" pad="J2.2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RELAY-2-SRD">
<description>&lt;b&gt;2-Channel Relay Module&lt;/b&gt; based on &lt;b&gt;SRD-05VDC-SL-C&lt;/b&gt; relays
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/two+channel+relay+module+optocoupler+5v"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=RELAY-2-SRD"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RELAY-2-SRD"/>
</gates>
<devices>
<device name="" package="RELAY-2-SRD">
<connects>
<connect gate="G$1" pin="GND.1" pad="J1.4"/>
<connect gate="G$1" pin="GND.2" pad="J2.3"/>
<connect gate="G$1" pin="IN1" pad="J1.3"/>
<connect gate="G$1" pin="IN2" pad="J1.2"/>
<connect gate="G$1" pin="JD-VCC" pad="J2.1"/>
<connect gate="G$1" pin="VCC.1" pad="J1.1"/>
<connect gate="G$1" pin="VCC.2" pad="J2.2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RTC-EEPROM-BATTERY">
<description>&lt;b&gt;RTC Module with Battery and EEPROM&lt;/b&gt; based on &lt;b&gt;DS1307&lt;/b&gt; and &lt;b&gt;AT24C32&lt;/b&gt; chips
&lt;p&gt;More details available here:&lt;br&gt;&lt;a href="http://henrysbench.capnfatz.com/henrys-bench/arduino-sensors-and-input/arduino-tiny-rtc-d1307-tutorial/"&gt;
http://henrysbench.capnfatz.com/henrys-bench/arduino-sensors-and-input/arduino-tiny-rtc-d1307-tutorial/&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/tiny+rtc+arduino"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=RTC-EEPROM-BATTERY"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RTC-EEPROM-BATTERY"/>
</gates>
<devices>
<device name="" package="RTC-EEPROM-BATTERY">
<connects>
<connect gate="G$1" pin="BAT" pad="J2.1"/>
<connect gate="G$1" pin="DS.1" pad="J1.5"/>
<connect gate="G$1" pin="DS.2" pad="J2.6"/>
<connect gate="G$1" pin="GND.1" pad="J1.1"/>
<connect gate="G$1" pin="GND.2" pad="J2.2"/>
<connect gate="G$1" pin="SCL.1" pad="J1.4"/>
<connect gate="G$1" pin="SCL.2" pad="J2.5"/>
<connect gate="G$1" pin="SDA.1" pad="J1.3"/>
<connect gate="G$1" pin="SDA.2" pad="J2.4"/>
<connect gate="G$1" pin="SQ" pad="J2.7"/>
<connect gate="G$1" pin="VCC.1" pad="J1.2"/>
<connect gate="G$1" pin="VCC.2" pad="J2.3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOIL-MOISTURE-SENSOR">
<description>&lt;b&gt;Soil Moisture Sensor&lt;/b&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/soil+moisture+sensor+arduino"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=SOIL-MOISTURE-SENSOR"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SOIL-MOISTURE-SENSOR"/>
</gates>
<devices>
<device name="" package="SOIL-MOISTURE-SENSOR">
<connects>
<connect gate="G$1" pin="A0" pad="J1.1"/>
<connect gate="G$1" pin="DO" pad="J1.2"/>
<connect gate="G$1" pin="GND" pad="J1.3"/>
<connect gate="G$1" pin="SENS.1" pad="J2.1"/>
<connect gate="G$1" pin="SENS.2" pad="J2.2"/>
<connect gate="G$1" pin="VCC" pad="J1.4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOUND-DETECTOR">
<description>&lt;b&gt;Sound Detection Module&lt;/b&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=SOUND-DETECTOR"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SOUND-DETECTOR"/>
</gates>
<devices>
<device name="" package="SOUND-DETECTOR">
<connects>
<connect gate="G$1" pin="+5V" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ULTRASONIC-HC-SR04">
<description>&lt;b&gt;Ultrasonic Ranging Module HC-SR04&lt;/b&gt;
&lt;p&gt;More details available here:&lt;br&gt;
&lt;a href="http://randomnerdtutorials.com/complete-guide-for-ultrasonic-sensor-hc-sr04/"&gt;
http://randomnerdtutorials.com/complete-guide-for-ultrasonic-sensor-hc-sr04/&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/hc+sr04+ultrasonic"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=ULTRASONIC-HC-SR04"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ULTRASONIC-HC-SR04"/>
</gates>
<devices>
<device name="" package="ULTRASONIC-HC-SR04">
<connects>
<connect gate="G$1" pin="ECHO" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="TRIG" pad="2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="#V" package="ULTRASONIC-HC-SR04#V">
<connects>
<connect gate="G$1" pin="ECHO" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="TRIG" pad="2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WIRELESS-WIFI-ESP-01">
<description>&lt;b&gt;Wireless Wi-Fi ESP-01 Module&lt;/b&gt; based on &lt;b&gt;ESP8266&lt;/b&gt; chip
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/esp8266+esp+01+transceiver"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=WIRELESS-WIFI-ESP-01"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="WIRELESS-WIFI-ESP-01"/>
</gates>
<devices>
<device name="" package="WIRELESS-WIFI-ESP-01">
<connects>
<connect gate="G$1" pin="CH_PD" pad="B2"/>
<connect gate="G$1" pin="GND" pad="A1"/>
<connect gate="G$1" pin="GPIO0" pad="C1"/>
<connect gate="G$1" pin="GPIO2" pad="B1"/>
<connect gate="G$1" pin="RST" pad="C2"/>
<connect gate="G$1" pin="URXD" pad="D1"/>
<connect gate="G$1" pin="UTXD" pad="A2"/>
<connect gate="G$1" pin="VCC" pad="D2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DC-DC-STEP-UP-5V">
<description>&lt;b&gt;DC/DC Step-Up Converter&lt;/b&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=DC-DC-STEP-UP-5V"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DC-DC-STEP-UP-5V"/>
</gates>
<devices>
<device name="" package="DC-DC-STEP-UP-5V">
<connects>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="IN+" pad="IN+"/>
<connect gate="G$1" pin="IN-" pad="IN-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WIRELESS-NRF24L01-PA-EXT" prefix="M">
<description>&lt;b&gt;2.4 GHz Wireless Module&lt;/b&gt; based on &lt;b&gt;NRF24L01&lt;/b&gt; chip with preamplifier and external antenna
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/nrf24l01+pa+lna+sma"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=WIRELESS-NRF24L01-PA-EXT"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="WIRELESS-NRF24L01-PA-EXT"/>
</gates>
<devices>
<device name="" package="WIRELESS-NRF24L01-PA-EXT">
<connects>
<connect gate="G$1" pin="CE" pad="3"/>
<connect gate="G$1" pin="CSN" pad="4"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IRQ" pad="8"/>
<connect gate="G$1" pin="MISO" pad="7"/>
<connect gate="G$1" pin="MOSI" pad="6"/>
<connect gate="G$1" pin="SCK" pad="5"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AC-DC-3.5W">
<description>&lt;b&gt;AC/DC 3.5W Converter&lt;/b&gt;
&lt;p&gt;More details available here:&lt;br&gt;
&lt;a href="https://www.itead.cc/wiki/AC-DC_Power_Module_5V_700mA"&gt;https://www.itead.cc/wiki/AC-DC_Power_Module_5V_700mA&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/ac+dc+3.5w+buck+step"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=AC-DC-3.5W"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="AC-DC-3.5W"/>
</gates>
<devices>
<device name="" package="AC-DC-3.5W">
<connects>
<connect gate="G$1" pin="5V" pad="J2.2"/>
<connect gate="G$1" pin="AC1" pad="J1.1"/>
<connect gate="G$1" pin="AC2" pad="J1.2"/>
<connect gate="G$1" pin="OUT+" pad="J2.3"/>
<connect gate="G$1" pin="OUT-" pad="J2.1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BATTERY-CHARGER-LI-5V">
<description>&lt;b&gt;Lithium Battery 5V Charger&lt;/b&gt;
&lt;p&gt;More details available here:&lt;br&gt;
&lt;a href="http://www.buildcircuit.com/how-to-use-micro-usb-5v-1a-lithium-battery-charging-board-charger-module/"&gt;
http://www.buildcircuit.com/how-to-use-micro-usb-5v-1a-lithium-battery-charging-board-charger-module/&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/tp4056+charger+usb"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=BATTERY-CHARGER-LI-5V"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BATTERY-CHARGER-LI-5V"/>
</gates>
<devices>
<device name="" package="BATTERY-CHARGER-LI-5V">
<connects>
<connect gate="G$1" pin="BAT+" pad="BAT+"/>
<connect gate="G$1" pin="BAT-" pad="BAT-"/>
<connect gate="G$1" pin="IN+" pad="IN+"/>
<connect gate="G$1" pin="IN-" pad="IN-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FLAME-DETECTOR">
<description>&lt;b&gt;Flame Detector&lt;/b&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/flame+detector+arduino"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=FLAME-DETECTOR"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="FLAME-DETECTOR"/>
</gates>
<devices>
<device name="" package="FLAME-DETECTOR">
<connects>
<connect gate="G$1" pin="AO" pad="4"/>
<connect gate="G$1" pin="DO" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR-RECEIVER">
<description>&lt;b&gt;IR Receiver Module&lt;/b&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=IR-RECEIVER"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="IR-RECEIVER"/>
</gates>
<devices>
<device name="" package="IR-RECEIVER">
<connects>
<connect gate="G$1" pin="GND" pad="C.2"/>
<connect gate="G$1" pin="GND.1" pad="A.2"/>
<connect gate="G$1" pin="GND.2" pad="B.2"/>
<connect gate="G$1" pin="IN" pad="C.1"/>
<connect gate="G$1" pin="IN.1" pad="A.3"/>
<connect gate="G$1" pin="IN.2" pad="B.3"/>
<connect gate="G$1" pin="VCC" pad="C.3"/>
<connect gate="G$1" pin="VCC.1" pad="A.1"/>
<connect gate="G$1" pin="VCC.2" pad="B.1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IR-RECEIVER#NC">
<description>&lt;b&gt;IR Receiver Module&lt;/b&gt; without IR sensor connector
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=IR-RECEIVER"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="IR-RECEIVER#NC"/>
</gates>
<devices>
<device name="" package="IR-RECEIVER#NC">
<connects>
<connect gate="G$1" pin="GND.1" pad="A.2"/>
<connect gate="G$1" pin="GND.2" pad="B.2"/>
<connect gate="G$1" pin="IN.1" pad="A.3"/>
<connect gate="G$1" pin="IN.2" pad="B.3"/>
<connect gate="G$1" pin="VCC.1" pad="A.1"/>
<connect gate="G$1" pin="VCC.2" pad="B.1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STEPPER-MOTOR-EASY-DRIVER">
<description>&lt;b&gt;Stepper Motor Easy Driver&lt;/b&gt;
&lt;p&gt;Project page: &lt;a href="http://www.schmalzhaus.com/EasyDriver/"&gt;http://www.schmalzhaus.com/EasyDriver/&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/easydriver+stepper+motor+driver"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=STEPPER-MOTOR-EASY-DRIVER"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="STEPPER-MOTOR-EASY-DRIVER"/>
</gates>
<devices>
<device name="" package="STEPPER-MOTOR-EASY-DRIVER">
<connects>
<connect gate="G$1" pin="+5V" pad="JP4.1"/>
<connect gate="G$1" pin="A.1" pad="JP3.1"/>
<connect gate="G$1" pin="A.2" pad="JP3.2"/>
<connect gate="G$1" pin="B.1" pad="JP3.3"/>
<connect gate="G$1" pin="B.2" pad="JP3.4"/>
<connect gate="G$1" pin="DIR" pad="JP2.3"/>
<connect gate="G$1" pin="ENA" pad="JP6.1"/>
<connect gate="G$1" pin="GND" pad="JP1.1"/>
<connect gate="G$1" pin="GND.1" pad="JP4.2"/>
<connect gate="G$1" pin="GND.2" pad="JP2.1"/>
<connect gate="G$1" pin="M+" pad="JP1.2"/>
<connect gate="G$1" pin="MS1" pad="JP5.1"/>
<connect gate="G$1" pin="MS2" pad="JP6.2"/>
<connect gate="G$1" pin="PFD" pad="JP7.1"/>
<connect gate="G$1" pin="RST" pad="JP7.2"/>
<connect gate="G$1" pin="SLP" pad="JP5.2"/>
<connect gate="G$1" pin="STER" pad="JP2.2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RS485-TTL-CONVERTER">
<description>&lt;b&gt;RS485 to TTL converter&lt;/b&gt; based on &lt;b&gt;MAX485&lt;/b&gt; chip
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=RS485-TTL-CONVERTER"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RS485-TTL-CONVERTER"/>
</gates>
<devices>
<device name="" package="RS485-TTL-CONVERTER">
<connects>
<connect gate="G$1" pin="A" pad="J2.3"/>
<connect gate="G$1" pin="B" pad="J2.2"/>
<connect gate="G$1" pin="DE" pad="J1.2"/>
<connect gate="G$1" pin="DI" pad="J1.1"/>
<connect gate="G$1" pin="GND" pad="J2.4"/>
<connect gate="G$1" pin="RE" pad="J1.3"/>
<connect gate="G$1" pin="RO" pad="J1.4"/>
<connect gate="G$1" pin="VCC" pad="J2.1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TOUCH-KEYPAD-4X4">
<description>&lt;b&gt;16 Channel Capacitive Touch Keypad&lt;/b&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/ttp229+16+channel+digital+capacitive+touch+sensor"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=TOUCH-KEYPAD-4X4"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TOUCH-KEYPAD-4X4"/>
</gates>
<devices>
<device name="" package="TOUCH-KEYPAD-4X4">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT1" pad="5"/>
<connect gate="G$1" pin="OUT2" pad="6"/>
<connect gate="G$1" pin="OUT3" pad="7"/>
<connect gate="G$1" pin="OUT4" pad="8"/>
<connect gate="G$1" pin="OUT5" pad="9"/>
<connect gate="G$1" pin="OUT6" pad="10"/>
<connect gate="G$1" pin="OUT7" pad="11"/>
<connect gate="G$1" pin="OUT8" pad="12"/>
<connect gate="G$1" pin="SCL" pad="3"/>
<connect gate="G$1" pin="SDO" pad="4"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOUND-BUZZER">
<description>&lt;b&gt;Sound Buzzer Module&lt;/b&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/passive+buzzer+beep+module"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=SOUND-BUZZER"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SOUND-BUZZER"/>
</gates>
<devices>
<device name="" package="SOUND-BUZZER">
<connects>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GSM-MODEM-SIM900A">
<description>&lt;b&gt;GSM Mini Module&lt;/b&gt; based on &lt;b&gt;SIM900A&lt;/b&gt;
&lt;p&gt;Schematic available here:&lt;br /&gt;&lt;a href="http://www.electrodragon.com/w/SIM900_(SIM900A)_Mini_DEV_Board"&gt;http://www.electrodragon.com/w/SIM900_(SIM900A)_Mini_DEV_Board&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=GSM-MODEM-SIM900A"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="GSM-MODEM-SIM900A"/>
</gates>
<devices>
<device name="" package="GSM-MODEM-SIM900A">
<connects>
<connect gate="G$1" pin="GND.1" pad="J1.2"/>
<connect gate="G$1" pin="GND.2" pad="J1.7"/>
<connect gate="G$1" pin="RST" pad="J1.8"/>
<connect gate="G$1" pin="SIMR" pad="J1.5"/>
<connect gate="G$1" pin="SIMT" pad="J1.6"/>
<connect gate="G$1" pin="VCC4" pad="J1.3"/>
<connect gate="G$1" pin="VCC5" pad="J1.1"/>
<connect gate="G$1" pin="VCCMCU" pad="J1.4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-24XRGB-RING">
<description>&lt;b&gt;24 LEDs RGB Ring&lt;/b&gt; based on &lt;b&gt;WS2812B&lt;/b&gt;
&lt;p&gt;More details about controlling &lt;b&gt;WS2812B&lt;/b&gt; RGB LEDs are available here:&lt;br&gt;
&lt;a href="https://learn.sparkfun.com/tutorials/ws2812-breakout-hookup-guide"&gt;https://learn.sparkfun.com/tutorials/ws2812-breakout-hookup-guide&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/ws2812+24+bit+ring"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=LED-24XRGB-RING"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LED-24XRGB-RING"/>
</gates>
<devices>
<device name="" package="LED-24XRGB-RING">
<connects>
<connect gate="G$1" pin="DIN" pad="3"/>
<connect gate="G$1" pin="DOUT" pad="4"/>
<connect gate="G$1" pin="GND.1" pad="1"/>
<connect gate="G$1" pin="GND.2" pad="6"/>
<connect gate="G$1" pin="VCC.1" pad="2"/>
<connect gate="G$1" pin="VCC.2" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="N-MOSFET-SWITCH">
<description>&lt;b&gt;Low Side N-MOSFET Switch&lt;/b&gt; with &lt;b&gt;Optocoupler&lt;/b&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/1+route+mosfet+button+irf540"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=N-MOSFET-SWITCH"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="N-MOSFET-SWITCH"/>
</gates>
<devices>
<device name="" package="N-MOSFET-SWITCH">
<connects>
<connect gate="G$1" pin="CTRL" pad="J1.3"/>
<connect gate="G$1" pin="GND" pad="J1.1"/>
<connect gate="G$1" pin="VCC" pad="J1.2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="N-MOSFET-SWITCH#IC">
<description>&lt;b&gt;Low Side N-MOSFET Switch&lt;/b&gt; with &lt;b&gt;Optocoupler&lt;/b&gt;&lt;br /&gt;
Device with connector pins
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/1+route+mosfet+button+irf540"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=N-MOSFET-SWITCH"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="N-MOSFET-SWITCH#IC"/>
</gates>
<devices>
<device name="" package="N-MOSFET-SWITCH#IC">
<connects>
<connect gate="G$1" pin="CTRL" pad="J1.3"/>
<connect gate="G$1" pin="GND" pad="J1.1"/>
<connect gate="G$1" pin="IN.COM" pad="P1.2"/>
<connect gate="G$1" pin="IN.V+" pad="P1.1"/>
<connect gate="G$1" pin="OUT.SW" pad="P2.2"/>
<connect gate="G$1" pin="OUT.V+" pad="P2.1"/>
<connect gate="G$1" pin="VCC" pad="J1.2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BREADBOARD-POWER-V2">
<description>&lt;b&gt;Breadboard Power Adapter&lt;/b&gt; with onboard 3.3V and 5V regulators
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/breadboard+power+mb102"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=BREADBOARD-POWER-V2"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BREADBOARD-POWER-V2"/>
<gate name="G$2" symbol="BREADBOARD-POWER-V2"/>
</gates>
<devices>
<device name="" package="BREADBOARD-POWER-V2">
<connects>
<connect gate="G$1" pin="M.1" pad="A.M.1"/>
<connect gate="G$1" pin="M.2" pad="A.M.2"/>
<connect gate="G$1" pin="P.1" pad="A.P.1"/>
<connect gate="G$1" pin="P.2" pad="A.P.2"/>
<connect gate="G$2" pin="M.1" pad="B.M.1"/>
<connect gate="G$2" pin="M.2" pad="B.M.2"/>
<connect gate="G$2" pin="P.1" pad="B.P.1"/>
<connect gate="G$2" pin="P.2" pad="B.P.2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARKFUN-AD-MUX-16X1">
<description>&lt;b&gt;SparkFun Analog/Digital MUX Breakout&lt;/b&gt; based on &lt;b&gt;CD74HC4067&lt;/b&gt; chip&lt;br /&gt;&lt;br /&gt;
Source: &lt;a href="https://www.sparkfun.com/products/9056"&gt;https://www.sparkfun.com/products/9056&lt;/a&gt;&lt;br /&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=SPARKFUN-AD-MUX-16X1"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SPARKFUN-AD-MUX-16X1"/>
</gates>
<devices>
<device name="" package="SPARKFUN-AD-MUX-16X1">
<connects>
<connect gate="G$1" pin="C0" pad="J1.1"/>
<connect gate="G$1" pin="C1" pad="J1.2"/>
<connect gate="G$1" pin="C10" pad="J1.11"/>
<connect gate="G$1" pin="C11" pad="J1.12"/>
<connect gate="G$1" pin="C12" pad="J1.13"/>
<connect gate="G$1" pin="C13" pad="J1.14"/>
<connect gate="G$1" pin="C14" pad="J1.15"/>
<connect gate="G$1" pin="C15" pad="J1.16"/>
<connect gate="G$1" pin="C2" pad="J1.3"/>
<connect gate="G$1" pin="C3" pad="J1.4"/>
<connect gate="G$1" pin="C4" pad="J1.5"/>
<connect gate="G$1" pin="C5" pad="J1.6"/>
<connect gate="G$1" pin="C6" pad="J1.7"/>
<connect gate="G$1" pin="C7" pad="J1.8"/>
<connect gate="G$1" pin="C8" pad="J1.9"/>
<connect gate="G$1" pin="C9" pad="J1.10"/>
<connect gate="G$1" pin="EN" pad="J2.3"/>
<connect gate="G$1" pin="GND" pad="J2.1"/>
<connect gate="G$1" pin="S0" pad="J2.4"/>
<connect gate="G$1" pin="S1" pad="J2.5"/>
<connect gate="G$1" pin="S2" pad="J2.6"/>
<connect gate="G$1" pin="S3" pad="J2.7"/>
<connect gate="G$1" pin="SIG" pad="J2.8"/>
<connect gate="G$1" pin="VCC" pad="J2.2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DC-DC-LM2596-DISP">
<description>&lt;b&gt;DC/DC Step-Down Regulator&lt;/b&gt; with &lt;b&gt;Voltage Display&lt;/b&gt; based on &lt;b&gt;LM2596-ADJ&lt;/b&gt; chip
&lt;p&gt;More details available here:&lt;br /&gt;&lt;a href="http://www.instructables.com/id/The-Introduction-of-LM2596-Step-Down-Power-Module-/"&gt;http://www.instructables.com/id/The-Introduction-of-LM2596-Step-Down-Power-Module-/&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;LM2596&lt;/b&gt; datasheet available here:&lt;br /&gt;&lt;a href="http://www.ti.com/lit/ds/symlink/lm2596.pdf"&gt;http://www.ti.com/lit/ds/symlink/lm2596.pdf&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/lm2596+led+voltmeter+40"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=DC-DC-LM2596-DISP"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DC-DC-LM2596-DISP"/>
</gates>
<devices>
<device name="" package="DC-DC-LM2596-DISP">
<connects>
<connect gate="G$1" pin="IN+" pad="IN+"/>
<connect gate="G$1" pin="IN-" pad="IN-"/>
<connect gate="G$1" pin="OUT+" pad="OUT+"/>
<connect gate="G$1" pin="OUT-" pad="OUT-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BATTERY-HOLDER-2AAA">
<description>&lt;b&gt;Battery Holder 2 x AAA&lt;/b&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/battery+plastic+holder+aaa+2x1.5v"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=BATTERY-HOLDER-2AAA"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BATTERY-HOLDER-2AAA"/>
</gates>
<devices>
<device name="" package="BATTERY-HOLDER-2AAA">
<connects>
<connect gate="G$1" pin="BAT+" pad="BAT+"/>
<connect gate="G$1" pin="BAT-" pad="BAT-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TOUCH-KEYPAD-4X1">
<description>&lt;b&gt;4 Channel Capacitive Touch Keypad&lt;/b&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/ttp224+4+channel+digital+capacitive+touch+sensor"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=TOUCH-KEYPAD-4X1"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TOUCH-KEYPAD-4X1"/>
</gates>
<devices>
<device name="" package="TOUCH-KEYPAD-4X1">
<connects>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="2"/>
<connect gate="G$1" pin="OUT3" pad="3"/>
<connect gate="G$1" pin="OUT4" pad="4"/>
<connect gate="G$1" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TOUCH-KEYPAD-4X2">
<description>&lt;b&gt;8 Channel Capacitive Touch Keypad&lt;/b&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/ttp226+8+channel+digital+capacitive+touch+sensor"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=TOUCH-KEYPAD-4X2"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TOUCH-KEYPAD-4X2"/>
</gates>
<devices>
<device name="" package="TOUCH-KEYPAD-4X2">
<connects>
<connect gate="G$1" pin="DV" pad="1"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="OUT1" pad="9"/>
<connect gate="G$1" pin="OUT2" pad="8"/>
<connect gate="G$1" pin="OUT3" pad="7"/>
<connect gate="G$1" pin="OUT4" pad="6"/>
<connect gate="G$1" pin="OUT5" pad="5"/>
<connect gate="G$1" pin="OUT6" pad="4"/>
<connect gate="G$1" pin="OUT7" pad="3"/>
<connect gate="G$1" pin="OUT8" pad="2"/>
<connect gate="G$1" pin="VCC" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RELAY-1-SRD">
<description>&lt;b&gt;1-Channel Relay Module&lt;/b&gt; based on &lt;b&gt;SRD-05VDC-SL-C&lt;/b&gt; relays
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/one+channel+isolated+relay+5v"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=RELAY-1-SRD"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RELAY-1-SRD"/>
</gates>
<devices>
<device name="" package="RELAY-1-SRD">
<connects>
<connect gate="G$1" pin="GND" pad="J1.1"/>
<connect gate="G$1" pin="IN1" pad="J1.2"/>
<connect gate="G$1" pin="JD-VCC" pad="J2.1"/>
<connect gate="G$1" pin="VCC.1" pad="J1.3"/>
<connect gate="G$1" pin="VCC.2" pad="J2.2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RELAY-1-SRD#RC">
<description>&lt;b&gt;1-Channel Relay Module&lt;/b&gt; based on &lt;b&gt;SRD-05VDC-SL-C&lt;/b&gt; relays&lt;br&gt;
Symbol with relays pins
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/one+channel+isolated+relay+5v"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=RELAY-1-SRD"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RELAY-1-SRD#RC"/>
</gates>
<devices>
<device name="" package="RELAY-1-SRD#RC">
<connects>
<connect gate="G$1" pin="GND" pad="J1.1"/>
<connect gate="G$1" pin="IN1" pad="J1.2"/>
<connect gate="G$1" pin="JD-VCC" pad="J2.1"/>
<connect gate="G$1" pin="REL.1.COM" pad="P1.2"/>
<connect gate="G$1" pin="REL.1.NC" pad="P1.3"/>
<connect gate="G$1" pin="REL.1.NO" pad="P1.1"/>
<connect gate="G$1" pin="VCC.1" pad="J1.3"/>
<connect gate="G$1" pin="VCC.2" pad="J2.2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RELAY-4-SRD">
<description>&lt;b&gt;4-Channel Relay Module&lt;/b&gt; based on &lt;b&gt;SRD-05VDC-SL-C&lt;/b&gt; relays
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/four+channel+relay+module+optocoupler+5v"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=RELAY-4-SRD"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RELAY-4-SRD"/>
</gates>
<devices>
<device name="" package="RELAY-4-SRD">
<connects>
<connect gate="G$1" pin="GND" pad="J1.6"/>
<connect gate="G$1" pin="IN1" pad="J1.5"/>
<connect gate="G$1" pin="IN2" pad="J1.4"/>
<connect gate="G$1" pin="IN3" pad="J1.3"/>
<connect gate="G$1" pin="IN4" pad="J1.2"/>
<connect gate="G$1" pin="JD-VCC" pad="J2.1"/>
<connect gate="G$1" pin="VCC.1" pad="J1.1"/>
<connect gate="G$1" pin="VCC.2" pad="J2.2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RELAY-4-SRD#RC">
<description>&lt;b&gt;4-Channel Relay Module&lt;/b&gt; based on &lt;b&gt;SRD-05VDC-SL-C&lt;/b&gt; relays&lt;br&gt;
Symbol with relays pins
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/four+channel+relay+module+optocoupler+5v"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=RELAY-4-SRD"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RELAY-4-SRD#RC"/>
</gates>
<devices>
<device name="" package="RELAY-4-SRD#RC">
<connects>
<connect gate="G$1" pin="GND" pad="J1.6"/>
<connect gate="G$1" pin="IN1" pad="J1.5"/>
<connect gate="G$1" pin="IN2" pad="J1.4"/>
<connect gate="G$1" pin="IN3" pad="J1.3"/>
<connect gate="G$1" pin="IN4" pad="J1.2"/>
<connect gate="G$1" pin="JD-VCC" pad="J2.1"/>
<connect gate="G$1" pin="REL.1.COM" pad="P2.5"/>
<connect gate="G$1" pin="REL.1.NC" pad="P2.6"/>
<connect gate="G$1" pin="REL.1.NO" pad="P2.4"/>
<connect gate="G$1" pin="REL.2.COM" pad="P2.2"/>
<connect gate="G$1" pin="REL.2.NC" pad="P2.3"/>
<connect gate="G$1" pin="REL.2.NO" pad="P2.1"/>
<connect gate="G$1" pin="REL.3.COM" pad="P1.5"/>
<connect gate="G$1" pin="REL.3.NC" pad="P1.6"/>
<connect gate="G$1" pin="REL.3.NO" pad="P1.4"/>
<connect gate="G$1" pin="REL.4.COM" pad="P1.2"/>
<connect gate="G$1" pin="REL.4.NC" pad="P1.3"/>
<connect gate="G$1" pin="REL.4.NO" pad="P1.1"/>
<connect gate="G$1" pin="VCC.1" pad="J1.1"/>
<connect gate="G$1" pin="VCC.2" pad="J2.2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RELAY-8-SRD">
<description>&lt;b&gt;8-Channel Relay Module&lt;/b&gt; based on &lt;b&gt;SRD-05VDC-SL-C&lt;/b&gt; relays
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/eight+channel+relay+module+optocoupler+5v"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=RELAY-8-SRD"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RELAY-8-SRD"/>
</gates>
<devices>
<device name="" package="RELAY-8-SRD">
<connects>
<connect gate="G$1" pin="GND.1" pad="J1.10"/>
<connect gate="G$1" pin="GND.2" pad="J2.3"/>
<connect gate="G$1" pin="IN1" pad="J1.9"/>
<connect gate="G$1" pin="IN2" pad="J1.8"/>
<connect gate="G$1" pin="IN3" pad="J1.7"/>
<connect gate="G$1" pin="IN4" pad="J1.6"/>
<connect gate="G$1" pin="IN5" pad="J1.5"/>
<connect gate="G$1" pin="IN6" pad="J1.4"/>
<connect gate="G$1" pin="IN7" pad="J1.3"/>
<connect gate="G$1" pin="IN8" pad="J1.2"/>
<connect gate="G$1" pin="JD-VCC" pad="J2.1"/>
<connect gate="G$1" pin="VCC.1" pad="J1.1"/>
<connect gate="G$1" pin="VCC.2" pad="J2.2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RELAY-8-SRD#RC">
<description>&lt;b&gt;8-Channel Relay Module&lt;/b&gt; based on &lt;b&gt;SRD-05VDC-SL-C&lt;/b&gt; relays&lt;br&gt;
Symbol with relays pins
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/eight+channel+relay+module+optocoupler+5v"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=RELAY-8-SRD"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RELAY-8-SRD#RC"/>
</gates>
<devices>
<device name="" package="RELAY-8-SRD#RC">
<connects>
<connect gate="G$1" pin="GND.1" pad="J1.10"/>
<connect gate="G$1" pin="GND.2" pad="J2.3"/>
<connect gate="G$1" pin="IN1" pad="J1.9"/>
<connect gate="G$1" pin="IN2" pad="J1.8"/>
<connect gate="G$1" pin="IN3" pad="J1.7"/>
<connect gate="G$1" pin="IN4" pad="J1.6"/>
<connect gate="G$1" pin="IN5" pad="J1.5"/>
<connect gate="G$1" pin="IN6" pad="J1.4"/>
<connect gate="G$1" pin="IN7" pad="J1.3"/>
<connect gate="G$1" pin="IN8" pad="J1.2"/>
<connect gate="G$1" pin="JD-VCC" pad="J2.1"/>
<connect gate="G$1" pin="REL.1.COM" pad="P4.5"/>
<connect gate="G$1" pin="REL.1.NC" pad="P4.6"/>
<connect gate="G$1" pin="REL.1.NO" pad="P4.4"/>
<connect gate="G$1" pin="REL.2.COM" pad="P4.2"/>
<connect gate="G$1" pin="REL.2.NC" pad="P4.3"/>
<connect gate="G$1" pin="REL.2.NO" pad="P4.1"/>
<connect gate="G$1" pin="REL.3.COM" pad="P3.5"/>
<connect gate="G$1" pin="REL.3.NC" pad="P3.6"/>
<connect gate="G$1" pin="REL.3.NO" pad="P3.4"/>
<connect gate="G$1" pin="REL.4.COM" pad="P3.2"/>
<connect gate="G$1" pin="REL.4.NC" pad="P3.3"/>
<connect gate="G$1" pin="REL.4.NO" pad="P3.1"/>
<connect gate="G$1" pin="REL.5.COM" pad="P2.5"/>
<connect gate="G$1" pin="REL.5.NC" pad="P2.6"/>
<connect gate="G$1" pin="REL.5.NO" pad="P2.4"/>
<connect gate="G$1" pin="REL.6.COM" pad="P2.2"/>
<connect gate="G$1" pin="REL.6.NC" pad="P2.3"/>
<connect gate="G$1" pin="REL.6.NO" pad="P2.1"/>
<connect gate="G$1" pin="REL.7.COM" pad="P1.5"/>
<connect gate="G$1" pin="REL.7.NC" pad="P1.6"/>
<connect gate="G$1" pin="REL.7.NO" pad="P1.4"/>
<connect gate="G$1" pin="REL.8.COM" pad="P1.2"/>
<connect gate="G$1" pin="REL.8.NC" pad="P1.3"/>
<connect gate="G$1" pin="REL.8.NO" pad="P1.1"/>
<connect gate="G$1" pin="VCC.1" pad="J1.1"/>
<connect gate="G$1" pin="VCC.2" pad="J2.2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BATTERY-CHARGER-LI-PROT">
<description>&lt;b&gt;Lithium Battery 5V Charger&lt;/b&gt; with protection circuit
&lt;p&gt;More details available here:&lt;br&gt;
&lt;a href="http://www.instructables.com/id/DIY-Lithium-ion-Battery-Charger/step4/TP4056-based-lithium-ion-battery-charger-module/"&gt;
http://www.instructables.com/id/DIY-Lithium-ion-Battery-Charger/step4/TP4056-based-lithium-ion-battery-charger-module/&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/tp4056+charger+usb+protection"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=BATTERY-CHARGER-LI-PROT"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BATTERY-CHARGER-LI-PROT"/>
</gates>
<devices>
<device name="" package="BATTERY-CHARGER-LI-PROT">
<connects>
<connect gate="G$1" pin="B+" pad="B+"/>
<connect gate="G$1" pin="B-" pad="B-"/>
<connect gate="G$1" pin="IN+" pad="IN+"/>
<connect gate="G$1" pin="IN-" pad="IN-"/>
<connect gate="G$1" pin="OUT+" pad="OUT+"/>
<connect gate="G$1" pin="OUT-" pad="OUT-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DC-DC-LM2596-DISP#RC">
<description>&lt;b&gt;DC/DC Step-Down Regulator&lt;/b&gt; with &lt;b&gt;Voltage Display&lt;/b&gt; based on &lt;b&gt;LM2596-ADJ&lt;/b&gt; chip&lt;br&gt;
Symbol with input and output connectors
&lt;p&gt;More details available here:&lt;br /&gt;&lt;a href="http://www.instructables.com/id/The-Introduction-of-LM2596-Step-Down-Power-Module-/"&gt;http://www.instructables.com/id/The-Introduction-of-LM2596-Step-Down-Power-Module-/&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;LM2596&lt;/b&gt; datasheet available here:&lt;br /&gt;&lt;a href="http://www.ti.com/lit/ds/symlink/lm2596.pdf"&gt;http://www.ti.com/lit/ds/symlink/lm2596.pdf&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/lm2596+led+voltmeter+40"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=DC-DC-LM2596-DISP"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DC-DC-LM2596-DISP#RC"/>
</gates>
<devices>
<device name="" package="DC-DC-LM2596-DISP#RC">
<connects>
<connect gate="G$1" pin="C.IN+" pad="P1.1"/>
<connect gate="G$1" pin="C.IN-" pad="P1.2"/>
<connect gate="G$1" pin="C.OUT+" pad="P2.2"/>
<connect gate="G$1" pin="C.OUT-" pad="P2.1"/>
<connect gate="G$1" pin="IN+" pad="IN+"/>
<connect gate="G$1" pin="IN-" pad="IN-"/>
<connect gate="G$1" pin="OUT+" pad="OUT+"/>
<connect gate="G$1" pin="OUT-" pad="OUT-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-8XRGB-LINE">
<description>&lt;b&gt;8 LEDs RGB Line Display&lt;/b&gt; based on &lt;b&gt;WS2812B&lt;/b&gt;
&lt;p&gt;More details about controlling &lt;b&gt;WS2812B&lt;/b&gt; RGB LEDs are available here:&lt;br&gt;
&lt;a href="https://learn.sparkfun.com/tutorials/ws2812-breakout-hookup-guide"&gt;https://learn.sparkfun.com/tutorials/ws2812-breakout-hookup-guide&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/ws2812+8+bit+rainbow"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=LED-8XRGB-LINE"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LED-8XRGB-LINE"/>
</gates>
<devices>
<device name="" package="LED-8XRGB-LINE">
<connects>
<connect gate="G$1" pin="DIN" pad="B.2"/>
<connect gate="G$1" pin="DOUT" pad="A.2"/>
<connect gate="G$1" pin="GND.1" pad="A.1"/>
<connect gate="G$1" pin="GND.2" pad="A.4"/>
<connect gate="G$1" pin="GND.3" pad="B.1"/>
<connect gate="G$1" pin="GND.4" pad="B.4"/>
<connect gate="G$1" pin="VCC.1" pad="A.3"/>
<connect gate="G$1" pin="VCC.2" pad="B.3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-15XRGB-QRING">
<description>&lt;b&gt;15 LEDs RGB Quarter-Ring&lt;/b&gt; based on &lt;b&gt;WS2812B&lt;/b&gt;
&lt;p&gt;More details about controlling &lt;b&gt;WS2812B&lt;/b&gt; RGB LEDs are available here:&lt;br&gt;
&lt;a href="https://learn.sparkfun.com/tutorials/ws2812-breakout-hookup-guide"&gt;https://learn.sparkfun.com/tutorials/ws2812-breakout-hookup-guide&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/ws2812+60+ring"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;br /&gt;
&lt;b&gt;Note:&lt;/b&gt; Sold in packs of 4 pieces.&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=LED-15XRGB-QRING"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LED-15XRGB-QRING"/>
</gates>
<devices>
<device name="" package="LED-15XRGB-QRING">
<connects>
<connect gate="G$1" pin="DIN" pad="2"/>
<connect gate="G$1" pin="DOUT" pad="5"/>
<connect gate="G$1" pin="GND.1" pad="1"/>
<connect gate="G$1" pin="GND.2" pad="4"/>
<connect gate="G$1" pin="VCC.1" pad="3"/>
<connect gate="G$1" pin="VCC.2" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WIRELESS-BLUETOOTH-XS3868">
<description>&lt;b&gt;Bluetooth Stereo Audio Module&lt;/b&gt; based on &lt;b&gt;OVC3860&lt;/b&gt; chip
&lt;p&gt;More details available here:&lt;br&gt;
&lt;a href="http://artofcircuits.com/product/bluetooth-2-0-edr-stereo-audio-ovc3860-module-model-xs-3868"&gt;
http://artofcircuits.com/product/bluetooth-2-0-edr-stereo-audio-ovc3860-module-model-xs-3868&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/xs3868+bluetooth+audio+module"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=WIRELESS-BLUETOOTH-XS3868"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="WIRELESS-BLUETOOTH-XS3868"/>
</gates>
<devices>
<device name="" package="WIRELESS-BLUETOOTH-XS3868">
<connects>
<connect gate="G$1" pin="1.8V_OUT" pad="12"/>
<connect gate="G$1" pin="AGND" pad="1"/>
<connect gate="G$1" pin="ALEFT" pad="3"/>
<connect gate="G$1" pin="ARIGHT" pad="2"/>
<connect gate="G$1" pin="BACK" pad="22"/>
<connect gate="G$1" pin="CH.POW" pad="8"/>
<connect gate="G$1" pin="CH.STAT" pad="6"/>
<connect gate="G$1" pin="CHRG" pad="7"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="MIC+" pad="4"/>
<connect gate="G$1" pin="MIC-" pad="5"/>
<connect gate="G$1" pin="NC.1" pad="10"/>
<connect gate="G$1" pin="NC.2" pad="14"/>
<connect gate="G$1" pin="NC.3" pad="17"/>
<connect gate="G$1" pin="NC.4" pad="20"/>
<connect gate="G$1" pin="NEXT" pad="21"/>
<connect gate="G$1" pin="PLAY" pad="23"/>
<connect gate="G$1" pin="RST" pad="13"/>
<connect gate="G$1" pin="RX" pad="19"/>
<connect gate="G$1" pin="TX" pad="18"/>
<connect gate="G$1" pin="VBAT" pad="11"/>
<connect gate="G$1" pin="VOL+" pad="15"/>
<connect gate="G$1" pin="VOL-" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISPLAY-OLED-128X64">
<description>&lt;b&gt;128x64 Dot Matrix OLED Module&lt;/b&gt; based on &lt;b&gt;SSD1306&lt;/b&gt; chip&lt;br /&gt;
Variant with &lt;b&gt;SPI interface&lt;/b&gt;
&lt;p&gt;More details available here:&lt;br /&gt;
&lt;a href="http://www.instructables.com/id/How-to-use-OLED-display-arduino-module/"&gt;http://www.instructables.com/id/How-to-use-OLED-display-arduino-module/&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SSD1306&lt;/b&gt; datasheet:&lt;br&gt;
&lt;a href="https://cdn-shop.adafruit.com/datasheets/SSD1306.pdf"&gt;https://cdn-shop.adafruit.com/datasheets/SSD1306.pdf&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/oled+display+128x64"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;br /&gt;
&lt;b&gt;Note:&lt;/b&gt; There are two variants: I2C and SPI. Search for the proper version.&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=DISPLAY-OLED-128X64"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DISPLAY-OLED-128X64"/>
</gates>
<devices>
<device name="" package="DISPLAY-OLED-128X64">
<connects>
<connect gate="G$1" pin="CS" pad="7"/>
<connect gate="G$1" pin="D0" pad="3"/>
<connect gate="G$1" pin="D1" pad="4"/>
<connect gate="G$1" pin="DC" pad="6"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="RES" pad="5"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DFPLAYER-MINI-MODULE">
<description>&lt;b&gt;DFPlayer Mini&lt;/b&gt; - MP3 player module based on &lt;b&gt;YX5200&lt;/b&gt; chip
&lt;p&gt;More details available here:&lt;br&gt;&lt;a href="https://www.dfrobot.com/wiki/index.php/DFPlayer_Mini_SKU:DFR0299"&gt;https://www.dfrobot.com/wiki/index.php/DFPlayer_Mini_SKU:DFR0299&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/dfplayer+mini"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=DFPLAYER-MINI-MODULE"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DFPLAYER-MINI-MODULE"/>
</gates>
<devices>
<device name="" package="DFPLAYER-MINI-MODULE">
<connects>
<connect gate="G$1" pin="ADKEY_1" pad="12"/>
<connect gate="G$1" pin="ADKEY_2" pad="13"/>
<connect gate="G$1" pin="BUSY" pad="16"/>
<connect gate="G$1" pin="DAC_I" pad="5"/>
<connect gate="G$1" pin="DAC_R" pad="4"/>
<connect gate="G$1" pin="GND.1" pad="7"/>
<connect gate="G$1" pin="GND.2" pad="10"/>
<connect gate="G$1" pin="IO_1" pad="9"/>
<connect gate="G$1" pin="IO_2" pad="11"/>
<connect gate="G$1" pin="RX" pad="2"/>
<connect gate="G$1" pin="SPK_1" pad="6"/>
<connect gate="G$1" pin="SPK_2" pad="8"/>
<connect gate="G$1" pin="TX" pad="3"/>
<connect gate="G$1" pin="USB+" pad="14"/>
<connect gate="G$1" pin="USB-" pad="15"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BATTERY-LI-MH12210">
<description>&lt;b&gt;Lithium-Ion MH12210 Rechargeable Battery&lt;/b&gt;
&lt;p&gt;&lt;b&gt;Panasonic NCR18650PF&lt;/b&gt; battery datasheet available here:&lt;br /&gt;&lt;a href="https://industrial.panasonic.com/cdbs/www-data/pdf2/ACI4000/ACI4000C12.pdf"&gt;https://industrial.panasonic.com/cdbs/www-data/pdf2/ACI4000/ACI4000C12.pdf&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/ncr18650b+battery"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=BATTERY-LI-MH12210"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BATTERY-LI-MH12210"/>
</gates>
<devices>
<device name="" package="BATTERY-LI-MH12210">
<connects>
<connect gate="G$1" pin="BAT+" pad="BAT+"/>
<connect gate="G$1" pin="BAT-" pad="BAT-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEMP-HUM-SENSOR-DHT11">
<description>&lt;b&gt;DHT11 - digital humidity &amp; temperature sensor&lt;/b&gt;
&lt;p&gt;&lt;b&gt;DHT11&lt;/b&gt; datasheet available here:&lt;br&gt;
&lt;a href="https://akizukidenshi.com/download/ds/aosong/DHT11.pdf"&gt;https://akizukidenshi.com/download/ds/aosong/DHT11.pdf&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/dht11+digital+sensor"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=TEMP-HUM-SENSOR-DHT11"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TEMP-HUM-SENSOR-DHT11"/>
</gates>
<devices>
<device name="" package="TEMP-HUM-SENSOR-DHT11">
<connects>
<connect gate="G$1" pin="DAT" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="N.C." pad="3"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEMP-HUM-SENSOR-DHT22">
<description>&lt;b&gt;DHT22 - digital humidity &amp; temperature sensor&lt;/b&gt;&lt;br /&gt;
Also known as: &lt;b&gt;AM2302&lt;/b&gt;
&lt;p&gt;&lt;b&gt;AM2302&lt;/b&gt; datasheet available here:&lt;br&gt;
&lt;a href="http://akizukidenshi.com/download/ds/aosong/AM2302.pdf"&gt;http://akizukidenshi.com/download/ds/aosong/AM2302.pdf&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/dht22+digital+sensor"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=TEMP-HUM-SENSOR-DHT22"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TEMP-HUM-SENSOR-DHT22"/>
</gates>
<devices>
<device name="" package="TEMP-HUM-SENSOR-DHT22">
<connects>
<connect gate="G$1" pin="DAT" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="N.C." pad="3"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RADIO-RECEIVER-DCF77">
<description>&lt;b&gt;DCF-77 Longwave Radio Time Signal Receiver&lt;/b&gt; based on &lt;b&gt;MAS6180B1&lt;/b&gt; chip
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=RADIO-RECEIVER-DCF77"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RADIO-RECEIVER-DCF77"/>
</gates>
<devices>
<device name="" package="RADIO-RECEIVER-DCF77">
<connects>
<connect gate="G$1" pin="ANT1" pad="A1"/>
<connect gate="G$1" pin="ANT2" pad="A2"/>
<connect gate="G$1" pin="AON" pad="AON"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="P1" pad="5"/>
<connect gate="G$1" pin="P2" pad="3"/>
<connect gate="G$1" pin="T" pad="4"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISPLAY-OLED-128X32">
<description>&lt;b&gt;128x32 Dot Matrix OLED Module&lt;/b&gt; with &lt;b&gt;I2C&lt;/b&gt; interface based on &lt;b&gt;SSD1306&lt;/b&gt; chip
&lt;p&gt;More details available here:&lt;br&gt;
&lt;a href="http://www.tinyosshop.com/index.php?route=product/product&amp;product_id=953"&gt;http://www.tinyosshop.com/index.php?route=product/product&amp;product_id=953&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Schematic available here:&lt;br&gt;
&lt;a href="http://www.tinyosshop.com/datasheet/OLED%2012832.pdf"&gt;http://www.tinyosshop.com/datasheet/OLED%2012832.pdf&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SSD1306&lt;/b&gt; datasheet:&lt;br&gt;
&lt;a href="https://cdn-shop.adafruit.com/datasheets/SSD1306.pdf"&gt;https://cdn-shop.adafruit.com/datasheets/SSD1306.pdf&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/oled+display+128x32+i2c"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=DISPLAY-OLED-128X32"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DISPLAY-OLED-128X32"/>
</gates>
<devices>
<device name="" package="DISPLAY-OLED-128X32">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="SCL" pad="3"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DC-DC-STEP-DOWN-MP2307">
<description>&lt;b&gt;DC/DC Step-Down Regulator&lt;/b&gt; based on &lt;b&gt;MP2307DN&lt;/b&gt; chip
&lt;p&gt;&lt;b&gt;MP2307&lt;/b&gt; datasheet available here:&lt;br&gt;
&lt;a href="https://cdn-shop.adafruit.com/datasheets/MP2307_r1.9.pdf"&gt;https://cdn-shop.adafruit.com/datasheets/MP2307_r1.9.pdf&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/dc+dc+3a+mini+converter"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;

&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=DC-DC-STEP-DOWN-MP2307"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DC-DC-STEP-DOWN-MP2307"/>
</gates>
<devices>
<device name="" package="DC-DC-STEP-DOWN-MP2307">
<connects>
<connect gate="G$1" pin="IN+" pad="IN+"/>
<connect gate="G$1" pin="IN-" pad="IN-"/>
<connect gate="G$1" pin="OUT+" pad="OUT+"/>
<connect gate="G$1" pin="OUT-" pad="OUT-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="THERMOCOUPLE-MAX31855">
<description>&lt;b&gt;Thermocouple Analog-to-Digital Converter&lt;/b&gt; based on &lt;b&gt;MAX31855&lt;/b&gt; chip
&lt;p&gt;&lt;b&gt;MAX31855&lt;/b&gt; datasheet available here:&lt;br /&gt;
&lt;a href="https://www.maximintegrated.com/en/products/analog/sensors-and-sensor-interface/MAX31855.html"&gt;https://www.maximintegrated.com/en/products/analog/sensors-and-sensor-interface/MAX31855.html&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/max31855k+module"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=THERMOCOUPLE-MAX31855"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="THERMOCOUPLE-MAX31855"/>
</gates>
<devices>
<device name="" package="THERMOCOUPLE-MAX31855">
<connects>
<connect gate="G$1" pin="CS" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SCK" pad="5"/>
<connect gate="G$1" pin="SO" pad="3"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="THERMOCOUPLE-MAX31855#IC">
<description>&lt;b&gt;Thermocouple Analog-to-Digital Converter&lt;/b&gt; based on &lt;b&gt;MAX31855&lt;/b&gt; chip&lt;br /&gt;
Symbol with thermocouple connector pins
&lt;p&gt;&lt;b&gt;MAX31855&lt;/b&gt; datasheet available here:&lt;br /&gt;
&lt;a href="https://www.maximintegrated.com/en/products/analog/sensors-and-sensor-interface/MAX31855.html"&gt;https://www.maximintegrated.com/en/products/analog/sensors-and-sensor-interface/MAX31855.html&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/max31855k+module"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=THERMOCOUPLE-MAX31855"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="THERMOCOUPLE-MAX31855#IC"/>
</gates>
<devices>
<device name="" package="THERMOCOUPLE-MAX31855#IC">
<connects>
<connect gate="G$1" pin="CS" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SCK" pad="5"/>
<connect gate="G$1" pin="SO" pad="3"/>
<connect gate="G$1" pin="T+" pad="P1.2"/>
<connect gate="G$1" pin="T-" pad="P1.1"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LEVEL-SHIFTER-4CH">
<description>&lt;b&gt;4-Channel Bi-Directional  Logic Level Converter&lt;/b&gt; based on &lt;b&gt;BSS128&lt;/b&gt; transistors
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/i2c+logic+converter+module"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=LEVEL-SHIFTER-4CH"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LEVEL-SHIFTER-4CH"/>
</gates>
<devices>
<device name="" package="LEVEL-SHIFTER-4CH">
<connects>
<connect gate="G$1" pin="GND.1" pad="J1.4"/>
<connect gate="G$1" pin="GND.2" pad="J2.4"/>
<connect gate="G$1" pin="HV" pad="J2.3"/>
<connect gate="G$1" pin="HV1" pad="J2.1"/>
<connect gate="G$1" pin="HV2" pad="J2.2"/>
<connect gate="G$1" pin="HV3" pad="J2.5"/>
<connect gate="G$1" pin="HV4" pad="J2.6"/>
<connect gate="G$1" pin="LV" pad="J1.3"/>
<connect gate="G$1" pin="LV1" pad="J1.1"/>
<connect gate="G$1" pin="LV2" pad="J1.2"/>
<connect gate="G$1" pin="LV3" pad="J1.5"/>
<connect gate="G$1" pin="LV4" pad="J1.6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RTC-DS3231-AT24C32">
<description>&lt;b&gt;RTC Module with Battery and EEPROM&lt;/b&gt; based on &lt;b&gt;DS3231&lt;/b&gt; and &lt;b&gt;AT24C32&lt;/b&gt; chips
&lt;p&gt;Tutorial can be found here:&lt;br /&gt;
&lt;a href="https://edwardmallon.wordpress.com/2014/05/21/using-a-cheap-3-ds3231-rtc-at24c32-eeprom-from-ebay/"&gt;https://edwardmallon.wordpress.com/2014/05/21/using-a-cheap-3-ds3231-rtc-at24c32-eeprom-from-ebay/&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/DS3231+AT24C32+module"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=RTC-DS3231-AT24C32"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RTC-DS3231-AT24C32"/>
</gates>
<devices>
<device name="" package="RTC-DS3231-AT24C32">
<connects>
<connect gate="G$1" pin="32K" pad="J1.1"/>
<connect gate="G$1" pin="GND.1" pad="J1.6"/>
<connect gate="G$1" pin="GND.2" pad="J2.4"/>
<connect gate="G$1" pin="SCL.1" pad="J1.3"/>
<connect gate="G$1" pin="SCL.2" pad="J2.1"/>
<connect gate="G$1" pin="SDA.1" pad="J1.4"/>
<connect gate="G$1" pin="SDA.2" pad="J2.2"/>
<connect gate="G$1" pin="SQW" pad="J1.2"/>
<connect gate="G$1" pin="VCC.1" pad="J1.5"/>
<connect gate="G$1" pin="VCC.2" pad="J2.3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WIRELESS-LORA-RFM95W">
<description>&lt;b&gt;868/915 MHz LoRa Radio Transceiver Module&lt;/b&gt; based on &lt;b&gt;SX1276&lt;/b&gt; chip
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/RFM95W+transceiver"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=WIRELESS-LORA-RFM95W"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="WIRELESS-LORA-RFM95W"/>
</gates>
<devices>
<device name="#THT" package="WIRELESS-LORA-RFM95W#THT">
<connects>
<connect gate="G$1" pin="3.3V" pad="B4"/>
<connect gate="G$1" pin="ANT" pad="B8"/>
<connect gate="G$1" pin="DIO0" pad="B3"/>
<connect gate="G$1" pin="DIO1" pad="B2"/>
<connect gate="G$1" pin="DIO2" pad="B1"/>
<connect gate="G$1" pin="DIO3" pad="B6"/>
<connect gate="G$1" pin="DIO4" pad="B5"/>
<connect gate="G$1" pin="DIO5" pad="A7"/>
<connect gate="G$1" pin="GND.1" pad="A1"/>
<connect gate="G$1" pin="GND.2" pad="A8"/>
<connect gate="G$1" pin="GND.3" pad="B7"/>
<connect gate="G$1" pin="MISO" pad="A2"/>
<connect gate="G$1" pin="MOSI" pad="A3"/>
<connect gate="G$1" pin="NSS" pad="A5"/>
<connect gate="G$1" pin="RST" pad="A6"/>
<connect gate="G$1" pin="SCK" pad="A4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="#SMD" package="WIRELESS-LORA-RFM95W#SMD">
<connects>
<connect gate="G$1" pin="3.3V" pad="B4"/>
<connect gate="G$1" pin="ANT" pad="B8"/>
<connect gate="G$1" pin="DIO0" pad="B3"/>
<connect gate="G$1" pin="DIO1" pad="B2"/>
<connect gate="G$1" pin="DIO2" pad="B1"/>
<connect gate="G$1" pin="DIO3" pad="B6"/>
<connect gate="G$1" pin="DIO4" pad="B5"/>
<connect gate="G$1" pin="DIO5" pad="A7"/>
<connect gate="G$1" pin="GND.1" pad="A1"/>
<connect gate="G$1" pin="GND.2" pad="A8"/>
<connect gate="G$1" pin="GND.3" pad="B7"/>
<connect gate="G$1" pin="MISO" pad="A2"/>
<connect gate="G$1" pin="MOSI" pad="A3"/>
<connect gate="G$1" pin="NSS" pad="A5"/>
<connect gate="G$1" pin="RST" pad="A6"/>
<connect gate="G$1" pin="SCK" pad="A4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEMP-HUM-PRES-BME280">
<description>&lt;b&gt;Digital Humidity-Temperature-Pressure Sensor&lt;/b&gt; based on &lt;b&gt;BME280&lt;/b&gt; device
&lt;p&gt;More information about &lt;b&gt;BME280&lt;/b&gt; device is available here:&lt;br&gt;
&lt;a href="https://www.bosch-sensortec.com/bst/products/all_products/bme280"&gt;https://www.bosch-sensortec.com/bst/products/all_products/bme280&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/bme280+breakout"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=TEMP-HUM-PRES-BME280"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TEMP-HUM-PRES-BME280"/>
</gates>
<devices>
<device name="" package="TEMP-HUM-PRES-BME280">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SCL" pad="3"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEMP-HUM-SENSOR-HTU21D">
<description>&lt;b&gt;Digital Humidity &amp; Temperature Sensor&lt;/b&gt; based on &lt;b&gt;HTU21D&lt;/b&gt; device
&lt;p&gt;More information about &lt;b&gt;HTU21D&lt;/b&gt; device is available here:&lt;br&gt;
&lt;a href="http://futureeverything.org/wp-content/uploads/2014/05/Humidity-Datasheet.pdf"&gt;http://futureeverything.org/wp-content/uploads/2014/05/Humidity-Datasheet.pdf&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;HTU21D&lt;/b&gt; Arudino Library is available here:&lt;br&gt;
&lt;a href="https://learn.sparkfun.com/tutorials/htu21d-humidity-sensor-hookup-guide/htu21d-library-and-functions"&gt;https://learn.sparkfun.com/tutorials/htu21d-humidity-sensor-hookup-guide/htu21d-library-and-functions&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/htu21d+board"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=TEMP-HUM-SENSOR-HTU21D"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TEMP-HUM-SENSOR-HTU21D"/>
</gates>
<devices>
<device name="" package="TEMP-HUM-SENSOR-HTU21D">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SCL" pad="3"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB-SERIAL-FT232R">
<description>&lt;b&gt;USB to Serial UART Converter&lt;/b&gt; based on &lt;b&gt;FT232R&lt;/b&gt; chip
&lt;p&gt;More information about &lt;b&gt;FT232R&lt;/b&gt; chip is available here:&lt;br&gt;
&lt;a href="http://www.ftdichip.com/Products/ICs/FT232R.htm"&gt;http://www.ftdichip.com/Products/ICs/FT232R.htm&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/ft232rl+arduino+download+max232"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=USB-SERIAL-FT232R"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="USB-SERIAL-FT232R"/>
</gates>
<devices>
<device name="" package="USB-SERIAL-FT232R">
<connects>
<connect gate="G$1" pin="CTS" pad="5"/>
<connect gate="G$1" pin="DTR" pad="1"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="RX" pad="2"/>
<connect gate="G$1" pin="TX" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DATA-LOGGER-MINI">
<description>&lt;b&gt;Mini Data Logger&lt;/b&gt; with &lt;b&gt;microSD card&lt;/b&gt; and  battery powered &lt;b&gt;RTC&lt;/b&gt; based on &lt;b&gt;DS1307&lt;/b&gt; chip

&lt;p&gt;Arduino library for &lt;b&gt;DS1307&lt;/b&gt; and description are available here:&lt;br&gt;
&lt;a href="https://www.pjrc.com/teensy/td_libs_DS1307RTC.html"&gt;https://www.pjrc.com/teensy/td_libs_DS1307RTC.html&lt;/a&gt;&lt;/p&gt;

&lt;p&gt;Tutorial how to use &lt;b&gt;SD card&lt;/b&gt; with Arduino:&lt;br&gt;
&lt;a href="https://www.arduino.cc/en/reference/SD"&gt;https://www.arduino.cc/en/reference/SD&lt;/a&gt;&lt;/p&gt;

&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/mini+data+logger+arduino"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=DATA-LOGGER-MINI"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DATA-LOGGER-MINI"/>
</gates>
<devices>
<device name="" package="DATA-LOGGER-MINI">
<connects>
<connect gate="G$1" pin="5V" pad="1"/>
<connect gate="G$1" pin="CS" pad="8"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="MISO" pad="6"/>
<connect gate="G$1" pin="MOSI" pad="7"/>
<connect gate="G$1" pin="SCK" pad="5"/>
<connect gate="G$1" pin="SCL" pad="4"/>
<connect gate="G$1" pin="SDA" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GAS-SENSOR-MQ2">
<description>&lt;b&gt;Gas Sensor&lt;/b&gt; based on &lt;b&gt;MQ-2&lt;/b&gt; device
&lt;p&gt;Guide describing how to use &lt;b&gt;MQ-2&lt;/b&gt; sensor with Arduino is available here:&lt;br /&gt;
&lt;a href="http://www.instructables.com/id/How-to-use-MQ2-Gas-Sensor-Arduino-Tutorial/"&gt;http://www.instructables.com/id/How-to-use-MQ2-Gas-Sensor-Arduino-Tutorial/&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;MQ-2&lt;/b&gt; sensor datasheet is available here:&lt;br /&gt;
&lt;a href="http://gas-sensor.ru/pdf/combustible-gas-sensor.pdf"&gt;http://gas-sensor.ru/pdf/combustible-gas-sensor.pdf&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/mq2+sensor+module+smoke"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=GAS-SENSOR-MQ2"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="GAS-SENSOR-MQ2"/>
</gates>
<devices>
<device name="" package="GAS-SENSOR-MQ2">
<connects>
<connect gate="G$1" pin="AO" pad="4"/>
<connect gate="G$1" pin="DO" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UV-SENSOR-ML8511">
<description>&lt;b&gt;UV  Sensor&lt;/b&gt; based on &lt;b&gt;ML8511&lt;/b&gt; device
&lt;p&gt;&lt;b&gt;ML8511&lt;/b&gt; user's guide is available here:&lt;br /&gt;
&lt;a href="https://learn.sparkfun.com/tutorials/ml8511-uv-sensor-hookup-guide/using-the-ml8511"&gt;https://learn.sparkfun.com/tutorials/ml8511-uv-sensor-hookup-guide/using-the-ml8511&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;ML8511&lt;/b&gt; datasheet is available here:&lt;br /&gt;
&lt;a href="https://www.mcs.anl.gov/research/projects/waggle/downloads/datasheets/lightsense/ml8511.pdf"&gt;https://www.mcs.anl.gov/research/projects/waggle/downloads/datasheets/lightsense/ml8511.pdf&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/ml8511+module"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=UV-SENSOR-ML8511"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="UV-SENSOR-ML8511"/>
</gates>
<devices>
<device name="" package="UV-SENSOR-ML8511">
<connects>
<connect gate="G$1" pin="3V3" pad="2"/>
<connect gate="G$1" pin="EN" pad="5"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC-4CH-ADS1115">
<description>&lt;b&gt;4 Channel 16-Bit Analog-to-Digital Converter&lt;/b&gt; based on &lt;b&gt;ADS1115&lt;/b&gt; chip
&lt;p&gt;Arduino &lt;b&gt;ADS1115&lt;/b&gt; Getting Started Tutorial is available here:&lt;br /&gt;
&lt;a href="http://henrysbench.capnfatz.com/henrys-bench/arduino-voltage-measurements/arduino-ads1115-module-getting-started-tutorial/"&gt;http://henrysbench.capnfatz.com/henrys-bench/arduino-voltage-measurements/arduino-ads1115-module-getting-started-tutorial/&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;ADS1115&lt;/b&gt; datasheet is available here:&lt;br /&gt;
&lt;a href="http://www.ti.com/lit/ds/symlink/ads1115.pdf"&gt;http://www.ti.com/lit/ds/symlink/ads1115.pdf&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/ads1115+module"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=ADC-4CH-ADS1115"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ADC-4CH-ADS1115"/>
</gates>
<devices>
<device name="" package="ADC-4CH-ADS1115">
<connects>
<connect gate="G$1" pin="A0" pad="7"/>
<connect gate="G$1" pin="A1" pad="8"/>
<connect gate="G$1" pin="A2" pad="9"/>
<connect gate="G$1" pin="A3" pad="10"/>
<connect gate="G$1" pin="ADDR" pad="5"/>
<connect gate="G$1" pin="ALRT" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SCL" pad="3"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WIRELESS-BLUETOOTH-BK8000">
<description>&lt;b&gt;Bluetooth Audio Module&lt;/b&gt; based on &lt;b&gt;BK8000L&lt;/b&gt; chip
&lt;p&gt;More details available here:&lt;br /&gt;
&lt;a href="http://www.electrodragon.com/w/BK8000L"&gt;http://www.electrodragon.com/w/BK8000L&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/bk8000l+module"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=WIRELESS-BLUETOOTH-BK8000"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="WIRELESS-BLUETOOTH-BK8000"/>
</gates>
<devices>
<device name="" package="WIRELESS-BLUETOOTH-BK8000">
<connects>
<connect gate="G$1" pin="3V_OUT" pad="30"/>
<connect gate="G$1" pin="ANT" pad="2"/>
<connect gate="G$1" pin="AUD_LN" pad="24"/>
<connect gate="G$1" pin="AUD_LP" pad="25"/>
<connect gate="G$1" pin="AUD_RN" pad="27"/>
<connect gate="G$1" pin="AUD_RP" pad="26"/>
<connect gate="G$1" pin="GND.1" pad="1"/>
<connect gate="G$1" pin="GND.2" pad="3"/>
<connect gate="G$1" pin="GND.3" pad="16"/>
<connect gate="G$1" pin="GND.4" pad="17"/>
<connect gate="G$1" pin="GND.5" pad="32"/>
<connect gate="G$1" pin="GPIO11" pad="18"/>
<connect gate="G$1" pin="GPIO2" pad="12"/>
<connect gate="G$1" pin="GPIO3" pad="13"/>
<connect gate="G$1" pin="GPIO4" pad="14"/>
<connect gate="G$1" pin="GPIO5" pad="15"/>
<connect gate="G$1" pin="IN_L" pad="20"/>
<connect gate="G$1" pin="IN_R" pad="19"/>
<connect gate="G$1" pin="MBISTEN" pad="9"/>
<connect gate="G$1" pin="MIC_N" pad="21"/>
<connect gate="G$1" pin="MIC_P" pad="22"/>
<connect gate="G$1" pin="RSTN" pad="8"/>
<connect gate="G$1" pin="RX/GPIO0" pad="10"/>
<connect gate="G$1" pin="TCK" pad="5"/>
<connect gate="G$1" pin="TDI" pad="7"/>
<connect gate="G$1" pin="TDO" pad="6"/>
<connect gate="G$1" pin="TMS" pad="4"/>
<connect gate="G$1" pin="TX/GPIO1" pad="11"/>
<connect gate="G$1" pin="VADC" pad="31"/>
<connect gate="G$1" pin="VBAT" pad="29"/>
<connect gate="G$1" pin="VBUS" pad="28"/>
<connect gate="G$1" pin="VMIC" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GPS-RECEIVER-NEO6M">
<description>&lt;b&gt;GPS Receiver Module&lt;/b&gt; based on &lt;b&gt;NEO-6&lt;/b&gt; device

&lt;p&gt;Short tutorial how to use &lt;b&gt;NEO-6&lt;/b&gt; module with Arduino:&lt;br&gt;
&lt;a href="http://www.xarg.org/2016/06/neo6mv2-gps-module-with-arduino/"&gt;http://www.xarg.org/2016/06/neo6mv2-gps-module-with-arduino/&lt;/a&gt;&lt;/p&gt;

&lt;p&gt;&lt;b&gt;NEO-6&lt;/b&gt; datasheet is available here:&lt;br&gt;
&lt;a href="https://www.u-blox.com/sites/default/files/products/documents/NEO-6_DataSheet_%28GPS.G6-HW-09005%29.pdf"&gt;https://www.u-blox.com/sites/default/files/products/documents/NEO-6_DataSheet_%28GPS.G6-HW-09005%29.pdf&lt;/a&gt;&lt;/p&gt;

&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/gyneo6mv2"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=GPS-RECEIVER-NEO6M"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="GPS-RECEIVER-NEO6M"/>
</gates>
<devices>
<device name="" package="GPS-RECEIVER-NEO6M">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="PPS" pad="5"/>
<connect gate="G$1" pin="RXD" pad="4"/>
<connect gate="G$1" pin="TXD" pad="3"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="STEPPER-MOTOR-DRIVER-L6470">
<description>&lt;b&gt;Stepper Motor Driver&lt;/b&gt; based on &lt;b&gt;L6470&lt;/b&gt; chip
&lt;p&gt;More details can be found here:&lt;br /&gt;
&lt;a href="https://www.sparkfun.com/products/retired/10859"&gt;https://www.sparkfun.com/products/retired/10859&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;L6470&lt;/b&gt; datasheet is available here:&lt;br /&gt;
&lt;a href="www.st.com/resource/en/datasheet/CD00255075.pdf"&gt;www.st.com/resource/en/datasheet/CD00255075.pdf&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/l6470+breakout"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=STEPPER-MOTOR-DRIVER-L6470"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="STEPPER-MOTOR-DRIVER-L6470"/>
</gates>
<devices>
<device name="" package="STEPPER-MOTOR-DRIVER-L6470">
<connects>
<connect gate="G$1" pin="5V" pad="JP1.10"/>
<connect gate="G$1" pin="BSYN" pad="JP1.6"/>
<connect gate="G$1" pin="CK" pad="JP1.8"/>
<connect gate="G$1" pin="CSN" pad="JP1.5"/>
<connect gate="G$1" pin="FLGN" pad="JP1.4"/>
<connect gate="G$1" pin="GND.1" pad="JP5.2"/>
<connect gate="G$1" pin="GND.2" pad="JP8.2"/>
<connect gate="G$1" pin="GND.3" pad="JP1.1"/>
<connect gate="G$1" pin="O1A" pad="JP6.1"/>
<connect gate="G$1" pin="O1B" pad="JP6.2"/>
<connect gate="G$1" pin="O2A" pad="JP7.1"/>
<connect gate="G$1" pin="O2B" pad="JP7.2"/>
<connect gate="G$1" pin="R4.1" pad="R4.1"/>
<connect gate="G$1" pin="R4.2" pad="R4.2"/>
<connect gate="G$1" pin="R4.3" pad="R4.3"/>
<connect gate="G$1" pin="SDI" pad="JP1.7"/>
<connect gate="G$1" pin="SDO" pad="JP1.9"/>
<connect gate="G$1" pin="STBY" pad="JP1.2"/>
<connect gate="G$1" pin="STCK" pad="JP1.3"/>
<connect gate="G$1" pin="SW" pad="JP8.1"/>
<connect gate="G$1" pin="V+" pad="JP5.1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PWM-SERVO-DRIVER-16CH">
<description>&lt;b&gt;16-Channel 12-bit PWM/Servo Driver&lt;/b&gt; based on &lt;b&gt;PCA9685&lt;/b&gt; chip
&lt;p&gt;&lt;b&gt;PCA9685&lt;/b&gt; datasheet is available here:&lt;br /&gt;
&lt;a href="http://www.nxp.com/documents/data_sheet/PCA9685.pdf"&gt;http://www.nxp.com/documents/data_sheet/PCA9685.pdf&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Arduino Library&lt;/b&gt; for &lt;b&gt;PCA9685&lt;/b&gt; is available here:&lt;br /&gt;
&lt;a href="https://github.com/kasperskaarhoj/PCA9685-Arduino-Library"&gt;https://github.com/kasperskaarhoj/PCA9685-Arduino-Library&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/pwm+servo+module+pca9685"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=PWM-SERVO-DRIVER-16CH"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="PWM-SERVO-DRIVER-16CH"/>
</gates>
<devices>
<device name="" package="PWM-SERVO-DRIVER-16CH">
<connects>
<connect gate="G$1" pin="C0.GND" pad="C0.3"/>
<connect gate="G$1" pin="C0.PWM" pad="C0.1"/>
<connect gate="G$1" pin="C0.V+" pad="C0.2"/>
<connect gate="G$1" pin="C1.GND" pad="C1.3"/>
<connect gate="G$1" pin="C1.PWM" pad="C1.1"/>
<connect gate="G$1" pin="C1.V+" pad="C1.2"/>
<connect gate="G$1" pin="C10.GND" pad="C10.3"/>
<connect gate="G$1" pin="C10.PWM" pad="C10.1"/>
<connect gate="G$1" pin="C10.V+" pad="C10.2"/>
<connect gate="G$1" pin="C11.GND" pad="C11.3"/>
<connect gate="G$1" pin="C11.PWM" pad="C11.1"/>
<connect gate="G$1" pin="C11.V+" pad="C11.2"/>
<connect gate="G$1" pin="C12.GND" pad="C12.3"/>
<connect gate="G$1" pin="C12.PWM" pad="C12.1"/>
<connect gate="G$1" pin="C12.V+" pad="C12.2"/>
<connect gate="G$1" pin="C13.GND" pad="C13.3"/>
<connect gate="G$1" pin="C13.PWM" pad="C13.1"/>
<connect gate="G$1" pin="C13.V+" pad="C13.2"/>
<connect gate="G$1" pin="C14.GND" pad="C14.3"/>
<connect gate="G$1" pin="C14.PWM" pad="C14.1"/>
<connect gate="G$1" pin="C14.V+" pad="C14.2"/>
<connect gate="G$1" pin="C15.GND" pad="C15.3"/>
<connect gate="G$1" pin="C15.PWM" pad="C15.1"/>
<connect gate="G$1" pin="C15.V+" pad="C15.2"/>
<connect gate="G$1" pin="C2.GND" pad="C2.3"/>
<connect gate="G$1" pin="C2.PWM" pad="C2.1"/>
<connect gate="G$1" pin="C2.V+" pad="C2.2"/>
<connect gate="G$1" pin="C3.GND" pad="C3.3"/>
<connect gate="G$1" pin="C3.PWM" pad="C3.1"/>
<connect gate="G$1" pin="C3.V+" pad="C3.2"/>
<connect gate="G$1" pin="C4.GND" pad="C4.3"/>
<connect gate="G$1" pin="C4.PWM" pad="C4.1"/>
<connect gate="G$1" pin="C4.V+" pad="C4.2"/>
<connect gate="G$1" pin="C5.GND" pad="C5.3"/>
<connect gate="G$1" pin="C5.PWM" pad="C5.1"/>
<connect gate="G$1" pin="C5.V+" pad="C5.2"/>
<connect gate="G$1" pin="C6.GND" pad="C6.3"/>
<connect gate="G$1" pin="C6.PWM" pad="C6.1"/>
<connect gate="G$1" pin="C6.V+" pad="C6.2"/>
<connect gate="G$1" pin="C7.GND" pad="C7.3"/>
<connect gate="G$1" pin="C7.PWM" pad="C7.1"/>
<connect gate="G$1" pin="C7.V+" pad="C7.2"/>
<connect gate="G$1" pin="C8.GND" pad="C8.3"/>
<connect gate="G$1" pin="C8.PWM" pad="C8.1"/>
<connect gate="G$1" pin="C8.V+" pad="C8.2"/>
<connect gate="G$1" pin="C9.GND" pad="C9.3"/>
<connect gate="G$1" pin="C9.PWM" pad="C9.1"/>
<connect gate="G$1" pin="C9.V+" pad="C9.2"/>
<connect gate="G$1" pin="GND" pad="J1.1"/>
<connect gate="G$1" pin="GND.1" pad="JP3.6"/>
<connect gate="G$1" pin="GND.2" pad="JP4.6"/>
<connect gate="G$1" pin="OE.1" pad="JP3.5"/>
<connect gate="G$1" pin="OE.2" pad="JP4.5"/>
<connect gate="G$1" pin="SCL.1" pad="JP3.4"/>
<connect gate="G$1" pin="SCL.2" pad="JP4.4"/>
<connect gate="G$1" pin="SDA.1" pad="JP3.3"/>
<connect gate="G$1" pin="SDA.2" pad="JP4.3"/>
<connect gate="G$1" pin="V+" pad="J1.2"/>
<connect gate="G$1" pin="V+.1" pad="JP3.1"/>
<connect gate="G$1" pin="V+.2" pad="JP4.1"/>
<connect gate="G$1" pin="VCC.1" pad="JP3.2"/>
<connect gate="G$1" pin="VCC.2" pad="JP4.2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LEVEL-SHIFTER-8CH">
<description>&lt;b&gt;8-Channel Bi-Directional  Logic Level Converter&lt;/b&gt; based on &lt;b&gt;BSS128&lt;/b&gt; transistors
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/8+channel+level+converter"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;br /&gt;
&lt;b&gt;Note:&lt;/b&gt; There are many variants. Search for the proper version.&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=LEVEL-SHIFTER-8CH"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LEVEL-SHIFTER-8CH"/>
</gates>
<devices>
<device name="" package="LEVEL-SHIFTER-8CH">
<connects>
<connect gate="G$1" pin="GND.1" pad="J1.6"/>
<connect gate="G$1" pin="GND.2" pad="J2.6"/>
<connect gate="G$1" pin="HV" pad="J2.5"/>
<connect gate="G$1" pin="HV1" pad="J2.1"/>
<connect gate="G$1" pin="HV2" pad="J2.2"/>
<connect gate="G$1" pin="HV3" pad="J2.3"/>
<connect gate="G$1" pin="HV4" pad="J2.4"/>
<connect gate="G$1" pin="HV5" pad="J2.7"/>
<connect gate="G$1" pin="HV6" pad="J2.8"/>
<connect gate="G$1" pin="HV7" pad="J2.9"/>
<connect gate="G$1" pin="HV8" pad="J2.10"/>
<connect gate="G$1" pin="LV" pad="J1.5"/>
<connect gate="G$1" pin="LV1" pad="J1.1"/>
<connect gate="G$1" pin="LV2" pad="J1.2"/>
<connect gate="G$1" pin="LV3" pad="J1.3"/>
<connect gate="G$1" pin="LV4" pad="J1.4"/>
<connect gate="G$1" pin="LV5" pad="J1.7"/>
<connect gate="G$1" pin="LV6" pad="J1.8"/>
<connect gate="G$1" pin="LV7" pad="J1.9"/>
<connect gate="G$1" pin="LV8" pad="J1.10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LIGHT-SENSOR-BH1750">
<description>&lt;b&gt;Digital Light Sensor&lt;/b&gt; based on &lt;b&gt;BH1750&lt;/b&gt;
&lt;p&gt;&lt;b&gt;BH1750&lt;/b&gt; datasheet is available here:&lt;br /&gt;
&lt;a href="http://www.mouser.com/ds/2/348/bh1750fvi-e-186247.pdf"&gt;http://www.mouser.com/ds/2/348/bh1750fvi-e-186247.pdf&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Arduino Library&lt;/b&gt; for &lt;b&gt;BH1750&lt;/b&gt; is available here:&lt;br /&gt;
&lt;a href="https://github.com/claws/BH1750"&gt;https://github.com/claws/BH1750&lt;/a&gt;&lt;p/&gt;
&lt;p&gt;&lt;b&gt;Video Tutorial&lt;/b&gt; is available here:&lt;br /&gt;
&lt;a href="https://www.youtube.com/watch?v=UsLcHSbxf_8"&gt;https://www.youtube.com/watch?v=UsLcHSbxf_8&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/bh1750fvi+module"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;br /&gt;
&lt;b&gt;Note:&lt;/b&gt; There are many variants. Search for the proper version.&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=LIGHT-SENSOR-BH1750"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LIGHT-SENSOR-BH1750"/>
</gates>
<devices>
<device name="" package="LIGHT-SENSOR-BH1750">
<connects>
<connect gate="G$1" pin="ADDR" pad="5"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SCL" pad="3"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RANGING-SENSOR-VL53L0X">
<description>&lt;b&gt;Laser Ranging Sensor&lt;/b&gt; based on &lt;b&gt;VL53L0X&lt;/b&gt; device
&lt;p&gt;More information about &lt;b&gt;VL53L0X&lt;/b&gt; device can be found here:&lt;br /&gt;
&lt;a href="http://www.st.com/en/imaging-and-photonics-solutions/vl53l0x.html"&gt;http://www.st.com/en/imaging-and-photonics-solutions/vl53l0x.html&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Arduino Library&lt;/b&gt; for &lt;b&gt;VL53L0X&lt;/b&gt; is available here:&lt;br /&gt;
&lt;a href="https://github.com/pololu/vl53l0x-arduino"&gt;https://github.com/pololu/vl53l0x-arduino&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/GY+VL53L0X+module"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;br /&gt;
&lt;b&gt;Note:&lt;/b&gt; There are many variants. Search for the proper version.&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=RANGING-SENSOR-VL53L0X"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="RANGING-SENSOR-VL53L0X"/>
</gates>
<devices>
<device name="" package="RANGING-SENSOR-VL53L0X">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GPIO1" pad="5"/>
<connect gate="G$1" pin="SCL" pad="3"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="XSHUT" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WEMOS-D1-MINI-PRO">
<description>&lt;b&gt;WEMOS D1 mini Pro&lt;/b&gt;: Mini Wi-Fi Board based on &lt;b&gt;ESP-8266EX&lt;/b&gt; chip
&lt;p&gt;More details can be found here:&lt;br /&gt;
&lt;a href="https://www.wemos.cc/product/d1-mini-pro.html"&gt;https://www.wemos.cc/product/d1-mini-pro.html&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/wemos+d1+mini+pro"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=WEMOS-D1-MINI-PRO"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="WEMOS-D1-MINI-PRO"/>
</gates>
<devices>
<device name="" package="WEMOS-D1-MINI-PRO">
<connects>
<connect gate="G$1" pin="3V3" pad="JP1.8"/>
<connect gate="G$1" pin="5V" pad="JP2.8"/>
<connect gate="G$1" pin="A0" pad="JP1.2"/>
<connect gate="G$1" pin="D0" pad="JP1.3"/>
<connect gate="G$1" pin="D1" pad="JP2.3"/>
<connect gate="G$1" pin="D2" pad="JP2.4"/>
<connect gate="G$1" pin="D3" pad="JP2.5"/>
<connect gate="G$1" pin="D4" pad="JP2.6"/>
<connect gate="G$1" pin="D5" pad="JP1.4"/>
<connect gate="G$1" pin="D6" pad="JP1.5"/>
<connect gate="G$1" pin="D7" pad="JP1.6"/>
<connect gate="G$1" pin="D8" pad="JP1.7"/>
<connect gate="G$1" pin="GND" pad="JP2.7"/>
<connect gate="G$1" pin="RST" pad="JP1.1"/>
<connect gate="G$1" pin="RX" pad="JP2.2"/>
<connect gate="G$1" pin="TX" pad="JP2.1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WEMOS-D1-MINI-SHIELD">
<description>Template for &lt;b&gt;WEMOS D1 mini&lt;/b&gt; compatible shields
&lt;p&gt;&lt;b&gt;NOTICE:&lt;/b&gt; This is a template only.&lt;br /&gt;You can use it as a base to create symbols for &lt;b&gt;WEMOS D1 mini&lt;/b&gt; compatible shields.
&lt;p&gt;Official list of available shields can be found here:&lt;br /&gt;
&lt;a href="https://www.wemos.cc/D1-mini-Shields"&gt;https://www.wemos.cc/D1-mini-Shields&lt;/a&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="WEMOS-D1-MINI-SHIELD"/>
</gates>
<devices>
<device name="" package="WEMOS-D1-MINI-SHIELD">
<connects>
<connect gate="G$1" pin="3V3" pad="JP1.8"/>
<connect gate="G$1" pin="5V" pad="JP2.8"/>
<connect gate="G$1" pin="A0" pad="JP1.2"/>
<connect gate="G$1" pin="D0" pad="JP1.3"/>
<connect gate="G$1" pin="D1" pad="JP2.3"/>
<connect gate="G$1" pin="D2" pad="JP2.4"/>
<connect gate="G$1" pin="D3" pad="JP2.5"/>
<connect gate="G$1" pin="D4" pad="JP2.6"/>
<connect gate="G$1" pin="D5" pad="JP1.4"/>
<connect gate="G$1" pin="D6" pad="JP1.5"/>
<connect gate="G$1" pin="D7" pad="JP1.6"/>
<connect gate="G$1" pin="D8" pad="JP1.7"/>
<connect gate="G$1" pin="GND" pad="JP2.7"/>
<connect gate="G$1" pin="RST" pad="JP1.1"/>
<connect gate="G$1" pin="RX" pad="JP2.2"/>
<connect gate="G$1" pin="TX" pad="JP2.1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WEMOS-D1-MINI">
<description>&lt;b&gt;WEMOS D1 mini&lt;/b&gt;: Mini Wi-Fi Board based on &lt;b&gt;ESP-8266&lt;/b&gt; device
&lt;p&gt;More details can be found here:&lt;br /&gt;
&lt;a href="https://www.wemos.cc/product/d1-mini.html"&gt;https://www.wemos.cc/product/d1-mini.html&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/wemos+d1+mini+nodemcu"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=WEMOS-D1-MINI"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="WEMOS-D1-MINI"/>
</gates>
<devices>
<device name="" package="WEMOS-D1-MINI">
<connects>
<connect gate="G$1" pin="3V3" pad="JP1.8"/>
<connect gate="G$1" pin="5V" pad="JP2.8"/>
<connect gate="G$1" pin="A0" pad="JP1.2"/>
<connect gate="G$1" pin="D0" pad="JP1.3"/>
<connect gate="G$1" pin="D1" pad="JP2.3"/>
<connect gate="G$1" pin="D2" pad="JP2.4"/>
<connect gate="G$1" pin="D3" pad="JP2.5"/>
<connect gate="G$1" pin="D4" pad="JP2.6"/>
<connect gate="G$1" pin="D5" pad="JP1.4"/>
<connect gate="G$1" pin="D6" pad="JP1.5"/>
<connect gate="G$1" pin="D7" pad="JP1.6"/>
<connect gate="G$1" pin="D8" pad="JP1.7"/>
<connect gate="G$1" pin="GND" pad="JP2.7"/>
<connect gate="G$1" pin="RST" pad="JP1.1"/>
<connect gate="G$1" pin="RX" pad="JP2.2"/>
<connect gate="G$1" pin="TX" pad="JP2.1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEMP-HUM-SENSOR-AM2322">
<description>&lt;b&gt;AM2322 - digital humidity &amp; temperature sensor&lt;/b&gt;
&lt;p&gt;More information about &lt;b&gt;AM2322&lt;/b&gt; is available here:&lt;br&gt;
&lt;a href="http://www.electrodragon.com/w/AM2322"&gt;http://www.electrodragon.com/w/AM2322&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/am2322+digital+sensor"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=TEMP-HUM-SENSOR-AM2322"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TEMP-HUM-SENSOR-AM2322"/>
</gates>
<devices>
<device name="" package="TEMP-HUM-SENSOR-AM2322">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="SCL" pad="4"/>
<connect gate="G$1" pin="SDA" pad="2"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB-SERIAL-CP2102">
<description>&lt;b&gt;USB to Serial UART Converter&lt;/b&gt; based on &lt;b&gt;CP2102&lt;/b&gt; chip
&lt;p&gt;More information about &lt;b&gt;CP2102&lt;/b&gt; chip is available here:&lt;br&gt;
&lt;a href="https://www.silabs.com/documents/public/data-sheets/CP2102-9.pdf"&gt;https://www.silabs.com/documents/public/data-sheets/CP2102-9.pdf&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Drivers for &lt;b&gt;CP210x&lt;/b&gt; devices are available here:&lt;br&gt;
&lt;a href="http://www.silabs.com/products/development-tools/software/usb-to-uart-bridge-vcp-drivers"&gt;http://www.silabs.com/products/development-tools/software/usb-to-uart-bridge-vcp-drivers&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/cp2102+micro+usb"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=USB-SERIAL-CP2102"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="USB-SERIAL-CP2102"/>
</gates>
<devices>
<device name="" package="USB-SERIAL-CP2102">
<connects>
<connect gate="G$1" pin="+5V" pad="6"/>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="DTR" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="RXI" pad="3"/>
<connect gate="G$1" pin="TDO" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DC-DC-STEP-UP-MT3608">
<description>&lt;b&gt;DC/DC Step-Up Regulator&lt;/b&gt; based on &lt;b&gt;MT3608&lt;/b&gt; chip

&lt;p&gt;&lt;b&gt;MT3608&lt;/b&gt; datasheet available here:&lt;br /&gt;
&lt;a href="https://www.olimex.com/Products/Breadboarding/BB-PWR-3608/resources/MT3608.pdf"&gt;https://www.olimex.com/Products/Breadboarding/BB-PWR-3608/resources/MT3608.pdf&lt;/a&gt;&lt;/p&gt;

&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/mt3608+module"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=DC-DC-STEP-UP-MT3608"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DC-DC-STEP-UP-MT3608"/>
</gates>
<devices>
<device name="" package="DC-DC-STEP-UP-MT3608">
<connects>
<connect gate="G$1" pin="IN+" pad="IN+"/>
<connect gate="G$1" pin="IN-" pad="IN-"/>
<connect gate="G$1" pin="OUT+" pad="OUT+"/>
<connect gate="G$1" pin="OUT-" pad="OUT-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISPLAY-OLED-128X64-I2C">
<description>&lt;b&gt;128x64 Dot Matrix OLED Module&lt;/b&gt; based on &lt;b&gt;SSD1306&lt;/b&gt; chip&lt;br /&gt;
Variant with &lt;b&gt;I2C interface&lt;/b&gt;
&lt;p&gt;More details available here:&lt;br /&gt;
&lt;a href="http://www.instructables.com/id/Monochrome-096-i2c-OLED-display-with-arduino-SSD13/"&gt;http://www.instructables.com/id/Monochrome-096-i2c-OLED-display-with-arduino-SSD13/&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SSD1306&lt;/b&gt; datasheet:&lt;br&gt;
&lt;a href="https://cdn-shop.adafruit.com/datasheets/SSD1306.pdf"&gt;https://cdn-shop.adafruit.com/datasheets/SSD1306.pdf&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/oled+display+128x64+iic"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;br /&gt;
&lt;b&gt;Note:&lt;/b&gt; There are two variants: I2C and SPI. Search for the proper version.&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=DISPLAY-OLED-128X64-I2C"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DISPLAY-OLED-128X64-I2C"/>
</gates>
<devices>
<device name="" package="DISPLAY-OLED-128X64-I2C">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="SCL" pad="3"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="REG-AMS1117-3P-*">
<description>&lt;b&gt;Linear Regulator&lt;/b&gt; based on &lt;b&gt;AMS1117&lt;/b&gt; chip&lt;br /&gt;
3-pin version
&lt;p&gt;&lt;b&gt;AMS1117&lt;/b&gt; datasheet is available here:&lt;br /&gt;
&lt;a href="http://www.advanced-monolithic.com/pdf/ds1117.pdf"&gt;http://www.advanced-monolithic.com/pdf/ds1117.pdf&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/ams1117+module"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;br /&gt;
&lt;b&gt;Note:&lt;/b&gt; There are many variants. Search for the proper version.&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=REG-AMS1117-3P"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="REG-AMS1117-3P"/>
</gates>
<devices>
<device name="" package="REG-AMS1117-3P">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name="3.3V"/>
<technology name="5.0V"/>
</technologies>
</device>
<device name="#V" package="REG-AMS1117-3P#V">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name="3.3V"/>
<technology name="5.0V"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AC-VOLTAGE-SENSOR">
<description>&lt;b&gt;Isolated AC Voltage Sensor&lt;/b&gt; based on &lt;b&gt;ZMPT101B&lt;/b&gt; transformer
&lt;p&gt;&lt;b&gt;ZMPT101B&lt;/b&gt; Voltage Transformer Operating Guide is available here:&lt;br /&gt;
&lt;a href="http://www.zeming-e.com/file/0_2013_10_18_093344.pdf"&gt;http://www.zeming-e.com/file/0_2013_10_18_093344.pdf&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/arduino+voltage+transformer"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=AC-VOLTAGE-SENSOR"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="AC-VOLTAGE-SENSOR"/>
</gates>
<devices>
<device name="" package="AC-VOLTAGE-SENSOR">
<connects>
<connect gate="G$1" pin="GND.1" pad="2"/>
<connect gate="G$1" pin="GND.2" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AC-VOLTAGE-SENSOR#IC">
<description>&lt;b&gt;Isolated AC Voltage Sensor&lt;/b&gt; based on &lt;b&gt;ZMPT101B&lt;/b&gt; transformer&lt;br /&gt;
Symbol with input connector
&lt;p&gt;&lt;b&gt;ZMPT101B&lt;/b&gt; Voltage Transformer Operating Guide is available here:&lt;br /&gt;
&lt;a href="http://www.zeming-e.com/file/0_2013_10_18_093344.pdf"&gt;http://www.zeming-e.com/file/0_2013_10_18_093344.pdf&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/arduino+voltage+transformer"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=AC-VOLTAGE-SENSOR"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="AC-VOLTAGE-SENSOR#IC"/>
</gates>
<devices>
<device name="" package="AC-VOLTAGE-SENSOR#IC">
<connects>
<connect gate="G$1" pin="GND.1" pad="2"/>
<connect gate="G$1" pin="GND.2" pad="1"/>
<connect gate="G$1" pin="L" pad="P1.1"/>
<connect gate="G$1" pin="N" pad="P1.2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WIRELESS-BLUETOOTH-HC-05">
<description>&lt;b&gt;Bluetooth Transceiver Module&lt;/b&gt; based on &lt;b&gt;HC-05&lt;/b&gt; board
&lt;p&gt;Tutorial is available here:&lt;br /&gt;
&lt;a href="https://arduino-info.wikispaces.com/BlueTooth-HC05-HC06-Modules-How-To"&gt;https://arduino-info.wikispaces.com/BlueTooth-HC05-HC06-Modules-How-To&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/hc-05+module+rs232"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=WIRELESS-BLUETOOTH-HC-05"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="WIRELESS-BLUETOOTH-HC-05"/>
</gates>
<devices>
<device name="" package="WIRELESS-BLUETOOTH-HC-05">
<connects>
<connect gate="G$1" pin="+5V" pad="5"/>
<connect gate="G$1" pin="EN" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="RX" pad="2"/>
<connect gate="G$1" pin="STATE" pad="1"/>
<connect gate="G$1" pin="TX" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JOYSTICK-2AXIS-BUTTON">
<description>&lt;b&gt;2-Axis Analog Joystick&lt;/b&gt; with Push Button
&lt;p&gt;Tutorial is available here:&lt;br /&gt;
&lt;a href="http://henrysbench.capnfatz.com/henrys-bench/arduino-sensors-and-input/arduino-ps2-joystick-tutorial-keyes-ky-023-deek-robot/"&gt;http://henrysbench.capnfatz.com/henrys-bench/arduino-sensors-and-input/arduino-ps2-joystick-tutorial-keyes-ky-023-deek-robot/&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/joystick+ps2+module"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=JOYSTICK-2AXIS-BUTTON"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="JOYSTICK-2AXIS-BUTTON"/>
</gates>
<devices>
<device name="" package="JOYSTICK-2AXIS-BUTTON">
<connects>
<connect gate="G$1" pin="+5V" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="SW" pad="5"/>
<connect gate="G$1" pin="VRX" pad="3"/>
<connect gate="G$1" pin="VRY" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DC-DC-STEP-DOWN-MP1584">
<description>&lt;b&gt;DC/DC Step-Down Regulator&lt;/b&gt; based on &lt;b&gt;MP1584&lt;/b&gt; chip
&lt;p&gt;&lt;b&gt;MP1584&lt;/b&gt; datasheet available here:&lt;br /&gt;
&lt;a href="http://www.haoyuelectronics.com/Attachment/MP1584/MP1584.pdf"&gt;http://www.haoyuelectronics.com/Attachment/MP1584/MP1584.pdf&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;&lt;a href="http://www.ebay.com/sch/mp1584+module"&gt;Click here to find device on ebay.com&lt;/a&gt;&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;&lt;img alt="photo" src="http://www.diymodules.org/img/device-photo.php?name=DC-DC-STEP-DOWN-MP1584"&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DC-DC-STEP-DOWN-MP1584"/>
</gates>
<devices>
<device name="" package="DC-DC-STEP-DOWN-MP1584">
<connects>
<connect gate="G$1" pin="IN+.1" pad="IN+.1"/>
<connect gate="G$1" pin="IN+.2" pad="IN+.2"/>
<connect gate="G$1" pin="IN-.1" pad="IN-.1"/>
<connect gate="G$1" pin="IN-.2" pad="IN-.2"/>
<connect gate="G$1" pin="OUT+.1" pad="OUT+.1"/>
<connect gate="G$1" pin="OUT+.2" pad="OUT+.2"/>
<connect gate="G$1" pin="OUT-.1" pad="OUT-.1"/>
<connect gate="G$1" pin="OUT-.2" pad="OUT-.2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
