<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<library>
<description>&lt;h3&gt;SparkFun LilyPad Wearables&lt;/h3&gt;
This library contains button holes, sewtaps and petals used on our LilyPad boards. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PETAL-NOHOLE">
<description>&lt;h3&gt;Petal- No Hole &lt;/h3&gt;
Petal for wearable applications. No sew tap present- this is only for aesthetics on the board. Petal only on top layer.
&lt;p&gt;Specifications:
&lt;ul&gt;
&lt;li&gt;Petal Size: 0.2in wide, 0.1in height  &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;SEWTAP-NOHOLE&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="BUTTONHOLE-SM">
<description>&lt;h3&gt;Button Hole Small - Sewable connection point&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 1&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1 inches&lt;/li&gt;
&lt;li&gt;Hole count: 2&lt;/li&gt;
&lt;li&gt;Drill Hit: 0.06in  &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;BUTTONHOLE&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="BUTTONHOLE">
<description>&lt;h3&gt;Button Hole - Sewable connection point&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 1&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.2inches&lt;/li&gt;
&lt;li&gt;Hole count: 2&lt;/li&gt;
&lt;li&gt;Drill Hit: 0.08in  &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;BUTTONHOLE&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="PETAL-LONG-1">
<description>&lt;h3&gt;Petal-Long&lt;/h3&gt;
Sew tap with petal for wearable applications. Petal surronds sew tap and has concave edge for aesthetic design. Petal only on top layer.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 1&lt;/li&gt;
&lt;li&gt;Petal Size: 0.2in wide,0.2in height  &lt;/li&gt;
&lt;li&gt;Drill Hit: 0.11in  &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;SEWTAP&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="PETAL-LONG-2">
<description>&lt;h3&gt;Petal-Long - 2&lt;/h3&gt;
Sew tap with petal for wearable applications. Petal surronds sew tap and has convex point. Petal only on top layer.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 1&lt;/li&gt;
&lt;li&gt;Petal Size: 0.2in wide,0.25in height  &lt;/li&gt;
&lt;li&gt;Drill Hit: 0.11in  &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;SEWTAP&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="PETAL-MEDIUM">
<description>&lt;h3&gt;Petal-Medium &lt;/h3&gt;
Sew tap with petal for wearable applications. Petal overlaps sew tap. Petal only on top layer.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 1&lt;/li&gt;
&lt;li&gt;Petal Size: 0.3in wide,0.1in height  &lt;/li&gt;
&lt;li&gt;Drill Hit: 0.11in  &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;SEWTAP&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="PETAL-LARGE">
<description>&lt;h3&gt;Petal-Large&lt;/h3&gt;
Sew tap with petals for wearable applications. Petal only on top layer.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 1&lt;/li&gt;
&lt;li&gt;Petal Size: 0.4in wide,0.15in height  &lt;/li&gt;
&lt;li&gt;Drill Hit: 0.11in  &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;SEWTAP&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="PETAL-SMALL">
<description>&lt;h3&gt;Petal-Small &lt;/h3&gt;
Sew tap with petal for wearable applications. Petal overlaps sew tap. Petal only on top layer.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 1&lt;/li&gt;
&lt;li&gt;Petal Size: 0.2in wide,0.1in height  &lt;/li&gt;
&lt;li&gt;Drill Hit: 0.08in  &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;SEWTAP&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="PETAL-SMALL-2SIDE">
<description>&lt;h3&gt;Petal-Small &lt;/h3&gt;
Sew tap with petal for wearable applications. Petal overlaps sew tap. Petal on top and bottom layers.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 1&lt;/li&gt;
&lt;li&gt;Petal Size: 0.2in wide,0.1in height  &lt;/li&gt;
&lt;li&gt;Drill Hit: 0.08in  &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;SEWTAP&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="PETAL-NOHOLE-2SIDE">
<description>&lt;h3&gt;Petal- No Hole &lt;/h3&gt;
Petal for wearable applications. No sew tap present- this is only for aesthetics on the board. Petal on top and bottom layers.
&lt;p&gt;Specifications:
&lt;ul&gt;
&lt;li&gt;Petal Size: 0.2in wide, 0.1in height  &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;SEWTAP-NOHOLE&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="PETAL-LARGE-2SIDE">
<description>&lt;h3&gt;Petal-Large 2 Side&lt;/h3&gt;
Sew tap with petals for wearable applications. Petals on top and bottom layers.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 1&lt;/li&gt;
&lt;li&gt;Petal Size: 0.4in wide,0.15in height  &lt;/li&gt;
&lt;li&gt;Drill Hit: 0.11in  &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;SEWTAP&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="PETAL-MEDIUM-2SIDE">
<description>&lt;h3&gt;Petal-Medium 2 Side &lt;/h3&gt;
Sew tap with petal for wearable applications. Petal overlaps sew tap.Petal on top and bottom layers.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 1&lt;/li&gt;
&lt;li&gt;Petal Size: 0.3in wide,0.1in height  &lt;/li&gt;
&lt;li&gt;Drill Hit: 0.11in  &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;SEWTAP&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="PETAL-LONG-1-2SIDE">
<description>&lt;h3&gt;Petal-Long 2 Side&lt;/h3&gt;
Sew tap with petal for wearable applications. Petal surronds sew tap and has concave edge for aesthetic design. Petal on top and bottom layer.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 1&lt;/li&gt;
&lt;li&gt;Petal Size: 0.2in wide,0.2in height  &lt;/li&gt;
&lt;li&gt;Drill Hit: 0.11in  &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;SEWTAP&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="PETAL-LONG-2-2SIDE">
<description>&lt;h3&gt;Petal-Long - 2&lt;/h3&gt;
Sew tap with petal for wearable applications. Petal surronds sew tap and has convex point. Petal on top and bottom layers.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 1&lt;/li&gt;
&lt;li&gt;Petal Size: 0.2in wide,0.25in height  &lt;/li&gt;
&lt;li&gt;Drill Hit: 0.11in  &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;SEWTAP&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="PETAL-TINY">
<description>&lt;h3&gt;Petal-Tiny &lt;/h3&gt;
Sew tap with petal for wearable applications. Petal overlaps sew tap. Petal on top and bottom layers.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 1&lt;/li&gt;
&lt;li&gt;Petal Size: 0.1in wide,0.05in height  &lt;/li&gt;
&lt;li&gt;Drill Hit: 0.04in  &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;SEWTAP&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="PETAL-MEDIUM-2SIDE-NOHOLE">
<description>&lt;h3&gt;Petal-Medium 2-Side No Hole &lt;/h3&gt;
Petal for wearable applications. No sew tap present- this is only for aesthetics on the board. Petal on top and bottom layers.
&lt;p&gt;Specifications:
&lt;ul&gt;
&lt;li&gt;Petal Size: 0.3in wide,0.1in height  &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;SEWTAP-NOHOLE&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="PETAL-MEDIUM-NOHOLE">
<description>&lt;h3&gt;Petal-Medium 2-Side No Hole &lt;/h3&gt;
Petal for wearable applications. No sew tap present- this is only for aesthetics on the board. Petal only on top layer.
&lt;p&gt;Specifications:
&lt;ul&gt;
&lt;li&gt;Petal Size: 0.3in wide,0.1in height  &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;SEWTAP-NOHOLE&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
<symbols>
<symbol name="BUTTONHOLE">
<description>&lt;h3&gt;SparkFun Button Hole Connector&lt;/h3&gt;
&lt;p&gt;Sewable button-hole connector&lt;/p&gt;</description>
<pin name="P$1"/>
</symbol>
<symbol name="SEWTAP-NO_CONNECTION">
<description>&lt;h3&gt;SparkFun SewTap without Holes&lt;/h3&gt;
&lt;p&gt;Symbol for aesthetic sew tap - no holes, and no connections available&lt;/p&gt;</description>
</symbol>
<symbol name="SEWTAP">
<description>&lt;h3&gt;Sew Tap&lt;/h3&gt;
&lt;p&gt;Basic connector for sew taps for wearable boards&lt;/p&gt;</description>
<pin name="1"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="BUTTONHOLE" prefix="J">
<description>&lt;h3&gt;SparkFun Button Hole - Sewable button holes for connectors&lt;/h3&gt;
&lt;p&gt;Enables users to sew connections in wearables projects.&lt;/p&gt;
&lt;p&gt;SparkFun Products:
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/11214”&gt;MOSFET Power Controller&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BUTTONHOLE"/>
</gates>
<devices>
<device name="LARGE" package="BUTTONHOLE">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMALL" package="BUTTONHOLE-SM">
<connects>
<connect gate="G$1" pin="P$1" pad="P$3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEWTAP-NOHOLE" prefix="J">
<description>&lt;h3&gt;SparkFun LilyPad Sew Taps without Holes&lt;/h3&gt;
&lt;p&gt;Petals used for PCB aesthetics. No connection points for circuits, and no hole available for sewing.&lt;/p&gt;
&lt;p&gt;SparkFun Products:
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11008"&gt; LilyPad Vibe Board&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9267"&gt; LilyPad Accelerometer&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/8463"&gt;LilyPad Buzzer&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SEWTAP-NO_CONNECTION"/>
</gates>
<devices>
<device name="&quot;" package="PETAL-NOHOLE">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_2SIDE" package="PETAL-NOHOLE-2SIDE">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_MEDIUM-2SIDE" package="PETAL-MEDIUM-2SIDE-NOHOLE">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_MEDIUM" package="PETAL-MEDIUM-NOHOLE">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEWTAP" prefix="J">
<description>&lt;h3&gt;SparkFun LilyPad Sew Taps&lt;/h3&gt;
&lt;p&gt;Sewable connection points for LilyPad Boards&lt;/p&gt;
&lt;p&gt;SparkFun Products:
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13342”&gt;LilyPad Arduino 328 Main Board&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/10899”&gt;LilyTiny&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/11259”&gt;LilyPad Power Supply&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SEWTAP"/>
</gates>
<devices>
<device name="_LONG" package="PETAL-LONG-1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_LONG_ROUND" package="PETAL-LONG-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_MEDIUM" package="PETAL-MEDIUM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_LARGE" package="PETAL-LARGE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_SMALL" package="PETAL-SMALL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_SMALL-2SIDE" package="PETAL-SMALL-2SIDE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_LARGE-2SIDE" package="PETAL-LARGE-2SIDE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_MEDIUM-2SIDE" package="PETAL-MEDIUM-2SIDE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_LONG-2SIDE" package="PETAL-LONG-1-2SIDE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_LONG_ROUND-2SIDE" package="PETAL-LONG-2-2SIDE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_TINY" package="PETAL-TINY">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
