<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.1">
<drawing>
<library>
<description>&lt;h3&gt;SparkFun Coils&lt;/h3&gt;
In this library you'll find magnetics.

&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;Inductors&lt;/li&gt;
&lt;li&gt;Ferrite Beads&lt;/li&gt;
&lt;li&gt;Transformers&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;

&lt;br&gt;
&lt;p&gt;We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.&lt;/p&gt;</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="CR54">
<description>&lt;h3&gt;CR54 footprint&lt;/h3&gt;
&lt;p&gt;These vary by manufacturer, but we used the NPIS54LS footprint from &lt;a href="http://www.niccomp.com/catalog/npis_ls.pdf"&gt;here&lt;/a&gt;.</description>
</package>
<package name="CR75">
<description>&lt;h3&gt;4600 series footprint&lt;/h3&gt;
&lt;p&gt;Not messing with it since production uses it. Origin unknown but loosely based on this &lt;a href="http://www.murata-ps.com/data/magnetics/kmp_4600.pdf"&gt;datasheet&lt;/a&gt;.&lt;/p&gt;</description>
</package>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="SRN6045">
<description>&lt;h3&gt;SRN6045 series  footprint&lt;/h3&gt;
&lt;p&gt;Roughly based on the recommendation in this &lt;a href="http://www.mouser.com/ds/2/54/RN6045-778135.pdf"&gt;datasheet&lt;/a&gt;.&lt;/p&gt;</description>
</package>
<package name="INDUCTOR_4.7UH">
<description>&lt;h3&gt;CDRH2D18/HPNP footprint&lt;/h3&gt;
&lt;p&gt;Recommended footprint for CDRH2D18/HPNP series inductors from &lt;a href="http://products.sumida.com/products/pdf/CDRH2D18HP.pdf"&gt;here&lt;/a&gt;.&lt;/p&gt;</description>
</package>
<package name="INDUCTOR_SDR1307">
<description>&lt;h3&gt;SDR1307 series footprint&lt;/h3&gt;
&lt;p&gt;Footprint based on recommendation from &lt;a href="https://www.bourns.com/pdfs/SDR1307.pdf"&gt;here&lt;/a&gt;.&lt;/p&gt;</description>
</package>
<package name="0402">
<description>&lt;p&gt;&lt;b&gt;Generic 1005 (0402) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="COILCRAFT_DA230X">
<description>Coilcraft DA2303, DA2304</description>
</package>
<package name="TRANSFORMER">
</package>
<package name="TRANSFORMER_SMD">
<description>TTC-5023</description>
</package>
<package name="INDUCTOR_2.2UH">
</package>
<package name="INDUCTOR_4X4MM">
<description>&lt;h3&gt;4x4mm Inductor&lt;/h3&gt;
&lt;p&gt;This footprint may be acceptable for many 4x4mm inductors.  It was produced from the datasheet &lt;a href="http://www.vishay.com/docs/34295/sc15ah01.pdf"&gt;here&lt;/a&gt;, for the Vishay Dale IFSC1515AHER2R2M01.</description>
</package>
<package name="INDUCTOR-SRP4020">
</package>
<package name="INDUCTOR_LQH32">
</package>
<package name="INDUCTOR_3X3">
<description>&lt;h3&gt;Inductor - 3.0mm x 3.0mm&lt;/h3&gt;
&lt;p&gt;&lt;a href=file:///C:/Users/guita/Downloads/NRH3012T100MN_SS.pdf&gt;Example Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="XFL4020">
</package>
<package name="0806">
<description>&lt;h3&gt;2.2uH, 1.2A, Shielded 0806 Inductor&lt;/h3&gt;

Physical Characteristics: 
&lt;ul&gt;
&lt;li&gt;0806 Package (2016 metric)&lt;/li&gt;
&lt;li&gt;Landing Pads: 1.8 X .8mm&lt;/li&gt;
&lt;/ul&gt;</description>
</package>
<package name="MA5532-AE">
<description>&lt;h3&gt;MA5532-AE&lt;/h3&gt;

&lt;p&gt;Physical Characteristics&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;.461in x .138in x .102in&lt;/li&gt;
&lt;li&gt;Pads on part surrounded by housing.&lt;/li&gt;
&lt;li&gt;&lt;/li&gt;
&lt;/ul&gt;</description>
</package>
<package name="0402-TIGHT">
</package>
<package name="0805-WIDE">
</package>
<package name="0603_MURATA">
</package>
<package name="0402_MURATA">
</package>
</packages>
<symbols>
<symbol name="INDUCTOR">
<description>&lt;h3&gt;Inductors&lt;/h3&gt;
&lt;p&gt;Resist changes in electrical current. Basically a coil of wire.&lt;/p&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="FERRITE_BEAD">
<description>&lt;h3&gt;Ferrite Bead (blocks, cores, rings, chokes, etc.)&lt;/h3&gt;
&lt;p&gt;Inductor with layers of ferrite used to suppress high frequencies. Often used to isolate high frequency noise.&lt;/p&gt;</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="TRANSFORMER">
<pin name="1"/>
<pin name="4"/>
<pin name="2"/>
<pin name="3"/>
</symbol>
<symbol name="TRANSFORMER-QUADFILIAR">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="FERRITE_BEAD" prefix="FB">
<description>&lt;h3&gt;Ferrite Bead (blocks, cores, rings, chokes, etc.)&lt;/h3&gt;
&lt;p&gt;Inductor with layers of ferrite used to suppress high frequencies. Often used to isolate high frequency noise.&lt;/p&gt;
&lt;p&gt;SparkFun Products:
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13613"&gt;IOIO-OTG - V2.2&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13664"&gt;SparkFun SAMD21 Mini Breakout&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13339"&gt;SparkFun 6 Degrees of Freedom Breakout - LSM6DS3&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13672"&gt;SparkFun SAMD21 Dev Breakout&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="FERRITE_BEAD"/>
</gates>
<devices>
<device name="-0603" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NDUC-13805"/>
<attribute name="VALUE" value="30Ω/1.8A"/>
</technology>
</technologies>
</device>
<device name="" package="0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRANSFORMER">
<description>Small transformers</description>
<gates>
<gate name="G$1" symbol="TRANSFORMER"/>
</gates>
<devices>
<device name="PTH" package="TRANSFORMER">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="TRANSFORMER_SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRANSFORMER_QUADFILIAR" prefix="TX">
<description>Transformer with 4 independent windings</description>
<gates>
<gate name="G$1" symbol="TRANSFORMER-QUADFILIAR"/>
</gates>
<devices>
<device name="" package="COILCRAFT_DA230X">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
<connect gate="G$1" pin="3" pad="P$3"/>
<connect gate="G$1" pin="4" pad="P$4"/>
<connect gate="G$1" pin="5" pad="P$5"/>
<connect gate="G$1" pin="6" pad="P$6"/>
<connect gate="G$1" pin="7" pad="P$7"/>
<connect gate="G$1" pin="8" pad="P$8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INDUCTOR" prefix="L" uservalue="yes">
<description>&lt;h3&gt;Inductors&lt;/h3&gt;
&lt;p&gt;Resist changes in electrical current. Basically a coil of wire.&lt;/p&gt;
&lt;p&gt;SparkFun Products:
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13879"&gt;SparkFun Load Cell Amplifier - HX711&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13613"&gt;IOIO-OTG - V2.2&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=""&gt;&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="INDUCTOR"/>
</gates>
<devices>
<device name="-CR75-68UH" package="CR75">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NDUC-09739"/>
<attribute name="VALUE" value="68µH/±20%/1.05A"/>
</technology>
</technologies>
</device>
<device name="-SRN6045-33UH" package="SRN6045">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NDUC-11627"/>
<attribute name="VALUE" value="33µH/±20%/1.4A"/>
</technology>
</technologies>
</device>
<device name="-CDRH-4.7UH" package="INDUCTOR_4.7UH">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NDUC-10146"/>
<attribute name="VALUE" value="4.7µH/±30%/1.2A"/>
</technology>
</technologies>
</device>
<device name="-SDR13-27UH" package="INDUCTOR_SDR1307">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NDUC-12529"/>
<attribute name="VALUE" value="27µH/±20%/3.3A"/>
</technology>
</technologies>
</device>
<device name="-CR54-3.3UH" package="CR54">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NDUC-11157"/>
<attribute name="VALUE" value="3.3µH/±30%/3.4A"/>
</technology>
</technologies>
</device>
<device name="-CR54-47UH" package="CR54">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NDUC-10789"/>
<attribute name="VALUE" value="47µH/±30%/750mA"/>
</technology>
</technologies>
</device>
<device name="-0805-3.3UH" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NDUC-13076"/>
<attribute name="VALUE" value="3.3µH/±20%/450mA"/>
</technology>
</technologies>
</device>
<device name="-0603-33NH" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NDUC-07874"/>
<attribute name="VALUE" value="33nH/±5%/500mA"/>
</technology>
</technologies>
</device>
<device name="-0402-3.9NH" package="0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NDUC-13457"/>
<attribute name="VALUE" value="3.9NH"/>
</technology>
</technologies>
</device>
<device name="INDUCTOR_10UH" package="INDUCTOR_3X3">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NDUC-13913"/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
<device name="-CDRH-10UH" package="INDUCTOR_4.7UH">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NDUC-13968"/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
<device name="FB-30OHM" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NDUC-07859"/>
</technology>
</technologies>
</device>
<device name="" package="XFL4020">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0603-15NH" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NDUC-11660"/>
<attribute name="VALUE" value="15nH"/>
</technology>
</technologies>
</device>
<device name="-LHQ32-15UH" package="INDUCTOR_LQH32">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NDUC-14107"/>
<attribute name="VALUE" value="15uH"/>
</technology>
</technologies>
</device>
<device name="-0402_TIGHT-2.0NH" package="0402-TIGHT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NDUC-14238"/>
<attribute name="VALUE" value="2nH/?%/200mA/300mOhm"/>
</technology>
</technologies>
</device>
<device name="-0805_WIDE-1.0UH" package="0805-WIDE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NDUC-14237"/>
<attribute name="VALUE" value="1.0uH/?%/1.4A/70mOhm"/>
</technology>
</technologies>
</device>
<device name="-0402_TIGHT-2.7NH" package="0402-TIGHT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NDUC-14236"/>
<attribute name="VALUE" value="2.7nH/?%/900mA/70mOhm"/>
</technology>
</technologies>
</device>
<device name="-0805_WIDE-2.2UH" package="0805-WIDE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NDUC-14234"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INDUCTOR-XFL4020" prefix="L" uservalue="yes">
<gates>
<gate name="G$1" symbol="INDUCTOR"/>
</gates>
<devices>
<device name="" package="XFL4020">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="1.5UH">
<attribute name="PROD_ID" value="INDUC-13855"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FERRITE_BEAD-120_OHM" prefix="FB">
<description>&lt;h3&gt;Ferrite Bead (blocks, cores, rings, chokes, etc.)&lt;/h3&gt;
&lt;p&gt;Inductor with layers of ferrite used to suppress high frequencies. Often used to isolate high frequency noise.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="FERRITE_BEAD"/>
</gates>
<devices>
<device name="-0402" package="0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MFG_PART" value="BLM15HB121SN1D"/>
<attribute name="PROD_ID" value="NDUC-14206"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2.2μH_SHIELDED_INDUCTOR" prefix="L">
<description>&lt;h3&gt;Murata 2.2uH Inductor&lt;/h3&gt;

&lt;ul&gt;
&lt;li&gt;2.2uH&lt;/li&gt;
&lt;li&gt;1.2A&lt;/li&gt;
&lt;li&gt;110mOhm&lt;/li&gt;
&lt;li&gt;0806 Package&lt;/li&gt;
&lt;li&gt;Shielded&lt;/li&gt;
&lt;li&gt;&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="INDUCTOR"/>
</gates>
<devices>
<device name="" package="0806">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NDUC-14257"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MA5532-AE" prefix="L">
<description>&lt;h3&gt;RFID Transponder Coil - MA5532-AE&lt;/h3&gt;

&lt;p&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="INDUCTOR"/>
</gates>
<devices>
<device name="" package="MA5532-AE">
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NDUC-11334"/>
<attribute name="VALUE" value="100uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2.2μH" prefix="L" uservalue="yes">
<description>&lt;h3&gt;2.2μH Inductor&lt;/h3&gt;
&lt;p&gt;Resist changes in electrical current. Basically a coil of wire.&lt;/p&gt;
&lt;p&gt;SparkFun Products:
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/15170"&gt;SparkFun Edge - HX711&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=""&gt;&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="L1" symbol="INDUCTOR"/>
</gates>
<devices>
<device name="-0805_WIDE-2.2μH-1.7A-0.14OHM" package="0805-WIDE">
<connects>
<connect gate="L1" pin="1" pad="1"/>
<connect gate="L1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NDUC-14234"/>
<attribute name="VALUE" value="2.2μH"/>
</technology>
</technologies>
</device>
<device name="-4X4-2.2μH-3A-45MOHM" package="INDUCTOR_4X4MM">
<connects>
<connect gate="L1" pin="1" pad="P$1"/>
<connect gate="L1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NDUC-13770"/>
<attribute name="VALUE" value="2.2μH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1.0μH" prefix="L" uservalue="yes">
<description>&lt;h3&gt;1.0μH Inductor&lt;/h3&gt;
&lt;p&gt;Resist changes in electrical current. Basically a coil of wire.&lt;/p&gt;
&lt;p&gt;SparkFun Products:
&lt;ul&gt;&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/15170"&gt;SparkFun Edge&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=""&gt;&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="INDUCTOR"/>
</gates>
<devices>
<device name="-0805_WIDE-1.0μH-1.4A-0.07OHM-1.4MM_H" package="0805-WIDE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NDUC-14237"/>
<attribute name="VALUE" value="1.0μH"/>
</technology>
</technologies>
</device>
<device name="-0805_WIDE-1.0μH-1.45A-0.106OHM-1.0MM_H" package="0805-WIDE">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NDUC-14375"/>
<attribute name="VALUE" value="1.0μH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="19NH">
<gates>
<gate name="G$1" symbol="INDUCTOR"/>
</gates>
<devices>
<device name="-0402" package="0402_MURATA">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NDUC-14352"/>
<attribute name="VALUE" value="19 nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="24NH">
<gates>
<gate name="G$1" symbol="INDUCTOR"/>
</gates>
<devices>
<device name="-0603" package="0603_MURATA">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NDUC-14353"/>
<attribute name="VALUE" value="24 nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="11NH">
<gates>
<gate name="G$1" symbol="INDUCTOR"/>
</gates>
<devices>
<device name="-0603" package="0603_MURATA">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NDUC-14354"/>
<attribute name="VALUE" value="11 nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
