<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.0">
<drawing>
<library>
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMA-DIODE">
<description>&lt;B&gt;Diode&lt;/B&gt;
&lt;p&gt;Basic SMA packaged diode. Good for reverse polarization protection. Common part #: MBRA140&lt;/p&gt;
&lt;p&gt;SMA is the smallest package in the DO-214 standard (DO-214AC)&lt;/p&gt;</description>
</package>
<package name="DIODE-1N4001">
</package>
<package name="SOD-323">
<description>SOD-323 (Small Outline Diode)</description>
</package>
<package name="SOT23-3">
<description>SOT23-3</description>
</package>
<package name="DIODE-1N4148">
</package>
<package name="MSOP8">
<description>&lt;b&gt;8M, 8-Lead, 0.118" Wide, Miniature Small Outline Package&lt;/b&gt;&lt;p&gt;
MSOP&lt;br&gt;
8M-Package doc1097.pdf</description>
</package>
<package name="TO-92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
<package name="DPAK">
</package>
<package name="TO220V">
<description>&lt;b&gt;TO 220 Vertical&lt;/b&gt; Package works with various parts including N-Channel MOSFET SparkFun SKU: COM-10213</description>
</package>
<package name="8-SMD">
</package>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
<package name="DIP8SMD">
</package>
<package name="SOD-523">
<description>SOD-523 (Small Outline Diode)</description>
</package>
<package name="SOT323">
</package>
<package name="MICROFET_2X2">
<description>&lt;b&gt;1206-8 ChipFET&lt;/b&gt;&lt;p&gt;
Source: http://www.vishay.com/docs/72593/72593.pdf&lt;br&gt;
http://www.vishay.com/docs/71151/71151.pdf</description>
</package>
<package name="DIODE-1N4148-KIT">
</package>
<package name="DIODE-1N4001-KIT">
</package>
<package name="SOT26">
<description>Footprint for SOT-26 part DMP2240UDM</description>
</package>
<package name="PT17-21C-L41-TR8">
</package>
<package name="TO-263/D2PAK">
</package>
<package name="PANASONIC_SMINI2-F5-B">
<description>From http://www.semicon.panasonic.co.jp/ds4/DZ2J150_E.pdf</description>
</package>
<package name="TO-92-EZ">
</package>
<package name="SO08">
<description>SOIC, 0.15 inch width</description>
</package>
<package name="SC70-6">
<description>&lt;h3&gt;SC-88/SC70-6/SOT-363 6-pin Package&lt;/h3&gt;
&lt;p&gt;&lt;a href="http://www.onsemi.com/pub_link/Collateral/MBT3904DW1T1-D.PDF"&gt;Example Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="DIODE-MICRO-SMP">
</package>
<package name="SO16">
</package>
<package name="LTV-816_4PIN_DIP">
</package>
<package name="SOT363_PHILIPS">
<description>&lt;b&gt;Small Outline Transistor; 6 leads&lt;/b&gt;&lt;p&gt;
Philips Semiconductors, SOT363.pdf</description>
</package>
<package name="SOT-416FL">
</package>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
<symbols>
<symbol name="BAV99">
<description>Switching diode array with series-pair diode configuration</description>
<pin name="A1"/>
<pin name="C2"/>
<pin name="COM"/>
</symbol>
<symbol name="PNP">
<description>&lt;h3&gt; PNP Transistor&lt;/h3&gt;</description>
<pin name="B" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="E" direction="pas"/>
</symbol>
<symbol name="NPN">
<description>&lt;h3&gt; NPN Transistor&lt;/h3&gt;
Allows current flow when high potential at base.</description>
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="DIODE">
<description>Conventional Si diode</description>
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="DIODE-SCHOTTKY">
<description>&lt;h3&gt; Schottky Diode&lt;/h3&gt;
Diode with low voltage drop</description>
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="DIODE-ZENER">
<description>&lt;h3&gt;Zener Diode&lt;/h3&gt;
Allows current flow in one direction, but allows reverse flow when above breakdown voltage.</description>
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="ILD213T">
<pin name="C2"/>
<pin name="A2"/>
<pin name="C1"/>
<pin name="A1"/>
<pin name="ET2"/>
<pin name="CT2"/>
<pin name="ET1"/>
<pin name="CT1"/>
</symbol>
<symbol name="OPTOTRIAC_ZC">
<description>&lt;h3&gt; Opto-TRIAC Zero Crossing&lt;/h3&gt;
TRIAC that is triggered optically.</description>
<pin name="A"/>
<pin name="K"/>
<pin name="T2"/>
<pin name="T1"/>
</symbol>
<symbol name="OPTO_DARLINGTON">
<description>&lt;h3&gt; Darlington Opto-isolator&lt;/h3&gt;</description>
<pin name="C"/>
<pin name="A"/>
<pin name="VCC"/>
<pin name="VOUT"/>
<pin name="GND"/>
</symbol>
<symbol name="DMC2700UDM">
<pin name="G1"/>
<pin name="S1"/>
<pin name="D1"/>
<pin name="G2"/>
<pin name="S2"/>
<pin name="D2"/>
</symbol>
<symbol name="NPN_RESISTOR">
<description>&lt;h3&gt; NPN Transistor with Built-In Base Resistor &lt;/h3&gt;</description>
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="PNP_RESISTOR">
<description>&lt;h3&gt;PNP Transistor with Built-in Base Resistor&lt;/h3&gt;</description>
<pin name="B" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="E" direction="pas"/>
</symbol>
<symbol name="PHOTOTRANSISTOR">
<description>&lt;h3&gt; Phototransistor&lt;/h3&gt;
A light-sensitive transistor.</description>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="TRIAC-TAB">
<description>&lt;h3&gt; TRIAC with Isolated Tab&lt;/h3&gt;</description>
<pin name="G"/>
<pin name="T1"/>
<pin name="T2@1" direction="pas"/>
<pin name="T2@2" direction="pas"/>
</symbol>
<symbol name="OPTOISOLATOR">
<description>&lt;h3&gt;Dual Opto-isolator&lt;/h3&gt;
Dual channel. Isolates connections with use of light.</description>
<pin name="A1"/>
<pin name="A2"/>
<pin name="C1"/>
<pin name="C2"/>
<pin name="CL1"/>
<pin name="CL2"/>
<pin name="EM1"/>
<pin name="EM2"/>
</symbol>
<symbol name="PESD1CAN_DIODE">
<description>&lt;h3&gt;Two channel CAN BUS Diode &lt;/h3&gt;
Provides ESD protection</description>
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
</symbol>
<symbol name="DIODE-ZENER-ADJ">
<description>&lt;h3&gt; Adjustable Zener Diode&lt;/h3&gt;
Allows one-direction current flow, but will allow reverse flow when above the adjustable breakdown voltage.</description>
<pin name="A" direction="pas"/>
<pin name="ADJ"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="LABELED-NMOS">
<description>&lt;h3&gt; N-channel MOSFET transistor&lt;/h3&gt;
Switches electronic signals</description>
<pin name="G"/>
<pin name="S"/>
<pin name="D"/>
</symbol>
<symbol name="LABELED-PMOS">
<description>&lt;h3&gt;P-channel MOSFET&lt;/h3&gt;
Switches electrical signals</description>
<pin name="G"/>
<pin name="S"/>
<pin name="D"/>
</symbol>
<symbol name="TL431">
<description>&lt;h3&gt;TL431&lt;/h3&gt;
Adjustable shunt regulator</description>
<pin name="C"/>
<pin name="R"/>
<pin name="A"/>
</symbol>
<symbol name="OPTOISOLATOR_SINGLE">
<pin name="A1"/>
<pin name="C1"/>
<pin name="CL1"/>
<pin name="EM1"/>
</symbol>
<symbol name="OPTO_DARLINGTON_6N137">
<description>&lt;h3&gt;Lite-On 6N137S - High-Speed OptoIsolator&lt;/h3&gt;
&lt;p&gt;Opto-Isolator capable of 10 MBd.&lt;/p&gt;</description>
<pin name="C"/>
<pin name="A"/>
<pin name="VCC"/>
<pin name="VOUT"/>
<pin name="GND"/>
<pin name="EN"/>
</symbol>
<symbol name="LTV-816_OPTO_ISOLATOR">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
</symbol>
<symbol name="DIODE-TVS">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="BAV99" prefix="D">
<description>&lt;h3&gt;Series-pair diode array&lt;/h3&gt;
&lt;p&gt;Two small signal silicon diodes connected anode to cathode. Connections to all three nodes available.&lt;/p&gt;
&lt;p&gt;Link to &lt;a href='https://www.fairchildsemi.com/datasheets/BA/BAV99.pdf'&gt;datasheet&lt;/a&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13752”&gt;SparkFun AutoDriver&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BAV99"/>
</gates>
<devices>
<device name="" package="SOT23-3">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="C2" pad="2"/>
<connect gate="G$1" pin="COM" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-10647"/>
<attribute name="VALUE" value="200mA/70V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE-SCHOTTKY" prefix="D" uservalue="yes">
<description>&lt;h3&gt;Schottky diode&lt;/h3&gt;
&lt;p&gt;A Schottky diode is a semiconductor diode which has a low forward voltage drop and a very fast switching action.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE-SCHOTTKY"/>
</gates>
<devices>
<device name="-BAT20J" package="SOD-323">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-11623"/>
<attribute name="VALUE" value="1A/23V/620mV"/>
</technology>
</technologies>
</device>
<device name="-RB751S40" package="SOD-523">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-11018"/>
<attribute name="VALUE" value="120mA/40V/370mV"/>
</technology>
</technologies>
</device>
<device name="-SS14" package="SMA-DIODE">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-08053"/>
<attribute name="VALUE" value="1A/40V/500mV"/>
</technology>
</technologies>
</device>
<device name="-PMEG4005EJ" package="SOD-323">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-10955"/>
<attribute name="VALUE" value="0.5A/40V/420mV"/>
</technology>
</technologies>
</device>
<device name="-B340A" package="SMA-DIODE">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-09886"/>
<attribute name="VALUE" value="3A/40V/500mV"/>
</technology>
</technologies>
</device>
<device name="-ZLLS500" package="SOT23-3">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-08411"/>
<attribute name="VALUE" value="700mA/40V/533mV"/>
</technology>
</technologies>
</device>
<device name="-MSS1P6-M3/89A" package="DIODE-MICRO-SMP">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-13919"/>
<attribute name="VALUE" value="1A/60V/520mV"/>
</technology>
</technologies>
</device>
<device name="-BAT60A" package="SOD-323">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-14072"/>
<attribute name="VALUE" value="3A/10V/280mV"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE-ZENER" prefix="D">
<description>&lt;h3&gt;Zener Diode&lt;/h3&gt;
&lt;p&gt;A Zener diode allows current to flow from its anode to its cathode like a normal semiconductor diode, but it also permits current to flow in the reverse direction when its "Zener voltage" is reached. - WIkipedia&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE-ZENER"/>
</gates>
<devices>
<device name="-MM3Z3V3T1G" package="SOD-323">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-11284"/>
<attribute name="VALUE" value="3.3V"/>
</technology>
</technologies>
</device>
<device name="-MMSZ5232BS" package="SOD-323">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-12442"/>
<attribute name="VALUE" value="5.6V"/>
</technology>
</technologies>
</device>
<device name="-DZ2J150M0L" package="PANASONIC_SMINI2-F5-B">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-12989"/>
<attribute name="VALUE" value="15V"/>
</technology>
</technologies>
</device>
<device name="-BZT52C3V6S" package="SOD-323">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-08199"/>
<attribute name="VALUE" value="3.6V"/>
</technology>
</technologies>
</device>
<device name="-MMBZ5233BLT1G" package="SOT23-3">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-14123"/>
<attribute name="VALUE" value="6V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ILD213T" prefix="U">
<description>&lt;h3&gt;Dual Channel Phototransistor Optocoupler&lt;/h3&gt;
&lt;p&gt;Dual Channel 70 V 4000 Vrms Phototransistor Optocoupler in a standard SOIC-8 package. Used to couple signals between electrically isolated circuits.&lt;/p&gt;
&lt;br&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Components/SMD/ild205t.pdf”&gt;Datasheet&lt;/a&gt;&lt;/li&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/9118”&gt;SparkFun Opto-Isolator Breakout&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="ILD213T"/>
</gates>
<devices>
<device name="-IDL213T" package="SO08">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="C1" pad="2"/>
<connect gate="G$1" pin="C2" pad="4"/>
<connect gate="G$1" pin="CT1" pad="6"/>
<connect gate="G$1" pin="CT2" pad="8"/>
<connect gate="G$1" pin="ET1" pad="5"/>
<connect gate="G$1" pin="ET2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09076"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRIAC_OPTOCOUPLER" prefix="U">
<description>&lt;h3&gt;Zero-cross Triac Driver Optocoupler&lt;/h3&gt;
&lt;p&gt;SImplifies logic control of 115/240 VAC power. Zero voltage crossing to minimize conducted and radiated line noise.&lt;/p&gt;
&lt;p&gt;Link to &lt;a href='http://www.mouser.com/ds/2/149/MOC3063M-196324.pdf'&gt;datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Emitter:&lt;/b&gt;&amp;nbsp;V&lt;sub&gt;F&lt;/sub&gt;: 1.3V&amp;nbsp;I&lt;sub&gt;FT&lt;/sub&gt;: 5 mA&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Detector:&lt;/b&gt;&amp;nbsp;V&lt;sub&gt;DRM&lt;/sub&gt;: 600V&amp;nbsp;I&lt;sub&gt;TSM&lt;/sub&gt;: 1A&amp;nbsp;V&lt;sub&gt;ISO&lt;/sub&gt;: 4170V&amp;nbsp;&lt;sup&gt;DV&lt;/sup&gt;&amp;frasl;&lt;sub&gt;dt&lt;/sub&gt;: 1500&lt;sup&gt;V&lt;/sup&gt;&amp;frasl;&lt;sub&gt;µs&lt;/sub&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12781”&gt;SparkFun EL Sequencer&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/10878”&gt;SparkFun EL Escudo Dos&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="OPTOTRIAC_ZC"/>
</gates>
<devices>
<device name="-MOC3063SM" package="DIP8SMD">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="2"/>
<connect gate="G$1" pin="T1" pad="6"/>
<connect gate="G$1" pin="T2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-10683"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOSFET_PCH" prefix="Q">
<description>&lt;h3&gt;P-channel MOSFETs&lt;/h3&gt;
&lt;p&gt;Voltage controlled devices that allow control of high current outputs.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13907”&gt;SparkFun ESP32 Thing&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13231”&gt;SparkFun ESP8266 Thing&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/15316”&gt;SparkFun Pi Servo HAT V2&lt;/a&gt; DMG2305UX-7 (20V/4.2A/SOT23-3)&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LABELED-PMOS"/>
</gates>
<devices>
<device name="-IRLML2244" package="SOT23-3">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-11153"/>
<attribute name="VALUE" value="4.3A/20V/54mΩ"/>
</technology>
</technologies>
</device>
<device name="-SI2309DS" package="SOT23-3">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-08285"/>
<attribute name="VALUE" value="1.1A/60V/600mΩ"/>
</technology>
</technologies>
</device>
<device name="-DMG2307L" package="SOT23-3">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-11308"/>
<attribute name="VALUE" value="3.1A/30V/105mΩ"/>
</technology>
</technologies>
</device>
<device name="-NDP6020P" package="TO220V">
<connects>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-13060"/>
<attribute name="VALUE" value="24A/20V/50mΩ"/>
</technology>
</technologies>
</device>
<device name="-NDS8434" package="SO08">
<connects>
<connect gate="G$1" pin="D" pad="5 6 7 8"/>
<connect gate="G$1" pin="G" pad="4"/>
<connect gate="G$1" pin="S" pad="1 2 3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-08355"/>
<attribute name="VALUE" value="6.5A/20V/35mΩ"/>
</technology>
</technologies>
</device>
<device name="-DMG2305UX-7" package="SOT23-3">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRAN-14388"/>
<attribute name="VALUE" value="20V/4.2A/52mΩ/1.4W"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPTO_DARL_6N138S" prefix="U">
<description>&lt;h3&gt;Optoisolator, darlington pair output&lt;/h3&gt;
&lt;p&gt;Optocoupler consisting of an AlGaAs LED optically coupled to a high gain split darlington photodetector.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12898”&gt;SparkFun MIDI Shield&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="OPTO_DARLINGTON"/>
</gates>
<devices>
<device name="" package="8-SMD">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09482"/>
<attribute name="VALUE" value="6N138M"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRANS_NPN" prefix="Q">
<description>&lt;h3&gt;NPN transistor&lt;/h3&gt;
&lt;p&gt;Current controlled devices typically used to amplify current or used as a switch.&lt;/p&gt;
&lt;ul&gt;
  &lt;li&gt;
    BC547 - 
    &lt;a href="http://www.sparkfun.com/products/8928"&gt;COM-08928&lt;/a&gt;
    (TO-92 45V 100mA) (1.Collector 2.Base 3.Emitter)
  &lt;/li&gt;
  &lt;li&gt;
    2N3904 - 
    &lt;a href="http://www.sparkfun.com/products/521"&gt;COM-00521&lt;/a&gt;
    (TO-92 40V 200mA) (1.Emitter 2.Base 3.Collector)
  &lt;/li&gt;
  &lt;li&gt;
    P2N2222A - 
    &lt;a href="http://www.sparkfun.com/products/12852"&gt;COM-12852&lt;/a&gt;
    (TO-92 40V 600mA) (1.Collector 2.Base 3.Emitter)
  &lt;/li&gt;

&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="NPN"/>
</gates>
<devices>
<device name="-MMBT2222AL" package="SOT23-3">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-08049"/>
<attribute name="VALUE" value="600mA/40V"/>
</technology>
</technologies>
</device>
<device name="-2N3904" package="TO-92">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-08447"/>
<attribute name="VALUE" value="200mA/40V"/>
</technology>
</technologies>
</device>
<device name="-P2N2222A" package="TO-92">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
<connect gate="G$1" pin="E" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-09536"/>
<attribute name="VALUE" value="600mA/40V"/>
</technology>
</technologies>
</device>
<device name="-MMBTA42" package="SOT23-3">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-09116"/>
<attribute name="VALUE" value="500mA/300V"/>
</technology>
</technologies>
</device>
<device name="-2N3904-EZ" package="TO-92-EZ">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-08447"/>
<attribute name="VALUE" value="200mA/40V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRANS_PNP" prefix="Q">
<description>&lt;h3&gt;PNP transistor&lt;/h3&gt;
&lt;p&gt;Current controlled devices typically used to amplify current or used as a switch.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/9068”&gt;SparkFun Serial Enabled 16x2 LCD - Red on Black&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12772”&gt;SparkFun Logomatic&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="PNP"/>
</gates>
<devices>
<device name="-PMBT3906|MMBT3906L" package="SOT23-3">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-08052"/>
<attribute name="VALUE" value="200mA/40V"/>
</technology>
</technologies>
</device>
<device name="-MMBT4403" package="SOT23-3">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-09245"/>
<attribute name="VALUE" value="600mA/40V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE" prefix="D">
<description>&lt;h3&gt;Diode&lt;/h3&gt;
&lt;p&gt;These are standard reverse protection diodes and small signal diodes.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/11177”&gt;SparkFun SparkPunk Sound Kit&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13231”&gt;SparkFun ESP8266 Thing&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="-PTH" package="DIODE-1N4001">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-09176"/>
<attribute name="VALUE" value="1A/50V/1.1V"/>
</technology>
</technologies>
</device>
<device name="-BAS16J" package="SOD-323">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-09646"/>
<attribute name="VALUE" value="250mA/100V"/>
</technology>
</technologies>
</device>
<device name="-1N4148" package="DIODE-1N4148">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-08378"/>
<attribute name="VALUE" value="200mA/100V/1V"/>
</technology>
</technologies>
</device>
<device name="-KIT" package="DIODE-1N4148-KIT">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-08378"/>
<attribute name="VALUE" value="200mA/100V/1V"/>
</technology>
</technologies>
</device>
<device name="-KIT2" package="DIODE-1N4001-KIT">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-09176"/>
<attribute name="VALUE" value="1A/50V/1.1V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOSFET-NCH" prefix="Q">
<description>&lt;h3&gt;N-channel MOSFETs&lt;/h3&gt;
&lt;p&gt;Voltage controlled devices that allow control of high current outputs.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13261”&gt;SparkFun OpenScale&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12651”&gt;SparkFun Digital Sandbox&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/10182”&gt;SparkFun Monster Moto Shield&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/11214”&gt;SparkFun MOSFET Power Controller&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="NMOS" symbol="LABELED-NMOS"/>
</gates>
<devices>
<device name="-FDD8780" package="DPAK">
<connects>
<connect gate="NMOS" pin="D" pad="4"/>
<connect gate="NMOS" pin="G" pad="1"/>
<connect gate="NMOS" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-09984"/>
<attribute name="VALUE" value="35A/25V/8.5mΩ"/>
</technology>
</technologies>
</device>
<device name="-2N7002PW" package="SOT323">
<connects>
<connect gate="NMOS" pin="D" pad="3"/>
<connect gate="NMOS" pin="G" pad="1"/>
<connect gate="NMOS" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-11151"/>
<attribute name="VALUE" value="310mA/60V/1.6Ω"/>
</technology>
</technologies>
</device>
<device name="-FQP30N06L" package="TO220V">
<connects>
<connect gate="NMOS" pin="D" pad="2"/>
<connect gate="NMOS" pin="G" pad="1"/>
<connect gate="NMOS" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-10060"/>
<attribute name="VALUE" value="60V/32A/35mΩ"/>
</technology>
</technologies>
</device>
<device name="-BSS138" package="SOT23-3">
<connects>
<connect gate="NMOS" pin="D" pad="3"/>
<connect gate="NMOS" pin="G" pad="1"/>
<connect gate="NMOS" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-00830"/>
<attribute name="VALUE" value="220mA/50V/3.5Ω"/>
</technology>
</technologies>
</device>
<device name="-PSMN7R0" package="TO-263/D2PAK">
<connects>
<connect gate="NMOS" pin="D" pad="2"/>
<connect gate="NMOS" pin="G" pad="1"/>
<connect gate="NMOS" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-12437"/>
<attribute name="VALUE" value="100A/100V/6.8mΩ"/>
</technology>
</technologies>
</device>
<device name="-AO3404A" package="SOT23-3">
<connects>
<connect gate="NMOS" pin="D" pad="3"/>
<connect gate="NMOS" pin="G" pad="1"/>
<connect gate="NMOS" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-12988"/>
<attribute name="VALUE" value="5.8A/30V/35mΩ"/>
</technology>
</technologies>
</device>
<device name="-FDS6630A" package="SO08">
<connects>
<connect gate="NMOS" pin="D" pad="5 6 7 8"/>
<connect gate="NMOS" pin="G" pad="4"/>
<connect gate="NMOS" pin="S" pad="1 2 3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-08089"/>
<attribute name="VALUE" value="6.5A/30V/38mΩ"/>
</technology>
</technologies>
</device>
<device name="-RE1C00UNTL" package="SOT-416FL">
<connects>
<connect gate="NMOS" pin="D" pad="3"/>
<connect gate="NMOS" pin="G" pad="1"/>
<connect gate="NMOS" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-14399"/>
<attribute name="VALUE" value="20V/0.2A/8MHz/1.2Ω/1Vth"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRF7509" prefix="Q">
<description>&lt;h3&gt;Dual N and P Channel MOSFET&lt;/h3&gt;
&lt;p&gt;Dual N/P-Channel 30V 1.25 W 7.8/7.5 nC Hexfet Power Mosfet Surface Mount-MICRO-8.&lt;/p&gt;
&lt;p&gt;NMOS R&lt;sub&gt;DS(ON)&lt;/sub&gt; 0.11Ω. PMOS R&lt;sub&gt;DS(ON)&lt;/sub&gt; 0.20Ω.&lt;/p&gt;
&lt;p&gt;&lt;a href='http://www.irf.com/product-info/datasheets/data/irf7509pbf.pdf'&gt;Link to datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12097”&gt;SparkFun RedBot Mainboard&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/11447”&gt;SparkFun Wake on Shake&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="NMOS" symbol="LABELED-NMOS"/>
<gate name="PMOS" symbol="LABELED-PMOS"/>
</gates>
<devices>
<device name="" package="MSOP8">
<connects>
<connect gate="NMOS" pin="D" pad="7 8"/>
<connect gate="NMOS" pin="G" pad="2"/>
<connect gate="NMOS" pin="S" pad="1"/>
<connect gate="PMOS" pin="D" pad="5 6"/>
<connect gate="PMOS" pin="G" pad="4"/>
<connect gate="PMOS" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-07913"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOSFET_NCH_DUAL" prefix="Q">
<description>&lt;h3&gt;Dual N-Channel 30-V&lt;sub&gt;DS&lt;/sub&gt; MOSFET&lt;/h3&gt;
&lt;p&gt;&lt;a href='https://www.fairchildsemi.com/datasheets/FD/FDMA1024NZ.pdf'&gt;Link to datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/9627”&gt;SparkFun Mini FET Shield&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="A" symbol="LABELED-NMOS"/>
<gate name="B" symbol="LABELED-NMOS"/>
</gates>
<devices>
<device name="-FDMA1024NZ" package="MICROFET_2X2">
<connects>
<connect gate="A" pin="D" pad="D1 D1_2"/>
<connect gate="A" pin="G" pad="G1"/>
<connect gate="A" pin="S" pad="S1"/>
<connect gate="B" pin="D" pad="D2 D2_2"/>
<connect gate="B" pin="G" pad="G2"/>
<connect gate="B" pin="S" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-09516"/>
<attribute name="VALUE" value="5A/20V/54mΩ"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOSFET_COMPLIMENTARY_PAIR" prefix="Q">
<description>&lt;h3&gt;Complementary pair enhancement mode MOSFET&lt;/h3&gt;
&lt;p&gt;A P and N channel MOSFET in a single package. Rated to breakdown at 20V&lt;/p&gt;
&lt;p&gt;&lt;a href='http://www.diodes.com/_files/datasheets/DMC2700UDM.pdf'&gt;Link to datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12780”&gt;ZX Distance and Gesture Sensor&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DMC2700UDM"/>
</gates>
<devices>
<device name="-DMC2700UDM" package="SOT26">
<connects>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="G1" pad="G1"/>
<connect gate="G$1" pin="G2" pad="G2"/>
<connect gate="G$1" pin="S1" pad="S1"/>
<connect gate="G$1" pin="S2" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-11993"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRANS_NPN_RES" prefix="Q">
<description>&lt;h3&gt;NPN transistor with built in base resistor&lt;/h3&gt;
&lt;p&gt;Current controlled device with built in current control for tighter layouts.&lt;/p&gt;
&lt;p&gt;Link to &lt;a href='http://www.diodes.com/_files/datasheets/ds30399.pdf'&gt;datasheet&lt;/a&gt;.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/11644”&gt;SparkFun OpenSegment Serial Display - White&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/11644”&gt;SparkFun OpenSegment Serial Display - Red&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="NPN_RESISTOR"/>
</gates>
<devices>
<device name="-DDTD142TC-7-F" package="SOT23-3">
<connects>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-11480"/>
<attribute name="VALUE" value="500mA/50V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRANS_PNP_RES" prefix="Q">
<description>&lt;h3&gt;PNP transistor with built in base resistor&lt;/h3&gt;
&lt;p&gt;Current controlled device with built in current control for tighter layouts.&lt;/p&gt;
&lt;p&gt;Link to &lt;a href='http://www.diodes.com/_files/datasheets/ds30403.pdf'&gt;datasheet&lt;/a&gt;.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/11644”&gt;SparkFun OpenSegment Serial Display - White&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/11644”&gt;SparkFun OpenSegment Serial Display - Red&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="Q1" symbol="PNP_RESISTOR"/>
</gates>
<devices>
<device name="-DDTB142TC" package="SOT23-3">
<connects>
<connect gate="Q1" pin="B" pad="1"/>
<connect gate="Q1" pin="C" pad="3"/>
<connect gate="Q1" pin="E" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-11479"/>
<attribute name="VALUE" value="500mA"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PHOTOTRANSISTOR" prefix="Q">
<description>&lt;h3&gt;Phototransistor&lt;/h3&gt;
&lt;p&gt;PT17-21C/L41/TR8 is a phototransistor in miniature SMD package which is molded in a water clear with flat top view lens. 
&lt;br&gt;The device is Spectrally matched to visible and infrared emitting diode.
&lt;br&gt;&lt;a href=”http://www.everlight.com/file/ProductFile/PT17-21C-L41-TR8.pdf”&gt;Datasheet&lt;/a&gt;&lt;/li&gt;
&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12958”&gt;SparkFun Electric Imp imp002 Breakout&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="PHOTOTRANSISTOR"/>
</gates>
<devices>
<device name="PT17-21C-L41-TR8" package="PT17-21C-L41-TR8">
<connects>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-12141"/>
<attribute name="VALUE" value="20mA/30V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOSFET_PCH_DUAL" prefix="Q">
<description>&lt;h3&gt;Dual P-Channel -20V&lt;sub&gt;DS&lt;/sub&gt; MOSFET&lt;/h3&gt;
&lt;p&gt;&lt;a href='http://www.diodes.com/_files/datasheets/ds31197.pdf'&gt;Link to datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13229”&gt;SparkFun FreeSoC2 Development Board&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G1" symbol="LABELED-PMOS"/>
<gate name="G$1" symbol="LABELED-PMOS"/>
</gates>
<devices>
<device name="-DMP2240UDM" package="SOT26">
<connects>
<connect gate="G$1" pin="D" pad="D2"/>
<connect gate="G$1" pin="G" pad="G2"/>
<connect gate="G$1" pin="S" pad="S2"/>
<connect gate="G1" pin="D" pad="D1"/>
<connect gate="G1" pin="G" pad="G1"/>
<connect gate="G1" pin="S" pad="S1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-12444"/>
<attribute name="VALUE" value="2A/20V/150mΩ"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRIAC" prefix="Q">
<description>&lt;h3&gt;Bidirectional triode thyristor (TRIAC)&lt;/h3&gt;
&lt;p&gt;Four quadrant TRIAC. Useful for EL Wire Applications
&lt;br&gt;&lt;p&gt;Link to &lt;a href='https://cdn.sparkfun.com/datasheets/Components/EL/EL_Escudo_Dos/Z0103MN.pdf'&gt;datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12781”&gt;SparkFun EL Sequencer&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/10878”&gt;SparkFun EL Escudo Dos&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TRIAC-TAB"/>
</gates>
<devices>
<device name="-Z0103MN" package="SOT223">
<connects>
<connect gate="G$1" pin="G" pad="3"/>
<connect gate="G$1" pin="T1" pad="1"/>
<connect gate="G$1" pin="T2@1" pad="2"/>
<connect gate="G$1" pin="T2@2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-09120"/>
<attribute name="VALUE" value="1A/600V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DUAL-OPTOISOLATOR" prefix="U">
<description>&lt;h3&gt;Optocoupler, Phototransistor Output, Dual Channel&lt;/h3&gt;
&lt;p&gt;Optically coupled pairs with a gallium arsenide infrared LED and a silicon NPN phototransistor.
&lt;br&gt; Signal information, including a DC level, can be transmitted by the device while maintaining a high degree of electrical isolation between input and output.
&lt;br&gt;&lt;li&gt;&lt;a href='https://www.sparkfun.com/datasheets/Components/SMD/ild205t.pdf'&gt;Datasheet&lt;/a&gt;&lt;/li&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href='https://www.sparkfun.com/products/9118'&gt;SparkFun Opto-isolator Breakout&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="OPTOISOLATOR"/>
</gates>
<devices>
<device name="_SOIC8" package="SO08">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="C1" pad="2"/>
<connect gate="G$1" pin="C2" pad="4"/>
<connect gate="G$1" pin="CL1" pad="8"/>
<connect gate="G$1" pin="CL2" pad="6"/>
<connect gate="G$1" pin="EM1" pad="7"/>
<connect gate="G$1" pin="EM2" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09076"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PESD1CAN" prefix="D">
<description>&lt;h3&gt;CAN bus ESD protection diode&lt;/h3&gt;
&lt;p&gt;PESD1CAN is used to protect two CAN bus lines from ESD.&lt;/p&gt;
&lt;p&gt;Link to &lt;a href='http://www.nxp.com/documents/data_sheet/PESD1CAN-U.pdf'&gt;datasheet&lt;/a&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13262”&gt;SparkFun CAN-BUS Shield&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="PESD1CAN_DIODE"/>
</gates>
<devices>
<device name="" package="SOT23-3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-12501"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4051" prefix="U">
<description>&lt;h3&gt;Adjustable Shunt Voltage Reference&lt;/h3&gt;
&lt;p&gt;SOT-23 package without need for external capacitor. Adjustable from 1.24V to 10V. 60µA to 12mA&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/11177”&gt;SparkFun SparkPunk Sound Kit&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13231”&gt;SparkFun ESP8266 Thing&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE-ZENER-ADJ"/>
</gates>
<devices>
<device name="" package="SOT23-3">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="ADJ" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-13134"/>
<attribute name="VALUE" value="LM4051"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL431" prefix="U">
<description>&lt;h3&gt;TL431- Voltage Reference&lt;/h3&gt;
&lt;p&gt;Precision Programmable Shunt Regulator Diode
&lt;br&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Components/General%20IC/TL431-D.pdf"&gt;Datasheet&lt;/a&gt;
&lt;br&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/11078”&gt;TL431-Voltage Reference PTH&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/11087”&gt;SparkFun Uh-Oh Battery Level Indicator&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TL431"/>
</gates>
<devices>
<device name="PTH" package="TO-92">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="R" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-10947"/>
<attribute name="SF_ID" value="COM-11078"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRANS_NPN_DUAL" prefix="Q" uservalue="yes">
<description>&lt;h3&gt; Dual NPN Transistors in Single Package&lt;/h3&gt;
&lt;p&gt;The MBT3904W1 puts two general purpose 3904 NPN transistors in a single package.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.onsemi.com/pub_link/Collateral/MBT3904DW1T1-D.PDF"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13907”&gt;SparkFun ESP32 Thing&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="Q1" symbol="NPN"/>
<gate name="Q2" symbol="NPN"/>
</gates>
<devices>
<device name="-MBT3904DW1T1" package="SC70-6">
<connects>
<connect gate="Q1" pin="B" pad="5"/>
<connect gate="Q1" pin="C" pad="3"/>
<connect gate="Q1" pin="E" pad="4"/>
<connect gate="Q2" pin="B" pad="2"/>
<connect gate="Q2" pin="C" pad="6"/>
<connect gate="Q2" pin="E" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRANS-13337"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="QUAD-OPTOISOLATOR" prefix="U">
<gates>
<gate name="G1" symbol="OPTOISOLATOR_SINGLE"/>
<gate name="G2" symbol="OPTOISOLATOR_SINGLE"/>
<gate name="G3" symbol="OPTOISOLATOR_SINGLE"/>
<gate name="G4" symbol="OPTOISOLATOR_SINGLE"/>
</gates>
<devices>
<device name="" package="SO16">
<connects>
<connect gate="G1" pin="A1" pad="1"/>
<connect gate="G1" pin="C1" pad="2"/>
<connect gate="G1" pin="CL1" pad="16"/>
<connect gate="G1" pin="EM1" pad="15"/>
<connect gate="G2" pin="A1" pad="3"/>
<connect gate="G2" pin="C1" pad="4"/>
<connect gate="G2" pin="CL1" pad="14"/>
<connect gate="G2" pin="EM1" pad="13"/>
<connect gate="G3" pin="A1" pad="5"/>
<connect gate="G3" pin="C1" pad="6"/>
<connect gate="G3" pin="CL1" pad="12"/>
<connect gate="G3" pin="EM1" pad="11"/>
<connect gate="G4" pin="A1" pad="7"/>
<connect gate="G4" pin="C1" pad="8"/>
<connect gate="G4" pin="CL1" pad="10"/>
<connect gate="G4" pin="EM1" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-14121"/>
<attribute name="VALUE" value="TLP290-4"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6N137S" prefix="U">
<description>&lt;h3&gt;Lite-On 6N137 - High Speed Opto Isolator&lt;/h3&gt;
&lt;p&gt;Opto isolator capable of data rates up to 10MBd&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="OPTO_DARLINGTON_6N137"/>
</gates>
<devices>
<device name="" package="8-SMD">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="EN" pad="7"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-14151"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTV-816_OPTO_ISOLATOR" prefix="U">
<gates>
<gate name="U1" symbol="LTV-816_OPTO_ISOLATOR"/>
</gates>
<devices>
<device name="&quot;" package="LTV-816_4PIN_DIP">
<connects>
<connect gate="U1" pin="1" pad="1"/>
<connect gate="U1" pin="2" pad="2"/>
<connect gate="U1" pin="3" pad="3"/>
<connect gate="U1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-14145"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRANS_PNP_DUAL" prefix="Q" uservalue="yes">
<description>&lt;h3&gt; Dual PNP Transistors in Single Package&lt;/h3&gt;
&lt;p&gt;The BCM857BS puts two PNP transistors in a single package.&lt;/p&gt;
&lt;p&gt;Bipolar (BJT) Transistor Array 2 PNP (Dual) 45V 100mA 100MHz 200mW Surface Mount SOT-363&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.diodes.com/assets/Datasheets/BCM857BS.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com”&gt;SparkFun Pi Servo HAT V2&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="PNP"/>
<gate name="G$2" symbol="PNP"/>
</gates>
<devices>
<device name="SOT-363" package="SOT363_PHILIPS">
<connects>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="6"/>
<connect gate="G$1" pin="E" pad="1"/>
<connect gate="G$2" pin="B" pad="5"/>
<connect gate="G$2" pin="C" pad="3"/>
<connect gate="G$2" pin="E" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="TRAN-14386"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE_TVS" prefix="D">
<gates>
<gate name="G$1" symbol="DIODE-TVS"/>
</gates>
<devices>
<device name="" package="0603">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-14502"/>
<attribute name="VALUE" value="24V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
