<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<library>
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED_5MM">
<description>&lt;B&gt;LED 5mm PTH&lt;/B&gt;&lt;p&gt;
5 mm, round
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1inch&lt;/li&gt;
&lt;li&gt;Diameter: 5mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED-IR-THRU&lt;/li&gt;</description>
</package>
<package name="LED_3MM">
<description>&lt;h3&gt;LED 3MM PTH&lt;/h3&gt;

3 mm, round.

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1inch&lt;/li&gt;
&lt;li&gt;Diameter: 3mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="LED-1206">
<description>&lt;h3&gt;LED 1206 SMT&lt;/h3&gt;

1206, surface mount. 

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: &lt;/li&gt;
&lt;li&gt;Area: 0.125" x 0.06"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="LED-0603">
<description>&lt;B&gt;LED 0603 SMT&lt;/B&gt;&lt;p&gt;
0603, surface mount.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.075inch &lt;/li&gt;
&lt;li&gt;Area: 0.06" x 0.03"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED - BLUE&lt;/li&gt;</description>
</package>
<package name="LED_10MM">
<description>&lt;B&gt;LED 10mm PTH&lt;/B&gt;&lt;p&gt;
10 mm, round
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.2inch&lt;/li&gt;
&lt;li&gt;Diameter: 10mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;</description>
</package>
<package name="FKIT-LED-1206">
<description>&lt;B&gt;LED 1206 SMT&lt;/B&gt;&lt;p&gt;
1206, surface mount
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Area: 0.125"x 0.06" &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;</description>
</package>
<package name="LED_3MM-NS">
<description>&lt;h3&gt;LED 3MM PTH- No Silk&lt;/h3&gt;

3 mm, round, no silk outline of package

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1inch&lt;/li&gt;
&lt;li&gt;Diameter: 3mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="LED_5MM-KIT">
<description>&lt;h3&gt;LED 5mm KIT PTH&lt;/h3&gt;
&lt;p&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.&lt;/p&gt;

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1inch&lt;/li&gt;
&lt;li&gt;Diameter: 5mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example Device:
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="LED-TRICOLOR-SMD">
<description>&lt;h3&gt;Tri-Color SMD&lt;/h3&gt;
&lt;p&gt;&lt;b&gt;Specifications:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;Pin count: 4&lt;/li&gt;
&lt;li&gt;Pin pitch: 2.0mm&lt;/li&gt;
&lt;li&gt;Area: 2.6mm x 3.2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/DJS-BRGBC-TR8.pdf"&gt; DJS-BRGBC-TR8&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Example device(s):&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;/li&gt;
&lt;/ul&gt;TRI-COLOR LED&lt;/p&gt;</description>
</package>
<package name="LED_BARGRAPH_10">
<description>&lt;h3&gt;10 Segment LED Bar Graph&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 20&lt;/li&gt;
&lt;li&gt;Pin pitch: 1.74mm&lt;/li&gt;
&lt;li&gt;Area:10mm x 25.5mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt; &lt;a href="https://www.sparkfun.com/datasheets/Components/LED/YSLB-102510B5-10.pdf"&gt;YSLB-102510B5&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="LED_PIRANHA_5MM">
<description>&lt;h3&gt;LED 5mm PTH - Piranha&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 4&lt;/li&gt;
&lt;li&gt;Pin pitch: 1.5mm, 5.06 mm&lt;/li&gt;
&lt;li&gt;Area:5mm x 5mm &lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt; &lt;a href="http://cdn.sparkfun.com/datasheets/Components/LED/YSRGB7A5BSW25.pdf"&gt;YSRGB7A5BSW25&lt;/a&gt;&lt;/p&gt;

&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED Pirahana&lt;/li&gt;</description>
</package>
<package name="LED_RING">
<description>&lt;h3&gt;16 LED Ring - LED-CCL-A&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 20&lt;/li&gt;
&lt;li&gt;Area: 26 x 40mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt; &lt;a href="http://cdn.sparkfun.com/datasheets/Components/LED/LED-CCL-A.pdf"&gt;LED-CCL-A&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED Ring&lt;/li&gt;</description>
</package>
<package name="LTE-302">
<description>&lt;h3&gt;IR Emitter/Detector&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 2.54mm&lt;/li&gt;
&lt;li&gt;Area: 2.25 x 4.4 mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint&lt;/b&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/LTE-302.pdf"&gt; LTE-302&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LTE-302&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="LED-RGB-THRU">
<description>&lt;h3&gt;LED - RGB PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 4&lt;/li&gt;
&lt;li&gt;Area:5 x 5.8 mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Datasheet Referenced: &lt;a href="https://www.sparkfun.com/datasheets/Components/YSL-R596CR3G4B5C-C10.pdf"&gt;YSL-R596CR3G4B5C&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED-RGB-CA&lt;/li&gt;
&lt;li&gt;LED-RGB-CC&lt;/li&gt;</description>
</package>
<package name="LED-TRICOLOR-5050">
<description>&lt;h3&gt;5050 SMD RGB LED&lt;/h3&gt;
&lt;p&gt;&lt;b&gt;Specifications:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;Pin count: 6&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.6mm&lt;/li&gt;
&lt;li&gt;Area: 5.0mm x 5.mm&lt;/li&gt;
&lt;li&gt;Thickness: 2.6mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/LED/5060BRG4.pdf"&gt; 5060BRG4&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Example device(s):&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;LED-RGB&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="LED-TRICOLOR-5050-IC">
<description>&lt;h3&gt;5060 SMD RGB LED&lt;/h3&gt;
&lt;p&gt;&lt;b&gt;Specifications:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;Pin count: 6&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.6mm&lt;/li&gt;
&lt;li&gt;Area: 5.0mm x 5.0mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/LED/WS2812.pdf"&gt; WS2812&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Example device(s):&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;WS2812&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="LED-1206-BOTTOM">
<description>&lt;h3&gt;LED 1206 SMT&lt;/h3&gt;

1206, surface mount. 

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Area: 0.125" x 0.06"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="SFH4641">
<description>&lt;h3&gt;SFH4641&lt;/h3&gt;

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Size: 3.3 x 2.35 mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt; &lt;a href="http://www.mouser.com/ds/2/311/SFH%204641,%20Lead%20(Pb)%20Free%20Product%20-%20RoHS%20Compliant-318787.pdf"&gt;SFH 4641&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device:
&lt;ul&gt;&lt;li&gt;SFH4641&lt;/li&gt;</description>
</package>
<package name="SFH4641-NARROW">
<description>&lt;h3&gt;SFH4641&lt;/h3&gt;

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Size: 3.3 x 2.35 mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt; &lt;a href="http://www.mouser.com/ds/2/311/SFH%204641,%20Lead%20(Pb)%20Free%20Product%20-%20RoHS%20Compliant-318787.pdf"&gt;SFH 4641&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device:
&lt;ul&gt;&lt;li&gt;SFH4641&lt;/li&gt;</description>
</package>
<package name="SFH4641-SHORT">
<description>&lt;h3&gt;SFH4641&lt;/h3&gt;

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Size: 3.3 x 2.35 mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt; &lt;a href="http://www.mouser.com/ds/2/311/SFH%204641,%20Lead%20(Pb)%20Free%20Product%20-%20RoHS%20Compliant-318787.pdf"&gt;SFH 4641&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device:
&lt;ul&gt;&lt;li&gt;SFH4641&lt;/li&gt;</description>
</package>
<package name="SFH4641-OVERSIZE">
<description>&lt;h3&gt;SFH4641&lt;/h3&gt;

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Size: 3.3 x 2.35 mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt; &lt;a href="http://www.mouser.com/ds/2/311/SFH%204641,%20Lead%20(Pb)%20Free%20Product%20-%20RoHS%20Compliant-318787.pdf"&gt;SFH 4641&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device:
&lt;ul&gt;&lt;li&gt;SFH4641&lt;/li&gt;</description>
</package>
<package name="WS2812B">
<description>&lt;h3&gt;WS2812B&lt;/h3&gt;

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 4&lt;/li&gt;
&lt;li&gt;Size: 5.0 x 5.0 mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt; &lt;a href="http://cdn.sparkfun.com/datasheets/BreakoutBoards/WS2812B.pdf"&gt;WS2812B&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device:
&lt;ul&gt;&lt;li&gt;WS2812B&lt;/li&gt;</description>
</package>
<package name="PLCC-6-LED">
<description>&lt;h3&gt;PLCC-6-LED&lt;/h3&gt;

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 6&lt;/li&gt;
&lt;li&gt;Size: 3.2*2.8*1.39mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt; &lt;a href="http://www.osram-os.com/Graphics/XPic9/00134830_0.pdf"&gt;LTRB GFSF&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device:
&lt;ul&gt;&lt;li&gt;RGB-LED-PLCC&lt;/li&gt;</description>
</package>
<package name="LTST-C195KGJRKT">
<description>&lt;h3&gt;0606 - LED SMT&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.8mm&lt;/li&gt;
&lt;li&gt;Area:1.6mm L x 1.5mm W&lt;/li&gt;
&lt;li&gt;Height: 0.55m&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt; &lt;a href="http://optoelectronics.liteon.com/upload/download/DS22-2000-282/P_100_LTST-C195KGJRKT.pdf"&gt;LTST-C195KGJRKT&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LTST-C195KGJRKT&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SFH4641-SHORT2">
<description>&lt;h3&gt;SFH4641&lt;/h3&gt;

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Size: 3.3 x 2.35 mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt; &lt;a href="http://www.mouser.com/ds/2/311/SFH%204641,%20Lead%20(Pb)%20Free%20Product%20-%20RoHS%20Compliant-318787.pdf"&gt;SFH 4641&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device:
&lt;ul&gt;&lt;li&gt;SFH4641&lt;/li&gt;</description>
</package>
<package name="P-LCC-4-3">
<description>&lt;h3&gt;LED P-LCC-4-3 - SMT&lt;/h3&gt;

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 4&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.7mm &lt;/li&gt;
&lt;li&gt;Size: 3.2*2.8*1.9mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt; &lt;a href="http://www.fairchip.com/pdf/Everlight/67-23-R6GHBHC-B01-2T.pdf"&gt;R6GHBHC&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device:
&lt;ul&gt;&lt;li&gt;0.13_RGB_LED&lt;/li&gt;</description>
</package>
<package name="7-SEGMENT-4DIGIT-YOUNGSUN">
<description>This is a package for the 4-digit 7-segment RED LED from Young Sun.</description>
</package>
<package name="7-SEGMENT-1&quot;PTH">
<description>7 Segment display Storefront SKU#: COM-08546</description>
</package>
<package name="7-SEGMENT-4DIGIT-20MM">
</package>
<package name="7-SEGMENT-1&quot;PTH-EZ">
</package>
<package name="DIP12-HP-BUBBLE">
</package>
<package name="7-SEGMENT-4DIGIT-YOUNGSUN-LONGPADS">
</package>
<package name="RGB_BAR_GRAPH">
</package>
<package name="LED_BAR_SMD">
<description>&lt;h3&gt;SMA-B520LB LED Bargraph - 5 segment&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=””&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;[EXAMPLE DEVICE 1]&lt;/li&gt;
&lt;li&gt;[EXAMPLE DEVICE 2]&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SUPER_BRIGHT_SMD_LED_3014">
<description>3014 Package for LEDs</description>
</package>
<package name="PLCC4SMDLED">
</package>
<package name="APA102">
</package>
<package name="APA102-2020">
<description>&lt;h3&gt;APA102-2020&lt;/h3&gt;

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 8&lt;/li&gt;
&lt;li&gt;Size: 2.0 x 2.0 mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt; &lt;a href="https://cdn.sparkfun.com/assets/home_page_posts/2/3/9/8/APA102-2020_1.pdf"&gt;APA102-2020&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="APA102-5050">
<description>&lt;h3&gt;APA102C&lt;/h3&gt;

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 6&lt;/li&gt;
&lt;li&gt;Size: 5.0 x 5.0 mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt; &lt;a href="https://cdn.sparkfun.com/datasheets/Components/LED/APA102C.pdf"&gt;APA102C&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="WS2812B-PTH-KIT">
</package>
<package name="LED-1206-HIDDENSILK">
</package>
<package name="APA102-2020-TEST">
</package>
<package name="LED_5MM-KIT-NO-SILK">
<description>&lt;h3&gt;LED 5mm KIT PTH&lt;/h3&gt;
&lt;p&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.&lt;/p&gt;

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1inch&lt;/li&gt;
&lt;li&gt;Diameter: 5mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example Device:
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="WS2812-2020">
<description>&lt;h3&gt;WS2812-2020 - 2020 package for the WS2812&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 4&lt;/li&gt;
&lt;li&gt;Pin pitch: 1 mm&lt;/li&gt;
&lt;li&gt;Area: 2.2 mm x 2.0 mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=https://www.aliexpress.com/store/product/WS2812-2020-Intelligent-control-LED-integrated-light-source-2020-SMD-RGB-LED-with-built-in-WS2811/701799_32879024689.html?spm=2114.12010612.8148356.3.67626848TBx3Ev&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="PLCC-2">
</package>
</packages>
<symbols>
<symbol name="LED">
<description>&lt;h3&gt;LED&lt;/h3&gt;
&lt;p&gt;&lt;/p&gt;</description>
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="LED-RGB-CA">
<description>&lt;h3&gt;RGB LED - Common Anode&lt;/h3&gt;
&lt;p&gt;4 pin Common Anode RGB LED&lt;/p&gt;</description>
<pin name="GRN"/>
<pin name="BLU"/>
<pin name="A"/>
<pin name="RED"/>
</symbol>
<symbol name="LED_BARGRAPH_10">
<description>10 Pin LED Bar Graph (No Common Pins)</description>
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="A5" direction="pas"/>
<pin name="A6" direction="pas"/>
<pin name="A7" direction="pas"/>
<pin name="A8" direction="pas"/>
<pin name="A9" direction="pas"/>
<pin name="C1" direction="pas"/>
<pin name="C2" direction="pas"/>
<pin name="C3" direction="pas"/>
<pin name="C4" direction="pas"/>
<pin name="C5" direction="pas"/>
<pin name="C6" direction="pas"/>
<pin name="C7" direction="pas"/>
<pin name="C8" direction="pas"/>
<pin name="C9" direction="pas"/>
</symbol>
<symbol name="LED-RGB-CC">
<description>&lt;h3&gt;RGB LED - Common Cathode&lt;/h3&gt;
&lt;p&gt;4 pin Common Cathode RGB LED&lt;/p&gt;</description>
<pin name="GRN"/>
<pin name="BLU"/>
<pin name="C"/>
<pin name="RED"/>
</symbol>
<symbol name="LED_RING">
<description>&lt;h3&gt; 16 LED Ring - LED-CCLA&lt;/h3&gt;
&lt;p&gt;16 LEDs broken into quarters. 4 anode pins + 1 common ground / quadrant. &lt;/p&gt;</description>
<pin name="COM1" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="COM2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="COM3" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="COM0" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="LED-RGB-INDV">
<description>&lt;h3&gt;RGB LED - No Common&lt;/h3&gt;
&lt;p&gt;6 pin RGB LED&lt;/p&gt;</description>
<pin name="BLU-A"/>
<pin name="BLU-C"/>
<pin name="GRN-A"/>
<pin name="GRN-C"/>
<pin name="RED-A"/>
<pin name="RED-C"/>
</symbol>
<symbol name="LED-TRICOLOR-WS28X1">
<description>&lt;h3&gt;WS28X1 RGB LED - I2C Control&lt;/h3&gt;
&lt;p&gt;4 pin RGB LED with I2C Controller built-in&lt;/p&gt;</description>
<pin name="VDD"/>
<pin name="VSS"/>
<pin name="DI"/>
<pin name="DO"/>
</symbol>
<symbol name="LED-RG">
<description>&lt;h3&gt;RG LED - No Common&lt;/h3&gt;
&lt;p&gt;4 pin RG LED&lt;/p&gt;</description>
<pin name="GC" direction="pas"/>
<pin name="GA" direction="pas"/>
<pin name="RC" direction="pas"/>
<pin name="RA" direction="pas"/>
</symbol>
<symbol name="7-SEGMENT-4DIGIT-YOUNGSUN">
<pin name="DIG2"/>
<pin name="DIG3"/>
<pin name="DIG4"/>
<pin name="COL-A"/>
<pin name="APOS-A"/>
<pin name="A"/>
<pin name="B"/>
<pin name="C"/>
<pin name="D"/>
<pin name="E"/>
<pin name="F"/>
<pin name="G"/>
<pin name="DP"/>
<pin name="COL-C"/>
<pin name="APOS-C"/>
<pin name="DIG1"/>
</symbol>
<symbol name="7-SEGMENT-1&quot;">
<pin name="A"/>
<pin name="B"/>
<pin name="C"/>
<pin name="D"/>
<pin name="E"/>
<pin name="F"/>
<pin name="G"/>
<pin name="DP"/>
<pin name="G1"/>
<pin name="G2"/>
</symbol>
<symbol name="7-SEGMENT-4DIGIT-COUNTER">
<pin name="A"/>
<pin name="B"/>
<pin name="C"/>
<pin name="D"/>
<pin name="E"/>
<pin name="F"/>
<pin name="G"/>
<pin name="DP"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
</symbol>
<symbol name="RGB_BAR_GRAPH">
<description>48 Segment RGB Bar Graph - Common Anode</description>
<pin name="R1"/>
<pin name="G1"/>
<pin name="B1"/>
<pin name="R2"/>
<pin name="G2"/>
<pin name="B2"/>
<pin name="R3"/>
<pin name="G3"/>
<pin name="B3"/>
<pin name="C1"/>
<pin name="C2"/>
<pin name="C3"/>
<pin name="C4"/>
<pin name="C5"/>
<pin name="C6"/>
<pin name="C7"/>
<pin name="C8"/>
<pin name="C9"/>
<pin name="C10"/>
<pin name="C11"/>
<pin name="C12"/>
<pin name="C13"/>
<pin name="C14"/>
<pin name="C15"/>
<pin name="C16"/>
</symbol>
<symbol name="LED_BAR_SMD">
<description>&lt;h3&gt;5-segment LED Bar Graph&lt;/h3&gt;</description>
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
</symbol>
<symbol name="LED-RGB-I2C">
<description>&lt;h3&gt;RGB LED - I2C&lt;/h3&gt;
&lt;p&gt;6 pin Adafruit DotStar RGB LED&lt;/p&gt;</description>
<pin name="DI"/>
<pin name="DO"/>
<pin name="CI"/>
<pin name="CO"/>
<pin name="GND"/>
<pin name="VCC"/>
</symbol>
<symbol name="APA102">
<pin name="CO"/>
<pin name="DI"/>
<pin name="CI"/>
<pin name="GND"/>
<pin name="DO"/>
<pin name="VCC"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="LED" prefix="D" uservalue="yes">
<description>&lt;b&gt;LED (Generic)&lt;/b&gt;
&lt;p&gt;Standard schematic elements and footprints for 5mm, 3mm, 1206, and 0603 sized LEDs. Generic LEDs with no color specified.&lt;/p&gt;</description>
<gates>
<gate name="D1" symbol="LED"/>
</gates>
<devices>
<device name="5MM" package="LED_5MM">
<connects>
<connect gate="D1" pin="A" pad="A"/>
<connect gate="D1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3MM" package="LED_3MM">
<connects>
<connect gate="D1" pin="A" pad="A"/>
<connect gate="D1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-08794"/>
</technology>
</technologies>
</device>
<device name="1206" package="LED-1206">
<connects>
<connect gate="D1" pin="A" pad="A"/>
<connect gate="D1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603" package="LED-0603">
<connects>
<connect gate="D1" pin="A" pad="A"/>
<connect gate="D1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="10MM" package="LED_10MM">
<connects>
<connect gate="D1" pin="A" pad="A"/>
<connect gate="D1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-FKIT-1206" package="FKIT-LED-1206">
<connects>
<connect gate="D1" pin="A" pad="A"/>
<connect gate="D1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-3MM-NO_SILK" package="LED_3MM-NS">
<connects>
<connect gate="D1" pin="A" pad="A"/>
<connect gate="D1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM-KIT" package="LED_5MM-KIT">
<connects>
<connect gate="D1" pin="A" pad="A"/>
<connect gate="D1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206-BOTTOM" package="LED-1206-BOTTOM">
<connects>
<connect gate="D1" pin="A" pad="A"/>
<connect gate="D1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-5MM-KIT-NO-SILK" package="LED_5MM-KIT-NO-SILK">
<connects>
<connect gate="D1" pin="A" pad="A"/>
<connect gate="D1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PLCC" package="PLCC-2">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED_BARGRAPH_10" prefix="D" uservalue="yes">
<description>&lt;h3&gt;Young Sun LED Tech - YSLB-10251G5-10 10-Segment LED Bar Graph&lt;/h3&gt;
&lt;p&gt;Features:&lt;/p&gt;
&lt;ul&gt;&lt;li&gt;Red Vf = 2.1V, Ifmax = 20mA &lt;/a&gt;&lt;/li&gt;
&lt;li&gt;Yellow Vf = 2.1V, Ifmax = 20mA &lt;/a&gt;&lt;/li&gt;
&lt;li&gt;Blue Vf = 3.4V, Ifmax = 20mA &lt;/a&gt;&lt;/li&gt;
&lt;li&gt;Green Vf = 3.4V, Ifmax = 20mA &lt;/a&gt;&lt;/li&gt;&lt;/ul&gt;

&lt;p&gt;SparkFun Products:
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/9935”&gt;Red&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/9936”&gt;Yellow&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/9938”&gt;Green&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/9937”&gt;Blue&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LED_BARGRAPH_10"/>
</gates>
<devices>
<device name="RED" package="LED_BARGRAPH_10">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="7"/>
<connect gate="G$1" pin="A7" pad="8"/>
<connect gate="G$1" pin="A8" pad="9"/>
<connect gate="G$1" pin="A9" pad="10"/>
<connect gate="G$1" pin="C" pad="20"/>
<connect gate="G$1" pin="C1" pad="19"/>
<connect gate="G$1" pin="C2" pad="18"/>
<connect gate="G$1" pin="C3" pad="17"/>
<connect gate="G$1" pin="C4" pad="16"/>
<connect gate="G$1" pin="C5" pad="15"/>
<connect gate="G$1" pin="C6" pad="14"/>
<connect gate="G$1" pin="C7" pad="13"/>
<connect gate="G$1" pin="C8" pad="12"/>
<connect gate="G$1" pin="C9" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-10615"/>
<attribute name="VALUE" value="RED"/>
</technology>
</technologies>
</device>
<device name="YELLOW" package="LED_BARGRAPH_10">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="7"/>
<connect gate="G$1" pin="A7" pad="8"/>
<connect gate="G$1" pin="A8" pad="9"/>
<connect gate="G$1" pin="A9" pad="10"/>
<connect gate="G$1" pin="C" pad="20"/>
<connect gate="G$1" pin="C1" pad="19"/>
<connect gate="G$1" pin="C2" pad="18"/>
<connect gate="G$1" pin="C3" pad="17"/>
<connect gate="G$1" pin="C4" pad="16"/>
<connect gate="G$1" pin="C5" pad="15"/>
<connect gate="G$1" pin="C6" pad="14"/>
<connect gate="G$1" pin="C7" pad="13"/>
<connect gate="G$1" pin="C8" pad="12"/>
<connect gate="G$1" pin="C9" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-10614"/>
<attribute name="VALUE" value="YELLOW"/>
</technology>
</technologies>
</device>
<device name="BLUE" package="LED_BARGRAPH_10">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="7"/>
<connect gate="G$1" pin="A7" pad="8"/>
<connect gate="G$1" pin="A8" pad="9"/>
<connect gate="G$1" pin="A9" pad="10"/>
<connect gate="G$1" pin="C" pad="20"/>
<connect gate="G$1" pin="C1" pad="19"/>
<connect gate="G$1" pin="C2" pad="18"/>
<connect gate="G$1" pin="C3" pad="17"/>
<connect gate="G$1" pin="C4" pad="16"/>
<connect gate="G$1" pin="C5" pad="15"/>
<connect gate="G$1" pin="C6" pad="14"/>
<connect gate="G$1" pin="C7" pad="13"/>
<connect gate="G$1" pin="C8" pad="12"/>
<connect gate="G$1" pin="C9" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-10613"/>
<attribute name="VALUE" value="BLUE"/>
</technology>
</technologies>
</device>
<device name="GREEN" package="LED_BARGRAPH_10">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="7"/>
<connect gate="G$1" pin="A7" pad="8"/>
<connect gate="G$1" pin="A8" pad="9"/>
<connect gate="G$1" pin="A9" pad="10"/>
<connect gate="G$1" pin="C" pad="20"/>
<connect gate="G$1" pin="C1" pad="19"/>
<connect gate="G$1" pin="C2" pad="18"/>
<connect gate="G$1" pin="C3" pad="17"/>
<connect gate="G$1" pin="C4" pad="16"/>
<connect gate="G$1" pin="C5" pad="15"/>
<connect gate="G$1" pin="C6" pad="14"/>
<connect gate="G$1" pin="C7" pad="13"/>
<connect gate="G$1" pin="C8" pad="12"/>
<connect gate="G$1" pin="C9" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-10612"/>
<attribute name="VALUE" value="GREEN"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED_RING" prefix="D" uservalue="yes">
<description>&lt;h3&gt;Top Up Industry Corp 16 LED Ring - LED-CCLA&lt;/h3&gt;
&lt;p&gt;16 LEDs broken into quarters. 4 anode pins + 1 common ground / quadrant. &lt;/p&gt;

&lt;li&gt;&lt;b&gt;Forward Voltage: &lt;/b&gt;Red 2.4V; Blue 3.0V&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Forward Current: &lt;/b&gt;Red 25mA; Blue 30mA&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Wavelength: &lt;/b&gt; Red 624nm; Blue 465nm&lt;/li&gt;

&lt;p&gt;SparkFun Products:
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/11492”&gt;Blue LED Ring&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/10595”&gt;Red LED Ring&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LED_RING"/>
</gates>
<devices>
<device name="" package="LED_RING">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="COM0" pad="COM0"/>
<connect gate="G$1" pin="COM1" pad="COM1"/>
<connect gate="G$1" pin="COM2" pad="COM2"/>
<connect gate="G$1" pin="COM3" pad="COM3"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="COM-10595"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-GREEN" prefix="D" uservalue="yes">
<description>&lt;h3&gt;Green SMD LED&lt;/h3&gt;
&lt;p&gt;Used in manufacturing of various products at SparkFun&lt;/p&gt;

&lt;p&gt;&lt;b&gt;Packages:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;b&gt;0603&lt;/b&gt; - SMD 0603 package &lt;a href="http://www.futureelectronics.com/en/technologies/semiconductors/optoelectronics/leds/Pages/9894312-LTST-C190GKT.aspx?CrossPart=HSMG-C190&amp;IM=0"&gt;[Product Link]&lt;/li&gt;
&lt;li&gt;&lt;b&gt;LilyPad 1206&lt;/b&gt; - SMD1206 LilyPad package &lt;a href="http://www.futureelectronics.com/en/Technologies/Product.aspx?ProductID=IN150NGHARVATEKCORPORATION2049943&amp;IM=0"&gt;[Product Link]&lt;/li&gt;
&lt;li&gt;&lt;b&gt; 1206&lt;/b&gt; - SMD1206  package &lt;a href=http://www.futureelectronics.com/en/technologies/semiconductors/optoelectronics/leds/Pages/8315665-LTST-C150KGKT.aspx?IM=0"&gt;[Product Link]&lt;/li&gt;
&lt;li&gt;&lt;b&gt; 1206 Bottom Mount&lt;/b&gt; -SMD 1206 Bottom Mount &lt;a href=http://www.digikey.com/product-detail/en/lite-on-inc/LTST-C230KGKT/160-1456-1-ND/386854"&gt;[Product Link]&lt;/li&gt;
&lt;ul&gt;&lt;/p&gt;

&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/821”&gt;Pro Mini 328 -5V&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12757”&gt;RedBoard&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13720”&gt;MP3 Trigger&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/11076”&gt;Makey Makey&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="0603" package="LED-0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-00821"/>
<attribute name="VALUE" value="GREEN"/>
</technology>
</technologies>
</device>
<device name="LILYPAD" package="LED-1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-09910"/>
<attribute name="VALUE" value="GREEN"/>
</technology>
</technologies>
</device>
<device name="1206" package="LED-1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-00862"/>
<attribute name="VALUE" value="GREEN"/>
</technology>
</technologies>
</device>
<device name="1206-BOTTOM" package="LED-1206-BOTTOM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-11076"/>
<attribute name="VALUE" value="Green"/>
</technology>
</technologies>
</device>
<device name="_HIDDENSILK" package="LED-1206-HIDDENSILK">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-00862"/>
<attribute name="VALUE" value="GREEN"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-RED" prefix="D" uservalue="yes">
<description>&lt;h3&gt;Red SMD LED&lt;/h3&gt;
&lt;p&gt;Used in manufacturing of most products at SparkFun&lt;/p&gt;

&lt;p&gt;&lt;b&gt;Packages:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;b&gt;0603&lt;/b&gt; - SMD 0603 package &lt;a href="http://docs.avagotech.com/docs/AV02-0551EN"&gt;[Product Link]&lt;/li&gt;
&lt;li&gt;&lt;b&gt;0603 SMART&lt;/b&gt; - SMD 0603 SMART package ( more efficient and expensive)&lt;a href="http://www.osram-os.com/Graphics/XPic2/00077099_0.pdf"&gt;[Product Link]&lt;/li&gt;
&lt;li&gt;&lt;b&gt; 1206&lt;/b&gt; - SMD1206  package &lt;a href="https://www.sparkfun.com/datasheets/DevTools/LilyPad/Q150OVS4.pdff"&gt;[Product Link]&lt;/li&gt;
&lt;ul&gt;&lt;/p&gt;

&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/821”&gt;Pro Mini 328 -5V&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12757”&gt;RedBoard&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13613”&gt;IOIO-OTG&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="0603" package="LED-0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-00819"/>
<attribute name="VALUE" value="RED"/>
</technology>
</technologies>
</device>
<device name="1206" package="LED-1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-09912"/>
<attribute name="VALUE" value="RED"/>
</technology>
</technologies>
</device>
<device name="0603-SMART" package="LED-0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-11154"/>
<attribute name="VALUE" value="Red"/>
</technology>
</technologies>
</device>
<device name="_HIDDENSILK" package="LED-1206-HIDDENSILK">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-09912"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-WHITE" prefix="D" uservalue="yes">
<description>&lt;h3&gt;White SMD LED&lt;/h3&gt;

Used in manufacturing several products at SparkFun. 

&lt;p&gt;&lt;b&gt;Packages:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;b&gt; 0603&lt;/b&gt; - Bright White SMD 0603  package&lt;a href="http://www.kingbrightusa.com/product.asp?catalog_name=LED&amp;product_id=APT1608QWF/D"&gt;[Product Link]&lt;/li&gt;
&lt;li&gt;&lt;b&gt; 1206&lt;/b&gt; - Bright White SMD1206  package &lt;a href="http://www.kingbrightusa.com/product.asp?catalog_name=LED&amp;product_id=APT3216QWF/D"&gt;[Product Link]&lt;/li&gt;
&lt;li&gt;&lt;b&gt; 3014&lt;/b&gt; - Super Bright SMD 3014 package &lt;a href="http://www.lumileds.com/uploads/459/DS208-pdf"&gt;[Datasheet]&lt;/li&gt;
&lt;ul&gt;&lt;/p&gt;

&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13169”&gt;Blackberry Trackballer Breakout&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12651”&gt;Digital SandBox&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="1206" package="LED-1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-09955"/>
<attribute name="VALUE" value="WHITE"/>
</technology>
</technologies>
</device>
<device name="0603" package="LED-0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-09004"/>
<attribute name="VALUE" value="WHITE"/>
</technology>
</technologies>
</device>
<device name="3014" package="SUPER_BRIGHT_SMD_LED_3014">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-13728"/>
<attribute name="VALUE" value="White, 60mA"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-YELLOW" prefix="D" uservalue="yes">
<description>&lt;h3&gt;Yellow SMD LED&lt;/h3&gt;

Used in manufacturing several products at SparkFun. 

&lt;p&gt;&lt;b&gt;Packages:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;b&gt; 0603&lt;/b&gt; -  SMD 0603  package&lt;a href=http://www.kingbrightusa.com/product.asp?catalog_name=LED&amp;product_id=APT1608SYCK"&gt;[Product Link]&lt;/li&gt;
&lt;li&gt;&lt;b&gt; 0603 -SMART&lt;/b&gt; - SMART SMD 0603  package (more efficient/more expensive) &lt;a href="http://www.osram-os.com/osram_os/en/products/product-catalog/led-light-emitting-diodes/smartled-0603/ly-l29k/index.jsp"&gt;[Product Link]&lt;/li&gt;
&lt;li&gt;&lt;b&gt; LilyPad&lt;/b&gt; - SMD1206  package&lt;a href="https://www.sparkfun.com/datasheets/DevTools/LilyPad/Q150YUS4.pdf"&gt;[Product Datasheet]&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;


&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13794”&gt;Blynk Board&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13613”&gt;IOIO-OTG&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13225”&gt;XBee Explorer Serial&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="LILYPAD" package="LED-1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-09909"/>
<attribute name="VALUE" value="Yellow"/>
</technology>
</technologies>
</device>
<device name="0603" package="LED-0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-09003"/>
<attribute name="VALUE" value="Yellow"/>
</technology>
</technologies>
</device>
<device name="0603-SMART" package="LED-0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-11230"/>
<attribute name="VALUE" value="Yellow"/>
</technology>
</technologies>
</device>
<device name="_HIDDENSILK" package="LED-1206-HIDDENSILK">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-09909"/>
<attribute name="VALUE" value="YELLOW"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-RGB-CA" prefix="D" uservalue="yes">
<description>&lt;h3&gt;LED-RGB Diffused Common Anode&lt;/h3&gt;

&lt;p&gt;
&lt;li&gt;&lt;b&gt;Packages:&lt;/b&gt;&lt;/li&gt;
&lt;ul&gt;&lt;li&gt; LED RGB-THRU&lt;/li&gt;
&lt;li&gt; P-LCC-4-3&lt;/li&gt;
&lt;li&gt;LED-TRICOLOR-SMD&lt;/li&gt;
&lt;ul&gt;&lt;/p&gt;

&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”[https://www.sparkfun.com/products/10821]”&gt;RGB Diffused Common Anode- Diffuse&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”[https://www.sparkfun.com/products/10820]”&gt;RGB Diffused Common Anode - Clear&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”[https://www.sparkfun.com/products/13614]”&gt;Qduino Mini&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/7844”&gt;Triple Output LED RGB - SMD&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LED-RGB-CA"/>
</gates>
<devices>
<device name="DIFFUSE" package="LED-RGB-THRU">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="BLU" pad="4"/>
<connect gate="G$1" pin="GRN" pad="3"/>
<connect gate="G$1" pin="RED" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-10632"/>
<attribute name="VALUE" value="DIFFUSE"/>
</technology>
</technologies>
</device>
<device name="CLEAR" package="LED-RGB-THRU">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="BLU" pad="4"/>
<connect gate="G$1" pin="GRN" pad="3"/>
<connect gate="G$1" pin="RED" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-10631"/>
<attribute name="VALUE" value="CLEAR"/>
</technology>
</technologies>
</device>
<device name="PLCC" package="P-LCC-4-3">
<connects>
<connect gate="G$1" pin="A" pad="4"/>
<connect gate="G$1" pin="BLU" pad="3"/>
<connect gate="G$1" pin="GRN" pad="2"/>
<connect gate="G$1" pin="RED" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-12986"/>
<attribute name="VALUE" value="RGB"/>
</technology>
</technologies>
</device>
<device name="SMD" package="LED-TRICOLOR-SMD">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="BLU" pad="B"/>
<connect gate="G$1" pin="GRN" pad="G"/>
<connect gate="G$1" pin="RED" pad="R"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-08324"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-RGB-CC" prefix="D" uservalue="yes">
<description>&lt;h3&gt;LED-RGB Common Cathode&lt;/h3&gt;

&lt;li&gt;&lt;b&gt;Packages:&lt;/b&gt;&lt;/li&gt;
&lt;ul&gt;&lt;li&gt; LED RGB-THRU&lt;/li&gt;
&lt;li&gt; LED_PIRANHA_5MM&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;


&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”[https://www.sparkfun.com/products/9264]”&gt;RGB Diffused Common Cathode- Diffuse&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”[https://www.sparkfun.com/products/105]”&gt;RGB Diffused Common Cathode - Clear&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”[https://www.sparkfun.com/products/11679]”&gt;LED-RGB 5mm Square (Piranha)&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LED-RGB-CC"/>
</gates>
<devices>
<device name="DIFFUSE" package="LED-RGB-THRU">
<connects>
<connect gate="G$1" pin="BLU" pad="4"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="GRN" pad="3"/>
<connect gate="G$1" pin="RED" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-09434"/>
<attribute name="VALUE" value="DIFFUSE"/>
</technology>
</technologies>
</device>
<device name="CLEAR" package="LED-RGB-THRU">
<connects>
<connect gate="G$1" pin="BLU" pad="4"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="GRN" pad="3"/>
<connect gate="G$1" pin="RED" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-08418"/>
<attribute name="VALUE" value="CLEAR"/>
</technology>
</technologies>
</device>
<device name="PIRANHA" package="LED_PIRANHA_5MM">
<connects>
<connect gate="G$1" pin="BLU" pad="B"/>
<connect gate="G$1" pin="C" pad="-"/>
<connect gate="G$1" pin="GRN" pad="G"/>
<connect gate="G$1" pin="RED" pad="R"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_ID" value="COM-11679"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WS2812" prefix="U">
<description>&lt;h3&gt;WS2812 RGB LED w/ WS2811 driver&lt;/h3&gt;
5x5mm SMD LED with built-in controller IC.

&lt;p&gt;&lt;li&gt;&lt;b&gt;Color:&lt;/b&gt; Red/Green/Blue&lt;/li&gt;
&lt;li&gt;&lt;b&gt;mC Rating: &lt;/b&gt;RGB: 550, 1100, 200 mcd&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Current:&lt;/b&gt;RGB: 20, 20, 20 mA&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Forward Voltage: &lt;/b&gt; RGB: 1.8, 3.0, 3.2 V&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Packages:&lt;/b&gt;LED-TRICOLOR-5050-IC&lt;/li&gt;
&lt;/p&gt;
&lt;p&gt;SparkFun Products:
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/11821”&gt;LED-SMD RGB (WS2812)&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="U1" symbol="LED-TRICOLOR-WS28X1"/>
</gates>
<devices>
<device name="&quot;" package="LED-TRICOLOR-5050-IC">
<connects>
<connect gate="U1" pin="DI" pad="2" route="any"/>
<connect gate="U1" pin="DO" pad="1"/>
<connect gate="U1" pin="VDD" pad="3 5"/>
<connect gate="U1" pin="VSS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-11598"/>
<attribute name="VALUE" value="WS2812"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-BLUE" prefix="D" uservalue="yes">
<description>&lt;h3&gt;Blue SMD LED&lt;/h3&gt;
&lt;p&gt;Used in manufacturing of various products at SparkFun&lt;/p&gt;


&lt;p&gt;&lt;b&gt;Packages:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;b&gt;0603&lt;/b&gt; - SMD 0603 package &lt;a href="http://www.digikey.com/product-detail/en/SMLE12BC7TT86/511-1589-2-ND/1641808"&gt;[Product Link]&lt;/li&gt;
&lt;li&gt;&lt;b&gt;1206&lt;/b&gt; - SMD1206  package &lt;a href="http://www.digikey.com/product-detail/en/lite-on-inc/LTST-C150TBKT/160-1643-1-ND/573584"&gt;[Product Link]&lt;/li&gt;
&lt;ul&gt;&lt;/p&gt;

&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13711”&gt;ESP8266 Thing-Dev Board&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12757”&gt;RedBoard&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="0603" package="LED-0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-08575"/>
<attribute name="VALUE" value="BLUE"/>
</technology>
</technologies>
</device>
<device name="1206" package="LED-1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-09911"/>
<attribute name="VALUE" value="BLUE"/>
</technology>
</technologies>
</device>
<device name="_HIDDENSILK" package="LED-1206-HIDDENSILK">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-09911"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-PINK" prefix="D" uservalue="yes">
<description>&lt;h3&gt;Pink SMD LED&lt;/h3&gt;
&lt;p&gt;Used in manufacturing of various products at SparkFun&lt;/p&gt;

&lt;p&gt;&lt;b&gt;Packages:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;b&gt;0603&lt;/b&gt; - SMD 0603 package &lt;a href="http://cdn.sparkfun.com/datasheets/Components/General/S1206PKSBJC.pdf"&gt;[Product Link]&lt;/li&gt;
&lt;ul&gt;&lt;/p&gt;

&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/10962”&gt;LilyPad LED Pink&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="1206" package="LED-1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-10415"/>
<attribute name="VALUE" value="PINK"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SFH4641" prefix="D">
<description>&lt;h3&gt;OSRAM SFH 4641-Z - Infrared Emitters - High Power Infrared 940nm&lt;/h3&gt;

&lt;p&gt;
&lt;li&gt;&lt;b&gt;Wavelength:&lt;/b&gt;950nm&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Beam Angle:&lt;/b&gt;20 degree&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Forward Current:&lt;/b&gt;70mA&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Forward Voltage:&lt;/b&gt;1.6V&lt;/li&gt;

&lt;/p&gt;

&lt;p&gt;Variants:
&lt;ul&gt;&lt;li&gt;&lt;b&gt;Large&lt;/b&gt;:Large pads&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Narrow:&lt;/b&gt;Narrow pads&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Oversize:&lt;/b&gt;Oversize pads&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Short:&lt;/b&gt;Short pads&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Short2:&lt;/b&gt;Short, wide pads&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;

&lt;p&gt;SparkFun Products:
&lt;ul&gt;&lt;li&gt;&lt;a href=”[https://www.sparkfun.com/products/13162]”&gt;ZX Distance and Gesture Sensor&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="LARGE" package="SFH4641">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-11994"/>
</technology>
</technologies>
</device>
<device name="NARROW" package="SFH4641-NARROW">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-11994"/>
</technology>
</technologies>
</device>
<device name="SHORT" package="SFH4641-SHORT">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-11994"/>
</technology>
</technologies>
</device>
<device name="OVERSIZE" package="SFH4641-OVERSIZE">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-11994"/>
</technology>
</technologies>
</device>
<device name="SHORT2" package="SFH4641-SHORT2">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-11994"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WS2812B" prefix="D" uservalue="yes">
<description>&lt;h3&gt;WS2812B SMD addressable RGB LED&lt;/h3&gt;
5x5mm SMD LED with built-in controller IC.

&lt;p&gt;&lt;li&gt;&lt;b&gt;Color:&lt;/b&gt; Red/Green/Blue&lt;/li&gt;
&lt;li&gt;&lt;b&gt;mC Rating: &lt;/b&gt;RGB: 390, 660, 180 mcd&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Forward Voltage: &lt;/b&gt; RGB: 2.0, 3.0, 3.0 V&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Packages:&lt;/b&gt;WS2812B&lt;/li&gt;
&lt;/p&gt;
&lt;p&gt;SparkFun Products:
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13794”&gt;Blynk Board - ESP8266&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LED-TRICOLOR-WS28X1"/>
</gates>
<devices>
<device name="" package="WS2812B">
<connects>
<connect gate="G$1" pin="DI" pad="4"/>
<connect gate="G$1" pin="DO" pad="2"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-12503"/>
<attribute name="VALUE" value="WS2812B"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-IR" prefix="D">
<description>&lt;h3&gt;Infrared LED (IR)&lt;/h3&gt;
&lt;p&gt;&lt;li&gt;&lt;b&gt; Wavelength: &lt;/b&gt; 940nm&lt;/li&gt;

&lt;/p&gt;

&lt;p&gt;
&lt;li&gt;&lt;b&gt;Packages:&lt;/b&gt;&lt;/li&gt;
&lt;ul&gt;&lt;li&gt;&lt;b&gt;TSAL6100&lt;/b&gt; &lt;/li&gt;
&lt;li&gt;&lt;b&gt; LTE302&lt;/b&gt; - Side firing. Check SparkFun-Sensors.lbr for the receiver&lt;/li&gt; 
&lt;ul&gt;&lt;/p&gt;

&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”[https://www.sparkfun.com/products/12780]”&gt;ZX Distance and Gesture Sensor&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/241”&gt;Infrared Emitters and Detectors&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="TSAL6100" package="LED_5MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-12058"/>
</technology>
</technologies>
</device>
<device name="SIDE_EMITTER" package="LTE-302">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-14163"/>
<attribute name="SF_ID" value="SEN-00241"/>
</technology>
</technologies>
</device>
<device name="0603" package="LED-0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-14125"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-RGB" prefix="D" uservalue="yes">
<description>&lt;h3&gt;LED-RGB &lt;/h3&gt;
6 pin RGB LED (no common connector)
&lt;p&gt;

&lt;li&gt;&lt;b&gt;Packages:&lt;/b&gt;&lt;/li&gt;
&lt;ul&gt;&lt;li&gt; PLCC-6&lt;/li&gt;
&lt;li&gt;&lt;b&gt;LED-TRICOLOR-5050&lt;/b&gt; - No built-in IC&lt;/li&gt;
&lt;ul&gt;&lt;/p&gt;

&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/12651”&gt;Digital Sandbox&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/10866”&gt; LED- SMD RGB&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LED-RGB-INDV"/>
</gates>
<devices>
<device name="PLCC-6" package="PLCC-6-LED">
<connects>
<connect gate="G$1" pin="BLU-A" pad="AB"/>
<connect gate="G$1" pin="BLU-C" pad="CB"/>
<connect gate="G$1" pin="GRN-A" pad="AG"/>
<connect gate="G$1" pin="GRN-C" pad="CG"/>
<connect gate="G$1" pin="RED-A" pad="AR"/>
<connect gate="G$1" pin="RED-C" pad="CR"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-12113"/>
<attribute name="VALUE" value="RGB"/>
</technology>
</technologies>
</device>
<device name="NO_IC" package="LED-TRICOLOR-5050">
<connects>
<connect gate="G$1" pin="BLU-A" pad="3"/>
<connect gate="G$1" pin="BLU-C" pad="4"/>
<connect gate="G$1" pin="GRN-A" pad="1"/>
<connect gate="G$1" pin="GRN-C" pad="6"/>
<connect gate="G$1" pin="RED-A" pad="2"/>
<connect gate="G$1" pin="RED-C" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-10298"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-RG" prefix="D">
<description>&lt;h3&gt;LiteOn Technology Corporation LTST-C195KGJRKT - LED GREEN/RED CLEAR 0606 SMD&lt;/h3&gt;

&lt;p&gt;&lt;li&gt;&lt;b&gt;Color:&lt;/b&gt; Red/Green&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Lens Transparency: &lt;/b&gt; Clear&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Lens Style/Size:&lt;/b&gt; Rectangle with Flat top, 1.10 x 1.5 mm&lt;/li&gt;
&lt;li&gt;&lt;b&gt;mC Rating&lt;/b&gt;45mcd Red, 35 mcd Green&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Current:&lt;/b&gt; 20mA Red, 20mA Green&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Forward Voltage: &lt;/b&gt; 2V Red, 2V Green&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Packages:&lt;/b&gt; 0606&lt;/li&gt;
&lt;/p&gt;

&lt;p&gt;SparkFun Products:
&lt;ul&gt;&lt;li&gt;&lt;a href=”[https://www.sparkfun.com/products/12958]”&gt;Electric Imp imp002 Breakout&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LED-RG"/>
</gates>
<devices>
<device name="LTST-C195KGJRKT" package="LTST-C195KGJRKT">
<connects>
<connect gate="G$1" pin="GA" pad="P$1"/>
<connect gate="G$1" pin="GC" pad="P$3"/>
<connect gate="G$1" pin="RA" pad="P$2"/>
<connect gate="G$1" pin="RC" pad="P$4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-12140"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7-SEGMENT-4DIGIT-10MM" prefix="LED">
<description>&lt;h3&gt;4 Digit 7 Segment Display&lt;/h3&gt;
&lt;p&gt;This is a part for the 4-Digit 7-segment LEDs from Young Sun.  Different from the Digikey LEDs, all 16 pins are used.
&lt;br&gt;
The LONGPADS Variant is used for a test jig, but you may like it because there is more pad to solder to. If you are concerned about routing space, the standard works just fine though.&lt;/p&gt;
&lt;h4&gt;Datasheets:&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="http://www.sparkfun.com/datasheets/Components/LED/7-Segment/YSD-439AR6B-35.pdf"&gt;Red&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href="http://www.sparkfun.com/datasheets/Components/LED/7-Segment/YSD-439AY2B-35.pdf"&gt;Yellow&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href="http://www.sparkfun.com/datasheets/Components/LED/7-Segment/YSD-439AK2B-35.pdf"&gt;Kelly Green&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href="http://www.sparkfun.com/datasheets/Components/LED/7-Segment/YSD-439AB4B-35.pdf"&gt;Blue&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/LED/ATA3492BW_2.pdf"&gt;White&lt;/a&gt;&lt;/li&gt;

&lt;/ul&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;h5&gt;Raw Components&lt;/h5&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9483"&gt;7-Segment Display - 4-Digit (Red)&lt;/a&gt; (COM-09483)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9480"&gt;7-Segment Display - 4-Digit (Yellow)&lt;/a&gt; (COM-09480)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9482"&gt;7-Segment Display - 4-Digit (Kelly Green)&lt;/a&gt; (COM-09482)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9481"&gt;7-Segment Display - 4-Digit (Blue)&lt;/a&gt; (COM-09481)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/10931"&gt;7-Segment Display - 4-Digit (White)&lt;/a&gt; ( COM-10931)&lt;/li&gt;
&lt;h5&gt;Serial Controlled&lt;/h5&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11441"&gt;SparkFun 7-Segment Serial Display - Red&lt;/a&gt; (COM-11441)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11443"&gt;SparkFun 7-Segment Serial Display - Yellow&lt;/a&gt; (COM-11443)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11440"&gt;SparkFun 7-Segment Serial Display - Kelly Green&lt;/a&gt; (COM-11440)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11442"&gt;SparkFun 7-Segment Serial Display - Blue&lt;/a&gt; (COM-11442)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11629"&gt;SparkFun 7-Segment Serial Display - White&lt;/a&gt; (COM-11629)&lt;/li&gt;
&lt;h5&gt;Other&lt;/h5&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11734"&gt;SparkFun BigTime Watch Kit&lt;/a&gt; (KIT-11734)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="7-SEGMENT-4DIGIT-YOUNGSUN"/>
</gates>
<devices>
<device name="-RED" package="7-SEGMENT-4DIGIT-YOUNGSUN">
<connects>
<connect gate="G$1" pin="A" pad="14"/>
<connect gate="G$1" pin="APOS-A" pad="10"/>
<connect gate="G$1" pin="APOS-C" pad="9"/>
<connect gate="G$1" pin="B" pad="16"/>
<connect gate="G$1" pin="C" pad="13"/>
<connect gate="G$1" pin="COL-A" pad="4"/>
<connect gate="G$1" pin="COL-C" pad="12"/>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="DIG1" pad="1"/>
<connect gate="G$1" pin="DIG2" pad="2"/>
<connect gate="G$1" pin="DIG3" pad="6"/>
<connect gate="G$1" pin="DIG4" pad="8"/>
<connect gate="G$1" pin="DP" pad="7"/>
<connect gate="G$1" pin="E" pad="5"/>
<connect gate="G$1" pin="F" pad="11"/>
<connect gate="G$1" pin="G" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-09493"/>
<attribute name="VALUE" value="YSD-439AR6B-35"/>
</technology>
</technologies>
</device>
<device name="LONGPADS-RED" package="7-SEGMENT-4DIGIT-YOUNGSUN-LONGPADS">
<connects>
<connect gate="G$1" pin="A" pad="14"/>
<connect gate="G$1" pin="APOS-A" pad="10"/>
<connect gate="G$1" pin="APOS-C" pad="9"/>
<connect gate="G$1" pin="B" pad="16"/>
<connect gate="G$1" pin="C" pad="13"/>
<connect gate="G$1" pin="COL-A" pad="4"/>
<connect gate="G$1" pin="COL-C" pad="12"/>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="DIG1" pad="1"/>
<connect gate="G$1" pin="DIG2" pad="2"/>
<connect gate="G$1" pin="DIG3" pad="6"/>
<connect gate="G$1" pin="DIG4" pad="8"/>
<connect gate="G$1" pin="DP" pad="7"/>
<connect gate="G$1" pin="E" pad="5"/>
<connect gate="G$1" pin="F" pad="11"/>
<connect gate="G$1" pin="G" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-09493"/>
<attribute name="VALUE" value="YSD-439AR6B-35"/>
</technology>
</technologies>
</device>
<device name="-YELLOW" package="7-SEGMENT-4DIGIT-YOUNGSUN">
<connects>
<connect gate="G$1" pin="A" pad="14"/>
<connect gate="G$1" pin="APOS-A" pad="10"/>
<connect gate="G$1" pin="APOS-C" pad="9"/>
<connect gate="G$1" pin="B" pad="16"/>
<connect gate="G$1" pin="C" pad="13"/>
<connect gate="G$1" pin="COL-A" pad="4"/>
<connect gate="G$1" pin="COL-C" pad="12"/>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="DIG1" pad="1"/>
<connect gate="G$1" pin="DIG2" pad="2"/>
<connect gate="G$1" pin="DIG3" pad="6"/>
<connect gate="G$1" pin="DIG4" pad="8"/>
<connect gate="G$1" pin="DP" pad="7"/>
<connect gate="G$1" pin="E" pad="5"/>
<connect gate="G$1" pin="F" pad="11"/>
<connect gate="G$1" pin="G" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-09654"/>
<attribute name="VALUE" value="YSD-439AY2B-35"/>
</technology>
</technologies>
</device>
<device name="-KGREEN" package="7-SEGMENT-4DIGIT-YOUNGSUN">
<connects>
<connect gate="G$1" pin="A" pad="14"/>
<connect gate="G$1" pin="APOS-A" pad="10"/>
<connect gate="G$1" pin="APOS-C" pad="9"/>
<connect gate="G$1" pin="B" pad="16"/>
<connect gate="G$1" pin="C" pad="13"/>
<connect gate="G$1" pin="COL-A" pad="4"/>
<connect gate="G$1" pin="COL-C" pad="12"/>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="DIG1" pad="1"/>
<connect gate="G$1" pin="DIG2" pad="2"/>
<connect gate="G$1" pin="DIG3" pad="6"/>
<connect gate="G$1" pin="DIG4" pad="8"/>
<connect gate="G$1" pin="DP" pad="7"/>
<connect gate="G$1" pin="E" pad="5"/>
<connect gate="G$1" pin="F" pad="11"/>
<connect gate="G$1" pin="G" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-09665"/>
<attribute name="VALUE" value="YSD-439AK2B-35"/>
</technology>
</technologies>
</device>
<device name="-BLUE" package="7-SEGMENT-4DIGIT-YOUNGSUN">
<connects>
<connect gate="G$1" pin="A" pad="14"/>
<connect gate="G$1" pin="APOS-A" pad="10"/>
<connect gate="G$1" pin="APOS-C" pad="9"/>
<connect gate="G$1" pin="B" pad="16"/>
<connect gate="G$1" pin="C" pad="13"/>
<connect gate="G$1" pin="COL-A" pad="4"/>
<connect gate="G$1" pin="COL-C" pad="12"/>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="DIG1" pad="1"/>
<connect gate="G$1" pin="DIG2" pad="2"/>
<connect gate="G$1" pin="DIG3" pad="6"/>
<connect gate="G$1" pin="DIG4" pad="8"/>
<connect gate="G$1" pin="DP" pad="7"/>
<connect gate="G$1" pin="E" pad="5"/>
<connect gate="G$1" pin="F" pad="11"/>
<connect gate="G$1" pin="G" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-09664"/>
<attribute name="VALUE" value="YSD-439AB4B-35"/>
</technology>
</technologies>
</device>
<device name="-WHITE" package="7-SEGMENT-4DIGIT-YOUNGSUN">
<connects>
<connect gate="G$1" pin="A" pad="14"/>
<connect gate="G$1" pin="APOS-A" pad="10"/>
<connect gate="G$1" pin="APOS-C" pad="9"/>
<connect gate="G$1" pin="B" pad="16"/>
<connect gate="G$1" pin="C" pad="13"/>
<connect gate="G$1" pin="COL-A" pad="4"/>
<connect gate="G$1" pin="COL-C" pad="12"/>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="DIG1" pad="1"/>
<connect gate="G$1" pin="DIG2" pad="2"/>
<connect gate="G$1" pin="DIG3" pad="6"/>
<connect gate="G$1" pin="DIG4" pad="8"/>
<connect gate="G$1" pin="DP" pad="7"/>
<connect gate="G$1" pin="E" pad="5"/>
<connect gate="G$1" pin="F" pad="11"/>
<connect gate="G$1" pin="G" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-11430"/>
<attribute name="VALUE" value="WD03942-white / ATA3492BW"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7-SEGMENT-1DIGIT-1INCH">
<description>&lt;h3&gt;7-Segment Display, single digit, 1"&lt;/h3&gt;
&lt;p&gt;EZ is for kits. Pads are only exposed on the bottom side to help prevent soldering in upside down.
&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Components/LED/YSD-160AR4B-8.pdf"&gt;Datasheet (Red)&lt;/a&gt;
&lt;br&gt;
&lt;a href="https://cdn.sparkfun.com/datasheets/Components/LED/YSD-160AB3C-8.pdf"&gt;Datasheet (Blue)&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/8546"&gt;7-Segment Display - LED (Red)&lt;/a&gt; (COM-08546)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/9191"&gt;7-Segment Display - LED (Blue)&lt;/a&gt; (COM-09191)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="7-SEGMENT-1&quot;"/>
</gates>
<devices>
<device name="-RED" package="7-SEGMENT-1&quot;PTH">
<connects>
<connect gate="G$1" pin="A" pad="7"/>
<connect gate="G$1" pin="B" pad="6"/>
<connect gate="G$1" pin="C" pad="4"/>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="DP" pad="5"/>
<connect gate="G$1" pin="E" pad="1"/>
<connect gate="G$1" pin="F" pad="9"/>
<connect gate="G$1" pin="G" pad="10"/>
<connect gate="G$1" pin="G1" pad="3"/>
<connect gate="G$1" pin="G2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-08615"/>
<attribute name="VALUE" value="YSD-1601AR4B-8"/>
</technology>
</technologies>
</device>
<device name="-RED-EZ" package="7-SEGMENT-1&quot;PTH-EZ">
<connects>
<connect gate="G$1" pin="A" pad="7"/>
<connect gate="G$1" pin="B" pad="6"/>
<connect gate="G$1" pin="C" pad="4"/>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="DP" pad="5"/>
<connect gate="G$1" pin="E" pad="1"/>
<connect gate="G$1" pin="F" pad="9"/>
<connect gate="G$1" pin="G" pad="10"/>
<connect gate="G$1" pin="G1" pad="3"/>
<connect gate="G$1" pin="G2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-08615"/>
<attribute name="VALUE" value="YSD-1601AR4B-8"/>
</technology>
</technologies>
</device>
<device name="-BLUE" package="7-SEGMENT-1&quot;PTH">
<connects>
<connect gate="G$1" pin="A" pad="7"/>
<connect gate="G$1" pin="B" pad="6"/>
<connect gate="G$1" pin="C" pad="4"/>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="DP" pad="5"/>
<connect gate="G$1" pin="E" pad="1"/>
<connect gate="G$1" pin="F" pad="9"/>
<connect gate="G$1" pin="G" pad="10"/>
<connect gate="G$1" pin="G1" pad="3"/>
<connect gate="G$1" pin="G2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-09495"/>
<attribute name="VALUE" value="YSD-160AB3C-8"/>
</technology>
</technologies>
</device>
<device name="-BLUE-EZ" package="7-SEGMENT-1&quot;PTH-EZ">
<connects>
<connect gate="G$1" pin="A" pad="7"/>
<connect gate="G$1" pin="B" pad="6"/>
<connect gate="G$1" pin="C" pad="4"/>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="DP" pad="5"/>
<connect gate="G$1" pin="E" pad="1"/>
<connect gate="G$1" pin="F" pad="9"/>
<connect gate="G$1" pin="G" pad="10"/>
<connect gate="G$1" pin="G1" pad="3"/>
<connect gate="G$1" pin="G2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-09495"/>
<attribute name="VALUE" value="YSD-160AB3C-8"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7-SEGMENT-4DIGIT-20MM" prefix="DISP">
<description>&lt;h3&gt;4 Digit 7 Segment Display&lt;/h3&gt;
&lt;p&gt;This is a part for the 4-Digit 7-segment LEDs from Young Sun.  Different from the Digikey LEDs, all 16 pins are used.
&lt;br&gt;
The LONGPADS Variant is used for a test jig, but you may like it because there is more pad to solder to. If you are concerned about routing space, the standard works just fine though.&lt;/p&gt;
&lt;h4&gt;Datasheets:&lt;/h4&gt;
&lt;ul&gt;
&lt;li&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/LED/1LEDREDCC.pdf"&gt;Red&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/LED/1LEDYELCC.pdf"&gt;Yellow&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/LED/1LEDGRNCC.pdf"&gt;Green&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/LED/1LEDBLUCC.pdf"&gt;Blue&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/LED/1LEDWHTCC.pdf"&gt;White&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;
&lt;h4&gt;SparkFun Products&lt;/h4&gt;
&lt;ul&gt;
&lt;h5&gt;Raw Components&lt;/h5&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11405"&gt;7-Segment Display - 20mm (Red)&lt;/a&gt; (COM-11405)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11406"&gt;7-Segment Display - 20mm (Yellow)&lt;/a&gt; (COM-11406)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11407"&gt;7-Segment Display - 20mm (Green)&lt;/a&gt; (COM-11407)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11408"&gt;7-Segment Display - 20mm (Blue)&lt;/a&gt; (COM-11408)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11409"&gt;7-Segment Display - 20mm (White)&lt;/a&gt; (COM-11409)&lt;/li&gt;
&lt;h5&gt;Serial Controlled&lt;/h5&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11644"&gt;SparkFun OpenSegment Serial Display - 20mm (Red)&lt;/a&gt; (COM-11644)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11645"&gt;SparkFun OpenSegment Serial Display - 20mm (Yellow)&lt;/a&gt; (COM-11645)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11646"&gt;SparkFun OpenSegment Serial Display - 20mm (Green)&lt;/a&gt; (COM-11646)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11647"&gt;SparkFun OpenSegment Serial Display - 20mm (Blue)&lt;/a&gt; (COM-11647)&lt;/li&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/11648"&gt;SparkFun OpenSegment Serial Display - 20mm (White)&lt;/a&gt; (COM-11648)&lt;/li&gt;
&lt;h5&gt;Other&lt;/h5&gt;
&lt;li&gt;&lt;a href="https://www.sparkfun.com/products/13190"&gt;SparkFun OpenSegment Shield&lt;/a&gt; (DEV-13190)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="7-SEGMENT-4DIGIT-COUNTER"/>
</gates>
<devices>
<device name="-RED" package="7-SEGMENT-4DIGIT-20MM">
<connects>
<connect gate="G$1" pin="A" pad="11"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="C" pad="4"/>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="D1" pad="12"/>
<connect gate="G$1" pin="D2" pad="9"/>
<connect gate="G$1" pin="D3" pad="8"/>
<connect gate="G$1" pin="D4" pad="6"/>
<connect gate="G$1" pin="DP" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
<connect gate="G$1" pin="F" pad="10"/>
<connect gate="G$1" pin="G" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-11449"/>
<attribute name="VALUE" value="ATA8041ARBJ "/>
</technology>
</technologies>
</device>
<device name="-HP-BUBBLE" package="DIP12-HP-BUBBLE">
<connects>
<connect gate="G$1" pin="A" pad="12"/>
<connect gate="G$1" pin="B" pad="11"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="D" pad="8"/>
<connect gate="G$1" pin="D1" pad="1"/>
<connect gate="G$1" pin="D2" pad="10"/>
<connect gate="G$1" pin="D3" pad="4"/>
<connect gate="G$1" pin="D4" pad="6"/>
<connect gate="G$1" pin="DP" pad="5"/>
<connect gate="G$1" pin="E" pad="2"/>
<connect gate="G$1" pin="F" pad="9"/>
<connect gate="G$1" pin="G" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="STOREFRONT" value="COM-12710"/>
</technology>
</technologies>
</device>
<device name="-YELLOW" package="7-SEGMENT-4DIGIT-20MM">
<connects>
<connect gate="G$1" pin="A" pad="11"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="C" pad="4"/>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="D1" pad="12"/>
<connect gate="G$1" pin="D2" pad="9"/>
<connect gate="G$1" pin="D3" pad="8"/>
<connect gate="G$1" pin="D4" pad="6"/>
<connect gate="G$1" pin="DP" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
<connect gate="G$1" pin="F" pad="10"/>
<connect gate="G$1" pin="G" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-11448"/>
<attribute name="VALUE" value="ATA8041AY"/>
</technology>
</technologies>
</device>
<device name="-GREEN" package="7-SEGMENT-4DIGIT-20MM">
<connects>
<connect gate="G$1" pin="A" pad="11"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="C" pad="4"/>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="D1" pad="12"/>
<connect gate="G$1" pin="D2" pad="9"/>
<connect gate="G$1" pin="D3" pad="8"/>
<connect gate="G$1" pin="D4" pad="6"/>
<connect gate="G$1" pin="DP" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
<connect gate="G$1" pin="F" pad="10"/>
<connect gate="G$1" pin="G" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-11447"/>
<attribute name="VALUE" value="ATA8041AG"/>
</technology>
</technologies>
</device>
<device name="-BLUE" package="7-SEGMENT-4DIGIT-20MM">
<connects>
<connect gate="G$1" pin="A" pad="11"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="C" pad="4"/>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="D1" pad="12"/>
<connect gate="G$1" pin="D2" pad="9"/>
<connect gate="G$1" pin="D3" pad="8"/>
<connect gate="G$1" pin="D4" pad="6"/>
<connect gate="G$1" pin="DP" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
<connect gate="G$1" pin="F" pad="10"/>
<connect gate="G$1" pin="G" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-11446"/>
<attribute name="VALUE" value="ATA8041AB"/>
</technology>
</technologies>
</device>
<device name="-WHITE" package="7-SEGMENT-4DIGIT-20MM">
<connects>
<connect gate="G$1" pin="A" pad="11"/>
<connect gate="G$1" pin="B" pad="7"/>
<connect gate="G$1" pin="C" pad="4"/>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="D1" pad="12"/>
<connect gate="G$1" pin="D2" pad="9"/>
<connect gate="G$1" pin="D3" pad="8"/>
<connect gate="G$1" pin="D4" pad="6"/>
<connect gate="G$1" pin="DP" pad="3"/>
<connect gate="G$1" pin="E" pad="1"/>
<connect gate="G$1" pin="F" pad="10"/>
<connect gate="G$1" pin="G" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COMP-11445"/>
<attribute name="VALUE" value="ATA8041AW"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RGB_BAR_GRAPH" prefix="D">
<description>SparkFun 48 Segment RGB Bar Graph - Common Anode</description>
<gates>
<gate name="D1" symbol="RGB_BAR_GRAPH"/>
</gates>
<devices>
<device name="CA" package="RGB_BAR_GRAPH">
<connects>
<connect gate="D1" pin="B1" pad="24"/>
<connect gate="D1" pin="B2" pad="6"/>
<connect gate="D1" pin="B3" pad="14"/>
<connect gate="D1" pin="C1" pad="1"/>
<connect gate="D1" pin="C10" pad="8"/>
<connect gate="D1" pin="C11" pad="19"/>
<connect gate="D1" pin="C12" pad="18"/>
<connect gate="D1" pin="C13" pad="10"/>
<connect gate="D1" pin="C14" pad="11"/>
<connect gate="D1" pin="C15" pad="15"/>
<connect gate="D1" pin="C16" pad="12"/>
<connect gate="D1" pin="C2" pad="25"/>
<connect gate="D1" pin="C3" pad="3"/>
<connect gate="D1" pin="C4" pad="4"/>
<connect gate="D1" pin="C5" pad="23"/>
<connect gate="D1" pin="C6" pad="5"/>
<connect gate="D1" pin="C7" pad="22"/>
<connect gate="D1" pin="C8" pad="21"/>
<connect gate="D1" pin="C9" pad="20"/>
<connect gate="D1" pin="G1" pad="7"/>
<connect gate="D1" pin="G2" pad="16"/>
<connect gate="D1" pin="G3" pad="2"/>
<connect gate="D1" pin="R1" pad="9"/>
<connect gate="D1" pin="R2" pad="17"/>
<connect gate="D1" pin="R3" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="COM-13520"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SMA-B500" prefix="D">
<description>&lt;h3&gt;American Opto Plus LED Corp. - SMA-B520LB&lt;/h3&gt;
&lt;p&gt;5 segment SMD LED Bar Graph Display, Bright Blue&lt;/p&gt;
&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13688”&gt;MyoWare LED Shield&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LED_BAR_SMD"/>
</gates>
<devices>
<device name="" package="LED_BAR_SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-13127"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SUNLED" prefix="D">
<description>&lt;h3&gt;LED-RGB Common Cathode&lt;/h3&gt;
&lt;p&gt;XZM2CRKM2DGFBB45SCCB&lt;/p&gt;
&lt;li&gt;&lt;b&gt;Packages:&lt;/b&gt;&lt;/li&gt;
&lt;ul&gt;&lt;li&gt; PLCC4&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;


&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”[https://www.sparkfun.com/products/9264]”&gt;Lilypad Prototyping Board&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G1" symbol="LED-RGB-CC"/>
</gates>
<devices>
<device name="SMD1" package="PLCC4SMDLED">
<connects>
<connect gate="G1" pin="BLU" pad="3"/>
<connect gate="G1" pin="C" pad="4"/>
<connect gate="G1" pin="GRN" pad="2"/>
<connect gate="G1" pin="RED" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-13722"/>
<attribute name="VALUE" value="XZM2CRKM2DGFBB45SCCB"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="APA102" prefix="D">
<description>&lt;h3&gt;APA102 Addressable RGB LED&lt;/h3&gt;

&lt;p&gt;Used in manufacturing of various products at SparkFun&lt;/p&gt;


&lt;p&gt;&lt;b&gt;Packages:&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;&lt;b&gt;5050&lt;/b&gt;&lt;/li&gt;
&lt;li&gt;&lt;b&gt;2020&lt;/b&gt; &lt;/li&gt;
&lt;ul&gt;
&lt;/p&gt;

&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”https://www.sparkfun.com/categories/405”&gt;SparkFun Lumenati Boards&lt;/a&gt;&lt;/li&gt;</description>
<gates>
<gate name="G$1" symbol="APA102"/>
</gates>
<devices>
<device name="-2020" package="APA102-2020">
<connects>
<connect gate="G$1" pin="CI" pad="CKI"/>
<connect gate="G$1" pin="CO" pad="CKO"/>
<connect gate="G$1" pin="DI" pad="SDI"/>
<connect gate="G$1" pin="DO" pad="SDO"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VCC" pad="VDD"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-13883"/>
</technology>
</technologies>
</device>
<device name="-5050" package="APA102-5050">
<connects>
<connect gate="G$1" pin="CI" pad="P2"/>
<connect gate="G$1" pin="CO" pad="P5"/>
<connect gate="G$1" pin="DI" pad="P1"/>
<connect gate="G$1" pin="DO" pad="P6"/>
<connect gate="G$1" pin="GND" pad="P3"/>
<connect gate="G$1" pin="VCC" pad="P4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-13739"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WS2812B-PTH">
<description>&lt;h3&gt;WS2812B PTH addressable RGB LED&lt;/h3&gt;

5mm PTH LED with built-in controller IC.

&lt;p&gt;&lt;li&gt;&lt;b&gt;Color:&lt;/b&gt; Red/Green/Blue&lt;/li&gt;
&lt;li&gt;&lt;b&gt;mC Rating: &lt;/b&gt;RGB: 390, 660, 180 mcd&lt;/li&gt;
&lt;li&gt;&lt;b&gt;Forward Voltage: &lt;/b&gt; RGB: 2.0, 3.0, 3.0 V&lt;/li&gt;

&lt;/p&gt;
&lt;p&gt;SparkFun Products:

&lt;ul&gt;

&lt;li&gt;&lt;a href = https://www.sparkfun.com/products/12986&gt;LED - RGB Addressable, PTH, 5mm Diffused (5 Pack)&lt;/a&gt;&lt;/li&gt;



&lt;li&gt;&lt;a href = https://www.sparkfun.com/products/12999&gt;LED - RGB Addressable, PTH, 5mm Clear (5 Pack)&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;

&lt;/p&gt;

&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt; &lt;a href="https://cdn.sparkfun.com/datasheets/Components/LED/COM-12877.pdf"&gt;WS2812B-PTH&lt;/a&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LED-TRICOLOR-WS28X1"/>
</gates>
<devices>
<device name="" package="WS2812B-PTH-KIT">
<connects>
<connect gate="G$1" pin="DI" pad="1"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VSS" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WS2812-2020">
<gates>
<gate name="G$1" symbol="LED-TRICOLOR-WS28X1"/>
</gates>
<devices>
<device name="" package="WS2812-2020">
<connects>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-UV" prefix="D">
<gates>
<gate name="D1" symbol="LED"/>
</gates>
<devices>
<device name="PLCC" package="PLCC-2">
<connects>
<connect gate="D1" pin="A" pad="A"/>
<connect gate="D1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-14126"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
